From 6dac092b12755ccbc00412871cd9535b687d16d7 Mon Sep 17 00:00:00 2001
From: Rafa? Mi?ecki <zajec5@gmail.com>
Date: Fri, 3 Jan 2014 09:55:30 +0100
Subject: [PATCH] MIPS: BCM47XX: Enable buttons support on SSB

This is supported since implementing IRQ domain in ssb.

Signed-off-by: Rafa? Mi?ecki <zajec5@gmail.com>
---
 arch/mips/bcm47xx/buttons.c |    8 --------
 1 file changed, 8 deletions(-)

--- a/arch/mips/bcm47xx/buttons.c
+++ b/arch/mips/bcm47xx/buttons.c
@@ -3,7 +3,6 @@
 #include <linux/input.h>
 #include <linux/gpio_keys.h>
 #include <linux/interrupt.h>
-#include <linux/ssb/ssb_embedded.h>
 #include <bcm47xx_board.h>
 #include <bcm47xx.h>
 
@@ -371,13 +370,6 @@ int __init bcm47xx_buttons_register(void
 	enum bcm47xx_board board = bcm47xx_board_get();
 	int err;
 
-#ifdef CONFIG_BCM47XX_SSB
-	if (bcm47xx_bus_type == BCM47XX_BUS_TYPE_SSB) {
-		pr_debug("Buttons on SSB are not supported yet.\n");
-		return -ENOTSUPP;
-	}
-#endif
-
 	switch (board) {
 	case BCM47XX_BOARD_ASUS_RTN12:
 		err = bcm47xx_copy_bdata(bcm47xx_buttons_asus_rtn12);
