From 799e69d38053e344267360a583676eafe2ed8648 Mon Sep 17 00:00:00 2001
From: Sebastian Hesselbarth <sebastian.hesselbarth@gmail.com>
Date: Wed, 29 May 2013 09:32:43 +0000
Subject: [PATCH 20/29] net: mv643xx_eth: use phy_disconnect instead of
 phy_detach

Using a separated mdio bus driver with mvmdio, phy_detach on network device
removal will not stop the phy and finally lead to NULL pointer dereference
in mvmdio due to non-existent network device. Use phy_disconnect instead
to properly stop phy device from accessing network device prior removal of
the network device.

Signed-off-by: Sebastian Hesselbarth <sebastian.hesselbarth@gmail.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/ethernet/marvell/mv643xx_eth.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/net/ethernet/marvell/mv643xx_eth.c
+++ b/drivers/net/ethernet/marvell/mv643xx_eth.c
@@ -2803,7 +2803,7 @@ static int mv643xx_eth_remove(struct pla
 
 	unregister_netdev(mp->dev);
 	if (mp->phy != NULL)
-		phy_detach(mp->phy);
+		phy_disconnect(mp->phy);
 	cancel_work_sync(&mp->tx_timeout_task);
 
 	if (!IS_ERR(mp->clk))
