Adds AM33XX EDMA support to the am33xx.dtsi as documented in
Documentation/devicetree/bindings/dma/ti-edma.txt

[Joel Fernandes <joelf@ti.com>]
Drop DT entries that are non-hardware-description as discussed in [1]

[1] https://patchwork.kernel.org/patch/2226761/

Signed-off-by: Matt Porter <mporter@ti.com>
Signed-off-by: Joel A Fernandes <joelagnel@ti.com>

---
arch/arm/boot/dts/am33xx.dtsi | 12 ++++++++++++
 1 file changed, 12 insertions(+)

--- a/arch/arm/boot/dts/am33xx.dtsi
+++ b/arch/arm/boot/dts/am33xx.dtsi
@@ -100,6 +100,18 @@
 			reg = <0x48200000 0x1000>;
 		};
 
+		edma: edma@49000000 {
+			compatible = "ti,edma3";
+			ti,hwmods = "tpcc", "tptc0", "tptc1", "tptc2";
+			reg =	<0x49000000 0x10000>,
+				<0x44e10f90 0x10>;
+			interrupts = <12 13 14>;
+			#dma-cells = <1>;
+			dma-channels = <64>;
+			ti,edma-regions = <4>;
+			ti,edma-slots = <256>;
+		};
+
 		gpio0: gpio@44e07000 {
 			compatible = "ti,omap4-gpio";
 			ti,hwmods = "gpio1";
