From 9468f2e1fb54a67c70f627b3cc75a692b3c2ebce Mon Sep 17 00:00:00 2001
From: Hans de Goede <hdegoede@redhat.com>
Date: Tue, 17 Dec 2013 23:26:45 +0100
Subject: [PATCH] ARM: dts: sun7i: Fix ehci interrupt types

Signed-off-by: Hans de Goede <hdegoede@redhat.com>
---
 arch/arm/boot/dts/sun7i-a20.dtsi | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

diff --git a/arch/arm/boot/dts/sun7i-a20.dtsi b/arch/arm/boot/dts/sun7i-a20.dtsi
index 9f99959..dcee675 100644
--- a/arch/arm/boot/dts/sun7i-a20.dtsi
+++ b/arch/arm/boot/dts/sun7i-a20.dtsi
@@ -648,7 +648,7 @@
 		ehci0: ehci0@0x01c14000 {
 			compatible = "allwinner,sunxi-ehci";
 			reg = <0x01c14000 0x400 0x01c14800 0x4 0x01c13404 0x4>;
-			interrupts = <0 39 1>;
+			interrupts = <0 39 4>;
 			resets = <&usb_rst 1>;
 			reset-names = "ehci_reset";
 			clocks = <&usb 8>, <&ahb_gates 1>;
@@ -659,7 +659,7 @@
 		ehci1: ehci1@0x01c1c000 {
 			compatible = "allwinner,sunxi-ehci";
 			reg = <0x01c1c000 0x400 0x01c1c800 0x4 0x01c13404 0x4>;
-			interrupts = <0 40 1>;
+			interrupts = <0 40 4>;
 			resets = <&usb_rst 2>;
 			reset-names = "ehci_reset";
 			clocks = <&usb 8>, <&ahb_gates 3>;
-- 
1.8.5.1

