From c1bac171c4f203101611110869bd2511c8153974 Mon Sep 17 00:00:00 2001
From: Nishanth Menon <nm@ti.com>
Date: Thu, 10 Oct 2013 16:44:41 +0000
Subject: ARM: dts: omap4-panda-es: Do not reset gpio1

Do not reset GPIO1 at boot-up because GPIO 7 in GPIO1 block is used on
OMAP4460 PandaBoard-ES to select voltage register in TPS62361 which
supplies VDD_MPU.

Without this, OMAP4460 PandaBoard-ES boards fail to boot-up because
MPU voltage switches over to VSET0 voltage value (boot voltage) which
is not sufficient to operate the device at OPP100.

Signed-off-by: Nishanth Menon <nm@ti.com>
Signed-off-by: Benoit Cousson <bcousson@baylibre.com>
---
--- a/arch/arm/boot/dts/omap4-panda-es.dts
+++ b/arch/arm/boot/dts/omap4-panda-es.dts
@@ -62,3 +62,7 @@
 		gpios = <&gpio1 8 GPIO_ACTIVE_HIGH>;
 	};
 };
+
+&gpio1 {
+	 ti,no-reset-on-init;
+};
