--- a/arch/mips/bcm47xx/serial.c
+++ b/arch/mips/bcm47xx/serial.c
@@ -62,7 +62,7 @@ static int __init uart8250_init_bcma(voi
 
 		p->mapbase = (unsigned int) bcma_port->regs;
 		p->membase = (void *) bcma_port->regs;
-		p->irq = bcma_port->irq + 2;
+		p->irq = bcma_port->irq;
 		p->uartclk = bcma_port->baud_base;
 		p->regshift = bcma_port->reg_shift;
 		p->iotype = UPIO_MEM;
--- a/drivers/bcma/Kconfig
+++ b/drivers/bcma/Kconfig
@@ -26,6 +26,7 @@ config BCMA_HOST_PCI_POSSIBLE
 config BCMA_HOST_PCI
 	bool "Support for BCMA on PCI-host bus"
 	depends on BCMA_HOST_PCI_POSSIBLE
+	default y
 
 config BCMA_DRIVER_PCI_HOSTMODE
 	bool "Driver for PCI core working in hostmode"
@@ -34,8 +35,14 @@ config BCMA_DRIVER_PCI_HOSTMODE
 	  PCI core hostmode operation (external PCI bus).
 
 config BCMA_HOST_SOC
-	bool
-	depends on BCMA_DRIVER_MIPS
+	bool "Support for BCMA in a SoC"
+	depends on BCMA
+	help
+	  Host interface for a Broadcom AIX bus directly mapped into
+	  the memory. This only works with the Broadcom SoCs from the
+	  BCM47XX line.
+
+	  If unsure, say N
 
 config BCMA_DRIVER_MIPS
 	bool "BCMA Broadcom MIPS core driver"
@@ -48,12 +55,12 @@ config BCMA_DRIVER_MIPS
 
 config BCMA_SFLASH
 	bool
-	depends on BCMA_DRIVER_MIPS && BROKEN
+	depends on BCMA_DRIVER_MIPS
 	default y
 
 config BCMA_NFLASH
 	bool
-	depends on BCMA_DRIVER_MIPS && BROKEN
+	depends on BCMA_DRIVER_MIPS
 	default y
 
 config BCMA_DRIVER_GMAC_CMN
@@ -65,6 +72,14 @@ config BCMA_DRIVER_GMAC_CMN
 
 	  If unsure, say N
 
+config BCMA_DRIVER_GPIO
+	bool "BCMA GPIO driver"
+	depends on BCMA && GPIOLIB
+	help
+	  Driver to provide access to the GPIO pins of the bcma bus.
+
+	  If unsure, say N
+
 config BCMA_DEBUG
 	bool "BCMA debugging"
 	depends on BCMA
--- a/drivers/bcma/Makefile
+++ b/drivers/bcma/Makefile
@@ -6,6 +6,7 @@ bcma-y					+= driver_pci.o
 bcma-$(CONFIG_BCMA_DRIVER_PCI_HOSTMODE)	+= driver_pci_host.o
 bcma-$(CONFIG_BCMA_DRIVER_MIPS)		+= driver_mips.o
 bcma-$(CONFIG_BCMA_DRIVER_GMAC_CMN)	+= driver_gmac_cmn.o
+bcma-$(CONFIG_BCMA_DRIVER_GPIO)		+= driver_gpio.o
 bcma-$(CONFIG_BCMA_HOST_PCI)		+= host_pci.o
 bcma-$(CONFIG_BCMA_HOST_SOC)		+= host_soc.o
 obj-$(CONFIG_BCMA)			+= bcma.o
--- a/drivers/bcma/bcma_private.h
+++ b/drivers/bcma/bcma_private.h
@@ -22,6 +22,8 @@
 struct bcma_bus;
 
 /* main.c */
+bool bcma_wait_value(struct bcma_device *core, u16 reg, u32 mask, u32 value,
+		     int timeout);
 int __devinit bcma_bus_register(struct bcma_bus *bus);
 void bcma_bus_unregister(struct bcma_bus *bus);
 int __init bcma_bus_early_register(struct bcma_bus *bus,
@@ -31,6 +33,8 @@ int __init bcma_bus_early_register(struc
 int bcma_bus_suspend(struct bcma_bus *bus);
 int bcma_bus_resume(struct bcma_bus *bus);
 #endif
+struct bcma_device *bcma_find_core_unit(struct bcma_bus *bus, u16 coreid,
+					u8 unit);
 
 /* scan.c */
 int bcma_bus_scan(struct bcma_bus *bus);
@@ -45,15 +49,17 @@ int bcma_sprom_get(struct bcma_bus *bus)
 /* driver_chipcommon.c */
 #ifdef CONFIG_BCMA_DRIVER_MIPS
 void bcma_chipco_serial_init(struct bcma_drv_cc *cc);
+extern struct platform_device bcma_pflash_dev;
 #endif /* CONFIG_BCMA_DRIVER_MIPS */
 
 /* driver_chipcommon_pmu.c */
-u32 bcma_pmu_alp_clock(struct bcma_drv_cc *cc);
-u32 bcma_pmu_get_clockcpu(struct bcma_drv_cc *cc);
+u32 bcma_pmu_get_alp_clock(struct bcma_drv_cc *cc);
+u32 bcma_pmu_get_cpu_clock(struct bcma_drv_cc *cc);
 
 #ifdef CONFIG_BCMA_SFLASH
 /* driver_chipcommon_sflash.c */
 int bcma_sflash_init(struct bcma_drv_cc *cc);
+extern struct platform_device bcma_sflash_dev;
 #else
 static inline int bcma_sflash_init(struct bcma_drv_cc *cc)
 {
@@ -65,6 +71,7 @@ static inline int bcma_sflash_init(struc
 #ifdef CONFIG_BCMA_NFLASH
 /* driver_chipcommon_nflash.c */
 int bcma_nflash_init(struct bcma_drv_cc *cc);
+extern struct platform_device bcma_nflash_dev;
 #else
 static inline int bcma_nflash_init(struct bcma_drv_cc *cc)
 {
@@ -82,9 +89,26 @@ extern void __exit bcma_host_pci_exit(vo
 /* driver_pci.c */
 u32 bcma_pcie_read(struct bcma_drv_pci *pc, u32 address);
 
+extern int bcma_chipco_watchdog_register(struct bcma_drv_cc *cc);
+
 #ifdef CONFIG_BCMA_DRIVER_PCI_HOSTMODE
 bool __devinit bcma_core_pci_is_in_hostmode(struct bcma_drv_pci *pc);
 void __devinit bcma_core_pci_hostmode_init(struct bcma_drv_pci *pc);
 #endif /* CONFIG_BCMA_DRIVER_PCI_HOSTMODE */
 
+#ifdef CONFIG_BCMA_DRIVER_GPIO
+/* driver_gpio.c */
+int bcma_gpio_init(struct bcma_drv_cc *cc);
+int bcma_gpio_unregister(struct bcma_drv_cc *cc);
+#else
+static inline int bcma_gpio_init(struct bcma_drv_cc *cc)
+{
+	return -ENOTSUPP;
+}
+static inline int bcma_gpio_unregister(struct bcma_drv_cc *cc)
+{
+	return 0;
+}
+#endif /* CONFIG_BCMA_DRIVER_GPIO */
+
 #endif
--- a/drivers/bcma/core.c
+++ b/drivers/bcma/core.c
@@ -9,6 +9,25 @@
 #include <linux/export.h>
 #include <linux/bcma/bcma.h>
 
+static bool bcma_core_wait_value(struct bcma_device *core, u16 reg, u32 mask,
+				 u32 value, int timeout)
+{
+	unsigned long deadline = jiffies + timeout;
+	u32 val;
+
+	do {
+		val = bcma_aread32(core, reg);
+		if ((val & mask) == value)
+			return true;
+		cpu_relax();
+		udelay(10);
+	} while (!time_after_eq(jiffies, deadline));
+
+	bcma_warn(core->bus, "Timeout waiting for register 0x%04X!\n", reg);
+
+	return false;
+}
+
 bool bcma_core_is_enabled(struct bcma_device *core)
 {
 	if ((bcma_aread32(core, BCMA_IOCTL) & (BCMA_IOCTL_CLK | BCMA_IOCTL_FGC))
@@ -25,13 +44,15 @@ void bcma_core_disable(struct bcma_devic
 	if (bcma_aread32(core, BCMA_RESET_CTL) & BCMA_RESET_CTL_RESET)
 		return;
 
-	bcma_awrite32(core, BCMA_IOCTL, flags);
-	bcma_aread32(core, BCMA_IOCTL);
-	udelay(10);
+	bcma_core_wait_value(core, BCMA_RESET_ST, ~0, 0, 300);
 
 	bcma_awrite32(core, BCMA_RESET_CTL, BCMA_RESET_CTL_RESET);
 	bcma_aread32(core, BCMA_RESET_CTL);
 	udelay(1);
+
+	bcma_awrite32(core, BCMA_IOCTL, flags);
+	bcma_aread32(core, BCMA_IOCTL);
+	udelay(10);
 }
 EXPORT_SYMBOL_GPL(bcma_core_disable);
 
@@ -43,6 +64,7 @@ int bcma_core_enable(struct bcma_device
 	bcma_aread32(core, BCMA_IOCTL);
 
 	bcma_awrite32(core, BCMA_RESET_CTL, 0);
+	bcma_aread32(core, BCMA_RESET_CTL);
 	udelay(1);
 
 	bcma_awrite32(core, BCMA_IOCTL, (BCMA_IOCTL_CLK | flags));
@@ -65,7 +87,7 @@ void bcma_core_set_clockmode(struct bcma
 	switch (clkmode) {
 	case BCMA_CLKMODE_FAST:
 		bcma_set32(core, BCMA_CLKCTLST, BCMA_CLKCTLST_FORCEHT);
-		udelay(64);
+		usleep_range(64, 300);
 		for (i = 0; i < 1500; i++) {
 			if (bcma_read32(core, BCMA_CLKCTLST) &
 			    BCMA_CLKCTLST_HAVEHT) {
@@ -104,7 +126,13 @@ void bcma_core_pll_ctl(struct bcma_devic
 		if (i)
 			bcma_err(core->bus, "PLL enable timeout\n");
 	} else {
-		bcma_warn(core->bus, "Disabling PLL not supported yet!\n");
+		/*
+		 * Mask the PLL but don't wait for it to be disabled. PLL may be
+		 * shared between cores and will be still up if there is another
+		 * core using it.
+		 */
+		bcma_mask32(core, BCMA_CLKCTLST, ~req);
+		bcma_read32(core, BCMA_CLKCTLST);
 	}
 }
 EXPORT_SYMBOL_GPL(bcma_core_pll_ctl);
--- a/drivers/bcma/driver_chipcommon.c
+++ b/drivers/bcma/driver_chipcommon.c
@@ -4,12 +4,15 @@
  *
  * Copyright 2005, Broadcom Corporation
  * Copyright 2006, 2007, Michael Buesch <m@bues.ch>
+ * Copyright 2012, Hauke Mehrtens <hauke@hauke-m.de>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
 
 #include "bcma_private.h"
+#include <linux/bcm47xx_wdt.h>
 #include <linux/export.h>
+#include <linux/platform_device.h>
 #include <linux/bcma/bcma.h>
 
 static inline u32 bcma_cc_write32_masked(struct bcma_drv_cc *cc, u16 offset,
@@ -22,23 +25,130 @@ static inline u32 bcma_cc_write32_masked
 	return value;
 }
 
-void bcma_core_chipcommon_init(struct bcma_drv_cc *cc)
+u32 bcma_chipco_get_alp_clock(struct bcma_drv_cc *cc)
 {
-	u32 leddc_on = 10;
-	u32 leddc_off = 90;
+	if (cc->capabilities & BCMA_CC_CAP_PMU)
+		return bcma_pmu_get_alp_clock(cc);
 
-	if (cc->setup_done)
+	return 20000000;
+}
+EXPORT_SYMBOL_GPL(bcma_chipco_get_alp_clock);
+
+static u32 bcma_chipco_watchdog_get_max_timer(struct bcma_drv_cc *cc)
+{
+	struct bcma_bus *bus = cc->core->bus;
+	u32 nb;
+
+	if (cc->capabilities & BCMA_CC_CAP_PMU) {
+		if (bus->chipinfo.id == BCMA_CHIP_ID_BCM4706)
+			nb = 32;
+		else if (cc->core->id.rev < 26)
+			nb = 16;
+		else
+			nb = (cc->core->id.rev >= 37) ? 32 : 24;
+	} else {
+		nb = 28;
+	}
+	if (nb == 32)
+		return 0xffffffff;
+	else
+		return (1 << nb) - 1;
+}
+
+static u32 bcma_chipco_watchdog_timer_set_wdt(struct bcm47xx_wdt *wdt,
+					      u32 ticks)
+{
+	struct bcma_drv_cc *cc = bcm47xx_wdt_get_drvdata(wdt);
+
+	return bcma_chipco_watchdog_timer_set(cc, ticks);
+}
+
+static u32 bcma_chipco_watchdog_timer_set_ms_wdt(struct bcm47xx_wdt *wdt,
+						 u32 ms)
+{
+	struct bcma_drv_cc *cc = bcm47xx_wdt_get_drvdata(wdt);
+	u32 ticks;
+
+	ticks = bcma_chipco_watchdog_timer_set(cc, cc->ticks_per_ms * ms);
+	return ticks / cc->ticks_per_ms;
+}
+
+static int bcma_chipco_watchdog_ticks_per_ms(struct bcma_drv_cc *cc)
+{
+	struct bcma_bus *bus = cc->core->bus;
+
+	if (cc->capabilities & BCMA_CC_CAP_PMU) {
+		if (bus->chipinfo.id == BCMA_CHIP_ID_BCM4706)
+			/* 4706 CC and PMU watchdogs are clocked at 1/4 of ALP clock */
+			return bcma_chipco_get_alp_clock(cc) / 4000;
+		else
+			/* based on 32KHz ILP clock */
+			return 32;
+	} else {
+		return bcma_chipco_get_alp_clock(cc) / 1000;
+	}
+}
+
+int bcma_chipco_watchdog_register(struct bcma_drv_cc *cc)
+{
+	struct bcm47xx_wdt wdt = {};
+	struct platform_device *pdev;
+
+	wdt.driver_data = cc;
+	wdt.timer_set = bcma_chipco_watchdog_timer_set_wdt;
+	wdt.timer_set_ms = bcma_chipco_watchdog_timer_set_ms_wdt;
+	wdt.max_timer_ms = bcma_chipco_watchdog_get_max_timer(cc) / cc->ticks_per_ms;
+
+	pdev = platform_device_register_data(NULL, "bcm47xx-wdt",
+					     cc->core->bus->num, &wdt,
+					     sizeof(wdt));
+	if (IS_ERR(pdev))
+		return PTR_ERR(pdev);
+
+	cc->watchdog = pdev;
+
+	return 0;
+}
+
+void bcma_core_chipcommon_early_init(struct bcma_drv_cc *cc)
+{
+	if (cc->early_setup_done)
 		return;
 
+	spin_lock_init(&cc->gpio_lock);
+
 	if (cc->core->id.rev >= 11)
 		cc->status = bcma_cc_read32(cc, BCMA_CC_CHIPSTAT);
 	cc->capabilities = bcma_cc_read32(cc, BCMA_CC_CAP);
 	if (cc->core->id.rev >= 35)
 		cc->capabilities_ext = bcma_cc_read32(cc, BCMA_CC_CAP_EXT);
 
+	if (cc->capabilities & BCMA_CC_CAP_PMU)
+		bcma_pmu_early_init(cc);
+
+	cc->early_setup_done = true;
+}
+
+void bcma_core_chipcommon_init(struct bcma_drv_cc *cc)
+{
+	u32 leddc_on = 10;
+	u32 leddc_off = 90;
+
+	if (cc->setup_done)
+		return;
+
+	bcma_core_chipcommon_early_init(cc);
+
 	if (cc->core->id.rev >= 20) {
-		bcma_cc_write32(cc, BCMA_CC_GPIOPULLUP, 0);
-		bcma_cc_write32(cc, BCMA_CC_GPIOPULLDOWN, 0);
+		u32 pullup = 0, pulldown = 0;
+
+		if (cc->core->bus->chipinfo.id == BCMA_CHIP_ID_BCM43142) {
+			pullup = 0x402e0;
+			pulldown = 0x20500;
+		}
+
+		bcma_cc_write32(cc, BCMA_CC_GPIOPULLUP, pullup);
+		bcma_cc_write32(cc, BCMA_CC_GPIOPULLDOWN, pulldown);
 	}
 
 	if (cc->capabilities & BCMA_CC_CAP_PMU)
@@ -56,15 +166,33 @@ void bcma_core_chipcommon_init(struct bc
 			((leddc_on << BCMA_CC_GPIOTIMER_ONTIME_SHIFT) |
 			 (leddc_off << BCMA_CC_GPIOTIMER_OFFTIME_SHIFT)));
 	}
+	cc->ticks_per_ms = bcma_chipco_watchdog_ticks_per_ms(cc);
 
 	cc->setup_done = true;
 }
 
 /* Set chip watchdog reset timer to fire in 'ticks' backplane cycles */
-void bcma_chipco_watchdog_timer_set(struct bcma_drv_cc *cc, u32 ticks)
+u32 bcma_chipco_watchdog_timer_set(struct bcma_drv_cc *cc, u32 ticks)
 {
-	/* instant NMI */
-	bcma_cc_write32(cc, BCMA_CC_WATCHDOG, ticks);
+	u32 maxt;
+	enum bcma_clkmode clkmode;
+
+	maxt = bcma_chipco_watchdog_get_max_timer(cc);
+	if (cc->capabilities & BCMA_CC_CAP_PMU) {
+		if (ticks == 1)
+			ticks = 2;
+		else if (ticks > maxt)
+			ticks = maxt;
+		bcma_cc_write32(cc, BCMA_CC_PMU_WATCHDOG, ticks);
+	} else {
+		clkmode = ticks ? BCMA_CLKMODE_FAST : BCMA_CLKMODE_DYNAMIC;
+		bcma_core_set_clockmode(cc->core, clkmode);
+		if (ticks > maxt)
+			ticks = maxt;
+		/* instant NMI */
+		bcma_cc_write32(cc, BCMA_CC_WATCHDOG, ticks);
+	}
+	return ticks;
 }
 
 void bcma_chipco_irq_mask(struct bcma_drv_cc *cc, u32 mask, u32 value)
@@ -84,28 +212,99 @@ u32 bcma_chipco_gpio_in(struct bcma_drv_
 
 u32 bcma_chipco_gpio_out(struct bcma_drv_cc *cc, u32 mask, u32 value)
 {
-	return bcma_cc_write32_masked(cc, BCMA_CC_GPIOOUT, mask, value);
+	unsigned long flags;
+	u32 res;
+
+	spin_lock_irqsave(&cc->gpio_lock, flags);
+	res = bcma_cc_write32_masked(cc, BCMA_CC_GPIOOUT, mask, value);
+	spin_unlock_irqrestore(&cc->gpio_lock, flags);
+
+	return res;
 }
+EXPORT_SYMBOL_GPL(bcma_chipco_gpio_out);
 
 u32 bcma_chipco_gpio_outen(struct bcma_drv_cc *cc, u32 mask, u32 value)
 {
-	return bcma_cc_write32_masked(cc, BCMA_CC_GPIOOUTEN, mask, value);
+	unsigned long flags;
+	u32 res;
+
+	spin_lock_irqsave(&cc->gpio_lock, flags);
+	res = bcma_cc_write32_masked(cc, BCMA_CC_GPIOOUTEN, mask, value);
+	spin_unlock_irqrestore(&cc->gpio_lock, flags);
+
+	return res;
 }
+EXPORT_SYMBOL_GPL(bcma_chipco_gpio_outen);
 
+/*
+ * If the bit is set to 0, chipcommon controlls this GPIO,
+ * if the bit is set to 1, it is used by some part of the chip and not our code.
+ */
 u32 bcma_chipco_gpio_control(struct bcma_drv_cc *cc, u32 mask, u32 value)
 {
-	return bcma_cc_write32_masked(cc, BCMA_CC_GPIOCTL, mask, value);
+	unsigned long flags;
+	u32 res;
+
+	spin_lock_irqsave(&cc->gpio_lock, flags);
+	res = bcma_cc_write32_masked(cc, BCMA_CC_GPIOCTL, mask, value);
+	spin_unlock_irqrestore(&cc->gpio_lock, flags);
+
+	return res;
 }
 EXPORT_SYMBOL_GPL(bcma_chipco_gpio_control);
 
 u32 bcma_chipco_gpio_intmask(struct bcma_drv_cc *cc, u32 mask, u32 value)
 {
-	return bcma_cc_write32_masked(cc, BCMA_CC_GPIOIRQ, mask, value);
+	unsigned long flags;
+	u32 res;
+
+	spin_lock_irqsave(&cc->gpio_lock, flags);
+	res = bcma_cc_write32_masked(cc, BCMA_CC_GPIOIRQ, mask, value);
+	spin_unlock_irqrestore(&cc->gpio_lock, flags);
+
+	return res;
 }
 
 u32 bcma_chipco_gpio_polarity(struct bcma_drv_cc *cc, u32 mask, u32 value)
 {
-	return bcma_cc_write32_masked(cc, BCMA_CC_GPIOPOL, mask, value);
+	unsigned long flags;
+	u32 res;
+
+	spin_lock_irqsave(&cc->gpio_lock, flags);
+	res = bcma_cc_write32_masked(cc, BCMA_CC_GPIOPOL, mask, value);
+	spin_unlock_irqrestore(&cc->gpio_lock, flags);
+
+	return res;
+}
+
+u32 bcma_chipco_gpio_pullup(struct bcma_drv_cc *cc, u32 mask, u32 value)
+{
+	unsigned long flags;
+	u32 res;
+
+	if (cc->core->id.rev < 20)
+		return 0;
+
+	spin_lock_irqsave(&cc->gpio_lock, flags);
+	res = bcma_cc_write32_masked(cc, BCMA_CC_GPIOPULLUP, mask, value);
+	spin_unlock_irqrestore(&cc->gpio_lock, flags);
+
+	return res;
+}
+
+u32 bcma_chipco_gpio_pulldown(struct bcma_drv_cc *cc, u32 mask, u32 value)
+{
+	unsigned long flags;
+	u32 res;
+
+	if (cc->core->id.rev < 20)
+		return 0;
+
+	spin_lock_irqsave(&cc->gpio_lock, flags);
+	res = bcma_cc_write32_masked(cc, BCMA_CC_GPIOPULLDOWN, mask, value);
+	spin_unlock_irqrestore(&cc->gpio_lock, flags);
+
+	return res;
 }
 
 #ifdef CONFIG_BCMA_DRIVER_MIPS
@@ -118,8 +317,7 @@ void bcma_chipco_serial_init(struct bcma
 	struct bcma_serial_port *ports = cc->serial_ports;
 
 	if (ccrev >= 11 && ccrev != 15) {
-		/* Fixed ALP clock */
-		baud_base = bcma_pmu_alp_clock(cc);
+		baud_base = bcma_chipco_get_alp_clock(cc);
 		if (ccrev >= 21) {
 			/* Turn off UART clock before switching clocksource. */
 			bcma_cc_write32(cc, BCMA_CC_CORECTL,
@@ -141,7 +339,7 @@ void bcma_chipco_serial_init(struct bcma
 		return;
 	}
 
-	irq = bcma_core_mips_irq(cc->core);
+	irq = bcma_core_irq(cc->core);
 
 	/* Determine the registers of the UARTs */
 	cc->nr_serial_ports = (cc->capabilities & BCMA_CC_CAP_NRUART);
--- a/drivers/bcma/driver_chipcommon_nflash.c
+++ b/drivers/bcma/driver_chipcommon_nflash.c
@@ -5,15 +5,40 @@
  * Licensed under the GNU/GPL. See COPYING for details.
  */
 
+#include "bcma_private.h"
+
+#include <linux/platform_device.h>
 #include <linux/bcma/bcma.h>
-#include <linux/bcma/bcma_driver_chipcommon.h>
-#include <linux/delay.h>
 
-#include "bcma_private.h"
+struct platform_device bcma_nflash_dev = {
+	.name		= "bcma_nflash",
+	.num_resources	= 0,
+};
 
 /* Initialize NAND flash access */
 int bcma_nflash_init(struct bcma_drv_cc *cc)
 {
-	bcma_err(cc->core->bus, "NAND flash support is broken\n");
+	struct bcma_bus *bus = cc->core->bus;
+
+	if (bus->chipinfo.id != BCMA_CHIP_ID_BCM4706 &&
+	    cc->core->id.rev != 38) {
+		bcma_err(bus, "NAND flash on unsupported board!\n");
+		return -ENOTSUPP;
+	}
+
+	if (!(cc->capabilities & BCMA_CC_CAP_NFLASH)) {
+		bcma_err(bus, "NAND flash not present according to ChipCommon\n");
+		return -ENODEV;
+	}
+
+	cc->nflash.present = true;
+	if (cc->core->id.rev == 38 &&
+	    (cc->status & BCMA_CC_CHIPST_5357_NAND_BOOT))
+		cc->nflash.boot = true;
+
+	/* Prepare platform device, but don't register it yet. It's too early,
+	 * malloc (required by device_private_init) is not available yet. */
+	bcma_nflash_dev.dev.platform_data = &cc->nflash;
+
 	return 0;
 }
--- a/drivers/bcma/driver_chipcommon_pmu.c
+++ b/drivers/bcma/driver_chipcommon_pmu.c
@@ -13,12 +13,13 @@
 #include <linux/export.h>
 #include <linux/bcma/bcma.h>
 
-static u32 bcma_chipco_pll_read(struct bcma_drv_cc *cc, u32 offset)
+u32 bcma_chipco_pll_read(struct bcma_drv_cc *cc, u32 offset)
 {
 	bcma_cc_write32(cc, BCMA_CC_PLLCTL_ADDR, offset);
 	bcma_cc_read32(cc, BCMA_CC_PLLCTL_ADDR);
 	return bcma_cc_read32(cc, BCMA_CC_PLLCTL_DATA);
 }
+EXPORT_SYMBOL_GPL(bcma_chipco_pll_read);
 
 void bcma_chipco_pll_write(struct bcma_drv_cc *cc, u32 offset, u32 value)
 {
@@ -55,6 +56,109 @@ void bcma_chipco_regctl_maskset(struct b
 }
 EXPORT_SYMBOL_GPL(bcma_chipco_regctl_maskset);
 
+static u32 bcma_pmu_xtalfreq(struct bcma_drv_cc *cc)
+{
+	u32 ilp_ctl, alp_hz;
+
+	if (!(bcma_cc_read32(cc, BCMA_CC_PMU_STAT) &
+	      BCMA_CC_PMU_STAT_EXT_LPO_AVAIL))
+		return 0;
+
+	bcma_cc_write32(cc, BCMA_CC_PMU_XTAL_FREQ,
+			BIT(BCMA_CC_PMU_XTAL_FREQ_MEASURE_SHIFT));
+	usleep_range(1000, 2000);
+
+	ilp_ctl = bcma_cc_read32(cc, BCMA_CC_PMU_XTAL_FREQ);
+	ilp_ctl &= BCMA_CC_PMU_XTAL_FREQ_ILPCTL_MASK;
+
+	bcma_cc_write32(cc, BCMA_CC_PMU_XTAL_FREQ, 0);
+
+	alp_hz = ilp_ctl * 32768 / 4;
+	return (alp_hz + 50000) / 100000 * 100;
+}
+
+static void bcma_pmu2_pll_init0(struct bcma_drv_cc *cc, u32 xtalfreq)
+{
+	struct bcma_bus *bus = cc->core->bus;
+	u32 freq_tgt_target = 0, freq_tgt_current;
+	u32 pll0, mask;
+
+	switch (bus->chipinfo.id) {
+	case BCMA_CHIP_ID_BCM43142:
+		/* pmu2_xtaltab0_adfll_485 */
+		switch (xtalfreq) {
+		case 12000:
+			freq_tgt_target = 0x50D52;
+			break;
+		case 20000:
+			freq_tgt_target = 0x307FE;
+			break;
+		case 26000:
+			freq_tgt_target = 0x254EA;
+			break;
+		case 37400:
+			freq_tgt_target = 0x19EF8;
+			break;
+		case 52000:
+			freq_tgt_target = 0x12A75;
+			break;
+		}
+		break;
+	}
+
+	if (!freq_tgt_target) {
+		bcma_err(bus, "Unknown TGT frequency for xtalfreq %d\n",
+			 xtalfreq);
+		return;
+	}
+
+	pll0 = bcma_chipco_pll_read(cc, BCMA_CC_PMU15_PLL_PLLCTL0);
+	freq_tgt_current = (pll0 & BCMA_CC_PMU15_PLL_PC0_FREQTGT_MASK) >>
+		BCMA_CC_PMU15_PLL_PC0_FREQTGT_SHIFT;
+
+	if (freq_tgt_current == freq_tgt_target) {
+		bcma_debug(bus, "Target TGT frequency already set\n");
+		return;
+	}
+
+	/* Turn off PLL */
+	switch (bus->chipinfo.id) {
+	case BCMA_CHIP_ID_BCM43142:
+		mask = (u32)~(BCMA_RES_4314_HT_AVAIL |
+			      BCMA_RES_4314_MACPHY_CLK_AVAIL);
+
+		bcma_cc_mask32(cc, BCMA_CC_PMU_MINRES_MSK, mask);
+		bcma_cc_mask32(cc, BCMA_CC_PMU_MAXRES_MSK, mask);
+		bcma_wait_value(cc->core, BCMA_CLKCTLST,
+				BCMA_CLKCTLST_HAVEHT, 0, 20000);
+		break;
+	}
+
+	pll0 &= ~BCMA_CC_PMU15_PLL_PC0_FREQTGT_MASK;
+	pll0 |= freq_tgt_target << BCMA_CC_PMU15_PLL_PC0_FREQTGT_SHIFT;
+	bcma_chipco_pll_write(cc, BCMA_CC_PMU15_PLL_PLLCTL0, pll0);
+
+	/* Flush */
+	if (cc->pmu.rev >= 2)
+		bcma_cc_set32(cc, BCMA_CC_PMU_CTL, BCMA_CC_PMU_CTL_PLL_UPD);
+
+	/* TODO: Do we need to update OTP? */
+}
+
+static void bcma_pmu_pll_init(struct bcma_drv_cc *cc)
+{
+	struct bcma_bus *bus = cc->core->bus;
+	u32 xtalfreq = bcma_pmu_xtalfreq(cc);
+
+	switch (bus->chipinfo.id) {
+	case BCMA_CHIP_ID_BCM43142:
+		if (xtalfreq == 0)
+			xtalfreq = 20000;
+		bcma_pmu2_pll_init0(cc, xtalfreq);
+		break;
+	}
+}
+
 static void bcma_pmu_resources_init(struct bcma_drv_cc *cc)
 {
 	struct bcma_bus *bus = cc->core->bus;
@@ -65,6 +169,25 @@ static void bcma_pmu_resources_init(stru
 		min_msk = 0x200D;
 		max_msk = 0xFFFF;
 		break;
+	case BCMA_CHIP_ID_BCM43142:
+		min_msk = BCMA_RES_4314_LPLDO_PU |
+			  BCMA_RES_4314_PMU_SLEEP_DIS |
+			  BCMA_RES_4314_PMU_BG_PU |
+			  BCMA_RES_4314_CBUCK_LPOM_PU |
+			  BCMA_RES_4314_CBUCK_PFM_PU |
+			  BCMA_RES_4314_CLDO_PU |
+			  BCMA_RES_4314_LPLDO2_LVM |
+			  BCMA_RES_4314_WL_PMU_PU |
+			  BCMA_RES_4314_LDO3P3_PU |
+			  BCMA_RES_4314_OTP_PU |
+			  BCMA_RES_4314_WL_PWRSW_PU |
+			  BCMA_RES_4314_LQ_AVAIL |
+			  BCMA_RES_4314_LOGIC_RET |
+			  BCMA_RES_4314_MEM_SLEEP |
+			  BCMA_RES_4314_MACPHY_RET |
+			  BCMA_RES_4314_WL_CORE_READY;
+		max_msk = 0x3FFFFFFF;
+		break;
 	default:
 		bcma_debug(bus, "PMU resource config unknown or not needed for device 0x%04X\n",
 			   bus->chipinfo.id);
@@ -76,7 +199,10 @@ static void bcma_pmu_resources_init(stru
 	if (max_msk)
 		bcma_cc_write32(cc, BCMA_CC_PMU_MAXRES_MSK, max_msk);
 
-	/* Add some delay; allow resources to come up and settle. */
+	/*
+	 * Add some delay; allow resources to come up and settle.
+	 * Delay is required for SoC (early init).
+	 */
 	mdelay(2);
 }
 
@@ -101,7 +227,7 @@ void bcma_chipco_bcm4331_ext_pa_lines_ct
 	bcma_cc_write32(cc, BCMA_CC_CHIPCTL, val);
 }
 
-void bcma_pmu_workarounds(struct bcma_drv_cc *cc)
+static void bcma_pmu_workarounds(struct bcma_drv_cc *cc)
 {
 	struct bcma_bus *bus = cc->core->bus;
 
@@ -141,7 +267,7 @@ void bcma_pmu_workarounds(struct bcma_dr
 	}
 }
 
-void bcma_pmu_init(struct bcma_drv_cc *cc)
+void bcma_pmu_early_init(struct bcma_drv_cc *cc)
 {
 	u32 pmucap;
 
@@ -150,7 +276,10 @@ void bcma_pmu_init(struct bcma_drv_cc *c
 
 	bcma_debug(cc->core->bus, "Found rev %u PMU (capabilities 0x%08X)\n",
 		   cc->pmu.rev, pmucap);
+}
 
+void bcma_pmu_init(struct bcma_drv_cc *cc)
+{
 	if (cc->pmu.rev == 1)
 		bcma_cc_mask32(cc, BCMA_CC_PMU_CTL,
 			      ~BCMA_CC_PMU_CTL_NOILPONW);
@@ -158,28 +287,45 @@ void bcma_pmu_init(struct bcma_drv_cc *c
 		bcma_cc_set32(cc, BCMA_CC_PMU_CTL,
 			     BCMA_CC_PMU_CTL_NOILPONW);
 
+	bcma_pmu_pll_init(cc);
 	bcma_pmu_resources_init(cc);
 	bcma_pmu_workarounds(cc);
 }
 
-u32 bcma_pmu_alp_clock(struct bcma_drv_cc *cc)
+u32 bcma_pmu_get_alp_clock(struct bcma_drv_cc *cc)
 {
 	struct bcma_bus *bus = cc->core->bus;
 
 	switch (bus->chipinfo.id) {
+	case BCMA_CHIP_ID_BCM4313:
+	case BCMA_CHIP_ID_BCM43224:
+	case BCMA_CHIP_ID_BCM43225:
+	case BCMA_CHIP_ID_BCM43227:
+	case BCMA_CHIP_ID_BCM43228:
+	case BCMA_CHIP_ID_BCM4331:
+	case BCMA_CHIP_ID_BCM43421:
+	case BCMA_CHIP_ID_BCM43428:
+	case BCMA_CHIP_ID_BCM43431:
 	case BCMA_CHIP_ID_BCM4716:
-	case BCMA_CHIP_ID_BCM4748:
 	case BCMA_CHIP_ID_BCM47162:
-	case BCMA_CHIP_ID_BCM4313:
-	case BCMA_CHIP_ID_BCM5357:
+	case BCMA_CHIP_ID_BCM4748:
 	case BCMA_CHIP_ID_BCM4749:
+	case BCMA_CHIP_ID_BCM5357:
 	case BCMA_CHIP_ID_BCM53572:
+	case BCMA_CHIP_ID_BCM6362:
 		/* always 20Mhz */
 		return 20000 * 1000;
-	case BCMA_CHIP_ID_BCM5356:
 	case BCMA_CHIP_ID_BCM4706:
+	case BCMA_CHIP_ID_BCM5356:
 		/* always 25Mhz */
 		return 25000 * 1000;
+	case BCMA_CHIP_ID_BCM43460:
+	case BCMA_CHIP_ID_BCM4352:
+	case BCMA_CHIP_ID_BCM4360:
+		if (cc->status & BCMA_CC_CHIPST_4360_XTAL_40MZ)
+			return 40000 * 1000;
+		else
+			return 20000 * 1000;
 	default:
 		bcma_warn(bus, "No ALP clock specified for %04X device, pmu rev. %d, using default %d Hz\n",
 			  bus->chipinfo.id, cc->pmu.rev, BCMA_CC_PMU_ALP_CLOCK);
@@ -190,7 +336,7 @@ u32 bcma_pmu_alp_clock(struct bcma_drv_c
 /* Find the output of the "m" pll divider given pll controls that start with
  * pllreg "pll0" i.e. 12 for main 6 for phy, 0 for misc.
  */
-static u32 bcma_pmu_clock(struct bcma_drv_cc *cc, u32 pll0, u32 m)
+static u32 bcma_pmu_pll_clock(struct bcma_drv_cc *cc, u32 pll0, u32 m)
 {
 	u32 tmp, div, ndiv, p1, p2, fc;
 	struct bcma_bus *bus = cc->core->bus;
@@ -219,14 +365,14 @@ static u32 bcma_pmu_clock(struct bcma_dr
 	ndiv = (tmp & BCMA_CC_PPL_NDIV_MASK) >> BCMA_CC_PPL_NDIV_SHIFT;
 
 	/* Do calculation in Mhz */
-	fc = bcma_pmu_alp_clock(cc) / 1000000;
+	fc = bcma_pmu_get_alp_clock(cc) / 1000000;
 	fc = (p1 * ndiv * fc) / p2;
 
 	/* Return clock in Hertz */
 	return (fc / div) * 1000000;
 }
 
-static u32 bcma_pmu_clock_bcm4706(struct bcma_drv_cc *cc, u32 pll0, u32 m)
+static u32 bcma_pmu_pll_clock_bcm4706(struct bcma_drv_cc *cc, u32 pll0, u32 m)
 {
 	u32 tmp, ndiv, p1div, p2div;
 	u32 clock;
@@ -257,7 +403,7 @@ static u32 bcma_pmu_clock_bcm4706(struct
 }
 
 /* query bus clock frequency for PMU-enabled chipcommon */
-u32 bcma_pmu_get_clockcontrol(struct bcma_drv_cc *cc)
+u32 bcma_pmu_get_bus_clock(struct bcma_drv_cc *cc)
 {
 	struct bcma_bus *bus = cc->core->bus;
 
@@ -265,40 +411,43 @@ u32 bcma_pmu_get_clockcontrol(struct bcm
 	case BCMA_CHIP_ID_BCM4716:
 	case BCMA_CHIP_ID_BCM4748:
 	case BCMA_CHIP_ID_BCM47162:
-		return bcma_pmu_clock(cc, BCMA_CC_PMU4716_MAINPLL_PLL0,
-				      BCMA_CC_PMU5_MAINPLL_SSB);
+		return bcma_pmu_pll_clock(cc, BCMA_CC_PMU4716_MAINPLL_PLL0,
+					  BCMA_CC_PMU5_MAINPLL_SSB);
 	case BCMA_CHIP_ID_BCM5356:
-		return bcma_pmu_clock(cc, BCMA_CC_PMU5356_MAINPLL_PLL0,
-				      BCMA_CC_PMU5_MAINPLL_SSB);
+		return bcma_pmu_pll_clock(cc, BCMA_CC_PMU5356_MAINPLL_PLL0,
+					  BCMA_CC_PMU5_MAINPLL_SSB);
 	case BCMA_CHIP_ID_BCM5357:
 	case BCMA_CHIP_ID_BCM4749:
-		return bcma_pmu_clock(cc, BCMA_CC_PMU5357_MAINPLL_PLL0,
-				      BCMA_CC_PMU5_MAINPLL_SSB);
+		return bcma_pmu_pll_clock(cc, BCMA_CC_PMU5357_MAINPLL_PLL0,
+					  BCMA_CC_PMU5_MAINPLL_SSB);
 	case BCMA_CHIP_ID_BCM4706:
-		return bcma_pmu_clock_bcm4706(cc, BCMA_CC_PMU4706_MAINPLL_PLL0,
-					      BCMA_CC_PMU5_MAINPLL_SSB);
+		return bcma_pmu_pll_clock_bcm4706(cc,
+						  BCMA_CC_PMU4706_MAINPLL_PLL0,
+						  BCMA_CC_PMU5_MAINPLL_SSB);
 	case BCMA_CHIP_ID_BCM53572:
 		return 75000000;
 	default:
-		bcma_warn(bus, "No backplane clock specified for %04X device, pmu rev. %d, using default %d Hz\n",
+		bcma_warn(bus, "No bus clock specified for %04X device, pmu rev. %d, using default %d Hz\n",
 			  bus->chipinfo.id, cc->pmu.rev, BCMA_CC_PMU_HT_CLOCK);
 	}
 	return BCMA_CC_PMU_HT_CLOCK;
 }
+EXPORT_SYMBOL_GPL(bcma_pmu_get_bus_clock);
 
 /* query cpu clock frequency for PMU-enabled chipcommon */
-u32 bcma_pmu_get_clockcpu(struct bcma_drv_cc *cc)
+u32 bcma_pmu_get_cpu_clock(struct bcma_drv_cc *cc)
 {
 	struct bcma_bus *bus = cc->core->bus;
 
 	if (bus->chipinfo.id == BCMA_CHIP_ID_BCM53572)
 		return 300000000;
 
+	/* New PMUs can have different clock for bus and CPU */
 	if (cc->pmu.rev >= 5) {
 		u32 pll;
 		switch (bus->chipinfo.id) {
 		case BCMA_CHIP_ID_BCM4706:
-			return bcma_pmu_clock_bcm4706(cc,
+			return bcma_pmu_pll_clock_bcm4706(cc,
 						BCMA_CC_PMU4706_MAINPLL_PLL0,
 						BCMA_CC_PMU5_MAINPLL_CPU);
 		case BCMA_CHIP_ID_BCM5356:
@@ -313,10 +462,11 @@ u32 bcma_pmu_get_clockcpu(struct bcma_dr
 			break;
 		}
 
-		return bcma_pmu_clock(cc, pll, BCMA_CC_PMU5_MAINPLL_CPU);
+		return bcma_pmu_pll_clock(cc, pll, BCMA_CC_PMU5_MAINPLL_CPU);
 	}
 
-	return bcma_pmu_get_clockcontrol(cc);
+	/* On old PMUs CPU has the same clock as the bus */
+	return bcma_pmu_get_bus_clock(cc);
 }
 
 static void bcma_pmu_spuravoid_pll_write(struct bcma_drv_cc *cc, u32 offset,
@@ -362,7 +512,7 @@ void bcma_pmu_spuravoid_pllupdate(struct
 		tmp |= (bcm5357_bcm43236_ndiv[spuravoid]) << BCMA_CC_PMU1_PLL0_PC2_NDIV_INT_SHIFT;
 		bcma_cc_write32(cc, BCMA_CC_PLLCTL_DATA, tmp);
 
-		tmp = 1 << 10;
+		tmp = BCMA_CC_PMU_CTL_PLL_UPD;
 		break;
 
 	case BCMA_CHIP_ID_BCM4331:
@@ -383,7 +533,7 @@ void bcma_pmu_spuravoid_pllupdate(struct
 			bcma_pmu_spuravoid_pll_write(cc, BCMA_CC_PMU_PLL_CTL2,
 						     0x03000a08);
 		}
-		tmp = 1 << 10;
+		tmp = BCMA_CC_PMU_CTL_PLL_UPD;
 		break;
 
 	case BCMA_CHIP_ID_BCM43224:
@@ -416,7 +566,7 @@ void bcma_pmu_spuravoid_pllupdate(struct
 			bcma_pmu_spuravoid_pll_write(cc, BCMA_CC_PMU_PLL_CTL5,
 						     0x88888815);
 		}
-		tmp = 1 << 10;
+		tmp = BCMA_CC_PMU_CTL_PLL_UPD;
 		break;
 
 	case BCMA_CHIP_ID_BCM4716:
@@ -450,7 +600,7 @@ void bcma_pmu_spuravoid_pllupdate(struct
 						     0x88888815);
 		}
 
-		tmp = 3 << 9;
+		tmp = BCMA_CC_PMU_CTL_PLL_UPD | BCMA_CC_PMU_CTL_NOILPONW;
 		break;
 
 	case BCMA_CHIP_ID_BCM43227:
@@ -486,7 +636,7 @@ void bcma_pmu_spuravoid_pllupdate(struct
 			bcma_pmu_spuravoid_pll_write(cc, BCMA_CC_PMU_PLL_CTL5,
 						     0x88888815);
 		}
-		tmp = 1 << 10;
+		tmp = BCMA_CC_PMU_CTL_PLL_UPD;
 		break;
 	default:
 		bcma_err(bus, "Unknown spuravoidance settings for chip 0x%04X, not changing PLL\n",
--- a/drivers/bcma/driver_chipcommon_sflash.c
+++ b/drivers/bcma/driver_chipcommon_sflash.c
@@ -5,15 +5,161 @@
  * Licensed under the GNU/GPL. See COPYING for details.
  */
 
+#include "bcma_private.h"
+
+#include <linux/platform_device.h>
 #include <linux/bcma/bcma.h>
-#include <linux/bcma/bcma_driver_chipcommon.h>
-#include <linux/delay.h>
 
-#include "bcma_private.h"
+static struct resource bcma_sflash_resource = {
+	.name	= "bcma_sflash",
+	.start	= BCMA_SOC_FLASH2,
+	.end	= 0,
+	.flags  = IORESOURCE_MEM | IORESOURCE_READONLY,
+};
+
+struct platform_device bcma_sflash_dev = {
+	.name		= "bcma_sflash",
+	.resource	= &bcma_sflash_resource,
+	.num_resources	= 1,
+};
+
+struct bcma_sflash_tbl_e {
+	char *name;
+	u32 id;
+	u32 blocksize;
+	u16 numblocks;
+};
+
+static const struct bcma_sflash_tbl_e bcma_sflash_st_tbl[] = {
+	{ "M25P20", 0x11, 0x10000, 4, },
+	{ "M25P40", 0x12, 0x10000, 8, },
+
+	{ "M25P16", 0x14, 0x10000, 32, },
+	{ "M25P32", 0x15, 0x10000, 64, },
+	{ "M25P64", 0x16, 0x10000, 128, },
+	{ "M25FL128", 0x17, 0x10000, 256, },
+	{ 0 },
+};
+
+static const struct bcma_sflash_tbl_e bcma_sflash_sst_tbl[] = {
+	{ "SST25WF512", 1, 0x1000, 16, },
+	{ "SST25VF512", 0x48, 0x1000, 16, },
+	{ "SST25WF010", 2, 0x1000, 32, },
+	{ "SST25VF010", 0x49, 0x1000, 32, },
+	{ "SST25WF020", 3, 0x1000, 64, },
+	{ "SST25VF020", 0x43, 0x1000, 64, },
+	{ "SST25WF040", 4, 0x1000, 128, },
+	{ "SST25VF040", 0x44, 0x1000, 128, },
+	{ "SST25VF040B", 0x8d, 0x1000, 128, },
+	{ "SST25WF080", 5, 0x1000, 256, },
+	{ "SST25VF080B", 0x8e, 0x1000, 256, },
+	{ "SST25VF016", 0x41, 0x1000, 512, },
+	{ "SST25VF032", 0x4a, 0x1000, 1024, },
+	{ "SST25VF064", 0x4b, 0x1000, 2048, },
+	{ 0 },
+};
+
+static const struct bcma_sflash_tbl_e bcma_sflash_at_tbl[] = {
+	{ "AT45DB011", 0xc, 256, 512, },
+	{ "AT45DB021", 0x14, 256, 1024, },
+	{ "AT45DB041", 0x1c, 256, 2048, },
+	{ "AT45DB081", 0x24, 256, 4096, },
+	{ "AT45DB161", 0x2c, 512, 4096, },
+	{ "AT45DB321", 0x34, 512, 8192, },
+	{ "AT45DB642", 0x3c, 1024, 8192, },
+	{ 0 },
+};
+
+static void bcma_sflash_cmd(struct bcma_drv_cc *cc, u32 opcode)
+{
+	int i;
+	bcma_cc_write32(cc, BCMA_CC_FLASHCTL,
+			BCMA_CC_FLASHCTL_START | opcode);
+	for (i = 0; i < 1000; i++) {
+		if (!(bcma_cc_read32(cc, BCMA_CC_FLASHCTL) &
+		      BCMA_CC_FLASHCTL_BUSY))
+			return;
+		cpu_relax();
+	}
+	bcma_err(cc->core->bus, "SFLASH control command failed (timeout)!\n");
+}
 
 /* Initialize serial flash access */
 int bcma_sflash_init(struct bcma_drv_cc *cc)
 {
-	bcma_err(cc->core->bus, "Serial flash support is broken\n");
+	struct bcma_bus *bus = cc->core->bus;
+	struct bcma_sflash *sflash = &cc->sflash;
+	const struct bcma_sflash_tbl_e *e;
+	u32 id, id2;
+
+	switch (cc->capabilities & BCMA_CC_CAP_FLASHT) {
+	case BCMA_CC_FLASHT_STSER:
+		bcma_sflash_cmd(cc, BCMA_CC_FLASHCTL_ST_DP);
+
+		bcma_cc_write32(cc, BCMA_CC_FLASHADDR, 0);
+		bcma_sflash_cmd(cc, BCMA_CC_FLASHCTL_ST_RES);
+		id = bcma_cc_read32(cc, BCMA_CC_FLASHDATA);
+
+		bcma_cc_write32(cc, BCMA_CC_FLASHADDR, 1);
+		bcma_sflash_cmd(cc, BCMA_CC_FLASHCTL_ST_RES);
+		id2 = bcma_cc_read32(cc, BCMA_CC_FLASHDATA);
+
+		switch (id) {
+		case 0xbf:
+			for (e = bcma_sflash_sst_tbl; e->name; e++) {
+				if (e->id == id2)
+					break;
+			}
+			break;
+		case 0x13:
+			return -ENOTSUPP;
+		default:
+			for (e = bcma_sflash_st_tbl; e->name; e++) {
+				if (e->id == id)
+					break;
+			}
+			break;
+		}
+		if (!e->name) {
+			bcma_err(bus, "Unsupported ST serial flash (id: 0x%X, id2: 0x%X)\n", id, id2);
+			return -ENOTSUPP;
+		}
+
+		break;
+	case BCMA_CC_FLASHT_ATSER:
+		bcma_sflash_cmd(cc, BCMA_CC_FLASHCTL_AT_STATUS);
+		id = bcma_cc_read32(cc, BCMA_CC_FLASHDATA) & 0x3c;
+
+		for (e = bcma_sflash_at_tbl; e->name; e++) {
+			if (e->id == id)
+				break;
+		}
+		if (!e->name) {
+			bcma_err(bus, "Unsupported Atmel serial flash (id: 0x%X)\n", id);
+			return -ENOTSUPP;
+		}
+
+		break;
+	default:
+		bcma_err(bus, "Unsupported flash type\n");
+		return -ENOTSUPP;
+	}
+
+	sflash->window = BCMA_SOC_FLASH2;
+	sflash->blocksize = e->blocksize;
+	sflash->numblocks = e->numblocks;
+	sflash->size = sflash->blocksize * sflash->numblocks;
+	sflash->present = true;
+
+	bcma_info(bus, "Found %s serial flash (size: %dKiB, blocksize: 0x%X, blocks: %d)\n",
+		  e->name, sflash->size / 1024, sflash->blocksize,
+		  sflash->numblocks);
+
+	/* Prepare platform device, but don't register it yet. It's too early,
+	 * malloc (required by device_private_init) is not available yet. */
+	bcma_sflash_dev.resource[0].end = bcma_sflash_dev.resource[0].start +
+					  sflash->size;
+	bcma_sflash_dev.dev.platform_data = sflash;
+
 	return 0;
 }
--- /dev/null
+++ b/drivers/bcma/driver_gpio.c
@@ -0,0 +1,114 @@
+/*
+ * Broadcom specific AMBA
+ * GPIO driver
+ *
+ * Copyright 2011, Broadcom Corporation
+ * Copyright 2012, Hauke Mehrtens <hauke@hauke-m.de>
+ *
+ * Licensed under the GNU/GPL. See COPYING for details.
+ */
+
+#include <linux/gpio.h>
+#include <linux/export.h>
+#include <linux/bcma/bcma.h>
+
+#include "bcma_private.h"
+
+static inline struct bcma_drv_cc *bcma_gpio_get_cc(struct gpio_chip *chip)
+{
+	return container_of(chip, struct bcma_drv_cc, gpio);
+}
+
+static int bcma_gpio_get_value(struct gpio_chip *chip, unsigned gpio)
+{
+	struct bcma_drv_cc *cc = bcma_gpio_get_cc(chip);
+
+	return !!bcma_chipco_gpio_in(cc, 1 << gpio);
+}
+
+static void bcma_gpio_set_value(struct gpio_chip *chip, unsigned gpio,
+				int value)
+{
+	struct bcma_drv_cc *cc = bcma_gpio_get_cc(chip);
+
+	bcma_chipco_gpio_out(cc, 1 << gpio, value ? 1 << gpio : 0);
+}
+
+static int bcma_gpio_direction_input(struct gpio_chip *chip, unsigned gpio)
+{
+	struct bcma_drv_cc *cc = bcma_gpio_get_cc(chip);
+
+	bcma_chipco_gpio_outen(cc, 1 << gpio, 0);
+	return 0;
+}
+
+static int bcma_gpio_direction_output(struct gpio_chip *chip, unsigned gpio,
+				      int value)
+{
+	struct bcma_drv_cc *cc = bcma_gpio_get_cc(chip);
+
+	bcma_chipco_gpio_outen(cc, 1 << gpio, 1 << gpio);
+	bcma_chipco_gpio_out(cc, 1 << gpio, value ? 1 << gpio : 0);
+	return 0;
+}
+
+static int bcma_gpio_request(struct gpio_chip *chip, unsigned gpio)
+{
+	struct bcma_drv_cc *cc = bcma_gpio_get_cc(chip);
+
+	bcma_chipco_gpio_control(cc, 1 << gpio, 0);
+	/* clear pulldown */
+	bcma_chipco_gpio_pulldown(cc, 1 << gpio, 0);
+	/* Set pullup */
+	bcma_chipco_gpio_pullup(cc, 1 << gpio, 1 << gpio);
+
+	return 0;
+}
+
+static void bcma_gpio_free(struct gpio_chip *chip, unsigned gpio)
+{
+	struct bcma_drv_cc *cc = bcma_gpio_get_cc(chip);
+
+	/* clear pullup */
+	bcma_chipco_gpio_pullup(cc, 1 << gpio, 0);
+}
+
+static int bcma_gpio_to_irq(struct gpio_chip *chip, unsigned gpio)
+{
+	struct bcma_drv_cc *cc = bcma_gpio_get_cc(chip);
+
+	if (cc->core->bus->hosttype == BCMA_HOSTTYPE_SOC)
+		return bcma_core_irq(cc->core);
+	else
+		return -EINVAL;
+}
+
+int bcma_gpio_init(struct bcma_drv_cc *cc)
+{
+	struct gpio_chip *chip = &cc->gpio;
+
+	chip->label		= "bcma_gpio";
+	chip->owner		= THIS_MODULE;
+	chip->request		= bcma_gpio_request;
+	chip->free		= bcma_gpio_free;
+	chip->get		= bcma_gpio_get_value;
+	chip->set		= bcma_gpio_set_value;
+	chip->direction_input	= bcma_gpio_direction_input;
+	chip->direction_output	= bcma_gpio_direction_output;
+	chip->to_irq		= bcma_gpio_to_irq;
+	chip->ngpio		= 16;
+	/* There is just one SoC in one device and its GPIO addresses should be
+	 * deterministic to address them more easily. The other buses could get
+	 * a random base number. */
+	if (cc->core->bus->hosttype == BCMA_HOSTTYPE_SOC)
+		chip->base		= 0;
+	else
+		chip->base		= -1;
+
+	return gpiochip_add(chip);
+}
+
+int bcma_gpio_unregister(struct bcma_drv_cc *cc)
+{
+	return gpiochip_remove(&cc->gpio);
+}
--- a/drivers/bcma/driver_mips.c
+++ b/drivers/bcma/driver_mips.c
@@ -14,11 +14,33 @@
 
 #include <linux/bcma/bcma.h>
 
+#include <linux/mtd/physmap.h>
+#include <linux/platform_device.h>
 #include <linux/serial.h>
 #include <linux/serial_core.h>
 #include <linux/serial_reg.h>
 #include <linux/time.h>
 
+static const char * const part_probes[] = { "bcm47xxpart", NULL };
+
+static struct physmap_flash_data bcma_pflash_data = {
+	.part_probe_types	= part_probes,
+};
+
+static struct resource bcma_pflash_resource = {
+	.name	= "bcma_pflash",
+	.flags  = IORESOURCE_MEM,
+};
+
+struct platform_device bcma_pflash_dev = {
+	.name		= "physmap-flash",
+	.dev		= {
+		.platform_data  = &bcma_pflash_data,
+	},
+	.resource	= &bcma_pflash_resource,
+	.num_resources	= 1,
+};
+
 /* The 47162a0 hangs when reading MIPS DMP registers registers */
 static inline bool bcma_core_mips_bcm47162a0_quirk(struct bcma_device *dev)
 {
@@ -74,28 +96,41 @@ static u32 bcma_core_mips_irqflag(struct
 		return dev->core_index;
 	flag = bcma_aread32(dev, BCMA_MIPS_OOBSELOUTA30);
 
-	return flag & 0x1F;
+	if (flag)
+		return flag & 0x1F;
+	else
+		return 0x3f;
 }
 
 /* Get the MIPS IRQ assignment for a specified device.
  * If unassigned, 0 is returned.
+ * If disabled, 5 is returned.
+ * If not supported, 6 is returned.
  */
-unsigned int bcma_core_mips_irq(struct bcma_device *dev)
+static unsigned int bcma_core_mips_irq(struct bcma_device *dev)
 {
 	struct bcma_device *mdev = dev->bus->drv_mips.core;
 	u32 irqflag;
 	unsigned int irq;
 
 	irqflag = bcma_core_mips_irqflag(dev);
+	if (irqflag == 0x3f)
+		return 6;
 
-	for (irq = 1; irq <= 4; irq++)
+	for (irq = 0; irq <= 4; irq++)
 		if (bcma_read32(mdev, BCMA_MIPS_MIPS74K_INTMASK(irq)) &
 		    (1 << irqflag))
 			return irq;
 
-	return 0;
+	return 5;
+}
+
+unsigned int bcma_core_irq(struct bcma_device *dev)
+{
+	unsigned int mips_irq = bcma_core_mips_irq(dev);
+	return mips_irq <= 4 ? mips_irq + 2 : 0;
 }
-EXPORT_SYMBOL(bcma_core_mips_irq);
+EXPORT_SYMBOL(bcma_core_irq);
 
 static void bcma_core_mips_set_irq(struct bcma_device *dev, unsigned int irq)
 {
@@ -114,8 +149,8 @@ static void bcma_core_mips_set_irq(struc
 		bcma_write32(mdev, BCMA_MIPS_MIPS74K_INTMASK(0),
 			    bcma_read32(mdev, BCMA_MIPS_MIPS74K_INTMASK(0)) &
 			    ~(1 << irqflag));
-	else
-		bcma_write32(mdev, BCMA_MIPS_MIPS74K_INTMASK(irq), 0);
+	else if (oldirq != 5)
+		bcma_write32(mdev, BCMA_MIPS_MIPS74K_INTMASK(oldirq), 0);
 
 	/* assign the new one */
 	if (irq == 0) {
@@ -123,9 +158,9 @@ static void bcma_core_mips_set_irq(struc
 			    bcma_read32(mdev, BCMA_MIPS_MIPS74K_INTMASK(0)) |
 			    (1 << irqflag));
 	} else {
-		u32 oldirqflag = bcma_read32(mdev,
-					     BCMA_MIPS_MIPS74K_INTMASK(irq));
-		if (oldirqflag) {
+		u32 irqinitmask = bcma_read32(mdev,
+					      BCMA_MIPS_MIPS74K_INTMASK(irq));
+		if (irqinitmask) {
 			struct bcma_device *core;
 
 			/* backplane irq line is in use, find out who uses
@@ -133,7 +168,7 @@ static void bcma_core_mips_set_irq(struc
 			 */
 			list_for_each_entry(core, &bus->cores, list) {
 				if ((1 << bcma_core_mips_irqflag(core)) ==
-				    oldirqflag) {
+				    irqinitmask) {
 					bcma_core_mips_set_irq(core, 0);
 					break;
 				}
@@ -143,15 +178,31 @@ static void bcma_core_mips_set_irq(struc
 			     1 << irqflag);
 	}
 
-	bcma_info(bus, "set_irq: core 0x%04x, irq %d => %d\n",
-		  dev->id.id, oldirq + 2, irq + 2);
+	bcma_debug(bus, "set_irq: core 0x%04x, irq %d => %d\n",
+		   dev->id.id, oldirq <= 4 ? oldirq + 2 : 0, irq + 2);
+}
+
+static void bcma_core_mips_set_irq_name(struct bcma_bus *bus, unsigned int irq,
+					u16 coreid, u8 unit)
+{
+	struct bcma_device *core;
+
+	core = bcma_find_core_unit(bus, coreid, unit);
+	if (!core) {
+		bcma_warn(bus,
+			  "Can not find core (id: 0x%x, unit %i) for IRQ configuration.\n",
+			  coreid, unit);
+		return;
+	}
+
+	bcma_core_mips_set_irq(core, irq);
 }
 
 static void bcma_core_mips_print_irq(struct bcma_device *dev, unsigned int irq)
 {
 	int i;
 	static const char *irq_name[] = {"2(S)", "3", "4", "5", "6", "D", "I"};
-	printk(KERN_INFO KBUILD_MODNAME ": core 0x%04x, irq :", dev->id.id);
+	printk(KERN_DEBUG KBUILD_MODNAME ": core 0x%04x, irq :", dev->id.id);
 	for (i = 0; i <= 6; i++)
 		printk(" %s%s", irq_name[i], i == irq ? "*" : " ");
 	printk("\n");
@@ -171,7 +222,7 @@ u32 bcma_cpu_clock(struct bcma_drv_mips
 	struct bcma_bus *bus = mcore->core->bus;
 
 	if (bus->drv_cc.capabilities & BCMA_CC_CAP_PMU)
-		return bcma_pmu_get_clockcpu(&bus->drv_cc);
+		return bcma_pmu_get_cpu_clock(&bus->drv_cc);
 
 	bcma_err(bus, "No PMU available, need this to get the cpu clock\n");
 	return 0;
@@ -181,85 +232,143 @@ EXPORT_SYMBOL(bcma_cpu_clock);
 static void bcma_core_mips_flash_detect(struct bcma_drv_mips *mcore)
 {
 	struct bcma_bus *bus = mcore->core->bus;
+	struct bcma_drv_cc *cc = &bus->drv_cc;
+	struct bcma_pflash *pflash = &cc->pflash;
 
-	switch (bus->drv_cc.capabilities & BCMA_CC_CAP_FLASHT) {
+	switch (cc->capabilities & BCMA_CC_CAP_FLASHT) {
 	case BCMA_CC_FLASHT_STSER:
 	case BCMA_CC_FLASHT_ATSER:
 		bcma_debug(bus, "Found serial flash\n");
-		bcma_sflash_init(&bus->drv_cc);
+		bcma_sflash_init(cc);
 		break;
 	case BCMA_CC_FLASHT_PARA:
 		bcma_debug(bus, "Found parallel flash\n");
-		bus->drv_cc.pflash.window = 0x1c000000;
-		bus->drv_cc.pflash.window_size = 0x02000000;
+		pflash->present = true;
+		pflash->window = BCMA_SOC_FLASH2;
+		pflash->window_size = BCMA_SOC_FLASH2_SZ;
 
-		if ((bcma_read32(bus->drv_cc.core, BCMA_CC_FLASH_CFG) &
+		if ((bcma_read32(cc->core, BCMA_CC_FLASH_CFG) &
 		     BCMA_CC_FLASH_CFG_DS) == 0)
-			bus->drv_cc.pflash.buswidth = 1;
+			pflash->buswidth = 1;
 		else
-			bus->drv_cc.pflash.buswidth = 2;
+			pflash->buswidth = 2;
+
+		bcma_pflash_data.width = pflash->buswidth;
+		bcma_pflash_resource.start = pflash->window;
+		bcma_pflash_resource.end = pflash->window + pflash->window_size;
+
 		break;
 	default:
 		bcma_err(bus, "Flash type not supported\n");
 	}
 
-	if (bus->drv_cc.core->id.rev == 38 ||
+	if (cc->core->id.rev == 38 ||
 	    bus->chipinfo.id == BCMA_CHIP_ID_BCM4706) {
-		if (bus->drv_cc.capabilities & BCMA_CC_CAP_NFLASH) {
+		if (cc->capabilities & BCMA_CC_CAP_NFLASH) {
 			bcma_debug(bus, "Found NAND flash\n");
-			bcma_nflash_init(&bus->drv_cc);
+			bcma_nflash_init(cc);
 		}
 	}
 }
 
+void bcma_core_mips_early_init(struct bcma_drv_mips *mcore)
+{
+	struct bcma_bus *bus = mcore->core->bus;
+
+	if (mcore->early_setup_done)
+		return;
+
+	bcma_chipco_serial_init(&bus->drv_cc);
+	bcma_core_mips_flash_detect(mcore);
+
+	mcore->early_setup_done = true;
+}
+
+static void bcma_fix_i2s_irqflag(struct bcma_bus *bus)
+{
+	struct bcma_device *cpu, *pcie, *i2s;
+
+	/* Fixup the interrupts in 4716/4748 for i2s core (2010 Broadcom SDK)
+	 * (IRQ flags > 7 are ignored when setting the interrupt masks)
+	 */
+	if (bus->chipinfo.id != BCMA_CHIP_ID_BCM4716 &&
+	    bus->chipinfo.id != BCMA_CHIP_ID_BCM4748)
+		return;
+
+	cpu = bcma_find_core(bus, BCMA_CORE_MIPS_74K);
+	pcie = bcma_find_core(bus, BCMA_CORE_PCIE);
+	i2s = bcma_find_core(bus, BCMA_CORE_I2S);
+	if (cpu && pcie && i2s &&
+	    bcma_aread32(cpu, BCMA_MIPS_OOBSELINA74) == 0x08060504 &&
+	    bcma_aread32(pcie, BCMA_MIPS_OOBSELINA74) == 0x08060504 &&
+	    bcma_aread32(i2s, BCMA_MIPS_OOBSELOUTA30) == 0x88) {
+		bcma_awrite32(cpu, BCMA_MIPS_OOBSELINA74, 0x07060504);
+		bcma_awrite32(pcie, BCMA_MIPS_OOBSELINA74, 0x07060504);
+		bcma_awrite32(i2s, BCMA_MIPS_OOBSELOUTA30, 0x87);
+		bcma_debug(bus,
+			   "Moved i2s interrupt to oob line 7 instead of 8\n");
+	}
+}
+
 void bcma_core_mips_init(struct bcma_drv_mips *mcore)
 {
 	struct bcma_bus *bus;
 	struct bcma_device *core;
 	bus = mcore->core->bus;
 
-	bcma_info(bus, "Initializing MIPS core...\n");
+	if (mcore->setup_done)
+		return;
 
-	if (!mcore->setup_done)
-		mcore->assigned_irqs = 1;
+	bcma_debug(bus, "Initializing MIPS core...\n");
 
-	/* Assign IRQs to all cores on the bus */
-	list_for_each_entry(core, &bus->cores, list) {
-		int mips_irq;
-		if (core->irq)
-			continue;
-
-		mips_irq = bcma_core_mips_irq(core);
-		if (mips_irq > 4)
-			core->irq = 0;
-		else
-			core->irq = mips_irq + 2;
-		if (core->irq > 5)
-			continue;
-		switch (core->id.id) {
-		case BCMA_CORE_PCI:
-		case BCMA_CORE_PCIE:
-		case BCMA_CORE_ETHERNET:
-		case BCMA_CORE_ETHERNET_GBIT:
-		case BCMA_CORE_MAC_GBIT:
-		case BCMA_CORE_80211:
-		case BCMA_CORE_USB20_HOST:
-			/* These devices get their own IRQ line if available,
-			 * the rest goes on IRQ0
-			 */
-			if (mcore->assigned_irqs <= 4)
-				bcma_core_mips_set_irq(core,
-						       mcore->assigned_irqs++);
-			break;
+	bcma_core_mips_early_init(mcore);
+
+	bcma_fix_i2s_irqflag(bus);
+
+	switch (bus->chipinfo.id) {
+	case BCMA_CHIP_ID_BCM4716:
+	case BCMA_CHIP_ID_BCM4748:
+		bcma_core_mips_set_irq_name(bus, 1, BCMA_CORE_80211, 0);
+		bcma_core_mips_set_irq_name(bus, 2, BCMA_CORE_MAC_GBIT, 0);
+		bcma_core_mips_set_irq_name(bus, 3, BCMA_CORE_USB20_HOST, 0);
+		bcma_core_mips_set_irq_name(bus, 4, BCMA_CORE_PCIE, 0);
+		bcma_core_mips_set_irq_name(bus, 0, BCMA_CORE_CHIPCOMMON, 0);
+		bcma_core_mips_set_irq_name(bus, 0, BCMA_CORE_I2S, 0);
+		break;
+	case BCMA_CHIP_ID_BCM5356:
+	case BCMA_CHIP_ID_BCM47162:
+	case BCMA_CHIP_ID_BCM53572:
+		bcma_core_mips_set_irq_name(bus, 1, BCMA_CORE_80211, 0);
+		bcma_core_mips_set_irq_name(bus, 2, BCMA_CORE_MAC_GBIT, 0);
+		bcma_core_mips_set_irq_name(bus, 0, BCMA_CORE_CHIPCOMMON, 0);
+		break;
+	case BCMA_CHIP_ID_BCM5357:
+	case BCMA_CHIP_ID_BCM4749:
+		bcma_core_mips_set_irq_name(bus, 1, BCMA_CORE_80211, 0);
+		bcma_core_mips_set_irq_name(bus, 2, BCMA_CORE_MAC_GBIT, 0);
+		bcma_core_mips_set_irq_name(bus, 3, BCMA_CORE_USB20_HOST, 0);
+		bcma_core_mips_set_irq_name(bus, 0, BCMA_CORE_CHIPCOMMON, 0);
+		bcma_core_mips_set_irq_name(bus, 0, BCMA_CORE_I2S, 0);
+		break;
+	case BCMA_CHIP_ID_BCM4706:
+		bcma_core_mips_set_irq_name(bus, 1, BCMA_CORE_PCIE, 0);
+		bcma_core_mips_set_irq_name(bus, 2, BCMA_CORE_4706_MAC_GBIT,
+					    0);
+		bcma_core_mips_set_irq_name(bus, 3, BCMA_CORE_PCIE, 1);
+		bcma_core_mips_set_irq_name(bus, 4, BCMA_CORE_USB20_HOST, 0);
+		bcma_core_mips_set_irq_name(bus, 0, BCMA_CORE_4706_CHIPCOMMON,
+					    0);
+		break;
+	default:
+		list_for_each_entry(core, &bus->cores, list) {
+			core->irq = bcma_core_irq(core);
 		}
+		bcma_err(bus,
+			 "Unknown device (0x%x) found, can not configure IRQs\n",
+			 bus->chipinfo.id);
 	}
-	bcma_info(bus, "IRQ reconfiguration done\n");
+	bcma_debug(bus, "IRQ reconfiguration done\n");
 	bcma_core_mips_dump_irq(bus);
 
-	if (mcore->setup_done)
-		return;
-
-	bcma_chipco_serial_init(&bus->drv_cc);
-	bcma_core_mips_flash_detect(mcore);
 	mcore->setup_done = true;
 }
--- a/drivers/bcma/driver_pci.c
+++ b/drivers/bcma/driver_pci.c
@@ -31,7 +31,7 @@ static void bcma_pcie_write(struct bcma_
 	pcicore_write32(pc, BCMA_CORE_PCI_PCIEIND_DATA, data);
 }
 
-static void bcma_pcie_mdio_set_phy(struct bcma_drv_pci *pc, u8 phy)
+static void bcma_pcie_mdio_set_phy(struct bcma_drv_pci *pc, u16 phy)
 {
 	u32 v;
 	int i;
@@ -51,11 +51,11 @@ static void bcma_pcie_mdio_set_phy(struc
 		v = pcicore_read32(pc, BCMA_CORE_PCI_MDIO_CONTROL);
 		if (v & BCMA_CORE_PCI_MDIOCTL_ACCESS_DONE)
 			break;
-		msleep(1);
+		usleep_range(1000, 2000);
 	}
 }
 
-static u16 bcma_pcie_mdio_read(struct bcma_drv_pci *pc, u8 device, u8 address)
+static u16 bcma_pcie_mdio_read(struct bcma_drv_pci *pc, u16 device, u8 address)
 {
 	int max_retries = 10;
 	u16 ret = 0;
@@ -92,13 +92,13 @@ static u16 bcma_pcie_mdio_read(struct bc
 			ret = pcicore_read32(pc, BCMA_CORE_PCI_MDIO_DATA);
 			break;
 		}
-		msleep(1);
+		usleep_range(1000, 2000);
 	}
 	pcicore_write32(pc, BCMA_CORE_PCI_MDIO_CONTROL, 0);
 	return ret;
 }
 
-static void bcma_pcie_mdio_write(struct bcma_drv_pci *pc, u8 device,
+static void bcma_pcie_mdio_write(struct bcma_drv_pci *pc, u16 device,
 				u8 address, u16 data)
 {
 	int max_retries = 10;
@@ -132,11 +132,18 @@ static void bcma_pcie_mdio_write(struct
 		v = pcicore_read32(pc, BCMA_CORE_PCI_MDIO_CONTROL);
 		if (v & BCMA_CORE_PCI_MDIOCTL_ACCESS_DONE)
 			break;
-		msleep(1);
+		usleep_range(1000, 2000);
 	}
 	pcicore_write32(pc, BCMA_CORE_PCI_MDIO_CONTROL, 0);
 }
 
+static u16 bcma_pcie_mdio_writeread(struct bcma_drv_pci *pc, u16 device,
+				    u8 address, u16 data)
+{
+	bcma_pcie_mdio_write(pc, device, address, data);
+	return bcma_pcie_mdio_read(pc, device, address);
+}
+
 /**************************************************
  * Workarounds.
  **************************************************/
@@ -229,6 +236,32 @@ void __devinit bcma_core_pci_init(struct
 		bcma_core_pci_clientmode_init(pc);
 }
 
+void bcma_core_pci_power_save(struct bcma_bus *bus, bool up)
+{
+	struct bcma_drv_pci *pc;
+	u16 data;
+
+	if (bus->hosttype != BCMA_HOSTTYPE_PCI)
+		return;
+
+	pc = &bus->drv_pci[0];
+
+	if (pc->core->id.rev >= 15 && pc->core->id.rev <= 20) {
+		data = up ? 0x74 : 0x7C;
+		bcma_pcie_mdio_writeread(pc, BCMA_CORE_PCI_MDIO_BLK1,
+					 BCMA_CORE_PCI_MDIO_BLK1_MGMT1, 0x7F64);
+		bcma_pcie_mdio_writeread(pc, BCMA_CORE_PCI_MDIO_BLK1,
+					 BCMA_CORE_PCI_MDIO_BLK1_MGMT3, data);
+	} else if (pc->core->id.rev >= 21 && pc->core->id.rev <= 22) {
+		data = up ? 0x75 : 0x7D;
+		bcma_pcie_mdio_writeread(pc, BCMA_CORE_PCI_MDIO_BLK1,
+					 BCMA_CORE_PCI_MDIO_BLK1_MGMT1, 0x7E65);
+		bcma_pcie_mdio_writeread(pc, BCMA_CORE_PCI_MDIO_BLK1,
+					 BCMA_CORE_PCI_MDIO_BLK1_MGMT3, data);
+	}
+}
+EXPORT_SYMBOL_GPL(bcma_core_pci_power_save);
+
 int bcma_core_pci_irq_ctl(struct bcma_drv_pci *pc, struct bcma_device *core,
 			  bool enable)
 {
@@ -262,7 +295,7 @@ out:
 }
 EXPORT_SYMBOL_GPL(bcma_core_pci_irq_ctl);
 
-void bcma_core_pci_extend_L1timer(struct bcma_drv_pci *pc, bool extend)
+static void bcma_core_pci_extend_L1timer(struct bcma_drv_pci *pc, bool extend)
 {
 	u32 w;
 
@@ -274,4 +307,29 @@ void bcma_core_pci_extend_L1timer(struct
 	bcma_pcie_write(pc, BCMA_CORE_PCI_DLLP_PMTHRESHREG, w);
 	bcma_pcie_read(pc, BCMA_CORE_PCI_DLLP_PMTHRESHREG);
 }
-EXPORT_SYMBOL_GPL(bcma_core_pci_extend_L1timer);
+
+void bcma_core_pci_up(struct bcma_bus *bus)
+{
+	struct bcma_drv_pci *pc;
+
+	if (bus->hosttype != BCMA_HOSTTYPE_PCI)
+		return;
+
+	pc = &bus->drv_pci[0];
+
+	bcma_core_pci_extend_L1timer(pc, true);
+}
+EXPORT_SYMBOL_GPL(bcma_core_pci_up);
+
+void bcma_core_pci_down(struct bcma_bus *bus)
+{
+	struct bcma_drv_pci *pc;
+
+	if (bus->hosttype != BCMA_HOSTTYPE_PCI)
+		return;
+
+	pc = &bus->drv_pci[0];
+
+	bcma_core_pci_extend_L1timer(pc, false);
+}
+EXPORT_SYMBOL_GPL(bcma_core_pci_down);
--- a/drivers/bcma/driver_pci_host.c
+++ b/drivers/bcma/driver_pci_host.c
@@ -35,11 +35,6 @@ bool __devinit bcma_core_pci_is_in_hostm
 	    chipid_top != 0x5300)
 		return false;
 
-	if (bus->sprom.boardflags_lo & BCMA_CORE_PCI_BFL_NOPCI) {
-		bcma_info(bus, "This PCI core is disabled and not working\n");
-		return false;
-	}
-
 	bcma_core_enable(pc->core, 0);
 
 	return !mips_busprobe32(tmp, pc->core->io_addr);
@@ -99,19 +94,19 @@ static int bcma_extpci_read_config(struc
 	if (dev == 0) {
 		/* we support only two functions on device 0 */
 		if (func > 1)
-			return -EINVAL;
+			goto out;
 
 		/* accesses to config registers with offsets >= 256
 		 * requires indirect access.
 		 */
 		if (off >= PCI_CONFIG_SPACE_SIZE) {
 			addr = (func << 12);
-			addr |= (off & 0x0FFF);
+			addr |= (off & 0x0FFC);
 			val = bcma_pcie_read_config(pc, addr);
 		} else {
 			addr = BCMA_CORE_PCI_PCICFG0;
 			addr |= (func << 8);
-			addr |= (off & 0xfc);
+			addr |= (off & 0xFC);
 			val = pcicore_read32(pc, addr);
 		}
 	} else {
@@ -124,11 +119,9 @@ static int bcma_extpci_read_config(struc
 			goto out;
 
 		if (mips_busprobe32(val, mmio)) {
-			val = 0xffffffff;
+			val = 0xFFFFFFFF;
 			goto unmap;
 		}
-
-		val = readl(mmio);
 	}
 	val >>= (8 * (off & 3));
 
@@ -156,7 +149,7 @@ static int bcma_extpci_write_config(stru
 				   const void *buf, int len)
 {
 	int err = -EINVAL;
-	u32 addr = 0, val = 0;
+	u32 addr, val;
 	void __iomem *mmio = 0;
 	u16 chipid = pc->core->bus->chipinfo.id;
 
@@ -164,16 +157,22 @@ static int bcma_extpci_write_config(stru
 	if (unlikely(len != 1 && len != 2 && len != 4))
 		goto out;
 	if (dev == 0) {
+		/* we support only two functions on device 0 */
+		if (func > 1)
+			goto out;
+
 		/* accesses to config registers with offsets >= 256
 		 * requires indirect access.
 		 */
-		if (off < PCI_CONFIG_SPACE_SIZE) {
-			addr = pc->core->addr + BCMA_CORE_PCI_PCICFG0;
+		if (off >= PCI_CONFIG_SPACE_SIZE) {
+			addr = (func << 12);
+			addr |= (off & 0x0FFC);
+			val = bcma_pcie_read_config(pc, addr);
+		} else {
+			addr = BCMA_CORE_PCI_PCICFG0;
 			addr |= (func << 8);
-			addr |= (off & 0xfc);
-			mmio = ioremap_nocache(addr, sizeof(val));
-			if (!mmio)
-				goto out;
+			addr |= (off & 0xFC);
+			val = pcicore_read32(pc, addr);
 		}
 	} else {
 		addr = bcma_get_cfgspace_addr(pc, dev, func, off);
@@ -185,19 +184,17 @@ static int bcma_extpci_write_config(stru
 			goto out;
 
 		if (mips_busprobe32(val, mmio)) {
-			val = 0xffffffff;
+			val = 0xFFFFFFFF;
 			goto unmap;
 		}
 	}
 
 	switch (len) {
 	case 1:
-		val = readl(mmio);
 		val &= ~(0xFF << (8 * (off & 3)));
 		val |= *((const u8 *)buf) << (8 * (off & 3));
 		break;
 	case 2:
-		val = readl(mmio);
 		val &= ~(0xFFFF << (8 * (off & 3)));
 		val |= *((const u16 *)buf) << (8 * (off & 3));
 		break;
@@ -205,13 +202,14 @@ static int bcma_extpci_write_config(stru
 		val = *((const u32 *)buf);
 		break;
 	}
-	if (dev == 0 && !addr) {
+	if (dev == 0) {
 		/* accesses to config registers with offsets >= 256
 		 * requires indirect access.
 		 */
-		addr = (func << 12);
-		addr |= (off & 0x0FFF);
-		bcma_pcie_write_config(pc, addr, val);
+		if (off >= PCI_CONFIG_SPACE_SIZE)
+			bcma_pcie_write_config(pc, addr, val);
+		else
+			pcicore_write32(pc, addr, val);
 	} else {
 		writel(val, mmio);
 
@@ -282,7 +280,7 @@ static u8 __devinit bcma_find_pci_capabi
 	/* check for Header type 0 */
 	bcma_extpci_read_config(pc, dev, func, PCI_HEADER_TYPE, &byte_val,
 				sizeof(u8));
-	if ((byte_val & 0x7f) != PCI_HEADER_TYPE_NORMAL)
+	if ((byte_val & 0x7F) != PCI_HEADER_TYPE_NORMAL)
 		return cap_ptr;
 
 	/* check if the capability pointer field exists */
@@ -396,12 +394,19 @@ void __devinit bcma_core_pci_hostmode_in
 
 	bcma_info(bus, "PCIEcore in host mode found\n");
 
+	if (bus->sprom.boardflags_lo & BCMA_CORE_PCI_BFL_NOPCI) {
+		bcma_info(bus, "This PCIE core is disabled and not working\n");
+		return;
+	}
+
 	pc_host = kzalloc(sizeof(*pc_host), GFP_KERNEL);
 	if (!pc_host)  {
 		bcma_err(bus, "can not allocate memory");
 		return;
 	}
 
+	spin_lock_init(&pc_host->cfgspace_lock);
+
 	pc->host_controller = pc_host;
 	pc_host->pci_controller.io_resource = &pc_host->io_resource;
 	pc_host->pci_controller.mem_resource = &pc_host->mem_resource;
@@ -425,9 +430,9 @@ void __devinit bcma_core_pci_hostmode_in
 	pc_host->io_resource.flags = IORESOURCE_IO | IORESOURCE_PCI_FIXED;
 
 	/* Reset RC */
-	udelay(3000);
+	usleep_range(3000, 5000);
 	pcicore_write32(pc, BCMA_CORE_PCI_CTL, BCMA_CORE_PCI_CTL_RST_OE);
-	udelay(1000);
+	msleep(50);
 	pcicore_write32(pc, BCMA_CORE_PCI_CTL, BCMA_CORE_PCI_CTL_RST |
 			BCMA_CORE_PCI_CTL_RST_OE);
 
@@ -452,6 +457,8 @@ void __devinit bcma_core_pci_hostmode_in
 			pc_host->mem_resource.start = BCMA_SOC_PCI_MEM;
 			pc_host->mem_resource.end = BCMA_SOC_PCI_MEM +
 						    BCMA_SOC_PCI_MEM_SZ - 1;
+			pc_host->io_resource.start = 0x100;
+			pc_host->io_resource.end = 0x47F;
 			pci_membase_1G = BCMA_SOC_PCIE_DMA_H32;
 			pcicore_write32(pc, BCMA_CORE_PCI_SBTOPCI0,
 					tmp | BCMA_SOC_PCI_MEM);
@@ -459,6 +466,8 @@ void __devinit bcma_core_pci_hostmode_in
 			pc_host->mem_resource.start = BCMA_SOC_PCI1_MEM;
 			pc_host->mem_resource.end = BCMA_SOC_PCI1_MEM +
 						    BCMA_SOC_PCI_MEM_SZ - 1;
+			pc_host->io_resource.start = 0x480;
+			pc_host->io_resource.end = 0x7FF;
 			pci_membase_1G = BCMA_SOC_PCIE1_DMA_H32;
 			pc_host->host_cfg_addr = BCMA_SOC_PCI1_CFG;
 			pcicore_write32(pc, BCMA_CORE_PCI_SBTOPCI0,
@@ -481,10 +490,21 @@ void __devinit bcma_core_pci_hostmode_in
 	 * before issuing configuration requests to PCI Express
 	 * devices.
 	 */
-	udelay(100000);
+	msleep(100);
 
 	bcma_core_pci_enable_crs(pc);
 
+	if (bus->chipinfo.id == BCMA_CHIP_ID_BCM4706 ||
+	    bus->chipinfo.id == BCMA_CHIP_ID_BCM4716) {
+		u16 val16;
+		bcma_extpci_read_config(pc, 0, 0, BCMA_CORE_PCI_CFG_DEVCTRL,
+					&val16, sizeof(val16));
+		val16 |= (2 << 5);	/* Max payload size of 512 */
+		val16 |= (2 << 12);	/* MRRS 512 */
+		bcma_extpci_write_config(pc, 0, 0, BCMA_CORE_PCI_CFG_DEVCTRL,
+					 &val16, sizeof(val16));
+	}
+
 	/* Enable PCI bridge BAR0 memory & master access */
 	tmp = PCI_COMMAND_MASTER | PCI_COMMAND_MEMORY;
 	bcma_extpci_write_config(pc, 0, 0, PCI_COMMAND, &tmp, sizeof(tmp));
@@ -501,7 +521,7 @@ void __devinit bcma_core_pci_hostmode_in
 	set_io_port_base(pc_host->pci_controller.io_map_base);
 	/* Give some time to the PCI controller to configure itself with the new
 	 * values. Not waiting at this point causes crashes of the machine. */
-	mdelay(10);
+	usleep_range(10000, 15000);
 	register_pci_controller(&pc_host->pci_controller);
 	return;
 }
@@ -534,7 +554,7 @@ DECLARE_PCI_FIXUP_EARLY(PCI_ANY_ID, PCI_
 static void bcma_core_pci_fixup_addresses(struct pci_dev *dev)
 {
 	struct resource *res;
-	int pos;
+	int pos, err;
 
 	if (dev->bus->ops->read != bcma_core_pci_hostmode_read_config) {
 		/* This is not a device on the PCI-core bridge. */
@@ -547,8 +567,12 @@ static void bcma_core_pci_fixup_addresse
 
 	for (pos = 0; pos < 6; pos++) {
 		res = &dev->resource[pos];
-		if (res->flags & (IORESOURCE_IO | IORESOURCE_MEM))
-			pci_assign_resource(dev, pos);
+		if (res->flags & (IORESOURCE_IO | IORESOURCE_MEM)) {
+			err = pci_assign_resource(dev, pos);
+			if (err)
+				pr_err("PCI: Problem fixing up the addresses on %s\n",
+				       pci_name(dev));
+		}
 	}
 }
 DECLARE_PCI_FIXUP_HEADER(PCI_ANY_ID, PCI_ANY_ID, bcma_core_pci_fixup_addresses);
@@ -558,6 +582,7 @@ DECLARE_PCI_FIXUP_HEADER(PCI_ANY_ID, PCI
 int bcma_core_pci_plat_dev_init(struct pci_dev *dev)
 {
 	struct bcma_drv_pci_host *pc_host;
+	int readrq;
 
 	if (dev->bus->ops->read != bcma_core_pci_hostmode_read_config) {
 		/* This is not a device on the PCI-core bridge. */
@@ -569,9 +594,14 @@ int bcma_core_pci_plat_dev_init(struct p
 	pr_info("PCI: Fixing up device %s\n", pci_name(dev));
 
 	/* Fix up interrupt lines */
-	dev->irq = bcma_core_mips_irq(pc_host->pdev->core) + 2;
+	dev->irq = bcma_core_irq(pc_host->pdev->core);
 	pci_write_config_byte(dev, PCI_INTERRUPT_LINE, dev->irq);
 
+	readrq = pcie_get_readrq(dev);
+	if (readrq > 128) {
+		pr_info("change PCIe max read request size from %i to 128\n", readrq);
+		pcie_set_readrq(dev, 128);
+	}
 	return 0;
 }
 EXPORT_SYMBOL(bcma_core_pci_plat_dev_init);
@@ -588,6 +618,6 @@ int bcma_core_pci_pcibios_map_irq(const
 
 	pc_host = container_of(dev->bus->ops, struct bcma_drv_pci_host,
 			       pci_ops);
-	return bcma_core_mips_irq(pc_host->pdev->core) + 2;
+	return bcma_core_irq(pc_host->pdev->core);
 }
 EXPORT_SYMBOL(bcma_core_pci_pcibios_map_irq);
--- a/drivers/bcma/host_pci.c
+++ b/drivers/bcma/host_pci.c
@@ -77,8 +77,8 @@ static void bcma_host_pci_write32(struct
 }
 
 #ifdef CONFIG_BCMA_BLOCKIO
-void bcma_host_pci_block_read(struct bcma_device *core, void *buffer,
-			      size_t count, u16 offset, u8 reg_width)
+static void bcma_host_pci_block_read(struct bcma_device *core, void *buffer,
+				     size_t count, u16 offset, u8 reg_width)
 {
 	void __iomem *addr = core->bus->mmio + offset;
 	if (core->bus->mapped_core != core)
@@ -100,8 +100,9 @@ void bcma_host_pci_block_read(struct bcm
 	}
 }
 
-void bcma_host_pci_block_write(struct bcma_device *core, const void *buffer,
-			       size_t count, u16 offset, u8 reg_width)
+static void bcma_host_pci_block_write(struct bcma_device *core,
+				      const void *buffer, size_t count,
+				      u16 offset, u8 reg_width)
 {
 	void __iomem *addr = core->bus->mmio + offset;
 	if (core->bus->mapped_core != core)
@@ -139,7 +140,7 @@ static void bcma_host_pci_awrite32(struc
 	iowrite32(value, core->bus->mmio + (1 * BCMA_CORE_SIZE) + offset);
 }
 
-const struct bcma_host_ops bcma_host_pci_ops = {
+static const struct bcma_host_ops bcma_host_pci_ops = {
 	.read8		= bcma_host_pci_read8,
 	.read16		= bcma_host_pci_read16,
 	.read32		= bcma_host_pci_read32,
@@ -237,7 +238,7 @@ static void __devexit bcma_host_pci_remo
 	pci_set_drvdata(dev, NULL);
 }
 
-#ifdef CONFIG_PM
+#ifdef CONFIG_PM_SLEEP
 static int bcma_host_pci_suspend(struct device *dev)
 {
 	struct pci_dev *pdev = to_pci_dev(dev);
@@ -260,11 +261,11 @@ static SIMPLE_DEV_PM_OPS(bcma_pm_ops, bc
 			 bcma_host_pci_resume);
 #define BCMA_PM_OPS	(&bcma_pm_ops)
 
-#else /* CONFIG_PM */
+#else /* CONFIG_PM_SLEEP */
 
 #define BCMA_PM_OPS     NULL
 
-#endif /* CONFIG_PM */
+#endif /* CONFIG_PM_SLEEP */
 
 static DEFINE_PCI_DEVICE_TABLE(bcma_pci_bridge_tbl) = {
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x0576) },
@@ -272,7 +273,9 @@ static DEFINE_PCI_DEVICE_TABLE(bcma_pci_
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4331) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4353) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4357) },
+	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4358) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4359) },
+	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4365) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4727) },
 	{ 0, },
 };
--- a/drivers/bcma/host_soc.c
+++ b/drivers/bcma/host_soc.c
@@ -143,7 +143,7 @@ static void bcma_host_soc_awrite32(struc
 	writel(value, core->io_wrap + offset);
 }
 
-const struct bcma_host_ops bcma_host_soc_ops = {
+static const struct bcma_host_ops bcma_host_soc_ops = {
 	.read8		= bcma_host_soc_read8,
 	.read16		= bcma_host_soc_read16,
 	.read32		= bcma_host_soc_read32,
--- a/drivers/bcma/main.c
+++ b/drivers/bcma/main.c
@@ -7,6 +7,7 @@
 
 #include "bcma_private.h"
 #include <linux/module.h>
+#include <linux/platform_device.h>
 #include <linux/bcma/bcma.h>
 #include <linux/slab.h>
 
@@ -80,6 +81,37 @@ struct bcma_device *bcma_find_core(struc
 }
 EXPORT_SYMBOL_GPL(bcma_find_core);
 
+struct bcma_device *bcma_find_core_unit(struct bcma_bus *bus, u16 coreid,
+					u8 unit)
+{
+	struct bcma_device *core;
+
+	list_for_each_entry(core, &bus->cores, list) {
+		if (core->id.id == coreid && core->core_unit == unit)
+			return core;
+	}
+	return NULL;
+}
+
+bool bcma_wait_value(struct bcma_device *core, u16 reg, u32 mask, u32 value,
+		     int timeout)
+{
+	unsigned long deadline = jiffies + timeout;
+	u32 val;
+
+	do {
+		val = bcma_read32(core, reg);
+		if ((val & mask) == value)
+			return true;
+		cpu_relax();
+		udelay(10);
+	} while (!time_after_eq(jiffies, deadline));
+
+	bcma_warn(core->bus, "Timeout waiting for register 0x%04X!\n", reg);
+
+	return false;
+}
+
 static void bcma_release_core_dev(struct device *dev)
 {
 	struct bcma_device *core = container_of(dev, struct bcma_device, dev);
@@ -107,6 +139,11 @@ static int bcma_register_cores(struct bc
 			continue;
 		}
 
+		/* Only first GMAC core on BCM4706 is connected and working */
+		if (core->id.id == BCMA_CORE_4706_MAC_GBIT &&
+		    core->core_unit > 0)
+			continue;
+
 		core->dev.release = bcma_release_core_dev;
 		core->dev.bus = &bcma_bus_type;
 		dev_set_name(&core->dev, "bcma%d:%d", bus->num, dev_id);
@@ -136,6 +173,41 @@ static int bcma_register_cores(struct bc
 		dev_id++;
 	}
 
+#ifdef CONFIG_BCMA_DRIVER_MIPS
+	if (bus->drv_cc.pflash.present) {
+		err = platform_device_register(&bcma_pflash_dev);
+		if (err)
+			bcma_err(bus, "Error registering parallel flash\n");
+	}
+#endif
+
+#ifdef CONFIG_BCMA_SFLASH
+	if (bus->drv_cc.sflash.present) {
+		err = platform_device_register(&bcma_sflash_dev);
+		if (err)
+			bcma_err(bus, "Error registering serial flash\n");
+	}
+#endif
+
+#ifdef CONFIG_BCMA_NFLASH
+	if (bus->drv_cc.nflash.present) {
+		err = platform_device_register(&bcma_nflash_dev);
+		if (err)
+			bcma_err(bus, "Error registering NAND flash\n");
+	}
+#endif
+	err = bcma_gpio_init(&bus->drv_cc);
+	if (err == -ENOTSUPP)
+		bcma_debug(bus, "GPIO driver not activated\n");
+	else if (err)
+		bcma_err(bus, "Error registering GPIO driver: %i\n", err);
+
+	if (bus->hosttype == BCMA_HOSTTYPE_SOC) {
+		err = bcma_chipco_watchdog_register(&bus->drv_cc);
+		if (err)
+			bcma_err(bus, "Error registering watchdog driver\n");
+	}
+
 	return 0;
 }
 
@@ -148,6 +220,8 @@ static void bcma_unregister_cores(struct
 		if (core->dev_registered)
 			device_unregister(&core->dev);
 	}
+	if (bus->hosttype == BCMA_HOSTTYPE_SOC)
+		platform_device_unregister(bus->drv_cc.watchdog);
 }
 
 int __devinit bcma_bus_register(struct bcma_bus *bus)
@@ -163,9 +237,23 @@ int __devinit bcma_bus_register(struct b
 	err = bcma_bus_scan(bus);
 	if (err) {
 		bcma_err(bus, "Failed to scan: %d\n", err);
-		return -1;
+		return err;
 	}
 
+	/* Early init CC core */
+	core = bcma_find_core(bus, bcma_cc_core_id(bus));
+	if (core) {
+		bus->drv_cc.core = core;
+		bcma_core_chipcommon_early_init(&bus->drv_cc);
+	}
+
+	/* Try to get SPROM */
+	err = bcma_sprom_get(bus);
+	if (err == -ENOENT) {
+		bcma_err(bus, "No SPROM available\n");
+	} else if (err)
+		bcma_err(bus, "Failed to get SPROM: %d\n", err);
+
 	/* Init CC core */
 	core = bcma_find_core(bus, bcma_cc_core_id(bus));
 	if (core) {
@@ -181,10 +269,17 @@ int __devinit bcma_bus_register(struct b
 	}
 
 	/* Init PCIE core */
-	core = bcma_find_core(bus, BCMA_CORE_PCIE);
+	core = bcma_find_core_unit(bus, BCMA_CORE_PCIE, 0);
 	if (core) {
-		bus->drv_pci.core = core;
-		bcma_core_pci_init(&bus->drv_pci);
+		bus->drv_pci[0].core = core;
+		bcma_core_pci_init(&bus->drv_pci[0]);
+	}
+
+	/* Init PCIE core */
+	core = bcma_find_core_unit(bus, BCMA_CORE_PCIE, 1);
+	if (core) {
+		bus->drv_pci[1].core = core;
+		bcma_core_pci_init(&bus->drv_pci[1]);
 	}
 
 	/* Init GBIT MAC COMMON core */
@@ -194,13 +289,6 @@ int __devinit bcma_bus_register(struct b
 		bcma_core_gmac_cmn_init(&bus->drv_gmac_cmn);
 	}
 
-	/* Try to get SPROM */
-	err = bcma_sprom_get(bus);
-	if (err == -ENOENT) {
-		bcma_err(bus, "No SPROM available\n");
-	} else if (err)
-		bcma_err(bus, "Failed to get SPROM: %d\n", err);
-
 	/* Register found cores */
 	bcma_register_cores(bus);
 
@@ -211,7 +299,24 @@ int __devinit bcma_bus_register(struct b
 
 void bcma_bus_unregister(struct bcma_bus *bus)
 {
+	struct bcma_device *cores[3];
+	int err;
+
+	err = bcma_gpio_unregister(&bus->drv_cc);
+	if (err == -EBUSY)
+		bcma_err(bus, "Some GPIOs are still in use.\n");
+	else if (err)
+		bcma_err(bus, "Can not unregister GPIO driver: %i\n", err);
+
+	cores[0] = bcma_find_core(bus, BCMA_CORE_MIPS_74K);
+	cores[1] = bcma_find_core(bus, BCMA_CORE_PCIE);
+	cores[2] = bcma_find_core(bus, BCMA_CORE_4706_MAC_GBIT_COMMON);
+
 	bcma_unregister_cores(bus);
+
+	kfree(cores[2]);
+	kfree(cores[1]);
+	kfree(cores[0]);
 }
 
 int __init bcma_bus_early_register(struct bcma_bus *bus,
@@ -248,18 +353,18 @@ int __init bcma_bus_early_register(struc
 		return -1;
 	}
 
-	/* Init CC core */
+	/* Early init CC core */
 	core = bcma_find_core(bus, bcma_cc_core_id(bus));
 	if (core) {
 		bus->drv_cc.core = core;
-		bcma_core_chipcommon_init(&bus->drv_cc);
+		bcma_core_chipcommon_early_init(&bus->drv_cc);
 	}
 
-	/* Init MIPS core */
+	/* Early init MIPS core */
 	core = bcma_find_core(bus, BCMA_CORE_MIPS_74K);
 	if (core) {
 		bus->drv_mips.core = core;
-		bcma_core_mips_init(&bus->drv_mips);
+		bcma_core_mips_early_init(&bus->drv_mips);
 	}
 
 	bcma_info(bus, "Early bus registered\n");
--- a/drivers/bcma/scan.c
+++ b/drivers/bcma/scan.c
@@ -32,6 +32,18 @@ static const struct bcma_device_id_name
 	{ BCMA_CORE_4706_CHIPCOMMON, "BCM4706 ChipCommon" },
 	{ BCMA_CORE_4706_SOC_RAM, "BCM4706 SOC RAM" },
 	{ BCMA_CORE_4706_MAC_GBIT, "BCM4706 GBit MAC" },
+	{ BCMA_CORE_PCIEG2, "PCIe Gen 2" },
+	{ BCMA_CORE_DMA, "DMA" },
+	{ BCMA_CORE_SDIO3, "SDIO3" },
+	{ BCMA_CORE_USB20, "USB 2.0" },
+	{ BCMA_CORE_USB30, "USB 3.0" },
+	{ BCMA_CORE_A9JTAG, "ARM Cortex A9 JTAG" },
+	{ BCMA_CORE_DDR23, "Denali DDR2/DDR3 memory controller" },
+	{ BCMA_CORE_ROM, "ROM" },
+	{ BCMA_CORE_NAND, "NAND flash controller" },
+	{ BCMA_CORE_QSPI, "SPI flash controller" },
+	{ BCMA_CORE_CHIPCOMMON_B, "Chipcommon B" },
+	{ BCMA_CORE_ARMCA9, "ARM Cortex A9 core (ihost)" },
 	{ BCMA_CORE_AMEMC, "AMEMC (DDR)" },
 	{ BCMA_CORE_ALTA, "ALTA (I2S)" },
 	{ BCMA_CORE_INVALID, "Invalid" },
@@ -84,6 +96,8 @@ static const struct bcma_device_id_name
 	{ BCMA_CORE_I2S, "I2S" },
 	{ BCMA_CORE_SDR_DDR1_MEM_CTL, "SDR/DDR1 Memory Controller" },
 	{ BCMA_CORE_SHIM, "SHIM" },
+	{ BCMA_CORE_PCIE2, "PCIe Gen2" },
+	{ BCMA_CORE_ARM_CR4, "ARM CR4" },
 	{ BCMA_CORE_DEFAULT, "Default" },
 };
 
@@ -137,19 +151,19 @@ static void bcma_scan_switch_core(struct
 				       addr);
 }
 
-static u32 bcma_erom_get_ent(struct bcma_bus *bus, u32 **eromptr)
+static u32 bcma_erom_get_ent(struct bcma_bus *bus, u32 __iomem **eromptr)
 {
 	u32 ent = readl(*eromptr);
 	(*eromptr)++;
 	return ent;
 }
 
-static void bcma_erom_push_ent(u32 **eromptr)
+static void bcma_erom_push_ent(u32 __iomem **eromptr)
 {
 	(*eromptr)--;
 }
 
-static s32 bcma_erom_get_ci(struct bcma_bus *bus, u32 **eromptr)
+static s32 bcma_erom_get_ci(struct bcma_bus *bus, u32 __iomem **eromptr)
 {
 	u32 ent = bcma_erom_get_ent(bus, eromptr);
 	if (!(ent & SCAN_ER_VALID))
@@ -159,14 +173,14 @@ static s32 bcma_erom_get_ci(struct bcma_
 	return ent;
 }
 
-static bool bcma_erom_is_end(struct bcma_bus *bus, u32 **eromptr)
+static bool bcma_erom_is_end(struct bcma_bus *bus, u32 __iomem **eromptr)
 {
 	u32 ent = bcma_erom_get_ent(bus, eromptr);
 	bcma_erom_push_ent(eromptr);
 	return (ent == (SCAN_ER_TAG_END | SCAN_ER_VALID));
 }
 
-static bool bcma_erom_is_bridge(struct bcma_bus *bus, u32 **eromptr)
+static bool bcma_erom_is_bridge(struct bcma_bus *bus, u32 __iomem **eromptr)
 {
 	u32 ent = bcma_erom_get_ent(bus, eromptr);
 	bcma_erom_push_ent(eromptr);
@@ -175,7 +189,7 @@ static bool bcma_erom_is_bridge(struct b
 		((ent & SCAN_ADDR_TYPE) == SCAN_ADDR_TYPE_BRIDGE));
 }
 
-static void bcma_erom_skip_component(struct bcma_bus *bus, u32 **eromptr)
+static void bcma_erom_skip_component(struct bcma_bus *bus, u32 __iomem **eromptr)
 {
 	u32 ent;
 	while (1) {
@@ -189,7 +203,7 @@ static void bcma_erom_skip_component(str
 	bcma_erom_push_ent(eromptr);
 }
 
-static s32 bcma_erom_get_mst_port(struct bcma_bus *bus, u32 **eromptr)
+static s32 bcma_erom_get_mst_port(struct bcma_bus *bus, u32 __iomem **eromptr)
 {
 	u32 ent = bcma_erom_get_ent(bus, eromptr);
 	if (!(ent & SCAN_ER_VALID))
@@ -199,7 +213,7 @@ static s32 bcma_erom_get_mst_port(struct
 	return ent;
 }
 
-static s32 bcma_erom_get_addr_desc(struct bcma_bus *bus, u32 **eromptr,
+static u32 bcma_erom_get_addr_desc(struct bcma_bus *bus, u32 __iomem **eromptr,
 				  u32 type, u8 port)
 {
 	u32 addrl, addrh, sizel, sizeh = 0;
@@ -211,7 +225,7 @@ static s32 bcma_erom_get_addr_desc(struc
 	    ((ent & SCAN_ADDR_TYPE) != type) ||
 	    (((ent & SCAN_ADDR_PORT) >> SCAN_ADDR_PORT_SHIFT) != port)) {
 		bcma_erom_push_ent(eromptr);
-		return -EINVAL;
+		return (u32)-EINVAL;
 	}
 
 	addrl = ent & SCAN_ADDR_ADDR;
@@ -255,11 +269,13 @@ static struct bcma_device *bcma_find_cor
 	return NULL;
 }
 
+#define IS_ERR_VALUE_U32(x) ((x) >= (u32)-MAX_ERRNO)
+
 static int bcma_get_next_core(struct bcma_bus *bus, u32 __iomem **eromptr,
 			      struct bcma_device_id *match, int core_num,
 			      struct bcma_device *core)
 {
-	s32 tmp;
+	u32 tmp;
 	u8 i, j;
 	s32 cia, cib;
 	u8 ports[2], wrappers[2];
@@ -337,11 +353,11 @@ static int bcma_get_next_core(struct bcm
 	 * the main register space for the core
 	 */
 	tmp = bcma_erom_get_addr_desc(bus, eromptr, SCAN_ADDR_TYPE_SLAVE, 0);
-	if (tmp <= 0) {
+	if (tmp == 0 || IS_ERR_VALUE_U32(tmp)) {
 		/* Try again to see if it is a bridge */
 		tmp = bcma_erom_get_addr_desc(bus, eromptr,
 					      SCAN_ADDR_TYPE_BRIDGE, 0);
-		if (tmp <= 0) {
+		if (tmp == 0 || IS_ERR_VALUE_U32(tmp)) {
 			return -EILSEQ;
 		} else {
 			bcma_info(bus, "Bridge found\n");
@@ -355,7 +371,7 @@ static int bcma_get_next_core(struct bcm
 		for (j = 0; ; j++) {
 			tmp = bcma_erom_get_addr_desc(bus, eromptr,
 				SCAN_ADDR_TYPE_SLAVE, i);
-			if (tmp < 0) {
+			if (IS_ERR_VALUE_U32(tmp)) {
 				/* no more entries for port _i_ */
 				/* pr_debug("erom: slave port %d "
 				 * "has %d descriptors\n", i, j); */
@@ -372,7 +388,7 @@ static int bcma_get_next_core(struct bcm
 		for (j = 0; ; j++) {
 			tmp = bcma_erom_get_addr_desc(bus, eromptr,
 				SCAN_ADDR_TYPE_MWRAP, i);
-			if (tmp < 0) {
+			if (IS_ERR_VALUE_U32(tmp)) {
 				/* no more entries for port _i_ */
 				/* pr_debug("erom: master wrapper %d "
 				 * "has %d descriptors\n", i, j); */
@@ -390,7 +406,7 @@ static int bcma_get_next_core(struct bcm
 		for (j = 0; ; j++) {
 			tmp = bcma_erom_get_addr_desc(bus, eromptr,
 				SCAN_ADDR_TYPE_SWRAP, i + hack);
-			if (tmp < 0) {
+			if (IS_ERR_VALUE_U32(tmp)) {
 				/* no more entries for port _i_ */
 				/* pr_debug("erom: master wrapper %d "
 				 * has %d descriptors\n", i, j); */
--- a/drivers/bcma/sprom.c
+++ b/drivers/bcma/sprom.c
@@ -72,12 +72,12 @@ fail:
  * R/W ops.
  **************************************************/
 
-static void bcma_sprom_read(struct bcma_bus *bus, u16 offset, u16 *sprom)
+static void bcma_sprom_read(struct bcma_bus *bus, u16 offset, u16 *sprom,
+			    size_t words)
 {
 	int i;
-	for (i = 0; i < SSB_SPROMSIZE_WORDS_R4; i++)
-		sprom[i] = bcma_read16(bus->drv_cc.core,
-				       offset + (i * 2));
+	for (i = 0; i < words; i++)
+		sprom[i] = bcma_read16(bus->drv_cc.core, offset + (i * 2));
 }
 
 /**************************************************
@@ -124,29 +124,29 @@ static inline u8 bcma_crc8(u8 crc, u8 da
 	return t[crc ^ data];
 }
 
-static u8 bcma_sprom_crc(const u16 *sprom)
+static u8 bcma_sprom_crc(const u16 *sprom, size_t words)
 {
 	int word;
 	u8 crc = 0xFF;
 
-	for (word = 0; word < SSB_SPROMSIZE_WORDS_R4 - 1; word++) {
+	for (word = 0; word < words - 1; word++) {
 		crc = bcma_crc8(crc, sprom[word] & 0x00FF);
 		crc = bcma_crc8(crc, (sprom[word] & 0xFF00) >> 8);
 	}
-	crc = bcma_crc8(crc, sprom[SSB_SPROMSIZE_WORDS_R4 - 1] & 0x00FF);
+	crc = bcma_crc8(crc, sprom[words - 1] & 0x00FF);
 	crc ^= 0xFF;
 
 	return crc;
 }
 
-static int bcma_sprom_check_crc(const u16 *sprom)
+static int bcma_sprom_check_crc(const u16 *sprom, size_t words)
 {
 	u8 crc;
 	u8 expected_crc;
 	u16 tmp;
 
-	crc = bcma_sprom_crc(sprom);
-	tmp = sprom[SSB_SPROMSIZE_WORDS_R4 - 1] & SSB_SPROM_REVISION_CRC;
+	crc = bcma_sprom_crc(sprom, words);
+	tmp = sprom[words - 1] & SSB_SPROM_REVISION_CRC;
 	expected_crc = tmp >> SSB_SPROM_REVISION_CRC_SHIFT;
 	if (crc != expected_crc)
 		return -EPROTO;
@@ -154,21 +154,25 @@ static int bcma_sprom_check_crc(const u1
 	return 0;
 }
 
-static int bcma_sprom_valid(const u16 *sprom)
+static int bcma_sprom_valid(struct bcma_bus *bus, const u16 *sprom,
+			    size_t words)
 {
 	u16 revision;
 	int err;
 
-	err = bcma_sprom_check_crc(sprom);
+	err = bcma_sprom_check_crc(sprom, words);
 	if (err)
 		return err;
 
-	revision = sprom[SSB_SPROMSIZE_WORDS_R4 - 1] & SSB_SPROM_REVISION_REV;
-	if (revision != 8 && revision != 9) {
+	revision = sprom[words - 1] & SSB_SPROM_REVISION_REV;
+	if (revision != 8 && revision != 9 && revision != 10) {
 		pr_err("Unsupported SPROM revision: %d\n", revision);
 		return -ENOENT;
 	}
 
+	bus->sprom.revision = revision;
+	bcma_debug(bus, "Found SPROM revision %d\n", revision);
+
 	return 0;
 }
 
@@ -208,15 +212,13 @@ static void bcma_sprom_extract_r8(struct
 	BUILD_BUG_ON(ARRAY_SIZE(pwr_info_offset) !=
 			ARRAY_SIZE(bus->sprom.core_pwr_info));
 
-	bus->sprom.revision = sprom[SSB_SPROMSIZE_WORDS_R4 - 1] &
-		SSB_SPROM_REVISION_REV;
-
 	for (i = 0; i < 3; i++) {
 		v = sprom[SPOFF(SSB_SPROM8_IL0MAC) + i];
 		*(((__be16 *)bus->sprom.il0mac) + i) = cpu_to_be16(v);
 	}
 
 	SPEX(board_rev, SSB_SPROM8_BOARDREV, ~0, 0);
+	SPEX(board_type, SSB_SPROM1_SPID, ~0, 0);
 
 	SPEX(txpid2g[0], SSB_SPROM4_TXPID2G01, SSB_SPROM4_TXPID2G0,
 	     SSB_SPROM4_TXPID2G0_SHIFT);
@@ -501,13 +503,15 @@ static bool bcma_sprom_onchip_available(
 	case BCMA_CHIP_ID_BCM4331:
 		present = chip_status & BCMA_CC_CHIPST_4331_OTP_PRESENT;
 		break;
-
+	case BCMA_CHIP_ID_BCM43142:
 	case BCMA_CHIP_ID_BCM43224:
 	case BCMA_CHIP_ID_BCM43225:
 		/* for these chips OTP is always available */
 		present = true;
 		break;
+	case BCMA_CHIP_ID_BCM43227:
 	case BCMA_CHIP_ID_BCM43228:
+	case BCMA_CHIP_ID_BCM43428:
 		present = chip_status & BCMA_CC_CHIPST_43228_OTP_PRESENT;
 		break;
 	default:
@@ -547,7 +551,9 @@ int bcma_sprom_get(struct bcma_bus *bus)
 {
 	u16 offset = BCMA_CC_SPROM;
 	u16 *sprom;
-	int err = 0;
+	size_t sprom_sizes[] = { SSB_SPROMSIZE_WORDS_R4,
+				 SSB_SPROMSIZE_WORDS_R10, };
+	int i, err = 0;
 
 	if (!bus->drv_cc.core)
 		return -EOPNOTSUPP;
@@ -576,29 +582,37 @@ int bcma_sprom_get(struct bcma_bus *bus)
 		}
 	}
 
-	sprom = kcalloc(SSB_SPROMSIZE_WORDS_R4, sizeof(u16),
-			GFP_KERNEL);
-	if (!sprom)
-		return -ENOMEM;
-
 	if (bus->chipinfo.id == BCMA_CHIP_ID_BCM4331 ||
 	    bus->chipinfo.id == BCMA_CHIP_ID_BCM43431)
 		bcma_chipco_bcm4331_ext_pa_lines_ctl(&bus->drv_cc, false);
 
 	bcma_debug(bus, "SPROM offset 0x%x\n", offset);
-	bcma_sprom_read(bus, offset, sprom);
+	for (i = 0; i < ARRAY_SIZE(sprom_sizes); i++) {
+		size_t words = sprom_sizes[i];
+
+		sprom = kcalloc(words, sizeof(u16), GFP_KERNEL);
+		if (!sprom)
+			return -ENOMEM;
+
+		bcma_sprom_read(bus, offset, sprom, words);
+		err = bcma_sprom_valid(bus, sprom, words);
+		if (!err)
+			break;
+
+		kfree(sprom);
+	}
 
 	if (bus->chipinfo.id == BCMA_CHIP_ID_BCM4331 ||
 	    bus->chipinfo.id == BCMA_CHIP_ID_BCM43431)
 		bcma_chipco_bcm4331_ext_pa_lines_ctl(&bus->drv_cc, true);
 
-	err = bcma_sprom_valid(sprom);
-	if (err)
-		goto out;
-
-	bcma_sprom_extract_r8(bus, sprom);
+	if (err) {
+		bcma_warn(bus, "Invalid SPROM read from the PCIe card, trying to use fallback SPROM\n");
+		err = bcma_fill_sprom_with_fallback(bus, &bus->sprom);
+	} else {
+		bcma_sprom_extract_r8(bus, sprom);
+		kfree(sprom);
+	}
 
-out:
-	kfree(sprom);
 	return err;
 }
--- a/include/linux/bcma/bcma.h
+++ b/include/linux/bcma/bcma.h
@@ -10,7 +10,7 @@
 #include <linux/bcma/bcma_driver_gmac_cmn.h>
 #include <linux/ssb/ssb.h> /* SPROM sharing */
 
-#include "bcma_regs.h"
+#include <linux/bcma/bcma_regs.h>
 
 struct bcma_device;
 struct bcma_bus;
@@ -72,7 +72,19 @@ struct bcma_host_ops {
 /* Core-ID values. */
 #define BCMA_CORE_OOB_ROUTER		0x367	/* Out of band */
 #define BCMA_CORE_4706_CHIPCOMMON	0x500
+#define BCMA_CORE_PCIEG2		0x501
+#define BCMA_CORE_DMA			0x502
+#define BCMA_CORE_SDIO3			0x503
+#define BCMA_CORE_USB20			0x504
+#define BCMA_CORE_USB30			0x505
+#define BCMA_CORE_A9JTAG		0x506
+#define BCMA_CORE_DDR23			0x507
+#define BCMA_CORE_ROM			0x508
+#define BCMA_CORE_NAND			0x509
+#define BCMA_CORE_QSPI			0x50A
+#define BCMA_CORE_CHIPCOMMON_B		0x50B
 #define BCMA_CORE_4706_SOC_RAM		0x50E
+#define BCMA_CORE_ARMCA9		0x510
 #define BCMA_CORE_4706_MAC_GBIT		0x52D
 #define BCMA_CORE_AMEMC			0x52E	/* DDR1/2 memory controller core */
 #define BCMA_CORE_ALTA			0x534	/* I2S core */
@@ -134,12 +146,17 @@ struct bcma_host_ops {
 #define BCMA_CORE_I2S			0x834
 #define BCMA_CORE_SDR_DDR1_MEM_CTL	0x835	/* SDR/DDR1 memory controller core */
 #define BCMA_CORE_SHIM			0x837	/* SHIM component in ubus/6362 */
+#define BCMA_CORE_PHY_AC		0x83B
+#define BCMA_CORE_PCIE2			0x83C	/* PCI Express Gen2 */
+#define BCMA_CORE_USB30_DEV		0x83D
+#define BCMA_CORE_ARM_CR4		0x83E
 #define BCMA_CORE_DEFAULT		0xFFF
 
 #define BCMA_MAX_NR_CORES		16
 
 /* Chip IDs of PCIe devices */
 #define BCMA_CHIP_ID_BCM4313	0x4313
+#define BCMA_CHIP_ID_BCM43142	43142
 #define BCMA_CHIP_ID_BCM43224	43224
 #define  BCMA_PKG_ID_BCM43224_FAB_CSM	0x8
 #define  BCMA_PKG_ID_BCM43224_FAB_SMIC	0xa
@@ -157,6 +174,7 @@ struct bcma_host_ops {
 
 /* Chip IDs of SoCs */
 #define BCMA_CHIP_ID_BCM4706	0x5300
+#define  BCMA_PKG_ID_BCM4706L	1
 #define BCMA_CHIP_ID_BCM4716	0x4716
 #define  BCMA_PKG_ID_BCM4716	8
 #define  BCMA_PKG_ID_BCM4717	9
@@ -166,7 +184,70 @@ struct bcma_host_ops {
 #define BCMA_CHIP_ID_BCM4749	0x4749
 #define BCMA_CHIP_ID_BCM5356	0x5356
 #define BCMA_CHIP_ID_BCM5357	0x5357
+#define  BCMA_PKG_ID_BCM5358	9
+#define  BCMA_PKG_ID_BCM47186	10
+#define  BCMA_PKG_ID_BCM5357	11
 #define BCMA_CHIP_ID_BCM53572	53572
+#define  BCMA_PKG_ID_BCM47188	9
+#define BCMA_CHIP_ID_BCM4707	53010
+#define  BCMA_PKG_ID_BCM4707	1
+#define  BCMA_PKG_ID_BCM4708	2
+#define  BCMA_PKG_ID_BCM4709	0
+#define BCMA_CHIP_ID_BCM53018	53018
+
+/* Board types (on PCI usually equals to the subsystem dev id) */
+/* BCM4313 */
+#define BCMA_BOARD_TYPE_BCM94313BU	0X050F
+#define BCMA_BOARD_TYPE_BCM94313HM	0X0510
+#define BCMA_BOARD_TYPE_BCM94313EPA	0X0511
+#define BCMA_BOARD_TYPE_BCM94313HMG	0X051C
+/* BCM4716 */
+#define BCMA_BOARD_TYPE_BCM94716NR2	0X04CD
+/* BCM43224 */
+#define BCMA_BOARD_TYPE_BCM943224X21	0X056E
+#define BCMA_BOARD_TYPE_BCM943224X21_FCC	0X00D1
+#define BCMA_BOARD_TYPE_BCM943224X21B	0X00E9
+#define BCMA_BOARD_TYPE_BCM943224M93	0X008B
+#define BCMA_BOARD_TYPE_BCM943224M93A	0X0090
+#define BCMA_BOARD_TYPE_BCM943224X16	0X0093
+#define BCMA_BOARD_TYPE_BCM94322X9	0X008D
+#define BCMA_BOARD_TYPE_BCM94322M35E	0X008E
+/* BCM43228 */
+#define BCMA_BOARD_TYPE_BCM943228BU8	0X0540
+#define BCMA_BOARD_TYPE_BCM943228BU9	0X0541
+#define BCMA_BOARD_TYPE_BCM943228BU	0X0542
+#define BCMA_BOARD_TYPE_BCM943227HM4L	0X0543
+#define BCMA_BOARD_TYPE_BCM943227HMB	0X0544
+#define BCMA_BOARD_TYPE_BCM943228HM4L	0X0545
+#define BCMA_BOARD_TYPE_BCM943228SD	0X0573
+/* BCM4331 */
+#define BCMA_BOARD_TYPE_BCM94331X19	0X00D6
+#define BCMA_BOARD_TYPE_BCM94331X28	0X00E4
+#define BCMA_BOARD_TYPE_BCM94331X28B	0X010E
+#define BCMA_BOARD_TYPE_BCM94331PCIEBT3AX	0X00E4
+#define BCMA_BOARD_TYPE_BCM94331X12_2G	0X00EC
+#define BCMA_BOARD_TYPE_BCM94331X12_5G	0X00ED
+#define BCMA_BOARD_TYPE_BCM94331X29B	0X00EF
+#define BCMA_BOARD_TYPE_BCM94331CSAX	0X00EF
+#define BCMA_BOARD_TYPE_BCM94331X19C	0X00F5
+#define BCMA_BOARD_TYPE_BCM94331X33	0X00F4
+#define BCMA_BOARD_TYPE_BCM94331BU	0X0523
+#define BCMA_BOARD_TYPE_BCM94331S9BU	0X0524
+#define BCMA_BOARD_TYPE_BCM94331MC	0X0525
+#define BCMA_BOARD_TYPE_BCM94331MCI	0X0526
+#define BCMA_BOARD_TYPE_BCM94331PCIEBT4	0X0527
+#define BCMA_BOARD_TYPE_BCM94331HM	0X0574
+#define BCMA_BOARD_TYPE_BCM94331PCIEDUAL	0X059B
+#define BCMA_BOARD_TYPE_BCM94331MCH5	0X05A9
+#define BCMA_BOARD_TYPE_BCM94331CS	0X05C6
+#define BCMA_BOARD_TYPE_BCM94331CD	0X05DA
+/* BCM53572 */
+#define BCMA_BOARD_TYPE_BCM953572BU	0X058D
+#define BCMA_BOARD_TYPE_BCM953572NR2	0X058E
+#define BCMA_BOARD_TYPE_BCM947188NR2	0X058F
+#define BCMA_BOARD_TYPE_BCM953572SDRNR2	0X0590
+/* BCM43142 */
+#define BCMA_BOARD_TYPE_BCM943142HM	0X05E0
 
 struct bcma_device {
 	struct bcma_bus *bus;
@@ -251,7 +332,7 @@ struct bcma_bus {
 	u8 num;
 
 	struct bcma_drv_cc drv_cc;
-	struct bcma_drv_pci drv_pci;
+	struct bcma_drv_pci drv_pci[2];
 	struct bcma_drv_mips drv_mips;
 	struct bcma_drv_gmac_cmn drv_gmac_cmn;
 
@@ -345,6 +426,7 @@ extern void bcma_core_set_clockmode(stru
 				    enum bcma_clkmode clkmode);
 extern void bcma_core_pll_ctl(struct bcma_device *core, u32 req, u32 status,
 			      bool on);
+extern u32 bcma_chipco_pll_read(struct bcma_drv_cc *cc, u32 offset);
 #define BCMA_DMA_TRANSLATION_MASK	0xC0000000
 #define  BCMA_DMA_TRANSLATION_NONE	0x00000000
 #define  BCMA_DMA_TRANSLATION_DMA32_CMT	0x40000000 /* Client Mode Translation for 32-bit DMA */
--- a/include/linux/bcma/bcma_driver_chipcommon.h
+++ b/include/linux/bcma/bcma_driver_chipcommon.h
@@ -1,6 +1,9 @@
 #ifndef LINUX_BCMA_DRIVER_CC_H_
 #define LINUX_BCMA_DRIVER_CC_H_
 
+#include <linux/platform_device.h>
+#include <linux/gpio.h>
+
 /** ChipCommon core registers. **/
 #define BCMA_CC_ID			0x0000
 #define  BCMA_CC_ID_ID			0x0000FFFF
@@ -24,7 +27,7 @@
 #define   BCMA_CC_FLASHT_NONE		0x00000000	/* No flash */
 #define   BCMA_CC_FLASHT_STSER		0x00000100	/* ST serial flash */
 #define   BCMA_CC_FLASHT_ATSER		0x00000200	/* Atmel serial flash */
-#define   BCMA_CC_FLASHT_NFLASH		0x00000200	/* NAND flash */
+#define   BCMA_CC_FLASHT_NAND		0x00000300	/* NAND flash */
 #define	  BCMA_CC_FLASHT_PARA		0x00000700	/* Parallel flash */
 #define  BCMA_CC_CAP_PLLT		0x00038000	/* PLL Type */
 #define   BCMA_PLLTYPE_NONE		0x00000000
@@ -100,6 +103,8 @@
 #define  BCMA_CC_CHIPST_4706_SFLASH_TYPE	BIT(2) /* 0: 8b-p/ST-s flash, 1: 16b-p/Atmal-s flash */
 #define  BCMA_CC_CHIPST_4706_MIPS_BENDIAN	BIT(3) /* 0: little, 1: big endian */
 #define  BCMA_CC_CHIPST_4706_PCIE1_DISABLE	BIT(5) /* PCIE1 enable strap pin */
+#define  BCMA_CC_CHIPST_5357_NAND_BOOT		BIT(4) /* NAND boot, valid for CC rev 38 and/or BCM5357 */
+#define  BCMA_CC_CHIPST_4360_XTAL_40MZ		0x00000001
 #define BCMA_CC_JCMD			0x0030		/* Rev >= 10 only */
 #define  BCMA_CC_JCMD_START		0x80000000
 #define  BCMA_CC_JCMD_BUSY		0x80000000
@@ -266,6 +271,29 @@
 #define  BCMA_CC_SROM_CONTROL_SIZE_16K	0x00000004
 #define  BCMA_CC_SROM_CONTROL_SIZE_SHIFT	1
 #define  BCMA_CC_SROM_CONTROL_PRESENT	0x00000001
+/* Block 0x140 - 0x190 registers are chipset specific */
+#define BCMA_CC_4706_FLASHSCFG		0x18C		/* Flash struct configuration */
+#define  BCMA_CC_4706_FLASHSCFG_MASK	0x000000ff
+#define  BCMA_CC_4706_FLASHSCFG_SF1	0x00000001	/* 2nd serial flash present */
+#define  BCMA_CC_4706_FLASHSCFG_PF1	0x00000002	/* 2nd parallel flash present */
+#define  BCMA_CC_4706_FLASHSCFG_SF1_TYPE	0x00000004	/* 2nd serial flash type : 0 : ST, 1 : Atmel */
+#define  BCMA_CC_4706_FLASHSCFG_NF1	0x00000008	/* 2nd NAND flash present */
+#define  BCMA_CC_4706_FLASHSCFG_1ST_MADDR_SEG_MASK	0x000000f0
+#define  BCMA_CC_4706_FLASHSCFG_1ST_MADDR_SEG_4MB	0x00000010	/* 4MB */
+#define  BCMA_CC_4706_FLASHSCFG_1ST_MADDR_SEG_8MB	0x00000020	/* 8MB */
+#define  BCMA_CC_4706_FLASHSCFG_1ST_MADDR_SEG_16MB	0x00000030	/* 16MB */
+#define  BCMA_CC_4706_FLASHSCFG_1ST_MADDR_SEG_32MB	0x00000040	/* 32MB */
+#define  BCMA_CC_4706_FLASHSCFG_1ST_MADDR_SEG_64MB	0x00000050	/* 64MB */
+#define  BCMA_CC_4706_FLASHSCFG_1ST_MADDR_SEG_128MB	0x00000060	/* 128MB */
+#define  BCMA_CC_4706_FLASHSCFG_1ST_MADDR_SEG_256MB	0x00000070	/* 256MB */
+/* NAND flash registers for BCM4706 (corerev = 31) */
+#define BCMA_CC_NFLASH_CTL		0x01A0
+#define  BCMA_CC_NFLASH_CTL_ERR		0x08000000
+#define BCMA_CC_NFLASH_CONF		0x01A4
+#define BCMA_CC_NFLASH_COL_ADDR		0x01A8
+#define BCMA_CC_NFLASH_ROW_ADDR		0x01AC
+#define BCMA_CC_NFLASH_DATA		0x01B0
+#define BCMA_CC_NFLASH_WAITCNT0		0x01B4
 /* 0x1E0 is defined as shared BCMA_CLKCTLST */
 #define BCMA_CC_HW_WORKAROUND		0x01E4 /* Hardware workaround (rev >= 20) */
 #define BCMA_CC_UART0_DATA		0x0300
@@ -288,6 +316,9 @@
 #define BCMA_CC_PMU_CTL			0x0600 /* PMU control */
 #define  BCMA_CC_PMU_CTL_ILP_DIV	0xFFFF0000 /* ILP div mask */
 #define  BCMA_CC_PMU_CTL_ILP_DIV_SHIFT	16
+#define  BCMA_CC_PMU_CTL_RES		0x00006000 /* reset control mask */
+#define  BCMA_CC_PMU_CTL_RES_SHIFT	13
+#define  BCMA_CC_PMU_CTL_RES_RELOAD	0x2	/* reload POR values */
 #define  BCMA_CC_PMU_CTL_PLL_UPD	0x00000400
 #define  BCMA_CC_PMU_CTL_NOILPONW	0x00000200 /* No ILP on wait */
 #define  BCMA_CC_PMU_CTL_HTREQEN	0x00000100 /* HT req enable */
@@ -299,6 +330,8 @@
 #define BCMA_CC_PMU_CAP			0x0604 /* PMU capabilities */
 #define  BCMA_CC_PMU_CAP_REVISION	0x000000FF /* Revision mask */
 #define BCMA_CC_PMU_STAT		0x0608 /* PMU status */
+#define  BCMA_CC_PMU_STAT_EXT_LPO_AVAIL	0x00000100
+#define  BCMA_CC_PMU_STAT_WDRESET	0x00000080
 #define  BCMA_CC_PMU_STAT_INTPEND	0x00000040 /* Interrupt pending */
 #define  BCMA_CC_PMU_STAT_SBCLKST	0x00000030 /* Backplane clock status? */
 #define  BCMA_CC_PMU_STAT_HAVEALP	0x00000008 /* ALP available */
@@ -324,7 +357,66 @@
 #define BCMA_CC_REGCTL_DATA		0x065C
 #define BCMA_CC_PLLCTL_ADDR		0x0660
 #define BCMA_CC_PLLCTL_DATA		0x0664
+#define BCMA_CC_PMU_STRAPOPT		0x0668 /* (corerev >= 28) */
+#define BCMA_CC_PMU_XTAL_FREQ		0x066C /* (pmurev >= 10) */
+#define  BCMA_CC_PMU_XTAL_FREQ_ILPCTL_MASK	0x00001FFF
+#define  BCMA_CC_PMU_XTAL_FREQ_MEASURE_MASK	0x80000000
+#define  BCMA_CC_PMU_XTAL_FREQ_MEASURE_SHIFT	31
 #define BCMA_CC_SPROM			0x0800 /* SPROM beginning */
+/* NAND flash MLC controller registers (corerev >= 38) */
+#define BCMA_CC_NAND_REVISION		0x0C00
+#define BCMA_CC_NAND_CMD_START		0x0C04
+#define BCMA_CC_NAND_CMD_ADDR_X		0x0C08
+#define BCMA_CC_NAND_CMD_ADDR		0x0C0C
+#define BCMA_CC_NAND_CMD_END_ADDR	0x0C10
+#define BCMA_CC_NAND_CS_NAND_SELECT	0x0C14
+#define BCMA_CC_NAND_CS_NAND_XOR	0x0C18
+#define BCMA_CC_NAND_SPARE_RD0		0x0C20
+#define BCMA_CC_NAND_SPARE_RD4		0x0C24
+#define BCMA_CC_NAND_SPARE_RD8		0x0C28
+#define BCMA_CC_NAND_SPARE_RD12		0x0C2C
+#define BCMA_CC_NAND_SPARE_WR0		0x0C30
+#define BCMA_CC_NAND_SPARE_WR4		0x0C34
+#define BCMA_CC_NAND_SPARE_WR8		0x0C38
+#define BCMA_CC_NAND_SPARE_WR12		0x0C3C
+#define BCMA_CC_NAND_ACC_CONTROL	0x0C40
+#define BCMA_CC_NAND_CONFIG		0x0C48
+#define BCMA_CC_NAND_TIMING_1		0x0C50
+#define BCMA_CC_NAND_TIMING_2		0x0C54
+#define BCMA_CC_NAND_SEMAPHORE		0x0C58
+#define BCMA_CC_NAND_DEVID		0x0C60
+#define BCMA_CC_NAND_DEVID_X		0x0C64
+#define BCMA_CC_NAND_BLOCK_LOCK_STATUS	0x0C68
+#define BCMA_CC_NAND_INTFC_STATUS	0x0C6C
+#define BCMA_CC_NAND_ECC_CORR_ADDR_X	0x0C70
+#define BCMA_CC_NAND_ECC_CORR_ADDR	0x0C74
+#define BCMA_CC_NAND_ECC_UNC_ADDR_X	0x0C78
+#define BCMA_CC_NAND_ECC_UNC_ADDR	0x0C7C
+#define BCMA_CC_NAND_READ_ERROR_COUNT	0x0C80
+#define BCMA_CC_NAND_CORR_STAT_THRESHOLD	0x0C84
+#define BCMA_CC_NAND_READ_ADDR_X	0x0C90
+#define BCMA_CC_NAND_READ_ADDR		0x0C94
+#define BCMA_CC_NAND_PAGE_PROGRAM_ADDR_X	0x0C98
+#define BCMA_CC_NAND_PAGE_PROGRAM_ADDR	0x0C9C
+#define BCMA_CC_NAND_COPY_BACK_ADDR_X	0x0CA0
+#define BCMA_CC_NAND_COPY_BACK_ADDR	0x0CA4
+#define BCMA_CC_NAND_BLOCK_ERASE_ADDR_X	0x0CA8
+#define BCMA_CC_NAND_BLOCK_ERASE_ADDR	0x0CAC
+#define BCMA_CC_NAND_INV_READ_ADDR_X	0x0CB0
+#define BCMA_CC_NAND_INV_READ_ADDR	0x0CB4
+#define BCMA_CC_NAND_BLK_WR_PROTECT	0x0CC0
+#define BCMA_CC_NAND_ACC_CONTROL_CS1	0x0CD0
+#define BCMA_CC_NAND_CONFIG_CS1		0x0CD4
+#define BCMA_CC_NAND_TIMING_1_CS1	0x0CD8
+#define BCMA_CC_NAND_TIMING_2_CS1	0x0CDC
+#define BCMA_CC_NAND_SPARE_RD16		0x0D30
+#define BCMA_CC_NAND_SPARE_RD20		0x0D34
+#define BCMA_CC_NAND_SPARE_RD24		0x0D38
+#define BCMA_CC_NAND_SPARE_RD28		0x0D3C
+#define BCMA_CC_NAND_CACHE_ADDR		0x0D40
+#define BCMA_CC_NAND_CACHE_DATA		0x0D44
+#define BCMA_CC_NAND_CTRL_CONFIG	0x0D48
+#define BCMA_CC_NAND_CTRL_STATUS	0x0D4C
 
 /* Divider allocation in 4716/47162/5356 */
 #define BCMA_CC_PMU5_MAINPLL_CPU	1
@@ -350,6 +442,23 @@
 #define  BCMA_CC_PMU6_4706_PROC_NDIV_MODE_MASK	0x00000007
 #define  BCMA_CC_PMU6_4706_PROC_NDIV_MODE_SHIFT	0
 
+/* PMU rev 15 */
+#define BCMA_CC_PMU15_PLL_PLLCTL0	0
+#define  BCMA_CC_PMU15_PLL_PC0_CLKSEL_MASK	0x00000003
+#define  BCMA_CC_PMU15_PLL_PC0_CLKSEL_SHIFT	0
+#define  BCMA_CC_PMU15_PLL_PC0_FREQTGT_MASK	0x003FFFFC
+#define  BCMA_CC_PMU15_PLL_PC0_FREQTGT_SHIFT	2
+#define  BCMA_CC_PMU15_PLL_PC0_PRESCALE_MASK	0x00C00000
+#define  BCMA_CC_PMU15_PLL_PC0_PRESCALE_SHIFT	22
+#define  BCMA_CC_PMU15_PLL_PC0_KPCTRL_MASK	0x07000000
+#define  BCMA_CC_PMU15_PLL_PC0_KPCTRL_SHIFT	24
+#define  BCMA_CC_PMU15_PLL_PC0_FCNTCTRL_MASK	0x38000000
+#define  BCMA_CC_PMU15_PLL_PC0_FCNTCTRL_SHIFT	27
+#define  BCMA_CC_PMU15_PLL_PC0_FDCMODE_MASK	0x40000000
+#define  BCMA_CC_PMU15_PLL_PC0_FDCMODE_SHIFT	30
+#define  BCMA_CC_PMU15_PLL_PC0_CTRLBIAS_MASK	0x80000000
+#define  BCMA_CC_PMU15_PLL_PC0_CTRLBIAS_SHIFT	31
+
 /* ALP clock on pre-PMU chips */
 #define BCMA_CC_PMU_ALP_CLOCK		20000000
 /* HT clock for systems with PMU-enabled chipcommon */
@@ -415,6 +524,44 @@
 /* 4313 Chip specific ChipControl register bits */
 #define BCMA_CCTRL_4313_12MA_LED_DRIVE		0x00000007	/* 12 mA drive strengh for later 4313 */
 
+/* BCM5357 ChipControl register bits */
+#define BCMA_CHIPCTL_5357_EXTPA			BIT(14)
+#define BCMA_CHIPCTL_5357_ANT_MUX_2O3		BIT(15)
+#define BCMA_CHIPCTL_5357_NFLASH		BIT(16)
+#define BCMA_CHIPCTL_5357_I2S_PINS_ENABLE	BIT(18)
+#define BCMA_CHIPCTL_5357_I2CSPI_PINS_ENABLE	BIT(19)
+
+#define BCMA_RES_4314_LPLDO_PU			BIT(0)
+#define BCMA_RES_4314_PMU_SLEEP_DIS		BIT(1)
+#define BCMA_RES_4314_PMU_BG_PU			BIT(2)
+#define BCMA_RES_4314_CBUCK_LPOM_PU		BIT(3)
+#define BCMA_RES_4314_CBUCK_PFM_PU		BIT(4)
+#define BCMA_RES_4314_CLDO_PU			BIT(5)
+#define BCMA_RES_4314_LPLDO2_LVM		BIT(6)
+#define BCMA_RES_4314_WL_PMU_PU			BIT(7)
+#define BCMA_RES_4314_LNLDO_PU			BIT(8)
+#define BCMA_RES_4314_LDO3P3_PU			BIT(9)
+#define BCMA_RES_4314_OTP_PU			BIT(10)
+#define BCMA_RES_4314_XTAL_PU			BIT(11)
+#define BCMA_RES_4314_WL_PWRSW_PU		BIT(12)
+#define BCMA_RES_4314_LQ_AVAIL			BIT(13)
+#define BCMA_RES_4314_LOGIC_RET			BIT(14)
+#define BCMA_RES_4314_MEM_SLEEP			BIT(15)
+#define BCMA_RES_4314_MACPHY_RET		BIT(16)
+#define BCMA_RES_4314_WL_CORE_READY		BIT(17)
+#define BCMA_RES_4314_ILP_REQ			BIT(18)
+#define BCMA_RES_4314_ALP_AVAIL			BIT(19)
+#define BCMA_RES_4314_MISC_PWRSW_PU		BIT(20)
+#define BCMA_RES_4314_SYNTH_PWRSW_PU		BIT(21)
+#define BCMA_RES_4314_RX_PWRSW_PU		BIT(22)
+#define BCMA_RES_4314_RADIO_PU			BIT(23)
+#define BCMA_RES_4314_VCO_LDO_PU		BIT(24)
+#define BCMA_RES_4314_AFE_LDO_PU		BIT(25)
+#define BCMA_RES_4314_RX_LDO_PU			BIT(26)
+#define BCMA_RES_4314_TX_LDO_PU			BIT(27)
+#define BCMA_RES_4314_HT_AVAIL			BIT(28)
+#define BCMA_RES_4314_MACPHY_CLK_AVAIL		BIT(29)
+
 /* Data for the PMU, if available.
  * Check availability with ((struct bcma_chipcommon)->capabilities & BCMA_CC_CAP_PMU)
  */
@@ -425,11 +572,36 @@ struct bcma_chipcommon_pmu {
 
 #ifdef CONFIG_BCMA_DRIVER_MIPS
 struct bcma_pflash {
+	bool present;
 	u8 buswidth;
 	u32 window;
 	u32 window_size;
 };
 
+#ifdef CONFIG_BCMA_SFLASH
+struct bcma_sflash {
+	bool present;
+	u32 window;
+	u32 blocksize;
+	u16 numblocks;
+	u32 size;
+
+	struct mtd_info *mtd;
+	void *priv;
+};
+#endif
+
+#ifdef CONFIG_BCMA_NFLASH
+struct mtd_info;
+
+struct bcma_nflash {
+	bool present;
+	bool boot;		/* This is the flash the SoC boots from */
+
+	struct mtd_info *mtd;
+};
+#endif
+
 struct bcma_serial_port {
 	void *regs;
 	unsigned long clockspeed;
@@ -445,15 +617,30 @@ struct bcma_drv_cc {
 	u32 capabilities;
 	u32 capabilities_ext;
 	u8 setup_done:1;
+	u8 early_setup_done:1;
 	/* Fast Powerup Delay constant */
 	u16 fast_pwrup_delay;
 	struct bcma_chipcommon_pmu pmu;
 #ifdef CONFIG_BCMA_DRIVER_MIPS
 	struct bcma_pflash pflash;
+#ifdef CONFIG_BCMA_SFLASH
+	struct bcma_sflash sflash;
+#endif
+#ifdef CONFIG_BCMA_NFLASH
+	struct bcma_nflash nflash;
+#endif
 
 	int nr_serial_ports;
 	struct bcma_serial_port serial_ports[4];
 #endif /* CONFIG_BCMA_DRIVER_MIPS */
+	u32 ticks_per_ms;
+	struct platform_device *watchdog;
+
+	/* Lock for GPIO register access. */
+	spinlock_t gpio_lock;
+#ifdef CONFIG_BCMA_DRIVER_GPIO
+	struct gpio_chip gpio;
+#endif
 };
 
 /* Register access */
@@ -470,14 +657,16 @@ struct bcma_drv_cc {
 	bcma_cc_write32(cc, offset, (bcma_cc_read32(cc, offset) & (mask)) | (set))
 
 extern void bcma_core_chipcommon_init(struct bcma_drv_cc *cc);
+extern void bcma_core_chipcommon_early_init(struct bcma_drv_cc *cc);
 
 extern void bcma_chipco_suspend(struct bcma_drv_cc *cc);
 extern void bcma_chipco_resume(struct bcma_drv_cc *cc);
 
 void bcma_chipco_bcm4331_ext_pa_lines_ctl(struct bcma_drv_cc *cc, bool enable);
 
-extern void bcma_chipco_watchdog_timer_set(struct bcma_drv_cc *cc,
-					  u32 ticks);
+extern u32 bcma_chipco_watchdog_timer_set(struct bcma_drv_cc *cc, u32 ticks);
+
+extern u32 bcma_chipco_get_alp_clock(struct bcma_drv_cc *cc);
 
 void bcma_chipco_irq_mask(struct bcma_drv_cc *cc, u32 mask, u32 value);
 
@@ -490,9 +679,12 @@ u32 bcma_chipco_gpio_outen(struct bcma_d
 u32 bcma_chipco_gpio_control(struct bcma_drv_cc *cc, u32 mask, u32 value);
 u32 bcma_chipco_gpio_intmask(struct bcma_drv_cc *cc, u32 mask, u32 value);
 u32 bcma_chipco_gpio_polarity(struct bcma_drv_cc *cc, u32 mask, u32 value);
+u32 bcma_chipco_gpio_pullup(struct bcma_drv_cc *cc, u32 mask, u32 value);
+u32 bcma_chipco_gpio_pulldown(struct bcma_drv_cc *cc, u32 mask, u32 value);
 
 /* PMU support */
 extern void bcma_pmu_init(struct bcma_drv_cc *cc);
+extern void bcma_pmu_early_init(struct bcma_drv_cc *cc);
 
 extern void bcma_chipco_pll_write(struct bcma_drv_cc *cc, u32 offset,
 				  u32 value);
@@ -504,4 +696,6 @@ extern void bcma_chipco_regctl_maskset(s
 				       u32 offset, u32 mask, u32 set);
 extern void bcma_pmu_spuravoid_pllupdate(struct bcma_drv_cc *cc, int spuravoid);
 
+extern u32 bcma_pmu_get_bus_clock(struct bcma_drv_cc *cc);
+
 #endif /* LINUX_BCMA_DRIVER_CC_H_ */
--- a/include/linux/bcma/bcma_driver_mips.h
+++ b/include/linux/bcma/bcma_driver_mips.h
@@ -28,6 +28,7 @@
 #define BCMA_MIPS_MIPS74K_GPIOEN	0x0048
 #define BCMA_MIPS_MIPS74K_CLKCTLST	0x01E0
 
+#define BCMA_MIPS_OOBSELINA74		0x004
 #define BCMA_MIPS_OOBSELOUTA30		0x100
 
 struct bcma_device;
@@ -35,17 +36,24 @@ struct bcma_device;
 struct bcma_drv_mips {
 	struct bcma_device *core;
 	u8 setup_done:1;
-	unsigned int assigned_irqs;
+	u8 early_setup_done:1;
 };
 
 #ifdef CONFIG_BCMA_DRIVER_MIPS
 extern void bcma_core_mips_init(struct bcma_drv_mips *mcore);
+extern void bcma_core_mips_early_init(struct bcma_drv_mips *mcore);
+
+extern unsigned int bcma_core_irq(struct bcma_device *core);
 #else
 static inline void bcma_core_mips_init(struct bcma_drv_mips *mcore) { }
+static inline void bcma_core_mips_early_init(struct bcma_drv_mips *mcore) { }
+
+static inline unsigned int bcma_core_irq(struct bcma_device *core)
+{
+	return 0;
+}
 #endif
 
 extern u32 bcma_cpu_clock(struct bcma_drv_mips *mcore);
 
-extern unsigned int bcma_core_mips_irq(struct bcma_device *dev);
-
 #endif /* LINUX_BCMA_DRIVER_MIPS_H_ */
--- a/include/linux/bcma/bcma_driver_pci.h
+++ b/include/linux/bcma/bcma_driver_pci.h
@@ -179,10 +179,33 @@ struct pci_dev;
 #define BCMA_CORE_PCI_CFG_FUN_MASK		7	/* Function mask */
 #define BCMA_CORE_PCI_CFG_OFF_MASK		0xfff	/* Register mask */
 
+#define BCMA_CORE_PCI_CFG_DEVCTRL		0xd8
+
+#define BCMA_CORE_PCI_
+
+/* MDIO devices (SERDES modules) */
+#define BCMA_CORE_PCI_MDIO_IEEE0		0x000
+#define BCMA_CORE_PCI_MDIO_IEEE1		0x001
+#define BCMA_CORE_PCI_MDIO_BLK0			0x800
+#define BCMA_CORE_PCI_MDIO_BLK1			0x801
+#define  BCMA_CORE_PCI_MDIO_BLK1_MGMT0		0x16
+#define  BCMA_CORE_PCI_MDIO_BLK1_MGMT1		0x17
+#define  BCMA_CORE_PCI_MDIO_BLK1_MGMT2		0x18
+#define  BCMA_CORE_PCI_MDIO_BLK1_MGMT3		0x19
+#define  BCMA_CORE_PCI_MDIO_BLK1_MGMT4		0x1A
+#define BCMA_CORE_PCI_MDIO_BLK2			0x802
+#define BCMA_CORE_PCI_MDIO_BLK3			0x803
+#define BCMA_CORE_PCI_MDIO_BLK4			0x804
+#define BCMA_CORE_PCI_MDIO_TXPLL		0x808	/* TXPLL register block idx */
+#define BCMA_CORE_PCI_MDIO_TXCTRL0		0x820
+#define BCMA_CORE_PCI_MDIO_SERDESID		0x831
+#define BCMA_CORE_PCI_MDIO_RXCTRL0		0x840
+
 /* PCIE Root Capability Register bits (Host mode only) */
 #define BCMA_CORE_PCI_RC_CRS_VISIBILITY		0x0001
 
 struct bcma_drv_pci;
+struct bcma_bus;
 
 #ifdef CONFIG_BCMA_DRIVER_PCI_HOSTMODE
 struct bcma_drv_pci_host {
@@ -217,7 +240,9 @@ struct bcma_drv_pci {
 extern void __devinit bcma_core_pci_init(struct bcma_drv_pci *pc);
 extern int bcma_core_pci_irq_ctl(struct bcma_drv_pci *pc,
 				 struct bcma_device *core, bool enable);
-extern void bcma_core_pci_extend_L1timer(struct bcma_drv_pci *pc, bool extend);
+extern void bcma_core_pci_up(struct bcma_bus *bus);
+extern void bcma_core_pci_down(struct bcma_bus *bus);
+extern void bcma_core_pci_power_save(struct bcma_bus *bus, bool up);
 
 extern int bcma_core_pci_pcibios_map_irq(const struct pci_dev *dev);
 extern int bcma_core_pci_plat_dev_init(struct pci_dev *dev);
--- a/include/linux/bcma/bcma_regs.h
+++ b/include/linux/bcma/bcma_regs.h
@@ -11,11 +11,13 @@
 #define  BCMA_CLKCTLST_HAVEHTREQ	0x00000010 /* HT available request */
 #define  BCMA_CLKCTLST_HWCROFF		0x00000020 /* Force HW clock request off */
 #define  BCMA_CLKCTLST_EXTRESREQ	0x00000700 /* Mask of external resource requests */
+#define  BCMA_CLKCTLST_EXTRESREQ_SHIFT	8
 #define  BCMA_CLKCTLST_HAVEALP		0x00010000 /* ALP available */
 #define  BCMA_CLKCTLST_HAVEHT		0x00020000 /* HT available */
 #define  BCMA_CLKCTLST_BP_ON_ALP	0x00040000 /* RO: running on ALP clock */
 #define  BCMA_CLKCTLST_BP_ON_HT		0x00080000 /* RO: running on HT clock */
 #define  BCMA_CLKCTLST_EXTRESST		0x07000000 /* Mask of external resource status */
+#define  BCMA_CLKCTLST_EXTRESST_SHIFT	24
 /* Is there any BCM4328 on BCMA bus? */
 #define  BCMA_CLKCTLST_4328A0_HAVEHT	0x00010000 /* 4328a0 has reversed bits */
 #define  BCMA_CLKCTLST_4328A0_HAVEALP	0x00020000 /* 4328a0 has reversed bits */
@@ -35,6 +37,7 @@
 #define  BCMA_IOST_BIST_DONE		0x8000
 #define BCMA_RESET_CTL			0x0800
 #define  BCMA_RESET_CTL_RESET		0x0001
+#define BCMA_RESET_ST			0x0804
 
 /* BCMA PCI config space registers. */
 #define BCMA_PCI_PMCSR			0x44
@@ -83,4 +86,9 @@
 							 * (2 ZettaBytes), high 32 bits
 							 */
 
+#define BCMA_SOC_FLASH1			0x1fc00000	/* MIPS Flash Region 1 */
+#define BCMA_SOC_FLASH1_SZ		0x00400000	/* MIPS Size of Flash Region 1 */
+#define BCMA_SOC_FLASH2			0x1c000000	/* Flash Region 2 (region 1 shadowed here) */
+#define BCMA_SOC_FLASH2_SZ		0x02000000	/* Size of Flash Region 2 */
+
 #endif /* LINUX_BCMA_REGS_H_ */
--- a/drivers/net/wireless/b43/main.c
+++ b/drivers/net/wireless/b43/main.c
@@ -4622,7 +4622,7 @@ static int b43_wireless_core_init(struct
 	switch (dev->dev->bus_type) {
 #ifdef CONFIG_B43_BCMA
 	case B43_BUS_BCMA:
-		bcma_core_pci_irq_ctl(&dev->dev->bdev->bus->drv_pci,
+		bcma_core_pci_irq_ctl(&dev->dev->bdev->bus->drv_pci[0],
 				      dev->dev->bdev, true);
 		break;
 #endif
--- a/drivers/net/wireless/brcm80211/brcmsmac/aiutils.c
+++ b/drivers/net/wireless/brcm80211/brcmsmac/aiutils.c
@@ -688,27 +688,6 @@ bool ai_clkctl_cc(struct si_pub *sih, en
 	return mode == BCMA_CLKMODE_FAST;
 }
 
-void ai_pci_up(struct si_pub *sih)
-{
-	struct si_info *sii;
-
-	sii = container_of(sih, struct si_info, pub);
-
-	if (sii->icbus->hosttype == BCMA_HOSTTYPE_PCI)
-		bcma_core_pci_extend_L1timer(&sii->icbus->drv_pci, true);
-}
-
-/* Unconfigure and/or apply various WARs when going down */
-void ai_pci_down(struct si_pub *sih)
-{
-	struct si_info *sii;
-
-	sii = container_of(sih, struct si_info, pub);
-
-	if (sii->icbus->hosttype == BCMA_HOSTTYPE_PCI)
-		bcma_core_pci_extend_L1timer(&sii->icbus->drv_pci, false);
-}
-
 /* Enable BT-COEX & Ex-PA for 4313 */
 void ai_epa_4313war(struct si_pub *sih)
 {
--- a/drivers/net/wireless/brcm80211/brcmsmac/main.c
+++ b/drivers/net/wireless/brcm80211/brcmsmac/main.c
@@ -4689,7 +4689,7 @@ static int brcms_b_attach(struct brcms_c
 	brcms_c_coredisable(wlc_hw);
 
 	/* Match driver "down" state */
-	ai_pci_down(wlc_hw->sih);
+	bcma_core_pci_down(wlc_hw->d11core->bus);
 
 	/* turn off pll and xtal to match driver "down" state */
 	brcms_b_xtal(wlc_hw, OFF);
@@ -5077,7 +5077,7 @@ static int brcms_b_up_prep(struct brcms_
 	 * Configure pci/pcmcia here instead of in brcms_c_attach()
 	 * to allow mfg hotswap:  down, hotswap (chip power cycle), up.
 	 */
-	bcma_core_pci_irq_ctl(&wlc_hw->d11core->bus->drv_pci, wlc_hw->d11core,
+	bcma_core_pci_irq_ctl(&wlc_hw->d11core->bus->drv_pci[0], wlc_hw->d11core,
 			      true);
 
 	/*
@@ -5087,12 +5087,12 @@ static int brcms_b_up_prep(struct brcms_
 	 */
 	if (brcms_b_radio_read_hwdisabled(wlc_hw)) {
 		/* put SB PCI in down state again */
-		ai_pci_down(wlc_hw->sih);
+		bcma_core_pci_down(wlc_hw->d11core->bus);
 		brcms_b_xtal(wlc_hw, OFF);
 		return -ENOMEDIUM;
 	}
 
-	ai_pci_up(wlc_hw->sih);
+	bcma_core_pci_up(wlc_hw->d11core->bus);
 
 	/* reset the d11 core */
 	brcms_b_corereset(wlc_hw, BRCMS_USE_COREFLAGS);
@@ -5295,7 +5295,7 @@ static int brcms_b_down_finish(struct br
 
 		/* turn off primary xtal and pll */
 		if (!wlc_hw->noreset) {
-			ai_pci_down(wlc_hw->sih);
+			bcma_core_pci_down(wlc_hw->d11core->bus);
 			brcms_b_xtal(wlc_hw, OFF);
 		}
 	}
--- a/drivers/net/wireless/brcm80211/brcmsmac/aiutils.h
+++ b/drivers/net/wireless/brcm80211/brcmsmac/aiutils.h
@@ -183,9 +183,6 @@ extern u16 ai_clkctl_fast_pwrup_delay(st
 extern bool ai_clkctl_cc(struct si_pub *sih, enum bcma_clkmode mode);
 extern bool ai_deviceremoved(struct si_pub *sih);
 
-extern void ai_pci_down(struct si_pub *sih);
-extern void ai_pci_up(struct si_pub *sih);
-
 /* Enable Ex-PA for 4313 */
 extern void ai_epa_4313war(struct si_pub *sih);
 
