From 22a3eff19679e0e592e061201690670a2f5fdba7 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime.ripard@free-electrons.com>
Date: Thu, 7 Nov 2013 12:01:48 +0100
Subject: [PATCH] ARM: sun5i: a13: Add support for the High Speed Timers
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

The Allwinner A13 has support for two high speed timers. Now that we
have a driver to support it, we can enable them in the device tree.

Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
Tested-by: Emilio López <emilio@elopez.com.ar>
Signed-off-by: Daniel Lezcano <daniel.lezcano@linaro.org>
---
 arch/arm/boot/dts/sun5i-a13.dtsi | 7 +++++++
 1 file changed, 7 insertions(+)

diff --git a/arch/arm/boot/dts/sun5i-a13.dtsi b/arch/arm/boot/dts/sun5i-a13.dtsi
index ce8ef2a..1ccd75d 100644
--- a/arch/arm/boot/dts/sun5i-a13.dtsi
+++ b/arch/arm/boot/dts/sun5i-a13.dtsi
@@ -273,5 +273,12 @@
 			clock-frequency = <100000>;
 			status = "disabled";
 		};
+
+		timer@01c60000 {
+			compatible = "allwinner,sun5i-a13-hstimer";
+			reg = <0x01c60000 0x1000>;
+			interrupts = <82>, <83>;
+			clocks = <&ahb_gates 28>;
+		};
 	};
 };
-- 
1.8.5.1

