###############################################################################
# Proxmox VE host performance assessment  (READ-ONLY)
# Host:      pfv-tsys4 (pfv-tsys4.knel.net)
# FQDN:      pfv-tsys4.knel.net
# All IPs:   100.70.77.93 192.168.3.191 10.100.100.4 fd7a:115c:a1e0::3f3b:4d5d 
# Collected: 2026-07-29T10:09:07Z (UTC)
# Kernel:    6.17.9-1-pve
# Machine:   x86_64 GNU/Linux
# Caller:    root (uid=0)
# Script:    check.sh  -  strictly READ-ONLY
###############################################################################

###############################################################################
# 1. TOOL AVAILABILITY MATRIX
###############################################################################

--- command presence + path + version
    $ # Each line: name | present? | path | version
printf '%-22s %-8s %-30s %s\n' "TOOL" "PRESENT" "PATH" "VERSION/NOTE"
printf '%-22s %-8s %-30s %s\n' "----" "-------" "----" "------------"
for t in \
    pveversion pvecm qm pct pvesm pvesh pveperf proxmox-backup-client \
    ip ss ethtool bridge brctl nmcli \
    tcpdump mtr nstat netstat nicstat ifstat \
    dmidecode lscpu lshw hwinfo inxi lspci lsusb numactl numastat \
    cpupower turbostat x86_energy_perf_policy rdmsr \
    tuned-adm irqbalance \
    zpool zfs zdb arcstat arc_summary \
    lsblk blkid blockdev findmnt smartctl nvme hdparm \
    storcli storcli64 MegaCli MegaCli64 tw-cli arcconf \
    sas2ircu sas3ircu hpssacli ssacli perccli \
    multipath pvs vgs lvs lvdisplay \
    xfs_info dumpe2fs btrfs \
    fio iperf iperf3 sysbench bonnie++ iozone \
    iostat mpstat pidstat sar vmstat \
    top htop atop glances dstat nethogs iftop iotop smem pmap slabtop \
    perf strace lsof fatrace \
    dig host nslookup \
    chronyc ntpq timedatectl \
    nft iptables iptables-save ipset ufw \
    jq bc awk smartctl nvme \
    apt dpkg
do
    p="$(command -v "$t" 2>/dev/null)"
    if [ -n "$p" ]; then
        v=""
        case "$t" in
            zpool|zfs)        v="$(timeout 3 "$t" version 2>/dev/null | head -n 2 | tr '\n' ' ')" ;;
            iperf3|fio|sysbench|smartctl|nvme|tuned-adm|ethtool|cpupower)
                v="$(timeout 3 "$t" --version 2>&1 | head -n 1)" ;;
            pveversion)       v="$(timeout 3 "$t" 2>/dev/null)" ;;
            storcli64|storcli|MegaCli64|MegaCli|arcconf|sas2ircu|sas3ircu|ssacli|hpssacli)
                v="(storage HBA CLI - present)" ;;
        esac
        printf '%-22s %-8s %-30s %s\n' "$t" "yes" "$p" "$v"
    else
        printf '%-22s %-8s %-30s %s\n' "$t" "no" "-" "-"
    fi
done
TOOL                   PRESENT  PATH                           VERSION/NOTE
----                   -------  ----                           ------------
pveversion             yes      /usr/bin/pveversion            pve-manager/9.1.5/80cf92a64bef6889 (running kernel: 6.17.9-1-pve)
pvecm                  yes      /usr/bin/pvecm                 
qm                     yes      /usr/sbin/qm                   
pct                    yes      /usr/sbin/pct                  
pvesm                  yes      /usr/sbin/pvesm                
pvesh                  yes      /usr/bin/pvesh                 
pveperf                yes      /usr/bin/pveperf               
proxmox-backup-client  yes      /usr/bin/proxmox-backup-client 
ip                     yes      /usr/sbin/ip                   
ss                     yes      /usr/bin/ss                    
ethtool                yes      /usr/sbin/ethtool              ethtool version 6.14.2
bridge                 yes      /usr/sbin/bridge               
brctl                  yes      /usr/sbin/brctl                
nmcli                  no       -                              -
tcpdump                yes      /usr/bin/tcpdump               
mtr                    no       -                              -
nstat                  yes      /usr/bin/nstat                 
netstat                yes      /usr/bin/netstat               
nicstat                no       -                              -
ifstat                 no       -                              -
dmidecode              yes      /usr/sbin/dmidecode            
lscpu                  yes      /usr/bin/lscpu                 
lshw                   yes      /usr/bin/lshw                  
hwinfo                 no       -                              -
inxi                   no       -                              -
lspci                  yes      /usr/bin/lspci                 
lsusb                  yes      /usr/bin/lsusb                 
numactl                no       -                              -
numastat               no       -                              -
cpupower               yes      /usr/bin/cpupower              cpupower 6.12
turbostat              yes      /usr/sbin/turbostat            
x86_energy_perf_policy yes      /usr/sbin/x86_energy_perf_policy 
rdmsr                  no       -                              -
tuned-adm              yes      /usr/sbin/tuned-adm            
irqbalance             no       -                              -
zpool                  yes      /usr/sbin/zpool                zfs-2.4.0-pve1 zfs-kmod-2.4.0-pve1 
zfs                    yes      /usr/sbin/zfs                  zfs-2.4.0-pve1 zfs-kmod-2.4.0-pve1 
zdb                    yes      /usr/sbin/zdb                  
arcstat                no       -                              -
arc_summary            no       -                              -
lsblk                  yes      /usr/bin/lsblk                 
blkid                  yes      /usr/sbin/blkid                
blockdev               yes      /usr/sbin/blockdev             
findmnt                yes      /usr/bin/findmnt               
smartctl               yes      /usr/sbin/smartctl             smartctl 7.4 2024-10-15 r5620 [x86_64-linux-6.17.9-1-pve] (local build)
nvme                   no       -                              -
hdparm                 yes      /usr/sbin/hdparm               
storcli                no       -                              -
storcli64              no       -                              -
MegaCli                no       -                              -
MegaCli64              no       -                              -
tw-cli                 no       -                              -
arcconf                no       -                              -
sas2ircu               no       -                              -
sas3ircu               no       -                              -
hpssacli               no       -                              -
ssacli                 no       -                              -
perccli                no       -                              -
multipath              no       -                              -
pvs                    yes      /usr/sbin/pvs                  
vgs                    yes      /usr/sbin/vgs                  
lvs                    yes      /usr/sbin/lvs                  
lvdisplay              yes      /usr/sbin/lvdisplay            
xfs_info               yes      /usr/sbin/xfs_info             
dumpe2fs               yes      /usr/sbin/dumpe2fs             
btrfs                  yes      /usr/bin/btrfs                 
fio                    no       -                              -
iperf                  no       -                              -
iperf3                 yes      /usr/bin/iperf3                iperf 3.18 (cJSON 1.7.15)
sysbench               no       -                              -
bonnie++               no       -                              -
iozone                 no       -                              -
iostat                 yes      /usr/bin/iostat                
mpstat                 yes      /usr/bin/mpstat                
pidstat                yes      /usr/bin/pidstat               
sar                    yes      /usr/bin/sar                   
vmstat                 yes      /usr/bin/vmstat                
top                    yes      /usr/bin/top                   
htop                   yes      /usr/bin/htop                  
atop                   no       -                              -
glances                yes      /usr/bin/glances               
dstat                  no       -                              -
nethogs                no       -                              -
iftop                  no       -                              -
iotop                  yes      /usr/sbin/iotop                
smem                   no       -                              -
pmap                   yes      /usr/bin/pmap                  
slabtop                yes      /usr/bin/slabtop               
perf                   yes      /usr/bin/perf                  
strace                 yes      /usr/bin/strace                
lsof                   yes      /usr/bin/lsof                  
fatrace                no       -                              -
dig                    yes      /usr/bin/dig                   
host                   yes      /usr/bin/host                  
nslookup               yes      /usr/bin/nslookup              
chronyc                yes      /usr/bin/chronyc               
ntpq                   no       -                              -
timedatectl            yes      /usr/bin/timedatectl           
nft                    yes      /usr/sbin/nft                  
iptables               yes      /usr/sbin/iptables             
iptables-save          yes      /usr/sbin/iptables-save        
ipset                  yes      /usr/sbin/ipset                
ufw                    no       -                              -
jq                     no       -                              -
bc                     yes      /usr/bin/bc                    
awk                    yes      /usr/bin/awk                   
smartctl               yes      /usr/sbin/smartctl             smartctl 7.4 2024-10-15 r5620 [x86_64-linux-6.17.9-1-pve] (local build)
nvme                   no       -                              -
apt                    yes      /usr/bin/apt                   
dpkg                   yes      /usr/bin/dpkg                  

--- Debian packages relevant to perf/storage/net
    $ dpkg -l 2>/dev/null | awk '/^ii/ && ($2 ~ /^(proxmox-|pve-|zfs|zfsutils|nfs|nfs-kernel-server|nfs-common|open-iscsi|ceph|tuned|irqbalance|sysstat|smartmontools|nvme-cli|ethtool|bridge-utils|ifenslave|fio|iperf3|sysbench|glances|htop|atop|lm-sensors|numactl|cpufrequtils|linux-image-|pve-kernel|qemu|libvirt|corosync|pacemaker)/) {print $2"  "$3}' | head -n 80
bridge-utils  1.7.1-4+b1
ceph-common  19.2.3-pve2
ceph-fuse  19.2.3-pve2
corosync  3.1.9-pve2
ethtool  1:6.14.2-1
glances  4.3.1+dfsg-1
htop  3.4.1-5
ifenslave  2.14
iperf3  3.18-2+deb13u2
libvirt-common  11.3.0-3+deb13u2
libvirt0:amd64  11.3.0-3+deb13u2
nfs-common  1:2.8.3-1
nfs-kernel-server  1:2.8.3-1
open-iscsi  2.1.11-1+deb13u1
proxmox-archive-keyring  4.0
proxmox-backup-client  4.1.2-1
proxmox-backup-file-restore  4.1.2-1
proxmox-backup-restore-image  1.0.0
proxmox-default-kernel  2.0.2
proxmox-firewall  1.2.1
proxmox-kernel-6.17  6.17.9-1
proxmox-kernel-6.17.2-1-pve-signed  6.17.2-1
proxmox-kernel-6.17.9-1-pve-signed  6.17.9-1
proxmox-kernel-helper  9.0.4
proxmox-mail-forward  1.0.2
proxmox-mini-journalreader  1.6
proxmox-offline-mirror-docs  0.7.3
proxmox-offline-mirror-helper  0.7.3
proxmox-termproxy  2.0.3
proxmox-ve  9.1.0
proxmox-websocket-tunnel  1.0.0
proxmox-widget-toolkit  5.1.5
pve-cluster  9.0.7
pve-container  6.1.1
pve-docs  9.1.2
pve-edk2-firmware  4.2025.05-2
pve-edk2-firmware-legacy  4.2025.05-2
pve-edk2-firmware-ovmf  4.2025.05-2
pve-esxi-import-tools  1.0.1
pve-firewall  6.0.4
pve-firmware  3.17-2
pve-ha-manager  5.1.0
pve-i18n  3.6.6
pve-lxc-syscalld  2.0.2
pve-manager  9.1.5
pve-nvidia-vgpu-helper  0.3.0
pve-qemu-kvm  10.1.2-6
pve-xtermjs  5.5.0-3
pve-yew-mobile-gui  0.6.4
pve-yew-mobile-i18n  3.6.6
qemu-server  9.1.4
smartmontools  7.4-pve1
sysstat  12.7.5-2
tuned  2.25.1-1
zfs-initramfs  2.4.0-pve1
zfs-zed  2.4.0-pve1
zfsutils-linux  2.4.0-pve1

--- kernel modules available (relevant to perf)
    $ for m in kvm_intel kvm_amd \
         ixgbe i40e i40iw ice igb igc mlx4_en mlx5_core mlx4_core bnx2x bnx2 tg3 be2net qed qede virtio_net \
         nvme nvme-tcp nvme-fabrics sd_mod sr_mod \
         zfs spl znvpair zcommon zunicode zavl icp zlua \
         megaraid_sas mpt3sas hpsa aacraid smartpqi isci \
         dm_multipath multipath \
         tcp_dctcp tcp_bbr tcp_cubic tcp_htcp \
         8021q bonding bridge br_netfilter \
         vhost_net vhost_scsi target_core_mod \
         nfsv4 nfsv3 rpcsec_gss_krb5
do
    modinfo "$m" >/dev/null 2>&1 && printf 'available : %s (%s)\n' "$m" "$(modinfo -F version "$m" 2>/dev/null || echo built-in)"
done
available : kvm_intel ()
available : kvm_amd ()
available : ixgbe ()
available : i40e ()
available : i40iw ()
available : ice ()
available : igb ()
available : igc ()
available : mlx4_en (4.0-0)
available : mlx5_core ()
available : mlx4_core (4.0-0)
available : bnx2x ()
available : bnx2 ()
available : tg3 ()
available : be2net ()
available : qed ()
available : qede ()
available : virtio_net ()
available : nvme (1.0)
available : nvme-tcp ()
available : nvme-fabrics ()
available : sd_mod ()
available : sr_mod ()
available : zfs (2.4.0-pve1)
available : spl (2.4.0-pve1)
available : znvpair (2.4.0-pve1)
available : zcommon (2.4.0-pve1)
available : zunicode (2.4.0-pve1)
available : zavl (2.4.0-pve1)
available : icp (2.4.0-pve1)
available : zlua (2.4.0-pve1)
available : megaraid_sas (07.734.00.00-rc1)
available : mpt3sas (52.100.00.00)
available : hpsa (3.4.20-200)
available : aacraid (1.2.1[50983]-custom)
available : smartpqi (2.1.34-035)
available : isci (1.2.0)
available : dm_multipath ()
available : tcp_dctcp ()
available : tcp_bbr ()
available : tcp_cubic (2.3)
available : tcp_htcp ()
available : 8021q (1.8)
available : bonding ()
available : bridge (2.3)
available : br_netfilter ()
available : vhost_net (0.0.1)
available : vhost_scsi ()
available : target_core_mod ()
available : nfsv4 ()
available : nfsv3 ()
available : rpcsec_gss_krb5 ()

--- currently loaded modules (filtered)
    $ lsmod | awk 'NR==1 || $1 ~ /^(kvm|virtio|vhost|ixgb|i40e|ice|igb|mlx|bnx|tg3|be2|qed|nvme|zfs|spl|z|dm_|megaraid|mpt|hpsa|aacraid|smartpqi|8021q|bonding|bridge|nfsv|tcp_|rpc|sunrpc|loop)/{print}'
Module                  Size  Used by
tcp_diag               12288  0
tcp_bbr                20480  56
bonding               245760  0
kvm_intel             532480  4
kvm                  1376256  3 kvm_intel
sunrpc                786432  51 nfsd,auth_rpcgss,lockd,nfs_acl
zfs                  6234112  6
spl                   151552  1 zfs
vhost_net              32768  1
vhost                  69632  1 vhost_net
vhost_iotlb            16384  1 vhost
dm_thin_pool           94208  2
dm_persistent_data    114688  1 dm_thin_pool
dm_bio_prison          24576  1 dm_thin_pool
dm_bufio               53248  1 dm_persistent_data

###############################################################################
# 2. OS / DISTRO / UPTIME
###############################################################################

--- os-release
    --- /etc/os-release ---
PRETTY_NAME="Debian GNU/Linux 13 (trixie)"
NAME="Debian GNU/Linux"
VERSION_ID="13"
VERSION="13 (trixie)"
VERSION_CODENAME=trixie
DEBIAN_VERSION_FULL=13.3
ID=debian
HOME_URL="https://www.debian.org/"
SUPPORT_URL="https://www.debian.org/support"
BUG_REPORT_URL="https://bugs.debian.org/"

--- debian version
    $ cat /etc/debian_version
13.3

--- uptime
    $ uptime
 05:09:15 up 4 days, 13:11,  3 users,  load average: 7.98, 7.06, 6.30

--- uptime raw (since boot)
    $ cat /proc/uptime
393071.37 2395613.87

--- last reboot
    $ last -x reboot
reboot   system boot  6.17.9-1-pve     Fri Jul 24 15:58 - still running
reboot   system boot  6.17.9-1-pve     Fri Jul 24 13:35 - 15:56  (02:20)
shutdown system down  6.17.9-1-pve     Fri Jul 24 15:56 - 15:58  (00:01)
reboot   system boot  6.17.9-1-pve     Fri Jul 24 13:26 - 13:34  (00:08)
shutdown system down  6.17.9-1-pve     Fri Jul 24 13:34 - 13:35  (00:00)
reboot   system boot  6.17.9-1-pve     Fri Jul 24 11:58 - 12:02  (00:03)
shutdown system down  6.17.9-1-pve     Fri Jul 24 12:02 - 13:26  (01:24)
reboot   system boot  6.17.9-1-pve     Fri Apr 24 08:17 - 11:08 (91+02:50)
shutdown system down  6.17.9-1-pve     Fri Jul 24 11:08 - 11:58  (00:49)
reboot   system boot  6.17.9-1-pve     Tue Apr  7 12:19 - 08:17 (16+19:57)
shutdown system down  6.17.9-1-pve     Fri Apr 24 08:17 - 08:17  (00:00)
reboot   system boot  6.17.9-1-pve     Sat Apr  4 09:57 - 12:18 (3+02:21)
shutdown system down  6.17.9-1-pve     Tue Apr  7 12:18 - 12:19  (00:01)
reboot   system boot  6.17.9-1-pve     Sat Apr  4 09:53 - 09:56  (00:02)
shutdown system down  6.17.9-1-pve     Sat Apr  4 09:56 - 09:57  (00:00)
reboot   system boot  6.17.9-1-pve     Sat Apr  4 09:46 - crash 
reboot   system boot  6.17.9-1-pve     Sat Apr  4 09:42 - crash 
reboot   system boot  6.17.9-1-pve     Mon Mar 30 16:51 - 09:41 (4+16:49)
shutdown system down  6.17.9-1-pve     Sat Apr  4 09:41 - 09:42  (00:01)
reboot   system boot  6.17.9-1-pve     Mon Mar 30 16:42 - 16:51  (00:08)
shutdown system down  6.17.9-1-pve     Mon Mar 30 16:51 - 16:51  (00:00)
reboot   system boot  6.17.9-1-pve     Mon Mar 30 16:27 - 16:42  (00:14)
shutdown system down  6.17.9-1-pve     Mon Mar 30 16:42 - 16:42  (00:00)
reboot   system boot  6.17.9-1-pve     Mon Mar 30 16:20 - 16:26  (00:05)
shutdown system down  6.17.9-1-pve     Mon Mar 30 16:26 - 16:27  (00:00)
reboot   system boot  6.17.9-1-pve     Mon Mar 30 16:03 - 16:20  (00:17)
shutdown system down  6.17.9-1-pve     Mon Mar 30 16:20 - 16:20  (00:00)
reboot   system boot  6.17.9-1-pve     Tue Mar 24 19:57 - 14:45 (5+18:48)
shutdown system down  6.17.9-1-pve     Mon Mar 30 14:45 - 16:03  (01:17)
reboot   system boot  6.17.9-1-pve     Sun Mar  8 14:24 - crash 
reboot   system boot  6.17.9-1-pve     Fri Mar  6 13:02 - 14:23 (2+00:21)
shutdown system down  6.17.9-1-pve     Sun Mar  8 14:23 - 14:24  (00:00)
reboot   system boot  6.17.9-1-pve     Fri Mar  6 12:40 - crash 
reboot   system boot  6.17.9-1-pve     Fri Mar  6 11:09 - 12:39  (01:30)
shutdown system down  6.17.9-1-pve     Fri Mar  6 12:39 - 12:40  (00:00)
reboot   system boot  6.17.9-1-pve     Thu Mar  5 12:27 - 11:06  (22:39)
shutdown system down  6.17.9-1-pve     Fri Mar  6 11:06 - 11:09  (00:02)
reboot   system boot  6.17.9-1-pve     Thu Mar  5 12:23 - 12:26  (00:02)
shutdown system down  6.17.9-1-pve     Thu Mar  5 12:26 - 12:27  (00:00)
reboot   system boot  6.17.9-1-pve     Thu Mar  5 10:05 - 11:58  (01:53)
shutdown system down  6.17.9-1-pve     Thu Mar  5 11:58 - 12:23  (00:25)
reboot   system boot  6.17.9-1-pve     Thu Mar  5 09:55 - 10:00  (00:05)
shutdown system down  6.17.9-1-pve     Thu Mar  5 10:00 - 10:05  (00:04)
reboot   system boot  6.17.9-1-pve     Wed Mar  4 10:51 - 09:55  (23:03)
shutdown system down  6.17.9-1-pve     Thu Mar  5 09:55 - 09:55  (00:00)
reboot   system boot  6.17.2-1-pve     Mon Feb 23 12:07 - 20:54 (8+08:46)
shutdown system down  6.17.2-1-pve     Tue Mar  3 20:54 - 10:51  (13:57)
reboot   system boot  6.17.2-1-pve     Mon Feb 23 11:48 - 12:07  (00:18)
shutdown system down  6.17.2-1-pve     Mon Feb 23 12:07 - 12:07  (00:00)
reboot   system boot  6.17.2-1-pve     Mon Feb 23 11:38 - 11:46  (00:07)
shutdown system down  6.17.2-1-pve     Mon Feb 23 11:46 - 11:48  (00:02)
reboot   system boot  6.17.2-1-pve     Mon Feb 23 11:36 - 11:37  (00:01)
shutdown system down  6.17.2-1-pve     Mon Feb 23 11:37 - 11:38  (00:00)
reboot   system boot  6.17.2-1-pve     Mon Feb 23 11:19 - 11:31  (00:11)
shutdown system down  6.17.2-1-pve     Mon Feb 23 11:31 - 11:36  (00:04)
reboot   system boot  6.17.2-1-pve     Mon Feb 23 10:52 - 11:14  (00:21)
shutdown system down  6.17.2-1-pve     Mon Feb 23 11:14 - 11:19  (00:05)

wtmpdb begins Mon Feb 23 10:52:50 2026

--- last logins
    $ last
root     pts/0        100.87.49.37     Tue Jul 28 20:00 - 20:00  (00:00)
root     pts/0        100.87.49.37     Tue Jul 28 19:38 - 19:38  (00:00)
root     pts/0        100.87.49.37     Mon Jul 27 13:08 - 13:13  (00:04)
root     pts/0        100.87.49.37     Mon Jul 27 12:50 - 13:06  (00:16)
root     pts/0        100.87.49.37     Mon Jul 27 10:54 - 11:12  (00:17)
root     pts/0        100.87.49.37     Mon Jul 27 10:47 - 10:52  (00:04)
root     pts/0        100.87.49.37     Sun Jul 26 16:29 - 17:02  (00:33)
root     pts/0        100.87.49.37     Sun Jul 26 15:45 - 15:45  (00:00)
root     pts/0        100.87.49.37     Sun Jul 26 15:11 - 15:39  (00:27)
root     pts/1        100.87.49.37     Sun Jul 26 14:41 - 14:54  (00:12)
root     pts/0        100.87.49.37     Sun Jul 26 14:28 - 15:06  (00:37)
root     pts/0        100.87.49.37     Sun Jul 26 13:20 - 13:33  (00:12)
root     pts/0        100.87.49.37     Sun Jul 26 12:24 - 12:24  (00:00)
root     pts/0        100.87.49.37     Sat Jul 25 11:25 - 11:32  (00:07)
root     pts/0        100.87.49.37     Sat Jul 25 10:42 - 10:43  (00:01)
root     pts/0        100.87.49.37     Fri Jul 24 22:47 - 22:51  (00:04)
root     pts/1        100.87.49.37     Fri Jul 24 22:16 - 22:17  (00:01)
root     pts/0        100.87.49.37     Fri Jul 24 22:15 - 22:18  (00:02)
root     pts/0        100.87.49.37     Fri Jul 24 18:14 - 18:22  (00:07)
root     pts/0        100.87.49.37     Fri Jul 24 17:35 - 17:38  (00:02)
root     pts/0        100.87.49.37     Fri Jul 24 17:35 - 17:35  (00:00)
root     pts/0        100.87.49.37     Fri Jul 24 17:19 - 17:19  (00:00)
root     pts/0        100.87.49.37     Fri Jul 24 17:03 - 17:08  (00:05)
root     pts/0        100.87.49.37     Fri Jul 24 16:31 - 16:31  (00:00)
root     tty1                          Fri Jul 24 16:09 - 16:10  (00:00)
reboot   system boot  6.17.9-1-pve     Fri Jul 24 15:58 - still running
root     pts/0        100.87.49.37     Fri Jul 24 15:23 - 15:30  (00:07)
root     pts/0        100.87.49.37     Fri Jul 24 13:52 - 13:59  (00:06)
root     tty1                          Fri Jul 24 13:36 - 13:37  (00:00)
reboot   system boot  6.17.9-1-pve     Fri Jul 24 13:35 - 15:56  (02:20)
root     tty1                          Fri Jul 24 13:28 - 13:34  (00:06)
reboot   system boot  6.17.9-1-pve     Fri Jul 24 13:26 - 13:34  (00:08)
reboot   system boot  6.17.9-1-pve     Fri Jul 24 11:58 - 12:02  (00:03)
root     pts/0        100.87.49.37     Thu Jul 23 13:07 - 13:18  (00:11)
root     pts/1        100.87.49.37     Wed Jul 22 20:08 - 20:08  (00:00)
root     pts/1        100.87.49.37     Wed Jul 22 19:04 - 19:16  (00:11)
root     pts/1        100.87.49.37     Wed Jul 22 18:39 - 18:51  (00:12)
root     pts/1        100.87.49.37     Wed Jul 22 18:34 - 18:37  (00:02)
root     pts/0        100.87.49.37     Wed Jul 22 18:26 - 20:30  (02:03)
root     pts/0        100.87.49.37     Wed Jul 22 17:48 - 17:52  (00:03)
root     pts/0        100.87.49.37     Wed Jul 22 17:45 - 17:47  (00:01)
root     pts/1        100.87.49.37     Mon Jul 20 20:03 - 20:05  (00:02)
root     pts/0        100.87.49.37     Mon Jul 20 20:02 - 20:05  (00:03)
root     pts/0        100.87.49.37     Mon Jul 20 20:02 - 20:02  (00:00)
root     pts/0        100.87.49.37     Mon Jul 20 19:17 - 19:19  (00:02)
root     pts/0        100.87.49.37     Mon Jul 20 19:06 - 19:16  (00:10)
root     pts/1        100.87.49.37     Mon Jul 20 19:02 - 19:17  (00:15)
root     pts/1        100.87.49.37     Mon Jul 20 18:40 - 19:02  (00:21)
root     pts/3        100.87.49.37     Mon Jul 20 12:27 - 12:28  (00:00)
root     pts/1        100.109.70.137   Mon Jul 20 12:26 - 17:16  (04:50)
root     pts/1        100.87.49.37     Mon Jul 20 11:28 - 11:29  (00:00)
root     pts/1        100.87.49.37     Mon Jul 20 11:12 - 11:13  (00:00)
root     pts/1        100.87.49.37     Mon Jul 20 10:53 - 10:54  (00:00)
root     pts/1        100.87.49.37     Sun Jul 19 18:03 - 18:04  (00:00)
root     pts/1        100.87.49.37     Sun Jul 19 17:52 - 18:02  (00:10)
root     pts/1        100.87.49.37     Sun Jul 19 17:50 - 17:52  (00:01)
root     pts/1                         Sat Jul 11 12:44 - 12:45  (00:00)
root     pts/5                         Fri Jun 26 11:23 - 11:23  (00:00)
root     pts/4                         Fri Jun 26 11:23 - 11:23  (00:00)
root     pts/3                         Fri Jun 26 11:23 - 11:23  (00:00)
root     pts/1                         Fri Jun 26 11:22 - 11:23  (00:01)
root     pts/1        100.118.91.16    Mon Apr 27 13:45 - 13:52  (00:06)
root     pts/1        100.118.91.16    Mon Apr 27 13:26 - 13:40  (00:13)
root     pts/1        100.118.91.16    Mon Apr 27 13:23 - 13:26  (00:02)
root     pts/1        100.118.91.16    Mon Apr 27 12:49 - 12:56  (00:06)
root     pts/1        100.118.91.16    Sat Apr 25 16:21 - 17:26  (01:04)
root     pts/2        100.118.91.16    Sat Apr 25 16:11 - 16:13  (00:01)
root     pts/2        100.118.91.16    Sat Apr 25 16:07 - 16:07  (00:00)
root     pts/2        100.118.91.16    Sat Apr 25 16:06 - 16:06  (00:00)
root     pts/1        100.118.91.16    Sat Apr 25 16:04 - 16:20  (00:16)
reboot   system boot  6.17.9-1-pve     Fri Apr 24 08:17 - 11:08 (91+02:50)
root     pts/0        100.118.91.16    Mon Apr 13 11:10 - 11:15  (00:05)
reboot   system boot  6.17.9-1-pve     Tue Apr  7 12:19 - 08:17 (16+19:57)
root     pts/0        100.118.91.16    Mon Apr  6 08:43 - 08:44  (00:00)
root     pts/0        100.118.91.16    Sun Apr  5 11:26 - 11:28  (00:02)
root     pts/0        100.118.91.16    Sun Apr  5 11:06 - 11:20  (00:14)
root     pts/0        100.118.91.16    Sun Apr  5 10:59 - 11:02  (00:03)
root     pts/0        100.118.91.16    Sun Apr  5 10:40 - 10:46  (00:05)
root     pts/0        100.118.91.16    Sun Apr  5 08:20 - 08:51  (00:30)
root     pts/0        100.118.91.16    Sun Apr  5 07:07 - 07:24  (00:16)
root     pts/0        100.118.91.16    Sun Apr  5 06:21 - 07:03  (00:42)
reboot   system boot  6.17.9-1-pve     Sat Apr  4 09:57 - 12:18 (3+02:21)
reboot   system boot  6.17.9-1-pve     Sat Apr  4 09:53 - 09:56  (00:02)
reboot   system boot  6.17.9-1-pve     Sat Apr  4 09:46 - crash 
reboot   system boot  6.17.9-1-pve     Sat Apr  4 09:42 - crash 
root     pts/0        100.118.91.16    Sat Apr  4 09:11 - 09:31  (00:19)
root     pts/0        100.118.91.16    Sat Apr  4 02:06 - 02:22  (00:15)
root     pts/0        100.118.91.16    Sat Apr  4 01:55 - 02:05  (00:10)
root     pts/0        100.118.91.16    Sat Apr  4 01:49 - 01:52  (00:03)
root     pts/0        100.118.91.16    Sat Apr  4 01:48 - 01:48  (00:00)
root     pts/0        100.109.70.137   Fri Apr  3 00:04 - 18:05  (18:01)
root     pts/0        100.118.91.16    Mon Mar 30 17:05 - 17:12  (00:06)
reboot   system boot  6.17.9-1-pve     Mon Mar 30 16:51 - 09:41 (4+16:49)
root     tty1                          Mon Mar 30 16:46 - 16:51  (00:05)
reboot   system boot  6.17.9-1-pve     Mon Mar 30 16:42 - 16:51  (00:08)
reboot   system boot  6.17.9-1-pve     Mon Mar 30 16:27 - 16:42  (00:14)
reboot   system boot  6.17.9-1-pve     Mon Mar 30 16:20 - 16:26  (00:05)
reboot   system boot  6.17.9-1-pve     Mon Mar 30 16:03 - 16:20  (00:17)
root     pts/0        100.118.91.16    Mon Mar 30 10:44 - 10:49  (00:04)
reboot   system boot  6.17.9-1-pve     Tue Mar 24 19:57 - 14:45 (5+18:48)
root     pts/0        100.109.70.137   Fri Mar 20 11:06 - crash 
root     pts/2        100.118.91.16    Wed Mar 18 14:04 - 14:05  (00:01)
root     pts/2        100.118.91.16    Wed Mar 18 14:04 - 14:04  (00:00)
root     pts/2        100.118.91.16    Wed Mar 18 13:52 - 14:03  (00:11)
root     pts/1        100.109.70.137   Tue Mar 17 13:42 - 11:06 (2+21:23)
root     pts/0        100.109.70.137   Tue Mar 17 13:22 - 11:06 (2+21:43)
reboot   system boot  6.17.9-1-pve     Sun Mar  8 14:24 - crash 
root     pts/0        100.109.70.137   Fri Mar  6 13:09 - 14:23 (2+00:14)
reboot   system boot  6.17.9-1-pve     Fri Mar  6 13:02 - 14:23 (2+00:21)
root     pts/0        100.109.70.137   Fri Mar  6 12:47 - 13:01  (00:13)
reboot   system boot  6.17.9-1-pve     Fri Mar  6 12:40 - crash 
root     pts/0        100.78.152.116   Fri Mar  6 11:15 - 11:16  (00:01)
reboot   system boot  6.17.9-1-pve     Fri Mar  6 11:09 - 12:39  (01:30)
root     pts/3        100.78.152.116   Fri Mar  6 10:41 - 11:06  (00:25)
root     pts/2        100.109.70.137   Fri Mar  6 10:26 - 11:06  (00:40)
root     pts/1        100.109.70.137   Thu Mar  5 13:00 - 11:06  (22:06)
root     pts/0        100.109.70.137   Thu Mar  5 13:00 - 11:06  (22:06)
reboot   system boot  6.17.9-1-pve     Thu Mar  5 12:27 - 11:06  (22:39)
reboot   system boot  6.17.9-1-pve     Thu Mar  5 12:23 - 12:26  (00:02)
root     pts/1        100.109.70.137   Thu Mar  5 11:28 - 11:58  (00:29)
root     pts/0        100.109.70.137   Thu Mar  5 10:32 - 11:58  (01:25)
root     pts/0        10.100.100.1     Thu Mar  5 10:06 - 10:19  (00:12)
reboot   system boot  6.17.9-1-pve     Thu Mar  5 10:05 - 11:58  (01:53)
root     pts/0        10.100.100.1     Thu Mar  5 09:57 - 10:00  (00:03)
reboot   system boot  6.17.9-1-pve     Thu Mar  5 09:55 - 10:00  (00:05)
root     pts/0        10.100.100.1     Thu Mar  5 09:51 - 09:55  (00:03)
reboot   system boot  6.17.9-1-pve     Wed Mar  4 10:51 - 09:55  (23:03)
root     pts/0        100.109.70.137   Tue Mar  3 19:49 - 20:54  (01:04)
root     pts/3        100.78.152.116   Thu Feb 26 18:44 - 18:46  (00:02)
root     pts/2        100.78.152.116   Thu Feb 26 18:22 - 18:46  (00:24)
root     pts/1        100.78.152.116   Thu Feb 26 09:52 - 18:46  (08:54)
root     pts/0        100.78.152.116   Thu Feb 26 09:41 - 18:46  (09:05)
root     pts/0        100.78.152.116   Thu Feb 26 09:06 - 09:37  (00:30)
root     pts/1        100.109.70.137   Wed Feb 25 20:32 - 20:39  (00:07)
root     pts/0        100.109.70.137   Wed Feb 25 20:28 - 20:39  (00:10)
root     pts/2        100.109.70.137   Wed Feb 25 16:59 - 20:25  (03:26)
root     pts/1        100.109.70.137   Wed Feb 25 16:56 - 18:38  (01:41)
root     pts/0        100.109.70.137   Wed Feb 25 16:56 - 20:25  (03:29)
root     pts/1        100.109.70.137   Wed Feb 25 16:55 - 16:55  (00:00)
root     pts/0        100.109.70.137   Wed Feb 25 16:49 - 16:55  (00:06)
root     pts/0        100.109.70.137   Tue Feb 24 15:54 - 16:18  (00:24)
root     pts/0        100.109.70.137   Tue Feb 24 10:26 - 10:54  (00:27)
root     pts/1        100.109.70.137   Tue Feb 24 09:52 - 09:53  (00:01)
root     pts/1                         Tue Feb 24 07:29 - 07:29  (00:00)
root     pts/1                         Tue Feb 24 07:29 - 07:29  (00:00)
root     pts/1                         Tue Feb 24 07:24 - 07:25  (00:00)
root     pts/0        100.109.70.137   Tue Feb 24 07:24 - 10:09  (02:45)
root     pts/0                         Tue Feb 24 07:19 - 07:21  (00:02)
root     pts/0                         Mon Feb 23 22:23 - 06:54  (08:31)
root     pts/1                         Mon Feb 23 21:28 - 22:08  (00:39)
root     pts/0                         Mon Feb 23 21:12 - 22:08  (00:55)
root     pts/0        100.109.70.137   Mon Feb 23 17:36 - crash 
root     pts/1        100.109.70.137   Mon Feb 23 12:18 - 17:34  (05:15)
root     pts/0        100.109.70.137   Mon Feb 23 12:14 - 17:01  (04:47)
reboot   system boot  6.17.2-1-pve     Mon Feb 23 12:07 - 20:54 (8+08:46)
root     pts/0        100.109.70.137   Mon Feb 23 11:50 - 12:07  (00:16)
reboot   system boot  6.17.2-1-pve     Mon Feb 23 11:48 - 12:07  (00:18)
reboot   system boot  6.17.2-1-pve     Mon Feb 23 11:38 - 11:46  (00:07)
reboot   system boot  6.17.2-1-pve     Mon Feb 23 11:36 - 11:37  (00:01)
root     pts/0        100.109.70.137   Mon Feb 23 11:22 - 11:31  (00:08)
reboot   system boot  6.17.2-1-pve     Mon Feb 23 11:19 - 11:31  (00:11)
root     pts/1        100.109.70.137   Mon Feb 23 11:13 - 11:14  (00:00)
root     pts/0        192.168.3.36     Mon Feb 23 11:02 - 11:14  (00:11)
root     tty1                          Mon Feb 23 10:54 - 11:10  (00:16)
reboot   system boot  6.17.2-1-pve     Mon Feb 23 10:52 - 11:14  (00:21)

wtmpdb begins Mon Feb 23 10:52:50 2026

--- uname
    $ uname -a
Linux pfv-tsys4 6.17.9-1-pve #1 SMP PREEMPT_DYNAMIC PMX 6.17.9-1 (2026-01-12T16:25Z) x86_64 GNU/Linux

--- /proc/cmdline (boot args)
    $ cat /proc/cmdline
BOOT_IMAGE=/boot/vmlinuz-6.17.9-1-pve root=/dev/mapper/pve-root ro quiet

###############################################################################
# 3. HARDWARE INVENTORY
###############################################################################

--- dmidecode -t system
    $ dmidecode -t system
# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 2.7 present.

Handle 0x0001, DMI type 1, 27 bytes
System Information
	Manufacturer: Dell Inc.
	Product Name: Precision T1700
	Version: 01
	Serial Number: C9PBB42
	UUID: 4c4c4544-0039-5010-8042-c3c04f423432
	Wake-up Type: Power Switch
	SKU Number: Precision T1700
	Family: Not Specified

Handle 0x0026, DMI type 12, 5 bytes
System Configuration Options
	Option 1: To Be Filled By O.E.M.

Handle 0x0027, DMI type 15, 35 bytes
System Event Log
	Area Length: 4 bytes
	Header Start Offset: 0x0000
	Header Length: 2 bytes
	Data Start Offset: 0x0002
	Access Method: Indexed I/O, one 16-bit index port, one 8-bit data port
	Access Address: Index 0x046A, Data 0x046C
	Status: Invalid, Not Full
	Change Token: 0x00000000
	Header Format: No Header
	Supported Log Type Descriptors: 6
	Descriptor 1: End of log
	Data Format 1: OEM-specific
	Descriptor 2: End of log
	Data Format 2: OEM-specific
	Descriptor 3: End of log
	Data Format 3: OEM-specific
	Descriptor 4: End of log
	Data Format 4: OEM-specific
	Descriptor 5: End of log
	Data Format 5: OEM-specific
	Descriptor 6: End of log
	Data Format 6: OEM-specific

Handle 0x002A, DMI type 32, 20 bytes
System Boot Information
	Status: No errors detected


--- dmidecode -t baseboard
    $ dmidecode -t baseboard
# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 2.7 present.

Handle 0x0002, DMI type 2, 15 bytes
Base Board Information
	Manufacturer: Dell Inc.
	Product Name: 048DY8
	Version: A00
	Serial Number: /C9PBB42/CN7220051D007C/
	Asset Tag: Not Specified
	Features:
		Board is a hosting board
		Board is replaceable
	Location In Chassis: Not Specified
	Chassis Handle: 0x0003
	Type: Motherboard
	Contained Object Handles: 0

Handle 0x0024, DMI type 10, 8 bytes
On Board Device 1 Information
	Type: Video
	Status: Enabled
	Description: "Intel HD Graphics"
On Board Device 2 Information
	Type: Ethernet
	Status: Enabled
	Description: NETWORK_NAME_STRING

Handle 0x0034, DMI type 41, 11 bytes
Onboard Device
	Reference Designation:  Onboard IGD
	Type: Video
	Status: Enabled
	Type Instance: 1
	Bus Address: 0000:00:02.0

Handle 0x0035, DMI type 41, 11 bytes
Onboard Device
	Reference Designation:  Onboard LAN
	Type: Ethernet
	Status: Enabled
	Type Instance: 1
	Bus Address: 0000:00:19.0

Handle 0x0036, DMI type 41, 11 bytes
Onboard Device
	Reference Designation:  Onboard 1394
	Type: Other
	Status: Enabled
	Type Instance: 1
	Bus Address: 0000:03:1c.2


--- dmidecode -t bios
    $ dmidecode -t bios
# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 2.7 present.

Handle 0x0000, DMI type 0, 24 bytes
BIOS Information
	Vendor: Dell Inc.
	Version: A13
	Release Date: 12/19/2014
	Address: 0xF0000
	Runtime Size: 64 kB
	ROM Size: 12 MB
	Characteristics:
		PCI is supported
		PNP is supported
		BIOS is upgradeable
		BIOS shadowing is allowed
		Boot from CD is supported
		Selectable boot is supported
		EDD is supported
		5.25"/1.2 MB floppy services are supported (int 13h)
		3.5"/720 kB floppy services are supported (int 13h)
		3.5"/2.88 MB floppy services are supported (int 13h)
		Print screen service is supported (int 5h)
		8042 keyboard services are supported (int 9h)
		Serial services are supported (int 14h)
		Printer services are supported (int 17h)
		ACPI is supported
		USB legacy is supported
		BIOS boot specification is supported
		Function key-initiated network boot is supported
		Targeted content distribution is supported
		UEFI is supported
	BIOS Revision: 4.6

Handle 0xDEE1, DMI type 13, 22 bytes
BIOS Language Information
	Language Description Format: Long
	Installable Languages: 1
		en|US|iso8859-1
	Currently Installed Language: en|US|iso8859-1


--- dmidecode -t chassis
    $ dmidecode -t chassis
# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 2.7 present.

Handle 0x0003, DMI type 3, 22 bytes
Chassis Information
	Manufacturer: Dell Inc.
	Type: Mini Tower
	Lock: Not Present
	Version:  
	Serial Number: C9PBB42
	Asset Tag: Not Specified
	Boot-up State: Safe
	Power Supply State: Safe
	Thermal State: Safe
	Security Status: None
	OEM Information: 0x00000000
	Height: Unspecified
	Number Of Power Cords: 1
	Contained Elements: 0
	SKU Number: To be filled by O.E.M.


--- dmidecode -t processor
    $ dmidecode -t processor
# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 2.7 present.

Handle 0x003A, DMI type 4, 42 bytes
Processor Information
	Socket Designation: SOCKET 0
	Type: Central Processor
	Family: Xeon
	Manufacturer: Intel
	ID: C3 06 03 00 FF FB EB BF
	Signature: Type 0, Family 6, Model 60, Stepping 3
	Flags:
		FPU (Floating-point unit on-chip)
		VME (Virtual mode extension)
		DE (Debugging extension)
		PSE (Page size extension)
		TSC (Time stamp counter)
		MSR (Model specific registers)
		PAE (Physical address extension)
		MCE (Machine check exception)
		CX8 (CMPXCHG8 instruction supported)
		APIC (On-chip APIC hardware supported)
		SEP (Fast system call)
		MTRR (Memory type range registers)
		PGE (Page global enable)
		MCA (Machine check architecture)
		CMOV (Conditional move instruction supported)
		PAT (Page attribute table)
		PSE-36 (36-bit page size extension)
		CLFSH (CLFLUSH instruction supported)
		DS (Debug store)
		ACPI (ACPI supported)
		MMX (MMX technology supported)
		FXSR (FXSAVE and FXSTOR instructions supported)
		SSE (Streaming SIMD extensions)
		SSE2 (Streaming SIMD extensions 2)
		SS (Self-snoop)
		HTT (Multi-threading)
		TM (Thermal monitor supported)
		PBE (Pending break enabled)
	Version: Intel(R) Xeon(R) CPU E3-1246 v3 @ 3.50GHz
	Voltage: 1.2 V
	External Clock: 100 MHz
	Max Speed: 3800 MHz
	Current Speed: 3500 MHz
	Status: Populated, Enabled
	Upgrade: Other
	L1 Cache Handle: 0x003B
	L2 Cache Handle: 0x003C
	L3 Cache Handle: 0x003D
	Serial Number: Not Specified
	Asset Tag: Fill By OEM
	Part Number: Fill By OEM
	Core Count: 4
	Core Enabled: 4
	Thread Count: 8
	Characteristics:
		64-bit capable


--- dmidecode -t memory
    $ dmidecode -t memory
# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 2.7 present.

Handle 0x003E, DMI type 16, 23 bytes
Physical Memory Array
	Location: System Board Or Motherboard
	Use: System Memory
	Error Correction Type: Single-bit ECC
	Maximum Capacity: 32 GB
	Error Information Handle: Not Provided
	Number Of Devices: 4

Handle 0x003F, DMI type 17, 34 bytes
Memory Device
	Array Handle: 0x003E
	Error Information Handle: Not Provided
	Total Width: 72 bits
	Data Width: 64 bits
	Size: 4 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM3
	Bank Locator: Not Specified
	Type: DDR3
	Type Detail: Synchronous
	Speed: 1600 MT/s
	Manufacturer: Hynix/Hyundai
	Serial Number: 0D30D903604B
	Asset Tag: 01132700
	Part Number: HMT351U7EFR8A-PB  
	Rank: 2
	Configured Memory Speed: 1600 MT/s

Handle 0x0041, DMI type 17, 34 bytes
Memory Device
	Array Handle: 0x003E
	Error Information Handle: Not Provided
	Total Width: 72 bits
	Data Width: 64 bits
	Size: 4 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM1
	Bank Locator: Not Specified
	Type: DDR3
	Type Detail: Synchronous
	Speed: 1600 MT/s
	Manufacturer: Hynix/Hyundai
	Serial Number: 0D00D902604B
	Asset Tag: 01132700
	Part Number: HMT351U7EFR8A-PB  
	Rank: 2
	Configured Memory Speed: 1600 MT/s

Handle 0x0043, DMI type 17, 34 bytes
Memory Device
	Array Handle: 0x003E
	Error Information Handle: Not Provided
	Total Width: 72 bits
	Data Width: 64 bits
	Size: 4 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM4
	Bank Locator: Not Specified
	Type: DDR3
	Type Detail: Synchronous
	Speed: 1600 MT/s
	Manufacturer: Hynix/Hyundai
	Serial Number: 0D303306903C
	Asset Tag: 01124600
	Part Number: HMT351U7CFR8C-PB  
	Rank: 2
	Configured Memory Speed: 1600 MT/s

Handle 0x0045, DMI type 17, 34 bytes
Memory Device
	Array Handle: 0x003E
	Error Information Handle: Not Provided
	Total Width: 72 bits
	Data Width: 64 bits
	Size: 4 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM2
	Bank Locator: Not Specified
	Type: DDR3
	Type Detail: Synchronous
	Speed: 1600 MT/s
	Manufacturer: Hynix/Hyundai
	Serial Number: 0280530C1028
	Asset Tag: 01131200
	Part Number: HMT351U7CFR8C-PB  
	Rank: 2
	Configured Memory Speed: 1600 MT/s


--- dmidecode -t cache
    $ dmidecode -t cache
# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 2.7 present.

Handle 0x003B, DMI type 7, 19 bytes
Cache Information
	Socket Designation: CPU Internal L1
	Configuration: Enabled, Not Socketed, Level 1
	Operational Mode: Write Back
	Location: Internal
	Installed Size: 256 kB
	Maximum Size: 256 kB
	Supported SRAM Types:
		Unknown
	Installed SRAM Type: Unknown
	Speed: Unknown
	Error Correction Type: Single-bit ECC
	System Type: Other
	Associativity: 8-way Set-associative

Handle 0x003C, DMI type 7, 19 bytes
Cache Information
	Socket Designation: CPU Internal L2
	Configuration: Enabled, Not Socketed, Level 2
	Operational Mode: Write Back
	Location: Internal
	Installed Size: 1 MB
	Maximum Size: 1 MB
	Supported SRAM Types:
		Unknown
	Installed SRAM Type: Unknown
	Speed: Unknown
	Error Correction Type: Single-bit ECC
	System Type: Unified
	Associativity: 8-way Set-associative

Handle 0x003D, DMI type 7, 19 bytes
Cache Information
	Socket Designation: CPU Internal L3
	Configuration: Enabled, Not Socketed, Level 3
	Operational Mode: Write Back
	Location: Internal
	Installed Size: 8 MB
	Maximum Size: 8 MB
	Supported SRAM Types:
		Unknown
	Installed SRAM Type: Unknown
	Speed: Unknown
	Error Correction Type: Single-bit ECC
	System Type: Unified
	Associativity: 16-way Set-associative


--- dmidecode -t connector
    $ dmidecode -t connector
# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 2.7 present.

Handle 0x0004, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J1A1
	Internal Connector Type: None
	External Reference Designator: PS2Mouse
	External Connector Type: PS/2
	Port Type: Mouse Port

Handle 0x0005, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J1A1
	Internal Connector Type: None
	External Reference Designator: Keyboard
	External Connector Type: PS/2
	Port Type: Keyboard Port

Handle 0x0006, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J6A2A
	Internal Connector Type: None
	External Reference Designator: COM A
	External Connector Type: DB-9 male
	Port Type: Serial Port 16550A Compatible

Handle 0x0007, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J6A2B
	Internal Connector Type: None
	External Reference Designator: Video
	External Connector Type: DB-15 female
	Port Type: Video Port

Handle 0x0008, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J2A1
	Internal Connector Type: None
	External Reference Designator: USB1
	External Connector Type: Access Bus (USB)
	Port Type: USB

Handle 0x0009, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J2A1
	Internal Connector Type: None
	External Reference Designator: USB2
	External Connector Type: Access Bus (USB)
	Port Type: USB

Handle 0x000A, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J5A1
	Internal Connector Type: None
	External Reference Designator: USB3
	External Connector Type: Access Bus (USB)
	Port Type: USB

Handle 0x000B, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J5A1
	Internal Connector Type: None
	External Reference Designator: USB4
	External Connector Type: Access Bus (USB)
	Port Type: USB

Handle 0x000C, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J5A1
	Internal Connector Type: None
	External Reference Designator: USB5
	External Connector Type: Access Bus (USB)
	Port Type: USB

Handle 0x000D, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J5A1
	Internal Connector Type: None
	External Reference Designator: USB6
	External Connector Type: Access Bus (USB)
	Port Type: USB

Handle 0x000E, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J8A1
	Internal Connector Type: None
	External Reference Designator: USB7
	External Connector Type: Access Bus (USB)
	Port Type: USB

Handle 0x000F, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J8A1
	Internal Connector Type: None
	External Reference Designator: USB8
	External Connector Type: Access Bus (USB)
	Port Type: USB

Handle 0x0010, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J8A1
	Internal Connector Type: None
	External Reference Designator: USB9
	External Connector Type: Access Bus (USB)
	Port Type: USB

Handle 0x0011, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J8A1
	Internal Connector Type: None
	External Reference Designator: USB10
	External Connector Type: Access Bus (USB)
	Port Type: USB

Handle 0x0012, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J2A1
	Internal Connector Type: None
	External Reference Designator: LAN
	External Connector Type: RJ-45
	Port Type: Network Port

Handle 0x0013, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J2A1
	Internal Connector Type: None
	External Reference Designator: Display Port1
	External Connector Type: Other
	Port Type: Video Port

Handle 0x0014, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J3A1
	Internal Connector Type: None
	External Reference Designator: Display Port2
	External Connector Type: Other
	Port Type: Video Port

Handle 0x0015, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J7A1
	Internal Connector Type: None
	External Reference Designator: MIC-IN
	External Connector Type: Mini Jack (headphones)
	Port Type: Audio Port

Handle 0x0016, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J7A1
	Internal Connector Type: None
	External Reference Designator: HP-OUT
	External Connector Type: Mini Jack (headphones)
	Port Type: Audio Port

Handle 0x0017, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J7A1
	Internal Connector Type: None
	External Reference Designator: LINE-OUT
	External Connector Type: Mini Jack (headphones)
	Port Type: Audio Port

Handle 0x0018, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J7A1
	Internal Connector Type: None
	External Reference Designator: LINE-IN
	External Connector Type: Mini Jack (headphones)
	Port Type: Audio Port

Handle 0x0019, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J7J3 - SATA PORT1
	Internal Connector Type: Other
	External Reference Designator: Not Specified
	External Connector Type: None
	Port Type: Other

Handle 0x001A, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J8J1 - SATA PORT0
	Internal Connector Type: Other
	External Reference Designator: Not Specified
	External Connector Type: None
	Port Type: Other

Handle 0x001B, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J2B3 - CPU FAN
	Internal Connector Type: Other
	External Reference Designator: Not Specified
	External Connector Type: None
	Port Type: Other

Handle 0x001C, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J7H1 - SATA PORT2
	Internal Connector Type: Other
	External Reference Designator: Not Specified
	External Connector Type: None
	Port Type: Other

Handle 0x001D, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J7H2 - SATA PORT3
	Internal Connector Type: Other
	External Reference Designator: Not Specified
	External Connector Type: None
	Port Type: Other

Handle 0x001E, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J1D1 - INTRUDER
	Internal Connector Type: Other
	External Reference Designator: Not Specified
	External Connector Type: None
	Port Type: Other

Handle 0x001F, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J2D3 - INTERNAL USB
	Internal Connector Type: Other
	External Reference Designator: Not Specified
	External Connector Type: None
	Port Type: Other

Handle 0x0020, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J2D4 - INTERNAL USB
	Internal Connector Type: Other
	External Reference Designator: Not Specified
	External Connector Type: None
	Port Type: Other

Handle 0x0021, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J2B3 - SYSTEM_FAN
	Internal Connector Type: Other
	External Reference Designator: Not Specified
	External Connector Type: None
	Port Type: Other

Handle 0x0022, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: J9E5 - INT_SPKR
	Internal Connector Type: Other
	External Reference Designator: Not Specified
	External Connector Type: None
	Port Type: Other


--- dmidecode -t slot
    $ dmidecode -t slot
# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 2.7 present.

Handle 0x0023, DMI type 9, 17 bytes
System Slot Information
	Designation: X16 
	Type: PCI Express 3 x16
	Data Bus Width: 16x or x16
	Current Usage: Available
	Length: Long
	ID: 1
	Characteristics:
		3.3 V is provided
		Opening is shared
		PME signal is supported
	Bus Address: 0000:00:01.0

Handle 0xDED2, DMI type 9, 17 bytes
System Slot Information
	Designation: X1  
	Type: PCI Express 2 x1
	Data Bus Width: 1x or x1
	Current Usage: Available
	Length: Short
	ID: 2
	Characteristics:
		3.3 V is provided
		Opening is shared
		PME signal is supported
	Bus Address: 0000:00:1c.2

Handle 0xDED7, DMI type 9, 17 bytes
System Slot Information
	Designation: PCI 
	Type: PCI
	Data Bus Width: 32 bit
	Current Usage: Available
	Length: Short
	ID: 3
	Characteristics:
		3.3 V is provided
		Opening is shared
		PME signal is supported
	Bus Address: 0000:03:02.0

Handle 0xDEDC, DMI type 9, 17 bytes
System Slot Information
	Designation: X4  
	Type: PCI Express 2 x4
	Data Bus Width: 4x or x4
	Current Usage: Available
	Length: Short
	ID: 4
	Characteristics:
		3.3 V is provided
		Opening is shared
		PME signal is supported
	Bus Address: 0000:00:1c.4


--- lscpu
    $ lscpu
Architecture:                            x86_64
CPU op-mode(s):                          32-bit, 64-bit
Address sizes:                           39 bits physical, 48 bits virtual
Byte Order:                              Little Endian
CPU(s):                                  8
On-line CPU(s) list:                     0-7
Vendor ID:                               GenuineIntel
Model name:                              Intel(R) Xeon(R) CPU E3-1246 v3 @ 3.50GHz
CPU family:                              6
Model:                                   60
Thread(s) per core:                      2
Core(s) per socket:                      4
Socket(s):                               1
Stepping:                                3
CPU(s) scaling MHz:                      98%
CPU max MHz:                             3900.0000
CPU min MHz:                             800.0000
BogoMIPS:                                6983.74
Flags:                                   fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush dts acpi mmx fxsr sse sse2 ss ht tm pbe syscall nx pdpe1gb rdtscp lm constant_tsc arch_perfmon pebs bts rep_good nopl xtopology nonstop_tsc cpuid aperfmperf pni pclmulqdq dtes64 monitor ds_cpl vmx smx est tm2 ssse3 sdbg fma cx16 xtpr pdcm pcid sse4_1 sse4_2 x2apic movbe popcnt tsc_deadline_timer aes xsave avx f16c rdrand lahf_lm abm cpuid_fault epb pti ssbd ibrs ibpb stibp tpr_shadow flexpriority ept vpid ept_ad fsgsbase tsc_adjust bmi1 avx2 smep bmi2 erms invpcid xsaveopt dtherm ida arat pln pts vnmi md_clear flush_l1d
Virtualization:                          VT-x
L1d cache:                               128 KiB (4 instances)
L1i cache:                               128 KiB (4 instances)
L2 cache:                                1 MiB (4 instances)
L3 cache:                                8 MiB (1 instance)
NUMA node(s):                            1
NUMA node0 CPU(s):                       0-7
Vulnerability Gather data sampling:      Not affected
Vulnerability Ghostwrite:                Not affected
Vulnerability Indirect target selection: Not affected
Vulnerability Itlb multihit:             KVM: Mitigation: Split huge pages
Vulnerability L1tf:                      Mitigation; PTE Inversion; VMX conditional cache flushes, SMT vulnerable
Vulnerability Mds:                       Mitigation; Clear CPU buffers; SMT vulnerable
Vulnerability Meltdown:                  Mitigation; PTI
Vulnerability Mmio stale data:           Not affected
Vulnerability Old microcode:             Not affected
Vulnerability Reg file data sampling:    Not affected
Vulnerability Retbleed:                  Not affected
Vulnerability Spec rstack overflow:      Not affected
Vulnerability Spec store bypass:         Mitigation; Speculative Store Bypass disabled via prctl
Vulnerability Spectre v1:                Mitigation; usercopy/swapgs barriers and __user pointer sanitization
Vulnerability Spectre v2:                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP conditional; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected
Vulnerability Srbds:                     Mitigation; Microcode
Vulnerability Tsa:                       Not affected
Vulnerability Tsx async abort:           Not affected
Vulnerability Vmscape:                   Mitigation; IBPB before exit to userspace

--- lscpu cache
    $ lscpu -C
NAME ONE-SIZE ALL-SIZE WAYS TYPE        LEVEL SETS PHY-LINE COHERENCY-SIZE
L1d       32K     128K    8 Data            1   64        1             64
L1i       32K     128K    8 Instruction     1   64        1             64
L2       256K       1M    8 Unified         2  512        1             64
L3         8M       8M   16 Unified         3 8192        1             64

--- numactl --hardware
    $ numactl --hardware
/root/check.sh: line 45: numactl: command not found
    [exit=127 / not installed or not permitted]

--- numactl --show
    $ numactl --show
/root/check.sh: line 45: numactl: command not found
    [exit=127 / not installed or not permitted]

--- lspci -nnvv (verbose)
    $ lspci -nnvv
00:00.0 Host bridge [0600]: Intel Corporation Xeon E3-1200 v3 Processor DRAM Controller [8086:0c08] (rev 06)
	Subsystem: Dell Device [1028:05a6]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap+ 66MHz- UDF- FastB2B+ ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort+ >SERR- <PERR- INTx-
	Latency: 0
	IOMMU group: 1
	Capabilities: [e0] Vendor Specific Information: Len=0c <?>
	Kernel driver in use: ie31200_edac
	Kernel modules: ie31200_edac

00:02.0 VGA compatible controller [0300]: Intel Corporation Xeon E3-1200 v3 Processor Integrated Graphics Controller [8086:041a] (rev 06) (prog-if 00 [VGA controller])
	DeviceName:  Onboard IGD
	Subsystem: Dell Device [1028:05a6]
	Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
	Status: Cap+ 66MHz- UDF- FastB2B+ ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0
	Interrupt: pin A routed to IRQ 39
	IOMMU group: 0
	Region 0: Memory at f7800000 (64-bit, non-prefetchable) [size=4M]
	Region 2: Memory at e0000000 (64-bit, prefetchable) [size=256M]
	Region 4: I/O ports at f000 [size=64]
	Expansion ROM at 000c0000 [virtual] [disabled] [size=128K]
	Capabilities: [90] MSI: Enable+ Count=1/1 Maskable- 64bit-
		Address: fee00018  Data: 0000
	Capabilities: [d0] Power Management version 2
		Flags: PMEClk- DSI+ D1- D2- AuxCurrent=0mA PME(D0-,D1-,D2-,D3hot-,D3cold-)
		Status: D3 NoSoftRst- PME-Enable- DSel=0 DScale=0 PME-
	Capabilities: [a4] PCI Advanced Features
		AFCap: TP+ FLR+
		AFCtrl: FLR-
		AFStatus: TP-
	Kernel driver in use: i915
	Kernel modules: i915

00:03.0 Audio device [0403]: Intel Corporation Xeon E3-1200 v3/4th Gen Core Processor HD Audio Controller [8086:0c0c] (rev 06)
	Subsystem: Dell Device [1028:05a6]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
	Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0, Cache Line Size: 64 bytes
	Interrupt: pin A routed to IRQ 40
	IOMMU group: 2
	Region 0: Memory at f7c30000 (64-bit, non-prefetchable) [size=16K]
	Capabilities: [50] Power Management version 2
		Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0-,D1-,D2-,D3hot-,D3cold-)
		Status: D3 NoSoftRst- PME-Enable- DSel=0 DScale=0 PME-
	Capabilities: [60] MSI: Enable+ Count=1/1 Maskable- 64bit-
		Address: fee00458  Data: 0000
	Capabilities: [70] Express (v1) Root Complex Integrated Endpoint, IntMsgNum 0
		DevCap:	MaxPayload 128 bytes, PhantFunc 0
			ExtTag- RBE- FLReset+ TEE-IO-
		DevCtl:	CorrErr- NonFatalErr- FatalErr- UnsupReq-
			RlxdOrd- ExtTag- PhantFunc- AuxPwr- NoSnoop- FLReset-
			MaxPayload 128 bytes, MaxReadReq 128 bytes
		DevSta:	CorrErr- NonFatalErr- FatalErr- UnsupReq- AuxPwr- TransPend-
	Kernel driver in use: snd_hda_intel
	Kernel modules: snd_hda_intel

00:14.0 USB controller [0c03]: Intel Corporation 8 Series/C220 Series Chipset Family USB xHCI [8086:8c31] (rev 04) (prog-if 30 [XHCI])
	Subsystem: Dell Device [1028:05a6]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
	Status: Cap+ 66MHz- UDF- FastB2B+ ParErr- DEVSEL=medium >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0
	Interrupt: pin A routed to IRQ 30
	IOMMU group: 3
	Region 0: Memory at f7c20000 (64-bit, non-prefetchable) [size=64K]
	Capabilities: [70] Power Management version 2
		Flags: PMEClk- DSI- D1- D2- AuxCurrent=375mA PME(D0-,D1-,D2-,D3hot+,D3cold+)
		Status: D0 NoSoftRst+ PME-Enable+ DSel=0 DScale=0 PME-
	Capabilities: [80] MSI: Enable+ Count=8/8 Maskable- 64bit+
		Address: 00000000fee00318  Data: 0000
	Kernel driver in use: xhci_hcd
	Kernel modules: xhci_pci

00:16.0 Communication controller [0780]: Intel Corporation 8 Series/C220 Series Chipset Family MEI Controller #1 [8086:8c3a] (rev 04)
	Subsystem: Dell Device [1028:05a6]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
	Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0
	Interrupt: pin A routed to IRQ 38
	IOMMU group: 4
	Region 0: Memory at f7c3b000 (64-bit, non-prefetchable) [size=16]
	Capabilities: [50] Power Management version 3
		Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
		Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=0 PME-
	Capabilities: [8c] MSI: Enable+ Count=1/1 Maskable- 64bit+
		Address: 00000000fee00438  Data: 0000
	Kernel driver in use: mei_me
	Kernel modules: mei_me

00:19.0 Ethernet controller [0200]: Intel Corporation Ethernet Connection I217-LM [8086:153a] (rev 04)
	DeviceName:  Onboard LAN
	Subsystem: Dell Device [1028:05a6]
	Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
	Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0
	Interrupt: pin A routed to IRQ 29
	IOMMU group: 5
	Region 0: Memory at f7c00000 (32-bit, non-prefetchable) [size=128K]
	Region 1: Memory at f7c38000 (32-bit, non-prefetchable) [size=4K]
	Region 2: I/O ports at f060 [size=32]
	Capabilities: [c8] Power Management version 2
		Flags: PMEClk- DSI+ D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
		Status: D0 NoSoftRst- PME-Enable- DSel=0 DScale=1 PME-
	Capabilities: [d0] MSI: Enable+ Count=1/1 Maskable- 64bit+
		Address: 00000000fee002f8  Data: 0000
	Capabilities: [e0] PCI Advanced Features
		AFCap: TP+ FLR+
		AFCtrl: FLR-
		AFStatus: TP-
	Kernel driver in use: e1000e
	Kernel modules: e1000e

00:1a.0 USB controller [0c03]: Intel Corporation 8 Series/C220 Series Chipset Family USB EHCI #2 [8086:8c2d] (rev 04) (prog-if 20 [EHCI])
	Subsystem: Dell Device [1028:05a6]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap+ 66MHz- UDF- FastB2B+ ParErr- DEVSEL=medium >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0
	Interrupt: pin A routed to IRQ 16
	IOMMU group: 6
	Region 0: Memory at f7c37000 (32-bit, non-prefetchable) [size=1K]
	Capabilities: [50] Power Management version 2
		Flags: PMEClk- DSI- D1- D2- AuxCurrent=375mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
		Status: D0 NoSoftRst- PME-Enable- DSel=0 DScale=0 PME-
	Capabilities: [58] Debug port: BAR=1 offset=00a0
	Capabilities: [98] PCI Advanced Features
		AFCap: TP+ FLR+
		AFCtrl: FLR-
		AFStatus: TP-
	Kernel driver in use: ehci-pci
	Kernel modules: ehci_pci

00:1c.0 PCI bridge [0604]: Intel Corporation 8 Series/C220 Series Chipset Family PCI Express Root Port #1 [8086:8c10] (rev d4) (prog-if 00 [Normal decode])
	Subsystem: Dell Device [1028:05a6]
	Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
	Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0, Cache Line Size: 64 bytes
	Interrupt: pin A routed to IRQ 26
	IOMMU group: 7
	Bus: primary=00, secondary=01, subordinate=01, sec-latency=0
	I/O behind bridge: [disabled] [16-bit]
	Memory behind bridge: [disabled] [32-bit]
	Prefetchable memory behind bridge: [disabled] [64-bit]
	Secondary status: 66MHz- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- <SERR- <PERR-
	BridgeCtl: Parity- SERR+ NoISA- VGA- VGA16+ MAbort- >Reset- FastB2B-
		PriDiscTmr- SecDiscTmr- DiscTmrStat- DiscTmrSERREn-
	Capabilities: [40] Express (v2) Root Port (Slot-), IntMsgNum 0
		DevCap:	MaxPayload 128 bytes, PhantFunc 0
			ExtTag- RBE+ TEE-IO-
		DevCtl:	CorrErr- NonFatalErr- FatalErr- UnsupReq-
			RlxdOrd- ExtTag- PhantFunc- AuxPwr- NoSnoop-
			MaxPayload 128 bytes, MaxReadReq 128 bytes
		DevSta:	CorrErr- NonFatalErr- FatalErr- UnsupReq- AuxPwr+ TransPend-
		LnkCap:	Port #1, Speed 5GT/s, Width x1, ASPM L0s L1, Exit Latency L0s <1us, L1 <4us
			ClockPM- Surprise- LLActRep+ BwNot+ ASPMOptComp-
		LnkCtl:	ASPM L0s L1 Enabled; RCB 64 bytes, LnkDisable- CommClk-
			ExtSynch- ClockPM- AutWidDis- BWInt+ AutBWInt+
		LnkSta:	Speed 2.5GT/s, Width x0
			TrErr- Train- SlotClk+ DLActive- BWMgmt- ABWMgmt-
		RootCap: CRSVisible-
		RootCtl: ErrCorrectable- ErrNon-Fatal- ErrFatal- PMEIntEna- CRSVisible-
		RootSta: PME ReqID 0000, PMEStatus- PMEPending-
		DevCap2: Completion Timeout: Range ABC, TimeoutDis+ NROPrPrP- LTR+
			 10BitTagComp- 10BitTagReq- OBFF Via WAKE#, ExtFmt- EETLPPrefix-
			 EmergencyPowerReduction Not Supported, EmergencyPowerReductionInit-
			 FRS- LN System CLS Not Supported, TPHComp- ExtTPHComp- ARIFwd-
			 AtomicOpsCap: Routing- 32bit- 64bit- 128bitCAS-
		DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis- ARIFwd-
			 AtomicOpsCtl: ReqEn- EgressBlck-
			 IDOReq- IDOCompl- LTR+ EmergencyPowerReductionReq-
			 10BitTagReq- OBFF Disabled, EETLPPrefixBlk-
		LnkCtl2: Target Link Speed: 5GT/s, EnterCompliance- SpeedDis-
			 Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
			 Compliance Preset/De-emphasis: -6dB de-emphasis, 0dB preshoot
		LnkSta2: Current De-emphasis Level: -3.5dB, EqualizationComplete- EqualizationPhase1-
			 EqualizationPhase2- EqualizationPhase3- LinkEqualizationRequest-
			 Retimer- 2Retimers- CrosslinkRes: unsupported
	Capabilities: [80] MSI: Enable+ Count=1/1 Maskable- 64bit-
		Address: fee00218  Data: 0000
	Capabilities: [90] Subsystem: Dell Device [1028:05a6]
	Capabilities: [a0] Power Management version 3
		Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
		Status: D0 NoSoftRst- PME-Enable- DSel=0 DScale=0 PME-
	Kernel driver in use: pcieport

00:1c.1 PCI bridge [0604]: Intel Corporation 8 Series/C220 Series Chipset Family PCI Express Root Port #2 [8086:8c12] (rev d4) (prog-if 00 [Normal decode])
	Subsystem: Dell Device [1028:05a6]
	Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
	Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0, Cache Line Size: 64 bytes
	Interrupt: pin B routed to IRQ 27
	IOMMU group: 8
	Bus: primary=00, secondary=02, subordinate=03, sec-latency=0
	I/O behind bridge: [disabled] [16-bit]
	Memory behind bridge: [disabled] [32-bit]
	Prefetchable memory behind bridge: [disabled] [64-bit]
	Secondary status: 66MHz- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- <SERR- <PERR-
	BridgeCtl: Parity- SERR+ NoISA- VGA- VGA16+ MAbort- >Reset- FastB2B-
		PriDiscTmr- SecDiscTmr- DiscTmrStat- DiscTmrSERREn-
	Capabilities: [40] Express (v2) Root Port (Slot+), IntMsgNum 0
		DevCap:	MaxPayload 128 bytes, PhantFunc 0
			ExtTag- RBE+ TEE-IO-
		DevCtl:	CorrErr- NonFatalErr- FatalErr- UnsupReq-
			RlxdOrd- ExtTag- PhantFunc- AuxPwr- NoSnoop-
			MaxPayload 128 bytes, MaxReadReq 128 bytes
		DevSta:	CorrErr- NonFatalErr- FatalErr- UnsupReq- AuxPwr+ TransPend-
		LnkCap:	Port #2, Speed 5GT/s, Width x1, ASPM L0s L1, Exit Latency L0s <512ns, L1 <16us
			ClockPM- Surprise- LLActRep+ BwNot+ ASPMOptComp-
		LnkCtl:	ASPM Disabled; RCB 64 bytes, LnkDisable- CommClk+
			ExtSynch- ClockPM- AutWidDis- BWInt+ AutBWInt+
		LnkSta:	Speed 2.5GT/s, Width x1
			TrErr- Train- SlotClk+ DLActive+ BWMgmt- ABWMgmt-
		SltCap:	AttnBtn- PwrCtrl- MRL- AttnInd- PwrInd- HotPlug- Surprise-
			Slot #1, PowerLimit 10W; Interlock- NoCompl+
		SltCtl:	Enable: AttnBtn- PwrFlt- MRL- PresDet- CmdCplt- HPIrq- LinkChg-
			Control: AttnInd Unknown, PwrInd Unknown, Power- Interlock-
		SltSta:	Status: AttnBtn- PowerFlt- MRL- CmdCplt- PresDet+ Interlock-
			Changed: MRL- PresDet- LinkState-
		RootCap: CRSVisible-
		RootCtl: ErrCorrectable- ErrNon-Fatal- ErrFatal- PMEIntEna- CRSVisible-
		RootSta: PME ReqID 0000, PMEStatus- PMEPending-
		DevCap2: Completion Timeout: Range ABC, TimeoutDis+ NROPrPrP- LTR+
			 10BitTagComp- 10BitTagReq- OBFF Not Supported, ExtFmt- EETLPPrefix-
			 EmergencyPowerReduction Not Supported, EmergencyPowerReductionInit-
			 FRS- LN System CLS Not Supported, TPHComp- ExtTPHComp- ARIFwd-
			 AtomicOpsCap: Routing- 32bit- 64bit- 128bitCAS-
		DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis- ARIFwd-
			 AtomicOpsCtl: ReqEn- EgressBlck-
			 IDOReq- IDOCompl- LTR+ EmergencyPowerReductionReq-
			 10BitTagReq- OBFF Disabled, EETLPPrefixBlk-
		LnkCtl2: Target Link Speed: 5GT/s, EnterCompliance- SpeedDis-
			 Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
			 Compliance Preset/De-emphasis: -6dB de-emphasis, 0dB preshoot
		LnkSta2: Current De-emphasis Level: -3.5dB, EqualizationComplete- EqualizationPhase1-
			 EqualizationPhase2- EqualizationPhase3- LinkEqualizationRequest-
			 Retimer- 2Retimers- CrosslinkRes: unsupported
	Capabilities: [80] MSI: Enable+ Count=1/1 Maskable- 64bit-
		Address: fee00258  Data: 0000
	Capabilities: [90] Subsystem: Dell Device [1028:05a6]
	Capabilities: [a0] Power Management version 3
		Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
		Status: D0 NoSoftRst- PME-Enable- DSel=0 DScale=0 PME-
	Kernel driver in use: pcieport

00:1c.4 PCI bridge [0604]: Intel Corporation 8 Series/C220 Series Chipset Family PCI Express Root Port #5 [8086:8c18] (rev d4) (prog-if 00 [Normal decode])
	Subsystem: Dell Device [1028:05a6]
	Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
	Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0, Cache Line Size: 64 bytes
	Interrupt: pin A routed to IRQ 28
	IOMMU group: 9
	Bus: primary=00, secondary=04, subordinate=04, sec-latency=0
	I/O behind bridge: 2000-2fff [size=4K] [16-bit]
	Memory behind bridge: df200000-df3fffff [size=2M] [32-bit]
	Prefetchable memory behind bridge: df400000-df5fffff [size=2M] [32-bit]
	Secondary status: 66MHz- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- <SERR- <PERR-
	BridgeCtl: Parity- SERR+ NoISA- VGA- VGA16+ MAbort- >Reset- FastB2B-
		PriDiscTmr- SecDiscTmr- DiscTmrStat- DiscTmrSERREn-
	Capabilities: [40] Express (v2) Root Port (Slot+), IntMsgNum 0
		DevCap:	MaxPayload 128 bytes, PhantFunc 0
			ExtTag- RBE+ TEE-IO-
		DevCtl:	CorrErr- NonFatalErr- FatalErr- UnsupReq-
			RlxdOrd- ExtTag- PhantFunc- AuxPwr- NoSnoop-
			MaxPayload 128 bytes, MaxReadReq 128 bytes
		DevSta:	CorrErr- NonFatalErr- FatalErr- UnsupReq- AuxPwr+ TransPend-
		LnkCap:	Port #5, Speed 5GT/s, Width x4, ASPM L0s L1, Exit Latency L0s <1us, L1 <16us
			ClockPM- Surprise- LLActRep+ BwNot+ ASPMOptComp-
		LnkCtl:	ASPM L0s L1 Enabled; RCB 64 bytes, LnkDisable- CommClk-
			ExtSynch- ClockPM- AutWidDis- BWInt+ AutBWInt+
		LnkSta:	Speed 2.5GT/s, Width x0
			TrErr- Train- SlotClk+ DLActive- BWMgmt- ABWMgmt-
		SltCap:	AttnBtn- PwrCtrl- MRL- AttnInd- PwrInd- HotPlug+ Surprise+
			Slot #4, PowerLimit 25W; Interlock- NoCompl+
		SltCtl:	Enable: AttnBtn- PwrFlt- MRL- PresDet- CmdCplt- HPIrq- LinkChg-
			Control: AttnInd Unknown, PwrInd Unknown, Power- Interlock-
		SltSta:	Status: AttnBtn- PowerFlt- MRL- CmdCplt- PresDet- Interlock-
			Changed: MRL- PresDet- LinkState-
		RootCap: CRSVisible-
		RootCtl: ErrCorrectable- ErrNon-Fatal- ErrFatal- PMEIntEna- CRSVisible-
		RootSta: PME ReqID 0000, PMEStatus- PMEPending-
		DevCap2: Completion Timeout: Range ABC, TimeoutDis+ NROPrPrP- LTR+
			 10BitTagComp- 10BitTagReq- OBFF Not Supported, ExtFmt- EETLPPrefix-
			 EmergencyPowerReduction Not Supported, EmergencyPowerReductionInit-
			 FRS- LN System CLS Not Supported, TPHComp- ExtTPHComp- ARIFwd-
			 AtomicOpsCap: Routing- 32bit- 64bit- 128bitCAS-
		DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis- ARIFwd-
			 AtomicOpsCtl: ReqEn- EgressBlck-
			 IDOReq- IDOCompl- LTR+ EmergencyPowerReductionReq-
			 10BitTagReq- OBFF Disabled, EETLPPrefixBlk-
		LnkCtl2: Target Link Speed: 5GT/s, EnterCompliance- SpeedDis-
			 Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
			 Compliance Preset/De-emphasis: -6dB de-emphasis, 0dB preshoot
		LnkSta2: Current De-emphasis Level: -3.5dB, EqualizationComplete- EqualizationPhase1-
			 EqualizationPhase2- EqualizationPhase3- LinkEqualizationRequest-
			 Retimer- 2Retimers- CrosslinkRes: unsupported
	Capabilities: [80] MSI: Enable+ Count=1/1 Maskable- 64bit-
		Address: fee00278  Data: 0000
	Capabilities: [90] Subsystem: Dell Device [1028:05a6]
	Capabilities: [a0] Power Management version 3
		Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
		Status: D0 NoSoftRst- PME-Enable- DSel=0 DScale=0 PME-
	Kernel driver in use: pcieport

00:1d.0 USB controller [0c03]: Intel Corporation 8 Series/C220 Series Chipset Family USB EHCI #1 [8086:8c26] (rev 04) (prog-if 20 [EHCI])
	Subsystem: Dell Device [1028:05a6]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap+ 66MHz- UDF- FastB2B+ ParErr- DEVSEL=medium >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0
	Interrupt: pin A routed to IRQ 23
	IOMMU group: 10
	Region 0: Memory at f7c36000 (32-bit, non-prefetchable) [size=1K]
	Capabilities: [50] Power Management version 2
		Flags: PMEClk- DSI- D1- D2- AuxCurrent=375mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
		Status: D0 NoSoftRst- PME-Enable- DSel=0 DScale=0 PME-
	Capabilities: [58] Debug port: BAR=1 offset=00a0
	Capabilities: [98] PCI Advanced Features
		AFCap: TP+ FLR+
		AFCtrl: FLR-
		AFStatus: TP-
	Kernel driver in use: ehci-pci
	Kernel modules: ehci_pci

00:1f.0 ISA bridge [0601]: Intel Corporation C226 Series Chipset Family Server Advanced SKU LPC Controller [8086:8c56] (rev 04)
	Subsystem: Dell Device [1028:05a6]
	Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=medium >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0
	IOMMU group: 11
	Capabilities: [e0] Vendor Specific Information: Len=0c <?>
	Kernel driver in use: lpc_ich
	Kernel modules: lpc_ich

00:1f.2 IDE interface [0101]: Intel Corporation 8 Series/C220 Series Chipset Family 4-port SATA Controller 1 [IDE mode] [8086:8c00] (rev 04) (prog-if 8f [PCI native mode controller, supports both channels switched to ISA compatibility mode, supports bus mastering])
	Subsystem: Dell Device [1028:05a6]
	Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap+ 66MHz+ UDF- FastB2B+ ParErr- DEVSEL=medium >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0
	Interrupt: pin B routed to IRQ 19
	IOMMU group: 11
	Region 0: I/O ports at f0d0 [size=8]
	Region 1: I/O ports at f0c0 [size=4]
	Region 2: I/O ports at f0b0 [size=8]
	Region 3: I/O ports at f0a0 [size=4]
	Region 4: I/O ports at f090 [size=16]
	Region 5: I/O ports at f080 [size=16]
	Capabilities: [70] Power Management version 3
		Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0-,D1-,D2-,D3hot-,D3cold-)
		Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=0 PME-
	Kernel driver in use: ata_piix
	Kernel modules: pata_acpi

00:1f.3 SMBus [0c05]: Intel Corporation 8 Series/C220 Series Chipset Family SMBus Controller [8086:8c22] (rev 04)
	Subsystem: Dell Device [1028:05a6]
	Control: I/O+ Mem+ BusMaster- SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B+ ParErr- DEVSEL=medium >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Interrupt: pin C routed to IRQ 18
	IOMMU group: 11
	Region 0: Memory at f7c35000 (64-bit, non-prefetchable) [size=256]
	Region 4: I/O ports at f040 [size=32]
	Kernel driver in use: i801_smbus
	Kernel modules: i2c_i801

02:00.0 PCI bridge [0604]: Texas Instruments XIO2001 PCI Express-to-PCI Bridge [104c:8240] (prog-if 00 [Normal decode])
	Subsystem: Dell Device [1028:05a6]
	Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0, Cache Line Size: 64 bytes
	IOMMU group: 12
	Bus: primary=02, secondary=03, subordinate=03, sec-latency=32
	I/O behind bridge: [disabled] [32-bit]
	Memory behind bridge: [disabled] [32-bit]
	Prefetchable memory behind bridge: [disabled] [64-bit]
	Secondary status: 66MHz+ FastB2B+ ParErr- DEVSEL=medium >TAbort- <TAbort- <MAbort- <SERR- <PERR-
	BridgeCtl: Parity- SERR+ NoISA- VGA- VGA16+ MAbort- >Reset- FastB2B-
		PriDiscTmr- SecDiscTmr- DiscTmrStat- DiscTmrSERREn-
	Capabilities: [40] Subsystem: Dell Device [1028:05a6]
	Capabilities: [48] Power Management version 3
		Flags: PMEClk- DSI- D1+ D2+ AuxCurrent=0mA PME(D0-,D1-,D2-,D3hot-,D3cold-)
		Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=0 PME-
		Bridge: PM- B3-
	Capabilities: [50] MSI: Enable- Count=1/16 Maskable- 64bit+
		Address: 0000000000000000  Data: 0000
	Capabilities: [70] Express (v2) PCI-Express to PCI/PCI-X Bridge, IntMsgNum 0
		DevCap:	MaxPayload 512 bytes, PhantFunc 0
			ExtTag- AttnBtn- AttnInd- PwrInd- RBE+ SlotPowerLimit 10W TEE-IO-
		DevCtl:	CorrErr+ NonFatalErr+ FatalErr+ UnsupReq+
			RlxdOrd- ExtTag- PhantFunc- AuxPwr- NoSnoop- BrConfRtry-
			MaxPayload 128 bytes, MaxReadReq 512 bytes
		DevSta:	CorrErr+ NonFatalErr- FatalErr- UnsupReq+ AuxPwr+ TransPend-
		LnkCap:	Port #0, Speed 2.5GT/s, Width x1, ASPM L0s L1, Exit Latency L0s <512ns, L1 <16us
			ClockPM+ Surprise- LLActRep- BwNot- ASPMOptComp-
		LnkCtl:	ASPM Disabled; RCB 64 bytes, LnkDisable- CommClk+
			ExtSynch- ClockPM- AutWidDis- BWInt- AutBWInt-
		LnkSta:	Speed 2.5GT/s, Width x1
			TrErr- Train- SlotClk+ DLActive- BWMgmt- ABWMgmt-
		DevCap2: Completion Timeout: Not Supported, TimeoutDis- NROPrPrP- LTR-
			 10BitTagComp- 10BitTagReq- OBFF Not Supported, ExtFmt- EETLPPrefix-
			 EmergencyPowerReduction Not Supported, EmergencyPowerReductionInit-
			 FRS-
		DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis-
			 IDOReq- IDOCompl- LTR- EmergencyPowerReductionReq-
			 10BitTagReq- OBFF Disabled, EETLPPrefixBlk-
		LnkCtl2: Target Link Speed: 2.5GT/s, EnterCompliance- SpeedDis-
			 Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
			 Compliance Preset/De-emphasis: -6dB de-emphasis, 0dB preshoot
		LnkSta2: Current De-emphasis Level: -6dB, EqualizationComplete- EqualizationPhase1-
			 EqualizationPhase2- EqualizationPhase3- LinkEqualizationRequest-
			 Retimer- 2Retimers- CrosslinkRes: unsupported
	Capabilities: [100 v1] Advanced Error Reporting
		UESta:	DLP- SDES- TLP- FCP- CmpltTO- CmpltAbrt- UnxCmplt- RxOF- MalfTLP-
			ECRC- UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		UEMsk:	DLP- SDES- TLP- FCP- CmpltTO- CmpltAbrt- UnxCmplt- RxOF- MalfTLP-
			ECRC- UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		UESvrt:	DLP+ SDES+ TLP- FCP+ CmpltTO- CmpltAbrt- UnxCmplt- RxOF+ MalfTLP+
			ECRC- UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		CESta:	RxErr- BadTLP- BadDLLP- Rollover- Timeout- AdvNonFatalErr+ CorrIntErr- HeaderOF-
		CEMsk:	RxErr- BadTLP- BadDLLP- Rollover- Timeout- AdvNonFatalErr+ CorrIntErr- HeaderOF-
		AERCap:	First Error Pointer: 00, ECRCGenCap+ ECRCGenEn- ECRCChkCap+ ECRCChkEn-
			MultHdrRecCap- MultHdrRecEn- TLPPfxPres- HdrLogCap-
		HeaderLog: 00000000 00000000 00000000 00000000


--- lspci -tv (tree)
    $ lspci -tv
-[0000:00]-+-00.0  Intel Corporation Xeon E3-1200 v3 Processor DRAM Controller
           +-02.0  Intel Corporation Xeon E3-1200 v3 Processor Integrated Graphics Controller
           +-03.0  Intel Corporation Xeon E3-1200 v3/4th Gen Core Processor HD Audio Controller
           +-14.0  Intel Corporation 8 Series/C220 Series Chipset Family USB xHCI
           +-16.0  Intel Corporation 8 Series/C220 Series Chipset Family MEI Controller #1
           +-19.0  Intel Corporation Ethernet Connection I217-LM
           +-1a.0  Intel Corporation 8 Series/C220 Series Chipset Family USB EHCI #2
           +-1c.0-[01]--
           +-1c.1-[02-03]----00.0-[03]--
           +-1c.4-[04]--
           +-1d.0  Intel Corporation 8 Series/C220 Series Chipset Family USB EHCI #1
           +-1f.0  Intel Corporation C226 Series Chipset Family Server Advanced SKU LPC Controller
           +-1f.2  Intel Corporation 8 Series/C220 Series Chipset Family 4-port SATA Controller 1 [IDE mode]
           \-1f.3  Intel Corporation 8 Series/C220 Series Chipset Family SMBus Controller

--- lspci numa nodes
    $ cat /sys/bus/pci/devices/0000:00:00.0/numa_node /sys/bus/pci/devices/0000:00:02.0/numa_node /sys/bus/pci/devices/0000:00:03.0/numa_node /sys/bus/pci/devices/0000:00:14.0/numa_node /sys/bus/pci/devices/0000:00:16.0/numa_node /sys/bus/pci/devices/0000:00:19.0/numa_node /sys/bus/pci/devices/0000:00:1a.0/numa_node /sys/bus/pci/devices/0000:00:1c.0/numa_node /sys/bus/pci/devices/0000:00:1c.1/numa_node /sys/bus/pci/devices/0000:00:1c.4/numa_node /sys/bus/pci/devices/0000:00:1d.0/numa_node /sys/bus/pci/devices/0000:00:1f.0/numa_node /sys/bus/pci/devices/0000:00:1f.2/numa_node /sys/bus/pci/devices/0000:00:1f.3/numa_node /sys/bus/pci/devices/0000:02:00.0/numa_node
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1

--- lsusb
    $ lsusb
Bus 001 Device 001: ID 1d6b:0002 Linux Foundation 2.0 root hub
Bus 001 Device 002: ID 8087:8008 Intel Corp. Integrated Rate Matching Hub
Bus 001 Device 004: ID 2109:2817 VIA Labs, Inc. USB2.0 Hub             
Bus 001 Device 005: ID 0bda:5411 Realtek Semiconductor Corp. RTS5411 Hub
Bus 001 Device 006: ID 0bda:5411 Realtek Semiconductor Corp. RTS5411 Hub
Bus 001 Device 007: ID 2109:2817 VIA Labs, Inc. USB2.0 Hub             
Bus 001 Device 008: ID 2109:2815 VIA Labs, Inc. USB2.0 Hub             
Bus 001 Device 009: ID 067b:2303 Prolific Technology, Inc. PL2303 Serial Port / Mobile Phone Data Cable
Bus 001 Device 010: ID 067b:2303 Prolific Technology, Inc. PL2303 Serial Port / Mobile Phone Data Cable
Bus 001 Device 011: ID 067b:2303 Prolific Technology, Inc. PL2303 Serial Port / Mobile Phone Data Cable
Bus 001 Device 012: ID 067b:2303 Prolific Technology, Inc. PL2303 Serial Port / Mobile Phone Data Cable
Bus 001 Device 013: ID 2109:2815 VIA Labs, Inc. USB2.0 Hub             
Bus 001 Device 014: ID 067b:2303 Prolific Technology, Inc. PL2303 Serial Port / Mobile Phone Data Cable
Bus 001 Device 016: ID 067b:2303 Prolific Technology, Inc. PL2303 Serial Port / Mobile Phone Data Cable
Bus 001 Device 017: ID 067b:2303 Prolific Technology, Inc. PL2303 Serial Port / Mobile Phone Data Cable
Bus 001 Device 018: ID 067b:2303 Prolific Technology, Inc. PL2303 Serial Port / Mobile Phone Data Cable
Bus 001 Device 019: ID 067b:2303 Prolific Technology, Inc. PL2303 Serial Port / Mobile Phone Data Cable
Bus 002 Device 001: ID 1d6b:0002 Linux Foundation 2.0 root hub
Bus 002 Device 002: ID 8087:8000 Intel Corp. Integrated Rate Matching Hub
Bus 003 Device 001: ID 1d6b:0002 Linux Foundation 2.0 root hub
Bus 004 Device 001: ID 1d6b:0003 Linux Foundation 3.0 root hub
Bus 004 Device 002: ID 2109:0817 VIA Labs, Inc. USB3.0 Hub             
Bus 004 Device 003: ID 0bda:0411 Realtek Semiconductor Corp. Hub
Bus 004 Device 004: ID 0bda:0411 Realtek Semiconductor Corp. Hub
Bus 004 Device 005: ID 2109:0817 VIA Labs, Inc. USB3.0 Hub             
Bus 004 Device 006: ID 0b95:1790 ASIX Electronics Corp. AX88179 Gigabit Ethernet
Bus 004 Device 007: ID 174c:55aa ASMedia Technology Inc. ASM1051E SATA 6Gb/s bridge, ASM1053E SATA 6Gb/s bridge, ASM1153 SATA 3Gb/s bridge, ASM1153E SATA 6Gb/s bridge
Bus 004 Device 008: ID 2109:0815 VIA Labs, Inc. USB3.0 Hub             
Bus 004 Device 009: ID 1058:2647 Western Digital Technologies, Inc. easystore 2647
Bus 004 Device 010: ID 0b95:1790 ASIX Electronics Corp. AX88179 Gigabit Ethernet
Bus 004 Device 011: ID 2109:0815 VIA Labs, Inc. USB3.0 Hub             

--- lshw -short
    $ lshw -short
H/W path                   Device           Class          Description
======================================================================
                                            system         Precision T1700 (Precision T1700)
/0                                          bus            048DY8
/0/0                                        memory         64KiB BIOS
/0/3a                                       processor      Intel(R) Xeon(R) CPU E3-1246 v3 @ 3.50GHz
/0/3a/3b                                    memory         256KiB L1 cache
/0/3a/3c                                    memory         1MiB L2 cache
/0/3a/3d                                    memory         8MiB L3 cache
/0/3e                                       memory         16GiB System Memory
/0/3e/0                                     memory         4GiB DIMM DDR3 Synchronous 1600 MHz (0.6 ns)
/0/3e/1                                     memory         4GiB DIMM DDR3 Synchronous 1600 MHz (0.6 ns)
/0/3e/2                                     memory         4GiB DIMM DDR3 Synchronous 1600 MHz (0.6 ns)
/0/3e/3                                     memory         4GiB DIMM DDR3 Synchronous 1600 MHz (0.6 ns)
/0/100                                      bridge         Xeon E3-1200 v3 Processor DRAM Controller
/0/100/2                   /dev/fb0         display        Xeon E3-1200 v3 Processor Integrated Graphics Controller
/0/100/3                   card0            multimedia     Xeon E3-1200 v3/4th Gen Core Processor HD Audio Controller
/0/100/3/0                 input4           input          HDA Intel HDMI HDMI/DP,pcm=3
/0/100/3/1                 input5           input          HDA Intel HDMI HDMI/DP,pcm=7
/0/100/3/2                 input6           input          HDA Intel HDMI HDMI/DP,pcm=8
/0/100/14                                   bus            8 Series/C220 Series Chipset Family USB xHCI
/0/100/14/0                usb3             bus            xHCI Host Controller
/0/100/14/1                usb4             bus            xHCI Host Controller
/0/100/14/1/1                               bus            USB3.0 Hub
/0/100/14/1/1/4                             bus            USB3.0 Hub
/0/100/14/1/1/4/2          scsi3            storage        easystore 2647
/0/100/14/1/1/4/2/0.0.0    /dev/sdf         disk           5TB easystore 2647
/0/100/14/1/1/4/2/0.0.0/1  /dev/sdf1        volume         4657GiB EXT4 volume
/0/100/14/1/1/4/2/0.0.1                     generic        SES Device
/0/100/14/1/2                               bus            USB3.2 Hub
/0/100/14/1/2/1                             bus            USB3.2 Hub
/0/100/14/1/2/1/3          scsi2            storage        ThinkPlus
/0/100/14/1/2/1/3/0.0.0    /dev/sde         disk           512GB ThinkPlus
/0/100/14/1/2/1/3/0.0.0/1  /dev/sde1        volume         476GiB EXT4 volume
/0/100/14/1/2/2                             communication  AX88179A
/0/100/14/1/2/3                             bus            USB3.0 Hub
/0/100/14/1/2/3/3                           bus            USB3.0 Hub
/0/100/14/1/2/4                             communication  AX88179B
/0/100/16                                   communication  8 Series/C220 Series Chipset Family MEI Controller #1
/0/100/19                  nic0             network        Ethernet Connection I217-LM
/0/100/1a                                   bus            8 Series/C220 Series Chipset Family USB EHCI #2
/0/100/1a/1                usb1             bus            EHCI Host Controller
/0/100/1a/1/1                               bus            Integrated Rate Matching Hub
/0/100/1a/1/1/5                             bus            USB2.0 Hub
/0/100/1a/1/1/5/4                           bus            USB2.0 Hub
/0/100/1a/1/1/5/4/1                         generic        USB-Serial Controller D
/0/100/1a/1/1/5/4/4                         generic        USB-Serial Controller
/0/100/1a/1/1/6                             bus            USB2.1 Hub
/0/100/1a/1/1/6/1                           bus            USB2.1 Hub
/0/100/1a/1/1/6/3                           bus            USB2.0 Hub
/0/100/1a/1/1/6/3/1                         generic        USB-Serial Controller D
/0/100/1a/1/1/6/3/2                         generic        USB-Serial Controller
/0/100/1a/1/1/6/3/3                         bus            USB2.0 Hub
/0/100/1a/1/1/6/3/3/1                       generic        USB-Serial Controller
/0/100/1a/1/1/6/3/3/2                       generic        USB-Serial Controller D
/0/100/1a/1/1/6/3/3/3                       generic        USB-Serial Controller D
/0/100/1a/1/1/6/3/3/4                       generic        USB-Serial Controller
/0/100/1a/1/1/6/3/4                         generic        USB-Serial Controller
/0/100/1c                                   bridge         8 Series/C220 Series Chipset Family PCI Express Root Port #1
/0/100/1c.1                                 bridge         8 Series/C220 Series Chipset Family PCI Express Root Port #2
/0/100/1c.1/0                               bridge         XIO2001 PCI Express-to-PCI Bridge
/0/100/1c.4                                 bridge         8 Series/C220 Series Chipset Family PCI Express Root Port #5
/0/100/1d                                   bus            8 Series/C220 Series Chipset Family USB EHCI #1
/0/100/1d/1                usb2             bus            EHCI Host Controller
/0/100/1d/1/1                               bus            Integrated Rate Matching Hub
/0/100/1f                                   bridge         C226 Series Chipset Family Server Advanced SKU LPC Controller
/0/100/1f/0                                 system         PnP device PNP0c01
/0/100/1f/1                                 system         PnP device PNP0c02
/0/100/1f/2                                 system         PnP device PNP0b00
/0/100/1f/3                                 system         PnP device PNP0c02
/0/100/1f/4                                 system         PnP device PNP0c02
/0/100/1f/5                                 communication  PnP device PNP0501
/0/100/1f/6                                 system         PnP device PNP0c02
/0/100/1f.2                scsi0            storage        8 Series/C220 Series Chipset Family 4-port SATA Controller 1 [IDE mode]
/0/100/1f.2/0              /dev/sda         disk           2TB Hitachi HDS72302
/0/100/1f.2/0/1            /dev/sda1        volume         1863GiB EXT4 volume
/0/100/1f.2/1              /dev/sdb         volume         1863GiB HITACHI HUA72302
/0/100/1f.2/2              /dev/sdc         disk           3TB WDC WD30EFRX-68E
/0/100/1f.2/2/1            /dev/sdc1        volume         2794GiB EXT4 volume
/0/100/1f.2/3              /dev/sdd         disk           1TB WDC WD10EZRX-00A
/0/100/1f.2/3/1            /dev/sdd1        volume         1006KiB BIOS Boot partition
/0/100/1f.2/3/2            /dev/sdd2        volume         1023MiB Windows FAT volume
/0/100/1f.2/3/3            /dev/sdd3        volume         930GiB LVM Physical Volume
/0/100/1f.3                                 bus            8 Series/C220 Series Chipset Family SMBus Controller
/1                         input0           input          Power Button
/2                         input1           input          Power Button
/3                         input2           input          PC Speaker
/4                         input3           input          Video Bus
/5                         enx8cae4ccda926  network        Ethernet interface
/6                         enx80ae4ccdec03  network        Ethernet interface

--- PCIe AER errors
    [missing: /sys/bus/pci/devices/0000:02:00.0/aer_dev_correctable]

--- PCIe AER summary (errors matter for NIC/NVMe stability)
    $ found=0
for d in /sys/bus/pci/devices/*; do
    [ -d "$d" ] || continue
    addr="$(basename "$d")"
    class="$(cat "$d/class" 2>/dev/null)"
    case "$class" in
        0x020000|0x010802|0x010700) ;;  # ethernet, nvme, raid
        *) continue ;;
    esac
    for f in "$d"/aer_dev_*; do
        [ -r "$f" ] || continue
        val="$(cat "$f" 2>/dev/null)"
        [ "$val" = "0" ] && continue
        [ "$val" = "" ] && continue
        printf '%s %s = %s\n' "$addr" "$(basename "$f")" "$val"
        found=1
    done
done
[ "$found" = "0" ] && echo "  no AER errors on NIC/NVMe/RAID devices"
  no AER errors on NIC/NVMe/RAID devices

###############################################################################
# 4. CPU POWER / FREQUENCY / IDLE STATES
###############################################################################

--- scaling_governor per cpu (counts)
    $ for c in /sys/devices/system/cpu/cpu*/cpufreq/scaling_governor; do
    [ -e "$c" ] || continue
    cat "$c"
done | sort | uniq -c
      8 performance

--- scaling_driver / available governors / freq limits
    $ for f in /sys/devices/system/cpu/cpu0/cpufreq/*; do
    [ -r "$f" ] || continue
    [ -d "$f" ] && continue
    printf '%-40s = %s\n' "$(basename "$f")" "$(cat "$f" 2>/dev/null)"
done
affected_cpus                            = 0
cpuinfo_avg_freq                         = 3711839
cpuinfo_max_freq                         = 3900000
cpuinfo_min_freq                         = 800000
cpuinfo_transition_latency               = 20000
related_cpus                             = 0
scaling_available_governors              = conservative ondemand userspace powersave performance schedutil 
scaling_cur_freq                         = 3721565
scaling_driver                           = intel_cpufreq
scaling_governor                         = performance
scaling_max_freq                         = 3900000
scaling_min_freq                         = 3900000
scaling_setspeed                         = <unsupported>

--- EPP / EPB / intel_pstate
    $ echo "intel_pstate status: $(cat /sys/devices/system/cpu/intel_pstate/status 2>/dev/null)"
echo "intel_pstate no_turbo: $(cat /sys/devices/system/cpu/intel_pstate/no_turbo 2>/dev/null)"
echo "intel_pstate turbo_pct: $(cat /sys/devices/system/cpu/intel_pstate/turbo_pct 2>/dev/null)"
echo "intel_pstate max_perf_pct: $(cat /sys/devices/system/cpu/intel_pstate/max_perf_pct 2>/dev/null)"
echo "intel_pstate min_perf_pct: $(cat /sys/devices/system/cpu/intel_pstate/min_perf_pct 2>/dev/null)"
echo "EPB (energy_perf_bias) per cpu:"
for c in /sys/devices/system/cpu/cpu*/power/energy_perf_bias; do
    [ -r "$c" ] || continue
    printf '  %s : %s\n' "$(echo "$c" | cut -d/ -f5)" "$(cat "$c" 2>/dev/null)"
done | sort | uniq -c
echo "EPP (energy_performance_preference) per cpu:"
for c in /sys/devices/system/cpu/cpu*/cpufreq/energy_performance_preference; do
    [ -r "$c" ] || continue
    printf '  %s : %s\n' "$(echo "$c" | cut -d/ -f5)" "$(cat "$c" 2>/dev/null)"
done | sort | uniq -c
echo "available EPP:"
cat /sys/devices/system/cpu/cpu0/cpufreq/energy_performance_available_preferences 2>/dev/null
intel_pstate status: passive
intel_pstate no_turbo: 0
intel_pstate turbo_pct: 13
intel_pstate max_perf_pct: 100
intel_pstate min_perf_pct: 100
EPB (energy_perf_bias) per cpu:
      8   cpu : 0
EPP (energy_performance_preference) per cpu:
available EPP:
    [exit=1]

--- cpupower frequency-info
    $ cpupower frequency-info
analyzing CPU 6:
  driver: intel_cpufreq
  CPUs which run at the same hardware frequency: 6
  CPUs which need to have their frequency coordinated by software: 6
  maximum transition latency: 20.0 us
  hardware limits: 800 MHz - 3.90 GHz
  available cpufreq governors: conservative ondemand userspace powersave performance schedutil
  current policy: frequency should be within 3.90 GHz and 3.90 GHz.
                  The governor "performance" may decide which speed to use
                  within this range.
  current CPU frequency: Unable to call hardware
  current CPU frequency: 3.84 GHz (asserted by call to kernel)
  boost state support:
    Supported: yes
    Active: yes

--- turbostat snapshot
    $ timeout 3 turbostat --quiet --show CPU,Core,Bzy_MHz,IRQ,Busy%,Bzy_MHz,TSC_MHz,CoreTmp,PkgTmp sleep 1
1.001476 sec
Core	CPU	Busy%	Bzy_MHz	TSC_MHz	IRQ	CoreTmp	PkgTmp
-	-	0.82	3853	3492	3103	30	30
0	0	0.65	3845	3492	437	25	30
0	4	1.12	3866	3492	497
1	1	0.77	3867	3492	309	23
1	5	0.33	3850	3492	19
2	2	0.61	3830	3492	254	24
2	6	0.94	3855	3492	595
3	3	0.96	3838	3492	460	30
3	7	1.15	3856	3492	532

--- x86_energy_perf_policy -r
    $ x86_energy_perf_policy -r
cpu0: EPB 0
cpu1: EPB 0
cpu2: EPB 0
cpu3: EPB 0
cpu4: EPB 0
cpu5: EPB 0
cpu6: EPB 0
cpu7: EPB 0

--- C-states (idle) enabled per cpu0
    $ for s in /sys/devices/system/cpu/cpu0/cpuidle/state*; do
    [ -d "$s" ] || continue
    printf '  %s : %s disabled=%s  latency=%sus  residency=%sus\n' \
        "$(cat "$s/name" 2>/dev/null)" \
        "$(cat "$s/desc" 2>/dev/null)" \
        "$(cat "$s/disable" 2>/dev/null)" \
        "$(cat "$s/latency" 2>/dev/null)" \
        "$(cat "$s/time" 2>/dev/null)"
done
  POLL : CPUIDLE CORE POLL IDLE disabled=0  latency=0us  residency=7298042us
  C1 : MWAIT 0x00 disabled=0  latency=2us  residency=401817754us
  C1E : MWAIT 0x01 disabled=0  latency=10us  residency=1934479313us
  C3 : MWAIT 0x10 disabled=0  latency=33us  residency=6450125894us
  C6 : MWAIT 0x20 disabled=0  latency=133us  residency=1921855651us
  C7s : MWAIT 0x32 disabled=0  latency=166us  residency=378694876644us

--- THP enabled
    $ cat /sys/kernel/mm/transparent_hugepage/enabled
always [madvise] never

--- THP defrag
    $ cat /sys/kernel/mm/transparent_hugepage/defrag
always defer defer+madvise [madvise] never

--- THP khugepaged pages_to_scan
    $ cat /sys/kernel/mm/transparent_hugepage/khugepaged/pages_to_scan
4096

--- THP khugepaged defrag
    $ cat /sys/kernel/mm/transparent_hugepage/khugepaged/defrag
1

--- microcode
    $ dmesg
[    0.000000] Linux version 6.17.9-1-pve (build@proxmox) (gcc (Debian 14.2.0-19) 14.2.0, GNU ld (GNU Binutils for Debian) 2.44) #1 SMP PREEMPT_DYNAMIC PMX 6.17.9-1 (2026-01-12T16:25Z) ()
[    0.000000] Command line: BOOT_IMAGE=/boot/vmlinuz-6.17.9-1-pve root=/dev/mapper/pve-root ro quiet
[    0.000000] KERNEL supported cpus:
[    0.000000]   Intel GenuineIntel
[    0.000000]   AMD AuthenticAMD
[    0.000000]   Hygon HygonGenuine
[    0.000000]   Centaur CentaurHauls
[    0.000000]   zhaoxin   Shanghai  
[    0.000000] BIOS-provided physical RAM map:
[    0.000000] BIOS-e820: [mem 0x0000000000000000-0x000000000009ebff] usable
[    0.000000] BIOS-e820: [mem 0x000000000009ec00-0x000000000009ffff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000000e0000-0x00000000000fffff] reserved
[    0.000000] BIOS-e820: [mem 0x0000000000100000-0x00000000d1a67fff] usable
[    0.000000] BIOS-e820: [mem 0x00000000d1a68000-0x00000000d1a6efff] ACPI NVS
[    0.000000] BIOS-e820: [mem 0x00000000d1a6f000-0x00000000d1ea0fff] usable
[    0.000000] BIOS-e820: [mem 0x00000000d1ea1000-0x00000000d2331fff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000d2332000-0x00000000d7edafff] usable
[    0.000000] BIOS-e820: [mem 0x00000000d7edb000-0x00000000d7ffffff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000d8000000-0x00000000d875ffff] usable
[    0.000000] BIOS-e820: [mem 0x00000000d8760000-0x00000000d87fffff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000d8800000-0x00000000d8fadfff] usable
[    0.000000] BIOS-e820: [mem 0x00000000d8fae000-0x00000000d8ffffff] ACPI data
[    0.000000] BIOS-e820: [mem 0x00000000d9000000-0x00000000da71bfff] usable
[    0.000000] BIOS-e820: [mem 0x00000000da71c000-0x00000000da7fffff] ACPI NVS
[    0.000000] BIOS-e820: [mem 0x00000000da800000-0x00000000dbe0cfff] usable
[    0.000000] BIOS-e820: [mem 0x00000000dbe0d000-0x00000000dbffffff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000dd000000-0x00000000df1fffff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000f8000000-0x00000000fbffffff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000fec00000-0x00000000fec00fff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000fed00000-0x00000000fed03fff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000fed1c000-0x00000000fed1ffff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000fee00000-0x00000000fee00fff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000ff000000-0x00000000ffffffff] reserved
[    0.000000] BIOS-e820: [mem 0x0000000100000000-0x000000041edfffff] usable
[    0.000000] NX (Execute Disable) protection: active
[    0.000000] APIC: Static calls initialized
[    0.000000] SMBIOS 2.7 present.
[    0.000000] DMI: Dell Inc. Precision T1700/048DY8, BIOS A13 12/19/2014
[    0.000000] DMI: Memory slots populated: 4/4
[    0.000000] tsc: Fast TSC calibration using PIT
[    0.000000] tsc: Detected 3491.870 MHz processor
[    0.000721] e820: update [mem 0x00000000-0x00000fff] usable ==> reserved
[    0.000723] e820: remove [mem 0x000a0000-0x000fffff] usable
[    0.000733] last_pfn = 0x41ee00 max_arch_pfn = 0x400000000
[    0.000739] total RAM covered: 16318M
[    0.000886]  gran_size: 64K 	chunk_size: 64K 	num_reg: 10  	lose cover RAM: 110M
[    0.000887]  gran_size: 64K 	chunk_size: 128K 	num_reg: 10  	lose cover RAM: 110M
[    0.000889]  gran_size: 64K 	chunk_size: 256K 	num_reg: 10  	lose cover RAM: 110M
[    0.000890]  gran_size: 64K 	chunk_size: 512K 	num_reg: 10  	lose cover RAM: 110M
[    0.000891]  gran_size: 64K 	chunk_size: 1M 	num_reg: 10  	lose cover RAM: 110M
[    0.000892]  gran_size: 64K 	chunk_size: 2M 	num_reg: 10  	lose cover RAM: 110M
[    0.000893]  gran_size: 64K 	chunk_size: 4M 	num_reg: 10  	lose cover RAM: 110M
[    0.000894]  gran_size: 64K 	chunk_size: 8M 	num_reg: 10  	lose cover RAM: 110M
[    0.000895]  gran_size: 64K 	chunk_size: 16M 	num_reg: 10  	lose cover RAM: 110M
[    0.000896] *BAD*gran_size: 64K 	chunk_size: 32M 	num_reg: 10  	lose cover RAM: -18M
[    0.000897]  gran_size: 64K 	chunk_size: 64M 	num_reg: 10  	lose cover RAM: 0G
[    0.000899]  gran_size: 64K 	chunk_size: 128M 	num_reg: 10  	lose cover RAM: 0G
[    0.000900]  gran_size: 64K 	chunk_size: 256M 	num_reg: 10  	lose cover RAM: 0G
[    0.000901]  gran_size: 64K 	chunk_size: 512M 	num_reg: 10  	lose cover RAM: 0G
[    0.000902]  gran_size: 64K 	chunk_size: 1G 	num_reg: 10  	lose cover RAM: 0G
[    0.000903] *BAD*gran_size: 64K 	chunk_size: 2G 	num_reg: 10  	lose cover RAM: -1G
[    0.000904]  gran_size: 128K 	chunk_size: 128K 	num_reg: 10  	lose cover RAM: 110M
[    0.000905]  gran_size: 128K 	chunk_size: 256K 	num_reg: 10  	lose cover RAM: 110M
[    0.000906]  gran_size: 128K 	chunk_size: 512K 	num_reg: 10  	lose cover RAM: 110M
[    0.000907]  gran_size: 128K 	chunk_size: 1M 	num_reg: 10  	lose cover RAM: 110M
[    0.000908]  gran_size: 128K 	chunk_size: 2M 	num_reg: 10  	lose cover RAM: 110M
[    0.000909]  gran_size: 128K 	chunk_size: 4M 	num_reg: 10  	lose cover RAM: 110M
[    0.000910]  gran_size: 128K 	chunk_size: 8M 	num_reg: 10  	lose cover RAM: 110M
[    0.000911]  gran_size: 128K 	chunk_size: 16M 	num_reg: 10  	lose cover RAM: 110M
[    0.000912] *BAD*gran_size: 128K 	chunk_size: 32M 	num_reg: 10  	lose cover RAM: -18M
[    0.000913]  gran_size: 128K 	chunk_size: 64M 	num_reg: 10  	lose cover RAM: 0G
[    0.000914]  gran_size: 128K 	chunk_size: 128M 	num_reg: 10  	lose cover RAM: 0G
[    0.000915]  gran_size: 128K 	chunk_size: 256M 	num_reg: 10  	lose cover RAM: 0G
[    0.000916]  gran_size: 128K 	chunk_size: 512M 	num_reg: 10  	lose cover RAM: 0G
[    0.000918]  gran_size: 128K 	chunk_size: 1G 	num_reg: 10  	lose cover RAM: 0G
[    0.000919] *BAD*gran_size: 128K 	chunk_size: 2G 	num_reg: 10  	lose cover RAM: -1G
[    0.000920]  gran_size: 256K 	chunk_size: 256K 	num_reg: 10  	lose cover RAM: 110M
[    0.000921]  gran_size: 256K 	chunk_size: 512K 	num_reg: 10  	lose cover RAM: 110M
[    0.000922]  gran_size: 256K 	chunk_size: 1M 	num_reg: 10  	lose cover RAM: 110M
[    0.000923]  gran_size: 256K 	chunk_size: 2M 	num_reg: 10  	lose cover RAM: 110M
[    0.000924]  gran_size: 256K 	chunk_size: 4M 	num_reg: 10  	lose cover RAM: 110M
[    0.000925]  gran_size: 256K 	chunk_size: 8M 	num_reg: 10  	lose cover RAM: 110M
[    0.000926]  gran_size: 256K 	chunk_size: 16M 	num_reg: 10  	lose cover RAM: 110M
[    0.000927] *BAD*gran_size: 256K 	chunk_size: 32M 	num_reg: 10  	lose cover RAM: -18M
[    0.000928]  gran_size: 256K 	chunk_size: 64M 	num_reg: 10  	lose cover RAM: 0G
[    0.000929]  gran_size: 256K 	chunk_size: 128M 	num_reg: 10  	lose cover RAM: 0G
[    0.000930]  gran_size: 256K 	chunk_size: 256M 	num_reg: 10  	lose cover RAM: 0G
[    0.000931]  gran_size: 256K 	chunk_size: 512M 	num_reg: 10  	lose cover RAM: 0G
[    0.000932]  gran_size: 256K 	chunk_size: 1G 	num_reg: 10  	lose cover RAM: 0G
[    0.000933] *BAD*gran_size: 256K 	chunk_size: 2G 	num_reg: 10  	lose cover RAM: -1G
[    0.000934]  gran_size: 512K 	chunk_size: 512K 	num_reg: 10  	lose cover RAM: 110M
[    0.000935]  gran_size: 512K 	chunk_size: 1M 	num_reg: 10  	lose cover RAM: 110M
[    0.000936]  gran_size: 512K 	chunk_size: 2M 	num_reg: 10  	lose cover RAM: 110M
[    0.000937]  gran_size: 512K 	chunk_size: 4M 	num_reg: 10  	lose cover RAM: 110M
[    0.000938]  gran_size: 512K 	chunk_size: 8M 	num_reg: 10  	lose cover RAM: 110M
[    0.000939]  gran_size: 512K 	chunk_size: 16M 	num_reg: 10  	lose cover RAM: 110M
[    0.000940] *BAD*gran_size: 512K 	chunk_size: 32M 	num_reg: 10  	lose cover RAM: -18M
[    0.000942]  gran_size: 512K 	chunk_size: 64M 	num_reg: 10  	lose cover RAM: 0G
[    0.000943]  gran_size: 512K 	chunk_size: 128M 	num_reg: 10  	lose cover RAM: 0G
[    0.000944]  gran_size: 512K 	chunk_size: 256M 	num_reg: 10  	lose cover RAM: 0G
[    0.000945]  gran_size: 512K 	chunk_size: 512M 	num_reg: 10  	lose cover RAM: 0G
[    0.000946]  gran_size: 512K 	chunk_size: 1G 	num_reg: 10  	lose cover RAM: 0G
[    0.000947] *BAD*gran_size: 512K 	chunk_size: 2G 	num_reg: 10  	lose cover RAM: -1G
[    0.000948]  gran_size: 1M 	chunk_size: 1M 	num_reg: 10  	lose cover RAM: 110M
[    0.000949]  gran_size: 1M 	chunk_size: 2M 	num_reg: 10  	lose cover RAM: 110M
[    0.000950]  gran_size: 1M 	chunk_size: 4M 	num_reg: 10  	lose cover RAM: 110M
[    0.000951]  gran_size: 1M 	chunk_size: 8M 	num_reg: 10  	lose cover RAM: 110M
[    0.000952]  gran_size: 1M 	chunk_size: 16M 	num_reg: 10  	lose cover RAM: 110M
[    0.000953] *BAD*gran_size: 1M 	chunk_size: 32M 	num_reg: 10  	lose cover RAM: -18M
[    0.000954]  gran_size: 1M 	chunk_size: 64M 	num_reg: 10  	lose cover RAM: 0G
[    0.000955]  gran_size: 1M 	chunk_size: 128M 	num_reg: 10  	lose cover RAM: 0G
[    0.000956]  gran_size: 1M 	chunk_size: 256M 	num_reg: 10  	lose cover RAM: 0G
[    0.000957]  gran_size: 1M 	chunk_size: 512M 	num_reg: 10  	lose cover RAM: 0G
[    0.000958]  gran_size: 1M 	chunk_size: 1G 	num_reg: 10  	lose cover RAM: 0G
[    0.000959] *BAD*gran_size: 1M 	chunk_size: 2G 	num_reg: 10  	lose cover RAM: -1G
[    0.000960]  gran_size: 2M 	chunk_size: 2M 	num_reg: 10  	lose cover RAM: 110M
[    0.000961]  gran_size: 2M 	chunk_size: 4M 	num_reg: 10  	lose cover RAM: 110M
[    0.000962]  gran_size: 2M 	chunk_size: 8M 	num_reg: 10  	lose cover RAM: 110M
[    0.000963]  gran_size: 2M 	chunk_size: 16M 	num_reg: 10  	lose cover RAM: 110M
[    0.000964] *BAD*gran_size: 2M 	chunk_size: 32M 	num_reg: 10  	lose cover RAM: -18M
[    0.000965]  gran_size: 2M 	chunk_size: 64M 	num_reg: 10  	lose cover RAM: 0G
[    0.000966]  gran_size: 2M 	chunk_size: 128M 	num_reg: 10  	lose cover RAM: 0G
[    0.000967]  gran_size: 2M 	chunk_size: 256M 	num_reg: 10  	lose cover RAM: 0G
[    0.000968]  gran_size: 2M 	chunk_size: 512M 	num_reg: 10  	lose cover RAM: 0G
[    0.000969]  gran_size: 2M 	chunk_size: 1G 	num_reg: 10  	lose cover RAM: 0G
[    0.000970] *BAD*gran_size: 2M 	chunk_size: 2G 	num_reg: 10  	lose cover RAM: -1G
[    0.000971]  gran_size: 4M 	chunk_size: 4M 	num_reg: 10  	lose cover RAM: 110M
[    0.000972]  gran_size: 4M 	chunk_size: 8M 	num_reg: 10  	lose cover RAM: 110M
[    0.000973]  gran_size: 4M 	chunk_size: 16M 	num_reg: 10  	lose cover RAM: 110M
[    0.000974] *BAD*gran_size: 4M 	chunk_size: 32M 	num_reg: 10  	lose cover RAM: -18M
[    0.000976]  gran_size: 4M 	chunk_size: 64M 	num_reg: 10  	lose cover RAM: 2M
[    0.000977]  gran_size: 4M 	chunk_size: 128M 	num_reg: 10  	lose cover RAM: 2M
[    0.000978]  gran_size: 4M 	chunk_size: 256M 	num_reg: 10  	lose cover RAM: 2M
[    0.000979]  gran_size: 4M 	chunk_size: 512M 	num_reg: 10  	lose cover RAM: 2M
[    0.000980]  gran_size: 4M 	chunk_size: 1G 	num_reg: 10  	lose cover RAM: 2M
[    0.000981] *BAD*gran_size: 4M 	chunk_size: 2G 	num_reg: 10  	lose cover RAM: -1022M
[    0.000982]  gran_size: 8M 	chunk_size: 8M 	num_reg: 10  	lose cover RAM: 110M
[    0.000983]  gran_size: 8M 	chunk_size: 16M 	num_reg: 10  	lose cover RAM: 110M
[    0.000984] *BAD*gran_size: 8M 	chunk_size: 32M 	num_reg: 10  	lose cover RAM: -18M
[    0.000985]  gran_size: 8M 	chunk_size: 64M 	num_reg: 10  	lose cover RAM: 6M
[    0.000986]  gran_size: 8M 	chunk_size: 128M 	num_reg: 10  	lose cover RAM: 6M
[    0.000987]  gran_size: 8M 	chunk_size: 256M 	num_reg: 10  	lose cover RAM: 6M
[    0.000988]  gran_size: 8M 	chunk_size: 512M 	num_reg: 10  	lose cover RAM: 6M
[    0.000989]  gran_size: 8M 	chunk_size: 1G 	num_reg: 10  	lose cover RAM: 6M
[    0.000990] *BAD*gran_size: 8M 	chunk_size: 2G 	num_reg: 10  	lose cover RAM: -1018M
[    0.000991]  gran_size: 16M 	chunk_size: 16M 	num_reg: 10  	lose cover RAM: 110M
[    0.000992]  gran_size: 16M 	chunk_size: 32M 	num_reg: 10  	lose cover RAM: 238M
[    0.000993]  gran_size: 16M 	chunk_size: 64M 	num_reg: 9  	lose cover RAM: 14M
[    0.000994]  gran_size: 16M 	chunk_size: 128M 	num_reg: 9  	lose cover RAM: 14M
[    0.000995]  gran_size: 16M 	chunk_size: 256M 	num_reg: 9  	lose cover RAM: 14M
[    0.000996]  gran_size: 16M 	chunk_size: 512M 	num_reg: 9  	lose cover RAM: 14M
[    0.000997]  gran_size: 16M 	chunk_size: 1G 	num_reg: 9  	lose cover RAM: 14M
[    0.000998]  gran_size: 16M 	chunk_size: 2G 	num_reg: 10  	lose cover RAM: 14M
[    0.000999]  gran_size: 32M 	chunk_size: 32M 	num_reg: 10  	lose cover RAM: 62M
[    0.001000]  gran_size: 32M 	chunk_size: 64M 	num_reg: 9  	lose cover RAM: 30M
[    0.001001]  gran_size: 32M 	chunk_size: 128M 	num_reg: 8  	lose cover RAM: 30M
[    0.001002]  gran_size: 32M 	chunk_size: 256M 	num_reg: 8  	lose cover RAM: 30M
[    0.001003]  gran_size: 32M 	chunk_size: 512M 	num_reg: 8  	lose cover RAM: 30M
[    0.001004]  gran_size: 32M 	chunk_size: 1G 	num_reg: 8  	lose cover RAM: 30M
[    0.001005]  gran_size: 32M 	chunk_size: 2G 	num_reg: 9  	lose cover RAM: 30M
[    0.001007]  gran_size: 64M 	chunk_size: 64M 	num_reg: 10  	lose cover RAM: 62M
[    0.001008]  gran_size: 64M 	chunk_size: 128M 	num_reg: 8  	lose cover RAM: 62M
[    0.001009]  gran_size: 64M 	chunk_size: 256M 	num_reg: 8  	lose cover RAM: 62M
[    0.001010]  gran_size: 64M 	chunk_size: 512M 	num_reg: 8  	lose cover RAM: 62M
[    0.001011]  gran_size: 64M 	chunk_size: 1G 	num_reg: 8  	lose cover RAM: 62M
[    0.001012]  gran_size: 64M 	chunk_size: 2G 	num_reg: 9  	lose cover RAM: 62M
[    0.001013]  gran_size: 128M 	chunk_size: 128M 	num_reg: 8  	lose cover RAM: 190M
[    0.001014]  gran_size: 128M 	chunk_size: 256M 	num_reg: 8  	lose cover RAM: 190M
[    0.001015]  gran_size: 128M 	chunk_size: 512M 	num_reg: 8  	lose cover RAM: 190M
[    0.001016]  gran_size: 128M 	chunk_size: 1G 	num_reg: 8  	lose cover RAM: 190M
[    0.001017]  gran_size: 128M 	chunk_size: 2G 	num_reg: 9  	lose cover RAM: 190M
[    0.001018]  gran_size: 256M 	chunk_size: 256M 	num_reg: 6  	lose cover RAM: 446M
[    0.001019]  gran_size: 256M 	chunk_size: 512M 	num_reg: 8  	lose cover RAM: 446M
[    0.001020]  gran_size: 256M 	chunk_size: 1G 	num_reg: 8  	lose cover RAM: 446M
[    0.001021]  gran_size: 256M 	chunk_size: 2G 	num_reg: 9  	lose cover RAM: 446M
[    0.001022]  gran_size: 512M 	chunk_size: 512M 	num_reg: 4  	lose cover RAM: 958M
[    0.001023]  gran_size: 512M 	chunk_size: 1G 	num_reg: 4  	lose cover RAM: 958M
[    0.001024]  gran_size: 512M 	chunk_size: 2G 	num_reg: 4  	lose cover RAM: 958M
[    0.001025]  gran_size: 1G 	chunk_size: 1G 	num_reg: 4  	lose cover RAM: 958M
[    0.001026]  gran_size: 1G 	chunk_size: 2G 	num_reg: 4  	lose cover RAM: 958M
[    0.001027]  gran_size: 2G 	chunk_size: 2G 	num_reg: 3  	lose cover RAM: 1982M
[    0.001028] mtrr_cleanup: can not find optimal value
[    0.001029] please specify mtrr_gran_size/mtrr_chunk_size
[    0.001030] MTRR map: 9 entries (5 fixed + 4 variable; max 25), built from 10 variable MTRRs
[    0.001032] x86/PAT: Configuration [0-7]: WB  WC  UC- UC  WB  WP  UC- WT  
[    0.001327] e820: update [mem 0xdd000000-0xffffffff] usable ==> reserved
[    0.001331] last_pfn = 0xdbe0d max_arch_pfn = 0x400000000
[    0.007284] found SMP MP-table at [mem 0x000fd970-0x000fd97f]
[    0.007300] Using GB pages for direct mapping
[    0.007908] RAMDISK: [mem 0x2d651000-0x32b1ffff]
[    0.007917] ACPI: Early table checksum verification disabled
[    0.007920] ACPI: RSDP 0x00000000000F0490 000024 (v02 DELL  )
[    0.007923] ACPI: XSDT 0x00000000D8FED098 0000B4 (v01 DELL   CBX3     01072009 AMI  00010013)
[    0.007929] ACPI: FACP 0x00000000D8FF8D18 00010C (v05 DELL   CBX3     01072009 AMI  00010013)
[    0.007933] ACPI: DSDT 0x00000000D8FED1E0 00BB35 (v02 DELL   CBX3     00000014 INTL 20091112)
[    0.007936] ACPI: FACS 0x00000000DA7FE080 000040
[    0.007938] ACPI: APIC 0x00000000D8FF8E28 000092 (v03 DELL   CBX3     01072009 AMI  00010013)
[    0.007941] ACPI: FPDT 0x00000000D8FF8EC0 000044 (v01 DELL   CBX3     01072009 AMI  00010013)
[    0.007943] ACPI: SLIC 0x00000000D8FF8F08 000176 (v03 DELL   CBX3     01072009 MSFT 00010013)
[    0.007946] ACPI: LPIT 0x00000000D8FF9080 00005C (v01 DELL   CBX3     00000000 AMI. 00000005)
[    0.007948] ACPI: SSDT 0x00000000D8FF90E0 000539 (v01 PmRef  Cpu0Ist  00003000 INTL 20120711)
[    0.007951] ACPI: SSDT 0x00000000D8FF9620 000AD8 (v01 PmRef  CpuPm    00003000 INTL 20120711)
[    0.007954] ACPI: HPET 0x00000000D8FFA0F8 000038 (v01 DELL   CBX3     01072009 AMI. 00000005)
[    0.007956] ACPI: SSDT 0x00000000D8FFA130 000495 (v01 IdeRef IdeTable 00001000 INTL 20120711)
[    0.007959] ACPI: MCFG 0x00000000D8FFA5C8 00003C (v01 DELL   CBX3     01072009 MSFT 00000097)
[    0.007961] ACPI: SSDT 0x00000000D8FFA608 0034D6 (v01 SaSsdt SaSsdt   00003000 INTL 20091112)
[    0.007964] ACPI: ASF! 0x00000000D8FFDAE0 0000A5 (v32 INTEL   HCG     00000001 TFSM 000F4240)
[    0.007966] ACPI: MSDM 0x00000000D8FFDB88 000055 (v03 DELL   CBX3     06222004 AMI  00010013)
[    0.007969] ACPI: DMAR 0x00000000D8FFDBE0 0000B8 (v01 INTEL  HSW      00000001 INTL 00000001)
[    0.007972] ACPI: EINJ 0x00000000D8FFDC98 000130 (v01 AMI    AMI EINJ 00000000      00000000)
[    0.007974] ACPI: ERST 0x00000000D8FFDDC8 000230 (v01 AMIER  AMI ERST 00000000      00000000)
[    0.007978] ACPI: HEST 0x00000000D8FFDFF8 0000A8 (v01 AMI    AMI HEST 00000000      00000000)
[    0.007980] ACPI: BERT 0x00000000D8FFE0A0 000030 (v01 AMI    AMI BERT 00000000      00000000)
[    0.007982] ACPI: Reserving FACP table memory at [mem 0xd8ff8d18-0xd8ff8e23]
[    0.007983] ACPI: Reserving DSDT table memory at [mem 0xd8fed1e0-0xd8ff8d14]
[    0.007984] ACPI: Reserving FACS table memory at [mem 0xda7fe080-0xda7fe0bf]
[    0.007985] ACPI: Reserving APIC table memory at [mem 0xd8ff8e28-0xd8ff8eb9]
[    0.007985] ACPI: Reserving FPDT table memory at [mem 0xd8ff8ec0-0xd8ff8f03]
[    0.007986] ACPI: Reserving SLIC table memory at [mem 0xd8ff8f08-0xd8ff907d]
[    0.007986] ACPI: Reserving LPIT table memory at [mem 0xd8ff9080-0xd8ff90db]
[    0.007987] ACPI: Reserving SSDT table memory at [mem 0xd8ff90e0-0xd8ff9618]
[    0.007988] ACPI: Reserving SSDT table memory at [mem 0xd8ff9620-0xd8ffa0f7]
[    0.007988] ACPI: Reserving HPET table memory at [mem 0xd8ffa0f8-0xd8ffa12f]
[    0.007989] ACPI: Reserving SSDT table memory at [mem 0xd8ffa130-0xd8ffa5c4]
[    0.007990] ACPI: Reserving MCFG table memory at [mem 0xd8ffa5c8-0xd8ffa603]
[    0.007990] ACPI: Reserving SSDT table memory at [mem 0xd8ffa608-0xd8ffdadd]
[    0.007991] ACPI: Reserving ASF! table memory at [mem 0xd8ffdae0-0xd8ffdb84]
[    0.007991] ACPI: Reserving MSDM table memory at [mem 0xd8ffdb88-0xd8ffdbdc]
[    0.007992] ACPI: Reserving DMAR table memory at [mem 0xd8ffdbe0-0xd8ffdc97]
[    0.007993] ACPI: Reserving EINJ table memory at [mem 0xd8ffdc98-0xd8ffddc7]
[    0.007993] ACPI: Reserving ERST table memory at [mem 0xd8ffddc8-0xd8ffdff7]
[    0.007994] ACPI: Reserving HEST table memory at [mem 0xd8ffdff8-0xd8ffe09f]
[    0.007995] ACPI: Reserving BERT table memory at [mem 0xd8ffe0a0-0xd8ffe0cf]
[    0.008043] No NUMA configuration found
[    0.008044] Faking a node at [mem 0x0000000000000000-0x000000041edfffff]
[    0.008051] NODE_DATA(0) allocated [mem 0x41edd52c0-0x41edfffff]
[    0.008232] Zone ranges:
[    0.008232]   DMA      [mem 0x0000000000001000-0x0000000000ffffff]
[    0.008234]   DMA32    [mem 0x0000000001000000-0x00000000ffffffff]
[    0.008235]   Normal   [mem 0x0000000100000000-0x000000041edfffff]
[    0.008236]   Device   empty
[    0.008237] Movable zone start for each node
[    0.008239] Early memory node ranges
[    0.008240]   node   0: [mem 0x0000000000001000-0x000000000009dfff]
[    0.008241]   node   0: [mem 0x0000000000100000-0x00000000d1a67fff]
[    0.008242]   node   0: [mem 0x00000000d1a6f000-0x00000000d1ea0fff]
[    0.008242]   node   0: [mem 0x00000000d2332000-0x00000000d7edafff]
[    0.008243]   node   0: [mem 0x00000000d8000000-0x00000000d875ffff]
[    0.008244]   node   0: [mem 0x00000000d8800000-0x00000000d8fadfff]
[    0.008244]   node   0: [mem 0x00000000d9000000-0x00000000da71bfff]
[    0.008245]   node   0: [mem 0x00000000da800000-0x00000000dbe0cfff]
[    0.008245]   node   0: [mem 0x0000000100000000-0x000000041edfffff]
[    0.008248] Initmem setup node 0 [mem 0x0000000000001000-0x000000041edfffff]
[    0.008252] On node 0, zone DMA: 1 pages in unavailable ranges
[    0.008272] On node 0, zone DMA: 98 pages in unavailable ranges
[    0.013315] On node 0, zone DMA32: 7 pages in unavailable ranges
[    0.013479] On node 0, zone DMA32: 1169 pages in unavailable ranges
[    0.013496] On node 0, zone DMA32: 293 pages in unavailable ranges
[    0.013511] On node 0, zone DMA32: 160 pages in unavailable ranges
[    0.013551] On node 0, zone DMA32: 82 pages in unavailable ranges
[    0.013591] On node 0, zone DMA32: 228 pages in unavailable ranges
[    0.033764] On node 0, zone Normal: 16883 pages in unavailable ranges
[    0.033800] On node 0, zone Normal: 4608 pages in unavailable ranges
[    0.033807] Reserving Intel graphics memory at [mem 0xdd200000-0xdf1fffff]
[    0.033980] ACPI: PM-Timer IO Port: 0x1808
[    0.033989] ACPI: LAPIC_NMI (acpi_id[0xff] high edge lint[0x1])
[    0.033999] IOAPIC[0]: apic_id 8, version 32, address 0xfec00000, GSI 0-23
[    0.034002] ACPI: INT_SRC_OVR (bus 0 bus_irq 0 global_irq 2 dfl dfl)
[    0.034003] ACPI: INT_SRC_OVR (bus 0 bus_irq 9 global_irq 9 high level)
[    0.034007] ACPI: Using ACPI (MADT) for SMP configuration information
[    0.034008] ACPI: HPET id: 0x8086a701 base: 0xfed00000
[    0.034013] TSC deadline timer available
[    0.034017] CPU topo: Max. logical packages:   1
[    0.034017] CPU topo: Max. logical dies:       1
[    0.034018] CPU topo: Max. dies per package:   1
[    0.034022] CPU topo: Max. threads per core:   2
[    0.034023] CPU topo: Num. cores per package:     4
[    0.034023] CPU topo: Num. threads per package:   8
[    0.034024] CPU topo: Allowing 8 present CPUs plus 0 hotplug CPUs
[    0.034043] PM: hibernation: Registered nosave memory: [mem 0x00000000-0x00000fff]
[    0.034044] PM: hibernation: Registered nosave memory: [mem 0x0009e000-0x000fffff]
[    0.034046] PM: hibernation: Registered nosave memory: [mem 0xd1a68000-0xd1a6efff]
[    0.034047] PM: hibernation: Registered nosave memory: [mem 0xd1ea1000-0xd2331fff]
[    0.034049] PM: hibernation: Registered nosave memory: [mem 0xd7edb000-0xd7ffffff]
[    0.034050] PM: hibernation: Registered nosave memory: [mem 0xd8760000-0xd87fffff]
[    0.034052] PM: hibernation: Registered nosave memory: [mem 0xd8fae000-0xd8ffffff]
[    0.034053] PM: hibernation: Registered nosave memory: [mem 0xda71c000-0xda7fffff]
[    0.034055] PM: hibernation: Registered nosave memory: [mem 0xdbe0d000-0xffffffff]
[    0.034056] [mem 0xdf200000-0xf7ffffff] available for PCI devices
[    0.034057] Booting paravirtualized kernel on bare hardware
[    0.034059] clocksource: refined-jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 1910969940391419 ns
[    0.034066] setup_percpu: NR_CPUS:8192 nr_cpumask_bits:8 nr_cpu_ids:8 nr_node_ids:1
[    0.034549] percpu: Embedded 84 pages/cpu s221184 r8192 d114688 u524288
[    0.034555] pcpu-alloc: s221184 r8192 d114688 u524288 alloc=1*2097152
[    0.034557] pcpu-alloc: [0] 0 1 2 3 [0] 4 5 6 7 
[    0.034577] Kernel command line: BOOT_IMAGE=/boot/vmlinuz-6.17.9-1-pve root=/dev/mapper/pve-root ro quiet
[    0.034626] random: crng init done
[    0.034627] printk: log buffer data + meta data: 262144 + 917504 = 1179648 bytes
[    0.036303] Dentry cache hash table entries: 2097152 (order: 12, 16777216 bytes, linear)
[    0.037159] Inode-cache hash table entries: 1048576 (order: 11, 8388608 bytes, linear)
[    0.037288] software IO TLB: area num 8.
[    0.050573] Fallback order for Node 0: 0 
[    0.050578] Built 1 zonelists, mobility grouping on.  Total pages: 4170775
[    0.050579] Policy zone: Normal
[    0.050588] mem auto-init: stack:all(zero), heap alloc:on, heap free:off
[    0.088542] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=8, Nodes=1
[    0.088570] Kernel/User page tables isolation: enabled
[    0.097396] ftrace: allocating 58414 entries in 230 pages
[    0.097398] ftrace: allocated 230 pages with 5 groups
[    0.098209] Dynamic Preempt: voluntary
[    0.098279] rcu: Preemptible hierarchical RCU implementation.
[    0.098279] rcu: 	RCU restricting CPUs from NR_CPUS=8192 to nr_cpu_ids=8.
[    0.098281] 	Trampoline variant of Tasks RCU enabled.
[    0.098281] 	Rude variant of Tasks RCU enabled.
[    0.098281] 	Tracing variant of Tasks RCU enabled.
[    0.098282] rcu: RCU calculated value of scheduler-enlistment delay is 100 jiffies.
[    0.098282] rcu: Adjusting geometry for rcu_fanout_leaf=16, nr_cpu_ids=8
[    0.098291] RCU Tasks: Setting shift to 3 and lim to 1 rcu_task_cb_adjust=1 rcu_task_cpu_ids=8.
[    0.098293] RCU Tasks Rude: Setting shift to 3 and lim to 1 rcu_task_cb_adjust=1 rcu_task_cpu_ids=8.
[    0.098295] RCU Tasks Trace: Setting shift to 3 and lim to 1 rcu_task_cb_adjust=1 rcu_task_cpu_ids=8.
[    0.102576] NR_IRQS: 524544, nr_irqs: 488, preallocated irqs: 16
[    0.102772] rcu: srcu_init: Setting srcu_struct sizes based on contention.
[    0.104227] Console: colour VGA+ 80x25
[    0.104230] printk: legacy console [tty0] enabled
[    0.104284] ACPI: Core revision 20250404
[    0.104384] clocksource: hpet: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 133484882848 ns
[    0.104398] APIC: Switch to symmetric I/O mode setup
[    0.104400] DMAR: Host address width 39
[    0.104401] DMAR: DRHD base: 0x000000fed90000 flags: 0x0
[    0.104409] DMAR: dmar0: reg_base_addr fed90000 ver 1:0 cap c0000020660462 ecap f0101a
[    0.104411] DMAR: DRHD base: 0x000000fed91000 flags: 0x1
[    0.104414] DMAR: dmar1: reg_base_addr fed91000 ver 1:0 cap d2008020660462 ecap f010da
[    0.104415] DMAR: RMRR base: 0x000000dbf7e000 end: 0x000000dbf8bfff
[    0.104417] DMAR: RMRR base: 0x000000dd000000 end: 0x000000df1fffff
[    0.104419] DMAR-IR: IOAPIC id 8 under DRHD base  0xfed91000 IOMMU 1
[    0.104421] DMAR-IR: HPET id 0 under DRHD base 0xfed91000
[    0.104422] DMAR-IR: Queued invalidation will be enabled to support x2apic and Intr-remapping.
[    0.104907] DMAR-IR: Enabled IRQ remapping in x2apic mode
[    0.104909] x2apic enabled
[    0.104963] APIC: Switched APIC routing to: cluster x2apic
[    0.105374] ..TIMER: vector=0x30 apic1=0 pin1=2 apic2=-1 pin2=-1
[    0.109398] clocksource: tsc-early: mask: 0xffffffffffffffff max_cycles: 0x325550da278, max_idle_ns: 440795315424 ns
[    0.109402] Calibrating delay loop (skipped), value calculated using timer frequency.. 6983.74 BogoMIPS (lpj=3491870)
[    0.109425] CPU0: Thermal monitoring enabled (TM1)
[    0.109457] Last level iTLB entries: 4KB 1024, 2MB 1024, 4MB 1024
[    0.109459] Last level dTLB entries: 4KB 1024, 2MB 1024, 4MB 1024, 1GB 4
[    0.109462] process: using mwait in idle threads
[    0.109464] mitigations: Enabled attack vectors: user_kernel, user_user, guest_host, guest_guest, SMT mitigations: auto
[    0.109468] Speculative Store Bypass: Mitigation: Speculative Store Bypass disabled via prctl
[    0.109470] SRBDS: Mitigation: Microcode
[    0.109471] Spectre V2 : Mitigation: Retpolines
[    0.109472] Spectre V2 : User space: Mitigation: STIBP via prctl
[    0.109472] MDS: Mitigation: Clear CPU buffers
[    0.109473] VMSCAPE: Mitigation: IBPB before exit to userspace
[    0.109474] Spectre V1 : Mitigation: usercopy/swapgs barriers and __user pointer sanitization
[    0.109475] Spectre V2 : Spectre v2 / SpectreRSB: Filling RSB on context switch and VMEXIT
[    0.109476] Spectre V2 : Enabling Restricted Speculation for firmware calls
[    0.109477] Spectre V2 : mitigation: Enabling conditional Indirect Branch Prediction Barrier
[    0.109483] x86/fpu: Supporting XSAVE feature 0x001: 'x87 floating point registers'
[    0.109485] x86/fpu: Supporting XSAVE feature 0x002: 'SSE registers'
[    0.109486] x86/fpu: Supporting XSAVE feature 0x004: 'AVX registers'
[    0.109487] x86/fpu: xstate_offset[2]:  576, xstate_sizes[2]:  256
[    0.109488] x86/fpu: Enabled xstate features 0x7, context size is 832 bytes, using 'standard' format.
[    0.129518] Freeing SMP alternatives memory: 52K
[    0.129523] pid_max: default: 32768 minimum: 301
[    0.129570] LSM: initializing lsm=lockdown,capability,yama,apparmor,ima,evm
[    0.129588] Yama: becoming mindful.
[    0.129618] AppArmor: AppArmor initialized
[    0.129667] Mount-cache hash table entries: 32768 (order: 6, 262144 bytes, linear)
[    0.129680] Mountpoint-cache hash table entries: 32768 (order: 6, 262144 bytes, linear)
[    0.130042] smpboot: CPU0: Intel(R) Xeon(R) CPU E3-1246 v3 @ 3.50GHz (family: 0x6, model: 0x3c, stepping: 0x3)
[    0.130207] Performance Events: PEBS fmt2+, Haswell events, 16-deep LBR, full-width counters, Intel PMU driver.
[    0.130237] ... version:                3
[    0.130238] ... bit width:              48
[    0.130239] ... generic registers:      4
[    0.130240] ... value mask:             0000ffffffffffff
[    0.130241] ... max period:             00007fffffffffff
[    0.130242] ... fixed-purpose events:   3
[    0.130242] ... event mask:             000000070000000f
[    0.130391] signal: max sigframe size: 1776
[    0.130400] Estimated ratio of average max frequency by base frequency (times 1024): 1082
[    0.131553] rcu: Hierarchical SRCU implementation.
[    0.131556] rcu: 	Max phase no-delay instances is 400.
[    0.131602] Timer migration: 1 hierarchy levels; 8 children per group; 1 crossnode level
[    0.132160] NMI watchdog: Enabled. Permanently consumes one hw-PMU counter.
[    0.132226] smp: Bringing up secondary CPUs ...
[    0.132328] smpboot: x86: Booting SMP configuration:
[    0.132329] .... node  #0, CPUs:      #1 #2 #3 #4 #5 #6 #7
[    0.134813] MDS CPU bug present and SMT on, data leak possible. See https://www.kernel.org/doc/html/latest/admin-guide/hw-vuln/mds.html for more details.
[    0.134813] VMSCAPE: SMT on, STIBP is required for full protection. See https://www.kernel.org/doc/html/latest/admin-guide/hw-vuln/vmscape.html for more details.
[    0.134813] smp: Brought up 1 node, 8 CPUs
[    0.134813] smpboot: Total of 8 processors activated (55869.92 BogoMIPS)
[    0.136476] Memory: 16167948K/16683100K available (21402K kernel code, 3801K rwdata, 14948K rodata, 4948K init, 5380K bss, 496760K reserved, 0K cma-reserved)
[    0.136946] devtmpfs: initialized
[    0.136946] x86/mm: Memory block size: 128MB
[    0.138336] ACPI: PM: Registering ACPI NVS region [mem 0xd1a68000-0xd1a6efff] (28672 bytes)
[    0.138336] ACPI: PM: Registering ACPI NVS region [mem 0xda71c000-0xda7fffff] (933888 bytes)
[    0.138418] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 1911260446275000 ns
[    0.138418] posixtimers hash table entries: 4096 (order: 4, 65536 bytes, linear)
[    0.138426] futex hash table entries: 2048 (131072 bytes on 1 NUMA nodes, total 128 KiB, linear).
[    0.138484] pinctrl core: initialized pinctrl subsystem
[    0.138572] PM: RTC time: 20:58:04, date: 2026-07-24
[    0.138970] NET: Registered PF_NETLINK/PF_ROUTE protocol family
[    0.139143] DMA: preallocated 2048 KiB GFP_KERNEL pool for atomic allocations
[    0.139240] DMA: preallocated 2048 KiB GFP_KERNEL|GFP_DMA pool for atomic allocations
[    0.139404] DMA: preallocated 2048 KiB GFP_KERNEL|GFP_DMA32 pool for atomic allocations
[    0.139420] audit: initializing netlink subsys (disabled)
[    0.139431] audit: type=2000 audit(1784926684.035:1): state=initialized audit_enabled=0 res=1
[    0.139515] thermal_sys: Registered thermal governor 'fair_share'
[    0.139516] thermal_sys: Registered thermal governor 'bang_bang'
[    0.139517] thermal_sys: Registered thermal governor 'step_wise'
[    0.139518] thermal_sys: Registered thermal governor 'user_space'
[    0.139519] thermal_sys: Registered thermal governor 'power_allocator'
[    0.139531] cpuidle: using governor ladder
[    0.139534] cpuidle: using governor menu
[    0.139573] acpiphp: ACPI Hot Plug PCI Controller Driver version: 0.5
[    0.139653] PCI: ECAM [mem 0xf8000000-0xfbffffff] (base 0xf8000000) for domain 0000 [bus 00-3f]
[    0.139657] PCI: ECAM [mem 0xf8000000-0xfbffffff] reserved as E820 entry
[    0.139665] PCI: Using configuration type 1 for base access
[    0.139704] core: PMU erratum BJ122, BV98, HSD29 worked around, HT is on
[    0.139758] kprobes: kprobe jump-optimization is enabled. All kprobes are optimized if possible.
[    0.145432] HugeTLB: registered 1.00 GiB page size, pre-allocated 0 pages
[    0.145432] HugeTLB: 16380 KiB vmemmap can be freed for a 1.00 GiB page
[    0.145432] HugeTLB: registered 2.00 MiB page size, pre-allocated 0 pages
[    0.145432] HugeTLB: 28 KiB vmemmap can be freed for a 2.00 MiB page
[    0.145703] ACPI: Added _OSI(Module Device)
[    0.145705] ACPI: Added _OSI(Processor Device)
[    0.145706] ACPI: Added _OSI(Processor Aggregator Device)
[    0.153318] ACPI: 5 ACPI AML tables successfully acquired and loaded
[    0.154819] ACPI: [Firmware Bug]: BIOS _OSI(Linux) query ignored
[    0.168271] ACPI: Dynamic OEM Table Load:
[    0.168271] ACPI: SSDT 0xFFFF8A5A811A8000 0005AA (v01 PmRef  ApIst    00003000 INTL 20120711)
[    0.169686] ACPI: Interpreter enabled
[    0.169710] ACPI: PM: (supports S0 S4 S5)
[    0.169711] ACPI: Using IOAPIC for interrupt routing
[    0.170319] HEST: Table parsing has been initialized.
[    0.170400] GHES: APEI firmware first mode is enabled by WHEA _OSC.
[    0.170404] PCI: Using host bridge windows from ACPI; if necessary, use "pci=nocrs" and report a bug
[    0.170405] PCI: Using E820 reservations for host bridge windows
[    0.170581] ACPI: Enabled 8 GPEs in block 00 to 3F
[    0.182364] ACPI: PCI Root Bridge [PCI0] (domain 0000 [bus 00-3e])
[    0.182370] acpi PNP0A08:00: _OSC: OS supports [ExtendedConfig ASPM ClockPM Segments MSI EDR HPX-Type3]
[    0.182510] acpi PNP0A08:00: _OSC: platform does not support [PCIeHotplug SHPCHotplug PME]
[    0.182637] acpi PNP0A08:00: _OSC: OS now controls [AER PCIeCapability LTR DPC]
[    0.183094] PCI host bridge to bus 0000:00
[    0.183098] pci_bus 0000:00: root bus resource [io  0x0000-0x0cf7 window]
[    0.183100] pci_bus 0000:00: root bus resource [io  0x0d00-0xffff window]
[    0.183101] pci_bus 0000:00: root bus resource [mem 0x000a0000-0x000bffff window]
[    0.183103] pci_bus 0000:00: root bus resource [mem 0x000d4000-0x000e7fff window]
[    0.183104] pci_bus 0000:00: root bus resource [mem 0xdf200000-0xfeafffff window]
[    0.183105] pci_bus 0000:00: root bus resource [bus 00-3e]
[    0.183117] pci 0000:00:00.0: [8086:0c08] type 00 class 0x060000 conventional PCI endpoint
[    0.183181] pci 0000:00:02.0: [8086:041a] type 00 class 0x030000 conventional PCI endpoint
[    0.183194] pci 0000:00:02.0: BAR 0 [mem 0xf7800000-0xf7bfffff 64bit]
[    0.183196] pci 0000:00:02.0: BAR 2 [mem 0xe0000000-0xefffffff 64bit pref]
[    0.183198] pci 0000:00:02.0: BAR 4 [io  0xf000-0xf03f]
[    0.183205] pci 0000:00:02.0: Video device with shadowed ROM at [mem 0x000c0000-0x000dffff]
[    0.183287] pci 0000:00:03.0: [8086:0c0c] type 00 class 0x040300 PCIe Root Complex Integrated Endpoint
[    0.183300] pci 0000:00:03.0: BAR 0 [mem 0xf7c30000-0xf7c33fff 64bit]
[    0.183381] pci 0000:00:14.0: [8086:8c31] type 00 class 0x0c0330 conventional PCI endpoint
[    0.183413] pci 0000:00:14.0: BAR 0 [mem 0xf7c20000-0xf7c2ffff 64bit]
[    0.183442] pci 0000:00:14.0: PME# supported from D3hot D3cold
[    0.183534] pci 0000:00:16.0: [8086:8c3a] type 00 class 0x078000 conventional PCI endpoint
[    0.183567] pci 0000:00:16.0: BAR 0 [mem 0xf7c3b000-0xf7c3b00f 64bit]
[    0.183598] pci 0000:00:16.0: PME# supported from D0 D3hot D3cold
[    0.183653] pci 0000:00:19.0: [8086:153a] type 00 class 0x020000 conventional PCI endpoint
[    0.183683] pci 0000:00:19.0: BAR 0 [mem 0xf7c00000-0xf7c1ffff]
[    0.183686] pci 0000:00:19.0: BAR 1 [mem 0xf7c38000-0xf7c38fff]
[    0.183689] pci 0000:00:19.0: BAR 2 [io  0xf060-0xf07f]
[    0.183721] pci 0000:00:19.0: PME# supported from D0 D3hot D3cold
[    0.183792] pci 0000:00:1a.0: [8086:8c2d] type 00 class 0x0c0320 conventional PCI endpoint
[    0.183830] pci 0000:00:1a.0: BAR 0 [mem 0xf7c37000-0xf7c373ff]
[    0.183871] pci 0000:00:1a.0: PME# supported from D0 D3hot D3cold
[    0.183947] pci 0000:00:1c.0: [8086:8c10] type 01 class 0x060400 PCIe Root Port
[    0.183967] pci 0000:00:1c.0: PCI bridge to [bus 01]
[    0.184023] pci 0000:00:1c.0: PME# supported from D0 D3hot D3cold
[    0.184044] pci 0000:00:1c.0: Enabling MPC IRBNCE
[    0.184046] pci 0000:00:1c.0: Intel PCH root port ACS workaround enabled
[    0.184308] pci 0000:00:1c.1: [8086:8c12] type 01 class 0x060400 PCIe Root Port
[    0.184329] pci 0000:00:1c.1: PCI bridge to [bus 02-03]
[    0.184385] pci 0000:00:1c.1: PME# supported from D0 D3hot D3cold
[    0.184407] pci 0000:00:1c.1: Enabling MPC IRBNCE
[    0.184409] pci 0000:00:1c.1: Intel PCH root port ACS workaround enabled
[    0.184669] pci 0000:00:1c.4: [8086:8c18] type 01 class 0x060400 PCIe Root Port
[    0.184691] pci 0000:00:1c.4: PCI bridge to [bus 04]
[    0.184752] pci 0000:00:1c.4: PME# supported from D0 D3hot D3cold
[    0.184774] pci 0000:00:1c.4: Enabling MPC IRBNCE
[    0.184777] pci 0000:00:1c.4: Intel PCH root port ACS workaround enabled
[    0.185030] pci 0000:00:1d.0: [8086:8c26] type 00 class 0x0c0320 conventional PCI endpoint
[    0.185070] pci 0000:00:1d.0: BAR 0 [mem 0xf7c36000-0xf7c363ff]
[    0.185110] pci 0000:00:1d.0: PME# supported from D0 D3hot D3cold
[    0.185190] pci 0000:00:1f.0: [8086:8c56] type 00 class 0x060100 conventional PCI endpoint
[    0.185337] pci 0000:00:1f.2: [8086:8c00] type 00 class 0x01018f conventional PCI endpoint
[    0.185365] pci 0000:00:1f.2: BAR 0 [io  0xf0d0-0xf0d7]
[    0.185367] pci 0000:00:1f.2: BAR 1 [io  0xf0c0-0xf0c3]
[    0.185370] pci 0000:00:1f.2: BAR 2 [io  0xf0b0-0xf0b7]
[    0.185373] pci 0000:00:1f.2: BAR 3 [io  0xf0a0-0xf0a3]
[    0.185375] pci 0000:00:1f.2: BAR 4 [io  0xf090-0xf09f]
[    0.185378] pci 0000:00:1f.2: BAR 5 [io  0xf080-0xf08f]
[    0.185457] pci 0000:00:1f.3: [8086:8c22] type 00 class 0x0c0500 conventional PCI endpoint
[    0.185488] pci 0000:00:1f.3: BAR 0 [mem 0xf7c35000-0xf7c350ff 64bit]
[    0.185493] pci 0000:00:1f.3: BAR 4 [io  0xf040-0xf05f]
[    0.185601] acpiphp: Slot [1] registered
[    0.185607] pci 0000:00:1c.0: PCI bridge to [bus 01]
[    0.185690] pci 0000:02:00.0: [104c:8240] type 01 class 0x060400 PCIe to PCI/PCI-X bridge
[    0.185732] pci 0000:02:00.0: PCI bridge to [bus 03]
[    0.185851] pci 0000:02:00.0: supports D1 D2
[    0.185976] pci 0000:00:1c.1: PCI bridge to [bus 02-03]
[    0.186034] pci_bus 0000:03: extended config space not accessible
[    0.186118] pci 0000:02:00.0: PCI bridge to [bus 03]
[    0.186195] acpiphp: Slot [1-1] registered
[    0.186200] pci 0000:00:1c.4: PCI bridge to [bus 04]
[    0.186878] ACPI: PCI: Interrupt link LNKA configured for IRQ 11
[    0.186923] ACPI: PCI: Interrupt link LNKB configured for IRQ 3
[    0.186965] ACPI: PCI: Interrupt link LNKC configured for IRQ 10
[    0.187006] ACPI: PCI: Interrupt link LNKD configured for IRQ 10
[    0.187048] ACPI: PCI: Interrupt link LNKE configured for IRQ 5
[    0.187088] ACPI: PCI: Interrupt link LNKF configured for IRQ 0
[    0.187089] ACPI: PCI: Interrupt link LNKF disabled
[    0.187129] ACPI: PCI: Interrupt link LNKG configured for IRQ 0
[    0.187130] ACPI: PCI: Interrupt link LNKG disabled
[    0.187171] ACPI: PCI: Interrupt link LNKH configured for IRQ 11
[    0.187439] iommu: Default domain type: Translated
[    0.187439] iommu: DMA domain TLB invalidation policy: lazy mode
[    0.187558] SCSI subsystem initialized
[    0.187565] libata version 3.00 loaded.
[    0.187565] ACPI: bus type USB registered
[    0.187565] usbcore: registered new interface driver usbfs
[    0.187565] usbcore: registered new interface driver hub
[    0.187565] usbcore: registered new device driver usb
[    0.187565] pps_core: LinuxPPS API ver. 1 registered
[    0.187565] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.187565] PTP clock support registered
[    0.187565] EDAC MC: Ver: 3.0.0
[    0.187592] NetLabel: Initializing
[    0.187593] NetLabel:  domain hash size = 128
[    0.187594] NetLabel:  protocols = UNLABELED CIPSOv4 CALIPSO
[    0.187610] NetLabel:  unlabeled traffic allowed by default
[    0.187626] mctp: management component transport protocol core
[    0.187626] NET: Registered PF_MCTP protocol family
[    0.187626] PCI: Using ACPI for IRQ routing
[    0.189385] PCI: pci_cache_line_size set to 64 bytes
[    0.189416] e820: reserve RAM buffer [mem 0x0009ec00-0x0009ffff]
[    0.189418] e820: reserve RAM buffer [mem 0xd1a68000-0xd3ffffff]
[    0.189419] e820: reserve RAM buffer [mem 0xd1ea1000-0xd3ffffff]
[    0.189420] e820: reserve RAM buffer [mem 0xd7edb000-0xd7ffffff]
[    0.189421] e820: reserve RAM buffer [mem 0xd8760000-0xdbffffff]
[    0.189422] e820: reserve RAM buffer [mem 0xd8fae000-0xdbffffff]
[    0.189423] e820: reserve RAM buffer [mem 0xda71c000-0xdbffffff]
[    0.189424] e820: reserve RAM buffer [mem 0xdbe0d000-0xdbffffff]
[    0.189425] e820: reserve RAM buffer [mem 0x41ee00000-0x41fffffff]
[    0.189437] pci 0000:00:02.0: vgaarb: setting as boot VGA device
[    0.189437] pci 0000:00:02.0: vgaarb: bridge control possible
[    0.189437] pci 0000:00:02.0: vgaarb: VGA device added: decodes=io+mem,owns=io+mem,locks=none
[    0.189437] vgaarb: loaded
[    0.189486] hpet0: at MMIO 0xfed00000, IRQs 2, 8, 0, 0, 0, 0, 0, 0
[    0.189486] hpet0: 8 comparators, 64-bit 14.318180 MHz counter
[    0.191448] clocksource: Switched to clocksource tsc-early
[    0.192023] VFS: Disk quotas dquot_6.6.0
[    0.192032] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.192212] AppArmor: AppArmor Filesystem Enabled
[    0.192235] pnp: PnP ACPI init
[    0.192288] system 00:00: [mem 0xfed40000-0xfed44fff] has been reserved
[    0.192441] system 00:01: [io  0x0680-0x069f] has been reserved
[    0.192444] system 00:01: [io  0xffff] has been reserved
[    0.192445] system 00:01: [io  0xffff] has been reserved
[    0.192446] system 00:01: [io  0xffff] has been reserved
[    0.192447] system 00:01: [io  0x1c00-0x1cfe] has been reserved
[    0.192449] system 00:01: [io  0x1d00-0x1dfe] has been reserved
[    0.192450] system 00:01: [io  0x1e00-0x1efe] has been reserved
[    0.192451] system 00:01: [io  0x1f00-0x1ffe] has been reserved
[    0.192452] system 00:01: [io  0x1800-0x18fe] could not be reserved
[    0.192454] system 00:01: [io  0x164e-0x164f] has been reserved
[    0.192560] system 00:03: [io  0x0a00-0x0a0f] has been reserved
[    0.192599] system 00:04: [io  0x04d0-0x04d1] has been reserved
[    0.193047] pnp 00:05: [dma 0 disabled]
[    0.193380] system 00:06: [mem 0xfed1c000-0xfed1ffff] has been reserved
[    0.193383] system 00:06: [mem 0xfed10000-0xfed17fff] has been reserved
[    0.193384] system 00:06: [mem 0xfed18000-0xfed18fff] has been reserved
[    0.193385] system 00:06: [mem 0xfed19000-0xfed19fff] has been reserved
[    0.193386] system 00:06: [mem 0xf8000000-0xfbffffff] has been reserved
[    0.193388] system 00:06: [mem 0xfed20000-0xfed3ffff] has been reserved
[    0.193389] system 00:06: [mem 0xfed90000-0xfed93fff] could not be reserved
[    0.193390] system 00:06: [mem 0xfed45000-0xfed8ffff] has been reserved
[    0.193392] system 00:06: [mem 0xff000000-0xffffffff] has been reserved
[    0.193393] system 00:06: [mem 0xfee00000-0xfeefffff] could not be reserved
[    0.193394] system 00:06: [mem 0xf7fdf000-0xf7fdffff] has been reserved
[    0.193395] system 00:06: [mem 0xf7fe0000-0xf7feffff] has been reserved
[    0.193566] pnp: PnP ACPI: found 7 devices
[    0.199139] clocksource: acpi_pm: mask: 0xffffff max_cycles: 0xffffff, max_idle_ns: 2085701024 ns
[    0.199184] NET: Registered PF_INET protocol family
[    0.199292] IP idents hash table entries: 262144 (order: 9, 2097152 bytes, linear)
[    0.211560] tcp_listen_portaddr_hash hash table entries: 8192 (order: 5, 131072 bytes, linear)
[    0.211611] Table-perturb hash table entries: 65536 (order: 6, 262144 bytes, linear)
[    0.211698] TCP established hash table entries: 131072 (order: 8, 1048576 bytes, linear)
[    0.211874] TCP bind hash table entries: 65536 (order: 9, 2097152 bytes, linear)
[    0.212055] TCP: Hash tables configured (established 131072 bind 65536)
[    0.212137] MPTCP token hash table entries: 16384 (order: 7, 393216 bytes, linear)
[    0.212207] UDP hash table entries: 8192 (order: 7, 524288 bytes, linear)
[    0.212280] UDP-Lite hash table entries: 8192 (order: 7, 524288 bytes, linear)
[    0.212367] NET: Registered PF_UNIX/PF_LOCAL protocol family
[    0.212378] NET: Registered PF_XDP protocol family
[    0.212394] pci 0000:00:1c.4: bridge window [io  0x1000-0x0fff] to [bus 04] add_size 1000
[    0.212398] pci 0000:00:1c.4: bridge window [mem 0x00100000-0x000fffff 64bit pref] to [bus 04] add_size 200000 add_align 100000
[    0.212400] pci 0000:00:1c.4: bridge window [mem 0x00100000-0x000fffff] to [bus 04] add_size 200000 add_align 100000
[    0.212408] pci 0000:00:1c.4: bridge window [mem 0xdf200000-0xdf3fffff]: assigned
[    0.212410] pci 0000:00:1c.4: bridge window [mem 0xdf400000-0xdf5fffff 64bit pref]: assigned
[    0.212413] pci 0000:00:1c.4: bridge window [io  0x2000-0x2fff]: assigned
[    0.212416] pci 0000:00:1c.0: PCI bridge to [bus 01]
[    0.212426] pci 0000:02:00.0: PCI bridge to [bus 03]
[    0.212442] pci 0000:00:1c.1: PCI bridge to [bus 02-03]
[    0.212450] pci 0000:00:1c.4: PCI bridge to [bus 04]
[    0.212453] pci 0000:00:1c.4:   bridge window [io  0x2000-0x2fff]
[    0.212457] pci 0000:00:1c.4:   bridge window [mem 0xdf200000-0xdf3fffff]
[    0.212460] pci 0000:00:1c.4:   bridge window [mem 0xdf400000-0xdf5fffff 64bit pref]
[    0.212466] pci_bus 0000:00: resource 4 [io  0x0000-0x0cf7 window]
[    0.212467] pci_bus 0000:00: resource 5 [io  0x0d00-0xffff window]
[    0.212468] pci_bus 0000:00: resource 6 [mem 0x000a0000-0x000bffff window]
[    0.212469] pci_bus 0000:00: resource 7 [mem 0x000d4000-0x000e7fff window]
[    0.212471] pci_bus 0000:00: resource 8 [mem 0xdf200000-0xfeafffff window]
[    0.212472] pci_bus 0000:04: resource 0 [io  0x2000-0x2fff]
[    0.212473] pci_bus 0000:04: resource 1 [mem 0xdf200000-0xdf3fffff]
[    0.212474] pci_bus 0000:04: resource 2 [mem 0xdf400000-0xdf5fffff 64bit pref]
[    0.234686] pci 0000:00:1a.0: quirk_usb_early_handoff+0x0/0x740 took 15783 usecs
[    0.250686] pci 0000:00:1d.0: quirk_usb_early_handoff+0x0/0x740 took 15607 usecs
[    0.250704] PCI: CLS 64 bytes, default 64
[    0.250725] DMAR: No ATSR found
[    0.250725] DMAR: No SATC found
[    0.250726] DMAR: dmar0: Using Queued invalidation
[    0.250731] DMAR: dmar1: Using Queued invalidation
[    0.250776] Trying to unpack rootfs image as initramfs...
[    0.250851] pci 0000:00:02.0: Adding to iommu group 0
[    0.251183] pci 0000:00:00.0: Adding to iommu group 1
[    0.251192] pci 0000:00:03.0: Adding to iommu group 2
[    0.251198] pci 0000:00:14.0: Adding to iommu group 3
[    0.251207] pci 0000:00:16.0: Adding to iommu group 4
[    0.251214] pci 0000:00:19.0: Adding to iommu group 5
[    0.251221] pci 0000:00:1a.0: Adding to iommu group 6
[    0.251228] pci 0000:00:1c.0: Adding to iommu group 7
[    0.251235] pci 0000:00:1c.1: Adding to iommu group 8
[    0.251242] pci 0000:00:1c.4: Adding to iommu group 9
[    0.251249] pci 0000:00:1d.0: Adding to iommu group 10
[    0.251261] pci 0000:00:1f.0: Adding to iommu group 11
[    0.251268] pci 0000:00:1f.2: Adding to iommu group 11
[    0.251275] pci 0000:00:1f.3: Adding to iommu group 11
[    0.251282] pci 0000:02:00.0: Adding to iommu group 12
[    0.252105] DMAR: Intel(R) Virtualization Technology for Directed I/O
[    0.252107] PCI-DMA: Using software bounce buffering for IO (SWIOTLB)
[    0.252108] software IO TLB: mapped [mem 0x00000000d3edb000-0x00000000d7edb000] (64MB)
[    0.270756] Initialise system trusted keyrings
[    0.270767] Key type blacklist registered
[    0.270870] workingset: timestamp_bits=36 max_order=22 bucket_order=0
[    0.271097] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.271238] fuse: init (API version 7.44)
[    0.271417] integrity: Platform Keyring initialized
[    0.271419] integrity: Machine keyring initialized
[    0.281057] Key type asymmetric registered
[    0.281060] Asymmetric key parser 'x509' registered
[    0.281090] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 242)
[    0.281196] io scheduler mq-deadline registered
[    0.282153] ledtrig-cpu: registered to indicate activity on CPUs
[    0.282839] input: Power Button as /devices/LNXSYSTM:00/LNXSYBUS:00/PNP0C0C:00/input/input0
[    0.283084] ACPI: button: Power Button [PWRB]
[    0.283111] input: Power Button as /devices/LNXSYSTM:00/LNXPWRBN:00/input/input1
[    0.283203] ACPI: button: Power Button [PWRF]
[    0.284008] ACPI: \_TZ_.TZ00: _AL0 evaluation failure
[    0.284086] thermal LNXTHERM:00: registered as thermal_zone0
[    0.284087] ACPI: thermal: Thermal Zone [TZ00] (28 C)
[    0.284269] thermal LNXTHERM:01: registered as thermal_zone1
[    0.284270] ACPI: thermal: Thermal Zone [TZ01] (30 C)
[    0.284324] ERST: Error Record Serialization Table (ERST) support is initialized.
[    0.284347] pstore: Using crash dump compression: deflate
[    0.284348] pstore: Registered erst as persistent store backend
[    0.284461] Serial: 8250/16550 driver, 32 ports, IRQ sharing enabled
[    0.305351] 00:05: ttyS0 at I/O 0x3f8 (irq = 4, base_baud = 115200) is a 16550A
[    0.307438] Linux agpgart interface v0.103
[    0.309059] loop: module loaded
[    0.309262] ata_piix 0000:00:1f.2: MAP [ P0 P2 P1 P3 ]
[    0.309679] scsi host0: ata_piix
[    0.309846] scsi host1: ata_piix
[    0.309881] ata1: SATA max UDMA/133 cmd 0xf0d0 ctl 0xf0c0 bmdma 0xf090 irq 19 lpm-pol 0
[    0.309885] ata2: SATA max UDMA/133 cmd 0xf0b0 ctl 0xf0a0 bmdma 0xf098 irq 19 lpm-pol 0
[    0.309983] ACPI: bus type drm_connector registered
[    0.310260] tun: Universal TUN/TAP device driver, 1.6
[    0.310296] PPP generic driver version 2.4.2
[    0.310350] i8042: PNP: No PS/2 controller found.
[    0.310385] mousedev: PS/2 mouse device common for all mice
[    0.310452] rtc_cmos 00:02: RTC can wake from S4
[    0.310680] rtc_cmos 00:02: registered as rtc0
[    0.310711] rtc_cmos 00:02: setting system clock to 2026-07-24T20:58:04 UTC (1784926684)
[    0.310735] rtc_cmos 00:02: alarms up to one month, y3k, 242 bytes nvram, hpet irqs
[    0.310742] i2c_dev: i2c /dev entries driver
[    0.310898] device-mapper: core: CONFIG_IMA_DISABLE_HTABLE is disabled. Duplicate IMA measurements will not be recorded in the IMA log.
[    0.310911] device-mapper: uevent: version 1.0.3
[    0.310940] device-mapper: ioctl: 4.50.0-ioctl (2025-04-28) initialised: dm-devel@lists.linux.dev
[    0.310948] intel_pstate: Intel P-state driver initializing
[    0.311269] drop_monitor: Initializing network drop monitor service
[    0.311348] NET: Registered PF_INET6 protocol family
[    0.311579] Segment Routing with IPv6
[    0.311585] In-situ OAM (IOAM) with IPv6
[    0.311605] NET: Registered PF_PACKET protocol family
[    0.311628] Bridge firewalling registered
[    0.311656] Key type dns_resolver registered
[    0.312158] ENERGY_PERF_BIAS: Set to 'normal', was 'performance'
[    0.312259] microcode: Current revision: 0x00000028
[    0.312269] microcode: Updated early from: 0x0000001c
[    0.312495] IPI shorthand broadcast: enabled
[    0.313942] sched_clock: Marking stable (312001439, 1599372)->(317354175, -3753364)
[    0.314117] registered taskstats version 1
[    0.314685] Loading compiled-in X.509 certificates
[    0.315188] Loaded X.509 cert 'Build time autogenerated kernel key: 845ea0f525f9596080363f3ae23afd7a64d308b0'
[    0.318541] Demotion targets for Node 0: null
[    0.318672] Key type .fscrypt registered
[    0.318674] Key type fscrypt-provisioning registered
[    0.318725] Key type big_key registered
[    0.684824] Freeing initrd memory: 86844K
[    0.698054] Key type encrypted registered
[    0.698057] AppArmor: AppArmor sha256 policy hashing enabled
[    0.698065] ima: No TPM chip found, activating TPM-bypass!
[    0.698072] Loading compiled-in module X.509 certificates
[    0.698508] Loaded X.509 cert 'Build time autogenerated kernel key: 845ea0f525f9596080363f3ae23afd7a64d308b0'
[    0.698510] ima: Allocated hash algorithm: sha256
[    0.698520] ima: No architecture policies found
[    0.698530] evm: Initialising EVM extended attributes:
[    0.698531] evm: security.selinux
[    0.698532] evm: security.SMACK64
[    0.698533] evm: security.SMACK64EXEC
[    0.698533] evm: security.SMACK64TRANSMUTE
[    0.698534] evm: security.SMACK64MMAP
[    0.698535] evm: security.apparmor
[    0.698535] evm: security.ima
[    0.698536] evm: security.capability
[    0.698537] evm: HMAC attrs: 0x1
[    0.698857] PM:   Magic number: 2:376:1004
[    0.698881] input input1: hash matches
[    0.698898] system 00:06: hash matches
[    0.698933] memory memory43: hash matches
[    0.700079] RAS: Correctable Errors collector initialized.
[    0.704063] clk: Disabling unused clocks
[    0.704064] PM: genpd: Disabling unused power domains
[    1.071691] ata2.00: SATA link up 6.0 Gbps (SStatus 133 SControl 300)
[    1.071706] ata2.01: SATA link up 6.0 Gbps (SStatus 133 SControl 300)
[    1.071853] ata1.00: SATA link up 6.0 Gbps (SStatus 133 SControl 300)
[    1.071867] ata1.01: SATA link up 6.0 Gbps (SStatus 133 SControl 300)
[    1.076975] ata2.00: ATA-9: WDC WD30EFRX-68EUZN0, 82.00A82, max UDMA/133
[    1.076978] ata2.00: 5860533168 sectors, multi 16: LBA48 NCQ (depth 0/32)
[    1.077080] ata1.00: ATA-8: Hitachi HDS723020BLA642, MN6OA580, max UDMA/133
[    1.077084] ata1.00: 3907029168 sectors, multi 16: LBA48 NCQ (depth 0/32)
[    1.077174] ata2.01: ATA-8: WDC WD10EZRX-00A8LB0, 01.01A01, max UDMA/133
[    1.077177] ata2.01: 1953525168 sectors, multi 16: LBA48 NCQ (depth 0/32)
[    1.077301] ata1.01: ATA-8: HITACHI HUA723020ALA640, MK7ONS00, max UDMA/133
[    1.077304] ata1.01: 3907029168 sectors, multi 16: LBA48 NCQ (depth 0/32)
[    1.079977] ata2.00: configured for UDMA/133
[    1.082102] ata1.00: configured for UDMA/133
[    1.082870] ata2.01: configured for UDMA/133
[    1.086903] ata1.01: configured for UDMA/133
[    1.087051] scsi 0:0:0:0: Direct-Access     ATA      Hitachi HDS72302 A580 PQ: 0 ANSI: 5
[    1.087260] sd 0:0:0:0: Attached scsi generic sg0 type 0
[    1.087278] sd 0:0:0:0: [sda] 3907029168 512-byte logical blocks: (2.00 TB/1.82 TiB)
[    1.087287] sd 0:0:0:0: [sda] Write Protect is off
[    1.087289] sd 0:0:0:0: [sda] Mode Sense: 00 3a 00 00
[    1.087298] sd 0:0:0:0: [sda] Write cache: enabled, read cache: enabled, doesn't support DPO or FUA
[    1.087313] sd 0:0:0:0: [sda] Preferred minimum I/O size 512 bytes
[    1.087368] scsi 0:0:1:0: Direct-Access     ATA      HITACHI HUA72302 NS00 PQ: 0 ANSI: 5
[    1.087514] sd 0:0:1:0: Attached scsi generic sg1 type 0
[    1.087572] sd 0:0:1:0: [sdb] 3907029168 512-byte logical blocks: (2.00 TB/1.82 TiB)
[    1.087580] sd 0:0:1:0: [sdb] Write Protect is off
[    1.087583] sd 0:0:1:0: [sdb] Mode Sense: 00 3a 00 00
[    1.087591] sd 0:0:1:0: [sdb] Write cache: disabled, read cache: enabled, doesn't support DPO or FUA
[    1.087592] scsi 1:0:0:0: Direct-Access     ATA      WDC WD30EFRX-68E 0A82 PQ: 0 ANSI: 5
[    1.087625] sd 0:0:1:0: [sdb] Preferred minimum I/O size 512 bytes
[    1.087760] sd 1:0:0:0: Attached scsi generic sg2 type 0
[    1.087785] sd 1:0:0:0: [sdc] 5860533168 512-byte logical blocks: (3.00 TB/2.73 TiB)
[    1.087788] sd 1:0:0:0: [sdc] 4096-byte physical blocks
[    1.087795] sd 1:0:0:0: [sdc] Write Protect is off
[    1.087799] sd 1:0:0:0: [sdc] Mode Sense: 00 3a 00 00
[    1.087819] sd 1:0:0:0: [sdc] Write cache: enabled, read cache: enabled, doesn't support DPO or FUA
[    1.087835] sd 1:0:0:0: [sdc] Preferred minimum I/O size 4096 bytes
[    1.087859] scsi 1:0:1:0: Direct-Access     ATA      WDC WD10EZRX-00A 1A01 PQ: 0 ANSI: 5
[    1.088040] scsi 1:0:1:0: Attached scsi generic sg3 type 0
[    1.088092] sd 1:0:1:0: [sdd] 1953525168 512-byte logical blocks: (1.00 TB/932 GiB)
[    1.088094] sd 1:0:1:0: [sdd] 4096-byte physical blocks
[    1.088133] sd 1:0:1:0: [sdd] Write Protect is off
[    1.088134] sd 1:0:1:0: [sdd] Mode Sense: 00 3a 00 00
[    1.088147] sd 1:0:1:0: [sdd] Write cache: enabled, read cache: enabled, doesn't support DPO or FUA
[    1.088168] sd 1:0:1:0: [sdd] Preferred minimum I/O size 4096 bytes
[    1.102673]  sda: sda1
[    1.102730] sd 0:0:0:0: [sda] Attached SCSI disk
[    1.105889] sd 0:0:1:0: [sdb] Attached SCSI disk
[    1.244394]  sdd: sdd1 sdd2 sdd3
[    1.244651] sd 1:0:1:0: [sdd] Attached SCSI disk
[    1.244653]  sdc: sdc1
[    1.244728] sd 1:0:0:0: [sdc] Attached SCSI disk
[    1.245816] Freeing unused decrypted memory: 2028K
[    1.246381] Freeing unused kernel image (initmem) memory: 4948K
[    1.246444] Write protecting the kernel read-only data: 38912k
[    1.246936] Freeing unused kernel image (text/rodata gap) memory: 1124K
[    1.247260] Freeing unused kernel image (rodata/data gap) memory: 1436K
[    1.283266] x86/mm: Checked W+X mappings: passed, no W+X pages found.
[    1.283267] x86/mm: Checking user space page tables
[    1.317794] x86/mm: Checked W+X mappings: passed, no W+X pages found.
[    1.317804] tsc: Refined TSC clocksource calibration: 3491.913 MHz
[    1.317809] clocksource: tsc: mask: 0xffffffffffffffff max_cycles: 0x3255790e5ea, max_idle_ns: 440795224414 ns
[    1.317809] Run /init as init process
[    1.317822]   with arguments:
[    1.317824]     /init
[    1.317826]   with environment:
[    1.317827]     HOME=/
[    1.317828]     TERM=linux
[    1.317835] clocksource: Switched to clocksource tsc
[    1.478452] ACPI Warning: SystemIO range 0x0000000000001828-0x000000000000182F conflicts with OpRegion 0x0000000000001800-0x000000000000187F (\PMIO) (20250404/utaddress-204)
[    1.478463] ACPI: OSL: Resource conflict; ACPI support missing from driver?
[    1.478466] ACPI Warning: SystemIO range 0x0000000000001C40-0x0000000000001C4F conflicts with OpRegion 0x0000000000001C00-0x0000000000001FFF (\GPR) (20250404/utaddress-204)
[    1.478472] ACPI: OSL: Resource conflict; ACPI support missing from driver?
[    1.478474] ACPI Warning: SystemIO range 0x0000000000001C30-0x0000000000001C3F conflicts with OpRegion 0x0000000000001C00-0x0000000000001C3F (\GPRL) (20250404/utaddress-204)
[    1.478478] ACPI Warning: SystemIO range 0x0000000000001C30-0x0000000000001C3F conflicts with OpRegion 0x0000000000001C00-0x0000000000001FFF (\GPR) (20250404/utaddress-204)
[    1.478483] ACPI: OSL: Resource conflict; ACPI support missing from driver?
[    1.478485] ACPI Warning: SystemIO range 0x0000000000001C00-0x0000000000001C2F conflicts with OpRegion 0x0000000000001C00-0x0000000000001C3F (\GPRL) (20250404/utaddress-204)
[    1.478490] ACPI Warning: SystemIO range 0x0000000000001C00-0x0000000000001C2F conflicts with OpRegion 0x0000000000001C00-0x0000000000001FFF (\GPR) (20250404/utaddress-204)
[    1.478494] ACPI: OSL: Resource conflict; ACPI support missing from driver?
[    1.478495] lpc_ich: Resource conflict(s) found affecting gpio_ich
[    1.480712] ehci-pci 0000:00:1a.0: EHCI Host Controller
[    1.480720] ehci-pci 0000:00:1a.0: new USB bus registered, assigned bus number 1
[    1.480734] ehci-pci 0000:00:1a.0: debug port 2
[    1.483677] e1000e: Intel(R) PRO/1000 Network Driver
[    1.483681] e1000e: Copyright(c) 1999 - 2015 Intel Corporation.
[    1.483891] e1000e 0000:00:19.0: Interrupt Throttling Rate (ints/sec) set to dynamic conservative mode
[    1.484677] ehci-pci 0000:00:1a.0: irq 16, io mem 0xf7c37000
[    1.490664] ehci-pci 0000:00:1a.0: USB 2.0 started, EHCI 1.00
[    1.490734] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 6.17
[    1.490738] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.490740] usb usb1: Product: EHCI Host Controller
[    1.490742] usb usb1: Manufacturer: Linux 6.17.9-1-pve ehci_hcd
[    1.490744] usb usb1: SerialNumber: 0000:00:1a.0
[    1.490883] hub 1-0:1.0: USB hub found
[    1.490889] hub 1-0:1.0: 2 ports detected
[    1.491105] ehci-pci 0000:00:1d.0: EHCI Host Controller
[    1.491126] ehci-pci 0000:00:1d.0: new USB bus registered, assigned bus number 2
[    1.491138] ehci-pci 0000:00:1d.0: debug port 2
[    1.495214] ehci-pci 0000:00:1d.0: irq 23, io mem 0xf7c36000
[    1.500616] ehci-pci 0000:00:1d.0: USB 2.0 started, EHCI 1.00
[    1.502053] usb usb2: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 6.17
[    1.502058] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.502060] usb usb2: Product: EHCI Host Controller
[    1.502063] usb usb2: Manufacturer: Linux 6.17.9-1-pve ehci_hcd
[    1.502065] usb usb2: SerialNumber: 0000:00:1d.0
[    1.502248] hub 2-0:1.0: USB hub found
[    1.502262] hub 2-0:1.0: 2 ports detected
[    1.504051] xhci_hcd 0000:00:14.0: xHCI Host Controller
[    1.504058] xhci_hcd 0000:00:14.0: new USB bus registered, assigned bus number 3
[    1.505143] xhci_hcd 0000:00:14.0: hcc params 0x200077c1 hci version 0x100 quirks 0x0000000000009810
[    1.505386] xhci_hcd 0000:00:14.0: xHCI Host Controller
[    1.505389] xhci_hcd 0000:00:14.0: new USB bus registered, assigned bus number 4
[    1.505392] xhci_hcd 0000:00:14.0: Host supports USB 3.0 SuperSpeed
[    1.505455] usb usb3: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 6.17
[    1.505459] usb usb3: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.505462] usb usb3: Product: xHCI Host Controller
[    1.505464] usb usb3: Manufacturer: Linux 6.17.9-1-pve xhci-hcd
[    1.505465] usb usb3: SerialNumber: 0000:00:14.0
[    1.505590] hub 3-0:1.0: USB hub found
[    1.505624] hub 3-0:1.0: 15 ports detected
[    1.506711] i801_smbus 0000:00:1f.3: SPD Write Disable is set
[    1.506732] i801_smbus 0000:00:1f.3: SMBus using PCI interrupt
[    1.511094] i2c i2c-0: Successfully instantiated SPD at 0x50
[    1.511369] i2c i2c-0: Successfully instantiated SPD at 0x51
[    1.511653] i2c i2c-0: Successfully instantiated SPD at 0x52
[    1.511988] i2c i2c-0: Successfully instantiated SPD at 0x53
[    1.513000] usb usb4: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 6.17
[    1.513003] usb usb4: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.513004] usb usb4: Product: xHCI Host Controller
[    1.513006] usb usb4: Manufacturer: Linux 6.17.9-1-pve xhci-hcd
[    1.513007] usb usb4: SerialNumber: 0000:00:14.0
[    1.513121] hub 4-0:1.0: USB hub found
[    1.513140] hub 4-0:1.0: 6 ports detected
[    1.554276] e1000e 0000:00:19.0 0000:00:19.0 (uninitialized): registered PHC clock
[    1.618492] e1000e 0000:00:19.0 eth0: (PCI Express:2.5GT/s:Width x1) 98:90:96:c4:96:9a
[    1.618496] e1000e 0000:00:19.0 eth0: Intel(R) PRO/1000 Network Connection
[    1.618540] e1000e 0000:00:19.0 eth0: MAC: 11, PHY: 12, PBA No: FFFFFF-0FF
[    1.619678] e1000e 0000:00:19.0 eno1: renamed from eth0
[    1.727652] usb 1-1: new high-speed USB device number 2 using ehci-pci
[    1.735627] usb 2-1: new high-speed USB device number 2 using ehci-pci
[    1.833841] usb 4-1: new SuperSpeed USB device number 2 using xhci_hcd
[    1.847573] usb 4-1: New USB device found, idVendor=2109, idProduct=0817, bcdDevice=90.43
[    1.847577] usb 4-1: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    1.847578] usb 4-1: Product: USB3.0 Hub             
[    1.847579] usb 4-1: Manufacturer: VIA Labs, Inc.         
[    1.848866] hub 4-1:1.0: USB hub found
[    1.849034] hub 4-1:1.0: 4 ports detected
[    1.853110] usb 1-1: New USB device found, idVendor=8087, idProduct=8008, bcdDevice= 0.04
[    1.853113] usb 1-1: New USB device strings: Mfr=0, Product=0, SerialNumber=0
[    1.853437] hub 1-1:1.0: USB hub found
[    1.853596] hub 1-1:1.0: 6 ports detected
[    1.862006] usb 2-1: New USB device found, idVendor=8087, idProduct=8000, bcdDevice= 0.04
[    1.862010] usb 2-1: New USB device strings: Mfr=0, Product=0, SerialNumber=0
[    1.862297] hub 2-1:1.0: USB hub found
[    1.862357] hub 2-1:1.0: 8 ports detected
[    1.965444] usb 4-2: new SuperSpeed USB device number 3 using xhci_hcd
[    1.988925] usb 4-2: New USB device found, idVendor=0bda, idProduct=0411, bcdDevice= 0.01
[    1.988929] usb 4-2: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    1.988930] usb 4-2: Product: USB3.2 Hub
[    1.988932] usb 4-2: Manufacturer: Generic
[    1.992620] hub 4-2:1.0: USB hub found
[    1.993785] hub 4-2:1.0: 4 ports detected
[    2.137636] usb 1-1.2: new high-speed USB device number 3 using ehci-pci
[    2.225252] usb 1-1.2: New USB device found, idVendor=1a40, idProduct=0101, bcdDevice= 1.11
[    2.225255] usb 1-1.2: New USB device strings: Mfr=0, Product=1, SerialNumber=0
[    2.225256] usb 1-1.2: Product: USB 2.0 Hub
[    2.225519] hub 1-1.2:1.0: USB hub found
[    2.225594] hub 1-1.2:1.0: 4 ports detected
[    2.283325] usb 4-2.1: new SuperSpeed USB device number 4 using xhci_hcd
[    2.299639] usb 1-1.5: new high-speed USB device number 4 using ehci-pci
[    2.307367] usb 4-2.1: New USB device found, idVendor=0bda, idProduct=0411, bcdDevice= 0.01
[    2.307371] usb 4-2.1: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    2.307372] usb 4-2.1: Product: USB3.2 Hub
[    2.307374] usb 4-2.1: Manufacturer: Generic
[    2.312380] hub 4-2.1:1.0: USB hub found
[    2.314860] hub 4-2.1:1.0: 4 ports detected
[    2.374864] usb 4-1.4: new SuperSpeed USB device number 5 using xhci_hcd
[    2.377621] usb 1-1.5: New USB device found, idVendor=2109, idProduct=2817, bcdDevice=90.43
[    2.377624] usb 1-1.5: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    2.377626] usb 1-1.5: Product: USB2.0 Hub             
[    2.377627] usb 1-1.5: Manufacturer: VIA Labs, Inc.         
[    2.378021] hub 1-1.5:1.0: USB hub found
[    2.378243] hub 1-1.5:1.0: 4 ports detected
[    2.388330] usb 4-1.4: New USB device found, idVendor=2109, idProduct=0817, bcdDevice=90.43
[    2.388333] usb 4-1.4: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    2.388334] usb 4-1.4: Product: USB3.0 Hub             
[    2.388336] usb 4-1.4: Manufacturer: VIA Labs, Inc.         
[    2.450674] hub 4-1.4:1.0: USB hub found
[    2.450892] hub 4-1.4:1.0: 4 ports detected
[    2.458865] usb 4-2.2: new SuperSpeed USB device number 6 using xhci_hcd
[    2.583642] usb 1-1.6: new high-speed USB device number 5 using ehci-pci
[    2.609762] usb 4-2.1.3: new SuperSpeed USB device number 7 using xhci_hcd
[    2.621660] usb 4-2.1.3: New USB device found, idVendor=174c, idProduct=55aa, bcdDevice= 1.00
[    2.621664] usb 4-2.1.3: New USB device strings: Mfr=2, Product=3, SerialNumber=1
[    2.621666] usb 4-2.1.3: Product: ThinkPlus
[    2.621667] usb 4-2.1.3: Manufacturer: SSD
[    2.621668] usb 4-2.1.3: SerialNumber: AAAABBBB000C
[    2.626031] usbcore: registered new interface driver usb-storage
[    2.630172] scsi host2: uas
[    2.630241] usbcore: registered new interface driver uas
[    2.630765] scsi 2:0:0:0: Direct-Access     SSD      ThinkPlus        0    PQ: 0 ANSI: 6
[    2.633469] sd 2:0:0:0: Attached scsi generic sg4 type 0
[    2.634254] sd 2:0:0:0: [sde] 1000215216 512-byte logical blocks: (512 GB/477 GiB)
[    2.634386] sd 2:0:0:0: [sde] Write Protect is off
[    2.634388] sd 2:0:0:0: [sde] Mode Sense: 43 00 00 00
[    2.634585] sd 2:0:0:0: [sde] Write cache: enabled, read cache: enabled, doesn't support DPO or FUA
[    2.662884] sd 2:0:0:0: [sde] Preferred minimum I/O size 512 bytes
[    2.662898] sd 2:0:0:0: [sde] Optimal transfer size 33553920 bytes
[    2.683252] usb 1-1.6: New USB device found, idVendor=0bda, idProduct=5411, bcdDevice= 0.01
[    2.683257] usb 1-1.6: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    2.683259] usb 1-1.6: Product: USB2.1 Hub
[    2.683260] usb 1-1.6: Manufacturer: Generic
[    2.684055] hub 1-1.6:1.0: USB hub found
[    2.686250] hub 1-1.6:1.0: 4 ports detected
[    2.690325]  sde: sde1
[    2.690406] sd 2:0:0:0: [sde] Attached SCSI disk
[    2.745953] usb 4-2.2: New USB device found, idVendor=0b95, idProduct=1790, bcdDevice= 2.00
[    2.745968] usb 4-2.2: New USB device strings: Mfr=1, Product=2, SerialNumber=3
[    2.745970] usb 4-2.2: Product: AX88179A
[    2.745971] usb 4-2.2: Manufacturer: ASIX
[    2.745972] usb 4-2.2: SerialNumber: 00000000004885
[    2.811987] usbcore: registered new interface driver cdc_ether
[    2.872834] usb 4-2.3: new SuperSpeed USB device number 8 using xhci_hcd
[    2.912077] usb 4-2.3: New USB device found, idVendor=2109, idProduct=0815, bcdDevice= 7.04
[    2.912080] usb 4-2.3: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    2.912082] usb 4-2.3: Product: USB3.0 Hub             
[    2.912083] usb 4-2.3: Manufacturer: VIA Labs, Inc.         
[    2.923620] hub 4-2.3:1.0: USB hub found
[    2.923766] hub 4-2.3:1.0: 4 ports detected
[    2.970622] usb 1-1.6.1: new high-speed USB device number 6 using ehci-pci
[    2.974662] usb 4-1.4.2: new SuperSpeed USB device number 9 using xhci_hcd
[    2.986269] usb 4-1.4.2: New USB device found, idVendor=1058, idProduct=2647, bcdDevice=10.23
[    2.986271] usb 4-1.4.2: New USB device strings: Mfr=2, Product=3, SerialNumber=1
[    2.986273] usb 4-1.4.2: Product: easystore 2647
[    2.986274] usb 4-1.4.2: Manufacturer: Western Digital
[    2.986275] usb 4-1.4.2: SerialNumber: 57583532443431524C4B3846
[    2.988626] usb-storage 4-1.4.2:1.0: USB Mass Storage device detected
[    2.988961] scsi host3: usb-storage 4-1.4.2:1.0
[    3.010813] cdc_ncm 4-2.2:2.0: MAC-Address: 8c:ae:4c:cd:a9:26
[    3.010816] cdc_ncm 4-2.2:2.0: setting rx_max = 16384
[    3.023828] cdc_ncm 4-2.2:2.0: setting tx_max = 16384
[    3.033975] cdc_ncm 4-2.2:2.0 eth0: register 'cdc_ncm' at usb-0000:00:14.0-2.2, CDC NCM (NO ZLP), 8c:ae:4c:cd:a9:26
[    3.048523] usbcore: registered new interface driver cdc_ncm
[    3.050595] cdc_ncm 4-2.2:2.0 enx8cae4ccda926: renamed from eth0
[    3.053181] device-mapper: thin: Data device (dm-3) discard unsupported: Disabling discard passdown.
[    3.070640] usb 1-1.6.1: New USB device found, idVendor=0bda, idProduct=5411, bcdDevice= 0.01
[    3.070644] usb 1-1.6.1: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    3.070646] usb 1-1.6.1: Product: USB2.1 Hub
[    3.070647] usb 1-1.6.1: Manufacturer: Generic
[    3.071277] hub 1-1.6.1:1.0: USB hub found
[    3.072252] hub 1-1.6.1:1.0: 4 ports detected
[    3.093831] usb 4-2.4: new SuperSpeed USB device number 10 using xhci_hcd
[    3.111932] usb 4-2.4: New USB device found, idVendor=0b95, idProduct=1790, bcdDevice= 2.00
[    3.111936] usb 4-2.4: New USB device strings: Mfr=1, Product=2, SerialNumber=3
[    3.111937] usb 4-2.4: Product: AX88179B
[    3.111938] usb 4-2.4: Manufacturer: ASIX
[    3.111940] usb 4-2.4: SerialNumber: 00000000000102
[    3.142622] raid6: avx2x4   gen() 36067 MB/s
[    3.159620] raid6: avx2x2   gen() 34895 MB/s
[    3.166232] cdc_ncm 4-2.4:2.0: MAC-Address: 80:ae:4c:cd:ec:03
[    3.166235] cdc_ncm 4-2.4:2.0: setting rx_max = 16384
[    3.166524] cdc_ncm 4-2.4:2.0: setting tx_max = 16384
[    3.166940] cdc_ncm 4-2.4:2.0 eth0: register 'cdc_ncm' at usb-0000:00:14.0-2.4, CDC NCM (NO ZLP), 80:ae:4c:cd:ec:03
[    3.171900] cdc_ncm 4-2.4:2.0 enx80ae4ccdec03: renamed from eth0
[    3.176617] raid6: avx2x1   gen() 30750 MB/s
[    3.176619] raid6: using algorithm avx2x4 gen() 36067 MB/s
[    3.190629] usb 1-1.5.4: new high-speed USB device number 7 using ehci-pci
[    3.193621] raid6: .... xor() 12142 MB/s, rmw enabled
[    3.193622] raid6: using avx2x2 recovery algorithm
[    3.194673] xor: automatically using best checksumming function   avx       
[    3.195515] async_tx: api initialized (async)
[    3.332488] usb 1-1.5.4: New USB device found, idVendor=2109, idProduct=2817, bcdDevice=90.43
[    3.332492] usb 1-1.5.4: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    3.332494] usb 1-1.5.4: Product: USB2.0 Hub             
[    3.332495] usb 1-1.5.4: Manufacturer: VIA Labs, Inc.         
[    3.332899] hub 1-1.5.4:1.0: USB hub found
[    3.333098] hub 1-1.5.4:1.0: 4 ports detected
[    3.361443] Btrfs loaded, zoned=yes, fsverity=yes
[    3.404627] usb 1-1.6.3: new high-speed USB device number 8 using ehci-pci
[    3.493494] usb 1-1.6.3: New USB device found, idVendor=2109, idProduct=2815, bcdDevice= 7.04
[    3.493499] usb 1-1.6.3: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    3.493501] usb 1-1.6.3: Product: USB2.0 Hub             
[    3.493502] usb 1-1.6.3: Manufacturer: VIA Labs, Inc.         
[    3.493771] hub 1-1.6.3:1.0: USB hub found
[    3.494000] hub 1-1.6.3:1.0: 4 ports detected
[    3.534002] usb 1-1.2: USB disconnect, device number 3
[    3.544875] usb 4-2.3.3: new SuperSpeed USB device number 11 using xhci_hcd
[    3.585054] usb 4-2.3.3: New USB device found, idVendor=2109, idProduct=0815, bcdDevice= 7.04
[    3.585057] usb 4-2.3.3: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    3.585059] usb 4-2.3.3: Product: USB3.0 Hub             
[    3.585060] usb 4-2.3.3: Manufacturer: VIA Labs, Inc.         
[    3.586147] hub 4-2.3.3:1.0: USB hub found
[    3.586323] hub 4-2.3.3:1.0: 4 ports detected
[    3.654545] EXT4-fs (dm-1): orphan cleanup on readonly fs
[    3.654924] EXT4-fs (dm-1): mounted filesystem fe418106-acca-4171-8fba-1f4fa2c48260 ro with ordered data mode. Quota mode: none.
[    4.035661] usb 1-1.5.4.1: new full-speed USB device number 9 using ehci-pci
[    4.040347] scsi 3:0:0:0: Direct-Access     WD       easystore 2647   1023 PQ: 0 ANSI: 6
[    4.040679] scsi 3:0:0:1: Enclosure         WD       SES Device       1023 PQ: 0 ANSI: 6
[    4.044024] sd 3:0:0:0: Attached scsi generic sg5 type 0
[    4.044161] sd 3:0:0:0: [sdf] Very big device. Trying to use READ CAPACITY(16).
[    4.044183] scsi 3:0:0:1: Attached scsi generic sg6 type 13
[    4.044458] sd 3:0:0:0: [sdf] 9767475200 512-byte logical blocks: (5.00 TB/4.55 TiB)
[    4.044460] sd 3:0:0:0: [sdf] 4096-byte physical blocks
[    4.044737] sd 3:0:0:0: [sdf] Write Protect is off
[    4.044739] sd 3:0:0:0: [sdf] Mode Sense: 47 00 10 08
[    4.045017] sd 3:0:0:0: [sdf] No Caching mode page found
[    4.045019] sd 3:0:0:0: [sdf] Assuming drive cache: write through
[    4.076295]  sdf: sdf1
[    4.076359] sd 3:0:0:0: [sdf] Attached SCSI disk
[    4.172503] usb 1-1.5.4.1: New USB device found, idVendor=067b, idProduct=2303, bcdDevice= 4.00
[    4.172507] usb 1-1.5.4.1: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    4.172508] usb 1-1.5.4.1: Product: USB-Serial Controller D
[    4.172510] usb 1-1.5.4.1: Manufacturer: Prolific Technology Inc. 
[    4.294658] usb 1-1.6.3.1: new full-speed USB device number 10 using ehci-pci
[    4.432028] usb 1-1.6.3.1: New USB device found, idVendor=067b, idProduct=2303, bcdDevice= 4.00
[    4.432032] usb 1-1.6.3.1: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    4.432044] usb 1-1.6.3.1: Product: USB-Serial Controller D
[    4.432045] usb 1-1.6.3.1: Manufacturer: Prolific Technology Inc. 
[    4.443299] systemd[1]: Inserted module 'autofs4'
[    4.545106] systemd[1]: systemd 257.9-1~deb13u1 running in system mode (+PAM +AUDIT +SELINUX +APPARMOR +IMA +IPE +SMACK +SECCOMP +GCRYPT -GNUTLS +OPENSSL +ACL +BLKID +CURL +ELFUTILS +FIDO2 +IDN2 -IDN +IPTC +KMOD +LIBCRYPTSETUP +LIBCRYPTSETUP_PLUGINS +LIBFDISK +PCRE2 +PWQUALITY +P11KIT +QRENCODE +TPM2 +BZIP2 +LZ4 +XZ +ZLIB +ZSTD +BPF_FRAMEWORK +BTF -XKBCOMMON -UTMP +SYSVINIT +LIBARCHIVE)
[    4.545112] systemd[1]: Detected architecture x86-64.
[    4.554652] usb 1-1.5.4.4: new full-speed USB device number 11 using ehci-pci
[    4.563595] systemd[1]: Hostname set to <pfv-tsys4>.
[    4.637944] systemd[1]: bpf-restrict-fs: BPF LSM hook not enabled in the kernel, BPF LSM not supported.
[    4.692879] usb 1-1.5.4.4: New USB device found, idVendor=067b, idProduct=2303, bcdDevice= 3.00
[    4.692883] usb 1-1.5.4.4: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    4.692885] usb 1-1.5.4.4: Product: USB-Serial Controller
[    4.692886] usb 1-1.5.4.4: Manufacturer: Prolific Technology Inc.
[    4.813665] usb 1-1.6.3.2: new full-speed USB device number 12 using ehci-pci
[    4.952278] usb 1-1.6.3.2: New USB device found, idVendor=067b, idProduct=2303, bcdDevice= 3.00
[    4.952282] usb 1-1.6.3.2: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    4.952294] usb 1-1.6.3.2: Product: USB-Serial Controller
[    4.952295] usb 1-1.6.3.2: Manufacturer: Prolific Technology Inc.
[    5.075624] usb 1-1.6.3.3: new high-speed USB device number 13 using ehci-pci
[    5.213686] usb 1-1.6.3.3: New USB device found, idVendor=2109, idProduct=2815, bcdDevice= 7.04
[    5.213690] usb 1-1.6.3.3: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    5.213691] usb 1-1.6.3.3: Product: USB2.0 Hub             
[    5.213693] usb 1-1.6.3.3: Manufacturer: VIA Labs, Inc.         
[    5.214193] hub 1-1.6.3.3:1.0: USB hub found
[    5.214526] hub 1-1.6.3.3:1.0: 4 ports detected
[    5.459660] usb 1-1.6.3.4: new full-speed USB device number 14 using ehci-pci
[    5.598404] usb 1-1.6.3.4: New USB device found, idVendor=067b, idProduct=2303, bcdDevice= 3.00
[    5.598408] usb 1-1.6.3.4: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    5.598420] usb 1-1.6.3.4: Product: USB-Serial Controller
[    5.598422] usb 1-1.6.3.4: Manufacturer: Prolific Technology Inc.
[    5.621131] systemd[1]: Queued start job for default target graphical.target.
[    5.643340] systemd[1]: Created slice system-getty.slice - Slice /system/getty.
[    5.643760] systemd[1]: Created slice system-modprobe.slice - Slice /system/modprobe.
[    5.644119] systemd[1]: Created slice system-systemd\x2dfsck.slice - Slice /system/systemd-fsck.
[    5.644631] systemd[1]: Created slice system-xfs_scrub.slice - xfs_scrub background service slice.
[    5.644888] systemd[1]: Created slice user.slice - User and Session Slice.
[    5.644941] systemd[1]: Started systemd-ask-password-console.path - Dispatch Password Requests to Console Directory Watch.
[    5.644979] systemd[1]: Started systemd-ask-password-wall.path - Forward Password Requests to Wall Directory Watch.
[    5.645122] systemd[1]: Set up automount proc-sys-fs-binfmt_misc.automount - Arbitrary Executable File Formats File System Automount Point.
[    5.645143] systemd[1]: Expecting device dev-disk-by\x2duuid-1bb5976a\x2da9b9\x2d467d\x2dbdc1\x2daecf3810590b.device - /dev/disk/by-uuid/1bb5976a-a9b9-467d-bdc1-aecf3810590b...
[    5.645149] systemd[1]: Expecting device dev-disk-by\x2duuid-3898f700\x2d297d\x2d4a6b\x2da449\x2d71ccf7b22047.device - /dev/disk/by-uuid/3898f700-297d-4a6b-a449-71ccf7b22047...
[    5.645155] systemd[1]: Expecting device dev-disk-by\x2duuid-49bd1b9e\x2df31c\x2d4f0a\x2d9790\x2d5b4b330c5708.device - /dev/disk/by-uuid/49bd1b9e-f31c-4f0a-9790-5b4b330c5708...
[    5.645160] systemd[1]: Expecting device dev-disk-by\x2duuid-b53dcfc5\x2d02f4\x2d4b80\x2dbf72\x2d33feb8b03f09.device - /dev/disk/by-uuid/b53dcfc5-02f4-4b80-bf72-33feb8b03f09...
[    5.645165] systemd[1]: Expecting device dev-pve-swap.device - /dev/pve/swap...
[    5.645174] systemd[1]: Reached target ceph-fuse.target - ceph target allowing to start/stop all ceph-fuse@.service instances at once.
[    5.645185] systemd[1]: Reached target ceph.target - ceph target allowing to start/stop all ceph*@.service instances at once.
[    5.645211] systemd[1]: Reached target network-pre.target - Preparation for Network.
[    5.645227] systemd[1]: Reached target nss-lookup.target - Host and Network Name Lookups.
[    5.645234] systemd[1]: Reached target paths.target - Path Units.
[    5.645258] systemd[1]: Reached target slices.target - Slice Units.
[    5.645339] systemd[1]: Listening on dm-event.socket - Device-mapper event daemon FIFOs.
[    5.645394] systemd[1]: Listening on lvm2-lvmpolld.socket - LVM2 poll daemon socket.
[    5.648253] systemd[1]: Listening on rpcbind.socket - RPCbind Server Activation Socket.
[    5.649020] systemd[1]: Listening on systemd-creds.socket - Credential Encryption/Decryption.
[    5.649101] systemd[1]: Listening on systemd-initctl.socket - initctl Compatibility Named Pipe.
[    5.649194] systemd[1]: Listening on systemd-journald-dev-log.socket - Journal Socket (/dev/log).
[    5.649288] systemd[1]: Listening on systemd-journald.socket - Journal Sockets.
[    5.649318] systemd[1]: systemd-pcrextend.socket - TPM PCR Measurements was skipped because of an unmet condition check (ConditionSecurity=measured-uki).
[    5.649332] systemd[1]: systemd-pcrlock.socket - Make TPM PCR Policy was skipped because of an unmet condition check (ConditionSecurity=measured-uki).
[    5.649404] systemd[1]: Listening on systemd-udevd-control.socket - udev Control Socket.
[    5.649454] systemd[1]: Listening on systemd-udevd-kernel.socket - udev Kernel Socket.
[    5.657308] systemd[1]: Mounting dev-hugepages.mount - Huge Pages File System...
[    5.658012] systemd[1]: Mounting dev-mqueue.mount - POSIX Message Queue File System...
[    5.658090] systemd[1]: run-lock.mount: Directory /run/lock to mount over is not empty, mounting anyway.
[    5.658786] systemd[1]: Mounting run-lock.mount - Legacy Locks Directory /run/lock...
[    5.659462] systemd[1]: Mounting sys-kernel-debug.mount - Kernel Debug File System...
[    5.660475] systemd[1]: Mounting sys-kernel-tracing.mount - Kernel Trace File System...
[    5.660531] systemd[1]: auth-rpcgss-module.service - Kernel Module supporting RPCSEC_GSS was skipped because of an unmet condition check (ConditionPathExists=/etc/krb5.keytab).
[    5.661849] systemd[1]: Starting keyboard-setup.service - Set the console keyboard layout...
[    5.663082] systemd[1]: Starting kmod-static-nodes.service - Create List of Static Device Nodes...
[    5.664314] systemd[1]: Starting lvm2-monitor.service - Monitoring of LVM2 mirrors, snapshots etc. using dmeventd or progress polling...
[    5.665496] systemd[1]: Starting modprobe@configfs.service - Load Kernel Module configfs...
[    5.666701] systemd[1]: Starting modprobe@drm.service - Load Kernel Module drm...
[    5.667841] systemd[1]: Starting modprobe@efi_pstore.service - Load Kernel Module efi_pstore...
[    5.668612] usb 1-1.2: new high-speed USB device number 15 using ehci-pci
[    5.668968] systemd[1]: Starting modprobe@fuse.service - Load Kernel Module fuse...
[    5.669324] systemd[1]: systemd-fsck-root.service - File System Check on Root Device was skipped because of an unmet condition check (ConditionPathExists=!/run/initramfs/fsck-root).
[    5.669391] systemd[1]: systemd-hibernate-clear.service - Clear Stale Hibernate Storage Info was skipped because of an unmet condition check (ConditionPathExists=/sys/firmware/efi/efivars/HibernateLocation-8cf2644b-4b0b-428f-9387-6d876050dc67).
[    5.671962] systemd[1]: Starting systemd-journald.service - Journal Service...
[    5.710757] systemd[1]: Starting systemd-modules-load.service - Load Kernel Modules...
[    5.710777] systemd[1]: systemd-pcrmachine.service - TPM PCR Machine ID Measurement was skipped because of an unmet condition check (ConditionSecurity=measured-uki).
[    5.711665] systemd[1]: Starting systemd-remount-fs.service - Remount Root and Kernel File Systems...
[    5.711712] systemd[1]: systemd-tpm2-setup-early.service - Early TPM SRK Setup was skipped because of an unmet condition check (ConditionSecurity=measured-uki).
[    5.712494] systemd[1]: Starting systemd-udev-load-credentials.service - Load udev Rules from Credentials...
[    5.713304] systemd[1]: Starting systemd-udev-trigger.service - Coldplug All udev Devices...
[    5.720018] systemd[1]: Finished kmod-static-nodes.service - Create List of Static Device Nodes.
[    5.720510] systemd[1]: modprobe@configfs.service: Deactivated successfully.
[    5.720750] systemd[1]: Finished modprobe@configfs.service - Load Kernel Module configfs.
[    5.720990] systemd[1]: modprobe@drm.service: Deactivated successfully.
[    5.721132] systemd[1]: Finished modprobe@drm.service - Load Kernel Module drm.
[    5.721328] systemd[1]: modprobe@fuse.service: Deactivated successfully.
[    5.721443] systemd[1]: Finished modprobe@fuse.service - Load Kernel Module fuse.
[    5.722302] systemd[1]: Mounting sys-fs-fuse-connections.mount - FUSE Control File System...
[    5.723002] systemd[1]: Mounting sys-kernel-config.mount - Kernel Configuration File System...
[    5.723873] systemd[1]: Starting systemd-tmpfiles-setup-dev-early.service - Create Static Device Nodes in /dev gracefully...
[    5.741489] systemd[1]: modprobe@efi_pstore.service: Deactivated successfully.
[    5.741647] systemd[1]: Finished modprobe@efi_pstore.service - Load Kernel Module efi_pstore.
[    5.760224] usb 1-1.2: New USB device found, idVendor=1a40, idProduct=0101, bcdDevice= 1.11
[    5.760227] usb 1-1.2: New USB device strings: Mfr=0, Product=1, SerialNumber=0
[    5.760229] usb 1-1.2: Product: USB 2.0 Hub
[    5.760514] hub 1-1.2:1.0: USB hub found
[    5.760597] hub 1-1.2:1.0: 4 ports detected
[    5.909431] systemd[1]: Finished systemd-udev-load-credentials.service - Load udev Rules from Credentials.
[    5.913517] systemd-journald[394]: Collecting audit messages is disabled.
[    5.916630] usb 1-1.6.3.3.1: new full-speed USB device number 16 using ehci-pci
[    6.020147] systemd[1]: Finished systemd-udev-trigger.service - Coldplug All udev Devices.
[    6.055625] usb 1-1.6.3.3.1: New USB device found, idVendor=067b, idProduct=2303, bcdDevice= 3.00
[    6.055630] usb 1-1.6.3.3.1: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    6.055633] usb 1-1.6.3.3.1: Product: USB-Serial Controller
[    6.055635] usb 1-1.6.3.3.1: Manufacturer: Prolific Technology Inc.
[    6.067271] systemd[1]: Starting ifupdown2-pre.service - Helper to synchronize boot up for ifupdown...
[    6.068155] systemd[1]: Starting systemd-udev-settle.service - Wait for udev To Complete Device Initialization...
[    6.069075] systemd[1]: Mounted dev-hugepages.mount - Huge Pages File System.
[    6.069171] systemd[1]: Mounted dev-mqueue.mount - POSIX Message Queue File System.
[    6.069242] systemd[1]: Mounted run-lock.mount - Legacy Locks Directory /run/lock.
[    6.069314] systemd[1]: Mounted sys-kernel-debug.mount - Kernel Debug File System.
[    6.069381] systemd[1]: Mounted sys-kernel-tracing.mount - Kernel Trace File System.
[    6.069449] systemd[1]: Mounted sys-fs-fuse-connections.mount - FUSE Control File System.
[    6.069515] systemd[1]: Mounted sys-kernel-config.mount - Kernel Configuration File System.
[    6.085290] systemd[1]: Started systemd-journald.service - Journal Service.
[    6.090526] EXT4-fs (dm-1): re-mounted fe418106-acca-4171-8fba-1f4fa2c48260 r/w.
[    6.179681] usb 1-1.6.3.3.2: new full-speed USB device number 17 using ehci-pci
[    6.196341] systemd-journald[394]: Received client request to flush runtime journal.
[    6.317030] usb 1-1.6.3.3.2: New USB device found, idVendor=067b, idProduct=2303, bcdDevice= 4.00
[    6.317034] usb 1-1.6.3.3.2: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    6.317046] usb 1-1.6.3.3.2: Product: USB-Serial Controller D
[    6.317047] usb 1-1.6.3.3.2: Manufacturer: Prolific Technology Inc. 
[    6.440640] usb 1-1.6.3.3.3: new full-speed USB device number 18 using ehci-pci
[    6.578023] usb 1-1.6.3.3.3: New USB device found, idVendor=067b, idProduct=2303, bcdDevice= 4.00
[    6.578026] usb 1-1.6.3.3.3: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    6.578028] usb 1-1.6.3.3.3: Product: USB-Serial Controller D
[    6.578029] usb 1-1.6.3.3.3: Manufacturer: Prolific Technology Inc. 
[    6.606007] usb 1-1.2: USB disconnect, device number 15
[    6.701659] usb 1-1.6.3.3.4: new full-speed USB device number 19 using ehci-pci
[    6.830166] spl: loading out-of-tree module taints kernel.
[    7.083638] usb 1-1.6.3.3.4: device descriptor read/64, error -32
[    7.127707] zfs: module license 'CDDL' taints kernel.
[    7.127712] Disabling lock debugging due to kernel taint
[    7.127729] zfs: module license taints kernel.
[    7.329866] usb 1-1.6.3.3.4: New USB device found, idVendor=067b, idProduct=2303, bcdDevice= 3.00
[    7.329872] usb 1-1.6.3.3.4: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    7.329875] usb 1-1.6.3.3.4: Product: USB-Serial Controller
[    7.329877] usb 1-1.6.3.3.4: Manufacturer: Prolific Technology Inc.
[    7.711529] ZFS: Loaded module v2.4.0-pve1, ZFS pool version 5000, ZFS filesystem version 5
[    8.067618] RPC: Registered named UNIX socket transport module.
[    8.067622] RPC: Registered udp transport module.
[    8.067622] RPC: Registered tcp transport module.
[    8.067623] RPC: Registered tcp-with-tls transport module.
[    8.067624] RPC: Registered tcp NFSv4.1 backchannel transport module.
[   10.167987] EDAC MC0: Giving out device to module ie31200_edac controller IE31200: DEV 0000:00:00.0 (POLLED)
[   10.220298] usbcore: registered new interface driver usbserial_generic
[   10.220312] usbserial: USB Serial support registered for generic
[   10.311918] usbcore: registered new interface driver cdc_wdm
[   10.525433] usbcore: registered new interface driver pl2303
[   10.525444] usbserial: USB Serial support registered for pl2303
[   10.525464] pl2303 1-1.5.4.1:1.0: pl2303 converter detected
[   10.527346] usb 1-1.5.4.1: pl2303 converter now attached to ttyUSB0
[   10.527381] pl2303 1-1.6.3.1:1.0: pl2303 converter detected
[   10.528913] usb 1-1.6.3.1: pl2303 converter now attached to ttyUSB1
[   10.528930] pl2303 1-1.5.4.4:1.0: pl2303 converter detected
[   10.530958] usb 1-1.5.4.4: pl2303 converter now attached to ttyUSB2
[   10.530977] pl2303 1-1.6.3.2:1.0: pl2303 converter detected
[   10.532675] usb 1-1.6.3.2: pl2303 converter now attached to ttyUSB3
[   10.532692] pl2303 1-1.6.3.4:1.0: pl2303 converter detected
[   10.534443] usb 1-1.6.3.4: pl2303 converter now attached to ttyUSB4
[   10.534459] pl2303 1-1.6.3.3.1:1.0: pl2303 converter detected
[   10.536967] usb 1-1.6.3.3.1: pl2303 converter now attached to ttyUSB5
[   10.536988] pl2303 1-1.6.3.3.2:1.0: pl2303 converter detected
[   10.539452] usb 1-1.6.3.3.2: pl2303 converter now attached to ttyUSB6
[   10.539471] pl2303 1-1.6.3.3.3:1.0: pl2303 converter detected
[   10.541715] usb 1-1.6.3.3.3: pl2303 converter now attached to ttyUSB7
[   10.541735] pl2303 1-1.6.3.3.4:1.0: pl2303 converter detected
[   10.544217] usb 1-1.6.3.3.4: pl2303 converter now attached to ttyUSB8
[   10.547566] at24 0-0050: supply vcc not found, using dummy regulator
[   10.549040] at24 0-0050: 256 byte spd EEPROM, read-only
[   10.549069] at24 0-0051: supply vcc not found, using dummy regulator
[   10.550510] at24 0-0051: 256 byte spd EEPROM, read-only
[   10.550528] at24 0-0052: supply vcc not found, using dummy regulator
[   10.551998] at24 0-0052: 256 byte spd EEPROM, read-only
[   10.552014] at24 0-0053: supply vcc not found, using dummy regulator
[   10.553531] at24 0-0053: 256 byte spd EEPROM, read-only
[   10.826298] usbcore: registered new interface driver cdc_mbim
[   11.011635] e1000e 0000:00:19.0 nic0: renamed from eno1
[   11.140459] spi-nor spi0.0: supply vcc not found, using dummy regulator
[   11.509064] RAPL PMU: API unit is 2^-32 Joules, 4 fixed counters, 655360 ms ovfl timer
[   11.509070] RAPL PMU: hw unit of domain pp0-core 2^-14 Joules
[   11.509072] RAPL PMU: hw unit of domain package 2^-14 Joules
[   11.509073] RAPL PMU: hw unit of domain dram 2^-14 Joules
[   11.509074] RAPL PMU: hw unit of domain pp1-gpu 2^-14 Joules
[   11.699694] Creating 1 MTD partitions on "intel-spi":
[   11.699698] 0x000000000000-0x000000800000 : "BIOS"
[   11.701466] spi-nor spi0.1: supply vcc not found, using dummy regulator
[   11.702928] Creating 1 MTD partitions on "intel-spi-chip1":
[   11.702931] 0x000000000000-0x000000400000 : "BIOS1"
[   11.754617] scsi 3:0:0:1: Wrong diagnostic page; asked for 1 got 8
[   11.754621] scsi 3:0:0:1: Failed to get diagnostic page 0x1
[   11.754623] scsi 3:0:0:1: Failed to bind enclosure -19
[   11.754637] ses 3:0:0:1: Attached Enclosure device
[   11.903642] usb 1-1.2: new high-speed USB device number 20 using ehci-pci
[   11.991263] usb 1-1.2: New USB device found, idVendor=1a40, idProduct=0101, bcdDevice= 1.11
[   11.991267] usb 1-1.2: New USB device strings: Mfr=0, Product=1, SerialNumber=0
[   11.991268] usb 1-1.2: Product: USB 2.0 Hub
[   11.991663] hub 1-1.2:1.0: USB hub found
[   11.991730] hub 1-1.2:1.0: 4 ports detected
[   12.456612] input: PC Speaker as /devices/platform/pcspkr/input/input2
[   12.845593] dcdbas dcdbas: Dell Systems Management Base Driver (version 5.6.0-3.4)
[   14.784442] EXT4-fs (sde1): mounted filesystem b53dcfc5-02f4-4b80-bf72-33feb8b03f09 r/w with ordered data mode. Quota mode: none.
[   14.830770] Adding 8388604k swap on /dev/mapper/pve-swap.  Priority:-2 extents:1 across:8388604k 
[   14.848288] i915 0000:00:02.0: [drm] Found haswell (device ID 041a) integrated display version 7.00 stepping N/A
[   14.848524] i915 0000:00:02.0: [drm] VT-d active for gfx access
[   14.848551] i915 0000:00:02.0: vgaarb: deactivate vga console
[   14.848995] Console: switching to colour dummy device 80x25
[   14.849105] i915 0000:00:02.0: [drm] Using Transparent Hugepages
[   14.849109] i915 0000:00:02.0: [drm] DMAR active, disabling use of stolen memory
[   14.849720] i915 0000:00:02.0: vgaarb: VGA decodes changed: olddecodes=io+mem,decodes=io+mem:owns=io+mem
[   14.866630] i915 0000:00:02.0: [drm] Registered 3 planes with drm panic
[   14.866634] [drm] Initialized i915 1.6.0 for 0000:00:02.0 on minor 0
[   14.868112] ACPI: video: Video Device [GFX0] (multi-head: yes  rom: no  post: no)
[   14.868319] input: Video Bus as /devices/LNXSYSTM:00/LNXSYBUS:00/PNP0A08:00/LNXVIDEO:00/input/input3
[   14.891725] i915 0000:00:02.0: [drm] Cannot find any crtc or sizes
[   14.926937] intel_rapl_common: Found RAPL domain package
[   14.926939] intel_rapl_common: Found RAPL domain core
[   14.926940] intel_rapl_common: Found RAPL domain uncore
[   14.926941] intel_rapl_common: Found RAPL domain dram
[   14.926958] intel_rapl_common: package-0:package:long_term locked by BIOS
[   14.926960] intel_rapl_common: package-0:package:short_term locked by BIOS
[   14.931884] snd_hda_intel 0000:00:03.0: bound 0000:00:02.0 (ops intel_audio_component_bind_ops [i915])
[   14.944745] i915 0000:00:02.0: [drm] Cannot find any crtc or sizes
[   14.957673] i915 0000:00:02.0: [drm] Cannot find any crtc or sizes
[   14.963820] input: HDA Intel HDMI HDMI/DP,pcm=3 as /devices/pci0000:00/0000:00:03.0/sound/card0/input4
[   14.963870] input: HDA Intel HDMI HDMI/DP,pcm=7 as /devices/pci0000:00/0000:00:03.0/sound/card0/input5
[   14.963904] input: HDA Intel HDMI HDMI/DP,pcm=8 as /devices/pci0000:00/0000:00:03.0/sound/card0/input6
[   14.991480] EXT4-fs (sdc1): mounted filesystem 1bb5976a-a9b9-467d-bdc1-aecf3810590b r/w with ordered data mode. Quota mode: none.
[   15.152657] EXT4-fs (sdb): mounted filesystem 3898f700-297d-4a6b-a449-71ccf7b22047 r/w with ordered data mode. Quota mode: none.
[   17.358019] usb 1-1.2: USB disconnect, device number 20
[   55.655103] EXT4-fs (sdf1): mounted filesystem 49bd1b9e-f31c-4f0a-9790-5b4b330c5708 r/w with ordered data mode. Quota mode: none.
[   62.405642] vmbr0: port 1(nic0) entered blocking state
[   62.405646] vmbr0: port 1(nic0) entered disabled state
[   62.405662] e1000e 0000:00:19.0 nic0: entered allmulticast mode
[   62.405701] e1000e 0000:00:19.0 nic0: entered promiscuous mode
[   65.395789] e1000e 0000:00:19.0 nic0: NIC Link is Up 1000 Mbps Full Duplex, Flow Control: None
[   65.395829] vmbr0: port 1(nic0) entered blocking state
[   65.395832] vmbr0: port 1(nic0) entered forwarding state
[  116.474471] datanet: port 1(enx8cae4ccda926) entered blocking state
[  116.474475] datanet: port 1(enx8cae4ccda926) entered disabled state
[  116.474488] cdc_ncm 4-2.2:2.0 enx8cae4ccda926: entered allmulticast mode
[  116.474543] cdc_ncm 4-2.2:2.0 enx8cae4ccda926: entered promiscuous mode
[  116.803095] datanet: port 1(enx8cae4ccda926) entered blocking state
[  116.803101] datanet: port 1(enx8cae4ccda926) entered forwarding state
[  118.981050] audit: type=1400 audit(1784926803.169:2): apparmor="STATUS" operation="profile_load" profile="unconfined" name="/usr/bin/lxc-copy" pid=1262 comm="apparmor_parser"
[  119.141724] audit: type=1400 audit(1784926803.330:3): apparmor="STATUS" operation="profile_load" profile="unconfined" name="/usr/bin/lxc-start" pid=1300 comm="apparmor_parser"
[  119.554013] audit: type=1400 audit(1784926803.742:4): apparmor="STATUS" operation="profile_load" profile="unconfined" name="lxc-container-default" pid=1318 comm="apparmor_parser"
[  119.554019] audit: type=1400 audit(1784926803.742:5): apparmor="STATUS" operation="profile_load" profile="unconfined" name="lxc-container-default-cgns" pid=1318 comm="apparmor_parser"
[  119.554020] audit: type=1400 audit(1784926803.742:6): apparmor="STATUS" operation="profile_load" profile="unconfined" name="lxc-container-default-with-mounting" pid=1318 comm="apparmor_parser"
[  119.554021] audit: type=1400 audit(1784926803.742:7): apparmor="STATUS" operation="profile_load" profile="unconfined" name="lxc-container-default-with-nesting" pid=1318 comm="apparmor_parser"
[  127.558692] NFSD: Using nfsdcld client tracking operations.
[  127.558696] NFSD: starting 90-second grace period (net effffff9)
[  129.681303] kvm_intel: L1TF CPU bug present and SMT on, data leak possible. See CVE-2018-3646 and https://www.kernel.org/doc/html/latest/admin-guide/hw-vuln/l1tf.html for details.
[  130.289797] tap400i0: entered promiscuous mode
[  130.362352] vmbr0: port 2(fwpr400p0) entered blocking state
[  130.362357] vmbr0: port 2(fwpr400p0) entered disabled state
[  130.362368] fwpr400p0: entered allmulticast mode
[  130.362422] fwpr400p0: entered promiscuous mode
[  130.362467] vmbr0: port 2(fwpr400p0) entered blocking state
[  130.362470] vmbr0: port 2(fwpr400p0) entered forwarding state
[  130.369811] fwbr400i0: port 1(fwln400i0) entered blocking state
[  130.369815] fwbr400i0: port 1(fwln400i0) entered disabled state
[  130.369831] fwln400i0: entered allmulticast mode
[  130.369869] fwln400i0: entered promiscuous mode
[  130.369940] fwbr400i0: port 1(fwln400i0) entered blocking state
[  130.369943] fwbr400i0: port 1(fwln400i0) entered forwarding state
[  130.377204] fwbr400i0: port 2(tap400i0) entered blocking state
[  130.377208] fwbr400i0: port 2(tap400i0) entered disabled state
[  130.377223] tap400i0: entered allmulticast mode
[  130.377288] fwbr400i0: port 2(tap400i0) entered blocking state
[  130.377290] fwbr400i0: port 2(tap400i0) entered forwarding state
[  130.536262] NFSD: all clients done reclaiming, ending NFSv4 grace period (net effffff9)
[  134.023890] WARNING! power/level is deprecated; use power/control instead
[  290.175534] usb 1-1.2: new high-speed USB device number 21 using ehci-pci
[  290.262185] usb 1-1.2: New USB device found, idVendor=1a40, idProduct=0101, bcdDevice= 1.11
[  290.262189] usb 1-1.2: New USB device strings: Mfr=0, Product=1, SerialNumber=0
[  290.262190] usb 1-1.2: Product: USB 2.0 Hub
[  290.262471] hub 1-1.2:1.0: USB hub found
[  290.262619] hub 1-1.2:1.0: 4 ports detected
[  293.582315] usb 1-1.2: USB disconnect, device number 21
[  440.704244] usb 1-1.2: new high-speed USB device number 22 using ehci-pci
[  440.790859] usb 1-1.2: New USB device found, idVendor=1a40, idProduct=0101, bcdDevice= 1.11
[  440.790863] usb 1-1.2: New USB device strings: Mfr=0, Product=1, SerialNumber=0
[  440.790865] usb 1-1.2: Product: USB 2.0 Hub
[  440.791129] hub 1-1.2:1.0: USB hub found
[  440.791213] hub 1-1.2:1.0: 4 ports detected
[  445.390490] usb 1-1.2: USB disconnect, device number 22
[  446.847245] usb 1-1.2: new high-speed USB device number 23 using ehci-pci
[  446.933868] usb 1-1.2: New USB device found, idVendor=1a40, idProduct=0101, bcdDevice= 1.11
[  446.933871] usb 1-1.2: New USB device strings: Mfr=0, Product=1, SerialNumber=0
[  446.933872] usb 1-1.2: Product: USB 2.0 Hub
[  446.934142] hub 1-1.2:1.0: USB hub found
[  446.934209] hub 1-1.2:1.0: 4 ports detected
[  573.390632] usb 1-1.2: USB disconnect, device number 23
[  575.104413] usb 1-1.2: new high-speed USB device number 24 using ehci-pci
[  575.191133] usb 1-1.2: New USB device found, idVendor=1a40, idProduct=0101, bcdDevice= 1.11
[  575.191137] usb 1-1.2: New USB device strings: Mfr=0, Product=1, SerialNumber=0
[  575.191138] usb 1-1.2: Product: USB 2.0 Hub
[  575.191417] hub 1-1.2:1.0: USB hub found
[  575.191476] hub 1-1.2:1.0: 4 ports detected
[  649.046105] fbcon: i915drmfb (fb0) is primary device
[  649.088982] Console: switching to colour frame buffer device 240x67
[  649.100025] i915 0000:00:02.0: [drm] fb0: i915drmfb frame buffer device
[  671.743601] usb 1-1.2.2: new low-speed USB device number 25 using ehci-pci
[  671.938115] usb 1-1.2.2: New USB device found, idVendor=1a2c, idProduct=2124, bcdDevice= 1.10
[  671.938118] usb 1-1.2.2: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[  671.938120] usb 1-1.2.2: Product: USB Keyboard
[  671.938121] usb 1-1.2.2: Manufacturer: SEM
[  671.968458] hid: raw HID events driver (C) Jiri Kosina
[  671.991996] usbcore: registered new interface driver usbhid
[  671.991999] usbhid: USB HID core driver
[  671.993721] usbcore: registered new interface driver usbkbd
[  672.004969] input: SEM USB Keyboard as /devices/pci0000:00/0000:00:1a.0/usb1/1-1/1-1.2/1-1.2.2/1-1.2.2:1.0/0003:1A2C:2124.0001/input/input7
[  672.055829] hid-generic 0003:1A2C:2124.0001: input,hidraw0: USB HID v1.10 Keyboard [SEM USB Keyboard] on usb-0000:00:1a.0-1.2.2/input0
[  672.055980] input: SEM USB Keyboard Consumer Control as /devices/pci0000:00/0000:00:1a.0/usb1/1-1/1-1.2/1-1.2.2/1-1.2.2:1.1/0003:1A2C:2124.0002/input/input8
[  672.106756] input: SEM USB Keyboard System Control as /devices/pci0000:00/0000:00:1a.0/usb1/1-1/1-1.2/1-1.2.2/1-1.2.2:1.1/0003:1A2C:2124.0002/input/input9
[  672.106937] hid-generic 0003:1A2C:2124.0002: input,hidraw1: USB HID v1.10 Device [SEM USB Keyboard] on usb-0000:00:1a.0-1.2.2/input1
[  790.990873] usb 1-1.2: USB disconnect, device number 24
[  790.990877] usb 1-1.2.2: USB disconnect, device number 25
[ 1962.614544] usb 1-1.2: new high-speed USB device number 26 using ehci-pci
[ 1962.691136] usb 1-1.2: New USB device found, idVendor=1a40, idProduct=0101, bcdDevice= 1.11
[ 1962.691140] usb 1-1.2: New USB device strings: Mfr=0, Product=1, SerialNumber=0
[ 1962.691142] usb 1-1.2: Product: USB 2.0 Hub
[ 1962.691458] hub 1-1.2:1.0: USB hub found
[ 1962.691510] hub 1-1.2:1.0: 4 ports detected
[ 1963.075538] usb 1-1.2.1: new low-speed USB device number 27 using ehci-pci
[ 1963.268667] usb 1-1.2.1: New USB device found, idVendor=046d, idProduct=c077, bcdDevice=72.00
[ 1963.268670] usb 1-1.2.1: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[ 1963.268671] usb 1-1.2.1: Product: USB Optical Mouse
[ 1963.268672] usb 1-1.2.1: Manufacturer: Logitech
[ 1963.270595] input: Logitech USB Optical Mouse as /devices/pci0000:00/0000:00:1a.0/usb1/1-1/1-1.2/1-1.2.1/1-1.2.1:1.0/0003:046D:C077.0003/input/input10
[ 1963.270675] hid-generic 0003:046D:C077.0003: input,hidraw0: USB HID v1.11 Mouse [Logitech USB Optical Mouse] on usb-0000:00:1a.0-1.2.1/input0
[ 1963.299679] usbcore: registered new interface driver usbmouse
[ 1963.443578] usb 1-1.2.2: new low-speed USB device number 28 using ehci-pci
[ 1963.639184] usb 1-1.2.2: New USB device found, idVendor=1a2c, idProduct=2124, bcdDevice= 1.10
[ 1963.639188] usb 1-1.2.2: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[ 1963.639189] usb 1-1.2.2: Product: USB Keyboard
[ 1963.639190] usb 1-1.2.2: Manufacturer: SEM
[ 1963.641754] input: SEM USB Keyboard as /devices/pci0000:00/0000:00:1a.0/usb1/1-1/1-1.2/1-1.2.2/1-1.2.2:1.0/0003:1A2C:2124.0004/input/input11
[ 1963.723657] hid-generic 0003:1A2C:2124.0004: input,hidraw1: USB HID v1.10 Keyboard [SEM USB Keyboard] on usb-0000:00:1a.0-1.2.2/input0
[ 1963.726119] input: SEM USB Keyboard Consumer Control as /devices/pci0000:00/0000:00:1a.0/usb1/1-1/1-1.2/1-1.2.2/1-1.2.2:1.1/0003:1A2C:2124.0005/input/input12
[ 1963.776618] input: SEM USB Keyboard System Control as /devices/pci0000:00/0000:00:1a.0/usb1/1-1/1-1.2/1-1.2.2/1-1.2.2:1.1/0003:1A2C:2124.0005/input/input13
[ 1963.776667] hid-generic 0003:1A2C:2124.0005: input,hidraw2: USB HID v1.10 Device [SEM USB Keyboard] on usb-0000:00:1a.0-1.2.2/input1
[ 1964.752169] usb 1-1.2: USB disconnect, device number 26
[ 1964.752173] usb 1-1.2.1: USB disconnect, device number 27
[ 1964.778760] usb 1-1.2.2: USB disconnect, device number 28
[ 5839.723014] EXT4-fs (sda1): mounted filesystem 0510ec81-11e5-412d-8a33-56ee3bf8e8f5 r/w with ordered data mode. Quota mode: none.
[24623.023201] EXT4-fs (sda1): unmounting filesystem 0510ec81-11e5-412d-8a33-56ee3bf8e8f5.
[24628.551484] EXT4-fs (sda1): mounted filesystem 0510ec81-11e5-412d-8a33-56ee3bf8e8f5 r/w with ordered data mode. Quota mode: none.
[27473.641701] perf: interrupt took too long (2515 > 2500), lowering kernel.perf_event_max_sample_rate to 79000
[40134.345575] perf: interrupt took too long (3166 > 3143), lowering kernel.perf_event_max_sample_rate to 63000
[119162.807123] perf: interrupt took too long (3974 > 3957), lowering kernel.perf_event_max_sample_rate to 50000
[169761.002378] Kernel: 'panic_print' sysctl interface will be obsoleted by both 'panic_sys_info' and 'panic_console_replay'
[169770.468961] sh (531834): drop_caches: 3
[169774.032308] sh (531836): drop_caches: 3
[169777.124410] sh (531850): drop_caches: 3
[174485.688356] sh (550326): drop_caches: 3
[174489.002532] sh (550331): drop_caches: 3
[174492.059607] sh (550333): drop_caches: 3
[206942.490045] sd 3:0:0:0: [sdf] tag#0 FAILED Result: hostbyte=DID_OK driverbyte=DRIVER_OK cmd_age=0s
[206942.490060] sd 3:0:0:0: [sdf] tag#0 Sense Key : Illegal Request [current] 
[206942.490063] sd 3:0:0:0: [sdf] tag#0 Add. Sense: Invalid command operation code
[206942.490065] sd 3:0:0:0: [sdf] tag#0 CDB: Write same(16) 93 08 00 00 00 00 00 00 cb 70 00 03 3c 90 00 00
[206942.490076] critical target error, dev sdf, sector 52080 op 0x3:(DISCARD) flags 0x800 phys_seg 1 prio class 2
[280364.890227] sh (885320): drop_caches: 3
[280368.096846] sh (885325): drop_caches: 3
[280371.182014] sh (885341): drop_caches: 3
[347684.988118] perf: interrupt took too long (5015 > 4967), lowering kernel.perf_event_max_sample_rate to 39000
[360722.796637] systemd-journald[394]: Under memory pressure, flushing caches.
[360732.733412] systemd-journald[394]: Under memory pressure, flushing caches.
[360734.005247] systemd-journald[394]: Under memory pressure, flushing caches.
[360971.011664] systemd-journald[394]: Under memory pressure, flushing caches.
[360974.066301] systemd-journald[394]: Under memory pressure, flushing caches.
[361016.625818] systemd-journald[394]: Under memory pressure, flushing caches.
[365097.896931] systemd-journald[394]: Under memory pressure, flushing caches.
[365100.175032] systemd-journald[394]: Under memory pressure, flushing caches.
[365215.886083] systemd-journald[394]: Under memory pressure, flushing caches.

--- cpu MHz (live snapshot)
    $ grep -c ^processor /proc/cpuinfo
8

###############################################################################
# 5. MEMORY / NUMA / SWAP
###############################################################################

--- free -h
    $ free -h
               total        used        free      shared  buff/cache   available
Mem:            15Gi       2.1Gi       6.9Gi        27Mi       6.9Gi        13Gi
Swap:          8.0Gi       832Mi       7.2Gi

--- free -b
    $ free -b
               total        used        free      shared  buff/cache   available
Mem:     16673505280  2270343168  7408971776    28487680  7375622144 14403162112
Swap:     8589930496   873431040  7716499456

--- swapon
    $ swapon --show
NAME      TYPE      SIZE USED PRIO
/dev/dm-0 partition   8G 833M   -2

--- /proc/meminfo highlights
    $ grep -E MemTotal|MemFree|MemAvailable|Buffers|^Cached|SwapTotal|SwapFree|Hugepagesize|HugePages_Total|HugePages_Free|AnonHugePages|DirectMap|Slab|SReclaimable|SUnreclaim|Dirty|Writeback|AnonPages|Mapped|Shmem|KernelStack|PageTables|NFS_Unstable /proc/meminfo
MemTotal:       16282720 kB
MemFree:         7234520 kB
MemAvailable:   14064960 kB
Buffers:         2018140 kB
Cached:          4924008 kB
SwapTotal:       8388604 kB
SwapFree:        7535644 kB
Dirty:               968 kB
Writeback:             0 kB
AnonPages:       1472168 kB
Mapped:           118820 kB
Shmem:             27820 kB
Slab:             399520 kB
SReclaimable:     260784 kB
SUnreclaim:       138736 kB
KernelStack:        5380 kB
PageTables:        14344 kB
SecPageTables:      5792 kB
NFS_Unstable:          0 kB
WritebackTmp:          0 kB
AnonHugePages:    880640 kB
ShmemHugePages:     6144 kB
ShmemPmdMapped:        0 kB
FilePmdMapped:         0 kB
HugePages_Total:       0
HugePages_Free:        0
Hugepagesize:       2048 kB
DirectMap4k:      322024 kB
DirectMap2M:     7972864 kB
DirectMap1G:     9437184 kB

--- numa stat
    $ cat /proc/sys/vm/numa_stat
1

--- numa_balancing
    $ cat /proc/sys/kernel/numa_balancing
0

--- zone reclaim
    $ cat /proc/sys/vm/zone_reclaim_mode
0

--- slab top (top 20)
    $ slabtop -o -s c
 Active / Total Objects (% used)    : 2355070 / 2379286 (99.0%)
 Active / Total Slabs (% used)      : 60847 / 60847 (100.0%)
 Active / Total Caches (% used)     : 371 / 472 (78.6%)
 Active / Total Size (% used)       : 344264.00K / 353948.88K (97.3%)
 Minimum / Average / Maximum Object : 0.01K / 0.15K / 16.00K

  OBJS ACTIVE  USE OBJ SIZE  SLABS OBJ/SLAB CACHE SIZE NAME                   
1519362 1519362 100%    0.10K  38958       39    155832K buffer_head            
 92092  84318  91%    0.57K   3289       28     52624K radix_tree_node        
 13659  13659 100%    1.10K    471       29     15072K ext4_inode_cache       
 94172  94172 100%    0.15K   3622       26     14488K ext4_groupinfo_4k      
 63930  63927  99%    0.13K   2131       30      8524K kernfs_node_cache      
 39207  39207 100%    0.19K   1867       21      7468K dentry                 
  8325   8325 100%    0.62K    333       25      5328K inode_cache            
   408    386  94%   10.44K    136        3      4352K task_struct            
  5911   5551  93%    0.69K    257       23      4112K proc_inode_cache       
  1024   1024 100%    4.00K    128        8      4096K kmalloc-rnd-07-4k      
  7296   4401  60%    0.50K    228       32      3648K kmalloc-rnd-05-512     
 33212  33212 100%    0.09K    722       46      2888K lsm_inode_cache        
 14469  14437  99%    0.19K    689       21      2756K vm_area_struct         
  2720   2494  91%    0.77K    136       20      2176K shmem_inode_cache      
  8480   4723  55%    0.25K    265       32      2120K kmalloc-rnd-05-256     
 49062  49062 100%    0.04K    481      102      1924K extent_status          
 25760  25126  97%    0.07K    460       56      1840K vmap_area              
  1728   1674  96%    1.00K     54       32      1728K iommu_iova_magazine    
 24896  22904  91%    0.06K    389       64      1556K kmalloc-cg-64          
 23872  23367  97%    0.06K    373       64      1492K dmaengine-unmap-2      
  2976   2976 100%    0.50K     93       32      1488K kmalloc-rnd-07-512     
  2150   2150 100%    0.63K     86       25      1376K debugfs_inode_cache    
   656    568  86%    2.00K     41       16      1312K kmalloc-cg-2k          
  2624   2511  95%    0.50K     82       32      1312K kmalloc-rnd-14-512     
   465    465 100%    2.06K     31       15       992K sighand_cache          
   240    176  73%    4.00K     30        8       960K kmalloc-rnd-02-4k      
   812    776  95%    1.12K     29       28       928K signal_cache           
  1053   1053 100%    0.81K     27       39       864K sock_inode_cache       
   208    192  92%    4.00K     26        8       832K biovec-max             
   200    187  93%    4.00K     25        8       800K kmalloc-cg-4k          
   100    100 100%    8.00K     25        4       800K kmalloc-rnd-02-8k      
   192    182  94%    4.00K     24        8       768K kmalloc-rnd-15-4k      
   192    157  81%    4.00K     24        8       768K kmalloc-rnd-05-4k      
 12032  11537  95%    0.06K    188       64       752K anon_vma_chain         
  2976   2327  78%    0.25K     93       32       744K maple_node             
  7770   6655  85%    0.09K    185       42       740K kmalloc-cg-96          
  7176   7029  97%    0.10K    184       39       736K anon_vma               
   736    592  80%    1.00K     23       32       736K kmalloc-cg-1k          
  3759   3702  98%    0.19K    179       21       716K kmalloc-rnd-05-192     
   704    704 100%    1.00K     22       32       704K kmalloc-rnd-05-1k      
   588    588 100%    1.12K     21       28       672K drm_i915_gem_object    
  1280   1112  86%    0.50K     40       32       640K pool_workqueue         
  1280   1179  92%    0.50K     40       32       640K kmalloc-rnd-12-512     
   304    304 100%    2.00K     19       16       608K kmalloc-rnd-08-2k      
   608    608 100%    1.00K     19       32       608K kmalloc-rnd-04-1k      
   234    234 100%    2.38K     18       13       576K TCP                    
   288    288 100%    2.00K     18       16       576K kmalloc-rnd-10-2k      
   144    144 100%    4.00K     18        8       576K kmalloc-rnd-06-4k      
  2961   2879  97%    0.19K    141       21       564K filp                   
   256    192  75%    2.00K     16       16       512K kmalloc-rnd-05-2k      
   210    210 100%    2.19K     15       14       480K mem_cgroup             
   120    120 100%    4.00K     15        8       480K kmalloc-rnd-12-4k      
   112    112 100%    4.00K     14        8       448K names_cache            
   294    294 100%    1.50K     14       21       448K mm_struct              
  4410   4231  95%    0.09K    105       42       420K trace_event_file       
   104     88  84%    4.00K     13        8       416K kmalloc-4k             
  7519   7519 100%    0.05K    103       73       412K ftrace_event_field     
  1008   1008 100%    0.38K     48       21       384K mnt_cache              
    48     48 100%    8.00K     12        4       384K kmalloc-rnd-10-8k      
   506    483  95%    0.69K     22       23       352K skbuff_small_head      
   187    187 100%    1.88K     11       17       352K mem_cgroup_per_node    
   264    264 100%    1.31K     11       24       352K perf_event             
    88     88 100%    4.00K     11        8       352K kmalloc-rnd-10-4k      
   352    352 100%    1.00K     11       32       352K kmalloc-rnd-03-1k      
    44     44 100%    8.00K     11        4       352K kmalloc-rnd-01-8k      
   176    176 100%    2.00K     11       16       352K kmalloc-rnd-01-2k      
   352    352 100%    1.00K     11       32       352K kmalloc-1k             
  1785   1666  93%    0.19K     85       21       340K pid                    
  1312   1280  97%    0.25K     41       32       328K nf_conntrack           
   320    320 100%    1.00K     10       32       320K kmalloc-rnd-13-1k      
    40     40 100%    8.00K     10        4       320K kmalloc-rnd-11-8k      
    80     80 100%    4.00K     10        8       320K kmalloc-rnd-11-4k      
    80     80 100%    4.00K     10        8       320K kmalloc-rnd-09-4k      
   320    320 100%    1.00K     10       32       320K kmalloc-rnd-09-1k      
    40     40 100%    8.00K     10        4       320K kmalloc-rnd-05-8k      
   160    160 100%    2.00K     10       16       320K kmalloc-rnd-02-2k      
  1184   1142  96%    0.25K     37       32       296K skbuff_head_cache      
   234    234 100%    1.19K      9       26       288K RAWv6                  
   288    288 100%    1.00K      9       32       288K RAW                    
    36     36 100%    8.00K      9        4       288K kmalloc-rnd-14-8k      
   288    288 100%    1.00K      9       32       288K kmalloc-rnd-14-1k      
   144    144 100%    2.00K      9       16       288K kmalloc-rnd-11-2k      
    72     72 100%    4.00K      9        8       288K kmalloc-rnd-08-4k      
   144    144 100%    2.00K      9       16       288K kmalloc-rnd-03-2k      
   288    288 100%    1.00K      9       32       288K kmalloc-rnd-02-1k      
    36     36 100%    8.00K      9        4       288K kmalloc-8k             
  6630   6630 100%    0.04K     65      102       260K khugepaged_mm_slot     
   192    192 100%    1.32K      8       24       256K nfs4_client            
   184    184 100%    1.38K      8       23       256K UDPv6                  
    96     96 100%    2.56K      8       12       256K TCPv6                  
   288    288 100%    0.88K      8       36       256K fuse_inode             
   208    208 100%    1.19K      8       26       256K UDP                    
   128    128 100%    2.00K      8       16       256K biovec-128             
    64     64 100%    4.00K      8        8       256K memdup_user-4k         
    32     32 100%    8.00K      8        4       256K kmalloc-cg-8k          
    32     32 100%    8.00K      8        4       256K kmalloc-rnd-15-8k      
   128    128 100%    2.00K      8       16       256K kmalloc-rnd-15-2k      
    64     64 100%    4.00K      8        8       256K kmalloc-rnd-14-4k      
   128    128 100%    2.00K      8       16       256K kmalloc-rnd-14-2k      
   128    128 100%    2.00K      8       16       256K kmalloc-rnd-13-2k      
    32     32 100%    8.00K      8        4       256K kmalloc-rnd-12-8k      
   128    128 100%    2.00K      8       16       256K kmalloc-rnd-12-2k      
   256    256 100%    1.00K      8       32       256K kmalloc-rnd-12-1k      
   256    256 100%    1.00K      8       32       256K kmalloc-rnd-11-1k      
    32     32 100%    8.00K      8        4       256K kmalloc-rnd-09-8k      
   256    256 100%    1.00K      8       32       256K kmalloc-rnd-08-1k      
   128    128 100%    2.00K      8       16       256K kmalloc-rnd-07-2k      
   256    256 100%    1.00K      8       32       256K kmalloc-rnd-07-1k      
   128    128 100%    2.00K      8       16       256K kmalloc-rnd-06-2k      
   256    256 100%    1.00K      8       32       256K kmalloc-rnd-06-1k      
    64     64 100%    4.00K      8        8       256K kmalloc-rnd-04-4k      
   128    128 100%    2.00K      8       16       256K kmalloc-rnd-04-2k      
   256    256 100%    1.00K      8       32       256K kmalloc-rnd-01-1k      
   128    128 100%    2.00K      8       16       256K kmalloc-2k             
  2688   2688 100%    0.09K     64       42       256K kmalloc-96             
   992    916  92%    0.25K     31       32       248K kmalloc-rnd-10-256     
   224    224 100%    1.00K      7       32       224K kmalloc-rnd-10-1k      
   112    112 100%    2.00K      7       16       224K kmalloc-rnd-09-2k      
    28     28 100%    8.00K      7        4       224K kmalloc-rnd-03-8k      
   832    704  84%    0.25K     26       32       208K bio-200                
  1092   1092 100%    0.19K     52       21       208K kmalloc-cg-192         
   625    500  80%    0.31K     25       25       200K bio-256                
  1008   1008 100%    0.19K     48       21       192K proc_dir_entry         
   114    114 100%    1.62K      6       19       192K bdev_cache             
    24     24 100%    8.00K      6        4       192K kmalloc-rnd-13-8k      
    24     24 100%    8.00K      6        4       192K kmalloc-rnd-07-8k      
   384    384 100%    0.50K     12       32       192K kmalloc-rnd-06-512     
   736    736 100%    0.25K     23       32       184K kmalloc-rnd-14-256     
   736    736 100%    0.25K     23       32       184K kmalloc-rnd-07-256     
   253    253 100%    0.69K     11       23       176K files_cache            
   352    352 100%    0.50K     11       32       176K kmalloc-cg-512         
   352    352 100%    0.50K     11       32       176K kmalloc-rnd-15-512     
  1806   1674  92%    0.09K     43       42       172K kmalloc-rnd-02-96      
 11008  10955  99%    0.02K     43      256       172K kmalloc-rnd-01-16      
  1344   1290  95%    0.12K     42       32       168K bio_integrity_data     
  1312   1296  98%    0.12K     41       32       164K eventpoll_epi          
   861    848  98%    0.19K     41       21       164K kmalloc-rnd-01-192     
   160    160 100%    0.98K      5       32       160K request_queue          
    20     20 100%    8.00K      5        4       160K memdup_user-8k         
    80     80 100%    2.00K      5       16       160K memdup_user-2k         
   240    240 100%    0.65K     10       24       160K tracefs_inode_cache    
   250    250 100%    0.62K     10       25       160K task_group             
   160    160 100%    1.00K      5       32       160K kmalloc-rnd-15-1k      
    20     20 100%    8.00K      5        4       160K kmalloc-rnd-06-8k      
    40     40 100%    4.00K      5        8       160K kmalloc-rnd-01-4k      
   320    320 100%    0.50K     10       32       160K kmalloc-rnd-01-512     
   640    640 100%    0.25K     20       32       160K kmem_cache             
  4992   4949  99%    0.03K     39      128       156K kmalloc-rnd-01-32      
  1596   1596 100%    0.09K     38       42       152K kmalloc-rcl-96         
  2432   2190  90%    0.06K     38       64       152K kmalloc-rnd-11-64      
  1596   1596 100%    0.09K     38       42       152K kmalloc-rnd-11-96      
   608    608 100%    0.25K     19       32       152K kmalloc-rnd-03-256     
  1036   1036 100%    0.14K     37       28       148K nfsd_file              
   814    814 100%    0.18K     37       22       148K kvm_mmu_page_header    
   777    777 100%    0.19K     37       21       148K file_lock_cache        
   378    378 100%    0.38K     18       21       144K bio-320                
  1512   1117  73%    0.09K     36       42       144K kmalloc-rnd-13-96      
   576    576 100%    0.25K     18       32       144K kmalloc-rnd-08-256     
   288    288 100%    0.50K      9       32       144K kmalloc-rnd-04-512     
   288    288 100%    0.50K      9       32       144K kmalloc-rnd-03-512     
  2975   2975 100%    0.05K     35       85       140K shared_policy_node     
  4352   4352 100%    0.03K     34      128       136K kmalloc-rnd-08-32      
  2176   2176 100%    0.06K     34       64       136K kmalloc-rnd-03-64      
  1056   1056 100%    0.12K     33       32       132K kmalloc-rnd-05-128     
   248    248 100%    0.51K      8       31       128K nfs4_delegation        
  1088    952  87%    0.12K     32       34       128K jbd2_journal_head      
   224    224 100%    0.56K      8       28       128K kioctx                 
   128    128 100%    1.00K      4       32       128K PING                   
   128    128 100%    1.00K      4       32       128K memdup_user-1k         
   232    232 100%    0.55K      8       29       128K taskstats              
   256    256 100%    0.50K      8       32       128K kmalloc-rnd-13-512     
  8192   8192 100%    0.02K     32      256       128K kmalloc-rnd-13-16      
   256    256 100%    0.50K      8       32       128K kmalloc-rnd-11-512     
   256    256 100%    0.50K      8       32       128K kmalloc-rnd-10-512     
   256    256 100%    0.50K      8       32       128K kmalloc-rnd-09-512     
   256    256 100%    0.50K      8       32       128K kmalloc-rnd-08-512     
    16     16 100%    8.00K      4        4       128K kmalloc-rnd-04-8k      
   256    256 100%    0.50K      8       32       128K kmalloc-rnd-02-512     
   256    256 100%    0.50K      8       32       128K kmalloc-512            
   480    480 100%    0.25K     15       32       120K kmalloc-rnd-12-256     
   161    161 100%    0.69K      7       23       112K rpc_inode_cache        
  1008    868  86%    0.11K     28       36       112K ext4_prealloc_space    
  2044   1752  85%    0.05K     28       73       112K mb_cache_entry         
   259    259 100%    0.42K      7       37       112K uts_namespace          
  1792   1792 100%    0.06K     28       64       112K kmalloc-rnd-08-64      
   567    567 100%    0.19K     27       21       108K kmalloc-rnd-14-192     
  1326   1326 100%    0.08K     26       51       104K sigqueue               
  4420   4285  96%    0.02K     26      170       104K lsm_file_cache         
   416    416 100%    0.25K     13       32       104K kmalloc-rnd-15-256     
   525    525 100%    0.19K     25       21       100K kmalloc-192            
     9      9 100%    9.00K      3        3        96K kvm_vcpu               
    36     36 100%    2.61K      3       12        96K x86_emulator           
     6      6 100%   16.00K      3        2        96K zio_buf_comb_16384     
    15     15 100%    5.81K      3        5        96K net_namespace          
   768    768 100%    0.12K     24       32        96K kmalloc-rcl-128        
   504    504 100%    0.19K     24       21        96K kmalloc-rnd-15-192     
   384    384 100%    0.25K     12       32        96K kmalloc-rnd-13-256     
   704    610  86%    0.12K     22       32        88K kmalloc-cg-128         
   250    250 100%    0.31K     10       25        80K bio-264                
   130    130 100%    0.60K      5       26        80K user_namespace         
  2560   2560 100%    0.03K     20      128        80K kmalloc-rnd-10-32      
   288    288 100%    0.25K      9       32        72K kmalloc-cg-256         
  1152   1152 100%    0.06K     18       64        72K kmalloc-rnd-15-64      
  2304   2304 100%    0.03K     18      128        72K kmalloc-rnd-11-32      
   288    288 100%    0.25K      9       32        72K kmalloc-rnd-04-256     
  2304   2304 100%    0.03K     18      128        72K kmalloc-rnd-02-32      
   288    288 100%    0.25K      9       32        72K kmalloc-rnd-01-256     
   867    867 100%    0.08K     17       51        68K Acpi-State             
  2176   2176 100%    0.03K     17      128        68K kmalloc-cg-32          
   160    160 100%    0.39K      8       20        64K nfs4_openowner         
   208    208 100%    0.30K      8       26        64K btrfs_delayed_node     
    30     30 100%    2.06K      2       15        64K MPTCPv6                
   248    248 100%    0.26K      8       31        64K tw_sock_TCPv6          
    32     32 100%    1.94K      2       16        64K MPTCP                  
   248    248 100%    0.26K      8       31        64K tw_sock_TCP            
   200    200 100%    0.31K      8       25        64K request_sock_TCP       
   100    100 100%    0.62K      4       25        64K hugetlbfs_inode_cache  
    78     78 100%    0.81K      2       39        64K dax_cache              
   256    256 100%    0.25K      8       32        64K task_delay_info        
    16     16 100%    4.00K      2        8        64K kmalloc-rnd-13-4k      
   256    256 100%    0.25K      8       32        64K kmalloc-rnd-11-256     
  4096   4096 100%    0.02K     16      256        64K kmalloc-rnd-11-16      
   512    512 100%    0.12K     16       32        64K kmalloc-rnd-10-128     
   256    256 100%    0.25K      8       32        64K kmalloc-rnd-09-256     
   256    256 100%    0.25K      8       32        64K kmalloc-rnd-06-256     
   336    336 100%    0.19K     16       21        64K kmalloc-rnd-03-192     
   256    256 100%    0.25K      8       32        64K kmalloc-rnd-02-256     
   256    256 100%    0.25K      8       32        64K kmalloc-256            
   375    375 100%    0.16K     15       25        60K dm_bufio_buffer-16-1   
   960    960 100%    0.06K     15       64        60K kmalloc-rnd-07-64      
  7680   7680 100%    0.01K     15      512        60K kmalloc-rnd-01-8       
   294    294 100%    0.19K     14       21        56K jbd2_transaction_s     
   588    588 100%    0.09K     14       42        56K kmalloc-rnd-06-96      
   896    896 100%    0.06K     14       64        56K kmalloc-rnd-04-64      
   896    896 100%    0.06K     14       64        56K kmalloc-rnd-02-64      
   294    294 100%    0.19K     14       21        56K kmalloc-rnd-02-192     
   546    546 100%    0.09K     13       42        52K kmalloc-rnd-15-96      
   546    546 100%    0.09K     13       42        52K kmalloc-rnd-14-96      
   416    416 100%    0.12K     13       32        52K kmalloc-rnd-11-128     
   832    832 100%    0.06K     13       64        52K kmalloc-rnd-10-64      
   192    192 100%    0.25K      6       32        48K io_kiocb               
    96     96 100%    0.50K      3       32        48K memdup_user-512        
  1536   1536 100%    0.03K     12      128        48K kmalloc-rnd-14-32      
   384    384 100%    0.12K     12       32        48K kmalloc-rnd-03-128     
   768    768 100%    0.06K     12       64        48K kmem_cache_node        
   352    352 100%    0.12K     11       32        44K kmalloc-rnd-13-128     
   704    704 100%    0.06K     11       64        44K kmalloc-rnd-13-64      
   231    231 100%    0.19K     11       21        44K kmalloc-rnd-12-192     
   462    462 100%    0.09K     11       42        44K kmalloc-rnd-09-96      
   704    704 100%    0.06K     11       64        44K kmalloc-64             
  1408   1408 100%    0.03K     11      128        44K kmalloc-32             
   210    210 100%    0.19K     10       21        40K bio-136                
  1280   1280 100%    0.03K     10      128        40K kmalloc-rnd-13-32      
   640    640 100%    0.06K     10       64        40K kmalloc-rnd-12-64      
   210    210 100%    0.19K     10       21        40K kmalloc-rnd-11-192     
  1280   1280 100%    0.03K     10      128        40K kmalloc-rnd-06-32      
  2560   2560 100%    0.02K     10      256        40K kmalloc-rnd-04-16      
   420    420 100%    0.09K     10       42        40K kmalloc-rnd-04-96      
   420    420 100%    0.09K     10       42        40K kmalloc-rnd-03-96      
   288    288 100%    0.12K      9       32        36K scsi_sense_cache       
  4608   4608 100%    0.01K      9      512        36K kmalloc-cg-8           
   576    576 100%    0.06K      9       64        36K kmalloc-rnd-14-64      
   288    288 100%    0.12K      9       32        36K kmalloc-rnd-12-128     
  4608   4608 100%    0.01K      9      512        36K kmalloc-rnd-11-8       
   378    378 100%    0.09K      9       42        36K kmalloc-rnd-10-96      
  1152   1152 100%    0.03K      9      128        36K kmalloc-rnd-09-32      
   288    288 100%    0.12K      9       32        36K kmalloc-rnd-08-128     
   576    576 100%    0.06K      9       64        36K kmalloc-rnd-06-64      
  4608   4608 100%    0.01K      9      512        36K kmalloc-rnd-04-8       
   189    189 100%    0.19K      9       21        36K kmalloc-rnd-04-192     
   288    288 100%    0.12K      9       32        36K kmalloc-rnd-01-128     
   576    576 100%    0.06K      9       64        36K kmalloc-rnd-01-64      
   176    176 100%    0.18K      8       22        32K ip6-frags              
    10     10 100%    3.16K      1       10        32K kcopyd_job             
    34     34 100%    0.94K      1       34        32K mqueue_inode_cache     
   184    184 100%    0.17K      8       23        32K fuse_request           
   192    192 100%    0.16K      8       24        32K ext4_allocation_context
   512    512 100%    0.06K      8       64        32K ext4_io_end            
  1024   1024 100%    0.03K      8      128        32K pending_reservation    
  1024   1024 100%    0.03K      8      128        32K xsk_generic_xmit_cache 
   160     80  50%    0.20K      8       20        32K ip4-frags              
    80     80 100%    0.38K      4       20        32K request_sock_subflow_v4
   680    680 100%    0.05K      8       85        32K ip_fib_trie            
   584    584 100%    0.05K      8       73        32K ip_fib_alias           
  2048   2048 100%    0.02K      8      256        32K ep_head                
   512    512 100%    0.06K      8       64        32K memdup_user-64         
  1024   1024 100%    0.03K      8      128        32K memdup_user-32         
  2048   2048 100%    0.02K      8      256        32K memdup_user-16         
  4096   4096 100%    0.01K      8      512        32K memdup_user-8          
    15     15 100%    2.06K      1       15        32K dmaengine-unmap-256    
    30     30 100%    1.06K      1       30        32K dmaengine-unmap-128    
   200    200 100%    0.16K      8       25        32K file_lease_cache       
  1024   1024 100%    0.03K      8      128        32K pidfs_attr_cache       
   816    816 100%    0.04K      8      102        32K pde_opener             
   272    272 100%    0.12K      8       34        32K seq_file               
   448    448 100%    0.07K      8       56        32K nsproxy                
   312    312 100%    0.10K      8       39        32K Acpi-ParseExt          
  2048   2048 100%    0.02K      8      256        32K kmalloc-cg-16          
   168    168 100%    0.19K      8       21        32K kmalloc-rcl-192        
   256    256 100%    0.12K      8       32        32K kmalloc-rnd-15-128     
  1024   1024 100%    0.03K      8      128        32K kmalloc-rnd-15-32      
  2048   2048 100%    0.02K      8      256        32K kmalloc-rnd-15-16      
  4096   4096 100%    0.01K      8      512        32K kmalloc-rnd-15-8       
   256    256 100%    0.12K      8       32        32K kmalloc-rnd-14-128     
  2048   2048 100%    0.02K      8      256        32K kmalloc-rnd-14-16      
  4096   4096 100%    0.01K      8      512        32K kmalloc-rnd-14-8       
  4096   4096 100%    0.01K      8      512        32K kmalloc-rnd-13-8       
   168    168 100%    0.19K      8       21        32K kmalloc-rnd-13-192     
  1024   1024 100%    0.03K      8      128        32K kmalloc-rnd-12-32      
  2048   2048 100%    0.02K      8      256        32K kmalloc-rnd-12-16      
  4096   4096 100%    0.01K      8      512        32K kmalloc-rnd-12-8       
   336    336 100%    0.09K      8       42        32K kmalloc-rnd-12-96      
  2048   2048 100%    0.02K      8      256        32K kmalloc-rnd-10-16      
  4096   4096 100%    0.01K      8      512        32K kmalloc-rnd-10-8       
   168    168 100%    0.19K      8       21        32K kmalloc-rnd-10-192     
   512    512 100%    0.06K      8       64        32K kmalloc-rnd-09-64      
  4096   4096 100%    0.01K      8      512        32K kmalloc-rnd-09-8       
  2048   2048 100%    0.02K      8      256        32K kmalloc-rnd-08-16      
  4096   4096 100%    0.01K      8      512        32K kmalloc-rnd-08-8       
   336    336 100%    0.09K      8       42        32K kmalloc-rnd-08-96      
   256    256 100%    0.12K      8       32        32K kmalloc-rnd-07-128     
  1024   1024 100%    0.03K      8      128        32K kmalloc-rnd-07-32      
  2048   2048 100%    0.02K      8      256        32K kmalloc-rnd-07-16      
  4096   4096 100%    0.01K      8      512        32K kmalloc-rnd-07-8       
   168    168 100%    0.19K      8       21        32K kmalloc-rnd-07-192     
   336    336 100%    0.09K      8       42        32K kmalloc-rnd-07-96      
   256    256 100%    0.12K      8       32        32K kmalloc-rnd-06-128     
  2048   2048 100%    0.02K      8      256        32K kmalloc-rnd-06-16      
  4096   4096 100%    0.01K      8      512        32K kmalloc-rnd-06-8       
   168    168 100%    0.19K      8       21        32K kmalloc-rnd-06-192     
   512    512 100%    0.06K      8       64        32K kmalloc-rnd-05-64      
  1024   1024 100%    0.03K      8      128        32K kmalloc-rnd-05-32      
  2048   2048 100%    0.02K      8      256        32K kmalloc-rnd-05-16      
  4096   4096 100%    0.01K      8      512        32K kmalloc-rnd-05-8       
   336    336 100%    0.09K      8       42        32K kmalloc-rnd-05-96      
   256    256 100%    0.12K      8       32        32K kmalloc-rnd-04-128     
  1024   1024 100%    0.03K      8      128        32K kmalloc-rnd-04-32      
     8      8 100%    4.00K      1        8        32K kmalloc-rnd-03-4k      
  1024   1024 100%    0.03K      8      128        32K kmalloc-rnd-03-32      
  2048   2048 100%    0.02K      8      256        32K kmalloc-rnd-03-16      
  4096   4096 100%    0.01K      8      512        32K kmalloc-rnd-03-8       
   256    256 100%    0.12K      8       32        32K kmalloc-rnd-02-128     
  2048   2048 100%    0.02K      8      256        32K kmalloc-rnd-02-16      
  4096   4096 100%    0.01K      8      512        32K kmalloc-rnd-02-8       
   336    336 100%    0.09K      8       42        32K kmalloc-rnd-01-96      
  2048   2048 100%    0.02K      8      256        32K kmalloc-16             
  4096   4096 100%    0.01K      8      512        32K kmalloc-8              
   294    294 100%    0.09K      7       42        28K memdup_user-96         
   224    224 100%    0.12K      7       32        28K kmalloc-rnd-09-128     
   224    224 100%    0.12K      7       32        28K kmalloc-128            
   126    126 100%    0.19K      6       21        24K kmalloc-rnd-09-192     
   126    126 100%    0.19K      6       21        24K kmalloc-rnd-08-192     
   105    105 100%    0.19K      5       21        20K bio-176                
  1280   1280 100%    0.02K      5      256        20K jbd2_revoke_table_s    
    23     23 100%    0.69K      1       23        16K i915_request           
    21     21 100%    0.75K      1       21        16K intel_context          
    36     36 100%    0.44K      1       36        16K bio-384                
    36     36 100%    0.44K      1       36        16K bio-400                
    32     32 100%    0.50K      1       32        16K bio-456                
    50     50 100%    0.31K      2       25        16K xfrm_dst               
    50     50 100%    0.31K      2       25        16K bio-280                
    64     64 100%    0.25K      2       32        16K memdup_user-256        
  1024   1024 100%    0.02K      4      256        16K kmalloc-rnd-09-16      
    63     63 100%    0.19K      3       21        12K memdup_user-192        
    32     32 100%    0.25K      1       32         8K bio-240                
    34     34 100%    0.23K      1       34         8K arc_buf_hdr_t_full     
   170    170 100%    0.05K      2       85         8K bio_post_read_ctx      
    30     30 100%    0.27K      1       30         8K numa_policy            
    42     42 100%    0.09K      1       42         4K abd_t                  
    32     32 100%    0.12K      1       32         4K memdup_user-128        
    36     36 100%    0.11K      1       36         4K kmalloc_buckets        
     0      0   0%    0.20K      0       39         0K nf_conntrack_expect    
     0      0   0%    0.12K      0       32         0K i915_dependency        
     0      0   0%    0.06K      0       64         0K execute_cb             
     0      0   0%    0.35K      0       22         0K nfs4_lockowner         
     0      0   0%    0.09K      0       46         0K zfs_znode_hold_cache   
     0      0   0%    1.09K      0       29         0K zfs_znode_cache        
     0      0   0%    1.03K      0       31         0K zap_attr_long_cache    
     0      0   0%    1.07K      0       29         0K zap_name_long          
     0      0   0%    0.28K      0       28         0K zap_attr_cache         
     0      0   0%    0.32K      0       24         0K zap_name               
     0      0   0%    0.16K      0       24         0K sio_cache_2            
     0      0   0%    0.15K      0       26         0K sio_cache_1            
     0      0   0%    0.13K      0       30         0K sio_cache_0            
     0      0   0%    0.15K      0       26         0K zil_zcw_cache          
     0      0   0%    0.38K      0       20         0K zil_lwb_cache          
     0      0   0%    0.37K      0       21         0K dbuf_dirty_record_t    
     0      0   0%    0.36K      0       22         0K dmu_buf_impl_t         
     0      0   0%    0.03K      0      128         0K arc_buf_t              
     0      0   0%    0.09K      0       42         0K arc_buf_hdr_t_l2only   
     0      0   0%    0.91K      0       35         0K dnode_t                
     0      0   0%    0.25K      0       32         0K sa_cache               
     0      0   0%   16.00K      0        2         0K lz4_cache              
     0      0   0%   12.00K      0        2         0K zio_buf_comb_12288     
     0      0   0%    8.00K      0        4         0K zio_buf_comb_8192      
     0      0   0%    6.00K      0        5         0K zio_buf_comb_6144      
     0      0   0%    4.00K      0        8         0K zio_buf_comb_4096      
     0      0   0%    3.00K      0       10         0K zio_buf_comb_3072      
     0      0   0%    2.00K      0       16         0K zio_buf_comb_2048      
     0      0   0%    1.50K      0       21         0K zio_buf_comb_1536      
     0      0   0%    1.00K      0       32         0K zio_buf_comb_1024      
     0      0   0%    0.50K      0       32         0K zio_buf_comb_512       
     0      0   0%    0.05K      0       85         0K zio_link_cache         
     0      0   0%    1.12K      0       28         0K zio_cache              
     0      0   0%    0.32K      0       24         0K ddt_log_entry_trad_cache
     0      0   0%    0.14K      0       28         0K ddt_log_entry_flat_cache
     0      0   0%    0.41K      0       38         0K ddt_entry_trad_cache   
     0      0   0%    0.23K      0       34         0K ddt_entry_flat_cache   
     0      0   0%    0.16K      0       24         0K brt_entry_cache        
     0      0   0%    0.07K      0       56         0K metaslab_alloc_trace_cache
     0      0   0%    4.00K      0        8         0K zfs_btree_leaf_cache   
     0      0   0%    0.06K      0       64         0K kcf_context_cache      
     0      0   0%    0.41K      0       39         0K btrfs_ordered_extent   
     0      0   0%    0.23K      0       34         0K btrfs_extent_buffer    
     0      0   0%    1.00K      0       32         0K btrfs_inode            
     0      0   0%    0.26K      0       31         0K fsverity_info          
     0      0   0%    0.12K      0       32         0K fscrypt_inode_info     
     0      0   0%    0.31K      0       25         0K request_sock_TCPv6     
     0      0   0%    2.82K      0       11         0K dm_uevent              
     0      0   0%    1.00K      0       32         0K ecryptfs_inode_cache   
     0      0   0%    0.02K      0      256         0K ecryptfs_file_cache    
     0      0   0%    0.77K      0       20         0K fat_inode_cache        
     0      0   0%    0.04K      0      102         0K fat_cache              
     0      0   0%    0.69K      0       23         0K squashfs_inode_cache   
     0      0   0%    0.19K      0       21         0K userfaultfd_ctx_cache  
     0      0   0%    0.11K      0       36         0K fanotify_perm_event    
     0      0   0%    0.03K      0      128         0K dnotify_struct         
     0      0   0%    0.28K      0       28         0K pid_namespace          
     0      0   0%    0.38K      0       20         0K request_sock_subflow_v6
     0      0   0%    0.81K      0       39         0K xfrm_state             
     0      0   0%    0.25K      0       32         0K dquot                  
     0      0   0%    8.00K      0        4         0K msg_msg-8k             
     0      0   0%    4.00K      0        8         0K msg_msg-4k             
     0      0   0%    2.00K      0       16         0K msg_msg-2k             
     0      0   0%    1.00K      0       32         0K msg_msg-1k             
     0      0   0%    0.50K      0       32         0K msg_msg-512            
     0      0   0%    0.25K      0       32         0K msg_msg-256            
     0      0   0%    0.12K      0       32         0K msg_msg-128            
     0      0   0%    0.06K      0       64         0K msg_msg-64             
     0      0   0%    0.03K      0      128         0K msg_msg-32             
     0      0   0%    0.02K      0      256         0K msg_msg-16             
     0      0   0%    0.01K      0      512         0K msg_msg-8              
     0      0   0%    0.19K      0       21         0K msg_msg-192            
     0      0   0%    0.09K      0       42         0K msg_msg-96             
     0      0   0%    0.78K      0       20         0K x86_lbr                
     0      0   0%    0.02K      0      256         0K pidfs_xattr_cache      
     0      0   0%    0.25K      0       32         0K bfilp                  
     0      0   0%    0.10K      0       39         0K ima_iint_cache         
     0      0   0%    8.00K      0        4         0K dma-kmalloc-8k         
     0      0   0%    4.00K      0        8         0K dma-kmalloc-4k         
     0      0   0%    2.00K      0       16         0K dma-kmalloc-2k         
     0      0   0%    1.00K      0       32         0K dma-kmalloc-1k         
     0      0   0%    0.50K      0       32         0K dma-kmalloc-512        
     0      0   0%    0.25K      0       32         0K dma-kmalloc-256        
     0      0   0%    0.12K      0       32         0K dma-kmalloc-128        
     0      0   0%    0.06K      0       64         0K dma-kmalloc-64         
     0      0   0%    0.03K      0      128         0K dma-kmalloc-32         
     0      0   0%    0.02K      0      256         0K dma-kmalloc-16         
     0      0   0%    0.01K      0      512         0K dma-kmalloc-8          
     0      0   0%    0.19K      0       21         0K dma-kmalloc-192        
     0      0   0%    0.09K      0       42         0K dma-kmalloc-96         
     0      0   0%    8.00K      0        4         0K kmalloc-rcl-8k         
     0      0   0%    4.00K      0        8         0K kmalloc-rcl-4k         
     0      0   0%    2.00K      0       16         0K kmalloc-rcl-2k         
     0      0   0%    1.00K      0       32         0K kmalloc-rcl-1k         
     0      0   0%    0.50K      0       32         0K kmalloc-rcl-512        
     0      0   0%    0.25K      0       32         0K kmalloc-rcl-256        
     0      0   0%    0.06K      0       64         0K kmalloc-rcl-64         
     0      0   0%    0.03K      0      128         0K kmalloc-rcl-32         
     0      0   0%    0.02K      0      256         0K kmalloc-rcl-16         
     0      0   0%    0.01K      0      512         0K kmalloc-rcl-8          
     0      0   0%    8.00K      0        4         0K kmalloc-rnd-08-8k      

--- kswapd stats
    $ grep -E kswapd|pgmigrate|pgmigrate_failed|compact_ /proc/vmstat
pgdemote_kswapd 0
pgsteal_kswapd 227343685
pgscan_kswapd 229501560
kswapd_inodesteal 49
kswapd_low_wmark_hit_quickly 2442
kswapd_high_wmark_hit_quickly 21
pgmigrate_success 17652739
pgmigrate_fail 21542550
compact_migrate_scanned 1061298769
compact_free_scanned 2883093205
compact_isolated 60168809
compact_stall 15810
compact_fail 8906
compact_success 6904
compact_daemon_wake 10096
compact_daemon_migrate_scanned 756604512
compact_daemon_free_scanned 2880154900

###############################################################################
# 6. KERNEL TUNABLES / SYSCTL
###############################################################################

--- vm.* tunables
    $ sysctl -a 2>/dev/null | grep -E '^vm\.(dirty_(ratio|background_ratio|bytes|background_bytes|expire_centisecs|writeback_centisecs)|swappiness|vfs_cache_pressure|min_free_kbytes|watermark_scale_factor|overcommit_memory|overcommit_ratio|nr_hugepages|nr_overcommit_hugepages|zone_reclaim_mode|compact_unevictable_allowed|stat_interval|admin_reserve_kbytes|user_reserve_kbytes)'
vm.admin_reserve_kbytes = 8192
vm.compact_unevictable_allowed = 1
vm.dirty_background_bytes = 0
vm.dirty_background_ratio = 10
vm.dirty_bytes = 0
vm.dirty_expire_centisecs = 3000
vm.dirty_ratio = 40
vm.dirty_writeback_centisecs = 500
vm.min_free_kbytes = 67584
vm.nr_hugepages = 0
vm.nr_hugepages_mempolicy = 0
vm.nr_overcommit_hugepages = 0
vm.overcommit_memory = 0
vm.overcommit_ratio = 50
vm.stat_interval = 1
vm.swappiness = 1
vm.user_reserve_kbytes = 131072
vm.vfs_cache_pressure = 50
vm.vfs_cache_pressure_denom = 100
vm.watermark_scale_factor = 10
vm.zone_reclaim_mode = 0

--- fs.* tunables
    $ sysctl -a 2>/dev/null | grep -E '^fs\.(file-max|file-nr|aio-max-nr|aio-nr|nr_open|pipe-max-size|epoll/max_user_watches|lease-break-time|mqueue|max_user_ns)'
fs.aio-max-nr = 1048576
fs.aio-nr = 0
fs.file-max = 1000000
fs.file-nr = 2497	0	1000000
fs.lease-break-time = 45
fs.mqueue.msg_default = 10
fs.mqueue.msg_max = 10
fs.mqueue.msgsize_default = 8192
fs.mqueue.msgsize_max = 8192
fs.mqueue.queues_max = 256
fs.nr_open = 1073741816
fs.pipe-max-size = 1048576

--- kernel.* perf-relevant
    $ sysctl -a 2>/dev/null | grep -E '^kernel\.(sched_(child_runs_first|migration_cost|domain|rt_period|rt_runtime|idle)|numa_balancing|watchdog|nmi_watchdog|hung_task|randomize_va_space|max_pid|threads-max|sched_time_avg)'
kernel.hung_task_all_cpu_backtrace = 0
kernel.hung_task_check_count = 4194304
kernel.hung_task_check_interval_secs = 0
kernel.hung_task_detect_count = 0
kernel.hung_task_panic = 0
kernel.hung_task_timeout_secs = 120
kernel.hung_task_warnings = 10
kernel.nmi_watchdog = 1
kernel.numa_balancing = 0
kernel.numa_balancing_promote_rate_limit_MBps = 65536
kernel.randomize_va_space = 2
kernel.sched_rt_period_us = 1000000
kernel.sched_rt_runtime_us = 950000
kernel.threads-max = 126451
kernel.watchdog = 1
kernel.watchdog_cpumask = 0-7
kernel.watchdog_thresh = 10

###############################################################################
# 7. NETWORK SYSCTL / TCP
###############################################################################

--- net.core.* tunables
    $ sysctl -a 2>/dev/null | grep -E '^net\.core\.(rmem_default|rmem_max|wmem_default|wmem_max|optmem_max|somaxconn|netdev_max_backlog|netdev_budget|netdev_budget_usecs|netdev_tstamp_prequeue|rps_flow_cnt|busy_poll|busy_read|default_qdisc|dev_weight|xfrm)'
net.core.busy_poll = 0
net.core.busy_read = 0
net.core.default_qdisc = fq_codel
net.core.dev_weight = 64
net.core.dev_weight_rx_bias = 1
net.core.dev_weight_tx_bias = 1
net.core.netdev_budget = 300
net.core.netdev_budget_usecs = 2000
net.core.netdev_max_backlog = 5000
net.core.netdev_tstamp_prequeue = 1
net.core.optmem_max = 131072
net.core.rmem_default = 262144
net.core.rmem_max = 16777216
net.core.somaxconn = 1024
net.core.wmem_default = 262144
net.core.wmem_max = 16777216
net.core.xfrm_acq_expires = 30
net.core.xfrm_aevent_etime = 10
net.core.xfrm_aevent_rseqth = 2
net.core.xfrm_larval_drop = 1

--- net.ipv4.tcp.* tunables
    $ sysctl -a 2>/dev/null | grep -E '^net\.ipv4\.tcp_(rmem|wmem|congestion_control|available_congestion_control|mtu_probing|slow_start_after_idle|no_metrics_save|timestamps|window_scaling|sack|low_latency|fastopen|ecn|ecn_fallback|syncookies|max_syn_backlog|tw_reuse|fin_timeout|keepalive_time|keepalive_probes|keepalive_intvl|thp_linear_timeouts|pacing|pacing_ss_ratio|pacing_ca_ratio|no_ssthresh_metrics_save|md5sig|abort_on_overflow|buffer_split)'
net.ipv4.tcp_abort_on_overflow = 0
net.ipv4.tcp_available_congestion_control = reno cubic bbr
net.ipv4.tcp_congestion_control = bbr
net.ipv4.tcp_ecn = 2
net.ipv4.tcp_ecn_fallback = 1
net.ipv4.tcp_fastopen = 1
net.ipv4.tcp_fastopen_blackhole_timeout_sec = 0
net.ipv4.tcp_fastopen_key = 00000000-00000000-00000000-00000000
net.ipv4.tcp_fin_timeout = 60
net.ipv4.tcp_keepalive_intvl = 75
net.ipv4.tcp_keepalive_probes = 9
net.ipv4.tcp_keepalive_time = 7200
net.ipv4.tcp_low_latency = 0
net.ipv4.tcp_max_syn_backlog = 1024
net.ipv4.tcp_mtu_probing = 0
net.ipv4.tcp_no_metrics_save = 0
net.ipv4.tcp_no_ssthresh_metrics_save = 1
net.ipv4.tcp_pacing_ca_ratio = 120
net.ipv4.tcp_pacing_ss_ratio = 200
net.ipv4.tcp_rmem = 4096	87380	16777216
net.ipv4.tcp_sack = 1
net.ipv4.tcp_slow_start_after_idle = 1
net.ipv4.tcp_syncookies = 1
net.ipv4.tcp_timestamps = 1
net.ipv4.tcp_tw_reuse = 2
net.ipv4.tcp_tw_reuse_delay = 1000
net.ipv4.tcp_window_scaling = 1
net.ipv4.tcp_wmem = 4096	65536	16777216

--- other net.* sysctls
    $ sysctl -a 2>/dev/null | grep -E '^net\.(ipv4\.ip_(local_port_range|local_reserved_ports|no_pmtu_disc|forwarding)|ipv4\.conf\.all\.(rp_filter|accept_redirects|send_redirects)|ipv4\.conf\.default\.forwarding|core\.netdev_budget|ipv6\.conf\.all\.disable_ipv6)'
net.core.netdev_budget = 300
net.core.netdev_budget_usecs = 2000
net.ipv4.conf.all.accept_redirects = 1
net.ipv4.conf.all.rp_filter = 2
net.ipv4.conf.all.send_redirects = 1
net.ipv4.conf.default.forwarding = 0
net.ipv4.ip_local_port_range = 32768	60999
net.ipv4.ip_local_reserved_ports = 
net.ipv4.ip_no_pmtu_disc = 0
net.ipv6.conf.all.disable_ipv6 = 0

--- sysctl.d
total 12
drwxr-xr-x   2 root root 4096 Nov 18  2025 .
drwxr-xr-x 111 root root 4096 Jul 29 05:08 ..
-rw-r--r--   1 root root  269 Jul 30  2025 README.sysctl

--- /etc/sysctl.conf
    --- /etc/sysctl.conf ---

# pfv-tsys4 storage optimization
# VM tuning for storage server
vm.swappiness = 1
vm.vfs_cache_pressure = 50
vm.dirty_ratio = 40
vm.dirty_background_ratio = 10

# Network tuning for NFS
net.core.rmem_max = 16777216
net.core.wmem_max = 16777216
net.core.rmem_default = 262144
net.core.wmem_default = 262144
net.core.netdev_max_backlog = 5000
net.core.somaxconn = 1024

# TCP tuning
net.ipv4.tcp_rmem = 4096 87380 16777216
net.ipv4.tcp_wmem = 4096 65536 16777216
net.ipv4.tcp_congestion_control = bbr

# RPC/NFS tuning
sunrpc.tcp_max_slot_table_entries = 128
sunrpc.tcp_slot_table_entries = 128
sunrpc.udp_slot_table_entries = 128

# File handle cache
fs.file-max = 1000000

--- non-default sysctl values (sorted, filtered)
    $ # Show only sysctls that differ from running state vs an empty config;
# too noisy to dump all of /proc/sys. Just show /etc/sysctl.d content.
for f in /etc/sysctl.d/*.conf /etc/sysctl.conf; do
    [ -r "$f" ] || continue
    echo "=== $f ==="
    grep -vE '^\s*#|^\s*$' "$f" 2>/dev/null
done
=== /etc/sysctl.conf ===
vm.swappiness = 1
vm.vfs_cache_pressure = 50
vm.dirty_ratio = 40
vm.dirty_background_ratio = 10
net.core.rmem_max = 16777216
net.core.wmem_max = 16777216
net.core.rmem_default = 262144
net.core.wmem_default = 262144
net.core.netdev_max_backlog = 5000
net.core.somaxconn = 1024
net.ipv4.tcp_rmem = 4096 87380 16777216
net.ipv4.tcp_wmem = 4096 65536 16777216
net.ipv4.tcp_congestion_control = bbr
sunrpc.tcp_max_slot_table_entries = 128
sunrpc.tcp_slot_table_entries = 128
sunrpc.udp_slot_table_entries = 128
fs.file-max = 1000000

###############################################################################
# 8. tuned / irqbalance / udev
###############################################################################

--- tuned-adm active
    $ tuned-adm active
Current active profile: throughput-performance

--- tuned-adm list
    $ tuned-adm list
Available profiles:
- accelerator-performance     - Throughput performance based tuning with disabled higher latency STOP states
- atomic-guest                - Optimize virtual guests based on the Atomic variant
- atomic-host                 - Optimize bare metal systems running the Atomic variant
- aws                         - Optimize for aws ec2 instances
- balanced                    - General non-specialized tuned profile
- balanced-battery            - Balanced profile biased towards power savings changes for battery
- cpu-partitioning            - Optimize for CPU partitioning
- cpu-partitioning-powersave  - Optimize for CPU partitioning with additional powersave
- default                     - Legacy default tuned profile
- desktop                     - Optimize for the desktop use-case
- desktop-powersave           - Optmize for the desktop use-case with power saving
- enterprise-storage          - Legacy profile for RHEL6, for RHEL7, please use throughput-performance profile
- hpc-compute                 - Optimize for HPC compute workloads
- intel-sst                   - Configure for Intel Speed Select Base Frequency
- laptop-ac-powersave         - Optimize for laptop with power savings
- laptop-battery-powersave    - Optimize laptop profile with more aggressive power saving
- latency-performance         - Optimize for deterministic performance at the cost of increased power consumption
- mssql                       - Optimize for Microsoft SQL Server
- network-latency             - Optimize for deterministic performance at the cost of increased power consumption, focused on low latency network performance
- network-throughput          - Optimize for streaming network throughput, generally only necessary on older CPUs or 40G+ networks
- openshift                   - Optimize systems running OpenShift (parent profile)
- openshift-control-plane     - Optimize systems running OpenShift control plane
- openshift-node              - Optimize systems running OpenShift nodes
- optimize-serial-console     - Optimize for serial console use.
- oracle                      - Optimize for Oracle RDBMS
- postgresql                  - Optimize for PostgreSQL server
- powersave                   - Optimize for low power consumption
- realtime                    - Optimize for realtime workloads
- realtime-virtual-guest      - Optimize for realtime workloads running within a KVM guest
- realtime-virtual-host       - Optimize for KVM guests running realtime workloads
- sap-hana                    - Optimize for SAP HANA
- sap-hana-kvm-guest          - Optimize for running SAP HANA on KVM inside a virtual guest
- sap-netweaver               - Optimize for SAP NetWeaver
- server-powersave            - Optimize for server power savings
- spectrumscale-ece           - Optimized for Spectrum Scale Erasure Code Edition Servers
- spindown-disk               - Optimize for power saving by spinning-down rotational disks
- throughput-performance      - Broadly applicable tuning that provides excellent performance across a variety of common server workloads
- virtual-guest               - Optimize for running inside a virtual guest
- virtual-host                - Optimize for running KVM guests
Current active profile: throughput-performance

--- systemctl is-active tuned
    $ systemctl is-active tuned
active

--- irqbalance status
    $ systemctl is-active irqbalance
inactive
    [exit=4 / not installed or not permitted]

--- irqbalance config
    [missing: /etc/default/irqbalance]
    [missing: /etc/irqbalance.conf]

--- modprobe.d
total 24
drwxr-xr-x   2 root root 4096 Mar  6 10:31 .
drwxr-xr-x 111 root root 4096 Jul 29 05:08 ..
-rw-r--r--   1 root root  154 Oct 18  2025 intel-microcode-blacklist.conf
-rw-r--r--   1 root root  379 Mar  9  2025 mdadm.conf
-rw-r--r--   1 root root  172 Nov 18  2025 pve-blacklist.conf
-rw-r--r--   1 root root    0 Mar  6 10:32 tuned.conf
-rw-r--r--   1 root root   35 Feb 23 04:51 zfs.conf

--- udev rules.d
total 12
drwxr-xr-x 2 root root 4096 Jul 28 19:26 .
drwxr-xr-x 4 root root 4096 Nov 18  2025 ..
lrwxrwxrwx 1 root root    9 Feb 23 04:50 60-bridge-network-interface.rules -> /dev/null
-rw-r--r-- 1 root root 1468 Jul 28 19:42 99-console-ports.rules

--- modprobe.d files
    --- /etc/modprobe.d/intel-microcode-blacklist.conf ---
# The microcode module attempts to apply a microcode update when
# it autoloads.  This is not always safe, so we block it by default.
blacklist microcode
    --- /etc/modprobe.d/mdadm.conf ---
# mdadm module configuration file
# set start_ro=1 to make newly assembled arrays read-only initially,
# to prevent metadata writes.  This is needed in order to allow
# resume-from-disk to work - new boot should not perform writes
# because it will be done behind the back of the system being
# resumed.  See http://bugs.debian.org/415441 for details.

options md_mod start_ro=1
    --- /etc/modprobe.d/pve-blacklist.conf ---
# This file contains a list of modules which are not supported by Proxmox VE 

# nvidiafb see bugreport https://bugzilla.proxmox.com/show_bug.cgi?id=701
blacklist nvidiafb
    --- /etc/modprobe.d/tuned.conf ---
    --- /etc/modprobe.d/zfs.conf ---
options zfs zfs_arc_max=1667235840

--- module params: kvm_intel
    $ for p in /sys/module/kvm_intel/parameters/*; do
    [ -e "$p" ] && printf '  %s = %s\n' "$(basename "$p")" "$(cat "$p" 2>/dev/null)"
done
  allow_smaller_maxphyaddr = N
  dump_invalid_vmcs = N
  emulate_invalid_guest_state = Y
  enable_apicv = N
  enable_device_posted_irqs = N
  enable_ipiv = N
  enable_shadow_vmcs = Y
  enlightened_vmcs = N
  ept = Y
  eptad = Y
  error_on_inconsistent_vmcs_config = Y
  fasteoi = Y
  flexpriority = Y
  nested = Y
  nested_early_check = N
  ple_gap = 128
  ple_window = 4096
  ple_window_grow = 2
  ple_window_max = 4294967295
  ple_window_shrink = 0
  pml = N
  preemption_timer = Y
  sgx = N
  tdx = N
  unrestricted_guest = Y
  vmentry_l1d_flush = cond
  vnmi = Y
  vpid = Y

--- module params: kvm_amd
    $ for p in /sys/module/kvm_amd/parameters/*; do
    [ -e "$p" ] && printf '  %s = %s\n' "$(basename "$p")" "$(cat "$p" 2>/dev/null)"
done
    [exit=1]

--- module params: relevant net drivers
    $ for mod in i40e ixgbe mlx5_core igb ice bnx2x virtio_net; do
    [ -d "/sys/module/$mod/parameters" ] || continue
    echo "=== $mod ==="
    for p in /sys/module/$mod/parameters/*; do
        [ -e "$p" ] && printf '  %s = %s\n' "$(basename "$p")" "$(cat "$p" 2>/dev/null)"
    done
done
=== virtio_net ===
  csum = Y
  gso = Y
  napi_tx = Y
  napi_weight = 64

###############################################################################
# 9. PROXMOX VERSION & CLUSTER
###############################################################################

--- pveversion
    $ pveversion
pve-manager/9.1.5/80cf92a64bef6889 (running kernel: 6.17.9-1-pve)

--- pveversion -v
    $ pveversion -v
proxmox-ve: 9.1.0 (running kernel: 6.17.9-1-pve)
pve-manager: 9.1.5 (running version: 9.1.5/80cf92a64bef6889)
proxmox-kernel-helper: 9.0.4
proxmox-kernel-6.17.9-1-pve-signed: 6.17.9-1
proxmox-kernel-6.17: 6.17.9-1
proxmox-kernel-6.17.2-1-pve-signed: 6.17.2-1
ceph-fuse: 19.2.3-pve2
corosync: 3.1.9-pve2
criu: 4.1.1-1
frr-pythontools: 10.4.1-1+pve1
ifupdown2: 3.3.0-1+pmx12
intel-microcode: 3.20251111.1~deb13u1
ksm-control-daemon: 1.5-1
libjs-extjs: 7.0.0-5
libproxmox-acme-perl: 1.7.0
libproxmox-backup-qemu0: 2.0.2
libproxmox-rs-perl: 0.4.1
libpve-access-control: 9.0.5
libpve-apiclient-perl: 3.4.2
libpve-cluster-api-perl: 9.0.7
libpve-cluster-perl: 9.0.7
libpve-common-perl: 9.1.7
libpve-guest-common-perl: 6.0.2
libpve-http-server-perl: 6.0.5
libpve-network-perl: 1.2.5
libpve-rs-perl: 0.11.4
libpve-storage-perl: 9.1.0
libspice-server1: 0.15.2-1+b1
lvm2: 2.03.31-2+pmx1
lxc-pve: 6.0.5-4
lxcfs: 6.0.4-pve1
novnc-pve: 1.6.0-3
proxmox-backup-client: 4.1.2-1
proxmox-backup-file-restore: 4.1.2-1
proxmox-backup-restore-image: 1.0.0
proxmox-firewall: 1.2.1
proxmox-kernel-helper: 9.0.4
proxmox-mail-forward: 1.0.2
proxmox-mini-journalreader: 1.6
proxmox-offline-mirror-helper: 0.7.3
proxmox-widget-toolkit: 5.1.5
pve-cluster: 9.0.7
pve-container: 6.1.1
pve-docs: 9.1.2
pve-edk2-firmware: 4.2025.05-2
pve-esxi-import-tools: 1.0.1
pve-firewall: 6.0.4
pve-firmware: 3.17-2
pve-ha-manager: 5.1.0
pve-i18n: 3.6.6
pve-qemu-kvm: 10.1.2-6
pve-xtermjs: 5.5.0-3
qemu-server: 9.1.4
smartmontools: 7.4-pve1
spiceterm: 3.4.1
swtpm: 0.8.0+pve3
vncterm: 1.9.1
zfsutils-linux: 2.4.0-pve1

--- pvecm status
    $ pvecm status
Error: Corosync config '/etc/pve/corosync.conf' does not exist - is this node part of a cluster?
    [exit=2 / not installed or not permitted]

--- pvecm nodes
    $ pvecm nodes
Error: Corosync config '/etc/pve/corosync.conf' does not exist - is this node part of a cluster?
    [exit=2 / not installed or not permitted]

--- pvecm expected
    $ pvecm expected
400 not enough arguments
pvecm expected <expected>
    [exit=255 / not installed or not permitted]

--- pveperf
    $ timeout 15 pveperf
CPU BOGOMIPS:      55869.92
REGEX/SECOND:      4059031
HD SIZE:           93.93 GB (/dev/mapper/pve-root)
BUFFERED READS:    123.33 MB/sec
AVERAGE SEEK TIME: 37.61 ms
FSYNCS/SECOND:     14.16
    [exit=124 / not installed or not permitted]

--- corosync.conf
    [missing: /etc/pve/corosync.conf]

--- datacenter.cfg
    --- /etc/pve/datacenter.cfg ---
keyboard: en-us

--- storage.cfg
    --- /etc/pve/storage.cfg ---
dir: local
	path /var/lib/vz
	content iso,vztmpl,import,backup

lvmthin: local-lvm
	thinpool data
	vgname pve
	content rootdir,images

dir: D3
	path /mnt/tsys4/D3
	content images
	prune-backups keep-all=1
	shared 0


--- user.cfg
    --- /etc/pve/user.cfg ---
user:root@pam:1:0:::coo@turnsys.com::x:
token:root@pam!pdm-admin-tsys-proxmox-datacenter:0:0:auto-generated by PDM host 'tsys-proxmox-datacenter' on Mon, 23 Feb 2026 22%3A27%3A54 -0600:





--- domains.cfg
    [missing: /etc/pve/domains.cfg]

--- cluster resources (compact)
    $ pvesh get /cluster/resources --type node --output-format json 2>/dev/null \
  | jq -r '.[] | "\(.node)\tcpu=\(.cpu)\tmem=\(.mem)\tmaxmem=\(.maxmem)\tmaxdisk=\(.maxdisk)\tstatus=\(.status)\tssl_fingerprint=\(.ssl_fingerprint)"' 2>/dev/null \
  || pvesh get /cluster/resources --type node 2>/dev/null
┌────────────────┬──────┬─────────────┬─────────┬───────┬───────────┬──────────┬───────────┬─────────┬───────┬──────┬────────┬───────────┬───────────┬──────────┬─────────┬──────┬───────┬────────┬─────────┬──────────────┬───────────┬────────────┬──────┬──────────┬─────┬────────┬─────────┬──────┬──────────┬────────────┬──────┬───────────┐
│ id             │ type │ cgroup-mode │ content │   cpu │      disk │ diskread │ diskwrite │ hastate │ level │ lock │ maxcpu │   maxdisk │    maxmem │      mem │ memhost │ name │ netin │ netout │ network │ network-type │ node      │ plugintype │ pool │ protocol │ sdn │ status │ storage │ tags │ template │     uptime │ vmid │ zone-type │
╞════════════════╪══════╪═════════════╪═════════╪═══════╪═══════════╪══════════╪═══════════╪═════════╪═══════╪══════╪════════╪═══════════╪═══════════╪══════════╪═════════╪══════╪═══════╪════════╪═════════╪══════════════╪═══════════╪════════════╪══════╪══════════╪═════╪════════╪═════════╪══════╪══════════╪════════════╪══════╪═══════════╡
│ node/pfv-tsys4 │ node │           2 │         │ 1.31% │ 10.23 GiB │          │           │         │       │      │      8 │ 93.93 GiB │ 15.53 GiB │ 2.12 GiB │         │      │       │        │         │              │ pfv-tsys4 │            │      │          │     │ online │         │      │          │ 4d 13h 11m │      │           │
└────────────────┴──────┴─────────────┴─────────┴───────┴───────────┴──────────┴───────────┴─────────┴───────┴──────┴────────┴───────────┴───────────┴──────────┴─────────┴──────┴───────┴────────┴─────────┴──────────────┴───────────┴────────────┴──────┴──────────┴─────┴────────┴─────────┴──────┴──────────┴────────────┴──────┴───────────┘

###############################################################################
# 10. NETWORK: INTERFACES
###############################################################################

--- ip -d link
    $ ip -d link
1: lo: <LOOPBACK,UP,LOWER_UP> mtu 65536 qdisc noqueue state UNKNOWN mode DEFAULT group default qlen 1000
    link/loopback 00:00:00:00:00:00 brd 00:00:00:00:00:00 promiscuity 0 allmulti 0 minmtu 0 maxmtu 0 addrgenmode eui64 numtxqueues 1 numrxqueues 1 gso_max_size 65536 gso_max_segs 65535 tso_max_size 524280 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 
2: nic0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc fq_codel master vmbr0 state UP mode DEFAULT group default qlen 1000
    link/ether 98:90:96:c4:96:9a brd ff:ff:ff:ff:ff:ff promiscuity 1 allmulti 1 minmtu 68 maxmtu 9000 
    bridge_slave state forwarding priority 32 cost 5 hairpin off guard off root_block off fastleave off learning on flood on port_id 0x8001 port_no 0x1 designated_port 32769 designated_cost 0 designated_bridge 8000.98:90:96:c4:96:9a designated_root 8000.98:90:96:c4:96:9a hold_timer    0.00 message_age_timer    0.00 forward_delay_timer    0.00 topology_change_ack 0 config_pending 0 proxy_arp off proxy_arp_wifi off mcast_router 1 mcast_fast_leave off mcast_flood on bcast_flood on mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off group_fwd_mask 0 group_fwd_mask_str 0x0 vlan_tunnel off isolated off locked off mab off addrgenmode eui64 numtxqueues 1 numrxqueues 1 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 parentbus pci parentdev 0000:00:19.0 
    altname enp0s25
    altname enx989096c4969a
3: enx8cae4ccda926: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc fq_codel master datanet state UP mode DEFAULT group default qlen 1000
    link/ether 8c:ae:4c:cd:a9:26 brd ff:ff:ff:ff:ff:ff promiscuity 1 allmulti 1 minmtu 0 maxmtu 1500 
    bridge_slave state forwarding priority 32 cost 100 hairpin off guard off root_block off fastleave off learning on flood on port_id 0x8001 port_no 0x1 designated_port 32769 designated_cost 0 designated_bridge 8000.8c:ae:4c:cd:a9:26 designated_root 8000.8c:ae:4c:cd:a9:26 hold_timer    0.00 message_age_timer    0.00 forward_delay_timer    0.00 topology_change_ack 0 config_pending 0 proxy_arp off proxy_arp_wifi off mcast_router 1 mcast_fast_leave off mcast_flood on bcast_flood on mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off group_fwd_mask 0 group_fwd_mask_str 0x0 vlan_tunnel off isolated off locked off mab off addrgenmode eui64 numtxqueues 1 numrxqueues 1 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 parentbus usb parentdev 4-2.2:2.0 
4: enx80ae4ccdec03: <BROADCAST,MULTICAST> mtu 1500 qdisc noop state DOWN mode DEFAULT group default qlen 1000
    link/ether 80:ae:4c:cd:ec:03 brd ff:ff:ff:ff:ff:ff promiscuity 0 allmulti 0 minmtu 0 maxmtu 1500 addrgenmode eui64 numtxqueues 1 numrxqueues 1 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 parentbus usb parentdev 4-2.4:2.0 
5: tailscale0: <POINTOPOINT,MULTICAST,NOARP,UP,LOWER_UP> mtu 1280 qdisc fq_codel state UNKNOWN mode DEFAULT group default qlen 500
    link/none  promiscuity 0 allmulti 0 minmtu 68 maxmtu 65535 
    tun type tun pi off vnet_hdr on persist off addrgenmode random numtxqueues 1 numrxqueues 1 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 
6: vmbr0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000
    link/ether 98:90:96:c4:96:9a brd ff:ff:ff:ff:ff:ff promiscuity 0 allmulti 0 minmtu 68 maxmtu 65535 
    bridge forward_delay 0 hello_time 200 max_age 2000 ageing_time 30000 stp_state 0 priority 32768 vlan_filtering 0 vlan_protocol 802.1Q bridge_id 8000.98:90:96:c4:96:9a designated_root 8000.98:90:96:c4:96:9a root_port 0 root_path_cost 0 topology_change 0 topology_change_detected 0 hello_timer    0.00 tcn_timer    0.00 topology_change_timer    0.00 gc_timer    0.00 fdb_n_learned 103 fdb_max_learned 0 vlan_default_pvid 1 vlan_stats_enabled 0 vlan_stats_per_port 0 group_fwd_mask 0 group_address 01:80:c2:00:00:00 mcast_snooping 1 no_linklocal_learn 0 mcast_vlan_snooping 0 mst_enabled 0 mcast_router 1 mcast_query_use_ifaddr 0 mcast_querier 0 mcast_querier_ipv4_addr 0.0.0.0 mcast_querier_ipv4_port 2 mcast_querier_ipv4_other_timer 20us mcast_hash_elasticity 16 mcast_hash_max 4096 mcast_last_member_count 2 mcast_startup_query_count 2 mcast_last_member_interval 100 mcast_membership_interval 26000 mcast_querier_interval 25500 mcast_query_interval 12500 mcast_query_response_interval 1000 mcast_startup_query_interval 3125 mcast_stats_enabled 0 mcast_igmp_version 2 mcast_mld_version 1 nf_call_iptables 0 nf_call_ip6tables 0 nf_call_arptables 0 addrgenmode eui64 numtxqueues 1 numrxqueues 1 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 
7: datanet: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000
    link/ether 8c:ae:4c:cd:a9:26 brd ff:ff:ff:ff:ff:ff promiscuity 0 allmulti 0 minmtu 68 maxmtu 65535 
    bridge forward_delay 0 hello_time 200 max_age 2000 ageing_time 30000 stp_state 0 priority 32768 vlan_filtering 0 vlan_protocol 802.1Q bridge_id 8000.8c:ae:4c:cd:a9:26 designated_root 8000.8c:ae:4c:cd:a9:26 root_port 0 root_path_cost 0 topology_change 0 topology_change_detected 0 hello_timer    0.00 tcn_timer    0.00 topology_change_timer    0.00 gc_timer   30.21 fdb_n_learned 9 fdb_max_learned 0 vlan_default_pvid 1 vlan_stats_enabled 0 vlan_stats_per_port 0 group_fwd_mask 0 group_address 01:80:c2:00:00:00 mcast_snooping 1 no_linklocal_learn 0 mcast_vlan_snooping 0 mst_enabled 0 mcast_router 1 mcast_query_use_ifaddr 0 mcast_querier 0 mcast_hash_elasticity 16 mcast_hash_max 4096 mcast_last_member_count 2 mcast_startup_query_count 2 mcast_last_member_interval 100 mcast_membership_interval 26000 mcast_querier_interval 25500 mcast_query_interval 12500 mcast_query_response_interval 1000 mcast_startup_query_interval 3125 mcast_stats_enabled 0 mcast_igmp_version 2 mcast_mld_version 1 nf_call_iptables 0 nf_call_ip6tables 0 nf_call_arptables 0 addrgenmode eui64 numtxqueues 1 numrxqueues 1 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 
8: tap400i0: <BROADCAST,MULTICAST,PROMISC,UP,LOWER_UP> mtu 1500 qdisc fq_codel master fwbr400i0 state UNKNOWN mode DEFAULT group default qlen 1000
    link/ether 6e:59:53:32:e6:af brd ff:ff:ff:ff:ff:ff promiscuity 2 allmulti 1 minmtu 68 maxmtu 65521 
    tun type tap pi off vnet_hdr on persist off 
    bridge_slave state forwarding priority 32 cost 2 hairpin off guard off root_block off fastleave off learning on flood on port_id 0x8002 port_no 0x2 designated_port 32770 designated_cost 0 designated_bridge 8000.22:6f:ca:7c:50:23 designated_root 8000.22:6f:ca:7c:50:23 hold_timer    0.00 message_age_timer    0.00 forward_delay_timer    0.00 topology_change_ack 0 config_pending 0 proxy_arp off proxy_arp_wifi off mcast_router 1 mcast_fast_leave off mcast_flood on bcast_flood on mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off group_fwd_mask 0 group_fwd_mask_str 0x0 vlan_tunnel off isolated off locked off mab off addrgenmode eui64 numtxqueues 1 numrxqueues 1 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 
9: fwbr400i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000
    link/ether 22:6f:ca:7c:50:23 brd ff:ff:ff:ff:ff:ff promiscuity 0 allmulti 0 minmtu 68 maxmtu 65535 
    bridge forward_delay 0 hello_time 200 max_age 2000 ageing_time 30000 stp_state 0 priority 32768 vlan_filtering 0 vlan_protocol 802.1Q bridge_id 8000.22:6f:ca:7c:50:23 designated_root 8000.22:6f:ca:7c:50:23 root_port 0 root_path_cost 0 topology_change 0 topology_change_detected 0 hello_timer    0.00 tcn_timer    0.00 topology_change_timer    0.00 gc_timer   11.48 fdb_n_learned 78 fdb_max_learned 0 vlan_default_pvid 1 vlan_stats_enabled 0 vlan_stats_per_port 0 group_fwd_mask 0 group_address 01:80:c2:00:00:00 mcast_snooping 1 no_linklocal_learn 0 mcast_vlan_snooping 0 mst_enabled 0 mcast_router 1 mcast_query_use_ifaddr 0 mcast_querier 0 mcast_querier_ipv4_addr 0.0.0.0 mcast_querier_ipv4_port 11 mcast_querier_ipv4_other_timer 20us mcast_hash_elasticity 16 mcast_hash_max 4096 mcast_last_member_count 2 mcast_startup_query_count 2 mcast_last_member_interval 100 mcast_membership_interval 26000 mcast_querier_interval 25500 mcast_query_interval 12500 mcast_query_response_interval 1000 mcast_startup_query_interval 3125 mcast_stats_enabled 0 mcast_igmp_version 2 mcast_mld_version 1 nf_call_iptables 0 nf_call_ip6tables 0 nf_call_arptables 0 addrgenmode eui64 numtxqueues 1 numrxqueues 1 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 
10: fwpr400p0@fwln400i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master vmbr0 state UP mode DEFAULT group default qlen 1000
    link/ether 6e:fc:96:a6:43:f9 brd ff:ff:ff:ff:ff:ff promiscuity 1 allmulti 1 minmtu 68 maxmtu 65535 
    veth 
    bridge_slave state forwarding priority 32 cost 2 hairpin off guard off root_block off fastleave off learning on flood on port_id 0x8002 port_no 0x2 designated_port 32770 designated_cost 0 designated_bridge 8000.98:90:96:c4:96:9a designated_root 8000.98:90:96:c4:96:9a hold_timer    0.00 message_age_timer    0.00 forward_delay_timer    0.00 topology_change_ack 0 config_pending 0 proxy_arp off proxy_arp_wifi off mcast_router 1 mcast_fast_leave off mcast_flood on bcast_flood on mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off group_fwd_mask 0 group_fwd_mask_str 0x0 vlan_tunnel off isolated off locked off mab off addrgenmode eui64 numtxqueues 8 numrxqueues 8 gso_max_size 65536 gso_max_segs 65535 tso_max_size 524280 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 
11: fwln400i0@fwpr400p0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master fwbr400i0 state UP mode DEFAULT group default qlen 1000
    link/ether 22:6f:ca:7c:50:23 brd ff:ff:ff:ff:ff:ff promiscuity 1 allmulti 1 minmtu 68 maxmtu 65535 
    veth 
    bridge_slave state forwarding priority 32 cost 2 hairpin off guard off root_block off fastleave off learning on flood on port_id 0x8001 port_no 0x1 designated_port 32769 designated_cost 0 designated_bridge 8000.22:6f:ca:7c:50:23 designated_root 8000.22:6f:ca:7c:50:23 hold_timer    0.00 message_age_timer    0.00 forward_delay_timer    0.00 topology_change_ack 0 config_pending 0 proxy_arp off proxy_arp_wifi off mcast_router 1 mcast_fast_leave off mcast_flood on bcast_flood on mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off group_fwd_mask 0 group_fwd_mask_str 0x0 vlan_tunnel off isolated off locked off mab off addrgenmode eui64 numtxqueues 8 numrxqueues 8 gso_max_size 65536 gso_max_segs 65535 tso_max_size 524280 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 

--- ip -o link
    $ ip -o link
1: lo: <LOOPBACK,UP,LOWER_UP> mtu 65536 qdisc noqueue state UNKNOWN mode DEFAULT group default qlen 1000\    link/loopback 00:00:00:00:00:00 brd 00:00:00:00:00:00
2: nic0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc fq_codel master vmbr0 state UP mode DEFAULT group default qlen 1000\    link/ether 98:90:96:c4:96:9a brd ff:ff:ff:ff:ff:ff\    altname enp0s25\    altname enx989096c4969a
3: enx8cae4ccda926: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc fq_codel master datanet state UP mode DEFAULT group default qlen 1000\    link/ether 8c:ae:4c:cd:a9:26 brd ff:ff:ff:ff:ff:ff
4: enx80ae4ccdec03: <BROADCAST,MULTICAST> mtu 1500 qdisc noop state DOWN mode DEFAULT group default qlen 1000\    link/ether 80:ae:4c:cd:ec:03 brd ff:ff:ff:ff:ff:ff
5: tailscale0: <POINTOPOINT,MULTICAST,NOARP,UP,LOWER_UP> mtu 1280 qdisc fq_codel state UNKNOWN mode DEFAULT group default qlen 500\    link/none 
6: vmbr0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000\    link/ether 98:90:96:c4:96:9a brd ff:ff:ff:ff:ff:ff
7: datanet: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000\    link/ether 8c:ae:4c:cd:a9:26 brd ff:ff:ff:ff:ff:ff
8: tap400i0: <BROADCAST,MULTICAST,PROMISC,UP,LOWER_UP> mtu 1500 qdisc fq_codel master fwbr400i0 state UNKNOWN mode DEFAULT group default qlen 1000\    link/ether 6e:59:53:32:e6:af brd ff:ff:ff:ff:ff:ff
9: fwbr400i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000\    link/ether 22:6f:ca:7c:50:23 brd ff:ff:ff:ff:ff:ff
10: fwpr400p0@fwln400i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master vmbr0 state UP mode DEFAULT group default qlen 1000\    link/ether 6e:fc:96:a6:43:f9 brd ff:ff:ff:ff:ff:ff
11: fwln400i0@fwpr400p0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master fwbr400i0 state UP mode DEFAULT group default qlen 1000\    link/ether 22:6f:ca:7c:50:23 brd ff:ff:ff:ff:ff:ff

--- ip -o -4 addr
    $ ip -o -4 addr
1: lo    inet 127.0.0.1/8 scope host lo\       valid_lft forever preferred_lft forever
5: tailscale0    inet 100.70.77.93/32 scope global tailscale0\       valid_lft forever preferred_lft forever
6: vmbr0    inet 192.168.3.191/22 brd 192.168.3.255 scope global dynamic vmbr0\       valid_lft 500sec preferred_lft 500sec
7: datanet    inet 10.100.100.4/24 scope global datanet\       valid_lft forever preferred_lft forever

--- ip -o -6 addr (link-local filter)
    $ ip -o -6 addr
1: lo    inet6 ::1/128 scope host noprefixroute \       valid_lft forever preferred_lft forever
5: tailscale0    inet6 fd7a:115c:a1e0::3f3b:4d5d/128 scope global \       valid_lft forever preferred_lft forever
5: tailscale0    inet6 fe80::bcd2:a9d6:e5d0:8ba/64 scope link stable-privacy proto kernel_ll \       valid_lft forever preferred_lft forever
6: vmbr0    inet6 fe80::9a90:96ff:fec4:969a/64 scope link proto kernel_ll \       valid_lft forever preferred_lft forever
7: datanet    inet6 fe80::8eae:4cff:fecd:a926/64 scope link proto kernel_ll \       valid_lft forever preferred_lft forever

--- ip addr
    $ ip addr
1: lo: <LOOPBACK,UP,LOWER_UP> mtu 65536 qdisc noqueue state UNKNOWN group default qlen 1000
    link/loopback 00:00:00:00:00:00 brd 00:00:00:00:00:00
    inet 127.0.0.1/8 scope host lo
       valid_lft forever preferred_lft forever
    inet6 ::1/128 scope host noprefixroute 
       valid_lft forever preferred_lft forever
2: nic0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc fq_codel master vmbr0 state UP group default qlen 1000
    link/ether 98:90:96:c4:96:9a brd ff:ff:ff:ff:ff:ff
    altname enp0s25
    altname enx989096c4969a
3: enx8cae4ccda926: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc fq_codel master datanet state UP group default qlen 1000
    link/ether 8c:ae:4c:cd:a9:26 brd ff:ff:ff:ff:ff:ff
4: enx80ae4ccdec03: <BROADCAST,MULTICAST> mtu 1500 qdisc noop state DOWN group default qlen 1000
    link/ether 80:ae:4c:cd:ec:03 brd ff:ff:ff:ff:ff:ff
5: tailscale0: <POINTOPOINT,MULTICAST,NOARP,UP,LOWER_UP> mtu 1280 qdisc fq_codel state UNKNOWN group default qlen 500
    link/none 
    inet 100.70.77.93/32 scope global tailscale0
       valid_lft forever preferred_lft forever
    inet6 fd7a:115c:a1e0::3f3b:4d5d/128 scope global 
       valid_lft forever preferred_lft forever
    inet6 fe80::bcd2:a9d6:e5d0:8ba/64 scope link stable-privacy proto kernel_ll 
       valid_lft forever preferred_lft forever
6: vmbr0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP group default qlen 1000
    link/ether 98:90:96:c4:96:9a brd ff:ff:ff:ff:ff:ff
    inet 192.168.3.191/22 brd 192.168.3.255 scope global dynamic vmbr0
       valid_lft 500sec preferred_lft 500sec
    inet6 fe80::9a90:96ff:fec4:969a/64 scope link proto kernel_ll 
       valid_lft forever preferred_lft forever
7: datanet: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP group default qlen 1000
    link/ether 8c:ae:4c:cd:a9:26 brd ff:ff:ff:ff:ff:ff
    inet 10.100.100.4/24 scope global datanet
       valid_lft forever preferred_lft forever
    inet6 fe80::8eae:4cff:fecd:a926/64 scope link proto kernel_ll 
       valid_lft forever preferred_lft forever
8: tap400i0: <BROADCAST,MULTICAST,PROMISC,UP,LOWER_UP> mtu 1500 qdisc fq_codel master fwbr400i0 state UNKNOWN group default qlen 1000
    link/ether 6e:59:53:32:e6:af brd ff:ff:ff:ff:ff:ff
9: fwbr400i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP group default qlen 1000
    link/ether 22:6f:ca:7c:50:23 brd ff:ff:ff:ff:ff:ff
10: fwpr400p0@fwln400i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master vmbr0 state UP group default qlen 1000
    link/ether 6e:fc:96:a6:43:f9 brd ff:ff:ff:ff:ff:ff
11: fwln400i0@fwpr400p0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master fwbr400i0 state UP group default qlen 1000
    link/ether 22:6f:ca:7c:50:23 brd ff:ff:ff:ff:ff:ff

--- ip route
    $ ip route
default via 192.168.3.254 dev vmbr0 
10.100.100.0/24 dev datanet proto kernel scope link src 10.100.100.4 
192.168.0.0/22 dev vmbr0 proto kernel scope link src 192.168.3.191 

--- ip rule
    $ ip rule
0:	from all lookup local
5210:	from all fwmark 0x80000/0xff0000 lookup main
5230:	from all fwmark 0x80000/0xff0000 lookup default
5250:	from all fwmark 0x80000/0xff0000 unreachable
5270:	from all lookup 52
32766:	from all lookup main
32767:	from all lookup default

--- ip -s -s link (counters/errors)
    $ ip -s -s link
1: lo: <LOOPBACK,UP,LOWER_UP> mtu 65536 qdisc noqueue state UNKNOWN mode DEFAULT group default qlen 1000
    link/loopback 00:00:00:00:00:00 brd 00:00:00:00:00:00
    RX:  bytes packets errors dropped  missed   mcast           
       9928441   59588      0       0       0       0 
    RX errors:  length    crc   frame    fifo overrun
                     0      0       0       0       0 
    TX:  bytes packets errors dropped carrier collsns           
       9928441   59588      0       0       0       0 
    TX errors: aborted   fifo  window heartbt transns
                     0      0       0       0       0 
2: nic0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc fq_codel master vmbr0 state UP mode DEFAULT group default qlen 1000
    link/ether 98:90:96:c4:96:9a brd ff:ff:ff:ff:ff:ff
    RX:  bytes  packets errors dropped  missed   mcast           
    5479347044 20021845      0   13106       0 9680444 
    RX errors:   length    crc   frame    fifo overrun
                      0      0       0       0       0 
    TX:  bytes  packets errors dropped carrier collsns           
    4492576476  5447236      0       0       0       0 
    TX errors:  aborted   fifo  window heartbt transns
                      0      0       0       0       2 
    altname enp0s25
    altname enx989096c4969a
3: enx8cae4ccda926: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc fq_codel master datanet state UP mode DEFAULT group default qlen 1000
    link/ether 8c:ae:4c:cd:a9:26 brd ff:ff:ff:ff:ff:ff
    RX:    bytes   packets errors dropped  missed   mcast           
    470801677483 511367096      0   13104       0       0 
    RX errors:      length    crc   frame    fifo overrun
                         0      0       0       0       0 
    TX:    bytes   packets errors dropped carrier collsns           
    893465171139 693799520      0       6       0       0 
    TX errors:     aborted   fifo  window heartbt transns
                         0      0       0       0       2 
4: enx80ae4ccdec03: <BROADCAST,MULTICAST> mtu 1500 qdisc noop state DOWN mode DEFAULT group default qlen 1000
    link/ether 80:ae:4c:cd:ec:03 brd ff:ff:ff:ff:ff:ff
    RX:  bytes packets errors dropped  missed   mcast           
             0       0      0       0       0       0 
    RX errors:  length    crc   frame    fifo overrun
                     0      0       0       0       0 
    TX:  bytes packets errors dropped carrier collsns           
             0       0      0       0       0       0 
    TX errors: aborted   fifo  window heartbt transns
                     0      0       0       0       1 
5: tailscale0: <POINTOPOINT,MULTICAST,NOARP,UP,LOWER_UP> mtu 1280 qdisc fq_codel state UNKNOWN mode DEFAULT group default qlen 500
    link/none 
    RX:  bytes packets errors dropped  missed   mcast           
      28473988  243009      0       0       0       0 
    RX errors:  length    crc   frame    fifo overrun
                     0      0       0       0       0 
    TX:  bytes packets errors dropped carrier collsns           
     196913908  300933      0       0       0       0 
    TX errors: aborted   fifo  window heartbt transns
                     0      0       0       0       0 
6: vmbr0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000
    link/ether 98:90:96:c4:96:9a brd ff:ff:ff:ff:ff:ff
    RX:  bytes  packets errors dropped  missed   mcast           
    4129691188 14848391      0       0       0 8092801 
    RX errors:   length    crc   frame    fifo overrun
                      0      0       0       0       0 
    TX:  bytes  packets errors dropped carrier collsns           
    3984184084  1724240      0       0       0       0 
    TX errors:  aborted   fifo  window heartbt transns
                      0      0       0       0       2 
7: datanet: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000
    link/ether 8c:ae:4c:cd:a9:26 brd ff:ff:ff:ff:ff:ff
    RX:    bytes   packets errors dropped  missed   mcast           
    470796106321 511349528      0      15       0  328183 
    RX errors:      length    crc   frame    fifo overrun
                         0      0       0       0       0 
    TX:    bytes   packets errors dropped carrier collsns           
    893461840407 693786429      0       0       0       0 
    TX errors:     aborted   fifo  window heartbt transns
                         0      0       0       0       2 
8: tap400i0: <BROADCAST,MULTICAST,PROMISC,UP,LOWER_UP> mtu 1500 qdisc fq_codel master fwbr400i0 state UNKNOWN mode DEFAULT group default qlen 1000
    link/ether 6e:59:53:32:e6:af brd ff:ff:ff:ff:ff:ff
    RX:  bytes  packets errors dropped  missed   mcast           
     315378453  1188944      0       0       0       0 
    RX errors:   length    crc   frame    fifo overrun
                      0      0       0       0       0 
    TX:  bytes  packets errors dropped carrier collsns           
    1816815396 13922592      0    5168       0       0 
    TX errors:  aborted   fifo  window heartbt transns
                      0      0       0       0       0 
9: fwbr400i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000
    link/ether 22:6f:ca:7c:50:23 brd ff:ff:ff:ff:ff:ff
    RX:  bytes  packets errors dropped  missed   mcast           
    1093000652 11963056      0   15584       0 8091762 
    RX errors:   length    crc   frame    fifo overrun
                      0      0       0       0       0 
    TX:  bytes  packets errors dropped carrier collsns           
             0        0      0       0       0       0 
    TX errors:  aborted   fifo  window heartbt transns
                      0      0       0       0       2 
10: fwpr400p0@fwln400i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master vmbr0 state UP mode DEFAULT group default qlen 1000
    link/ether 6e:fc:96:a6:43:f9 brd ff:ff:ff:ff:ff:ff
    RX:  bytes  packets errors dropped  missed   mcast           
     318639606  1202041      0   13097       0       0 
    RX errors:   length    crc   frame    fifo overrun
                      0      0       0       0       0 
    TX:  bytes  packets errors dropped carrier collsns           
    1817340004 13927761      0       0       0       0 
    TX errors:  aborted   fifo  window heartbt transns
                      0      0       0       0       2 
11: fwln400i0@fwpr400p0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master fwbr400i0 state UP mode DEFAULT group default qlen 1000
    link/ether 22:6f:ca:7c:50:23 brd ff:ff:ff:ff:ff:ff
    RX:  bytes  packets errors dropped  missed   mcast           
    1817340004 13927761      0   13097       0       0 
    RX errors:   length    crc   frame    fifo overrun
                      0      0       0       0       0 
    TX:  bytes  packets errors dropped carrier collsns           
     318639606  1202041      0       0       0       0 
    TX errors:  aborted   fifo  window heartbt transns
                      0      0       0       0       2 

--- ip neigh
    $ ip neigh
10.100.100.6 dev datanet lladdr 00:21:9b:a2:7c:55 REACHABLE 
192.168.1.45 dev vmbr0 FAILED 
192.168.3.254 dev vmbr0 lladdr 6c:4b:b4:10:40:61 REACHABLE 
192.168.1.46 dev vmbr0 FAILED 
192.168.3.153 dev vmbr0 lladdr c6:39:21:93:cd:e5 STALE 
10.100.100.5 dev datanet lladdr 00:1b:78:5c:e9:ce REACHABLE 
192.168.3.169 dev vmbr0 lladdr 00:21:9b:a2:7c:53 STALE 
192.168.3.99 dev vmbr0 lladdr 00:a0:de:a2:81:87 REACHABLE 
192.168.1.47 dev vmbr0 FAILED 
192.168.0.20 dev vmbr0 lladdr 18:03:73:43:ce:de STALE 
192.168.0.21 dev vmbr0 lladdr ca:fe:0f:0e:b0:75 REACHABLE 
10.100.100.3 dev datanet lladdr 8c:ae:4c:cd:a7:74 REACHABLE 
192.168.3.78 dev vmbr0 lladdr bc:24:11:1a:8f:6f REACHABLE 
192.168.1.164 dev vmbr0 FAILED 
192.168.2.44 dev vmbr0 lladdr bc:24:11:e6:03:2d REACHABLE 
192.168.2.5 dev vmbr0 lladdr a4:4c:c8:08:d1:b8 STALE 
192.168.3.55 dev vmbr0 lladdr 54:e4:bd:d3:da:78 STALE 
192.168.3.16 dev vmbr0 lladdr bc:24:11:8a:69:04 STALE 
192.168.1.119 dev vmbr0 lladdr 68:db:f5:1c:e8:8f STALE 
192.168.3.32 dev vmbr0 lladdr a0:4a:5e:ca:46:f3 STALE 
192.168.3.250 dev vmbr0 lladdr 00:15:5d:64:e8:1e REACHABLE 
192.168.1.166 dev vmbr0 lladdr 00:00:c0:34:0c:dc REACHABLE 
10.100.100.1 dev datanet lladdr 8c:ae:4c:cd:a6:2d REACHABLE 
10.100.100.9 dev datanet lladdr 9c:69:d3:6a:5b:6c REACHABLE 
192.168.3.173 dev vmbr0 lladdr 96:86:dd:1b:81:5a STALE 
192.168.3.11 dev vmbr0 lladdr 34:17:eb:b3:b1:2d STALE 
192.168.0.1 dev vmbr0 lladdr a0:d0:dc:38:3b:41 STALE 
192.168.0.250 dev vmbr0 lladdr f8:bc:12:34:e0:74 STALE 
10.100.100.7 dev datanet lladdr f8:bc:12:34:e0:75 REACHABLE 
192.168.3.12 dev vmbr0 lladdr 02:5a:39:38:3e:9f STALE 
fe80::44ce:70d5:12e2:dc57 dev vmbr0 lladdr bc:24:11:1e:fe:57 STALE 
fe80::afa2:9f93:a83a:8815 dev vmbr0 lladdr bc:24:11:eb:f0:0f STALE 
fe80::436f:cf31:df06:ba90 dev vmbr0 lladdr bc:24:11:5e:dc:44 STALE 
fe80::966:b4b8:282d:dff8 dev vmbr0 lladdr bc:24:11:27:4f:1c STALE 
fe80::1041:575c:79d7:c3f3 dev vmbr0 lladdr c6:39:21:93:cd:e5 STALE 
fe80::be24:11ff:fea3:8761 dev vmbr0 lladdr bc:24:11:a3:87:61 STALE 
fe80::be24:11ff:febb:6af dev vmbr0 lladdr bc:24:11:bb:06:af STALE 
fe80::ab9a:119e:e167:cc2a dev vmbr0 lladdr 96:86:dd:1b:81:5a STALE 
fe80::be24:11ff:fe9e:1ce9 dev vmbr0 lladdr bc:24:11:9e:1c:e9 STALE 
fe80::fabc:12ff:fe34:e075 dev datanet lladdr f8:bc:12:34:e0:75 STALE 
fe80::eb49:b5fa:c882:b02c dev vmbr0 lladdr bc:24:11:ee:7e:7b STALE 
fe80::c0e:c2d8:9069:af43 dev vmbr0 lladdr 5a:cc:23:39:ec:f7 STALE 
fe80::562b:57ff:fe4b:7c72 dev vmbr0 lladdr 54:2b:57:4b:7c:72 STALE 
fe80::ec58:8902:551a:c823 dev vmbr0 lladdr bc:24:11:1e:61:cf STALE 
fe80::4924:f822:d560:bc2f dev vmbr0 lladdr bc:24:11:f6:74:e8 STALE 
fe80::5ee7:53ff:fead:95c dev vmbr0 lladdr 5c:e7:53:ad:09:5c STALE 
fe80::36bd:c8ff:fe2d:18c5 dev vmbr0 lladdr 34:bd:c8:2d:18:c5 STALE 
fe80::54e4:4111:b359:b994 dev vmbr0 lladdr 96:86:dd:1b:81:5a STALE 
fe80::907a:3764:9b08:16f3 dev vmbr0 lladdr bc:24:11:94:71:07 STALE 
fe80::bb7f:ace0:50d5:690b dev vmbr0 lladdr bc:24:11:40:25:f8 STALE 
fe80::7f67:9446:ea86:eb01 dev vmbr0 lladdr 68:ec:8a:0e:36:69 router STALE 
fe80::21b:78ff:fe5c:e9ce dev datanet lladdr 00:1b:78:5c:e9:ce STALE 
fe80::54f2:477f:64f3:562c dev vmbr0 lladdr bc:24:11:5c:96:1e STALE 
fe80::be24:11ff:feeb:f00f dev vmbr0 lladdr bc:24:11:eb:f0:0f STALE 
fe80::5ee7:53ff:fecf:45fa dev vmbr0 lladdr 5c:e7:53:cf:45:fa STALE 
fe80::2053:681c:dbc9:6350 dev vmbr0 lladdr bc:24:11:ee:08:c9 STALE 
fe80::4542:2d1f:b470:fc54 dev vmbr0 lladdr bc:24:11:fb:7d:38 STALE 
fe80::be24:11ff:fecb:f7aa dev vmbr0 lladdr bc:24:11:cb:f7:aa STALE 
fe80::b6f4:eaa:36af:1d47 dev vmbr0 lladdr f0:6e:0b:cf:c7:55 STALE 
fe80::10e8:fff4:c9c7:c57b dev vmbr0 lladdr ba:71:00:a6:a3:12 STALE 
fe80::be5d:167b:45a7:5d73 dev vmbr0 lladdr bc:24:11:96:f7:b9 STALE 
fe80::be24:11ff:fe6e:1269 dev vmbr0 lladdr bc:24:11:6e:12:69 STALE 
fe80::ac15:1b59:37bb:96f5 dev vmbr0 lladdr 9c:6b:00:9d:1c:48 STALE 
fe80::a311:54:4085:c6b8 dev vmbr0 lladdr bc:24:11:32:d0:36 STALE 
fe80::8d8c:54c7:7a35:50a5 dev vmbr0 lladdr 2c:54:91:2a:0d:59 STALE 
fe80::844:b84d:703c:46b6 dev vmbr0 lladdr 44:09:da:4e:84:63 STALE 
fe80::6bea:ca7:4c8c:182f dev vmbr0 lladdr bc:24:11:80:0d:16 STALE 
fe80::be24:11ff:fedd:29b8 dev vmbr0 lladdr bc:24:11:dd:29:b8 STALE 
fe80::df77:368f:7483:f207 dev vmbr0 lladdr 96:86:dd:1b:81:5a STALE 
fe80::238a:7296:ce20:940f dev vmbr0 lladdr bc:24:11:8a:69:04 STALE 
fe80::be24:11ff:fe74:d68a dev vmbr0 lladdr bc:24:11:74:d6:8a STALE 
fe80::466:5100:c752:a95d dev vmbr0 lladdr ca:c3:35:a4:7f:c4 STALE 
fe80::be24:11ff:fec3:dc75 dev vmbr0 lladdr bc:24:11:c3:dc:75 STALE 
fe80::be24:11ff:fe65:b2ac dev vmbr0 lladdr bc:24:11:65:b2:ac STALE 
fe80::be24:11ff:fec7:1171 dev vmbr0 lladdr bc:24:11:c7:11:71 STALE 
fe80::31a5:b7f8:2ff3:6959 dev vmbr0 lladdr 2c:54:91:2a:0d:59 STALE 
fe80::eae9:e541:ea1f:9987 dev vmbr0 lladdr 9c:c8:e9:63:4b:95 STALE 
fe80::cfc5:646d:62cd:4746 dev vmbr0 lladdr bc:24:11:6f:b0:06 STALE 
fe80::1d:8fb:68fc:746 dev vmbr0 lladdr 74:29:59:27:3a:b7 STALE 
fe80::7172:40ba:b966:69df dev vmbr0 lladdr 2c:54:91:2a:0d:5b STALE 
fe80::2e8d:48ff:fe22:31c dev vmbr0 lladdr 2c:8d:48:22:03:1c STALE 
fe80::ae76:5582:7949:6783 dev vmbr0 lladdr 2c:54:91:2a:0d:5b STALE 
fe80::be24:11ff:feee:2bb6 dev vmbr0 lladdr bc:24:11:ee:2b:b6 STALE 
fe80::be24:11ff:fef6:74e8 dev vmbr0 lladdr bc:24:11:f6:74:e8 STALE 
fe80::e11b:a5d6:370a:3839 dev vmbr0 lladdr bc:24:11:80:a1:3c STALE 
fe80::6ae7:a88a:4305:7761 dev vmbr0 lladdr e8:4e:06:af:b8:92 STALE 
fe80::109b:d06f:f2be:1dc4 dev vmbr0 lladdr 16:bc:55:38:d3:7f STALE 
fe80::8175:8cd5:2119:c58c dev vmbr0 lladdr bc:24:11:e2:1a:09 STALE 
fe80::b40f:d2ff:fe8b:6aec dev vmbr0 lladdr b6:0f:d2:8b:6a:ec STALE 
fe80::406a:9d5b:52e1:a762 dev vmbr0 lladdr bc:24:11:65:b2:ac STALE 
fe80::be24:11ff:feee:67e2 dev vmbr0 lladdr bc:24:11:ee:67:e2 STALE 
fe80::6e4b:b4ff:fe10:4061 dev vmbr0 lladdr 6c:4b:b4:10:40:61 router STALE 
fe80::1175:ecfd:44b2:57cb dev vmbr0 lladdr bc:24:11:38:c0:58 STALE 
fe80::be24:11ff:fe1a:8f6f dev vmbr0 lladdr bc:24:11:1a:8f:6f STALE 
fe80::aaba:ff4f:993a:3336 dev vmbr0 lladdr bc:24:11:36:16:3c STALE 
fe80::be24:11ff:fe86:ea1a dev vmbr0 lladdr bc:24:11:86:ea:1a STALE 
fe80::ef5a:24f4:f260:2b1e dev vmbr0 lladdr bc:24:11:44:73:92 STALE 
fe80::2f96:e883:f0b8:8de1 dev vmbr0 lladdr bc:24:11:78:11:ac STALE 
fe80::86b:90fc:88ab:7eee dev vmbr0 lladdr 2a:cc:df:57:21:d2 STALE 
fe80::af8e:5170:c28:5a12 dev vmbr0 lladdr bc:24:11:ca:b0:cd STALE 
fe80::be24:11ff:fe1f:9d83 dev vmbr0 lladdr bc:24:11:1f:9d:83 STALE 
fe80::30b4:e59a:dbc:6700 dev vmbr0 lladdr bc:24:11:e4:37:53 STALE 
fe80::be24:11ff:fee6:32d dev vmbr0 lladdr bc:24:11:e6:03:2d STALE 
fe80::571e:6df3:f3d6:ad57 dev vmbr0 lladdr bc:24:11:6d:60:fb STALE 
fe80::be24:11ff:fee4:3753 dev vmbr0 lladdr bc:24:11:e4:37:53 STALE 
fe80::11be:70aa:7f52:bcc4 dev vmbr0 lladdr bc:24:11:7a:44:5f STALE 
fe80::65f9:f271:9449:32fc dev vmbr0 lladdr bc:24:11:2e:5a:d6 STALE 

--- /proc/net/dev (counters)
    $ cat /proc/net/dev
Inter-|   Receive                                                |  Transmit
 face |bytes    packets errs drop fifo frame compressed multicast|bytes    packets errs drop fifo colls carrier compressed
    lo: 9928441   59588    0    0    0     0          0         0  9928441   59588    0    0    0     0       0          0
  nic0: 5479347044 20021845    0 13106    0     0          0   9680444 4492576476 5447236    0    0    0     0       0          0
enx8cae4ccda926: 470801681947 511367099    0 13104    0     0          0         0 893465171379 693799522    0    6    0     0       0          0
enx80ae4ccdec03:       0       0    0    0    0     0          0         0        0       0    0    0    0     0       0          0
tailscale0: 28473988  243009    0    0    0     0          0         0 196913908  300933    0    0    0     0       0          0
 vmbr0: 4129691188 14848391    0    0    0     0          0   8092801 3984184084 1724240    0    0    0     0       0          0
datanet: 470796110785 511349531    0   15    0     0          0    328183 893461840473 693786430    0    0    0     0       0          0
tap400i0: 315378453 1188944    0    0    0     0          0         0 1816815396 13922592    0 5168    0     0       0          0
fwbr400i0: 1093000652 11963056    0 15584    0     0          0   8091762        0       0    0    0    0     0       0          0
fwpr400p0: 318639606 1202041    0 13097    0     0          0         0 1817340004 13927761    0    0    0     0       0          0
fwln400i0: 1817340004 13927761    0 13097    0     0          0         0 318639606 1202041    0    0    0     0       0          0

--- ip -6 route (brief)
    $ ip -6 route
fd7a:115c:a1e0::3f3b:4d5d dev tailscale0 proto kernel metric 256 pref medium
fe80::/64 dev tailscale0 proto kernel metric 256 pref medium
fe80::/64 dev vmbr0 proto kernel metric 256 pref medium
fe80::/64 dev datanet proto kernel metric 256 pref medium

--- sysfs interface attributes
    $ for ifc in $NETIFS; do
    d="/sys/class/net/$ifc"
    [ -d "$d" ] || continue
    printf '%-16s speed=%-8s duplex=%-8s mtu=%-6s carrier=%-3s tx_queue_len=%-5s qlen=%-5s type=%s\n' \
        "$ifc" \
        "$(cat "$d/speed" 2>/dev/null)" \
        "$(cat "$d/duplex" 2>/dev/null)" \
        "$(cat "$d/mtu" 2>/dev/null)" \
        "$(cat "$d/carrier" 2>/dev/null)" \
        "$(cat "$d/tx_queue_len" 2>/dev/null)" \
        "$(cat "$d/tx_queue_len" 2>/dev/null)" \
        "$(cat "$d/type" 2>/dev/null)"
done
datanet          speed=0        duplex=unknown  mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
enx80ae4ccdec03  speed=         duplex=         mtu=1500   carrier=    tx_queue_len=1000  qlen=1000  type=1
enx8cae4ccda926  speed=0        duplex=unknown  mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
fwbr400i0        speed=10000    duplex=unknown  mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
fwln400i0        speed=10000    duplex=full     mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
fwpr400p0        speed=10000    duplex=full     mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
nic0             speed=1000     duplex=full     mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
tap400i0         speed=10000    duplex=full     mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
vmbr0            speed=10000    duplex=unknown  mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1

--- ethtool per-interface deep dump
    $ for ifc in $NETIFS; do
    [ -e "/sys/class/net/$ifc" ] || continue
    echo ""
    echo "----- ethtool: $ifc -----"
    echo "[driver/version/firmware/bus-info -i]"
    ethtool -i "$ifc" 2>&1
    echo "[settings - speed/duplex/autoneg/port]"
    ethtool "$ifc" 2>&1
    echo "[channels -l (RX/TX/combined queue counts)]"
    ethtool -l "$ifc" 2>&1
    echo "[coalesce -c (interrupt moderation)]"
    ethtool -c "$ifc" 2>&1
    echo "[ring -g (descriptor counts)]"
    ethtool -g "$ifc" 2>&1
    echo "[pause / flow-control -a]"
    ethtool -a "$ifc" 2>&1
    echo "[offload features -k]"
    ethtool -k "$ifc" 2>&1
    echo "[private flags --show-priv-flags]"
    ethtool --show-priv-flags "$ifc" 2>&1
    echo "[ntuple/RSS -n]"
    ethtool -n "$ifc" 2>&1 | head -n 40
    echo "[SFP/DOM transceiver -m]"
    ethtool -m "$ifc" 2>&1
    echo "[statistics -S (key error/drop counters only)]"
    ethtool -S "$ifc" 2>/dev/null \
        | grep -iE 'drop|discard|error|crc|miss|pause|fifo|no_buff|rx_no_|_err|fw_|_bad|oversiz|undersize|frag|jabber|length_err|alignment' \
        | head -n 60
    echo "[statistics -S (throughput counters)]"
    ethtool -S "$ifc" 2>/dev/null \
        | grep -iE 'rx_(octets|bytes|packets)|tx_(octets|bytes|packets)|rx_(unicast|multicast|broadcast)|tx_(unicast|multicast|broadcast)' \
        | head -n 30
done

----- ethtool: datanet -----
[driver/version/firmware/bus-info -i]
driver: bridge
version: 2.3
firmware-version: N/A
expansion-rom-version: 
bus-info: N/A
supports-statistics: no
supports-test: no
supports-eeprom-access: no
supports-register-dump: no
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for datanet:
	Supported ports: [  ]
	Supported link modes:   Not reported
	Supported pause frame use: No
	Supports auto-negotiation: No
	Supported FEC modes: Not reported
	Advertised link modes:  Not reported
	Advertised pause frame use: No
	Advertised auto-negotiation: No
	Advertised FEC modes: Not reported
	Speed: Unknown!
	Duplex: Unknown! (255)
	Auto-negotiation: off
	Port: Other
	PHYAD: 0
	Transceiver: internal
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
netlink error: Operation not supported
[coalesce -c (interrupt moderation)]
netlink error: Operation not supported
[ring -g (descriptor counts)]
netlink error: Operation not supported
[pause / flow-control -a]
netlink error: Operation not supported
[offload features -k]
Features for datanet:
rx-checksumming: off [fixed]
tx-checksumming: on
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: on
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: off [fixed]
scatter-gather: off
	tx-scatter-gather: off [requested on]
	tx-scatter-gather-fraglist: off [requested on]
tcp-segmentation-offload: off
	tx-tcp-segmentation: off [requested on]
	tx-tcp-ecn-segmentation: off [requested on]
	tx-tcp-mangleid-segmentation: off [requested on]
	tx-tcp6-segmentation: off [requested on]
	tx-tcp-accecn-segmentation: off [requested on]
generic-segmentation-offload: off [requested on]
generic-receive-offload: on
large-receive-offload: off [fixed]
rx-vlan-offload: off [fixed]
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: off [fixed]
highdma: off [requested on]
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [requested on]
tx-fcoe-segmentation: off [requested on]
tx-gre-segmentation: on
tx-gre-csum-segmentation: on
tx-ipxip4-segmentation: on
tx-ipxip6-segmentation: on
tx-udp_tnl-segmentation: on
tx-udp_tnl-csum-segmentation: on
tx-gso-partial: on
tx-tunnel-remcsum-segmentation: on
tx-sctp-segmentation: off [requested on]
tx-esp-segmentation: on
tx-udp-segmentation: off [requested on]
tx-gso-list: off [requested on]
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: on
rx-vlan-stag-hw-parse: off [fixed]
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
[statistics -S (throughput counters)]

----- ethtool: enx80ae4ccdec03 -----
[driver/version/firmware/bus-info -i]
driver: cdc_ncm
version: 6.17.9-1-pve
firmware-version: CDC NCM (NO ZLP)
expansion-rom-version: 
bus-info: usb-0000:00:14.0-2.4
supports-statistics: yes
supports-test: no
supports-eeprom-access: no
supports-register-dump: no
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for enx80ae4ccdec03:
	Supported ports: [  ]
	Supported link modes:   Not reported
	Supported pause frame use: No
	Supports auto-negotiation: No
	Supported FEC modes: Not reported
	Advertised link modes:  Not reported
	Advertised pause frame use: No
	Advertised auto-negotiation: No
	Advertised FEC modes: Not reported
	Speed: Unknown!
	Duplex: Unknown! (255)
	Auto-negotiation: off
	Port: Twisted Pair
	PHYAD: 0
	Transceiver: internal
	MDI-X: Unknown
        Current message level: 0x00000007 (7)
                               drv probe link
	Link detected: no
[channels -l (RX/TX/combined queue counts)]
netlink error: Operation not supported
[coalesce -c (interrupt moderation)]
netlink error: Operation not supported
[ring -g (descriptor counts)]
netlink error: Operation not supported
[pause / flow-control -a]
netlink error: Operation not supported
[offload features -k]
Features for enx80ae4ccdec03:
rx-checksumming: off [fixed]
tx-checksumming: off
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: off [fixed]
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: off [fixed]
scatter-gather: off
	tx-scatter-gather: off [fixed]
	tx-scatter-gather-fraglist: off [fixed]
tcp-segmentation-offload: off
	tx-tcp-segmentation: off [fixed]
	tx-tcp-ecn-segmentation: off [fixed]
	tx-tcp-mangleid-segmentation: off [fixed]
	tx-tcp6-segmentation: off [fixed]
	tx-tcp-accecn-segmentation: off [fixed]
generic-segmentation-offload: off [requested on]
generic-receive-offload: on
large-receive-offload: off [fixed]
rx-vlan-offload: off [fixed]
tx-vlan-offload: off [fixed]
ntuple-filters: off [fixed]
receive-hashing: off [fixed]
highdma: off [fixed]
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [fixed]
tx-fcoe-segmentation: off [fixed]
tx-gre-segmentation: off [fixed]
tx-gre-csum-segmentation: off [fixed]
tx-ipxip4-segmentation: off [fixed]
tx-ipxip6-segmentation: off [fixed]
tx-udp_tnl-segmentation: off [fixed]
tx-udp_tnl-csum-segmentation: off [fixed]
tx-gso-partial: off [fixed]
tx-tunnel-remcsum-segmentation: off [fixed]
tx-sctp-segmentation: off [fixed]
tx-esp-segmentation: off [fixed]
tx-udp-segmentation: off [fixed]
tx-gso-list: off [fixed]
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: off [fixed]
rx-vlan-stag-hw-parse: off [fixed]
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
[statistics -S (throughput counters)]

----- ethtool: enx8cae4ccda926 -----
[driver/version/firmware/bus-info -i]
driver: cdc_ncm
version: 6.17.9-1-pve
firmware-version: CDC NCM (NO ZLP)
expansion-rom-version: 
bus-info: usb-0000:00:14.0-2.2
supports-statistics: yes
supports-test: no
supports-eeprom-access: no
supports-register-dump: no
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for enx8cae4ccda926:
	Supported ports: [  ]
	Supported link modes:   Not reported
	Supported pause frame use: No
	Supports auto-negotiation: No
	Supported FEC modes: Not reported
	Advertised link modes:  Not reported
	Advertised pause frame use: No
	Advertised auto-negotiation: No
	Advertised FEC modes: Not reported
	Speed: Unknown!
	Duplex: Unknown! (255)
	Auto-negotiation: off
	Port: Twisted Pair
	PHYAD: 0
	Transceiver: internal
	MDI-X: Unknown
        Current message level: 0x00000007 (7)
                               drv probe link
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
netlink error: Operation not supported
[coalesce -c (interrupt moderation)]
netlink error: Operation not supported
[ring -g (descriptor counts)]
netlink error: Operation not supported
[pause / flow-control -a]
netlink error: Operation not supported
[offload features -k]
Features for enx8cae4ccda926:
rx-checksumming: off [fixed]
tx-checksumming: off
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: off [fixed]
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: off [fixed]
scatter-gather: off
	tx-scatter-gather: off [fixed]
	tx-scatter-gather-fraglist: off [fixed]
tcp-segmentation-offload: off
	tx-tcp-segmentation: off [fixed]
	tx-tcp-ecn-segmentation: off [fixed]
	tx-tcp-mangleid-segmentation: off [fixed]
	tx-tcp6-segmentation: off [fixed]
	tx-tcp-accecn-segmentation: off [fixed]
generic-segmentation-offload: off [requested on]
generic-receive-offload: on
large-receive-offload: off [fixed]
rx-vlan-offload: off [fixed]
tx-vlan-offload: off [fixed]
ntuple-filters: off [fixed]
receive-hashing: off [fixed]
highdma: off [fixed]
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [fixed]
tx-fcoe-segmentation: off [fixed]
tx-gre-segmentation: off [fixed]
tx-gre-csum-segmentation: off [fixed]
tx-ipxip4-segmentation: off [fixed]
tx-ipxip6-segmentation: off [fixed]
tx-udp_tnl-segmentation: off [fixed]
tx-udp_tnl-csum-segmentation: off [fixed]
tx-gso-partial: off [fixed]
tx-tunnel-remcsum-segmentation: off [fixed]
tx-sctp-segmentation: off [fixed]
tx-esp-segmentation: off [fixed]
tx-udp-segmentation: off [fixed]
tx-gso-list: off [fixed]
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: off [fixed]
rx-vlan-stag-hw-parse: off [fixed]
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
[statistics -S (throughput counters)]

----- ethtool: fwbr400i0 -----
[driver/version/firmware/bus-info -i]
driver: bridge
version: 2.3
firmware-version: N/A
expansion-rom-version: 
bus-info: N/A
supports-statistics: no
supports-test: no
supports-eeprom-access: no
supports-register-dump: no
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for fwbr400i0:
	Supported ports: [  ]
	Supported link modes:   Not reported
	Supported pause frame use: No
	Supports auto-negotiation: No
	Supported FEC modes: Not reported
	Advertised link modes:  Not reported
	Advertised pause frame use: No
	Advertised auto-negotiation: No
	Advertised FEC modes: Not reported
	Speed: 10000Mb/s
	Duplex: Unknown! (255)
	Auto-negotiation: off
	Port: Other
	PHYAD: 0
	Transceiver: internal
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
netlink error: Operation not supported
[coalesce -c (interrupt moderation)]
netlink error: Operation not supported
[ring -g (descriptor counts)]
netlink error: Operation not supported
[pause / flow-control -a]
netlink error: Operation not supported
[offload features -k]
Features for fwbr400i0:
rx-checksumming: off [fixed]
tx-checksumming: on
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: on
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: off [fixed]
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: on
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: on
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: on
generic-segmentation-offload: on
generic-receive-offload: on
large-receive-offload: off [fixed]
rx-vlan-offload: off [fixed]
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: off [fixed]
highdma: on
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [requested on]
tx-fcoe-segmentation: off [requested on]
tx-gre-segmentation: on
tx-gre-csum-segmentation: on
tx-ipxip4-segmentation: on
tx-ipxip6-segmentation: on
tx-udp_tnl-segmentation: on
tx-udp_tnl-csum-segmentation: on
tx-gso-partial: on
tx-tunnel-remcsum-segmentation: on
tx-sctp-segmentation: on
tx-esp-segmentation: on
tx-udp-segmentation: on
tx-gso-list: on
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: on
rx-vlan-stag-hw-parse: off [fixed]
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
[statistics -S (throughput counters)]

----- ethtool: fwln400i0 -----
[driver/version/firmware/bus-info -i]
driver: veth
version: 1.0
firmware-version: 
expansion-rom-version: 
bus-info: 
supports-statistics: yes
supports-test: no
supports-eeprom-access: no
supports-register-dump: no
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for fwln400i0:
	Supported ports: [  ]
	Supported link modes:   Not reported
	Supported pause frame use: No
	Supports auto-negotiation: No
	Supported FEC modes: Not reported
	Advertised link modes:  Not reported
	Advertised pause frame use: No
	Advertised auto-negotiation: No
	Advertised FEC modes: Not reported
	Speed: 10000Mb/s
	Duplex: Full
	Auto-negotiation: off
	Port: Twisted Pair
	PHYAD: 0
	Transceiver: internal
	MDI-X: Unknown
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
Channel parameters for fwln400i0:
Pre-set maximums:
RX:		8
TX:		8
Other:		n/a
Combined:	n/a
Current hardware settings:
RX:		1
TX:		1
Other:		n/a
Combined:	n/a
[coalesce -c (interrupt moderation)]
netlink error: Operation not supported
[ring -g (descriptor counts)]
netlink error: Operation not supported
[pause / flow-control -a]
netlink error: Operation not supported
[offload features -k]
Features for fwln400i0:
rx-checksumming: on
tx-checksumming: on
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: on
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: on
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: on
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: on
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: on
generic-segmentation-offload: on
generic-receive-offload: off
large-receive-offload: off [fixed]
rx-vlan-offload: on
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: off [fixed]
highdma: on
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [fixed]
tx-fcoe-segmentation: off [fixed]
tx-gre-segmentation: on
tx-gre-csum-segmentation: on
tx-ipxip4-segmentation: on
tx-ipxip6-segmentation: on
tx-udp_tnl-segmentation: on
tx-udp_tnl-csum-segmentation: on
tx-gso-partial: off [fixed]
tx-tunnel-remcsum-segmentation: off [fixed]
tx-sctp-segmentation: on
tx-esp-segmentation: off [fixed]
tx-udp-segmentation: on
tx-gso-list: on
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: on
rx-vlan-stag-hw-parse: on
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
     rx_queue_0_drops: 0
     rx_queue_0_xdp_drops: 0
     rx_queue_0_xdp_tx_errors: 0
     tx_queue_0_xdp_xmit_errors: 0
[statistics -S (throughput counters)]

----- ethtool: fwpr400p0 -----
[driver/version/firmware/bus-info -i]
driver: veth
version: 1.0
firmware-version: 
expansion-rom-version: 
bus-info: 
supports-statistics: yes
supports-test: no
supports-eeprom-access: no
supports-register-dump: no
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for fwpr400p0:
	Supported ports: [  ]
	Supported link modes:   Not reported
	Supported pause frame use: No
	Supports auto-negotiation: No
	Supported FEC modes: Not reported
	Advertised link modes:  Not reported
	Advertised pause frame use: No
	Advertised auto-negotiation: No
	Advertised FEC modes: Not reported
	Speed: 10000Mb/s
	Duplex: Full
	Auto-negotiation: off
	Port: Twisted Pair
	PHYAD: 0
	Transceiver: internal
	MDI-X: Unknown
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
Channel parameters for fwpr400p0:
Pre-set maximums:
RX:		8
TX:		8
Other:		n/a
Combined:	n/a
Current hardware settings:
RX:		1
TX:		1
Other:		n/a
Combined:	n/a
[coalesce -c (interrupt moderation)]
netlink error: Operation not supported
[ring -g (descriptor counts)]
netlink error: Operation not supported
[pause / flow-control -a]
netlink error: Operation not supported
[offload features -k]
Features for fwpr400p0:
rx-checksumming: on
tx-checksumming: on
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: on
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: on
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: on
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: on
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: on
generic-segmentation-offload: on
generic-receive-offload: off
large-receive-offload: off [fixed]
rx-vlan-offload: on
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: off [fixed]
highdma: on
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [fixed]
tx-fcoe-segmentation: off [fixed]
tx-gre-segmentation: on
tx-gre-csum-segmentation: on
tx-ipxip4-segmentation: on
tx-ipxip6-segmentation: on
tx-udp_tnl-segmentation: on
tx-udp_tnl-csum-segmentation: on
tx-gso-partial: off [fixed]
tx-tunnel-remcsum-segmentation: off [fixed]
tx-sctp-segmentation: on
tx-esp-segmentation: off [fixed]
tx-udp-segmentation: on
tx-gso-list: on
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: on
rx-vlan-stag-hw-parse: on
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
     rx_queue_0_drops: 0
     rx_queue_0_xdp_drops: 0
     rx_queue_0_xdp_tx_errors: 0
     tx_queue_0_xdp_xmit_errors: 0
[statistics -S (throughput counters)]

----- ethtool: nic0 -----
[driver/version/firmware/bus-info -i]
driver: e1000e
version: 6.17.9-1-pve
firmware-version: 0.13-4
expansion-rom-version: 
bus-info: 0000:00:19.0
supports-statistics: yes
supports-test: yes
supports-eeprom-access: yes
supports-register-dump: yes
supports-priv-flags: yes
[settings - speed/duplex/autoneg/port]
Settings for nic0:
	Supported ports: [ TP ]
	Supported link modes:   10baseT/Half 10baseT/Full
	                        100baseT/Half 100baseT/Full
	                        1000baseT/Full
	Supported pause frame use: Symmetric Receive-only
	Supports auto-negotiation: Yes
	Supported FEC modes: Not reported
	Advertised link modes:  10baseT/Half 10baseT/Full
	                        100baseT/Half 100baseT/Full
	                        1000baseT/Full
	Advertised pause frame use: Symmetric Receive-only
	Advertised auto-negotiation: Yes
	Advertised FEC modes: Not reported
	Link partner advertised link modes:  10baseT/Half 10baseT/Full
	                                     100baseT/Half 100baseT/Full
	                                     1000baseT/Full
	Link partner advertised pause frame use: No
	Link partner advertised auto-negotiation: Yes
	Link partner advertised FEC modes: Not reported
	Speed: 1000Mb/s
	Duplex: Full
	Auto-negotiation: on
	Port: Twisted Pair
	PHYAD: 1
	Transceiver: internal
	MDI-X: on (auto)
	Supports Wake-on: pumbg
	Wake-on: g
        Current message level: 0x00000007 (7)
                               drv probe link
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
netlink error: Operation not supported
[coalesce -c (interrupt moderation)]
Coalesce parameters for nic0:
Adaptive RX: n/a  TX: n/a
stats-block-usecs:	n/a
sample-interval:	n/a
pkt-rate-low:		n/a
pkt-rate-high:		n/a

rx-usecs:	3
rx-frames:	n/a
rx-usecs-irq:	n/a
rx-frames-irq:	n/a

tx-usecs:	n/a
tx-frames:	n/a
tx-usecs-irq:	n/a
tx-frames-irq:	n/a

rx-usecs-low:	n/a
rx-frame-low:	n/a
tx-usecs-low:	n/a
tx-frame-low:	n/a

rx-usecs-high:	n/a
rx-frame-high:	n/a
tx-usecs-high:	n/a
tx-frame-high:	n/a

CQE mode RX: n/a  TX: n/a

tx-aggr-max-bytes:	n/a
tx-aggr-max-frames:	n/a
tx-aggr-time-usecs:	n/a

[ring -g (descriptor counts)]
Ring parameters for nic0:
Pre-set maximums:
RX:			4096
RX Mini:		n/a
RX Jumbo:		n/a
TX:			4096
TX push buff len:	n/a
Current hardware settings:
RX:			256
RX Mini:		n/a
RX Jumbo:		n/a
TX:			256
RX Buf Len:		n/a
CQE Size:		n/a
TX Push:		off
RX Push:		off
TX push buff len:	n/a
TCP data split:		n/a
[pause / flow-control -a]
Pause parameters for nic0:
Autonegotiate:	on
RX:		off
TX:		off
RX negotiated: off
TX negotiated: off

[offload features -k]
Features for nic0:
rx-checksumming: on
tx-checksumming: on
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: on
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: off [fixed]
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: off [fixed]
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: off [fixed]
	tx-tcp-mangleid-segmentation: off
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: off [fixed]
generic-segmentation-offload: on
generic-receive-offload: on
large-receive-offload: off [fixed]
rx-vlan-offload: on
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: on
highdma: on [fixed]
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [fixed]
tx-fcoe-segmentation: off [fixed]
tx-gre-segmentation: off [fixed]
tx-gre-csum-segmentation: off [fixed]
tx-ipxip4-segmentation: off [fixed]
tx-ipxip6-segmentation: off [fixed]
tx-udp_tnl-segmentation: off [fixed]
tx-udp_tnl-csum-segmentation: off [fixed]
tx-gso-partial: off [fixed]
tx-tunnel-remcsum-segmentation: off [fixed]
tx-sctp-segmentation: off [fixed]
tx-esp-segmentation: off [fixed]
tx-udp-segmentation: off [fixed]
tx-gso-list: off [fixed]
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off
rx-all: off
tx-vlan-stag-hw-insert: off [fixed]
rx-vlan-stag-hw-parse: off [fixed]
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
Private flags for nic0:
s0ix-enabled: off
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
     rx_errors: 0
     tx_errors: 0
     tx_dropped: 0
     rx_length_errors: 0
     rx_over_errors: 0
     rx_crc_errors: 0
     rx_frame_errors: 0
     rx_no_buffer_count: 0
     rx_missed_errors: 0
     tx_aborted_errors: 0
     tx_carrier_errors: 0
     tx_fifo_errors: 0
     tx_heartbeat_errors: 0
     tx_window_errors: 0
     rx_long_length_errors: 0
     rx_short_length_errors: 0
     rx_align_errors: 0
     rx_csum_offload_errors: 1
     dropped_smbus: 0
     uncorr_ecc_errors: 0
     corr_ecc_errors: 0
[statistics -S (throughput counters)]
     rx_packets: 20021849
     tx_packets: 5447237
     rx_bytes: 5479347546
     tx_bytes: 4492576646
     rx_broadcast: 3856835
     tx_broadcast: 14913
     rx_multicast: 9680444
     tx_multicast: 75328

----- ethtool: tap400i0 -----
[driver/version/firmware/bus-info -i]
driver: tun
version: 1.6
firmware-version: 
expansion-rom-version: 
bus-info: tap
supports-statistics: no
supports-test: no
supports-eeprom-access: no
supports-register-dump: no
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for tap400i0:
	Supported ports: [  ]
	Supported link modes:   Not reported
	Supported pause frame use: No
	Supports auto-negotiation: No
	Supported FEC modes: Not reported
	Advertised link modes:  Not reported
	Advertised pause frame use: No
	Advertised auto-negotiation: No
	Advertised FEC modes: Not reported
	Speed: 10000Mb/s
	Duplex: Full
	Auto-negotiation: off
	Port: Twisted Pair
	PHYAD: 0
	Transceiver: internal
	MDI-X: Unknown
        Current message level: 0x00000000 (0)
                              
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
Channel parameters for tap400i0:
Pre-set maximums:
RX:		n/a
TX:		n/a
Other:		n/a
Combined:	1
Current hardware settings:
RX:		n/a
TX:		n/a
Other:		n/a
Combined:	1
[coalesce -c (interrupt moderation)]
Coalesce parameters for tap400i0:
Adaptive RX: n/a  TX: n/a
stats-block-usecs:	n/a
sample-interval:	n/a
pkt-rate-low:		n/a
pkt-rate-high:		n/a

rx-usecs:	n/a
rx-frames:	0
rx-usecs-irq:	n/a
rx-frames-irq:	n/a

tx-usecs:	n/a
tx-frames:	n/a
tx-usecs-irq:	n/a
tx-frames-irq:	n/a

rx-usecs-low:	n/a
rx-frame-low:	n/a
tx-usecs-low:	n/a
tx-frame-low:	n/a

rx-usecs-high:	n/a
rx-frame-high:	n/a
tx-usecs-high:	n/a
tx-frame-high:	n/a

CQE mode RX: n/a  TX: n/a

tx-aggr-max-bytes:	n/a
tx-aggr-max-frames:	n/a
tx-aggr-time-usecs:	n/a

[ring -g (descriptor counts)]
netlink error: Operation not supported
[pause / flow-control -a]
netlink error: Operation not supported
[offload features -k]
Features for tap400i0:
rx-checksumming: off [fixed]
tx-checksumming: on
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: on
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: off [fixed]
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: on
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: off
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: off [fixed]
generic-segmentation-offload: on
generic-receive-offload: on
large-receive-offload: off [fixed]
rx-vlan-offload: off [fixed]
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: off [fixed]
highdma: off [fixed]
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [fixed]
tx-fcoe-segmentation: off [fixed]
tx-gre-segmentation: off [fixed]
tx-gre-csum-segmentation: off [fixed]
tx-ipxip4-segmentation: off [fixed]
tx-ipxip6-segmentation: off [fixed]
tx-udp_tnl-segmentation: off
tx-udp_tnl-csum-segmentation: off
tx-gso-partial: off [fixed]
tx-tunnel-remcsum-segmentation: off [fixed]
tx-sctp-segmentation: off [fixed]
tx-esp-segmentation: off [fixed]
tx-udp-segmentation: on
tx-gso-list: off [fixed]
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: on
rx-vlan-stag-hw-parse: off [fixed]
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
[statistics -S (throughput counters)]

----- ethtool: vmbr0 -----
[driver/version/firmware/bus-info -i]
driver: bridge
version: 2.3
firmware-version: N/A
expansion-rom-version: 
bus-info: N/A
supports-statistics: no
supports-test: no
supports-eeprom-access: no
supports-register-dump: no
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for vmbr0:
	Supported ports: [  ]
	Supported link modes:   Not reported
	Supported pause frame use: No
	Supports auto-negotiation: No
	Supported FEC modes: Not reported
	Advertised link modes:  Not reported
	Advertised pause frame use: No
	Advertised auto-negotiation: No
	Advertised FEC modes: Not reported
	Speed: 10000Mb/s
	Duplex: Unknown! (255)
	Auto-negotiation: off
	Port: Other
	PHYAD: 0
	Transceiver: internal
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
netlink error: Operation not supported
[coalesce -c (interrupt moderation)]
netlink error: Operation not supported
[ring -g (descriptor counts)]
netlink error: Operation not supported
[pause / flow-control -a]
netlink error: Operation not supported
[offload features -k]
Features for vmbr0:
rx-checksumming: off [fixed]
tx-checksumming: on
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: on
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: off [fixed]
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: on
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: on
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: on
generic-segmentation-offload: on
generic-receive-offload: on
large-receive-offload: off [fixed]
rx-vlan-offload: off [fixed]
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: off [fixed]
highdma: on
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [requested on]
tx-fcoe-segmentation: off [requested on]
tx-gre-segmentation: on
tx-gre-csum-segmentation: on
tx-ipxip4-segmentation: on
tx-ipxip6-segmentation: on
tx-udp_tnl-segmentation: on
tx-udp_tnl-csum-segmentation: on
tx-gso-partial: on
tx-tunnel-remcsum-segmentation: on
tx-sctp-segmentation: on
tx-esp-segmentation: on
tx-udp-segmentation: on
tx-gso-list: on
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: on
rx-vlan-stag-hw-parse: off [fixed]
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
[statistics -S (throughput counters)]

###############################################################################
# 11. NETWORK: BRIDGES / BONDS / VLANS
###############################################################################

--- bridge link
    $ bridge link
2: nic0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 master vmbr0 state forwarding priority 32 cost 5 
3: enx8cae4ccda926: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 master datanet state forwarding priority 32 cost 100 
8: tap400i0: <BROADCAST,MULTICAST,PROMISC,UP,LOWER_UP> mtu 1500 master fwbr400i0 state forwarding priority 32 cost 2 
10: fwpr400p0@fwln400i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 master vmbr0 state forwarding priority 32 cost 2 
11: fwln400i0@fwpr400p0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 master fwbr400i0 state forwarding priority 32 cost 2 

--- bridge -d link
    $ bridge -d link
2: nic0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 master vmbr0 state forwarding priority 32 cost 5 
    hairpin off guard off root_block off fastleave off learning on flood on mcast_flood on bcast_flood on mcast_router 1 mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off vlan_tunnel off isolated off locked off mab off mcast_n_groups 51 mcast_max_groups 0 
3: enx8cae4ccda926: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 master datanet state forwarding priority 32 cost 100 
    hairpin off guard off root_block off fastleave off learning on flood on mcast_flood on bcast_flood on mcast_router 1 mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off vlan_tunnel off isolated off locked off mab off mcast_n_groups 2 mcast_max_groups 0 
8: tap400i0: <BROADCAST,MULTICAST,PROMISC,UP,LOWER_UP> mtu 1500 master fwbr400i0 state forwarding priority 32 cost 2 
    hairpin off guard off root_block off fastleave off learning on flood on mcast_flood on bcast_flood on mcast_router 1 mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off vlan_tunnel off isolated off locked off mab off mcast_n_groups 0 mcast_max_groups 0 
10: fwpr400p0@fwln400i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 master vmbr0 state forwarding priority 32 cost 2 
    hairpin off guard off root_block off fastleave off learning on flood on mcast_flood on bcast_flood on mcast_router 1 mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off vlan_tunnel off isolated off locked off mab off mcast_n_groups 0 mcast_max_groups 0 
11: fwln400i0@fwpr400p0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 master fwbr400i0 state forwarding priority 32 cost 2 
    hairpin off guard off root_block off fastleave off learning on flood on mcast_flood on bcast_flood on mcast_router 1 mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off vlan_tunnel off isolated off locked off mab off mcast_n_groups 47 mcast_max_groups 0 

--- bridge vlan
    $ bridge vlan
port              vlan-id  
nic0              1 PVID Egress Untagged
enx8cae4ccda926   1 PVID Egress Untagged
vmbr0             1 PVID Egress Untagged
datanet           1 PVID Egress Untagged
tap400i0          1 PVID Egress Untagged
fwbr400i0         1 PVID Egress Untagged
fwpr400p0         1 PVID Egress Untagged
fwln400i0         1 PVID Egress Untagged

--- bridge vlan show
    $ bridge vlan show
port              vlan-id  
nic0              1 PVID Egress Untagged
enx8cae4ccda926   1 PVID Egress Untagged
vmbr0             1 PVID Egress Untagged
datanet           1 PVID Egress Untagged
tap400i0          1 PVID Egress Untagged
fwbr400i0         1 PVID Egress Untagged
fwpr400p0         1 PVID Egress Untagged
fwln400i0         1 PVID Egress Untagged

--- brctl show
    $ brctl show
bridge name	bridge id		STP enabled	interfaces
datanet		8000.8cae4ccda926	no		enx8cae4ccda926
fwbr400i0		8000.226fca7c5023	no		fwln400i0
							tap400i0
vmbr0		8000.989096c4969a	no		fwpr400p0
							nic0

--- bonding state
    [missing: /proc/net/bonding/bond*]

--- vlan config
    $ cat /proc/net/vlan/config
cat: /proc/net/vlan/config: No such file or directory
    [exit=1 / not installed or not permitted]

--- /proc/net/vlan
    [missing: /proc/net/vlan]

--- /etc/network/interfaces
    --- /etc/network/interfaces ---
auto lo
iface lo inet loopback


### mgmt net
iface nic0 inet manual


auto vmbr0
iface vmbr0 inet dhcp
	bridge-ports nic0
	bridge-stp off
	bridge-fd 0



### datanet

#auto enx8cae4ccda926 
#iface enx8cae4ccda926 inet manual
#	bond-master bond0

#auto enx80ae4ccdec03 
#iface enx80ae4ccdec03 inet manual
#	bond-master bond0

#auto bond0
#iface bond0 inet manual
#    bond-mode 802.3ad
#    bond-miimon 100
#    bond-downdelay 200
#    bond-updelay 200
#    bond-lacp-rate fast
#    bond-slaves enx8cae4ccda926 enx80ae4ccdec03 


auto datanet
iface datanet inet static
	address 10.100.100.4
	netmask 255.255.255.0
	bridge-ports enx8cae4ccda926
	bridge-stp off
	bridge-fd 0

source /etc/network/interfaces.d/*


--- interfaces.d (per file)
    $ for f in /etc/network/interfaces.d/*; do
    [ -r "$f" ] || continue
    echo "--- $f ---"
    cat "$f"
done

###############################################################################
# 12. NETWORK: IRQ / RPS / XPS / aRFS / SOFTNET
###############################################################################

--- /proc/interrupts
    $ cat /proc/interrupts
           CPU0       CPU1       CPU2       CPU3       CPU4       CPU5       CPU6       CPU7       
  0:         25          0          0          0          0          0          0          0 IR-IO-APIC   2-edge      timer
  8:          1          0          0          0          0          0          0          0 IR-IO-APIC   8-edge      rtc0
  9:          0      35073          0          0          0          0          0          0 IR-IO-APIC   9-fasteoi   acpi
 16:          0          0     578640          0          0          0          0          0 IR-IO-APIC  16-fasteoi   ehci_hcd:usb1
 18:          0          0          0          0      26140          0          0          0 IR-IO-APIC  18-fasteoi   i801_smbus
 19:          0          0          0          0          0          0          0   41665750 IR-IO-APIC  19-fasteoi   ata_piix
 23:          0          0          0         47          0          0          0          0 IR-IO-APIC  23-fasteoi   ehci_hcd:usb2
 24:          0          0          0          0          0          0          0          0 DMAR-MSI   0-edge      dmar0
 25:          0          0          0          0          0          0          0          0 DMAR-MSI   1-edge      dmar1
 26:          0          0          0          0          0          0          0          0 IR-PCI-MSI-0000:00:1c.0   0-edge      PCIe bwctrl
 27:          0          0          0          0          0          1          0          0 IR-PCI-MSI-0000:00:1c.1   0-edge      PCIe bwctrl
 28:          0          0          0          0          0          0          0          0 IR-PCI-MSI-0000:00:1c.4   0-edge      PCIe bwctrl
 29:          0   18604033          0          0          0          0          0          0 IR-PCI-MSI-0000:00:19.0   0-edge      nic0
 30:          0          0          0          0  263202542          0          0          0 IR-PCI-MSI-0000:00:14.0   0-edge      xhci_hcd
 38:          0          0          0          0          0         26          0          0 IR-PCI-MSI-0000:00:16.0   0-edge      mei_me
 39:          0          0          0          0          0          0     212662          0 IR-PCI-MSI-0000:00:02.0   0-edge      i915
 40:          0          0          0          0          0          0          0        256 IR-PCI-MSI-0000:00:03.0   0-edge      snd_hda_intel:card0
NMI:        534        523        411        463       1026        376        359        432   Non-maskable interrupts
LOC:   84189123  112915142   73966477   86436542  164915120   87504363   82346611   55813628   Local timer interrupts
SPU:          0          0          0          0          0          0          0          0   Spurious interrupts
PMI:        534        523        411        463       1026        376        359        432   Performance monitoring interrupts
IWI:          0          0          0          1         26          0         14          0   IRQ work interrupts
RTR:          0          0          0          0          0          0          0          0   APIC ICR read retries
RES:     362847     282394     226318     404564     220373     365205     409410     130494   Rescheduling interrupts
CAL:    2150038    1440493    1049790    1062483    1848567     986749     972002     817253   Function call interrupts
TLB:     303299     309291     319522     300623     311422     317371     303840     311613   TLB shootdowns
TRM:          0          0          0          0          0          0          0          0   Thermal event interrupts
THR:          0          0          0          0          0          0          0          0   Threshold APIC interrupts
DFR:          0          0          0          0          0          0          0          0   Deferred Error APIC interrupts
MCE:          0          0          0          0          0          0          0          0   Machine check exceptions
MCP:       1200       1201       1201       1201       1201       1201       1201       1201   Machine check polls
ERR:          0
MIS:          0
PIN:          0          0          0          0          0          0          0          0   Posted-interrupt notification event
NPI:          0          0          0          0          0          0          0          0   Nested posted-interrupt event
PIW:          0          0          0          0          0          0          0          0   Posted-interrupt wakeup event

--- NIC IRQ affinities (which CPUs handle which queue)
    $ for ifc in $NETIFS; do
    [ -d "/sys/class/net/$ifc/device/msi_irqs" ] || continue
    echo "=== $ifc IRQ list (first 40) ==="
    ls "/sys/class/net/$ifc/device/msi_irqs" 2>/dev/null | head -n 40
done
=== nic0 IRQ list (first 40) ===
29

--- RPS masks (non-zero only)
    $ for q in /sys/class/net/*/queues/rx-*/rps_cpus; do
    [ -e "$q" ] || continue
    val=$(cat "$q")
    [ "$val" != "0" ] && printf '  %s = %s\n' "$q" "$val"
done | head -n 60
  /sys/class/net/datanet/queues/rx-0/rps_cpus = 00
  /sys/class/net/enx80ae4ccdec03/queues/rx-0/rps_cpus = 00
  /sys/class/net/enx8cae4ccda926/queues/rx-0/rps_cpus = 00
  /sys/class/net/fwbr400i0/queues/rx-0/rps_cpus = 00
  /sys/class/net/fwln400i0/queues/rx-0/rps_cpus = 00
  /sys/class/net/fwpr400p0/queues/rx-0/rps_cpus = 00
  /sys/class/net/lo/queues/rx-0/rps_cpus = 00
  /sys/class/net/nic0/queues/rx-0/rps_cpus = 00
  /sys/class/net/tailscale0/queues/rx-0/rps_cpus = 00
  /sys/class/net/tap400i0/queues/rx-0/rps_cpus = 00
  /sys/class/net/vmbr0/queues/rx-0/rps_cpus = 00

--- XPS masks (non-zero only)
    $ for q in /sys/class/net/*/queues/tx-*/xps_cpus; do
    [ -e "$q" ] || continue
    val=$(cat "$q")
    [ "$val" != "0" ] && printf '  %s = %s\n' "$q" "$val"
done | head -n 60
cat: /sys/class/net/datanet/queues/tx-0/xps_cpus: No such file or directory
cat: /sys/class/net/enx80ae4ccdec03/queues/tx-0/xps_cpus: No such file or directory
cat: /sys/class/net/enx8cae4ccda926/queues/tx-0/xps_cpus: No such file or directory
cat: /sys/class/net/fwbr400i0/queues/tx-0/xps_cpus: No such file or directory
cat: /sys/class/net/lo/queues/tx-0/xps_cpus: No such file or directory
cat: /sys/class/net/nic0/queues/tx-0/xps_cpus: No such file or directory
cat: /sys/class/net/tailscale0/queues/tx-0/xps_cpus: No such file or directory
cat: /sys/class/net/tap400i0/queues/tx-0/xps_cpus: No such file or directory
cat: /sys/class/net/vmbr0/queues/tx-0/xps_cpus: No such file or directory
  /sys/class/net/datanet/queues/tx-0/xps_cpus = 
  /sys/class/net/enx80ae4ccdec03/queues/tx-0/xps_cpus = 
  /sys/class/net/enx8cae4ccda926/queues/tx-0/xps_cpus = 
  /sys/class/net/fwbr400i0/queues/tx-0/xps_cpus = 
  /sys/class/net/fwln400i0/queues/tx-0/xps_cpus = 00
  /sys/class/net/fwpr400p0/queues/tx-0/xps_cpus = 00
  /sys/class/net/lo/queues/tx-0/xps_cpus = 
  /sys/class/net/nic0/queues/tx-0/xps_cpus = 
  /sys/class/net/tailscale0/queues/tx-0/xps_cpus = 
  /sys/class/net/tap400i0/queues/tx-0/xps_cpus = 
  /sys/class/net/vmbr0/queues/tx-0/xps_cpus = 

--- RFS flow counts
    $ for q in /sys/class/net/*/queues/rx-*/rps_flow_cnt; do
    [ -e "$q" ] || continue
    printf '  %s = %s\n' "$q" "$(cat "$q")"
done | head -n 60
  /sys/class/net/datanet/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/enx80ae4ccdec03/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/enx8cae4ccda926/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/fwbr400i0/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/fwln400i0/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/fwpr400p0/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/lo/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/nic0/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/tailscale0/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/tap400i0/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/vmbr0/queues/rx-0/rps_flow_cnt = 0

--- /proc/net/softnet_stat (drops/backlog)
    $ cat /proc/net/softnet_stat
00011896 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000
038f5224 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000001 00000000 00000000
0014d84f 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000002 00000000 00000000
00050174 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000003 00000000 00000000
3cf79af6 00000000 0000000b 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000004 00000000 00000000
0001041f 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000005 00000000 00000000
00018f27 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000006 00000000 00000000
0000f432 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000007 00000000 00000000

--- softnet_stat decoded
    $ # columns: TOTAL DROPPED DROPPED_BY_NETRX TIME_SQUEEZED CPU_COLLISIONS RPS_RECEIVED_FLOW_LIMIT
awk '{ printf "cpu%-2d total=%-8s dropped=%-6s time_squeezed=%-6s cpu_collision=%-4s rps_received=%-6s flow_limit=%s\n",
       NR-1, $1, $2, $4, $5, $6, $7 }' /proc/net/softnet_stat
cpu0  total=00011896 dropped=00000000 time_squeezed=00000000 cpu_collision=00000000 rps_received=00000000 flow_limit=00000000
cpu1  total=038f5226 dropped=00000000 time_squeezed=00000000 cpu_collision=00000000 rps_received=00000000 flow_limit=00000000
cpu2  total=0014d84f dropped=00000000 time_squeezed=00000000 cpu_collision=00000000 rps_received=00000000 flow_limit=00000000
cpu3  total=00050174 dropped=00000000 time_squeezed=00000000 cpu_collision=00000000 rps_received=00000000 flow_limit=00000000
cpu4  total=3cf79baa dropped=00000000 time_squeezed=00000000 cpu_collision=00000000 rps_received=00000000 flow_limit=00000000
cpu5  total=0001041f dropped=00000000 time_squeezed=00000000 cpu_collision=00000000 rps_received=00000000 flow_limit=00000000
cpu6  total=00018f27 dropped=00000000 time_squeezed=00000000 cpu_collision=00000000 rps_received=00000000 flow_limit=00000000
cpu7  total=0000f432 dropped=00000000 time_squeezed=00000000 cpu_collision=00000000 rps_received=00000000 flow_limit=00000000

--- netstat drop counters (significant ones)
    $ nstat -az 2>/dev/null | grep -iE '(Drop|Retrans|Fail|Abort|Overflow|Loss|ListenDrop|EmbryonicRsts|InErrs|OutErrs)' || \
netstat -s 2>/dev/null | grep -iE '(drop|retrans|fail|abort|overflow|loss|listen|error)' | head -n 60
IpReasmFails                    895880             0.0
IpFragFails                     0                  0.0
TcpAttemptFails                 110                0.0
TcpRetransSegs                  56080363           0.0
TcpInErrs                       0                  0.0
Ip6ReasmFails                   0                  0.0
Ip6FragFails                    0                  0.0
TcpExtSyncookiesFailed          0                  0.0
TcpExtEmbryonicRsts             1                  0.0
TcpExtLockDroppedIcmps          0                  0.0
TcpExtListenOverflows           0                  0.0
TcpExtListenDrops               0                  0.0
TcpExtTCPLossUndo               124                0.0
TcpExtTCPLostRetransmit         3046190            0.0
TcpExtTCPRenoFailures           0                  0.0
TcpExtTCPSackFailures           1                  0.0
TcpExtTCPLossFailures           10                 0.0
TcpExtTCPFastRetrans            56064939           0.0
TcpExtTCPSlowStartRetrans       1874               0.0
TcpExtTCPLossProbes             12422              0.0
TcpExtTCPLossProbeRecovery      749                0.0
TcpExtTCPRenoRecoveryFail       0                  0.0
TcpExtTCPSackRecoveryFail       675                0.0
TcpExtTCPAbortOnData            2518               0.0
TcpExtTCPAbortOnClose           42                 0.0
TcpExtTCPAbortOnMemory          0                  0.0
TcpExtTCPAbortOnTimeout         12                 0.0
TcpExtTCPAbortOnLinger          0                  0.0
TcpExtTCPAbortFailed            0                  0.0
TcpExtTCPMD5Failure             0                  0.0
TcpExtTCPBacklogDrop            0                  0.0
TcpExtPFMemallocDrop            0                  0.0
TcpExtTCPMinTTLDrop             0                  0.0
TcpExtTCPDeferAcceptDrop        0                  0.0
TcpExtTCPTimeWaitOverflow       0                  0.0
TcpExtTCPReqQFullDrop           0                  0.0
TcpExtTCPRetransFail            0                  0.0
TcpExtTCPOFODrop                0                  0.0
TcpExtTCPFastOpenActiveFail     0                  0.0
TcpExtTCPFastOpenPassiveFail    0                  0.0
TcpExtTCPFastOpenListenOverflow 0                  0.0
TcpExtTCPSynRetrans             785                0.0
TcpExtTCPMTUPFail               0                  0.0
TcpExtTCPZeroWindowDrop         0                  0.0
TcpExtTCPRcvQDrop               0                  0.0
TcpExtTCPMigrateReqFailure      0                  0.0
TcpExtTCPAODroppedIcmps         0                  0.0
MPTcpExtMPCapableSYNTXDrop      0                  0.0
MPTcpExtMPTCPRetrans            0                  0.0
MPTcpExtMPJoinSynAckHMacFailure 0                  0.0
MPTcpExtMPJoinAckHMacFailure    0                  0.0
MPTcpExtAddAddrTxDrop           0                  0.0
MPTcpExtEchoAddTxDrop           0                  0.0
MPTcpExtAddAddrDrop             0                  0.0
MPTcpExtRmAddrDrop              0                  0.0
MPTcpExtRmAddrTxDrop            0                  0.0
MPTcpExtMPFailTx                0                  0.0
MPTcpExtMPFailRx                0                  0.0
MPTcpExtFallbackFailed          0                  0.0

###############################################################################
# 13. NETWORK: SOCKET / TCP STATE
###############################################################################

--- ss -s
    $ ss -s
Total: 389
TCP:   72 (estab 39, closed 3, orphaned 0, timewait 1)

Transport Total     IP        IPv6
RAW	  0         0         0        
UDP	  18        10        8        
TCP	  69        58        11       
INET	  87        68        19       
FRAG	  0         0         0        


--- ss -t -m (top TCP with skmem/cwnd/rto)
    $ ss -tno state established ( dport != :22 and sport != :22 ) -m
Recv-Q Send-Q         Local Address:Port            Peer Address:Port                                                                                   
0      0               100.70.77.93:2004            100.70.77.93:38448 timer:(keepalive,65min,0)
	 skmem:(r0,rb87380,t0,tb3939840,f0,w0,o0,bl0,d0)      
0      0               10.100.100.4:2049            10.100.100.6:808  
	 skmem:(r0,rb15671440,t0,tb4125696,f0,w0,o0,bl0,d14750)                         
0      0               10.100.100.4:2049            10.100.100.1:857  
	 skmem:(r0,rb11393084,t0,tb3028992,f0,w0,o0,bl0,d50333)                         
0      0              192.168.3.191:49802         209.177.156.94:443   timer:(keepalive,15sec,0)
	 skmem:(r0,rb132680,t0,tb130560,f0,w0,o0,bl0,d0)      
0      0               100.70.77.93:54702           100.70.77.93:2001  timer:(keepalive,55min,0)
	 skmem:(r0,rb87380,t0,tb3939840,f0,w0,o0,bl0,d0)      
0      0               100.70.77.93:2002            100.70.77.93:60962 timer:(keepalive,55min,0)
	 skmem:(r0,rb87380,t0,tb3939840,f0,w0,o0,bl0,d0)      
0      0               10.100.100.4:2049            10.100.100.5:726  
	 skmem:(r0,rb1288276,t0,tb8512512,f0,w0,o0,bl0,d15257)                          
0      0               100.70.77.93:2007            100.70.77.93:33482 timer:(keepalive,65min,0)
	 skmem:(r0,rb87380,t0,tb3939840,f0,w0,o0,bl0,d4)      
0      0               100.70.77.93:2006            100.70.77.93:53816 timer:(keepalive,25min,0)
	 skmem:(r0,rb87380,t0,tb3939840,f0,w0,o0,bl0,d0)      
0      0               10.100.100.4:2049            10.100.100.3:716  
	 skmem:(r0,rb741219,t0,tb5104896,f0,w0,o0,bl0,d6260)                            
0      0               10.100.100.4:2049            10.100.100.6:972  
	 skmem:(r0,rb15263623,t0,tb4491264,f0,w0,o0,bl0,d14718)                         
0      0               10.100.100.4:2049            10.100.100.9:800  
	 skmem:(r0,rb11845692,t0,tb4491264,f0,w0,o0,bl0,d17498)                         
0      116             10.100.100.4:2049            10.100.100.1:843   timer:(on,214ms,0)
	 skmem:(r0,rb12093150,t0,tb3211776,f3020,w1076,o0,bl0,d50534)
0      0               100.70.77.93:33482           100.70.77.93:2007  timer:(keepalive,65min,0)
	 skmem:(r0,rb87380,t0,tb3939840,f0,w0,o0,bl0,d4)      
0      0              192.168.3.191:41882          192.200.0.107:443   timer:(keepalive,5.114sec,0)
	 skmem:(r0,rb87380,t0,tb130560,f0,w0,o0,bl0,d0)    
0      0               100.70.77.93:39370           100.70.77.93:2005  timer:(keepalive,34min,0)
	 skmem:(r0,rb87380,t0,tb3939840,f0,w0,o0,bl0,d0)      
0      0               100.70.77.93:45682           100.70.77.93:2003  timer:(keepalive,55min,0)
	 skmem:(r0,rb87380,t0,tb3939840,f0,w0,o0,bl0,d0)      
0      0               100.70.77.93:2003            100.70.77.93:45682 timer:(keepalive,55min,0)
	 skmem:(r0,rb87380,t0,tb3939840,f0,w0,o0,bl0,d0)      
0      0               100.70.77.93:2005            100.70.77.93:39370 timer:(keepalive,34min,0)
	 skmem:(r0,rb87380,t0,tb3939840,f0,w0,o0,bl0,d0)      
0      0               10.100.100.4:2049            10.100.100.6:964  
	 skmem:(r0,rb16777216,t0,tb5144064,f0,w0,o0,bl0,d14806)                         
0      0               10.100.100.4:2049            10.100.100.9:891  
	 skmem:(r0,rb14216601,t0,tb4856832,f0,w0,o0,bl0,d17345)                         
0      0               10.100.100.4:2049            10.100.100.7:807  
	 skmem:(r0,rb12878137,t0,tb3133440,f0,w0,o0,bl0,d43857)                         
0      0               10.100.100.4:2049            10.100.100.7:848  
	 skmem:(r0,rb16777216,t0,tb3694848,f0,w0,o0,bl0,d44788)                         
0      0               10.100.100.4:2049            10.100.100.9:674  
	 skmem:(r0,rb14482998,t0,tb4569600,f0,w0,o0,bl0,d17629)                         
0      0               100.70.77.93:2001            100.70.77.93:54702 timer:(keepalive,55min,0)
	 skmem:(r0,rb87380,t0,tb3939840,f0,w0,o0,bl0,d0)      
0      0               10.100.100.4:2049            10.100.100.9:842  
	 skmem:(r0,rb13248656,t0,tb4282368,f0,w0,o0,bl0,d17663)                         
0      0               100.70.77.93:60962           100.70.77.93:2002  timer:(keepalive,55min,0)
	 skmem:(r0,rb87380,t0,tb3939840,f0,w0,o0,bl0,d0)      
0      0               10.100.100.4:2049            10.100.100.6:753  
	 skmem:(r0,rb16777216,t0,tb4308480,f0,w0,o0,bl0,d14931)                         
0      0               10.100.100.4:2049            10.100.100.3:749  
	 skmem:(r0,rb920708,t0,tb3485952,f0,w0,o0,bl0,d6294)                            
0      0               10.100.100.4:2049            10.100.100.1:749  
	 skmem:(r0,rb13065661,t0,tb3368448,f0,w0,o0,bl0,d50335)                         
0      0               100.70.77.93:38448           100.70.77.93:2004  timer:(keepalive,65min,0)
	 skmem:(r0,rb176788,t0,tb3939840,f0,w0,o0,bl0,d0)     
0      0               10.100.100.4:2049            10.100.100.7:852  
	 skmem:(r0,rb16777216,t0,tb3472896,f0,w0,o0,bl0,d44633)                         
0      0               100.70.77.93:53816           100.70.77.93:2006  timer:(keepalive,25min,0)
	 skmem:(r0,rb87380,t0,tb3939840,f0,w0,o0,bl0,d0)      
0      0               10.100.100.4:2049            10.100.100.3:891  
	 skmem:(r0,rb1008266,t0,tb4647936,f0,w0,o0,bl0,d6255)                           
0      0               10.100.100.4:2049            10.100.100.1:718  
	 skmem:(r0,rb10730604,t0,tb3055104,f0,w0,o0,bl0,d50132)                         
0      0               10.100.100.4:2049            10.100.100.7:692  
	 skmem:(r0,rb16022431,t0,tb3002880,f0,w0,o0,bl0,d44584)                         
0      0               10.100.100.4:2049            10.100.100.3:752  
	 skmem:(r0,rb835559,t0,tb4373760,f0,w0,o0,bl0,d6202)                            
0      0      [::ffff:100.70.77.93]:45876 [::ffff:100.107.35.78]:43954 timer:(keepalive,8.920sec,0)
	 skmem:(r0,rb441849,t0,tb130560,f0,w0,o0,bl0,d4623)

--- ss -ti (TCP internals)
    $ ss -ti
State Recv-Q Send-Q         Local Address:Port            Peer Address:Port                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    
ESTAB 0      0               100.70.77.93:2004            100.70.77.93:38448       
	 bbr wscale:9,9 rto:201 rtt:0.014/0.002 ato:40 mss:22016 pmtu:65535 rcvmss:536 advmss:65483 cwnd:18 bytes_sent:78549 bytes_acked:78549 bytes_received:15 segs_out:2621 segs_in:2623 data_segs_out:2620 data_segs_in:1 bbr:(bw:19.6Gbps,mrtt:0.009,pacing_gain:2.88672,cwnd_gain:2.88672) send 226Gbps lastsnd:9968 lastrcv:32660928 lastack:9968 pacing_rate 229Gbps delivery_rate 19.6Gbps delivered:2621 app_limited busy:47ms rcv_space:43690 rcv_ssthresh:43690 minrtt:0.009 snd_wnd:44032 rcv_wnd:44032                                                                                                                                                                                                              
ESTAB 0      0               10.100.100.4:nfs             10.100.100.6:808         
	 bbr wscale:12,9 rto:210 rtt:9.374/13.639 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:308 ssthresh:168 bytes_sent:18333809780 bytes_retrans:154884 bytes_acked:18333654896 bytes_received:3807370344 segs_out:13658811 segs_in:6778499 data_segs_out:12964944 data_segs_in:2751113 bbr:(bw:980Mbps,mrtt:0.99,pacing_gain:1.25,cwnd_gain:2) send 381Mbps lastsnd:2556 lastrcv:2577 lastack:2555 pacing_rate 1.21Gbps delivery_rate 909Mbps delivered:12964669 busy:2298005ms retrans:0/282 dsack_dups:320 rcv_rtt:8.236 rcv_space:5203408 rcv_ssthresh:10406815 minrtt:0.378 rcv_ooopack:123628 snd_wnd:4345856 rcv_wnd:10406912 rehash:8                                                                       
ESTAB 0      0               10.100.100.4:nfs             10.100.100.1:857         
	 bbr wscale:12,9 rto:218 rtt:17.576/19.596 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:64 ssthresh:163 bytes_sent:29490393428 bytes_retrans:7161348048 bytes_acked:22329045380 bytes_received:12945562976 segs_out:25330105 segs_in:17141442 data_segs_out:21575224 data_segs_in:9335186 bbr:(bw:153Mbps,mrtt:0.543,pacing_gain:1.25,cwnd_gain:2) send 42.2Mbps lastsnd:261 lastrcv:5 lastack:5 pacing_rate 189Mbps delivery_rate 61.8Mbps delivered:16629168 app_limited busy:13265106ms retrans:0/4948405 dsack_dups:2365 reordering:179 reord_seen:116 rcv_rtt:24.789 rcv_space:3782860 rcv_ssthresh:7565719 minrtt:0.527 rcv_ooopack:11769 snd_wnd:16846848 rcv_wnd:7565824 rehash:159                     
ESTAB 0      0              192.168.3.191:49802         209.177.156.94:https       
	 bbr wscale:7,9 rto:214 rtt:13.41/1.847 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:32 bytes_sent:153618 bytes_retrans:193 bytes_acked:153426 bytes_received:1298351 segs_out:10294 segs_in:9933 data_segs_out:856 data_segs_in:7618 bbr:(bw:2.89Mbps,mrtt:13.753,pacing_gain:2.88672,cwnd_gain:2.88672) send 27.6Mbps lastsnd:12303 lastrcv:12289 lastack:12289 pacing_rate 23.3Mbps delivery_rate 2.89Mbps delivered:857 app_limited busy:6889ms retrans:0/1 dsack_dups:1 reord_seen:1 rcv_rtt:74239.1 rcv_space:44054 rcv_ssthresh:87470 minrtt:13.753 snd_wnd:205568 rcv_wnd:87552                                                                                                                         
ESTAB 0      0               100.70.77.93:ssh          100.101.187.119:54706       
	 bbr wscale:7,9 rto:207 rtt:6.116/9.84 ato:40 mss:1228 pmtu:1280 rcvmss:1228 advmss:1228 cwnd:27 bytes_sent:5653 bytes_acked:5653 bytes_received:3993 segs_out:24 segs_in:26 data_segs_out:17 data_segs_in:15 bbr:(bw:24.6Mbps,mrtt:0.701,pacing_gain:2.88672,cwnd_gain:2.88672) send 43.4Mbps lastsnd:1380 lastrcv:1380 lastack:1379 pacing_rate 377Mbps delivery_rate 24.6Mbps delivered:18 app_limited busy:106ms rcv_rtt:6 rcv_space:12400 rcv_ssthresh:78504 minrtt:0.701 snd_wnd:76928 rcv_wnd:78848                                                                                                                                                                                                                
ESTAB 0      0               100.70.77.93:54702           100.70.77.93:2001        
	 bbr wscale:9,9 rto:201 rtt:0.035/0.019 ato:40 mss:22016 pmtu:65535 rcvmss:536 advmss:65483 cwnd:11 bytes_sent:15 bytes_acked:16 bytes_received:8184 segs_out:1223 segs_in:1222 data_segs_out:1 data_segs_in:1220 bbr:(bw:14.7Gbps,mrtt:0.012,pacing_gain:2.88672,cwnd_gain:2.88672) send 55.4Gbps lastsnd:32660928 lastrcv:242160 lastack:242160 pacing_rate 128Gbps delivery_rate 14.7Gbps delivered:2 app_limited rcv_space:43690 rcv_ssthresh:43690 minrtt:0.012 snd_wnd:44032 rcv_wnd:44032                                                                                                                                                                                                                          
ESTAB 0      0               100.70.77.93:2002            100.70.77.93:60962       
	 bbr wscale:9,9 rto:201 rtt:0.018/0.007 ato:40 mss:22016 pmtu:65535 rcvmss:536 advmss:65483 cwnd:18 bytes_sent:641 bytes_acked:641 bytes_received:15 segs_out:97 segs_in:99 data_segs_out:96 data_segs_in:1 bbr:(bw:29.4Gbps,mrtt:0.006,pacing_gain:2.88672,cwnd_gain:2.88672) send 176Gbps lastsnd:271322 lastrcv:32660928 lastack:271321 pacing_rate 458Gbps delivery_rate 29.4Gbps delivered:97 app_limited busy:2ms rcv_space:43690 rcv_ssthresh:43690 minrtt:0.006 snd_wnd:44032 rcv_wnd:44032                                                                                                                                                                                                                       
ESTAB 0      0               10.100.100.4:nfs             10.100.100.5:726         
	 bbr wscale:12,9 rto:212 rtt:11.3/16.007 ato:67 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:48 ssthresh:174 bytes_sent:325275060 bytes_retrans:60916 bytes_acked:325214144 bytes_received:3564924388 segs_out:1547206 segs_in:2991844 data_segs_out:856831 data_segs_in:2573537 bbr:(bw:114Mbps,mrtt:0.58,pacing_gain:1.25,cwnd_gain:2) send 49.2Mbps lastsnd:1288 lastrcv:1289 lastack:1287 pacing_rate 142Mbps delivery_rate 114Mbps delivered:856628 app_limited busy:3054405ms rwnd_limited:1ms(0.0%) retrans:0/426 dsack_dups:304 rcv_rtt:4.863 rcv_space:427748 rcv_ssthresh:855495 minrtt:0.203 rcv_ooopack:361 snd_wnd:757760 rcv_wnd:855552 rehash:17                                                        
ESTAB 0      0               100.70.77.93:2007            100.70.77.93:33482       
	 bbr wscale:9,9 rto:201 rtt:0.011/0.006 ato:40 mss:22016 pmtu:65535 rcvmss:536 advmss:65483 cwnd:11 bytes_sent:135 bytes_acked:135 bytes_received:15 segs_out:10 segs_in:12 data_segs_out:1 data_segs_in:1 bbr:(bw:29.4Gbps,mrtt:0.006,pacing_gain:2.88672,cwnd_gain:2.88672) send 176Gbps lastsnd:32660160 lastrcv:32660928 lastack:3260357 pacing_rate 419Gbps delivery_rate 29.4Gbps delivered:2 app_limited rcv_space:43690 rcv_ssthresh:43690 minrtt:0.006 snd_wnd:44032 rcv_wnd:44032                                                                                                                                                                                                                               
ESTAB 0      0               100.70.77.93:2006            100.70.77.93:53816       
	 bbr wscale:9,9 rto:201 rtt:0.016/0.003 ato:40 mss:22016 pmtu:65535 rcvmss:536 advmss:65483 cwnd:18 bytes_sent:594 bytes_acked:594 bytes_received:15 segs_out:92 segs_in:94 data_segs_out:91 data_segs_in:1 bbr:(bw:25.2Gbps,mrtt:0.007,pacing_gain:2.88672,cwnd_gain:2.88672) send 198Gbps lastsnd:271661 lastrcv:32660928 lastack:271661 pacing_rate 387Gbps delivery_rate 25.2Gbps delivered:92 app_limited rcv_space:43690 rcv_ssthresh:43690 minrtt:0.007 snd_wnd:44032 rcv_wnd:44032                                                                                                                                                                                                                                
ESTAB 0      0               10.100.100.4:nfs             10.100.100.3:716         
	 bbr wscale:12,9 rto:211 rtt:10.547/14.706 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:955 bytes_sent:116905044 bytes_retrans:12204 bytes_acked:116892840 bytes_received:1059101216 segs_out:593792 segs_in:986612 data_segs_out:288188 data_segs_in:777323 bbr:(bw:681Mbps,mrtt:1.056,pacing_gain:2.88672,cwnd_gain:2.88672) send 1.05Gbps lastsnd:4713 lastrcv:4748 lastack:4669 pacing_rate 2.17Gbps delivery_rate 681Mbps delivered:288182 app_limited busy:1126638ms retrans:0/57 dsack_dups:57 rcv_rtt:5.535 rcv_space:246108 rcv_ssthresh:492215 minrtt:0.846 rcv_ooopack:141 snd_wnd:790528 rcv_wnd:492544 rehash:5                                                                                    
ESTAB 0      0               10.100.100.4:nfs             10.100.100.6:972         
	 bbr wscale:12,9 rto:208 rtt:7.581/11.73 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:236 ssthresh:207 bytes_sent:18288476556 bytes_retrans:180484 bytes_acked:18288296072 bytes_received:3848980464 segs_out:13628108 segs_in:6805979 data_segs_out:12933427 data_segs_in:2779815 bbr:(bw:703Mbps,mrtt:0.789,pacing_gain:1.25,cwnd_gain:2) send 361Mbps lastsnd:2791 lastrcv:2832 lastack:2790 pacing_rate 870Mbps delivery_rate 354Mbps delivered:12933261 busy:2292996ms retrans:0/259 dsack_dups:155 rcv_rtt:12.389 rcv_space:5068000 rcv_ssthresh:10135999 minrtt:0.436 rcv_ooopack:125219 snd_wnd:5484544 rcv_wnd:10136064 rehash:11                                                                      
ESTAB 0      0               10.100.100.4:nfs             10.100.100.9:800         
	 bbr wscale:12,9 rto:208 rtt:7.268/9.26 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:242 bytes_sent:7762665996 bytes_retrans:273288 bytes_acked:7762392708 bytes_received:6144339140 segs_out:6795085 segs_in:7154004 data_segs_out:5766179 data_segs_in:4339730 bbr:(bw:595Mbps,mrtt:0.998,pacing_gain:1.25,cwnd_gain:2) send 386Mbps lastsnd:2849 lastrcv:2863 lastack:2848 pacing_rate 737Mbps delivery_rate 355Mbps delivered:5765985 app_limited busy:4645381ms retrans:0/276 dsack_dups:117 rcv_rtt:13.101 rcv_space:3933140 rcv_ssthresh:7866279 minrtt:0.787 rcv_ooopack:67140 snd_wnd:1703936 rcv_wnd:7866368 rehash:6                                                                                 
ESTAB 0      0               10.100.100.4:nfs             10.100.100.1:843         
	 bbr wscale:12,9 rto:214 rtt:13.036/15.742 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:106 ssthresh:168 bytes_sent:29504041036 bytes_retrans:7154086964 bytes_acked:22349954072 bytes_received:12926615988 segs_out:25349530 segs_in:17006709 data_segs_out:21585006 data_segs_in:9321864 bbr:(bw:254Mbps,mrtt:0.565,pacing_gain:1.25,cwnd_gain:2) send 94.2Mbps lastsnd:8 lastrcv:19 lastack:5 pacing_rate 314Mbps delivery_rate 128Mbps delivered:16643835 app_limited busy:13342808ms retrans:0/4943331 dsack_dups:2171 reordering:179 reord_seen:268 rcv_rtt:31.637 rcv_space:4015304 rcv_ssthresh:8030607 minrtt:0.445 rcv_ooopack:8050 snd_wnd:4993024 rcv_wnd:8030720 rehash:183                        
ESTAB 0      0               100.70.77.93:33482           100.70.77.93:2007        
	 bbr wscale:9,9 rto:201 rtt:0.012/0.006 ato:40 mss:22016 pmtu:65535 rcvmss:536 advmss:65483 cwnd:11 bytes_sent:15 bytes_acked:16 bytes_received:135 segs_out:12 segs_in:11 data_segs_out:1 data_segs_in:1 bbr:(bw:35.2Gbps,mrtt:0.005,pacing_gain:2.88672,cwnd_gain:2.88672) send 161Gbps lastsnd:32660928 lastrcv:32660160 lastack:3260357 pacing_rate 384Gbps delivery_rate 35.2Gbps delivered:2 app_limited rcv_space:43690 rcv_ssthresh:43690 minrtt:0.005 snd_wnd:44032 rcv_wnd:44032                                                                                                                                                                                                                                
ESTAB 0      0              192.168.3.191:41882          192.200.0.107:https       
	 bbr wscale:10,9 rto:341 rtt:137.281/4.75 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:18 bytes_sent:2915 bytes_acked:2916 bytes_received:84533 segs_out:1320 segs_in:1327 data_segs_out:16 data_segs_in:683 bbr:(bw:343kbps,mrtt:134.466,pacing_gain:2.88672,cwnd_gain:2.88672) send 1.52Mbps lastsnd:1839583 lastrcv:4157 lastack:4157 pacing_rate 2.45Mbps delivery_rate 344kbps delivered:17 app_limited busy:1669ms rcv_rtt:137 rcv_space:19619 rcv_ssthresh:57388 minrtt:134.466 snd_wnd:80896 rcv_wnd:57856                                                                                                                                                                                              
ESTAB 0      0               100.70.77.93:39370           100.70.77.93:2005        
	 bbr wscale:9,9 rto:201 rtt:0.012/0.006 ato:49 mss:22016 pmtu:65535 rcvmss:536 advmss:65483 cwnd:11 bytes_sent:15 bytes_acked:16 bytes_received:1202 segs_out:62 segs_in:61 data_segs_out:1 data_segs_in:59 bbr:(bw:35.2Gbps,mrtt:0.005,pacing_gain:2.88672,cwnd_gain:2.88672) send 161Gbps lastsnd:32660929 lastrcv:159287 lastack:159287 pacing_rate 384Gbps delivery_rate 35.2Gbps delivered:2 app_limited rcv_space:43690 rcv_ssthresh:43690 minrtt:0.005 snd_wnd:44032 rcv_wnd:44032                                                                                                                                                                                                                                 
ESTAB 0      0               100.70.77.93:45682           100.70.77.93:2003        
	 bbr wscale:9,9 rto:201 rtt:0.011/0.006 ato:40 mss:22016 pmtu:65535 rcvmss:536 advmss:65483 cwnd:11 bytes_sent:15 bytes_acked:16 bytes_received:613 segs_out:98 segs_in:97 data_segs_out:1 data_segs_in:95 bbr:(bw:35.2Gbps,mrtt:0.005,pacing_gain:2.88672,cwnd_gain:2.88672) send 176Gbps lastsnd:32660929 lastrcv:272854 lastack:272854 pacing_rate 416Gbps delivery_rate 35.2Gbps delivered:2 app_limited rcv_space:43690 rcv_ssthresh:43690 minrtt:0.005 snd_wnd:44032 rcv_wnd:44032                                                                                                                                                                                                                                  
ESTAB 0      0               100.70.77.93:2003            100.70.77.93:45682       
	 bbr wscale:9,9 rto:201 rtt:0.018/0.005 ato:40 mss:22016 pmtu:65535 rcvmss:536 advmss:65483 cwnd:18 bytes_sent:613 bytes_acked:613 bytes_received:15 segs_out:96 segs_in:98 data_segs_out:95 data_segs_in:1 bbr:(bw:29.4Gbps,mrtt:0.006,pacing_gain:2.88672,cwnd_gain:2.88672) send 176Gbps lastsnd:272854 lastrcv:32660929 lastack:272854 pacing_rate 503Gbps delivery_rate 29.4Gbps delivered:96 app_limited busy:3ms rcv_space:43690 rcv_ssthresh:43690 minrtt:0.006 snd_wnd:44032 rcv_wnd:44032                                                                                                                                                                                                                       
ESTAB 0      0               100.70.77.93:2005            100.70.77.93:39370       
	 bbr wscale:9,9 rto:201 rtt:0.015/0 ato:40 mss:22016 pmtu:65535 rcvmss:536 advmss:65483 cwnd:18 bytes_sent:1202 bytes_acked:1202 bytes_received:15 segs_out:60 segs_in:62 data_segs_out:59 data_segs_in:1 bbr:(bw:25.2Gbps,mrtt:0.007,pacing_gain:2.88672,cwnd_gain:2.88672) send 211Gbps lastsnd:159287 lastrcv:32660929 lastack:159287 pacing_rate 458Gbps delivery_rate 25.2Gbps delivered:60 app_limited busy:4ms rcv_space:43690 rcv_ssthresh:43690 minrtt:0.007 snd_wnd:44032 rcv_wnd:44032                                                                                                                                                                                                                         
ESTAB 0      0               10.100.100.4:nfs             10.100.100.6:964         
	 bbr wscale:12,9 rto:208 rtt:7.532/11.22 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:264 ssthresh:205 bytes_sent:18157660412 bytes_retrans:101804 bytes_acked:18157558608 bytes_received:3836358324 segs_out:13537780 segs_in:6764792 data_segs_out:12843432 data_segs_in:2771150 bbr:(bw:686Mbps,mrtt:1.057,pacing_gain:1,cwnd_gain:2) send 406Mbps lastsnd:2524 lastrcv:2555 lastack:2523 pacing_rate 680Mbps delivery_rate 415Mbps delivered:12843347 busy:2288632ms retrans:0/235 dsack_dups:197 rcv_rtt:28.491 rcv_space:5928112 rcv_ssthresh:11141120 minrtt:0.382 rcv_ooopack:130456 snd_wnd:3158016 rcv_wnd:11141120 rehash:13                                                                         
ESTAB 0      0               10.100.100.4:nfs             10.100.100.9:891         
	 bbr wscale:12,9 rto:207 rtt:6.7/7.798 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:280 ssthresh:241 bytes_sent:7641538236 bytes_retrans:430172 bytes_acked:7641108064 bytes_received:6178911944 segs_out:6704532 segs_in:7172502 data_segs_out:5682185 data_segs_in:4363273 bbr:(bw:615Mbps,mrtt:1.321,pacing_gain:1.25,cwnd_gain:2) send 484Mbps lastsnd:2664 lastrcv:2664 lastack:2661 pacing_rate 761Mbps delivery_rate 356Mbps delivered:5681888 app_limited busy:4631223ms retrans:0/364 dsack_dups:106 rcv_rtt:66.891 rcv_space:4720356 rcv_ssthresh:9440711 minrtt:0.723 rcv_ooopack:68036 snd_wnd:1990656 rcv_wnd:9440768 rehash:1                                                                     
ESTAB 0      0               10.100.100.4:nfs             10.100.100.7:807         
	 bbr wscale:12,9 rto:218 rtt:17.566/19.733 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:188 ssthresh:177 bytes_sent:2212688424 bytes_retrans:39456 bytes_acked:2212648968 bytes_received:10169584924 segs_out:4987048 segs_in:8710352 data_segs_out:2624486 data_segs_in:7302477 bbr:(bw:1.03Gbps,mrtt:0.268,pacing_gain:1.25,cwnd_gain:2) send 124Mbps lastsnd:65 lastrcv:65 lastack:63 pacing_rate 1.27Gbps delivery_rate 957Mbps delivered:2624294 app_limited busy:8191105ms retrans:0/239 dsack_dups:317 rcv_rtt:37.922 rcv_space:4275944 rcv_ssthresh:8551887 minrtt:0.197 rcv_ooopack:588749 snd_wnd:2670592 rcv_wnd:8551936 rehash:7                                                                    
ESTAB 0      0               10.100.100.4:nfs             10.100.100.7:848         
	 bbr wscale:12,9 rto:212 rtt:11.48/16.296 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:244 ssthresh:213 bytes_sent:2211761756 bytes_retrans:44368 bytes_acked:2211717388 bytes_received:10176539620 segs_out:4967468 segs_in:8716298 data_segs_out:2617697 data_segs_in:7307308 bbr:(bw:976Mbps,mrtt:0.626,pacing_gain:1.25,cwnd_gain:2) send 246Mbps lastsnd:65 lastrcv:65 lastack:63 pacing_rate 1.21Gbps delivery_rate 943Mbps delivered:2617408 busy:8050405ms retrans:0/288 dsack_dups:457 rcv_rtt:34.684 rcv_space:7296640 rcv_ssthresh:11141120 minrtt:0.187 rcv_ooopack:517758 snd_wnd:2531328 rcv_wnd:11141120 rehash:10                                                                               
ESTAB 0      0               10.100.100.4:nfs             10.100.100.9:674         
	 bbr wscale:12,9 rto:209 rtt:8.571/10.613 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:236 ssthresh:267 bytes_sent:7635818008 bytes_retrans:202304 bytes_acked:7635615704 bytes_received:6056914204 segs_out:6700938 segs_in:7113443 data_segs_out:5678318 data_segs_in:4279463 bbr:(bw:1.03Gbps,mrtt:0.55,pacing_gain:1.25,cwnd_gain:2) send 319Mbps lastsnd:3377 lastrcv:3441 lastack:3374 pacing_rate 1.28Gbps delivery_rate 392Mbps delivered:5678181 app_limited busy:4651992ms rwnd_limited:1ms(0.0%) retrans:0/210 dsack_dups:73 rcv_rtt:94.945 rcv_space:4808808 rcv_ssthresh:9617615 minrtt:0.55 rcv_ooopack:62950 snd_wnd:2273280 rcv_wnd:9617920 rehash:4                                            
ESTAB 0      0               100.70.77.93:2001            100.70.77.93:54702       
	 bbr wscale:9,9 rto:201 rtt:0.019/0.005 ato:40 mss:22016 pmtu:65535 rcvmss:536 advmss:65483 cwnd:18 bytes_sent:8184 bytes_acked:8184 bytes_received:15 segs_out:1221 segs_in:1223 data_segs_out:1220 data_segs_in:1 bbr:(bw:25.2Gbps,mrtt:0.007,pacing_gain:2.88672,cwnd_gain:2.88672) send 167Gbps lastsnd:242161 lastrcv:32660929 lastack:242161 pacing_rate 174Gbps delivery_rate 25.2Gbps delivered:1221 app_limited busy:29ms rcv_space:43690 rcv_ssthresh:43690 minrtt:0.007 snd_wnd:44032 rcv_wnd:44032                                                                                                                                                                                                            
ESTAB 0      0               10.100.100.4:nfs             10.100.100.9:842         
	 bbr wscale:12,9 rto:209 rtt:8.332/10.226 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:224 ssthresh:246 bytes_sent:7632812244 bytes_retrans:158280 bytes_acked:7632653964 bytes_received:6152300824 segs_out:6709817 segs_in:7175171 data_segs_out:5676099 data_segs_in:4344964 bbr:(bw:922Mbps,mrtt:0.534,pacing_gain:1.25,cwnd_gain:2) send 311Mbps lastsnd:2688 lastrcv:2688 lastack:2685 pacing_rate 1.14Gbps delivery_rate 421Mbps delivered:5675908 app_limited busy:4636874ms retrans:0/190 dsack_dups:207 rcv_rtt:58.256 rcv_space:4398968 rcv_ssthresh:8797935 minrtt:0.534 rcv_ooopack:64374 snd_wnd:1908736 rcv_wnd:8798208 rehash:7                                                                 
ESTAB 0      0               100.70.77.93:60962           100.70.77.93:2002        
	 bbr wscale:9,9 rto:201 rtt:0.012/0.006 ato:40 mss:22016 pmtu:65535 rcvmss:536 advmss:65483 cwnd:11 bytes_sent:15 bytes_acked:16 bytes_received:641 segs_out:99 segs_in:98 data_segs_out:1 data_segs_in:96 bbr:(bw:29.4Gbps,mrtt:0.006,pacing_gain:2.88672,cwnd_gain:2.88672) send 161Gbps lastsnd:32660929 lastrcv:271322 lastack:271322 pacing_rate 384Gbps delivery_rate 29.4Gbps delivered:2 app_limited rcv_space:43690 rcv_ssthresh:43690 minrtt:0.006 snd_wnd:44032 rcv_wnd:44032                                                                                                                                                                                                                                  
ESTAB 0      0               10.100.100.4:nfs             10.100.100.6:753         
	 bbr wscale:12,9 rto:208 rtt:7.904/12.21 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:220 ssthresh:189 bytes_sent:18283994148 bytes_retrans:227124 bytes_acked:18283767024 bytes_received:3825824076 segs_out:13626884 segs_in:6776341 data_segs_out:12930470 data_segs_in:2764076 bbr:(bw:982Mbps,mrtt:0.475,pacing_gain:1.25,cwnd_gain:2) send 322Mbps lastsnd:1661 lastrcv:1673 lastack:1661 pacing_rate 1.22Gbps delivery_rate 705Mbps delivered:12930253 busy:2301178ms retrans:0/333 dsack_dups:327 rcv_rtt:14.065 rcv_space:6560888 rcv_ssthresh:11141120 minrtt:0.147 rcv_ooopack:128748 snd_wnd:2551808 rcv_wnd:11141120 rehash:15                                                                     
ESTAB 0      0               10.100.100.4:nfs             10.100.100.3:kerberos-adm
	 bbr wscale:12,9 rto:210 rtt:9.221/11.826 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:1060 bytes_sent:114250520 bytes_retrans:7216 bytes_acked:114243304 bytes_received:1058542184 segs_out:588083 segs_in:988135 data_segs_out:286325 data_segs_in:776986 bbr:(bw:844Mbps,mrtt:1.067,pacing_gain:2.88672,cwnd_gain:2.88672) send 1.33Gbps lastsnd:4150 lastrcv:4168 lastack:4146 pacing_rate 2.41Gbps delivery_rate 844Mbps delivered:286326 app_limited busy:1129430ms retrans:0/42 dsack_dups:42 rcv_rtt:4.782 rcv_space:305704 rcv_ssthresh:611407 minrtt:0.688 rcv_ooopack:117 snd_wnd:3198976 rcv_wnd:611840 rehash:1                                                                                    
ESTAB 0      0               10.100.100.4:nfs             10.100.100.1:kerberos-adm
	 bbr wscale:12,9 rto:215 rtt:14.708/16.91 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:56 ssthresh:193 bytes_sent:29536917460 bytes_retrans:7193633156 bytes_acked:22343284304 bytes_received:12931866060 segs_out:25361073 segs_in:17043825 data_segs_out:21607373 data_segs_in:9324942 bbr:(bw:127Mbps,mrtt:0.581,pacing_gain:1.25,cwnd_gain:2) send 44.1Mbps lastsnd:32 lastrcv:41 lastack:29 pacing_rate 158Mbps delivery_rate 42Mbps delivered:16639331 app_limited busy:13280290ms retrans:0/4970686 dsack_dups:2631 reordering:179 reord_seen:232 rcv_rtt:21.856 rcv_space:4338208 rcv_ssthresh:8676415 minrtt:0.443 rcv_ooopack:11322 snd_wnd:11345920 rcv_wnd:8676864 rehash:177                       
ESTAB 0      0               100.70.77.93:38448           100.70.77.93:2004        
	 bbr wscale:9,9 rto:201 rtt:0.011/0.006 ato:40 mss:22016 pmtu:65535 rcvmss:536 advmss:65483 cwnd:11 bytes_sent:15 bytes_acked:16 bytes_received:78549 segs_out:2623 segs_in:2622 data_segs_out:1 data_segs_in:2620 bbr:(bw:35.2Gbps,mrtt:0.005,pacing_gain:2.88672,cwnd_gain:2.88672) send 176Gbps lastsnd:32660929 lastrcv:9969 lastack:9969 pacing_rate 416Gbps delivery_rate 35.2Gbps delivered:2 app_limited rcv_rtt:86217.6 rcv_space:44197 rcv_ssthresh:43690 minrtt:0.005 snd_wnd:44032 rcv_wnd:44032                                                                                                                                                                                                              
ESTAB 0      0               10.100.100.4:nfs             10.100.100.7:852         
	 bbr wscale:12,9 rto:206 rtt:5.742/8.069 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:178 ssthresh:180 bytes_sent:2148420164 bytes_retrans:69776 bytes_acked:2148350388 bytes_received:10159709196 segs_out:4892268 segs_in:8673727 data_segs_out:2572049 data_segs_in:7294539 bbr:(bw:967Mbps,mrtt:0.239,pacing_gain:1.25,cwnd_gain:2) send 359Mbps lastsnd:65 lastrcv:65 lastack:63 pacing_rate 1.2Gbps delivery_rate 489Mbps delivered:2571733 busy:8015500ms retrans:0/319 dsack_dups:494 rcv_rtt:27.561 rcv_space:7819200 rcv_ssthresh:11141120 minrtt:0.116 rcv_ooopack:338257 snd_wnd:4440064 rcv_wnd:11141120 rehash:15                                                                                 
ESTAB 0      0               100.70.77.93:53816           100.70.77.93:2006        
	 bbr wscale:9,9 rto:201 rtt:0.011/0.006 ato:40 mss:22016 pmtu:65535 rcvmss:536 advmss:65483 cwnd:11 bytes_sent:15 bytes_acked:16 bytes_received:594 segs_out:94 segs_in:93 data_segs_out:1 data_segs_in:91 bbr:(bw:29.4Gbps,mrtt:0.006,pacing_gain:2.88672,cwnd_gain:2.88672) send 176Gbps lastsnd:32660929 lastrcv:271662 lastack:271662 pacing_rate 416Gbps delivery_rate 29.4Gbps delivered:2 app_limited rcv_space:43690 rcv_ssthresh:43690 minrtt:0.006 snd_wnd:44032 rcv_wnd:44032                                                                                                                                                                                                                                  
ESTAB 0      0               10.100.100.4:nfs             10.100.100.3:891         
	 bbr wscale:12,9 rto:212 rtt:11.206/14.357 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:1092 bytes_sent:117600064 bytes_retrans:7984 bytes_acked:117592080 bytes_received:1055415552 segs_out:594246 segs_in:986539 data_segs_out:288599 data_segs_in:774589 bbr:(bw:859Mbps,mrtt:1.423,pacing_gain:2.88672,cwnd_gain:2.88672) send 1.13Gbps lastsnd:4752 lastrcv:4752 lastack:4749 pacing_rate 2.45Gbps delivery_rate 859Mbps delivered:288599 app_limited busy:1126398ms retrans:0/44 dsack_dups:43 rcv_rtt:4.45 rcv_space:334776 rcv_ssthresh:669551 minrtt:0.825 rcv_ooopack:138 snd_wnd:1449984 rcv_wnd:669696                                                                                             
ESTAB 0      0               10.100.100.4:nfs             10.100.100.1:718         
	 bbr wscale:12,9 rto:217 rtt:16.024/18.686 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:64 ssthresh:178 bytes_sent:29504394196 bytes_retrans:7164578792 bytes_acked:22339815404 bytes_received:12879266344 segs_out:25333354 segs_in:16965918 data_segs_out:21585649 data_segs_in:9288840 bbr:(bw:145Mbps,mrtt:0.605,pacing_gain:1.25,cwnd_gain:2) send 46.3Mbps lastsnd:23 lastrcv:29 lastack:20 pacing_rate 180Mbps delivery_rate 136Mbps delivered:16637315 app_limited busy:13397678ms rwnd_limited:2ms(0.0%) retrans:0/4950668 dsack_dups:2316 reordering:179 reord_seen:215 rcv_rtt:23.044 rcv_space:3562896 rcv_ssthresh:7125791 minrtt:0.605 rcv_ooopack:9498 snd_wnd:8036352 rcv_wnd:7126016 rehash:153
ESTAB 0      0               10.100.100.4:nfs             10.100.100.7:692         
	 bbr wscale:12,9 rto:212 rtt:11.423/16.078 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:182 ssthresh:193 bytes_sent:2198920680 bytes_retrans:46792 bytes_acked:2198873888 bytes_received:10128686384 segs_out:4894303 segs_in:8672318 data_segs_out:2607446 data_segs_in:7273854 bbr:(bw:765Mbps,mrtt:0.319,pacing_gain:1.25,cwnd_gain:2) send 185Mbps lastsnd:66 lastrcv:64 lastack:64 pacing_rate 947Mbps delivery_rate 350Mbps delivered:2607166 app_limited busy:8039801ms retrans:0/276 dsack_dups:337 rcv_rtt:40.201 rcv_space:5319948 rcv_ssthresh:10639895 minrtt:0.193 rcv_ooopack:300078 snd_wnd:2813952 rcv_wnd:10640384 rehash:14                                                                   
ESTAB 0      0               10.100.100.4:nfs             10.100.100.3:752         
	 bbr wscale:12,9 rto:206 rtt:5.353/4.248 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:1173 bytes_sent:115757988 bytes_retrans:8156 bytes_acked:115749832 bytes_received:1051647840 segs_out:591801 segs_in:981467 data_segs_out:287345 data_segs_in:771983 bbr:(bw:963Mbps,mrtt:1.72,pacing_gain:2.88672,cwnd_gain:2.88672) send 2.54Gbps lastsnd:4142 lastrcv:4147 lastack:4139 pacing_rate 2.75Gbps delivery_rate 963Mbps delivered:287323 app_limited busy:1134060ms retrans:0/41 dsack_dups:51 rcv_rtt:4.162 rcv_space:277432 rcv_ssthresh:554863 minrtt:0.952 rcv_ooopack:208 snd_wnd:1011712 rcv_wnd:555008 rehash:2                                                                                      
ESTAB 0      0      [::ffff:100.70.77.93]:45876 [::ffff:100.107.35.78]:43954       
	 bbr wscale:11,9 rto:248 rtt:47.932/0.512 ato:40 mss:1228 pmtu:1280 rcvmss:688 advmss:1228 cwnd:24 bytes_sent:2537803 bytes_acked:2537803 bytes_received:345991 segs_out:20694 segs_in:18823 data_segs_out:6767 data_segs_in:7848 bbr:(bw:958kbps,mrtt:47.882,pacing_gain:2.88672,cwnd_gain:2.88672) send 4.92Mbps lastsnd:21439 lastrcv:21391 lastack:6059 pacing_rate 5.3Mbps delivery_rate 958kbps delivered:6768 app_limited busy:227621ms retrans:0/1 rcv_rtt:32775.9 rcv_space:65587 rcv_ssthresh:38912 minrtt:46.827 snd_wnd:555008 rcv_wnd:65024                                                                                                                                                                  

--- /proc/net/snmp (TCP summary)
    $ grep -A1 ^Tcp: /proc/net/snmp
Tcp: RtoAlgorithm RtoMin RtoMax MaxConn ActiveOpens PassiveOpens AttemptFails EstabResets CurrEstab InSegs OutSegs RetransSegs InErrs OutRsts InCsumErrors
Tcp: 1 200 120000 -1 6835 1363744 110 138 39 510827615 640752112 56080363 0 8581 0
Udp: InDatagrams NoPorts InErrors OutDatagrams RcvbufErrors SndbufErrors InCsumErrors IgnoredMulti MemErrors

--- TCP retrans stats
    $ grep -A1 ^Tcp: /proc/net/snmp
Tcp: RtoAlgorithm RtoMin RtoMax MaxConn ActiveOpens PassiveOpens AttemptFails EstabResets CurrEstab InSegs OutSegs RetransSegs InErrs OutRsts InCsumErrors
Tcp: 1 200 120000 -1 6835 1363744 110 138 39 510827615 640752112 56080363 0 8581 0
Udp: InDatagrams NoPorts InErrors OutDatagrams RcvbufErrors SndbufErrors InCsumErrors IgnoredMulti MemErrors

--- nstat TCP summary
    $ nstat -az Tcp_RetransSegs Tcp_InErrs Tcp_OutRsts Tcp_ActiveOpens Tcp_PassiveOpens
#kernel

###############################################################################
# 14. STORAGE: BLOCK DEVICES
###############################################################################

--- lsblk (key cols)
    $ lsblk -o NAME,SIZE,TYPE,MOUNTPOINT,FSTYPE,MODEL,SERIAL,STATE,ROTA,DISC-GRAN,DISC-MAX
NAME                           SIZE TYPE MOUNTPOINT    FSTYPE      MODEL                      SERIAL            STATE   ROTA DISC-GRAN DISC-MAX
sda                            1.8T disk                           Hitachi HDS723020BLA642    MN1220F30H4AND    running    1        0B       0B
└─sda1                         1.8T part /mnt/albert   ext4                                                                1        0B       0B
sdb                            1.8T disk /mnt/tsys4/D5 ext4        HITACHI HUA723020ALA640    YFJVEK7A          running    1        0B       0B
sdc                            2.7T disk                           WDC WD30EFRX-68EUZN0       WD-WCC4N3JUHH4F   running    1        0B       0B
└─sdc1                         2.7T part /mnt/tsys4/D2 ext4                                                                1        0B       0B
sdd                          931.5G disk                           WDC WD10EZRX-00A8LB0       WD-WMC1U9174429   running    1        0B       0B
├─sdd1                        1007K part                                                                                   1        0B       0B
├─sdd2                           1G part               vfat                                                                1        0B       0B
└─sdd3                       930.5G part               LVM2_member                                                         1        0B       0B
  ├─pve-swap                     8G lvm  [SWAP]        swap                                                     running    1        0B       0B
  ├─pve-root                    96G lvm  /             ext4                                                     running    1        0B       0B
  ├─pve-data_tmeta             8.1G lvm                                                                         running    1        0B       0B
  │ └─pve-data-tpool         794.3G lvm                                                                         running    1        0B       0B
  │   ├─pve-data             794.3G lvm                                                                         running    1        0B       0B
  │   └─pve-vm--400--disk--0    32G lvm                                                                         running    1       64K      64M
  └─pve-data_tdata           794.3G lvm                                                                         running    1        0B       0B
    └─pve-data-tpool         794.3G lvm                                                                         running    1        0B       0B
      ├─pve-data             794.3G lvm                                                                         running    1        0B       0B
      └─pve-vm--400--disk--0    32G lvm                                                                         running    1       64K      64M
sde                          476.9G disk                           SK hynix SC300B SATA 512GB EJ76N650710306R1N running    0        0B       0B
└─sde1                       476.9G part /mnt/tsys4/D3 ext4                                                                0        0B       0B
sdf                            4.5T disk                           WDC WD50NDZW-11MR8S1       WD-WX52D41RLK8F   running    1        4K       0B
└─sdf1                         4.5T part /mnt/backup   ext4                                                                1        4K       0B

--- lsblk -t
    $ lsblk -t
NAME                         ALIGNMENT MIN-IO   OPT-IO PHY-SEC LOG-SEC ROTA SCHED       RQ-SIZE    RA WSAME
sda                                  0    512        0     512     512    1 mq-deadline       2  8192    0B
└─sda1                               0    512        0     512     512    1 mq-deadline       2  8192    0B
sdb                                  0    512        0     512     512    1 mq-deadline       2  8192    0B
sdc                                  0   4096        0    4096     512    1 mq-deadline       2  8192    0B
└─sdc1                               0   4096        0    4096     512    1 mq-deadline       2  8192    0B
sdd                                  0   4096        0    4096     512    1 mq-deadline       2  8192    0B
├─sdd1                            3072   4096        0    4096     512    1 mq-deadline       2  8192    0B
├─sdd2                               0   4096        0    4096     512    1 mq-deadline       2  8192    0B
└─sdd3                               0   4096        0    4096     512    1 mq-deadline       2  8192    0B
  ├─pve-swap                         0   4096        0    4096     512    1                      8192    0B
  ├─pve-root                         0   4096        0    4096     512    1                      8192    0B
  ├─pve-data_tmeta                   0   4096        0    4096     512    1                      8192    0B
  │ └─pve-data-tpool                 0  65536    65536    4096     512    1                      8192    0B
  │   ├─pve-data                     0  65536    65536    4096     512    1                      8192    0B
  │   └─pve-vm--400--disk--0         0  65536    65536    4096     512    1                      8192    0B
  └─pve-data_tdata                   0   4096        0    4096     512    1                      8192    0B
    └─pve-data-tpool                 0  65536    65536    4096     512    1                      8192    0B
      ├─pve-data                     0  65536    65536    4096     512    1                      8192    0B
      └─pve-vm--400--disk--0         0  65536    65536    4096     512    1                      8192    0B
sde                                  0    512 33553920     512     512    0 mq-deadline      60 65532    0B
└─sde1                               0    512 33553920     512     512    0 mq-deadline      60 65532    0B
sdf                                  0   4096        0    4096     512    1 mq-deadline       2  4096    0B
└─sdf1                               0   4096        0    4096     512    1 mq-deadline       2  4096    0B

--- lsblk -O (everything, capped)
    $ lsblk -O
ALIGNMENT ID-LINK                                  ID                                   DISC-ALN DAX DISC-GRAN DISK-SEQ DISC-MAX DISC-ZERO FSAVAIL FSROOTS FSSIZE FSTYPE      FSUSED FSUSE% FSVER    GROUP HCTL       HOTPLUG KNAME LABEL LOG-SEC MAJ:MIN MAJ MIN MIN-IO MODE       MODEL                       MQ NAME                           OPT-IO OWNER PARTFLAGS PARTLABEL PARTN PARTTYPE                             PARTTYPENAME         PARTUUID                             PATH                             PHY-SEC PKNAME PTTYPE PTUUID                                  RA RAND      REV RM RO ROTA RQ-SIZE SCHED       SERIAL              SIZE   START STATE   SUBSYSTEMS         MOUNTPOINT    MOUNTPOINTS   TRAN TYPE UUID                                   VENDOR   WSAME WWN                ZONED ZONE-SZ ZONE-WGRAN ZONE-APP ZONE-NR ZONE-OMAX ZONE-AMAX
        0 wwn-0x5000cca369c6e1df                   0x5000cca369c6e1df                          0   0        0B        9       0B         0                                                           disk  0:0:0:0          0 sda             512   8:0   8   0      512 brw-rw---- Hitachi HDS723020BLA642      1 sda                                 0 root                                                                                                                           /dev/sda                             512        dos    7df370d5                              8192    1 MN6OA580  0  0    1       2 mq-deadline MN1220F30H4AND      1.8T         running block:scsi:pci                                 ata  disk                                        ATA         0B 0x5000cca369c6e1df none       0B         0B       0B       0         0         0
        0 wwn-0x5000cca369c6e1df-part1             0x5000cca369c6e1df-part1                    0   0        0B        9       0B         0    1.7T /         1.8T ext4            2M     0% 1.0      disk                   0 sda1            512   8:1   8   1      512 brw-rw----                              1 └─sda1                              0 root                          1 0x83                                 Linux                7df370d5-01                          /dev/sda1                            512 sda    dos    7df370d5                              8192    1           0  0    1       2 mq-deadline                     1.8T    2048         block:scsi:pci     /mnt/albert   /mnt/albert        part 0510ec81-11e5-412d-8a33-56ee3bf8e8f5               0B 0x5000cca369c6e1df none       0B         0B       0B       0         0         0
        0 wwn-0x5000cca223e8338b                   0x5000cca223e8338b                          0   0        0B       10       0B         0    1.5T /         1.8T ext4        209.1G    11% 1.0      disk  0:0:1:0          0 sdb             512   8:16  8   16     512 brw-rw---- HITACHI HUA723020ALA640      1 sdb                                 0 root                                                                                                                           /dev/sdb                             512                                                     8192    1 MK7ONS00  0  0    1       2 mq-deadline YFJVEK7A            1.8T         running block:scsi:pci     /mnt/tsys4/D5 /mnt/tsys4/D5 ata  disk 3898f700-297d-4a6b-a449-71ccf7b22047   ATA         0B 0x5000cca223e8338b none       0B         0B       0B       0         0         0
        0 wwn-0x50014ee20e225e1d                   0x50014ee20e225e1d                          0   0        0B       11       0B         0                                                           disk  1:0:0:0          0 sdc             512   8:32  8   32    4096 brw-rw---- WDC WD30EFRX-68EUZN0         1 sdc                                 0 root                                                                                                                           /dev/sdc                            4096        gpt    fb842831-6c68-11ea-af93-001c23c6347e  8192    1 82.00A82  0  0    1       2 mq-deadline WD-WCC4N3JUHH4F     2.7T         running block:scsi:pci                                 ata  disk                                        ATA         0B 0x50014ee20e225e1d none       0B         0B       0B       0         0         0
        0 wwn-0x50014ee20e225e1d-part1             0x50014ee20e225e1d-part1                    0   0        0B       11       0B         0    2.4T /         2.7T ext4        188.1G     7% 1.0      disk                   0 sdc1            512   8:33  8   33    4096 brw-rw----                              1 └─sdc1                              0 root                          1 0fc63daf-8483-4772-8e79-3d69d8477de4 Linux filesystem     9ec59a48-1030-4f42-b19b-5c7d4dd1aea7 /dev/sdc1                           4096 sdc    gpt    fb842831-6c68-11ea-af93-001c23c6347e  8192    1           0  0    1       2 mq-deadline                     2.7T    2048         block:scsi:pci     /mnt/tsys4/D2 /mnt/tsys4/D2      part 1bb5976a-a9b9-467d-bdc1-aecf3810590b               0B 0x50014ee20e225e1d none       0B         0B       0B       0         0         0
        0 wwn-0x50014ee25d49f2d7                   0x50014ee25d49f2d7                          0   0        0B       12       0B         0                                                           disk  1:0:1:0          0 sdd             512   8:48  8   48    4096 brw-rw---- WDC WD10EZRX-00A8LB0         1 sdd                                 0 root                                                                                                                           /dev/sdd                            4096        gpt    9105c713-b781-48da-a3bf-027455878851  8192    1 01.01A01  0  0    1       2 mq-deadline WD-WMC1U9174429   931.5G         running block:scsi:pci                                 ata  disk                                        ATA         0B 0x50014ee25d49f2d7 none       0B         0B       0B       0         0         0
     3072 wwn-0x50014ee25d49f2d7-part1             0x50014ee25d49f2d7-part1                    0   0        0B       12       0B         0                                                           disk                   0 sdd1            512   8:49  8   49    4096 brw-rw----                              1 ├─sdd1                              0 root                          1 21686148-6449-6e6f-744e-656564454649 BIOS boot            e4095617-ba64-49ad-b559-e172d6271cc2 /dev/sdd1                           4096 sdd    gpt    9105c713-b781-48da-a3bf-027455878851  8192    1           0  0    1       2 mq-deadline                    1007K      34         block:scsi:pci                                      part                                                    0B 0x50014ee25d49f2d7 none       0B         0B       0B       0         0         0
        0 wwn-0x50014ee25d49f2d7-part2             0x50014ee25d49f2d7-part2                    0   0        0B       12       0B         0                        vfat                      FAT32    disk                   0 sdd2            512   8:50  8   50    4096 brw-rw----                              1 ├─sdd2                              0 root                          2 c12a7328-f81f-11d2-ba4b-00a0c93ec93b EFI System           d05e0a67-4fdf-455f-a47e-bb86fe8508b0 /dev/sdd2                           4096 sdd    gpt    9105c713-b781-48da-a3bf-027455878851  8192    1           0  0    1       2 mq-deadline                       1G    2048         block:scsi:pci                                      part 0B43-A3C1                                          0B 0x50014ee25d49f2d7 none       0B         0B       0B       0         0         0
        0 wwn-0x50014ee25d49f2d7-part3             0x50014ee25d49f2d7-part3                    0   0        0B       12       0B         0                        LVM2_member               LVM2 001 disk                   0 sdd3            512   8:51  8   51    4096 brw-rw----                              1 └─sdd3                              0 root                          3 e6d6d379-f507-44c2-a23c-238f2a3df928 Linux LVM            318d51d7-692c-44bd-94f2-ae8634c84de1 /dev/sdd3                           4096 sdd    gpt    9105c713-b781-48da-a3bf-027455878851  8192    1           0  0    1       2 mq-deadline                   930.5G 2099200         block:scsi:pci                                      part gdYtuK-Msi6-pqoB-IY4X-za6e-2Dp1-MriYVA             0B 0x50014ee25d49f2d7 none       0B         0B       0B       0         0         0
        0 dm-name-pve-swap                         name-pve-swap                               0   0        0B       13       0B         0                        swap                      1        disk                   0 dm-0            512 252:0   252 0     4096 brw-rw----                              1   ├─pve-swap                        0 root                                                                                                                           /dev/mapper/pve-swap                4096 sdd3                                                8192    0           0  0    1                                           8G         running block              [SWAP]        [SWAP]             lvm  df0785c5-d395-43f5-aeab-0f74f50cf2b8               0B                    none       0B         0B       0B       0         0         0
        0 dm-name-pve-root                         name-pve-root                               0   0        0B       14       0B         0   78.9G /        93.9G ext4         10.2G    11% 1.0      disk                   0 dm-1            512 252:1   252 1     4096 brw-rw----                              1   ├─pve-root                        0 root                                                                                                                           /dev/mapper/pve-root                4096 sdd3                                                8192    0           0  0    1                                          96G         running block              /             /                  lvm  fe418106-acca-4171-8fba-1f4fa2c48260               0B                    none       0B         0B       0B       0         0         0
        0                                                                                      0   0        0B       15       0B         0                                                           disk                   0 dm-2            512 252:2   252 2     4096 brw-rw----                              1   ├─pve-data_tmeta                  0 root                                                                                                                           /dev/mapper/pve-data_tmeta          4096 sdd3                                                8192    0           0  0    1                                         8.1G         running block                                               lvm                                                     0B                    none       0B         0B       0B       0         0         0
        0                                                                                      0   0        0B       18       0B         0                                                           disk                   0 dm-4            512 252:4   252 4    65536 brw-rw----                              1   │ └─pve-data-tpool            65536 root                                                                                                                           /dev/mapper/pve-data-tpool          4096 dm-2                                                8192    0           0  0    1                                       794.3G         running block                                               lvm                                                     0B                    none       0B         0B       0B       0         0         0
        0                                                                                      0   0        0B       19       0B         0                                                           disk                   0 dm-5            512 252:5   252 5    65536 brw-rw----                              1   │   ├─pve-data                65536 root                                                                                                                           /dev/mapper/pve-data                4096 dm-4                                                8192    0           0  1    1                                       794.3G         running block                                               lvm                                                     0B                    none       0B         0B       0B       0         0         0
        0 dm-name-pve-vm--400--disk--0             name-pve-vm--400--disk--0                   0   0       64K       21      64M         0                                                           disk                   0 dm-6            512 252:6   252 6    65536 brw-rw----                              1   │   └─pve-vm--400--disk--0    65536 root                                                                                                                           /dev/mapper/pve-vm--400--disk--0    4096 dm-4   gpt    b4847a82-7c0b-4815-9650-c5568653da2d  8192    0           0  0    1                                          32G         running block                                               lvm                                                     0B                    none       0B         0B       0B       0         0         0
        0                                                                                      0   0        0B       16       0B         0                                                           disk                   0 dm-3            512 252:3   252 3     4096 brw-rw----                              1   └─pve-data_tdata                  0 root                                                                                                                           /dev/mapper/pve-data_tdata          4096 sdd3                                                8192    0           0  0    1                                       794.3G         running block                                               lvm                                                     0B                    none       0B         0B       0B       0         0         0
        0                                                                                      0   0        0B       18       0B         0                                                           disk                   0 dm-4            512 252:4   252 4    65536 brw-rw----                              1     └─pve-data-tpool            65536 root                                                                                                                           /dev/mapper/pve-data-tpool          4096 dm-3                                                8192    0           0  0    1                                       794.3G         running block                                               lvm                                                     0B                    none       0B         0B       0B       0         0         0
        0                                                                                      0   0        0B       19       0B         0                                                           disk                   0 dm-5            512 252:5   252 5    65536 brw-rw----                              1       ├─pve-data                65536 root                                                                                                                           /dev/mapper/pve-data                4096 dm-4                                                8192    0           0  1    1                                       794.3G         running block                                               lvm                                                     0B                    none       0B         0B       0B       0         0         0
        0 dm-name-pve-vm--400--disk--0             name-pve-vm--400--disk--0                   0   0       64K       21      64M         0                                                           disk                   0 dm-6            512 252:6   252 6    65536 brw-rw----                              1       └─pve-vm--400--disk--0    65536 root                                                                                                                           /dev/mapper/pve-vm--400--disk--0    4096 dm-4   gpt    b4847a82-7c0b-4815-9650-c5568653da2d  8192    0           0  0    1                                          32G         running block                                               lvm                                                     0B                    none       0B         0B       0B       0         0         0
        0 usb-SSD_ThinkPlus_AAAABBBB000C-0:0       SSD_ThinkPlus_AAAABBBB000C-0:0              0   0        0B       17       0B         0                                                           disk  2:0:0:0          1 sde             512   8:64  8   64     512 brw-rw---- SK hynix SC300B SATA 512GB   1 sde                          33553920 root                                                                                                                           /dev/sde                             512        gpt    41ce060d-9883-4aad-92ee-341bcbb44124 65532    0 20102P00  0  0    0      60 mq-deadline EJ76N650710306R1N 476.9G         running block:scsi:usb:pci                             usb  disk                                        SSD         0B                    none       0B         0B       0B       0         0         0
        0 usb-SSD_ThinkPlus_AAAABBBB000C-0:0-part1 SSD_ThinkPlus_AAAABBBB000C-0:0-part1        0   0        0B       17       0B         0  444.5G /       468.4G ext4            2M     0% 1.0      disk                   1 sde1            512   8:65  8   65     512 brw-rw----                              1 └─sde1                       33553920 root                          1 0fc63daf-8483-4772-8e79-3d69d8477de4 Linux filesystem     5f9bc49e-11d9-4e6f-853a-03ed3864a7d1 /dev/sde1                            512 sde    gpt    41ce060d-9883-4aad-92ee-341bcbb44124 65532    0           0  0    0      60 mq-deadline                   476.9G    2048         block:scsi:usb:pci /mnt/tsys4/D3 /mnt/tsys4/D3      part b53dcfc5-02f4-4b80-bf72-33feb8b03f09               0B                    none       0B         0B       0B       0         0         0
        0 wwn-0x50014ee2bf38011d                   0x50014ee2bf38011d                          0   0        4K       20       0B         0                                                           disk  3:0:0:0          1 sdf             512   8:80  8   80    4096 brw-rw---- WDC WD50NDZW-11MR8S1         1 sdf                                 0 root                                                                                                                           /dev/sdf                            4096        gpt    41a65ca1-39bc-40a3-af44-5cea1354952f  4096    1 02.01A02  0  0    1       2 mq-deadline WD-WX52D41RLK8F     4.5T         running block:scsi:usb:pci                             usb  disk                                        WD          0B 0x50014ee2bf38011d none       0B         0B       0B       0         0         0
        0 wwn-0x50014ee2bf38011d-part1             0x50014ee2bf38011d-part1                    0   0        4K       20       0B         0    4.3T /         4.5T ext4            2M     0% 1.0      disk                   1 sdf1            512   8:81  8   81    4096 brw-rw----                              1 └─sdf1                              0 root            easystore     1 ebd0a0a2-b9e5-4433-87c0-68b6b72699c7 Microsoft basic data afa5320c-682c-4c6a-8057-83cfab3fc015 /dev/sdf1                           4096 sdf    gpt    41a65ca1-39bc-40a3-af44-5cea1354952f  4096    1           0  0    1       2 mq-deadline                     4.5T    2048         block:scsi:usb:pci /mnt/backup   /mnt/backup        part 49bd1b9e-f31c-4f0a-9790-5b4b330c5708               0B 0x50014ee2bf38011d none       0B         0B       0B       0         0         0

--- blkid
    $ blkid
/dev/mapper/pve-root: UUID="fe418106-acca-4171-8fba-1f4fa2c48260" BLOCK_SIZE="4096" TYPE="ext4"
/dev/sdd2: UUID="0B43-A3C1" BLOCK_SIZE="512" TYPE="vfat" PARTUUID="d05e0a67-4fdf-455f-a47e-bb86fe8508b0"
/dev/sdd3: UUID="gdYtuK-Msi6-pqoB-IY4X-za6e-2Dp1-MriYVA" TYPE="LVM2_member" PARTUUID="318d51d7-692c-44bd-94f2-ae8634c84de1"
/dev/sdb: UUID="3898f700-297d-4a6b-a449-71ccf7b22047" BLOCK_SIZE="4096" TYPE="ext4"
/dev/mapper/pve-swap: UUID="df0785c5-d395-43f5-aeab-0f74f50cf2b8" TYPE="swap"
/dev/sde1: UUID="b53dcfc5-02f4-4b80-bf72-33feb8b03f09" BLOCK_SIZE="4096" TYPE="ext4" PARTUUID="5f9bc49e-11d9-4e6f-853a-03ed3864a7d1"
/dev/sdc1: UUID="1bb5976a-a9b9-467d-bdc1-aecf3810590b" BLOCK_SIZE="4096" TYPE="ext4" PARTUUID="9ec59a48-1030-4f42-b19b-5c7d4dd1aea7"
/dev/sda1: UUID="0510ec81-11e5-412d-8a33-56ee3bf8e8f5" BLOCK_SIZE="4096" TYPE="ext4" PARTUUID="7df370d5-01"
/dev/sdf1: UUID="49bd1b9e-f31c-4f0a-9790-5b4b330c5708" BLOCK_SIZE="4096" TYPE="ext4" PARTLABEL="easystore" PARTUUID="afa5320c-682c-4c6a-8057-83cfab3fc015"
/dev/sdd1: PARTUUID="e4095617-ba64-49ad-b559-e172d6271cc2"
/dev/mapper/pve-vm--400--disk--0: PTUUID="b4847a82-7c0b-4815-9650-c5568653da2d" PTTYPE="gpt"

--- /proc/partitions
    $ cat /proc/partitions
major minor  #blocks  name

   8        0 1953514584 sda
   8        1 1953513560 sda1
   8       16 1953514584 sdb
   8       32 2930266584 sdc
   8       33 2930265088 sdc1
   8       48  976762584 sdd
   8       49       1007 sdd1
   8       50    1048576 sdd2
   8       51  975712967 sdd3
 252        0    8388608 dm-0
 252        1  100663296 dm-1
 252        2    8495104 dm-2
 252        3  832888832 dm-3
   8       64  500107608 sde
   8       65  500106240 sde1
 252        4  832888832 dm-4
 252        5  832888832 dm-5
   8       80 4883737600 sdf
   8       81 4883735552 sdf1
 252        6   33554432 dm-6

--- fdisk -l
    $ fdisk -l
Disk /dev/sda: 1.82 TiB, 2000398934016 bytes, 3907029168 sectors
Disk model: Hitachi HDS72302
Units: sectors of 1 * 512 = 512 bytes
Sector size (logical/physical): 512 bytes / 512 bytes
I/O size (minimum/optimal): 512 bytes / 512 bytes
Disklabel type: dos
Disk identifier: 0x7df370d5

Device     Boot Start        End    Sectors  Size Id Type
/dev/sda1        2048 3907029167 3907027120  1.8T 83 Linux


Disk /dev/sdb: 1.82 TiB, 2000398934016 bytes, 3907029168 sectors
Disk model: HITACHI HUA72302
Units: sectors of 1 * 512 = 512 bytes
Sector size (logical/physical): 512 bytes / 512 bytes
I/O size (minimum/optimal): 512 bytes / 512 bytes


Disk /dev/sdc: 2.73 TiB, 3000592982016 bytes, 5860533168 sectors
Disk model: WDC WD30EFRX-68E
Units: sectors of 1 * 512 = 512 bytes
Sector size (logical/physical): 512 bytes / 4096 bytes
I/O size (minimum/optimal): 4096 bytes / 4096 bytes
Disklabel type: gpt
Disk identifier: FB842831-6C68-11EA-AF93-001C23C6347E

Device     Start        End    Sectors  Size Type
/dev/sdc1   2048 5860532223 5860530176  2.7T Linux filesystem


Disk /dev/sdd: 931.51 GiB, 1000204886016 bytes, 1953525168 sectors
Disk model: WDC WD10EZRX-00A
Units: sectors of 1 * 512 = 512 bytes
Sector size (logical/physical): 512 bytes / 4096 bytes
I/O size (minimum/optimal): 4096 bytes / 4096 bytes
Disklabel type: gpt
Disk identifier: 9105C713-B781-48DA-A3BF-027455878851

Device       Start        End    Sectors   Size Type
/dev/sdd1       34       2047       2014  1007K BIOS boot
/dev/sdd2     2048    2099199    2097152     1G EFI System
/dev/sdd3  2099200 1953525134 1951425935 930.5G Linux LVM

Partition 1 does not start on physical sector boundary.


Disk /dev/mapper/pve-swap: 8 GiB, 8589934592 bytes, 16777216 sectors
Units: sectors of 1 * 512 = 512 bytes
Sector size (logical/physical): 512 bytes / 4096 bytes
I/O size (minimum/optimal): 4096 bytes / 4096 bytes


Disk /dev/mapper/pve-root: 96 GiB, 103079215104 bytes, 201326592 sectors
Units: sectors of 1 * 512 = 512 bytes
Sector size (logical/physical): 512 bytes / 4096 bytes
I/O size (minimum/optimal): 4096 bytes / 4096 bytes


Disk /dev/sde: 476.94 GiB, 512110190592 bytes, 1000215216 sectors
Disk model: ThinkPlus       
Units: sectors of 1 * 512 = 512 bytes
Sector size (logical/physical): 512 bytes / 512 bytes
I/O size (minimum/optimal): 512 bytes / 33553920 bytes
Disklabel type: gpt
Disk identifier: 41CE060D-9883-4AAD-92EE-341BCBB44124

Device     Start        End    Sectors   Size Type
/dev/sde1   2048 1000214527 1000212480 476.9G Linux filesystem


Disk /dev/sdf: 4.55 TiB, 5000947302400 bytes, 9767475200 sectors
Disk model: easystore 2647  
Units: sectors of 1 * 512 = 512 bytes
Sector size (logical/physical): 512 bytes / 4096 bytes
I/O size (minimum/optimal): 4096 bytes / 4096 bytes
Disklabel type: gpt
Disk identifier: 41A65CA1-39BC-40A3-AF44-5CEA1354952F

Device     Start        End    Sectors  Size Type
/dev/sdf1   2048 9767473151 9767471104  4.5T Microsoft basic data


Disk /dev/mapper/pve-vm--400--disk--0: 32 GiB, 34359738368 bytes, 67108864 sectors
Units: sectors of 1 * 512 = 512 bytes
Sector size (logical/physical): 512 bytes / 4096 bytes
I/O size (minimum/optimal): 65536 bytes / 65536 bytes
Disklabel type: gpt
Disk identifier: B4847A82-7C0B-4815-9650-C5568653DA2D

Device                                   Start      End  Sectors  Size Type
/dev/mapper/pve-vm--400--disk--0-part1      34     2047     2014 1007K BIOS boot
/dev/mapper/pve-vm--400--disk--0-part2    2048  1050623  1048576  512M EFI System
/dev/mapper/pve-vm--400--disk--0-part3 1050624 67108830 66058207 31.5G Linux LVM

Partition 1 does not start on physical sector boundary.

--- parted -l
    $ parted -l
Warning: Not all of the space available to /dev/sdc appears to be used, you can
fix the GPT to use all of the space (an extra 7 blocks) or continue with the
current setting? 
Error: The backup GPT table is corrupt, but the primary appears OK, so that will
be used.
Warning: Not all of the space available to /dev/mapper/pve-data appears to be
used, you can fix the GPT to use all of the space (an extra 1598668800 blocks)
or continue with the current setting? 
Error: The backup GPT table is corrupt, but the primary appears OK, so that will
be used.
Warning: Not all of the space available to /dev/mapper/pve-data-tpool appears to
be used, you can fix the GPT to use all of the space (an extra 1598668800
blocks) or continue with the current setting? 
Error: The backup GPT table is corrupt, but the primary appears OK, so that will
be used.
Warning: Not all of the space available to /dev/mapper/pve-data_tdata appears to
be used, you can fix the GPT to use all of the space (an extra 1598668800
blocks) or continue with the current setting? 
Model: ATA Hitachi HDS72302 (scsi)
Disk /dev/sda: 2000GB
Sector size (logical/physical): 512B/512B
Partition Table: msdos
Disk Flags: 

Number  Start   End     Size    Type     File system  Flags
 1      1049kB  2000GB  2000GB  primary  ext4


Model: ATA HITACHI HUA72302 (scsi)
Disk /dev/sdb: 2000GB
Sector size (logical/physical): 512B/512B
Partition Table: loop
Disk Flags: 

Number  Start  End     Size    File system  Flags
 1      0.00B  2000GB  2000GB  ext4



                                                                          
Model: ATA WDC WD30EFRX-68E (scsi)
Disk /dev/sdc: 3001GB
Sector size (logical/physical): 512B/4096B
Partition Table: gpt
Disk Flags: 

Number  Start   End     Size    File system  Name  Flags
 1      1049kB  3001GB  3001GB  ext4


Model: ATA WDC WD10EZRX-00A (scsi)
Disk /dev/sdd: 1000GB
Sector size (logical/physical): 512B/4096B
Partition Table: gpt
Disk Flags: 

Number  Start   End     Size    File system  Name  Flags
 1      17.4kB  1049kB  1031kB                     bios_grub
 2      1049kB  1075MB  1074MB  fat32              boot, esp
 3      1075MB  1000GB  999GB                      lvm


Model: SSD ThinkPlus (scsi)
Disk /dev/sde: 512GB
Sector size (logical/physical): 512B/512B
Partition Table: gpt
Disk Flags: 

Number  Start   End    Size   File system  Name  Flags
 1      1049kB  512GB  512GB  ext4


Model: WD easystore 2647 (scsi)
Disk /dev/sdf: 5001GB
Sector size (logical/physical): 512B/4096B
Partition Table: gpt
Disk Flags: 

Number  Start   End     Size    File system  Name       Flags
 1      1049kB  5001GB  5001GB  ext4         easystore  msftdata


Model: Linux device-mapper (thin) (dm)
Disk /dev/mapper/pve-vm--400--disk--0: 34.4GB
Sector size (logical/physical): 512B/4096B
Partition Table: gpt
Disk Flags: 

Number  Start   End     Size    File system  Name  Flags
 1      17.4kB  1049kB  1031kB                     bios_grub
 2      1049kB  538MB   537MB   fat32              boot, esp
 3      538MB   34.4GB  33.8GB                     lvm



                                                                          

                                                                          
Model: Linux device-mapper (linear) (dm)
Disk /dev/mapper/pve-data: 853GB
Sector size (logical/physical): 512B/4096B
Partition Table: gpt
Disk Flags: 

Number  Start   End     Size    File system  Name  Flags
 1      17.4kB  1049kB  1031kB                     bios_grub
 2      1049kB  538MB   537MB                      boot, esp
 3      538MB   34.4GB  33.8GB                     lvm



                                                                          

                                                                          
Model: Linux device-mapper (thin-pool) (dm)
Disk /dev/mapper/pve-data-tpool: 853GB
Sector size (logical/physical): 512B/4096B
Partition Table: gpt
Disk Flags: 

Number  Start   End     Size    File system  Name  Flags
 1      17.4kB  1049kB  1031kB                     bios_grub
 2      1049kB  538MB   537MB                      boot, esp
 3      538MB   34.4GB  33.8GB                     lvm


Model: Linux device-mapper (linear) (dm)
Disk /dev/mapper/pve-root: 103GB
Sector size (logical/physical): 512B/4096B
Partition Table: loop
Disk Flags: 

Number  Start  End    Size   File system  Flags
 1      0.00B  103GB  103GB  ext4


Model: Linux device-mapper (linear) (dm)
Disk /dev/mapper/pve-swap: 8590MB
Sector size (logical/physical): 512B/4096B
Partition Table: loop
Disk Flags: 

Number  Start  End     Size    File system     Flags
 1      0.00B  8590MB  8590MB  linux-swap(v1)



                                                                          

                                                                          
Model: Linux device-mapper (linear) (dm)
Disk /dev/mapper/pve-data_tdata: 853GB
Sector size (logical/physical): 512B/4096B
Partition Table: gpt
Disk Flags: 

Number  Start   End     Size    File system  Name  Flags
 1      17.4kB  1049kB  1031kB                     bios_grub
 2      1049kB  538MB   537MB                      boot, esp
 3 Error: /dev/mapper/pve-data_tmeta: unrecognised disk label
     538MB   34.4GB  33.8GB                     lvm



                                                                          
Model: Linux device-mapper (linear) (dm)
Disk /dev/mapper/pve-data_tmeta: 8699MB
Sector size (logical/physical): 512B/4096B
Partition Table: unknown
Disk Flags: 


--- block device queue settings (per device)
    $ for d in $(ls /sys/block/ 2>/dev/null | grep -vE '^(loop|ram|md|dm-|sr|fd)'); do
    q="/sys/block/$d/queue"
    [ -d "$q" ] || continue
    printf '----- %s -----\n' "$d"
    for k in scheduler rotational nr_requests read_ahead_kb max_sectors_kb max_hw_sectors_kb \
             logical_block_size physical_block_size discard_granularity discard_max_hw_bytes \
             rq_affinity nomerges wbt_lat_usec write_cache stable_writes io_poll io_poll_delay \
             fua rot_stable_writes add_random zoned dma_alignment iostats;
    do
        f="$q/$k"
        [ -r "$f" ] && printf '  %-22s = %s\n' "$k" "$(cat "$f" 2>/dev/null)"
    done
    # NVMe-specific
    for f in /sys/block/$d/device/model /sys/block/$d/device/serial /sys/block/$d/device/transport /sys/block/$d/device/queue_count; do
        [ -r "$f" ] && printf '  %s = %s\n' "$(echo "$f" | sed "s|/sys/block/$d/device/||")" "$(cat "$f")"
    done
done
/root/check.sh: line 62: printf: --: invalid option
printf: usage: printf [-v var] format [arguments]
  scheduler              = none [mq-deadline] 
  rotational             = 1
  nr_requests            = 2
  read_ahead_kb          = 8192
  max_sectors_kb         = 4096
  max_hw_sectors_kb      = 32767
  logical_block_size     = 512
  physical_block_size    = 512
  discard_granularity    = 0
  discard_max_hw_bytes   = 0
  rq_affinity            = 1
  nomerges               = 0
  wbt_lat_usec           = 75000
  write_cache            = write back
  stable_writes          = 0
  io_poll                = 0
  io_poll_delay          = -1
  fua                    = 0
  add_random             = 1
  zoned                  = none
  dma_alignment          = 511
  iostats                = 1
  model = Hitachi HDS72302
/root/check.sh: line 62: printf: --: invalid option
printf: usage: printf [-v var] format [arguments]
  scheduler              = none [mq-deadline] 
  rotational             = 1
  nr_requests            = 2
  read_ahead_kb          = 8192
  max_sectors_kb         = 4096
  max_hw_sectors_kb      = 32767
  logical_block_size     = 512
  physical_block_size    = 512
  discard_granularity    = 0
  discard_max_hw_bytes   = 0
  rq_affinity            = 1
  nomerges               = 0
  wbt_lat_usec           = 75000
  write_cache            = write through
  stable_writes          = 0
  io_poll                = 0
  io_poll_delay          = -1
  fua                    = 0
  add_random             = 1
  zoned                  = none
  dma_alignment          = 511
  iostats                = 1
  model = HITACHI HUA72302
/root/check.sh: line 62: printf: --: invalid option
printf: usage: printf [-v var] format [arguments]
  scheduler              = none [mq-deadline] 
  rotational             = 1
  nr_requests            = 2
  read_ahead_kb          = 8192
  max_sectors_kb         = 4096
  max_hw_sectors_kb      = 32767
  logical_block_size     = 512
  physical_block_size    = 4096
  discard_granularity    = 0
  discard_max_hw_bytes   = 0
  rq_affinity            = 1
  nomerges               = 0
  wbt_lat_usec           = 75000
  write_cache            = write back
  stable_writes          = 0
  io_poll                = 0
  io_poll_delay          = -1
  fua                    = 0
  add_random             = 1
  zoned                  = none
  dma_alignment          = 511
  iostats                = 1
  model = WDC WD30EFRX-68E
/root/check.sh: line 62: printf: --: invalid option
printf: usage: printf [-v var] format [arguments]
  scheduler              = none [mq-deadline] 
  rotational             = 1
  nr_requests            = 2
  read_ahead_kb          = 8192
  max_sectors_kb         = 4096
  max_hw_sectors_kb      = 32767
  logical_block_size     = 512
  physical_block_size    = 4096
  discard_granularity    = 0
  discard_max_hw_bytes   = 0
  rq_affinity            = 1
  nomerges               = 0
  wbt_lat_usec           = 75000
  write_cache            = write back
  stable_writes          = 0
  io_poll                = 0
  io_poll_delay          = -1
  fua                    = 0
  add_random             = 1
  zoned                  = none
  dma_alignment          = 511
  iostats                = 1
  model = WDC WD10EZRX-00A
/root/check.sh: line 62: printf: --: invalid option
printf: usage: printf [-v var] format [arguments]
  scheduler              = none [mq-deadline] 
  rotational             = 0
  nr_requests            = 60
  read_ahead_kb          = 65532
  max_sectors_kb         = 512
  max_hw_sectors_kb      = 512
  logical_block_size     = 512
  physical_block_size    = 512
  discard_granularity    = 0
  discard_max_hw_bytes   = 0
  rq_affinity            = 1
  nomerges               = 0
  wbt_lat_usec           = 2000
  write_cache            = write back
  stable_writes          = 0
  io_poll                = 0
  io_poll_delay          = -1
  fua                    = 0
  add_random             = 0
  zoned                  = none
  dma_alignment          = 511
  iostats                = 1
  model = ThinkPlus       
/root/check.sh: line 62: printf: --: invalid option
printf: usage: printf [-v var] format [arguments]
  scheduler              = none [mq-deadline] 
  rotational             = 1
  nr_requests            = 2
  read_ahead_kb          = 4096
  max_sectors_kb         = 1024
  max_hw_sectors_kb      = 1024
  logical_block_size     = 512
  physical_block_size    = 4096
  discard_granularity    = 4096
  discard_max_hw_bytes   = 4294966784
  rq_affinity            = 1
  nomerges               = 0
  wbt_lat_usec           = 75000
  write_cache            = write through
  stable_writes          = 0
  io_poll                = 0
  io_poll_delay          = -1
  fua                    = 0
  add_random             = 1
  zoned                  = none
  dma_alignment          = 511
  iostats                = 1
  model = easystore 2647  
    [exit=1]

--- df -h (filesystem usage)
    $ df -h
Filesystem            Size  Used Avail Use% Mounted on
udev                  7.8G     0  7.8G   0% /dev
tmpfs                 1.6G  2.3M  1.6G   1% /run
/dev/mapper/pve-root   94G   11G   79G  12% /
tmpfs                 7.8G   34M  7.8G   1% /dev/shm
tmpfs                 1.0M     0  1.0M   0% /run/credentials/systemd-journald.service
tmpfs                 5.0M   28K  5.0M   1% /run/lock
/dev/sde1             469G  2.1M  445G   1% /mnt/tsys4/D3
tmpfs                 7.8G   28K  7.8G   1% /tmp
/dev/sdc1             2.7T  189G  2.4T   8% /mnt/tsys4/D2
/dev/sdb              1.8T  210G  1.5T  13% /mnt/tsys4/D5
/dev/sdf1             4.6T  2.1M  4.3T   1% /mnt/backup
/dev/fuse             128M   20K  128M   1% /etc/pve
tmpfs                 1.0M     0  1.0M   0% /run/credentials/getty@tty1.service
tmpfs                 1.6G  4.0K  1.6G   1% /run/user/0
/dev/sda1             1.8T  2.1M  1.7T   1% /mnt/albert

--- df -i (inode usage)
    $ df -i
Filesystem              Inodes IUsed     IFree IUse% Mounted on
udev                   2023292   799   2022493    1% /dev
tmpfs                  2035340  1313   2034027    1% /run
/dev/mapper/pve-root   6291456 78741   6212715    2% /
tmpfs                  2035340    79   2035261    1% /dev/shm
tmpfs                     1024     1      1023    1% /run/credentials/systemd-journald.service
tmpfs                  2035340    28   2035312    1% /run/lock
/dev/sde1             31260672    13  31260659    1% /mnt/tsys4/D3
tmpfs                  1048576    15   1048561    1% /tmp
/dev/sdc1            183148544    54 183148490    1% /mnt/tsys4/D2
/dev/sdb             122101760    56 122101704    1% /mnt/tsys4/D5
/dev/sdf1            152616960    12 152616948    1% /mnt/backup
/dev/fuse               262144    36    262108    1% /etc/pve
tmpfs                     1024     1      1023    1% /run/credentials/getty@tty1.service
tmpfs                   407068    26    407042    1% /run/user/0
/dev/sda1            122101760    12 122101748    1% /mnt/albert

###############################################################################
# 15. STORAGE: MOUNTS & FILESYSTEMS
###############################################################################

--- mount (filtered)
    $ mount
sysfs on /sys type sysfs (rw,nosuid,nodev,noexec,relatime)
proc on /proc type proc (rw,relatime)
udev on /dev type devtmpfs (rw,nosuid,relatime,size=8093168k,nr_inodes=2023292,mode=755,inode64)
devpts on /dev/pts type devpts (rw,nosuid,noexec,relatime,gid=5,mode=600,ptmxmode=000)
tmpfs on /run type tmpfs (rw,nosuid,nodev,noexec,relatime,size=1628272k,mode=755,inode64)
/dev/mapper/pve-root on / type ext4 (rw,relatime,errors=remount-ro)
securityfs on /sys/kernel/security type securityfs (rw,nosuid,nodev,noexec,relatime)
tmpfs on /dev/shm type tmpfs (rw,nosuid,nodev,inode64)
cgroup2 on /sys/fs/cgroup type cgroup2 (rw,nosuid,nodev,noexec,relatime)
none on /sys/fs/pstore type pstore (rw,nosuid,nodev,noexec,relatime)
bpf on /sys/fs/bpf type bpf (rw,nosuid,nodev,noexec,relatime,mode=700)
systemd-1 on /proc/sys/fs/binfmt_misc type autofs (rw,relatime,fd=37,pgrp=1,timeout=0,minproto=5,maxproto=5,direct,pipe_ino=10367)
tmpfs on /run/credentials/systemd-journald.service type tmpfs (ro,nosuid,nodev,noexec,relatime,nosymfollow,size=1024k,nr_inodes=1024,mode=700,inode64,noswap)
mqueue on /dev/mqueue type mqueue (rw,nosuid,nodev,noexec,relatime)
configfs on /sys/kernel/config type configfs (rw,nosuid,nodev,noexec,relatime)
debugfs on /sys/kernel/debug type debugfs (rw,nosuid,nodev,noexec,relatime)
tracefs on /sys/kernel/tracing type tracefs (rw,nosuid,nodev,noexec,relatime)
fusectl on /sys/fs/fuse/connections type fusectl (rw,nosuid,nodev,noexec,relatime)
hugetlbfs on /dev/hugepages type hugetlbfs (rw,nosuid,nodev,relatime,pagesize=2M)
tmpfs on /run/lock type tmpfs (rw,nosuid,nodev,noexec,relatime,size=5120k,inode64)
nfsd on /proc/fs/nfsd type nfsd (rw,relatime)
/dev/sde1 on /mnt/tsys4/D3 type ext4 (rw,relatime,errors=remount-ro,stripe=8191)
tmpfs on /tmp type tmpfs (rw,nosuid,nodev,nr_inodes=1048576,inode64)
/dev/sdc1 on /mnt/tsys4/D2 type ext4 (rw,relatime,errors=remount-ro)
/dev/sdb on /mnt/tsys4/D5 type ext4 (rw,relatime,errors=remount-ro,stripe=32)
/dev/sdf1 on /mnt/backup type ext4 (rw,relatime,errors=remount-ro)
binfmt_misc on /proc/sys/fs/binfmt_misc type binfmt_misc (rw,nosuid,nodev,noexec,relatime)
sunrpc on /run/rpc_pipefs type rpc_pipefs (rw,relatime)
lxcfs on /var/lib/lxcfs type fuse.lxcfs (rw,nosuid,nodev,relatime,user_id=0,group_id=0,allow_other)
/dev/fuse on /etc/pve type fuse (rw,nosuid,nodev,relatime,user_id=0,group_id=0,default_permissions,allow_other)
tmpfs on /run/credentials/getty@tty1.service type tmpfs (ro,nosuid,nodev,noexec,relatime,nosymfollow,size=1024k,nr_inodes=1024,mode=700,inode64,noswap)
tmpfs on /run/user/0 type tmpfs (rw,nosuid,nodev,relatime,size=1628272k,nr_inodes=407068,mode=700,inode64)
/dev/sda1 on /mnt/albert type ext4 (rw,relatime,errors=remount-ro)

--- findmnt (tree)
    $ findmnt -t nfs,nfs4,zfs,ext4,xfs,btrfs
TARGET          SOURCE               FSTYPE OPTIONS
/               /dev/mapper/pve-root ext4   rw,relatime,errors=remount-ro
├─/mnt/tsys4/D3 /dev/sde1            ext4   rw,relatime,errors=remount-ro,stripe=8191
├─/mnt/tsys4/D2 /dev/sdc1            ext4   rw,relatime,errors=remount-ro
├─/mnt/tsys4/D5 /dev/sdb             ext4   rw,relatime,errors=remount-ro,stripe=32
├─/mnt/backup   /dev/sdf1            ext4   rw,relatime,errors=remount-ro
└─/mnt/albert   /dev/sda1            ext4   rw,relatime,errors=remount-ro

--- /etc/fstab
    --- /etc/fstab ---
# <file system> <mount point> <type> <options> <dump> <pass>
/dev/pve/root / ext4 errors=remount-ro 0 1
/dev/pve/swap none swap sw 0 0
proc /proc proc defaults 0 0

### D1
# for later additon

### D2 /dev/sdc1: BLOCK_SIZE="4096" TYPE="ext4" PARTUUID="9ec59a48-1030-4f42-b19b-5c7d4dd1aea7"
UUID="1bb5976a-a9b9-467d-bdc1-aecf3810590b" /mnt/tsys4/D2 ext4 errors=remount-ro 0 1

### D3 /dev/sdd1: BLOCK_SIZE="4096" TYPE="ext4" PARTUUID="5f9bc49e-11d9-4e6f-853a-03ed3864a7d1"
### SSD drive on usb
UUID="b53dcfc5-02f4-4b80-bf72-33feb8b03f09"  /mnt/tsys4/D3 ext4 errors=remount-ro 0 1

### D4
# for later additon

### D5
#/dev/sdc: UUID="3898f700-297d-4a6b-a449-71ccf7b22047" BLOCK_SIZE="4096" TYPE="ext4"
UUID="3898f700-297d-4a6b-a449-71ccf7b22047" /mnt/tsys4/D5 ext4 errors=remount-ro 0 1

### D6 
# for later additon

### D7
# for later additon

### /mnt/backup
#Backuo /dev/sdf1: UUID="49bd1b9e-f31c-4f0a-9790-5b4b330c5708" BLOCK_SIZE="4096" TYPE="ext4" PARTLABEL="easystore" PARTUUID="afa5320c-682c-4c6a-8057-83cfab3fc015"
UUID="49bd1b9e-f31c-4f0a-9790-5b4b330c5708" /mnt/backup ext4 errors=remount-ro 0 1

### /mnt/albert
#/dev/sdf1: UUID="0510ec81-11e5-412d-8a33-56ee3bf8e8f5" BLOCK_SIZE="4096" TYPE="ext4" PARTUUID="7df370d5-01"
UUID="0510ec81-11e5-412d-8a33-56ee3bf8e8f5" /mnt/albert ext4 errors=remount-ro 0 1


--- ext4 reserved block % (per fs)
    $ for dev in $(awk '$3=="ext4"{print $1}' /proc/mounts 2>/dev/null); do
    echo "=== $dev ==="
    dumpe2fs -h "$dev" 2>/dev/null | grep -E 'Reserved|Block count|Free blocks|Block size|Mount count|Maximum mount|Last'
done
=== /dev/mapper/pve-root ===
Last mounted on:          /
Block count:              25165824
Reserved block count:     1258291
Free blocks:              21943872
Block size:               4096
Reserved GDT blocks:      1024
Last mount time:          Fri Jul 24 15:58:10 2026
Last write time:          Wed Jul 29 05:03:13 2026
Mount count:              33
Maximum mount count:      -1
Last checked:             Mon Feb 23 04:49:24 2026
Reserved blocks uid:      0 (user root)
Reserved blocks gid:      0 (group root)
=== /dev/sde1 ===
Last mounted on:          /mnt/tsys4/D3
Block count:              125026560
Reserved block count:     6251328
Free blocks:              122782942
Block size:               4096
Reserved GDT blocks:      1024
Last mount time:          Fri Jul 24 15:58:18 2026
Last write time:          Fri Jul 24 15:58:18 2026
Mount count:              23
Maximum mount count:      -1
Last checked:             Mon Feb 16 11:01:37 2026
Reserved blocks uid:      0 (user root)
Reserved blocks gid:      0 (group root)
=== /dev/sdc1 ===
Last mounted on:          /mnt/tsys4/D2
Block count:              732566272
Reserved block count:     36628313
Free blocks:              671473265
Block size:               4096
Reserved GDT blocks:      1024
Last mount time:          Fri Jul 24 15:58:18 2026
Last write time:          Wed Jul 29 04:58:43 2026
Mount count:              25
Maximum mount count:      -1
Last checked:             Mon Feb 23 18:17:29 2026
Reserved blocks uid:      0 (user root)
Reserved blocks gid:      0 (group root)
=== /dev/sdb ===
Last mounted on:          /mnt/tsys4/D5
Block count:              488378646
Reserved block count:     24418932
Free blocks:              425627496
Block size:               4096
Reserved GDT blocks:      1024
Last mount time:          Fri Jul 24 15:58:19 2026
Last write time:          Wed Jul 29 05:00:18 2026
Mount count:              26
Maximum mount count:      -1
Last checked:             Wed Feb 25 07:59:51 2026
Reserved blocks uid:      0 (user root)
Reserved blocks gid:      0 (group root)
=== /dev/sdf1 ===
Last mounted on:          <not available>
Block count:              1220933888
Reserved block count:     61046694
Free blocks:              1211022769
Block size:               4096
Reserved GDT blocks:      1024
Last mount time:          Fri Jul 24 15:58:59 2026
Last write time:          Fri Jul 24 15:58:59 2026
Mount count:              6
Maximum mount count:      -1
Last checked:             Sun Apr  5 10:41:36 2026
Reserved blocks uid:      0 (user root)
Reserved blocks gid:      0 (group root)
=== /dev/sda1 ===
Last mounted on:          <not available>
Block count:              488378390
Reserved block count:     24418919
Free blocks:              480430655
Block size:               4096
Reserved GDT blocks:      1024
Last mount time:          Fri Jul 24 22:48:32 2026
Last write time:          Fri Jul 24 22:48:32 2026
Mount count:              5
Maximum mount count:      -1
Last checked:             Fri Apr 24 08:31:43 2026
Reserved blocks uid:      0 (user root)
Reserved blocks gid:      0 (group root)

--- xfs info (per fs)
    $ for mp in $(awk '$3=="xfs"{print $2}' /proc/mounts 2>/dev/null); do
    echo "=== $mp ==="
    xfs_info "$mp" 2>/dev/null
done

###############################################################################
# 16. STORAGE: NFS (CLIENT + SERVER)
###############################################################################

--- nfsstat -m (mount options)
    $ nfsstat -m

--- nfsstat -c (client stats)
    $ nfsstat -c
Error: No Client Stats (/proc/net/rpc/nfs: No such file or directory). 
    [exit=2 / not installed or not permitted]

--- nfsstat -s (server stats)
    $ nfsstat -s
Server rpc stats:
calls      badcalls   badfmt     badauth    badclnt
28551145   0          0          0          0       

Server nfs v4:
null             compound         
21        0%     28559708 99%     

Server nfs v4 operations:
op0-unused       op1-unused       op2-future       access           close            
0         0%     0         0%     0         0%     3267      0%     866       0%     
commit           create           delegpurge       delegreturn      getattr          
1398239   1%     22        0%     0         0%     426       0%     6609930   7%     
getfh            link             lock             lockt            locku            
789       0%     0         0%     0         0%     0         0%     0         0%     
lookup           lookup_root      nverify          open             openattr         
732       0%     0         0%     0         0%     1422      0%     0         0%     
open_conf        open_dgrd        putfh            putpubfh         putrootfh        
0         0%     0         0%     28559004 31%     0         0%     127       0%     
read             readdir          readlink         remove           rename           
2818180   3%     1217      0%     0         0%     66        0%     6         0%     
renew            restorefh        savefh           secinfo          setattr          
0         0%     0         0%     6         0%     0         0%     120       0%     
setcltid         setcltidconf     verify           write            rellockowner     
0         0%     0         0%     0         0%     22786714 24%     0         0%     
bc_ctl           bind_conn        exchange_id      create_ses       destroy_ses      
0         0%     0         0%     44        0%     29        0%     19        0%     
free_stateid     getdirdeleg      getdevinfo       getdevlist       layoutcommit     
0         0%     217       0%     0         0%     0         0%     0         0%     
layoutget        layoutreturn     secinfononam     sequence         set_ssv          
0         0%     0         0%     61        0%     28559602 31%     0         0%     
test_stateid     want_deleg       destroy_clid     reclaim_comp     allocate         
0         0%     0         0%     14        0%     24        0%     38470     0%     
copy             copy_notify      deallocate       ioadvise         layouterror      
0         0%     0         0%     46309     0%     0         0%     0         0%     
layoutstats      offloadcancel    offloadstatus    readplus         seek             
0         0%     0         0%     0         0%     0         0%     614065    0%     
write_same       
0         0%     


--- nfsstat -234 (version stats)
    $ nfsstat -234
Server rpc stats:
calls      badcalls   badfmt     badauth    badclnt
28551145   0          0          0          0       

Server nfs v2:
null             getattr          setattr          root             lookup           
0         0%     0         0%     0         0%     0         0%     0         0%     
readlink         read             wrcache          write            create           
0         0%     0         0%     0         0%     0         0%     0         0%     
remove           rename           link             symlink          mkdir            
0         0%     0         0%     0         0%     0         0%     0         0%     
rmdir            readdir          fsstat           
0         0%     0         0%     0         0%     

Server nfs v3:
null             getattr          setattr          lookup           access           
0         0%     0         0%     0         0%     0         0%     0         0%     
readlink         read             write            create           mkdir            
0         0%     0         0%     0         0%     0         0%     0         0%     
symlink          mknod            remove           rmdir            rename           
0         0%     0         0%     0         0%     0         0%     0         0%     
link             readdir          readdirplus      fsstat           fsinfo           
0         0%     0         0%     0         0%     0         0%     0         0%     
pathconf         commit           
0         0%     0         0%     

Server nfs v4:
null             compound         
21        0%     28559708 99%     

Server nfs v4 operations:
op0-unused       op1-unused       op2-future       access           close            
0         0%     0         0%     0         0%     3267      0%     866       0%     
commit           create           delegpurge       delegreturn      getattr          
1398239   1%     22        0%     0         0%     426       0%     6609930   7%     
getfh            link             lock             lockt            locku            
789       0%     0         0%     0         0%     0         0%     0         0%     
lookup           lookup_root      nverify          open             openattr         
732       0%     0         0%     0         0%     1422      0%     0         0%     
open_conf        open_dgrd        putfh            putpubfh         putrootfh        
0         0%     0         0%     28559004 31%     0         0%     127       0%     
read             readdir          readlink         remove           rename           
2818180   3%     1217      0%     0         0%     66        0%     6         0%     
renew            restorefh        savefh           secinfo          setattr          
0         0%     0         0%     6         0%     0         0%     120       0%     
setcltid         setcltidconf     verify           write            rellockowner     
0         0%     0         0%     0         0%     22786714 24%     0         0%     
bc_ctl           bind_conn        exchange_id      create_ses       destroy_ses      
0         0%     0         0%     44        0%     29        0%     19        0%     
free_stateid     getdirdeleg      getdevinfo       getdevlist       layoutcommit     
0         0%     217       0%     0         0%     0         0%     0         0%     
layoutget        layoutreturn     secinfononam     sequence         set_ssv          
0         0%     0         0%     61        0%     28559602 31%     0         0%     
test_stateid     want_deleg       destroy_clid     reclaim_comp     allocate         
0         0%     0         0%     14        0%     24        0%     38470     0%     
copy             copy_notify      deallocate       ioadvise         layouterror      
0         0%     0         0%     46309     0%     0         0%     0         0%     
layoutstats      offloadcancel    offloadstatus    readplus         seek             
0         0%     0         0%     0         0%     0         0%     614065    0%     
write_same       
0         0%     


--- showmount -e (exports)
    $ showmount -e
clnt_create: RPC: Timed out
    [exit=1 / not installed or not permitted]

--- /proc/net/rpc/nfs
    $ cat /proc/net/rpc/nfs
cat: /proc/net/rpc/nfs: No such file or directory
    [exit=1 / not installed or not permitted]

--- /proc/net/rpc/nfsd
    $ cat /proc/net/rpc/nfsd
rc 0 0 28585575
fh 0 0 0 0 0
io 750033809968 415204622640
th 16 0 0.000 0.000 0.000 0.000 0.000 0.000 0.000 0.000 0.000 0.000
ra 0 0 0 0 0 0 0 0 0 0 0 0
net 28581838 0 28580354 58
rpc 28576979 0 0 0 0
proc3 22 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
proc4 2 21 28585554
proc4ops 76 0 0 0 3793 1056 1400349 22 0 440 6626311 789 0 0 0 0 732 0 0 1688 0 0 0 28584850 0 127 2818651 1450 0 66 6 0 0 6 0 121 0 0 0 22808207 0 0 0 44 29 19 0 253 0 0 0 0 0 61 28585448 0 0 0 14 24 38499 0 0 46338 0 0 0 0 0 0 614065 0 0 0 0 0 0
wdeleg_getattr 151

--- exports
    --- /etc/exports ---
/mnt/tsys4/D1 *(rw,no_root_squash)
/mnt/tsys4/D2 *(rw,no_root_squash)
/mnt/tsys4/D3 *(rw,no_root_squash)
#/mnt/tsys4/D4 *(rw,no_root_squash)
/mnt/tsys4/D5 *(rw,no_root_squash)
/mnt/tsys4/D7 *(rw,no_root_squash)
    [missing: /etc/exports.d/*.exports]

--- nfs.conf
    --- /etc/nfs.conf ---
#
# This is a general configuration for the
# NFS daemons and tools
#
[general]
pipefs-directory=/run/rpc_pipefs
#
[nfsrahead]
# nfs=15000
# nfs4=16000
#
[exports]
# rootdir=/export
#
[exportfs]
# debug=0
#
[gssd]
# verbosity=0
# rpc-verbosity=0
# use-memcache=0
# use-machine-creds=1
# use-gss-proxy=0
# avoid-dns=1
# limit-to-legacy-enctypes=0
# allowed-enctypes=aes256-cts-hmac-sha384-192,aes128-cts-hmac-sha256-128,camellia256-cts-cmac,camellia128-cts-cmac,aes256-cts-hmac-sha1-96,aes128-cts-hmac-sha1-96
# context-timeout=0
# rpc-timeout=5
# keytab-file=/etc/krb5.keytab
# cred-cache-directory=
# preferred-realm=
# set-home=1
# upcall-timeout=30
# cancel-timed-out-upcalls=0
#
[lockd]
# port=0
# udp-port=0
#
[exportd]
# debug="all|auth|call|general|parse"
# manage-gids=n
# state-directory-path=/var/lib/nfs
# threads=1
# cache-use-ipaddr=n
# ttl=1800
[mountd]
# debug="all|auth|call|general|parse"
manage-gids=y
# descriptors=0
# port=0
# threads=1
# reverse-lookup=n
# state-directory-path=/var/lib/nfs
# ha-callout=
# cache-use-ipaddr=n
# ttl=1800
#
[nfsdcld]
# debug=0
# storagedir=/var/lib/nfs/nfsdcld
#
[nfsd]
# debug=0
# threads=16
host=0.0.0.0
# port=0
# grace-time=90
# lease-time=90
# udp=n
# tcp=y
# vers3=y
# vers4=y
# vers4.0=y
# vers4.1=y
# vers4.2=y
# rdma=n
# rdma-port=20049

[statd]
# debug=0
# port=0
# outgoing-port=0
# name=
# state-directory-path=/var/lib/nfs/statd
# ha-callout=
# no-notify=0
#
[sm-notify]
# debug=0
# force=0
# retry-time=900
# outgoing-port=
# outgoing-addr=
# lift-grace=y
#
[svcgssd]
# principal=
    [missing: /etc/nfs.conf.d/*.conf]

--- nfs defaults
    --- /etc/default/nfs-kernel-server ---
# Runtime priority of server (see nice(1))
RPCNFSDPRIORITY=0

# Do you want to start the svcgssd daemon? It is only required for Kerberos
# exports. Valid alternatives are "yes" and "no"; the default is "no".
NEED_SVCGSSD=""
RPCNFSDCOUNT=64
    --- /etc/default/nfs-common ---
# If you do not set values for the NEED_ options, they will be attempted
# autodetected; this should be sufficient for most people. Valid alternatives
# for the NEED_ options are "yes" and "no".

# Do you want to start the statd daemon? It is not needed for NFSv4.
NEED_STATD=

# Do you want to start the idmapd daemon? It is only needed for NFSv4.
NEED_IDMAPD=

# Do you want to start the gssd daemon? It is required for Kerberos mounts.
NEED_GSSD=

--- idmapd.conf
    --- /etc/idmapd.conf ---
[General]

Verbosity = 0
# set your own domain here, if it differs from FQDN minus hostname
# Domain = localdomain

[Mapping]

Nobody-User = nobody
Nobody-Group = nogroup

--- pvesm status
    $ pvesm status
Name             Type     Status     Total (KiB)      Used (KiB) Available (KiB)        %
D3                dir     active       491133848            2080       466110072    0.00%
local             dir     active        98497780        10722188        82726044   10.89%
local-lvm     lvmthin     active       832888832        33565419       799323412    4.03%

--- pvesm list per storage
    $ for s in $(pvesm status 2>/dev/null | awk 'NR>1 && $3=="active"{print $1}'); do
    echo "--- storage: $s ---"
    pvesm list "$s" 2>/dev/null | head -n 30
    echo "--- pvesm config $s ---"
    pvesm config "$s" 2>/dev/null
done
--- storage: D3 ---
Volid Format  Type      Size VMID
--- pvesm config D3 ---
--- storage: local ---
Volid                                     Format  Type            Size VMID
local:iso/debian-13.3.0-amd64-netinst.iso iso     iso        790626304
local:iso/proxmox-backup-server_4.1-1.iso iso     iso       1514835968
local:iso/UCS_5.2-4-amd64.iso             iso     iso       1677721600
--- pvesm config local ---
--- storage: local-lvm ---
Volid                   Format  Type             Size VMID
local-lvm:vm-400-disk-0 raw     images    34359738368 400
--- pvesm config local-lvm ---
    [exit=255]

###############################################################################
# 17. STORAGE: LVM
###############################################################################

--- pvs
    $ pvs -v
  PV         VG  Fmt  Attr PSize    PFree  DevSize PV UUID                               
  /dev/sdd3  pve lvm2 a--  <930.51g 16.00g 930.51g gdYtuK-Msi6-pqoB-IY4X-za6e-2Dp1-MriYVA

--- vgs
    $ vgs -v
  VG  Attr   Ext   #PV #LV #SN VSize    VFree  VG UUID                                VProfile
  pve wz--n- 4.00m   1   4   0 <930.51g 16.00g 6CZe57-z0H0-2hDF-SPIV-cuTK-BENb-vXuZDF         

--- lvs
    $ lvs -o +lv_layout,role,pool_lv,data_percent,metadata_percent --units b
  LV            VG  Attr       LSize         Pool Origin Data%  Meta%  Move Log Cpy%Sync Convert Layout      Role       Pool Data%  Meta% 
  data          pve twi-aotz-- 852878163968B             4.03   0.34                             thin,pool   private         4.03   0.34  
  root          pve -wi-ao---- 103079215104B                                                     linear      public                       
  swap          pve -wi-ao----   8589934592B                                                     linear      public                       
  vm-400-disk-0 pve Vwi-aotz--  34359738368B data        99.98                                   thin,sparse public     data 99.98        

--- pvdisplay
    $ pvdisplay
  --- Physical volume ---
  PV Name               /dev/sdd3
  VG Name               pve
  PV Size               930.51 GiB / not usable 4.69 MiB
  Allocatable           yes 
  PE Size               4.00 MiB
  Total PE              238210
  Free PE               4096
  Allocated PE          234114
  PV UUID               gdYtuK-Msi6-pqoB-IY4X-za6e-2Dp1-MriYVA
   

--- vgdisplay
    $ vgdisplay
  --- Volume group ---
  VG Name               pve
  System ID             
  Format                lvm2
  Metadata Areas        1
  Metadata Sequence No  15
  VG Access             read/write
  VG Status             resizable
  MAX LV                0
  Cur LV                4
  Open LV               3
  Max PV                0
  Cur PV                1
  Act PV                1
  VG Size               <930.51 GiB
  PE Size               4.00 MiB
  Total PE              238210
  Alloc PE / Size       234114 / <914.51 GiB
  Free  PE / Size       4096 / 16.00 GiB
  VG UUID               6CZe57-z0H0-2hDF-SPIV-cuTK-BENb-vXuZDF
   

--- lvdisplay
    $ lvdisplay
  --- Logical volume ---
  LV Name                data
  VG Name                pve
  LV UUID                KAKIp7-1tUx-SBL4-nItm-CDfE-xAvY-hlDljD
  LV Write Access        read/write (activated read only)
  LV Creation host, time proxmox, 2026-02-23 04:45:41 -0600
  LV Pool metadata       data_tmeta
  LV Pool data           data_tdata
  LV Status              available
  # open                 0
  LV Size                794.30 GiB
  Allocated pool data    4.03%
  Allocated metadata     0.34%
  Current LE             203342
  Segments               1
  Allocation             inherit
  Read ahead sectors     auto
  - currently set to     16384
  Block device           252:5
   
  --- Logical volume ---
  LV Path                /dev/pve/swap
  LV Name                swap
  VG Name                pve
  LV UUID                V4WyMz-itd7-ssPF-OH67-hZBU-D7qV-tW8SX8
  LV Write Access        read/write
  LV Creation host, time proxmox, 2026-02-23 04:45:41 -0600
  LV Status              available
  # open                 1
  LV Size                8.00 GiB
  Current LE             2048
  Segments               1
  Allocation             inherit
  Read ahead sectors     auto
  - currently set to     16384
  Block device           252:0
   
  --- Logical volume ---
  LV Path                /dev/pve/root
  LV Name                root
  VG Name                pve
  LV UUID                Zv9Mnr-CsUh-5xFb-lAmQ-G1Gr-lGGo-zEaLhv
  LV Write Access        read/write
  LV Creation host, time proxmox, 2026-02-23 04:45:41 -0600
  LV Status              available
  # open                 1
  LV Size                96.00 GiB
  Current LE             24576
  Segments               1
  Allocation             inherit
  Read ahead sectors     auto
  - currently set to     16384
  Block device           252:1
   
  --- Logical volume ---
  LV Path                /dev/pve/vm-400-disk-0
  LV Name                vm-400-disk-0
  VG Name                pve
  LV UUID                GBky6X-Pk3G-6qjk-alPF-bJhQ-abpz-jtWmle
  LV Write Access        read/write
  LV Creation host, time pfv-tsys4, 2026-04-04 01:50:17 -0500
  LV Pool name           data
  LV Status              available
  # open                 1
  LV Size                32.00 GiB
  Mapped size            99.98%
  Current LE             8192
  Segments               1
  Allocation             inherit
  Read ahead sectors     auto
  - currently set to     16384
  Block device           252:6
   

--- lvm/lvm.conf (filters only)
    --- /etc/lvm/lvm.conf ---
# This is an example configuration file for the LVM2 system.
# It contains the default settings that would be used if there was no
# /etc/lvm/lvm.conf file.
#
# Refer to 'man lvm.conf' for further information including the file layout.
#
# Refer to 'man lvm.conf' for information about how settings configured in
# this file are combined with built-in values and command line options to
# arrive at the final values used by LVM.
#
# Refer to 'man lvmconfig' for information about displaying the built-in
# and configured values used by LVM.
#
# If a default value is set in this file (not commented out), then a
# new version of LVM using this file will continue using that value,
# even if the new version of LVM changes the built-in default value.
#
# To put this file in a different directory and override /etc/lvm set
# the environment variable LVM_SYSTEM_DIR before running the tools.
#
# N.B. Take care that each setting only appears once if uncommenting
# example settings in this file.


# Configuration section config.
# How LVM configuration settings are handled.
config {

	# Configuration option config/checks.
	# If enabled, any LVM configuration mismatch is reported.
	# This implies checking that the configuration key is understood by
	# LVM and that the value of the key is the proper type. If disabled,
	# any configuration mismatch is ignored and the default value is used
	# without any warning (a message about the configuration key not being
	# found is issued in verbose mode only).
	# This configuration option has an automatic default value.
	# checks = 1

	# Configuration option config/validate_metadata.
	# Allows to select the level of validation after metadata transformation.
	# Validation takes extra CPU time to verify internal consistency.
	# Accepted values:
	#   full
	#     Do a full metadata validation before disk write.
	#   none
	#     Skip any checks (unrecommended, slightly faster).
	#
	# This configuration option is advanced.
	# This configuration option has an automatic default value.
	# validate_metadata = "full"

	# Configuration option config/abort_on_errors.
	# Abort the LVM process if a configuration mismatch is found.
	# This configuration option has an automatic default value.
	# abort_on_errors = 0

	# Configuration option config/profile_dir.
	# Directory where LVM looks for configuration profiles.
	# This configuration option has an automatic default value.
	# profile_dir = "/etc/lvm/profile"
}

# Configuration section devices.
# How LVM uses block devices.
devices {

	# Configuration option devices/dir.
	# Directory in which to create volume group device nodes.
	# Commands also accept this as a prefix on volume group names.
	# This configuration option is advanced.
	# This configuration option has an automatic default value.
	# dir = "/dev"

	# Configuration option devices/scan.
	# Directories containing device nodes to use with LVM.
	# This configuration option is advanced.
	# This configuration option has an automatic default value.
	# scan = [ "/dev" ]

	# Configuration option devices/obtain_device_list_from_udev.
	# Obtain the list of available devices from udev.
	# This avoids opening or using any inapplicable non-block devices or
	# subdirectories found in the udev directory. Any device node or
	# symlink not managed by udev in the udev directory is ignored. This
	# setting applies only to the udev-managed device directory; other
	# directories will be scanned fully. LVM needs to be compiled with
	# udev support for this setting to apply.
	# This configuration option has an automatic default value.
	# obtain_device_list_from_udev = 0

	# Configuration option devices/external_device_info_source.
	# Enable device information from udev.
	# If set to "udev", lvm will supplement its own native device information
	# with information from libudev. This can potentially improve the detection
	# of MD component devices and multipath component devices.
	# This configuration option has an automatic default value.
	# external_device_info_source = "none"

	# Configuration option devices/hints.
	# Use a local file to remember which devices have PVs on them.
	# Some commands will use this as an optimization to reduce device
	# scanning, and will only scan the listed PVs. Removing the hint file
	# will cause lvm to generate a new one. Disable hints if PVs will
	# be copied onto devices using non-lvm commands, like dd.
	#
	# Accepted values:
	#   all
	#     Use all hints.
	#   none
	#     Use no hints.
	#
	# This configuration option has an automatic default value.
	# hints = "all"

	# Configuration option devices/preferred_names.
	# Select which path name to display for a block device.
	# If multiple path names exist for a block device, and LVM needs to
	# display a name for the device, the path names are matched against
	# each item in this list of regular expressions. The first match is
	# used. Try to avoid using undescriptive /dev/dm-N names, if present.
	# If no preferred name matches, or if preferred_names are not defined,
	# the following built-in preferences are applied in order until one
	# produces a preferred name:
	# Prefer names with path prefixes in the order of:
	# /dev/mapper, /dev/disk, /dev/dm-*, /dev/block.
	# Prefer the name with the least number of slashes.
	# Prefer a name that is a symlink.
	# Prefer the path with least value in lexicographical order.
	#
	# Example
	# preferred_names = [ "^/dev/mpath/", "^/dev/mapper/mpath", "^/dev/[hs]d" ]
	#
	# This configuration option does not have a default value defined.

	# Configuration option devices/use_devicesfile.
	# Enable or disable the use of a devices file.
	# When enabled, lvm will only use devices that
	# are listed in the devices file. A devices file will
	# be used, regardless of this setting, when the --devicesfile
	# option is set to a specific file name.
	# This configuration option has an automatic default value.
	# use_devicesfile = 0

	# Configuration option devices/devicesfile.
	# The name of the system devices file, listing devices that LVM should use.
	# This should not be used to select a non-system devices file.
	# The --devicesfile option is intended for alternative devices files.
	# This configuration option has an automatic default value.
	# devicesfile = "system.devices"

	# Configuration option devices/devicesfile_backup_limit.
	# The max number of backup files to keep in /etc/lvm/devices/backup.
	# LVM creates a backup of the devices file each time a new
	# version is created, or each time a modification is detected.
	# When the max number of backups is reached, the oldest are
	# removed to remain at the limit. Set to 0 to disable backups.
	# Only the system devices file is backed up.
	# This configuration option has an automatic default value.
	# devicesfile_backup_limit = 50

	# Configuration option devices/search_for_devnames.
	# Look outside of the devices file for missing devname entries.
	# A devname entry is used for a device that does not have a stable
	# device id, e.g. wwid, so the unstable device name is used as
	# the device id. After reboot, or if the device is reattached,
	# the device name may change, in which case lvm will not find
	# the expected PV on the device listed in the devices file.
	# This setting controls whether lvm will search other devices,
	# outside the devices file, to look for the missing PV on a
	# renamed device. If "none", lvm will not look at other devices,
	# and the PV may appear to be missing. If "auto", lvm will look
	# at other devices, but only those that are likely to have the PV.
	# If "all", lvm will look at all devices on the system.
	# This configuration option has an automatic default value.
	# search_for_devnames = "all"

	# Configuration option devices/device_ids_refresh.
	# Find PVs on new devices and update the device IDs in the devices file.
	# If PVs are restored or moved to a new system with new devices, but
	# an old system.devices remains with old device IDs, then search for
	# the PVIDs on new devices and update the device IDs in system.devices.
	# The original device IDs must also not be found on the new system.
	# See device_ids_refresh_check for conditions that trigger the refresh.
	# This configuration option has an automatic default value.
	# device_ids_refresh = 1

	# Configuration option devices/device_ids_refresh_checks.
	# Conditions that trigger device_ids_refresh to locate PVIDs on new devices.
	# product_uuid: refresh if /sys/devices/virtual/dmi/id/product_uuid does not
	# match the value saved in system.devices.
	# hostname: refresh if hostname does not match the value saved in system.devices.
	# (hostname is used if product_uuid is not available.)
	# Remove values from this list to prevent lvm from using them.
	# This configuration option has an automatic default value.
	# device_ids_refresh_checks = [ "product_uuid", "hostname" ]

	# Configuration option devices/filter.
	# Limit the block devices that are used by LVM commands.
	# This is a list of regular expressions used to accept or reject block
	# device path names. Each regex is delimited by a vertical bar '|'
	# (or any character) and is preceded by 'a' to accept the path, or
	# by 'r' to reject the path. The first regex in the list to match the
	# path is used, producing the 'a' or 'r' result for the device.
	# When multiple path names exist for a block device, if any path name
	# matches an 'a' pattern before an 'r' pattern, then the device is
	# accepted. If all the path names match an 'r' pattern first, then the
	# device is rejected. Unmatching path names do not affect the accept
	# or reject decision. If no path names for a device match a pattern,
	# then the device is accepted. Be careful mixing 'a' and 'r' patterns,
	# as the combination might produce unexpected results (test changes.)
	# Run vgscan after changing the filter to regenerate the cache.
	#
	# Example
	# Accept every block device:
	# filter = [ "a|.*|" ]
	# Reject the cdrom drive:
	# filter = [ "r|/dev/cdrom|" ]
	# Work with just loopback devices, e.g. for testing:
	# filter = [ "a|loop|", "r|.*|" ]
	# Accept all loop devices and ide drives except hdc:
	# filter = [ "a|loop|", "r|/dev/hdc|", "a|/dev/ide|", "r|.*|" ]
	# Use anchors to be very specific:
	# filter = [ "a|^/dev/hda8$|", "r|.*|" ]
	#
	# This configuration option has an automatic default value.
	# filter = [ "a|.*|" ]

	# Configuration option devices/global_filter.
	# Limit the block devices that are used by LVM system components.
	# Because devices/filter may be overridden from the command line, it is
	# not suitable for system-wide device filtering, e.g. udev.
	# Use global_filter to hide devices from these LVM system components.
	# The syntax is the same as devices/filter. Devices rejected by
	# global_filter are not opened by LVM.
	# This configuration option has an automatic default value.
	# global_filter = [ "a|.*|" ]

	# Configuration option devices/types.
	# List of additional acceptable block device types.
	# These are of device type names from /proc/devices, followed by the
	# maximum number of partitions.
	#
	# Example
	# types = [ "fd", 16 ]
	#
	# This configuration option is advanced.
	# This configuration option does not have a default value defined.

	# Configuration option devices/sysfs_scan.
	# Restrict device scanning to block devices appearing in sysfs.
	# This is a quick way of filtering out block devices that are not
	# present on the system. sysfs must be part of the kernel and mounted.)
	# This configuration option has an automatic default value.
	# sysfs_scan = 1

	# Configuration option devices/scan_lvs.
	# Allow LVM LVs to be used as PVs. When enabled, LVM commands will
	# scan active LVs to look for other PVs. Caution is required to
	# avoid using PVs that belong to guest images stored on LVs.
	# When enabled, the LVs scanned should be restricted using the
	# devices file or the filter. This option does not enable autoactivation
	# of layered VGs, which requires editing LVM udev rules (see LVM_PVSCAN_ON_LVS.)
	# This configuration option has an automatic default value.
	# scan_lvs = 0

	# Configuration option devices/multipath_component_detection.
	# Ignore devices that are components of DM multipath devices.
	# This configuration option has an automatic default value.
	# multipath_component_detection = 1

	# Configuration option devices/multipath_wwids_file.
	# The path to the multipath wwids file used for multipath component detection.
	# Set this to an empty string to disable the use of the multipath wwids file.
	# This configuration option has an automatic default value.
	# multipath_wwids_file = "/etc/multipath/wwids"

	# Configuration option devices/md_component_detection.
	# Enable detection and exclusion of MD component devices.
	# An MD component device is a block device that MD uses as part
	# of a software RAID virtual device. When an LVM PV is created
	# on an MD device, LVM must only use the top level MD device as
	# the PV, and should ignore the underlying component devices.
	# In cases where the MD superblock is located at the end of the
	# component devices, it is more difficult for LVM to consistently
	# identify an MD component, see the md_component_checks setting.
	# This configuration option has an automatic default value.
	# md_component_detection = 1

	# Configuration option devices/md_component_checks.
	# The checks LVM should use to detect MD component devices.
	# MD component devices are block devices used by MD software RAID.
	#
	# Accepted values:
	#   auto
	#     LVM will skip scanning the end of devices when it has other
	#     indications that the device is not an MD component.
	#   start
	#     LVM will only scan the start of devices for MD superblocks.
	#     This does not incur extra I/O by LVM.
	#   full

--- lvm.conf active filter
    $ grep -E '^\s*(filter|global_filter|use_devicesfile|obtain_device_list_from_udev)' /etc/lvm/lvm.conf 2>/dev/null
     global_filter=["r|/dev/zd.*|","r|/dev/rbd.*|"]

###############################################################################
# 18. STORAGE: MULTIPATH
###############################################################################

--- multipath -ll
    $ multipath -ll
/root/check.sh: line 45: multipath: command not found
    [exit=127 / not installed or not permitted]

--- multipath -v3 -ll (verbose, capped)
    $ multipath -v3 -ll
/root/check.sh: line 45: multipath: command not found
    [exit=127 / not installed or not permitted]

--- multipath.conf
    [missing: /etc/multipath.conf]

--- systemctl is-active multipathd
    $ systemctl is-active multipathd
inactive
    [exit=4 / not installed or not permitted]

###############################################################################
# 19. STORAGE: ZFS
###############################################################################

--- zfs version (userland)
    $ zfs version
zfs-2.4.0-pve1
zfs-kmod-2.4.0-pve1

--- zpool version
    $ zpool version
zfs-2.4.0-pve1
zfs-kmod-2.4.0-pve1

--- zpool list -v
    $ zpool list -v
no pools available

--- zpool status -v
    $ zpool status -v
no pools available

--- zpool key properties
    $ zpool get name,size,alloc,free,expandsize,fragmentation,capacity,health,ashift,autotrim,autoreplace,cachefile,comment,listsnapshots,multihost,version,bootfs,delegation,failmode,freeing,leaked,readonly

--- zfs per-dataset key properties
    $ zfs get -r -o name,property,value,source \
    compression,atime,recordsize,volblocksize,sync,primarycache,secondarycache,checksum,xattr,acltype,aclinherit,copies,logbias,refreservation,reservation,quota,used,avail,refer,mountpoint,mounted,canmount,relative_path,snapdir,version,primarycache,redundant_metadata,encryption 2>/dev/null
    [exit=2]

--- ARC stats
    $ cat /proc/spl/kstat/zfs/arcstats
21 1 0x01 147 39984 7487916394 393311362359697
name                            type data
hits                            4    0
iohits                          4    0
misses                          4    0
demand_data_hits                4    0
demand_data_iohits              4    0
demand_data_misses              4    0
demand_metadata_hits            4    0
demand_metadata_iohits          4    0
demand_metadata_misses          4    0
prefetch_data_hits              4    0
prefetch_data_iohits            4    0
prefetch_data_misses            4    0
prefetch_metadata_hits          4    0
prefetch_metadata_iohits        4    0
prefetch_metadata_misses        4    0
mru_hits                        4    0
mru_ghost_hits                  4    0
mfu_hits                        4    0
mfu_ghost_hits                  4    0
uncached_hits                   4    0
deleted                         4    0
mutex_miss                      4    0
access_skip                     4    0
evict_skip                      4    0
evict_not_enough                4    0
evict_l2_cached                 4    0
evict_l2_eligible               4    0
evict_l2_eligible_mfu           4    0
evict_l2_eligible_mru           4    0
evict_l2_ineligible             4    0
evict_l2_skip                   4    0
hash_elements                   4    0
hash_elements_max               4    0
hash_collisions                 4    0
hash_chains                     4    0
hash_chain_max                  4    0
meta                            4    1073741824
pd                              4    2147483648
pm                              4    2147483648
c                               4    521047040
c_min                           4    521047040
c_max                           4    1667235840
size                            4    1920
compressed_size                 4    0
uncompressed_size               4    0
overhead_size                   4    0
hdr_size                        4    1920
data_size                       4    0
metadata_size                   4    0
dbuf_size                       4    0
dnode_size                      4    0
bonus_size                      4    0
anon_size                       4    0
anon_data                       4    0
anon_metadata                   4    0
anon_evictable_data             4    0
anon_evictable_metadata         4    0
mru_size                        4    0
mru_data                        4    0
mru_metadata                    4    0
mru_evictable_data              4    0
mru_evictable_metadata          4    0
mru_ghost_size                  4    0
mru_ghost_data                  4    0
mru_ghost_metadata              4    0
mru_ghost_evictable_data        4    0
mru_ghost_evictable_metadata    4    0
mfu_size                        4    0
mfu_data                        4    0
mfu_metadata                    4    0
mfu_evictable_data              4    0
mfu_evictable_metadata          4    0
mfu_ghost_size                  4    0
mfu_ghost_data                  4    0
mfu_ghost_metadata              4    0
mfu_ghost_evictable_data        4    0
mfu_ghost_evictable_metadata    4    0
uncached_size                   4    0
uncached_data                   4    0
uncached_metadata               4    0
uncached_evictable_data         4    0
uncached_evictable_metadata     4    0
l2_hits                         4    0
l2_misses                       4    0
l2_prefetch_asize               4    0
l2_mru_asize                    4    0
l2_mfu_asize                    4    0
l2_bufc_data_asize              4    0
l2_bufc_metadata_asize          4    0
l2_feeds                        4    0
l2_rw_clash                     4    0
l2_read_bytes                   4    0
l2_write_bytes                  4    0
l2_writes_sent                  4    0
l2_writes_done                  4    0
l2_writes_error                 4    0
l2_writes_lock_retry            4    0
l2_evict_lock_retry             4    0
l2_evict_reading                4    0
l2_evict_l1cached               4    0
l2_free_on_write                4    0
l2_abort_lowmem                 4    0
l2_cksum_bad                    4    0
l2_io_error                     4    0
l2_size                         4    0
l2_asize                        4    0
l2_hdr_size                     4    0
l2_log_blk_writes               4    0
l2_log_blk_avg_asize            4    0
l2_log_blk_asize                4    0
l2_log_blk_count                4    0
l2_data_to_meta_ratio           4    0
l2_rebuild_success              4    0
l2_rebuild_unsupported          4    0
l2_rebuild_io_errors            4    0
l2_rebuild_dh_errors            4    0
l2_rebuild_cksum_lb_errors      4    0
l2_rebuild_lowmem               4    0
l2_rebuild_size                 4    0
l2_rebuild_asize                4    0
l2_rebuild_bufs                 4    0
l2_rebuild_bufs_precached       4    0
l2_rebuild_log_blks             4    0
memory_throttle_count           4    0
memory_direct_count             4    0
memory_indirect_count           4    0
memory_all_bytes                4    16673505280
memory_free_bytes               4    14355378176
memory_available_bytes          3    13710375936
arc_no_grow                     4    0
arc_tempreserve                 4    0
arc_loaned_bytes                4    0
arc_prune                       4    0
arc_meta_used                   4    1920
arc_dnode_limit                 4    166723584
async_upgrade_sync              4    0
predictive_prefetch             4    0
demand_hit_predictive_prefetch  4    0
demand_iohit_predictive_prefetch 4    0
prescient_prefetch              4    0
demand_hit_prescient_prefetch   4    0
demand_iohit_prescient_prefetch 4    0
arc_need_free                   4    0
arc_sys_free                    4    645002240
arc_raw_size                    4    0
cached_only_in_progress         4    0
abd_chunk_waste_size            4    0

--- dmu_tx
    $ cat /proc/spl/kstat/zfs/dmu_tx
17 1 0x01 13 3536 7486308075 393311363207696
name                            type data
dmu_tx_assigned                 4    0
dmu_tx_delay                    4    0
dmu_tx_error                    4    0
dmu_tx_suspended                4    0
dmu_tx_group                    4    0
dmu_tx_memory_reserve           4    0
dmu_tx_memory_reclaim           4    0
dmu_tx_dirty_throttle           4    0
dmu_tx_dirty_delay              4    0
dmu_tx_dirty_over_max           4    0
dmu_tx_dirty_frees_delay        4    0
dmu_tx_wrlog_delay              4    0
dmu_tx_quota                    4    0

--- zfetchstats
    $ cat /proc/spl/kstat/zfs/zfetchstats
16 1 0x01 8 2176 7486307541 393311364013984
name                            type data
hits                            4    0
future                          4    0
stride                          4    0
past                            4    0
misses                          4    0
max_streams                     4    0
io_issued                       4    0
io_active                       4    0

--- vdev_cache_stats
    $ cat /proc/spl/kstat/zfs/vdev_cache_stats
cat: /proc/spl/kstat/zfs/vdev_cache_stats: No such file or directory
    [exit=1 / not installed or not permitted]

--- abdstats
    $ cat /proc/spl/kstat/zfs/abdstats
14 1 0x01 20 5440 7486234986 393311365628453
name                            type data
struct_size                     4    96
linear_cnt                      4    0
linear_data_size                4    0
scatter_cnt                     4    1
scatter_data_size               4    4096
scatter_chunk_waste             4    0
scatter_order_0                 4    0
scatter_order_1                 4    0
scatter_order_2                 4    0
scatter_order_3                 4    0
scatter_order_4                 4    0
scatter_order_5                 4    0
scatter_order_6                 4    0
scatter_order_7                 4    0
scatter_order_8                 4    0
scatter_order_9                 4    0
scatter_page_multi_chunk        4    1
scatter_page_multi_zone         4    0
scatter_page_alloc_retry        4    0
scatter_sg_table_retry          4    0

--- ZFS module parameters (perf-relevant)
    $ for f in /sys/module/zfs/parameters/*; do
    [ -r "$f" ] || continue
    name="$(basename "$f")"
    case "$name" in
        zfs_arc_*|zfs_abd_*|zfs_dbuf_*|zfs_txg_*|zfs_vdev_*|zfs_sync_*|zfs_dirty_*|zfs_*io_*|zvol_*|l2arc_*|zfs_prefetch_*|zfs_*max_active|zfs_*_taskq*) ;;
        *) continue ;;
    esac
    printf '  %-50s = %s\n' "$name" "$(cat "$f")"
done
  l2arc_exclude_special                              = 0
  l2arc_feed_again                                   = 1
  l2arc_feed_min_ms                                  = 200
  l2arc_feed_secs                                    = 1
  l2arc_headroom                                     = 8
  l2arc_headroom_boost                               = 200
  l2arc_meta_percent                                 = 33
  l2arc_mfuonly                                      = 0
  l2arc_noprefetch                                   = 1
  l2arc_norw                                         = 0
  l2arc_rebuild_blocks_min_l2size                    = 1073741824
  l2arc_rebuild_enabled                              = 1
  l2arc_trim_ahead                                   = 0
  l2arc_write_boost                                  = 33554432
  l2arc_write_max                                    = 33554432
  zfs_abd_scatter_enabled                            = 1
  zfs_abd_scatter_max_order                          = 9
  zfs_abd_scatter_min_size                           = 1536
  zfs_arc_average_blocksize                          = 8192
  zfs_arc_dnode_limit                                = 0
  zfs_arc_dnode_limit_percent                        = 10
  zfs_arc_dnode_reduce_percent                       = 10
  zfs_arc_evict_batch_limit                          = 10
  zfs_arc_eviction_pct                               = 200
  zfs_arc_evict_threads                              = 3
  zfs_arc_grow_retry                                 = 0
  zfs_arc_lotsfree_percent                           = 10
  zfs_arc_max                                        = 1667235840
  zfs_arc_meta_balance                               = 500
  zfs_arc_min                                        = 0
  zfs_arc_min_prefetch_ms                            = 0
  zfs_arc_min_prescient_prefetch_ms                  = 0
  zfs_arc_pc_percent                                 = 0
  zfs_arc_prune_task_threads                         = 1
  zfs_arc_shrinker_limit                             = 0
  zfs_arc_shrinker_seeks                             = 2
  zfs_arc_shrink_shift                               = 0
  zfs_arc_sys_free                                   = 0
  zfs_dbuf_state_index                               = 0
  zfs_dio_enabled                                    = 1
  zfs_dio_strict                                     = 0
  zfs_dio_write_verify_events_per_second             = 20
  zfs_dirty_data_max                                 = 1667350528
  zfs_dirty_data_max_max                             = 4168376320
  zfs_dirty_data_max_max_percent                     = 25
  zfs_dirty_data_max_percent                         = 10
  zfs_dirty_data_sync_percent                        = 20
  zfs_prefetch_disable                               = 0
  zfs_slow_io_events_per_second                      = 20
  zfs_sync_pass_deferred_free                        = 2
  zfs_sync_pass_dont_compress                        = 8
  zfs_sync_pass_rewrite                              = 2
  zfs_txg_history                                    = 100
  zfs_txg_timeout                                    = 5
  zfs_vdev_aggregation_limit                         = 1048576
  zfs_vdev_aggregation_limit_non_rotating            = 131072
  zfs_vdev_async_read_max_active                     = 3
  zfs_vdev_async_read_min_active                     = 1
  zfs_vdev_async_write_active_max_dirty_percent      = 60
  zfs_vdev_async_write_active_min_dirty_percent      = 30
  zfs_vdev_async_write_max_active                    = 10
  zfs_vdev_async_write_min_active                    = 2
  zfs_vdev_default_ms_count                          = 200
  zfs_vdev_default_ms_shift                          = 29
  zfs_vdev_direct_write_verify                       = 1
  zfs_vdev_disk_max_segs                             = 0
  zfs_vdev_failfast_mask                             = 1
  zfs_vdev_initializing_max_active                   = 1
  zfs_vdev_initializing_min_active                   = 1
  zfs_vdev_max_active                                = 1000
  zfs_vdev_max_auto_ashift                           = 14
  zfs_vdev_max_ms_shift                              = 34
  zfs_vdev_min_auto_ashift                           = 9
  zfs_vdev_min_ms_count                              = 16
  zfs_vdev_mirror_non_rotating_inc                   = 0
  zfs_vdev_mirror_non_rotating_seek_inc              = 1
  zfs_vdev_mirror_rotating_inc                       = 0
  zfs_vdev_mirror_rotating_seek_inc                  = 5
  zfs_vdev_mirror_rotating_seek_offset               = 1048576
  zfs_vdev_ms_count_limit                            = 131072
  zfs_vdev_nia_credit                                = 5
  zfs_vdev_nia_delay                                 = 5
  zfs_vdev_open_timeout_ms                           = 1000
  zfs_vdev_raidz_impl                                = cycle [fastest] original scalar sse2 ssse3 avx2 
  zfs_vdev_read_gap_limit                            = 32768
  zfs_vdev_rebuild_max_active                        = 3
  zfs_vdev_rebuild_min_active                        = 1
  zfs_vdev_removal_max_active                        = 2
  zfs_vdev_removal_min_active                        = 1
  zfs_vdev_scrub_max_active                          = 3
  zfs_vdev_scrub_min_active                          = 1
  zfs_vdev_sync_read_max_active                      = 10
  zfs_vdev_sync_read_min_active                      = 10
  zfs_vdev_sync_write_max_active                     = 10
  zfs_vdev_sync_write_min_active                     = 10
  zfs_vdev_trim_max_active                           = 2
  zfs_vdev_trim_min_active                           = 1
  zfs_vdev_write_gap_limit                           = 4096
  zfs_zil_clean_taskq_maxalloc                       = 1048576
  zfs_zil_clean_taskq_minalloc                       = 1024
  zfs_zil_clean_taskq_nthr_pct                       = 100
  zvol_blk_mq_blocks_per_thread                      = 8
  zvol_blk_mq_queue_depth                            = 128
  zvol_enforce_quotas                                = 1
  zvol_inhibit_dev                                   = 0
  zvol_major                                         = 230
  zvol_max_discard_blocks                            = 16384
  zvol_num_taskqs                                    = 0
  zvol_open_timeout_ms                               = 1000
  zvol_prefetch_bytes                                = 131072
  zvol_request_sync                                  = 0
  zvol_threads                                       = 0
  zvol_use_blk_mq                                    = 0
  zvol_volmode                                       = 1

--- zpool iostat snapshot
    $ zpool iostat 1 1
no pools available

--- arc_summary (if present)
    $ arc_summary
/root/check.sh: line 45: arc_summary: command not found
    [exit=127 / not installed or not permitted]

--- zpool events -v (recent)
    $ zpool events -v
TIME                           CLASS

--- zpool history (last 30 events)
    $ zpool history -il 2>/dev/null | tail -n 30

###############################################################################
# 20. STORAGE: DRIVE HEALTH
###############################################################################

--- nvme list
    $ nvme list
/root/check.sh: line 45: nvme: command not found
    [exit=127 / not installed or not permitted]

--- nvme smart-log per device
    $ for n in /dev/nvme[0-9]*; do
    [ -b "$n" ] || continue
    echo "--- $n smart-log ---"
    nvme smart-log "$n" 2>&1
    echo "--- $n error-log (first 5) ---"
    nvme error-log "$n" 2>&1 | head -n 80
done

--- nvme id-ctrl per device (key fields)
    $ for n in /dev/nvme[0-9]*; do
    [ -b "$n" ] || continue
    echo "--- $n id-ctrl (filtered) ---"
    nvme id-ctrl "$n" 2>&1 | grep -E '^(mn|sn|fn|fr|tnvmcap|vid|IEEE|cntlid|ver|rab|lpa|elpe|npdg|mdts|hmpre|hmmin|cap|frmw|lba|ws|awun|awupf|acwu|apsta)'
done

--- smartctl -a per disk
    $ for d in $(ls /sys/block/ 2>/dev/null | grep -E '^(sd|vd)'); do
    dev="/dev/$d"
    [ -b "$dev" ] || continue
    echo "--- smartctl -a $dev ---"
    smartctl -a "$dev" 2>&1 | head -n 200
done
--- smartctl -a /dev/sda ---
smartctl 7.4 2024-10-15 r5620 [x86_64-linux-6.17.9-1-pve] (local build)
Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Hitachi Deskstar 7K3000
Device Model:     Hitachi HDS723020BLA642
Serial Number:    MN1220F30H4AND
LU WWN Device Id: 5 000cca 369c6e1df
Firmware Version: MN6OA580
User Capacity:    2,000,398,934,016 bytes [2.00 TB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    7200 rpm
Form Factor:      3.5 inches
Device is:        In smartctl database 7.3/5528
ATA Version is:   ATA8-ACS T13/1699-D revision 4
SATA Version is:  SATA 2.6, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Wed Jul 29 05:13:19 2026 CDT
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(19381) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 ( 323) minutes.
SCT capabilities: 	       (0x003d)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAG     VALUE WORST THRESH TYPE      UPDATED  WHEN_FAILED RAW_VALUE
  1 Raw_Read_Error_Rate     0x000b   100   100   016    Pre-fail  Always       -       0
  2 Throughput_Performance  0x0005   131   131   054    Pre-fail  Offline      -       97
  3 Spin_Up_Time            0x0007   155   155   024    Pre-fail  Always       -       362 (Average 377)
  4 Start_Stop_Count        0x0012   087   087   000    Old_age   Always       -       52372
  5 Reallocated_Sector_Ct   0x0033   100   100   005    Pre-fail  Always       -       0
  7 Seek_Error_Rate         0x000b   100   100   067    Pre-fail  Always       -       0
  8 Seek_Time_Performance   0x0005   133   133   020    Pre-fail  Offline      -       27
  9 Power_On_Hours          0x0012   090   090   000    Old_age   Always       -       74278
 10 Spin_Retry_Count        0x0013   100   100   060    Pre-fail  Always       -       0
 12 Power_Cycle_Count       0x0032   097   097   000    Old_age   Always       -       13303
192 Power-Off_Retract_Count 0x0032   057   057   000    Old_age   Always       -       52478
193 Load_Cycle_Count        0x0012   057   057   000    Old_age   Always       -       52478
194 Temperature_Celsius     0x0002   166   166   000    Old_age   Always       -       36 (Min/Max 20/57)
196 Reallocated_Event_Count 0x0032   100   100   000    Old_age   Always       -       0
197 Current_Pending_Sector  0x0022   100   100   000    Old_age   Always       -       0
198 Offline_Uncorrectable   0x0008   100   100   000    Old_age   Offline      -       0
199 UDMA_CRC_Error_Count    0x000a   200   200   000    Old_age   Always       -       0

SMART Error Log Version: 1
No Errors Logged

SMART Self-test log structure revision number 1
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Extended offline    Completed without error       00%      6263         -
# 2  Short offline       Completed without error       00%      6257         -
# 3  Extended offline    Completed without error       00%      6257         -
# 4  Selective offline   Completed without error       00%      6252         -
# 5  Short offline       Completed without error       00%     23404         -

SMART Selective self-test log data structure revision number 1
 SPAN     MIN_LBA     MAX_LBA  CURRENT_TEST_STATUS
    1           0    23441578  Not_testing
    2   970896897   994338475  Not_testing
    3  1941793794  1965235372  Not_testing
    4  2912690691  2936132269  Not_testing
    5  3883587589  3907029167  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

The above only provides legacy SMART information - try 'smartctl -x' for more

--- smartctl -a /dev/sdb ---
smartctl 7.4 2024-10-15 r5620 [x86_64-linux-6.17.9-1-pve] (local build)
Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Device Model:     HITACHI HUA723020ALA640
Serial Number:    YFJVEK7A
LU WWN Device Id: 5 000cca 223e8338b
Firmware Version: MK7ONS00
User Capacity:    2,000,398,934,016 bytes [2.00 TB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    7200 rpm
Form Factor:      3.5 inches
Device is:        Not in smartctl database 7.3/5528
ATA Version is:   ATA8-ACS T13/1699-D revision 4
SATA Version is:  SATA 2.6, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Wed Jul 29 05:13:21 2026 CDT
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(20946) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 ( 349) minutes.
SCT capabilities: 	       (0x003d)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAG     VALUE WORST THRESH TYPE      UPDATED  WHEN_FAILED RAW_VALUE
  1 Raw_Read_Error_Rate     0x000b   100   100   016    Pre-fail  Always       -       0
  2 Throughput_Performance  0x0005   100   100   054    Pre-fail  Offline      -       0
  3 Spin_Up_Time            0x0007   201   201   024    Pre-fail  Always       -       302 (Average 318)
  4 Start_Stop_Count        0x0012   100   100   000    Old_age   Always       -       434
  5 Reallocated_Sector_Ct   0x0033   100   100   005    Pre-fail  Always       -       0
  7 Seek_Error_Rate         0x000b   100   100   067    Pre-fail  Always       -       0
  8 Seek_Time_Performance   0x0005   100   100   020    Pre-fail  Offline      -       0
  9 Power_On_Hours          0x0012   089   089   000    Old_age   Always       -       80856
 10 Spin_Retry_Count        0x0013   100   100   060    Pre-fail  Always       -       0
 12 Power_Cycle_Count       0x0032   100   100   000    Old_age   Always       -       288
192 Power-Off_Retract_Count 0x0032   099   099   000    Old_age   Always       -       1719
193 Load_Cycle_Count        0x0012   099   099   000    Old_age   Always       -       1719
194 Temperature_Celsius     0x0002   133   133   000    Old_age   Always       -       45 (Min/Max 18/56)
196 Reallocated_Event_Count 0x0032   100   100   000    Old_age   Always       -       0
197 Current_Pending_Sector  0x0022   100   100   000    Old_age   Always       -       0
198 Offline_Uncorrectable   0x0008   100   100   000    Old_age   Offline      -       0
199 UDMA_CRC_Error_Count    0x000a   200   200   000    Old_age   Always       -       6

SMART Error Log Version: 1
ATA Error Count: 6 (device log contains only the most recent five errors)
	CR = Command Register [HEX]
	FR = Features Register [HEX]
	SC = Sector Count Register [HEX]
	SN = Sector Number Register [HEX]
	CL = Cylinder Low Register [HEX]
	CH = Cylinder High Register [HEX]
	DH = Device/Head Register [HEX]
	DC = Device Command Register [HEX]
	ER = Error register [HEX]
	ST = Status register [HEX]
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 6 occurred at disk power-on lifetime: 32366 hours (1348 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  84 51 80 00 5e 00 02  Error: ICRC, ABRT at LBA = 0x02005e00 = 33578496

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  61 80 00 00 5e 00 40 00      00:03:56.692  WRITE FPDMA QUEUED
  61 80 08 80 5d 00 40 00      00:03:56.691  WRITE FPDMA QUEUED
  61 80 00 00 5d 00 40 00      00:03:56.690  WRITE FPDMA QUEUED
  61 80 08 80 5c 00 40 00      00:03:56.690  WRITE FPDMA QUEUED
  61 80 00 00 5c 00 40 00      00:03:56.689  WRITE FPDMA QUEUED

Error 5 occurred at disk power-on lifetime: 32366 hours (1348 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  84 51 67 19 5e 00 02  Error: ICRC, ABRT at LBA = 0x02005e19 = 33578521

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  61 80 00 00 5e 00 40 00      00:03:56.692  WRITE FPDMA QUEUED
  61 80 08 80 5d 00 40 00      00:03:56.691  WRITE FPDMA QUEUED
  61 80 00 00 5d 00 40 00      00:03:56.690  WRITE FPDMA QUEUED
  61 80 08 80 5c 00 40 00      00:03:56.690  WRITE FPDMA QUEUED
  61 80 00 00 5c 00 40 00      00:03:56.689  WRITE FPDMA QUEUED

Error 4 occurred at disk power-on lifetime: 32354 hours (1348 days + 2 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  84 51 80 00 5d a9 0a  Error: ICRC, ABRT at LBA = 0x0aa95d00 = 178871552

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  61 80 10 80 5f a9 40 00      00:36:15.997  WRITE FPDMA QUEUED
  61 80 00 00 5f a9 40 00      00:36:15.997  WRITE FPDMA QUEUED
  61 80 30 80 5e a9 40 00      00:36:15.996  WRITE FPDMA QUEUED
  61 80 28 00 5e a9 40 00      00:36:15.996  WRITE FPDMA QUEUED
  61 80 08 80 5d a9 40 00      00:36:15.995  WRITE FPDMA QUEUED

Error 3 occurred at disk power-on lifetime: 32354 hours (1348 days + 2 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  84 51 7d 03 5d a9 0a  Error: ICRC, ABRT at LBA = 0x0aa95d03 = 178871555

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  61 80 10 80 5f a9 40 00      00:36:15.997  WRITE FPDMA QUEUED
  61 80 00 00 5f a9 40 00      00:36:15.997  WRITE FPDMA QUEUED
  61 80 30 80 5e a9 40 00      00:36:15.996  WRITE FPDMA QUEUED
  61 80 28 00 5e a9 40 00      00:36:15.996  WRITE FPDMA QUEUED
  61 80 08 80 5d a9 40 00      00:36:15.995  WRITE FPDMA QUEUED

Error 2 occurred at disk power-on lifetime: 32354 hours (1348 days + 2 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  84 51 80 80 a7 e5 07  Error: ICRC, ABRT at LBA = 0x07e5a780 = 132491136

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  61 80 18 00 a9 e5 40 00      00:31:45.204  WRITE FPDMA QUEUED
  61 80 10 80 a8 e5 40 00      00:31:45.203  WRITE FPDMA QUEUED
  61 80 00 00 a8 e5 40 00      00:31:45.203  WRITE FPDMA QUEUED
  61 80 08 80 a7 e5 40 00      00:31:45.202  WRITE FPDMA QUEUED
  61 80 20 00 a7 e5 40 00      00:31:45.202  WRITE FPDMA QUEUED

SMART Self-test log structure revision number 1
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%     32091         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

The above only provides legacy SMART information - try 'smartctl -x' for more

--- smartctl -a /dev/sdc ---
smartctl 7.4 2024-10-15 r5620 [x86_64-linux-6.17.9-1-pve] (local build)
Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Western Digital Red
Device Model:     WDC WD30EFRX-68EUZN0
Serial Number:    WD-WCC4N3JUHH4F
LU WWN Device Id: 5 0014ee 20e225e1d
Firmware Version: 82.00A82
User Capacity:    3,000,592,982,016 bytes [3.00 TB]
Sector Sizes:     512 bytes logical, 4096 bytes physical
Rotation Rate:    5400 rpm
Device is:        In smartctl database 7.3/5528
ATA Version is:   ACS-2 (minor revision not indicated)
SATA Version is:  SATA 3.0, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Wed Jul 29 05:13:22 2026 CDT
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x84)	Offline data collection activity
					was suspended by an interrupting command from host.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(39360) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 ( 395) minutes.
Conveyance self-test routine
recommended polling time: 	 (   5) minutes.
SCT capabilities: 	       (0x703d)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAG     VALUE WORST THRESH TYPE      UPDATED  WHEN_FAILED RAW_VALUE
  1 Raw_Read_Error_Rate     0x002f   200   200   051    Pre-fail  Always       -       0
  3 Spin_Up_Time            0x0027   190   179   021    Pre-fail  Always       -       5483
  4 Start_Stop_Count        0x0032   100   100   000    Old_age   Always       -       312
  5 Reallocated_Sector_Ct   0x0033   200   200   140    Pre-fail  Always       -       0
  7 Seek_Error_Rate         0x002e   200   200   000    Old_age   Always       -       0
  9 Power_On_Hours          0x0032   024   024   000    Old_age   Always       -       55504
 10 Spin_Retry_Count        0x0032   100   100   000    Old_age   Always       -       0
 11 Calibration_Retry_Count 0x0032   100   100   000    Old_age   Always       -       0
 12 Power_Cycle_Count       0x0032   100   100   000    Old_age   Always       -       257
192 Power-Off_Retract_Count 0x0032   200   200   000    Old_age   Always       -       191
193 Load_Cycle_Count        0x0032   180   180   000    Old_age   Always       -       62348
194 Temperature_Celsius     0x0022   114   090   000    Old_age   Always       -       36
196 Reallocated_Event_Count 0x0032   200   200   000    Old_age   Always       -       0
197 Current_Pending_Sector  0x0032   200   200   000    Old_age   Always       -       0
198 Offline_Uncorrectable   0x0030   200   200   000    Old_age   Offline      -       0
199 UDMA_CRC_Error_Count    0x0032   200   200   000    Old_age   Always       -       1
200 Multi_Zone_Error_Rate   0x0008   200   200   000    Old_age   Offline      -       0

SMART Error Log Version: 1
No Errors Logged

SMART Self-test log structure revision number 1
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%      1626         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

The above only provides legacy SMART information - try 'smartctl -x' for more

--- smartctl -a /dev/sdd ---
smartctl 7.4 2024-10-15 r5620 [x86_64-linux-6.17.9-1-pve] (local build)
Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Western Digital Green
Device Model:     WDC WD10EZRX-00A8LB0
Serial Number:    WD-WMC1U9174429
LU WWN Device Id: 5 0014ee 25d49f2d7
Firmware Version: 01.01A01
User Capacity:    1,000,204,886,016 bytes [1.00 TB]
Sector Sizes:     512 bytes logical, 4096 bytes physical
Device is:        In smartctl database 7.3/5528
ATA Version is:   ATA8-ACS (minor revision not indicated)
SATA Version is:  SATA 3.0, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Wed Jul 29 05:13:22 2026 CDT
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x84)	Offline data collection activity
					was suspended by an interrupting command from host.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(12360) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 ( 142) minutes.
Conveyance self-test routine
recommended polling time: 	 (   5) minutes.
SCT capabilities: 	       (0x30b5)	SCT Status supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAG     VALUE WORST THRESH TYPE      UPDATED  WHEN_FAILED RAW_VALUE
  1 Raw_Read_Error_Rate     0x002f   200   200   051    Pre-fail  Always       -       0
  3 Spin_Up_Time            0x0027   141   127   021    Pre-fail  Always       -       3950
  4 Start_Stop_Count        0x0032   100   100   000    Old_age   Always       -       724
  5 Reallocated_Sector_Ct   0x0033   200   200   140    Pre-fail  Always       -       0
  7 Seek_Error_Rate         0x002e   200   200   000    Old_age   Always       -       0
  9 Power_On_Hours          0x0032   001   001   000    Old_age   Always       -       82253
 10 Spin_Retry_Count        0x0032   100   100   000    Old_age   Always       -       0
 11 Calibration_Retry_Count 0x0032   100   100   000    Old_age   Always       -       0
 12 Power_Cycle_Count       0x0032   100   100   000    Old_age   Always       -       720
192 Power-Off_Retract_Count 0x0032   199   199   000    Old_age   Always       -       1408
193 Load_Cycle_Count        0x0032   121   121   000    Old_age   Always       -       237800
194 Temperature_Celsius     0x0022   108   078   000    Old_age   Always       -       35
196 Reallocated_Event_Count 0x0032   200   200   000    Old_age   Always       -       0
197 Current_Pending_Sector  0x0032   200   200   000    Old_age   Always       -       0
198 Offline_Uncorrectable   0x0030   200   200   000    Old_age   Offline      -       0
199 UDMA_CRC_Error_Count    0x0032   200   200   000    Old_age   Always       -       0
200 Multi_Zone_Error_Rate   0x0008   200   200   000    Old_age   Offline      -       0

SMART Error Log Version: 1
No Errors Logged

SMART Self-test log structure revision number 1
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

The above only provides legacy SMART information - try 'smartctl -x' for more

--- smartctl -a /dev/sde ---
smartctl 7.4 2024-10-15 r5620 [x86_64-linux-6.17.9-1-pve] (local build)
Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Device Model:     SK hynix SC300B SATA 512GB
Serial Number:    EJ76N650710306R1N
Firmware Version: 20102P00
User Capacity:    512,110,190,592 bytes [512 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
Form Factor:      2.5 inches
TRIM Command:     Available
Device is:        Not in smartctl database 7.3/5528
ATA Version is:   ATA8-ACS (minor revision not indicated)
SATA Version is:  SATA 3.1, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Wed Jul 29 05:13:23 2026 CDT
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x02)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(    7) seconds.
Offline data collection
capabilities: 			 (0x19) SMART execute Offline immediate.
					No Auto Offline data collection support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					No Selective Self-test supported.
SMART capabilities:            (0x0002)	Does not save SMART data before
					entering power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 (  60) minutes.

SMART Attributes Data Structure revision number: 0
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAG     VALUE WORST THRESH TYPE      UPDATED  WHEN_FAILED RAW_VALUE
  1 Raw_Read_Error_Rate     0x000f   166   166   006    Pre-fail  Always       -       0
  5 Reallocated_Sector_Ct   0x0032   253   253   036    Old_age   Always       -       0
  9 Power_On_Hours          0x0032   079   079   000    Old_age   Always       -       19011
 12 Power_Cycle_Count       0x0032   100   100   020    Old_age   Always       -       789
100 Unknown_Attribute       0x0032   100   100   000    Old_age   Always       -       13150021
171 Unknown_Attribute       0x0032   253   253   000    Old_age   Always       -       0
172 Unknown_Attribute       0x0032   253   253   000    Old_age   Always       -       0
174 Unknown_Attribute       0x0030   100   100   000    Old_age   Offline      -       93
175 Program_Fail_Count_Chip 0x0032   253   253   000    Old_age   Always       -       0
176 Erase_Fail_Count_Chip   0x0032   253   253   000    Old_age   Always       -       0
177 Wear_Leveling_Count     0x0032   097   097   000    Old_age   Always       -       100
178 Used_Rsvd_Blk_Cnt_Chip  0x0032   100   100   000    Old_age   Always       -       19
179 Used_Rsvd_Blk_Cnt_Tot   0x0032   100   100   000    Old_age   Always       -       117
180 Unused_Rsvd_Blk_Cnt_Tot 0x0032   100   100   000    Old_age   Always       -       8715
181 Program_Fail_Cnt_Total  0x0032   253   253   000    Old_age   Always       -       0
182 Erase_Fail_Count_Total  0x0032   253   253   000    Old_age   Always       -       0
183 Runtime_Bad_Block       0x0032   253   253   000    Old_age   Always       -       0
187 Reported_Uncorrect      0x0032   253   253   000    Old_age   Always       -       0
188 Command_Timeout         0x0032   253   253   000    Old_age   Always       -       0
191 Unknown_SSD_Attribute   0x0032   253   253   000    Old_age   Always       -       0
194 Temperature_Celsius     0x0002   025   000   000    Old_age   Always       -       25 (Min/Max 7/51)
195 Hardware_ECC_Recovered  0x0032   253   253   000    Old_age   Always       -       0
201 Unknown_SSD_Attribute   0x000e   100   100   000    Old_age   Always       -       0
204 Soft_ECC_Correction     0x000e   100   099   000    Old_age   Always       -       19
231 Unknown_SSD_Attribute   0x0033   253   253   010    Pre-fail  Always       -       0
234 Unknown_Attribute       0x0032   100   100   000    Old_age   Always       -       51681
241 Total_LBAs_Written      0x0032   100   100   000    Old_age   Always       -       7340
242 Total_LBAs_Read         0x0032   100   100   000    Old_age   Always       -       8823
250 Read_Error_Retry_Rate   0x0032   100   100   000    Old_age   Always       -       198354

SMART Error Log Version: 1
ATA Error Count: 162 (device log contains only the most recent five errors)
	CR = Command Register [HEX]
	FR = Features Register [HEX]
	SC = Sector Count Register [HEX]
	SN = Sector Number Register [HEX]
	CL = Cylinder Low Register [HEX]
	CH = Cylinder High Register [HEX]
	DH = Device/Head Register [HEX]
	DC = Device Command Register [HEX]
	ER = Error register [HEX]
	ST = Status register [HEX]
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 162 occurred at disk power-on lifetime: 15175 hours (632 days + 7 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 00 00 a7 8d 00  Error: UNC at LBA = 0x008da700 = 9283328

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 03 08 00 a7 8d 40 40      18:05:13.330  READ DMA EXT
  ef 03 46 00 a7 8d 00 00      18:05:13.330  SET FEATURES [Set transfer mode]
  ef 03 0c 00 a7 8d 00 00      18:05:13.330  SET FEATURES [Set transfer mode]
  ec 08 00 00 a7 8d 00 00      18:05:13.330  IDENTIFY DEVICE
  60 08 00 00 a7 8d 40 40      18:05:13.300  READ FPDMA QUEUED

Error 161 occurred at disk power-on lifetime: 15175 hours (632 days + 7 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 41 00 00 00 00 00  Error: UNC at LBA = 0x00000000 = 0

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  60 08 00 00 a7 8d 40 40      18:05:13.300  READ FPDMA QUEUED
  60 08 00 c0 a7 8d 40 40      18:05:13.300  READ FPDMA QUEUED
  60 08 00 f8 a6 8d 40 40      18:05:13.300  READ FPDMA QUEUED
  60 08 00 f8 a7 8d 40 40      18:05:13.300  READ FPDMA QUEUED
  60 08 00 f0 a7 8d 40 40      18:05:13.300  READ FPDMA QUEUED

Error 160 occurred at disk power-on lifetime: 15175 hours (632 days + 7 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 00 00 a7 8d 00  Error: UNC at LBA = 0x008da700 = 9283328

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 03 08 00 a7 8d 40 40      18:05:12.170  READ DMA EXT
  ef 03 46 00 a7 8d 00 00      18:05:12.170  SET FEATURES [Set transfer mode]
  ef 03 0c 00 a7 8d 00 00      18:05:12.170  SET FEATURES [Set transfer mode]
  ec 08 00 00 a7 8d 00 00      18:05:12.170  IDENTIFY DEVICE
  60 08 00 00 a7 8d 40 40      18:05:11.380  READ FPDMA QUEUED

Error 159 occurred at disk power-on lifetime: 15175 hours (632 days + 7 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 41 00 00 00 00 00  Error: UNC at LBA = 0x00000000 = 0

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  60 08 00 00 a7 8d 40 40      18:05:11.380  READ FPDMA QUEUED
  60 08 00 08 b0 11 40 40      18:05:11.380  READ FPDMA QUEUED
  60 08 00 f0 a6 8d 40 40      18:05:11.380  READ FPDMA QUEUED
  60 08 00 80 a6 8d 40 40      18:05:11.380  READ FPDMA QUEUED
  60 08 00 00 b0 11 40 40      18:05:11.380  READ FPDMA QUEUED

Error 158 occurred at disk power-on lifetime: 15175 hours (632 days + 7 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 00 00 a7 8d 00  Error: UNC at LBA = 0x008da700 = 9283328

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 03 04 00 a7 8d 40 40      18:04:55.590  READ DMA EXT
  ef 03 46 00 a7 8d 00 00      18:04:55.580  SET FEATURES [Set transfer mode]
  ef 03 0c 00 a7 8d 00 00      18:04:55.580  SET FEATURES [Set transfer mode]
  ec 04 00 00 a7 8d 00 00      18:04:55.580  IDENTIFY DEVICE
  60 04 00 00 a7 8d 40 40      18:04:55.540  READ FPDMA QUEUED

SMART Self-test log structure revision number 1
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%      5470         -
# 2  Short offline       Completed without error       00%        95         -
# 3  Short offline       Completed without error       00%        94         -
# 4  Short offline       Completed without error       00%        90         -
# 5  Short offline       Completed without error       00%        90         -
# 6  Short offline       Completed without error       00%        89         -
# 7  Short offline       Completed without error       00%        71         -
# 8  Short offline       Completed without error       00%        70         -
# 9  Short offline       Completed without error       00%         2         -

Selective Self-tests/Logging not supported

The above only provides legacy SMART information - try 'smartctl -x' for more

--- smartctl -a /dev/sdf ---
smartctl 7.4 2024-10-15 r5620 [x86_64-linux-6.17.9-1-pve] (local build)
Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Western Digital Elements / My Passport (USB, AF)
Device Model:     WDC WD50NDZW-11MR8S1
Serial Number:    WD-WX52D41RLK8F
LU WWN Device Id: 5 0014ee 2bf38011d
Firmware Version: 02.01A02
User Capacity:    5,000,947,523,584 bytes [5.00 TB]
Sector Sizes:     512 bytes logical, 4096 bytes physical
Rotation Rate:    5400 rpm
Form Factor:      2.5 inches
TRIM Command:     Available, deterministic
Device is:        In smartctl database 7.3/5528
ATA Version is:   ACS-3 (minor revision not indicated)
SATA Version is:  SATA 3.1, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Wed Jul 29 05:13:23 2026 CDT
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  360) seconds.
Offline data collection
capabilities: 			 (0x1b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					No Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (  11) minutes.
SCT capabilities: 	       (0x30b5)	SCT Status supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAG     VALUE WORST THRESH TYPE      UPDATED  WHEN_FAILED RAW_VALUE
  1 Raw_Read_Error_Rate     0x002f   100   253   051    Pre-fail  Always       -       0
  3 Spin_Up_Time            0x0027   253   253   021    Pre-fail  Always       -       2883
  4 Start_Stop_Count        0x0032   071   071   000    Old_age   Always       -       29033
  5 Reallocated_Sector_Ct   0x0033   200   200   140    Pre-fail  Always       -       0
  7 Seek_Error_Rate         0x002e   200   200   000    Old_age   Always       -       0
  9 Power_On_Hours          0x0032   071   071   000    Old_age   Always       -       21296
 10 Spin_Retry_Count        0x0032   100   100   000    Old_age   Always       -       0
 11 Calibration_Retry_Count 0x0032   100   253   000    Old_age   Always       -       0
 12 Power_Cycle_Count       0x0032   100   100   000    Old_age   Always       -       66
192 Power-Off_Retract_Count 0x0032   200   200   000    Old_age   Always       -       29
193 Load_Cycle_Count        0x0032   181   181   000    Old_age   Always       -       58234
194 Temperature_Celsius     0x0022   123   106   000    Old_age   Always       -       29
196 Reallocated_Event_Count 0x0032   200   200   000    Old_age   Always       -       0
197 Current_Pending_Sector  0x0032   200   200   000    Old_age   Always       -       0
198 Offline_Uncorrectable   0x0030   100   253   000    Old_age   Offline      -       0
199 UDMA_CRC_Error_Count    0x0032   200   200   000    Old_age   Always       -       0
200 Multi_Zone_Error_Rate   0x0008   100   253   000    Old_age   Offline      -       0

SMART Error Log Version: 1
No Errors Logged

SMART Self-test log structure revision number 1
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

Selective Self-tests/Logging not supported

The above only provides legacy SMART information - try 'smartctl -x' for more


###############################################################################
# 21. STORAGE: HBA / RAID CONTROLLERS
###############################################################################

###############################################################################
# 22. VIRTUAL MACHINES (qm)
###############################################################################

--- qm list
    $ qm list
      VMID NAME                 STATUS     MEM(MB)    BOOTDISK(GB) PID       
       400 pfv-proxmox-backup-server running    2048              32.00 1622      
      4000 KNELTemplate         stopped    2048              32.00 0         

--- qm config per VM
    $ for vmid in $(qm list 2>/dev/null | awk 'NR>1{print $1}'); do
    echo "--- VM $vmid ---"
    qm config "$vmid" 2>&1
    echo ""
done
--- VM 400 ---
boot: order=scsi0
cores: 2
cpu: host
ide2: local:iso/proxmox-backup-server_4.1-1.iso,media=cdrom,size=1479332K
memory: 2048
meta: creation-qemu=10.1.2,ctime=1771895002
name: pfv-proxmox-backup-server
net0: virtio=BC:24:11:6E:12:69,bridge=vmbr0,firewall=1
numa: 0
onboot: 1
ostype: l26
scsi0: local-lvm:vm-400-disk-0,iothread=1,size=32G
scsihw: virtio-scsi-single
smbios1: uuid=4659f1f3-292c-4951-817a-f5403fb1e979
sockets: 1
vmgenid: 7a8f6ed0-8980-4698-9859-7a5b568e863d

--- VM 4000 ---
agent: 1
balloon: 0
boot: order=virtio0;ide2;net0
cores: 2
cpu: host
ide2: local:iso/debian-13.3.0-amd64-netinst.iso,media=cdrom,size=754M
memory: 2048
meta: creation-qemu=10.1.2,ctime=1771939265
name: KNELTemplate
net0: virtio=BC:24:11:80:1D:23,bridge=vmbr0,firewall=1
numa: 0
onboot: 1
ostype: l26
scsihw: virtio-scsi-single
smbios1: uuid=53b22660-3d36-41f6-bcea-66b1e0d7bbf9
sockets: 1
template: 1
virtio0: D1:401/base-401-disk-0.qcow2,cache=writethrough,iothread=1,size=32G
vmgenid: 3fde3494-a706-4131-a054-8335786e4b22


--- VM runtime status (qm guest agent if running)
    $ for vmid in $(qm list 2>/dev/null | awk 'NR>1{print $1}'); do
    echo "--- VM $vmid runtime ---"
    qm guest cmd "$vmid" network-get-interfaces 2>/dev/null | head -n 40 || echo "  [no agent or VM not running]"
done
--- VM 400 runtime ---
--- VM 4000 runtime ---

--- /etc/pve/qemu-server
lrwxr-xr-x 1 root www-data 27 Dec 31  1969 /etc/pve/qemu-server -> nodes/pfv-tsys4/qemu-server

--- /etc/pve/firewall
total 0
drwxr-xr-x 2 root www-data 0 Feb 23 10:53 .
drwxr-xr-x 2 root www-data 0 Dec 31  1969 ..

###############################################################################
# 23. CONTAINERS (pct)
###############################################################################

--- pct list
    $ pct list

--- pct config per CT
    $ for ctid in $(pct list 2>/dev/null | awk 'NR>1{print $1}'); do
    echo "--- CT $ctid ---"
    pct config "$ctid" 2>&1
    echo ""
done

###############################################################################
# 24. SERVICES / FAILED UNITS
###############################################################################

--- running services
    $ systemctl list-units --type=service --state=running --no-pager
  UNIT                     LOAD   ACTIVE SUB     DESCRIPTION
  beszel-agent.service     loaded active running Beszel Agent Service
  chrony.service           loaded active running chrony, an NTP client/server
  conmand.service          loaded active running ConMan (Console Manager)
  cron.service             loaded active running Regular background program processing daemon
  dbus.service             loaded active running D-Bus System Message Bus
  dm-event.service         loaded active running Device-mapper event daemon
  fsidd.service            loaded active running NFS FSID Daemon
  getty@tty1.service       loaded active running Getty on tty1
  glances.service          loaded active running Glances
  ksmtuned.service         loaded active running Kernel Samepage Merging (KSM) Tuning Daemon
  lldpd.service            loaded active running LLDP daemon
  lxc-monitord.service     loaded active running LXC Container Monitoring Daemon
  lxcfs.service            loaded active running FUSE filesystem for LXC
  nfs-blkmap.service       loaded active running pNFS block layout mapping daemon
  nfs-idmapd.service       loaded active running NFSv4 ID-name mapping service
  nfs-mountd.service       loaded active running NFS Mount Daemon
  nfsdcld.service          loaded active running NFSv4 Client Tracking Daemon
  polkit.service           loaded active running Authorization Manager
  postfix.service          loaded active running Postfix Mail Transport Agent (main/default instance)
  proxmox-firewall.service loaded active running Proxmox nftables firewall
  pve-cluster.service      loaded active running The Proxmox VE cluster filesystem
  pve-firewall.service     loaded active running Proxmox VE firewall
  pve-lxc-syscalld.service loaded active running Proxmox VE LXC Syscall Daemon
  pvedaemon.service        loaded active running PVE API Daemon
  pvefw-logger.service     loaded active running Proxmox VE firewall logger
  pveproxy.service         loaded active running PVE API Proxy Server
  pvescheduler.service     loaded active running Proxmox VE scheduler
  pvestatd.service         loaded active running PVE Status Daemon
  qmeventd.service         loaded active running PVE Qemu Event Daemon
  rpc-statd.service        loaded active running NFS status monitor for NFSv2/3 locking.
  rpcbind.service          loaded active running RPC bind portmap service
  rrdcached.service        loaded active running Data caching daemon for rrdtool
  ser2net.service          loaded active running Serial port to network proxy
  smartmontools.service    loaded active running Self Monitoring and Reporting Technology (SMART) Daemon
  spiceproxy.service       loaded active running PVE SPICE Proxy Server
  ssh.service              loaded active running OpenBSD Secure Shell server
  systemd-journald.service loaded active running Journal Service
  systemd-logind.service   loaded active running User Login Management
  systemd-udevd.service    loaded active running Rule-based Manager for Device Events and Files
  tailscaled.service       loaded active running Tailscale node agent
  tuned.service            loaded active running Dynamic System Tuning Daemon
  user@0.service           loaded active running User Manager for UID 0
  zfs-zed.service          loaded active running ZFS Event Daemon (zed)

Legend: LOAD   → Reflects whether the unit definition was properly loaded.
        ACTIVE → The high-level unit activation state, i.e. generalization of SUB.
        SUB    → The low-level unit activation state, values depend on unit type.

43 loaded units listed.

--- failed services
    $ systemctl --failed --no-pager
  UNIT           LOAD   ACTIVE SUB    DESCRIPTION
● conman.service loaded failed failed serial console management program

Legend: LOAD   → Reflects whether the unit definition was properly loaded.
        ACTIVE → The high-level unit activation state, i.e. generalization of SUB.
        SUB    → The low-level unit activation state, values depend on unit type.

1 loaded units listed.

--- enabled services
    $ systemctl list-unit-files --state=enabled --no-pager
UNIT FILE                              STATE   PRESET
beszel-agent.service                   enabled enabled
blk-availability.service               enabled enabled
chrony.service                         enabled enabled
conman.service                         enabled enabled
conmand.service                        enabled enabled
console-setup.service                  enabled enabled
cron.service                           enabled enabled
disable-usb-autosuspend.service        enabled enabled
e2scrub_reap.service                   enabled enabled
fsidd.service                          enabled enabled
getty@.service                         enabled enabled
glances.service                        enabled enabled
grub-common.service                    enabled enabled
keyboard-setup.service                 enabled enabled
ksmtuned.service                       enabled enabled
lldpd.service                          enabled enabled
lvm2-monitor.service                   enabled enabled
lxc-monitord.service                   enabled enabled
lxc-net.service                        enabled enabled
lxc.service                            enabled enabled
lxcfs.service                          enabled enabled
netavark-dhcp-proxy.service            enabled enabled
netavark-firewalld-reload.service      enabled enabled
networking.service                     enabled enabled
nfs-blkmap.service                     enabled enabled
nfs-server.service                     enabled enabled
open-iscsi.service                     enabled enabled
postfix.service                        enabled enabled
proxmox-boot-cleanup.service           enabled enabled
proxmox-firewall.service               enabled enabled
pve-cluster.service                    enabled enabled
pve-firewall-commit.service            enabled enabled
pve-firewall.service                   enabled enabled
pve-guests.service                     enabled enabled
pve-lxc-syscalld.service               enabled enabled
pve-query-machine-capabilities.service enabled enabled
pve-sdn-commit.service                 enabled enabled
pvebanner.service                      enabled enabled
pvedaemon.service                      enabled enabled
pvefw-logger.service                   enabled enabled
pvenetcommit.service                   enabled enabled
pveproxy.service                       enabled enabled
pvescheduler.service                   enabled enabled
pvestatd.service                       enabled enabled
qmeventd.service                       enabled enabled
rbdmap.service                         enabled enabled
rpcbind.service                        enabled enabled
rrdcached.service                      enabled enabled
ser2net.service                        enabled enabled
smartmontools.service                  enabled enabled
spiceproxy.service                     enabled enabled
ssh.service                            enabled enabled
sshd-keygen.service                    enabled enabled
systemd-pstore.service                 enabled enabled
tailscaled.service                     enabled enabled
tuned.service                          enabled enabled
wtmpdb-update-boot.service             enabled enabled
zfs-import-cache.service               enabled enabled
zfs-mount.service                      enabled enabled
zfs-share.service                      enabled enabled
zfs-volume-wait.service                enabled enabled
zfs-zed.service                        enabled enabled
system-xfs_scrub.slice                 enabled enabled
dm-event.socket                        enabled enabled
iscsid.socket                          enabled enabled
lvm2-lvmpolld.socket                   enabled enabled
netavark-dhcp-proxy.socket             enabled enabled
rpcbind.socket                         enabled enabled
rrdcached.socket                       enabled enabled
uuidd.socket                           enabled enabled
ceph-fuse.target                       enabled enabled
ceph.target                            enabled enabled
nfs-client.target                      enabled enabled
remote-fs.target                       enabled enabled
zfs-import.target                      enabled enabled
zfs-volumes.target                     enabled enabled
zfs.target                             enabled enabled
apt-daily-upgrade.timer                enabled enabled
apt-daily.timer                        enabled enabled
beszel-agent-update.timer              enabled enabled
dpkg-db-backup.timer                   enabled enabled
e2scrub_all.timer                      enabled enabled
fstrim.timer                           enabled enabled
logrotate.timer                        enabled enabled
man-db.timer                           enabled enabled
mdcheck_continue.timer                 enabled enabled
mdcheck_start.timer                    enabled enabled
mdmonitor-oneshot.timer                enabled enabled
pve-daily-update.timer                 enabled enabled
xfs_scrub_all.timer                    enabled enabled

90 unit files listed.

--- pve-* service status
    $ systemctl status pve-cluster pvedaemon pveproxy pve-firewall pve-ha-crm pve-ha-lrm pvestatd pvebanner --no-pager 2>&1 | head -n 120
● pve-cluster.service - The Proxmox VE cluster filesystem
     Loaded: loaded (/usr/lib/systemd/system/pve-cluster.service; enabled; preset: enabled)
     Active: active (running) since Fri 2026-07-24 16:00:03 CDT; 4 days ago
 Invocation: e453235c99b847bcbaf3fee923948434
   Main PID: 1245 (pmxcfs)
      Tasks: 7 (limit: 18967)
     Memory: 24.7M (peak: 58.1M, swap: 23.6M, swap peak: 37.3M)
        CPU: 2min 40.688s
     CGroup: /system.slice/pve-cluster.service
             └─1245 /usr/bin/pmxcfs

Jul 24 16:00:01 pfv-tsys4 systemd[1]: Starting pve-cluster.service - The Proxmox VE cluster filesystem...
Jul 24 16:00:01 pfv-tsys4 pmxcfs[1214]: [main] notice: resolved node name 'pfv-tsys4' to '192.168.100.2' for default node IP address
Jul 24 16:00:01 pfv-tsys4 pmxcfs[1214]: [main] notice: resolved node name 'pfv-tsys4' to '192.168.100.2' for default node IP address
Jul 24 16:00:03 pfv-tsys4 systemd[1]: Started pve-cluster.service - The Proxmox VE cluster filesystem.

● pvedaemon.service - PVE API Daemon
     Loaded: loaded (/usr/lib/systemd/system/pvedaemon.service; enabled; preset: enabled)
     Active: active (running) since Fri 2026-07-24 16:00:09 CDT; 4 days ago
 Invocation: f51489cd36b04cccad4952818ae99b64
   Main PID: 1484 (pvedaemon)
      Tasks: 4 (limit: 18967)
     Memory: 73.8M (peak: 195.3M, swap: 150.6M, swap peak: 155.1M)
        CPU: 41.911s
     CGroup: /system.slice/pvedaemon.service
             ├─  1484 pvedaemon
             ├─980581 "pvedaemon worker"
             ├─981614 "pvedaemon worker"
             └─986538 "pvedaemon worker"

Jul 28 06:11:26 pfv-tsys4 pvedaemon[1484]: worker 980581 started
Jul 28 06:17:00 pfv-tsys4 pvedaemon[1486]: worker exit
Jul 28 06:17:01 pfv-tsys4 pvedaemon[1484]: worker 1486 finished
Jul 28 06:17:01 pfv-tsys4 pvedaemon[1484]: starting 1 worker(s)
Jul 28 06:17:01 pfv-tsys4 pvedaemon[1484]: worker 981614 started
Jul 28 06:43:00 pfv-tsys4 pvedaemon[1485]: worker exit
Jul 28 06:43:02 pfv-tsys4 pvedaemon[1484]: worker 1485 finished
Jul 28 06:43:02 pfv-tsys4 pvedaemon[1484]: starting 1 worker(s)
Jul 28 06:43:02 pfv-tsys4 pvedaemon[1484]: worker 986538 started
Jul 29 01:00:03 pfv-tsys4 pvedaemon[986538]: update new package list: /var/lib/pve-manager/pkgupdates

● pveproxy.service - PVE API Proxy Server
     Loaded: loaded (/usr/lib/systemd/system/pveproxy.service; enabled; preset: enabled)
     Active: active (running) since Fri 2026-07-24 16:00:10 CDT; 4 days ago
 Invocation: ad94467386064b43af42ee5db7a56e95
    Process: 1197532 ExecReload=/usr/bin/pveproxy restart (code=exited, status=0/SUCCESS)
   Main PID: 1553 (pveproxy)
      Tasks: 4 (limit: 18967)
     Memory: 247.6M (peak: 434.9M, swap: 4K, swap peak: 294.1M)
        CPU: 1min 42.182s
     CGroup: /system.slice/pveproxy.service
             ├─   1553 pveproxy
             ├─1197626 "pveproxy worker"
             ├─1197627 "pveproxy worker"
             └─1197628 "pveproxy worker"

Jul 29 00:56:50 pfv-tsys4 pveproxy[1553]: starting 3 worker(s)
Jul 29 00:56:50 pfv-tsys4 pveproxy[1553]: worker 1197626 started
Jul 29 00:56:50 pfv-tsys4 pveproxy[1553]: worker 1197627 started
Jul 29 00:56:50 pfv-tsys4 pveproxy[1553]: worker 1197628 started
Jul 29 00:56:55 pfv-tsys4 pveproxy[914956]: worker exit
Jul 29 00:56:55 pfv-tsys4 pveproxy[914957]: worker exit
Jul 29 00:56:55 pfv-tsys4 pveproxy[914955]: worker exit
Jul 29 00:57:00 pfv-tsys4 pveproxy[1553]: worker 914955 finished
Jul 29 00:57:00 pfv-tsys4 pveproxy[1553]: worker 914957 finished
Jul 29 00:57:00 pfv-tsys4 pveproxy[1553]: worker 914956 finished

● pve-firewall.service - Proxmox VE firewall
     Loaded: loaded (/usr/lib/systemd/system/pve-firewall.service; enabled; preset: enabled)
     Active: active (running) since Fri 2026-07-24 16:00:08 CDT; 4 days ago
 Invocation: 220e37055dfe450fbf381f28186dce38
   Main PID: 1449 (pve-firewall)
      Tasks: 1 (limit: 18967)
     Memory: 37.7M (peak: 128.3M, swap: 95.7M, swap peak: 95.7M)
        CPU: 37min 35.145s
     CGroup: /system.slice/pve-firewall.service
             └─1449 pve-firewall

Jul 24 16:00:03 pfv-tsys4 systemd[1]: Starting pve-firewall.service - Proxmox VE firewall...
Jul 24 16:00:08 pfv-tsys4 pve-firewall[1449]: starting server
Jul 24 16:00:08 pfv-tsys4 systemd[1]: Started pve-firewall.service - Proxmox VE firewall.
Jul 26 15:07:47 pfv-tsys4 pve-firewall[1449]: firewall update time (6.399 seconds)
Jul 27 21:51:02 pfv-tsys4 pve-firewall[1449]: firewall update time (8.277 seconds)

○ pve-ha-crm.service - PVE Cluster HA Resource Manager Daemon
     Loaded: loaded (/usr/lib/systemd/system/pve-ha-crm.service; disabled; preset: enabled)
     Active: inactive (dead)

○ pve-ha-lrm.service - PVE Local HA Resource Manager Daemon
     Loaded: loaded (/usr/lib/systemd/system/pve-ha-lrm.service; disabled; preset: enabled)
     Active: inactive (dead)

● pvestatd.service - PVE Status Daemon
     Loaded: loaded (/usr/lib/systemd/system/pvestatd.service; enabled; preset: enabled)
     Active: active (running) since Fri 2026-07-24 16:00:08 CDT; 4 days ago
 Invocation: b089fe7463334022a4ae1aef6d822c5b
   Main PID: 1465 (pvestatd)
      Tasks: 1 (limit: 18967)
     Memory: 46.5M (peak: 135.3M, swap: 87.8M, swap peak: 87.8M)
        CPU: 38min 43.355s
     CGroup: /system.slice/pvestatd.service
             └─1465 pvestatd

Jul 24 16:00:03 pfv-tsys4 systemd[1]: Starting pvestatd.service - PVE Status Daemon...
Jul 24 16:00:08 pfv-tsys4 pvestatd[1465]: starting server
Jul 24 16:00:08 pfv-tsys4 systemd[1]: Started pvestatd.service - PVE Status Daemon.
Jul 25 10:56:39 pfv-tsys4 pvestatd[1465]: auth key pair too old, rotating..
Jul 26 10:56:41 pfv-tsys4 pvestatd[1465]: auth key pair too old, rotating..
Jul 26 15:07:47 pfv-tsys4 pvestatd[1465]: status update time (5.596 seconds)
Jul 27 10:56:41 pfv-tsys4 pvestatd[1465]: auth key pair too old, rotating..
Jul 27 21:51:04 pfv-tsys4 pvestatd[1465]: status update time (9.260 seconds)
Jul 28 10:56:46 pfv-tsys4 pvestatd[1465]: auth key pair too old, rotating..
Jul 28 20:10:17 pfv-tsys4 pvestatd[1465]: status update time (6.866 seconds)

● pvebanner.service - Proxmox VE Login Banner
     Loaded: loaded (/usr/lib/systemd/system/pvebanner.service; enabled; preset: enabled)
     Active: active (exited) since Fri 2026-07-24 15:59:05 CDT; 4 days ago
 Invocation: e0b579aa68ba4e269f0c85573fec88c3
   Main PID: 904 (code=exited, status=0/SUCCESS)
   Mem peak: 34.8M

--- storage-related service status
    $ systemctl status nfs-kernel-server nfs-server rpcbind rpc-statd zfs-import zfs-mount zfs-target smartd nvme-stat multipathd --no-pager 2>&1 | head -n 80
● nfs-server.service - NFS server and services
     Loaded: loaded (/usr/lib/systemd/system/nfs-server.service; enabled; preset: enabled)
    Drop-In: /run/systemd/generator/nfs-server.service.d
             └─order-with-mounts.conf
     Active: active (exited) since Fri 2026-07-24 16:00:11 CDT; 4 days ago
 Invocation: 31e5f1e426a94cdc85e882117636b6f8
       Docs: man:rpc.nfsd(8)
             man:exportfs(8)
   Main PID: 1571 (code=exited, status=0/SUCCESS)
   Mem peak: 1.8M
        CPU: 15ms

Jul 24 16:00:11 pfv-tsys4 systemd[1]: Starting nfs-server.service - NFS server and services...
Jul 24 16:00:11 pfv-tsys4 exportfs[1569]: exportfs: Failed to stat /mnt/tsys4/D7: No such file or directory
Jul 24 16:00:11 pfv-tsys4 exportfs[1569]: exportfs: Failed to stat /mnt/tsys4/D1: No such file or directory
Jul 24 16:00:11 pfv-tsys4 sh[1572]: nfsdctl: lockd configuration failure
Jul 24 16:00:11 pfv-tsys4 systemd[1]: Finished nfs-server.service - NFS server and services.

● nfs-server.service - NFS server and services
     Loaded: loaded (/usr/lib/systemd/system/nfs-server.service; enabled; preset: enabled)
    Drop-In: /run/systemd/generator/nfs-server.service.d
             └─order-with-mounts.conf
     Active: active (exited) since Fri 2026-07-24 16:00:11 CDT; 4 days ago
 Invocation: 31e5f1e426a94cdc85e882117636b6f8
       Docs: man:rpc.nfsd(8)
             man:exportfs(8)
   Main PID: 1571 (code=exited, status=0/SUCCESS)
   Mem peak: 1.8M
        CPU: 15ms

Jul 24 16:00:11 pfv-tsys4 systemd[1]: Starting nfs-server.service - NFS server and services...
Jul 24 16:00:11 pfv-tsys4 exportfs[1569]: exportfs: Failed to stat /mnt/tsys4/D7: No such file or directory
Jul 24 16:00:11 pfv-tsys4 exportfs[1569]: exportfs: Failed to stat /mnt/tsys4/D1: No such file or directory
Jul 24 16:00:11 pfv-tsys4 sh[1572]: nfsdctl: lockd configuration failure
Jul 24 16:00:11 pfv-tsys4 systemd[1]: Finished nfs-server.service - NFS server and services.

● rpcbind.service - RPC bind portmap service
     Loaded: loaded (/usr/lib/systemd/system/rpcbind.service; enabled; preset: enabled)
     Active: active (running) since Fri 2026-07-24 15:59:00 CDT; 4 days ago
 Invocation: 5d2420eac98d451fb11735e771c51d2e
TriggeredBy: ● rpcbind.socket
       Docs: man:rpcbind(8)
   Main PID: 934 (rpcbind)
      Tasks: 1 (limit: 18967)
     Memory: 1M (peak: 2.1M, swap: 92K, swap peak: 92K)
        CPU: 3min 37.197s
     CGroup: /system.slice/rpcbind.service
             └─934 /usr/sbin/rpcbind -f -w

Jul 24 15:59:00 pfv-tsys4 systemd[1]: Starting rpcbind.service - RPC bind portmap service...
Jul 24 15:59:00 pfv-tsys4 systemd[1]: Started rpcbind.service - RPC bind portmap service.

● rpc-statd.service - NFS status monitor for NFSv2/3 locking.
     Loaded: loaded (/usr/lib/systemd/system/rpc-statd.service; static)
     Active: active (running) since Fri 2026-07-24 16:00:01 CDT; 4 days ago
 Invocation: aadb1d67946d4092bcd32f76d3054e6d
       Docs: man:rpc.statd(8)
   Main PID: 1234 (rpc.statd)
      Tasks: 1 (limit: 18967)
     Memory: 392K (peak: 1.7M, swap: 112K, swap peak: 112K)
        CPU: 7ms
     CGroup: /system.slice/rpc-statd.service
             └─1234 /usr/sbin/rpc.statd

Jul 24 16:00:01 pfv-tsys4 systemd[1]: Starting rpc-statd.service - NFS status monitor for NFSv2/3 locking....
Jul 24 16:00:01 pfv-tsys4 rpc.statd[1234]: Version 2.8.3 starting
Jul 24 16:00:01 pfv-tsys4 rpc.statd[1234]: Flags: TI-RPC
Jul 24 16:00:01 pfv-tsys4 systemd[1]: Started rpc-statd.service - NFS status monitor for NFSv2/3 locking..

○ zfs-import.service
     Loaded: masked (Reason: Unit zfs-import.service is masked.)
     Active: inactive (dead)

● zfs-mount.service - Mount ZFS filesystems
     Loaded: loaded (/usr/lib/systemd/system/zfs-mount.service; enabled; preset: enabled)
     Active: active (exited) since Fri 2026-07-24 15:58:19 CDT; 4 days ago
 Invocation: b949855e4d8447c799c35c9e8f7d6df5
       Docs: man:zfs(8)
   Main PID: 885 (code=exited, status=0/SUCCESS)
   Mem peak: 1.6M

###############################################################################
# 25. TIMERS / CRON
###############################################################################

--- systemctl list-timers
    $ systemctl list-timers --all --no-pager
NEXT                           LEFT LAST                              PASSED UNIT                         ACTIVATES
Wed 2026-07-29 06:17:01 CDT 1h 3min Tue 2026-07-28 06:31:29 CDT      22h ago apt-daily-upgrade.timer      apt-daily-upgrade.service
Wed 2026-07-29 14:50:57 CDT      9h Tue 2026-07-28 19:27:03 CDT       9h ago apt-daily.timer              apt-daily.service
Wed 2026-07-29 16:15:01 CDT     11h Tue 2026-07-28 16:15:01 CDT      12h ago systemd-tmpfiles-clean.timer systemd-tmpfiles-clean.service
Thu 2026-07-30 00:00:00 CDT     18h Wed 2026-07-29 00:00:23 CDT 5h 13min ago dpkg-db-backup.timer         dpkg-db-backup.service
Thu 2026-07-30 00:39:45 CDT     19h Wed 2026-07-29 00:56:29 CDT 4h 17min ago logrotate.timer              logrotate.service
Thu 2026-07-30 02:47:22 CDT     21h Wed 2026-07-29 03:59:29 CDT 1h 14min ago beszel-agent-update.timer    beszel-agent-update.service
Thu 2026-07-30 04:26:59 CDT     23h Wed 2026-07-29 03:19:29 CDT 1h 54min ago pve-daily-update.timer       pve-daily-update.service
Thu 2026-07-30 05:07:30 CDT     23h Wed 2026-07-29 01:26:29 CDT 3h 47min ago man-db.timer                 man-db.service
Sun 2026-08-02 03:10:20 CDT  3 days Sun 2026-07-26 03:10:21 CDT   3 days ago e2scrub_all.timer            e2scrub_all.service
Sun 2026-08-02 03:10:31 CDT  3 days Sun 2026-07-26 03:10:21 CDT   3 days ago xfs_scrub_all.timer          xfs_scrub_all.service
Mon 2026-08-03 00:31:21 CDT  4 days Mon 2026-07-27 01:27:07 CDT   2 days ago fstrim.timer                 fstrim.service

11 timers listed.

--- /etc/cron.d
total 24
drwxr-xr-x   2 root root 4096 Mar 21 12:20 .
drwxr-xr-x 111 root root 4096 Jul 29 05:12 ..
-rw-r--r--   1 root root  188 Jul 30  2025 e2scrub_all
-rw-r--r--   1 root root  102 Jun 13  2025 .placeholder
-rw-r--r--   1 root root  400 Jan 15  2024 sysstat
lrwxrwxrwx   1 root root   20 Feb 23 10:53 vzdump -> /etc/pve/vzdump.cron
-rw-r--r--   1 root root  377 Aug 26  2025 zfsutils-linux

--- /etc/cron.daily
total 32
drwxr-xr-x   2 root root 4096 Mar 21 12:20 .
drwxr-xr-x 111 root root 4096 Jul 29 05:12 ..
-rwxr-xr-x   1 root root 1478 Jun 24  2025 apt-compat
-rwxr-xr-x   1 root root  123 May 27  2025 dpkg
-rwxr-xr-x   1 root root  377 Jul 14  2024 logrotate
-rwxr-xr-x   1 root root 1395 May  2  2025 man-db
-rw-r--r--   1 root root  102 Jun 13  2025 .placeholder
-rwxr-xr-x   1 root root  526 Jan 15  2024 sysstat

--- /etc/cron.hourly
total 12
drwxr-xr-x   2 root root 4096 Feb 23 04:50 .
drwxr-xr-x 111 root root 4096 Jul 29 05:12 ..
-rw-r--r--   1 root root  102 Jun 13  2025 .placeholder

--- /etc/cron.weekly
total 16
drwxr-xr-x   2 root root 4096 Feb 23 04:50 .
drwxr-xr-x 111 root root 4096 Jul 29 05:12 ..
-rwxr-xr-x   1 root root 1055 May  2  2025 man-db
-rw-r--r--   1 root root  102 Jun 13  2025 .placeholder

--- crontabs
    --- /etc/crontab ---
# /etc/crontab: system-wide crontab
# Unlike any other crontab you don't have to run the `crontab'
# command to install the new version when you edit this file
# and files in /etc/cron.d. These files also have username fields,
# that none of the other crontabs do.

SHELL=/bin/sh
PATH=/usr/local/sbin:/usr/local/bin:/usr/sbin:/usr/bin:/sbin:/bin

# Example of job definition:
# .---------------- minute (0 - 59)
# |  .------------- hour (0 - 23)
# |  |  .---------- day of month (1 - 31)
# |  |  |  .------- month (1 - 12) OR jan,feb,mar,apr ...
# |  |  |  |  .---- day of week (0 - 6) (Sunday=0 or 7) OR sun,mon,tue,wed,thu,fri,sat
# |  |  |  |  |
# *  *  *  *  * user-name command to be executed
17 *	* * *	root	cd / && run-parts --report /etc/cron.hourly
25 6	* * *	root	test -x /usr/sbin/anacron || { cd / && run-parts --report /etc/cron.daily; }
47 6	* * 7	root	test -x /usr/sbin/anacron || { cd / && run-parts --report /etc/cron.weekly; }
52 6	1 * *	root	test -x /usr/sbin/anacron || { cd / && run-parts --report /etc/cron.monthly; }
#

--- root crontab
    $ crontab -l 2>/dev/null || echo "  [no root crontab]"
  [no root crontab]

###############################################################################
# 26. LIVE PERFORMANCE SNAPSHOT
###############################################################################

--- /proc/loadavg
    $ cat /proc/loadavg
7.04 6.57 6.31 2/328 1248683

--- vmstat 1 3
    $ vmstat 1 3
procs -----------memory---------- ---swap-- -----io---- -system-- -------cpu-------
 r  b   swpd   free   buff  cache   si   so    bi    bo   in   cs us sy id wa st gu
 0  0 852756 13305076  97252 940276    4    7   969  1136 2760    2  0  1 76 23  0  0
 0  2 852756 13317600  97388 940768    0    0     0  1416 3824 4705  0  1 79 21  0  0
 0  0 852756 13332124  97468 940820    0    0     0   332 2348 2726  0  0 91  9  0  0

--- mpstat 1 3 (per-cpu)
    $ mpstat 1 3
Linux 6.17.9-1-pve (pfv-tsys4) 	07/29/2026 	_x86_64_	(8 CPU)

05:13:42 AM  CPU    %usr   %nice    %sys %iowait    %irq   %soft  %steal  %guest  %gnice   %idle
05:13:43 AM  all    0.00    0.00    0.38   39.95    0.00    0.13    0.00    0.13    0.00   59.42
05:13:44 AM  all    0.13    0.00    0.88   29.81    0.00    0.00    0.00    0.00    0.00   69.18
05:13:45 AM  all    0.13    0.00    0.13   15.60    0.00    0.00    0.00    0.00    0.00   84.15
Average:     all    0.08    0.00    0.46   28.46    0.00    0.04    0.00    0.04    0.00   70.91

--- iostat -xz 1 3
    $ iostat -xz 1 3
Linux 6.17.9-1-pve (pfv-tsys4) 	07/29/2026 	_x86_64_	(8 CPU)

avg-cpu:  %user   %nice %system %iowait  %steal   %idle
           0.13    0.00    0.50   22.87    0.00   76.49

Device            r/s     rkB/s   rrqm/s  %rrqm r_await rareq-sz     w/s     wkB/s   wrqm/s  %wrqm w_await wareq-sz     d/s     dkB/s   drqm/s  %drqm d_await dareq-sz     f/s f_await  aqu-sz  %util
dm-0             1.04      4.20     0.00   0.00    9.39     4.05    1.29      7.22     0.00   0.00    8.55     5.61    0.00      0.00     0.00   0.00    0.00     0.00    0.00    0.00    0.02   0.88
dm-1             0.36     21.70     0.00   0.00   12.98    59.66    2.00      9.79     0.00   0.00    7.56     4.91    0.00      0.00     0.00   0.00    0.00     0.00    0.00    0.00    0.02   1.49
dm-2             0.00      0.04     0.00   0.00   20.84    19.94    0.00      0.00     0.00   0.00   33.00     0.00    0.00      0.00     0.00   0.00    0.00     0.00    0.00    0.00    0.00   0.00
dm-3             0.05      1.86     0.00   0.00   25.32    36.94    1.52      9.23     0.00   0.00   13.43     6.06    0.00      0.00     0.00   0.00    0.00     0.00    0.00    0.00    0.02   0.92
dm-4             0.05      1.82     0.00   0.00   25.34    36.26    1.52      9.23     0.00   0.00   13.43     6.06    0.00      0.00     0.00   0.00    0.00     0.00    0.00    0.00    0.02   0.91
dm-5             0.00      0.04     0.00   0.00   14.82   277.14    0.00      0.00     0.00   0.00   16.25     0.00    0.00      0.00     0.00   0.00    0.00     0.00    0.00    0.00    0.00   0.00
dm-6             0.05      1.74     0.00   0.00   46.61    34.89    1.52      9.23     0.00   0.00   16.19     6.06    0.00      0.00     0.00   0.00    0.00     0.00    0.00    0.00    0.03   0.92
sda              0.01      0.09     0.00  12.42    9.63    10.30    0.00      0.00     0.00   3.70    5.50     1.54    0.00      0.00     0.00   0.00    0.00     0.00    0.00    5.60    0.00   0.00
sdb              0.89    387.21    12.38  93.28   13.22   434.03   20.39    369.13     3.17  13.47   13.59    18.11    0.00      0.00     0.00   0.00    0.00     0.00    0.00    0.00    0.29  19.04
sdc              2.05    502.53     6.68  76.52   11.28   245.20   72.41    741.12     7.85   9.78    7.85    10.24    0.00      0.00     0.00   0.00    0.00     0.00   31.41   11.97    0.97  37.96
sdd              1.33     79.17     0.53  28.54    8.26    59.44    3.02     26.24     1.78  37.07    6.72     8.68    0.00      0.00     0.00   0.00    0.00     0.00    0.71   13.59    0.04   2.50
sde              0.00      0.13     0.00  33.65    0.95    37.46    0.00      0.00     0.00   9.68    1.61     2.29    0.00      0.00     0.00   0.00    0.00     0.00    0.00    1.86    0.00   0.00
sdf              0.02      0.16     0.00   6.83   20.60     7.84    0.00      0.02     0.00  99.17    8.57   481.14    0.00      0.27     0.00   0.00    0.00 106056.00    0.00    0.00    0.00   0.03


avg-cpu:  %user   %nice %system %iowait  %steal   %idle
           0.13    0.00    0.25   17.23    0.00   82.39

Device            r/s     rkB/s   rrqm/s  %rrqm r_await rareq-sz     w/s     wkB/s   wrqm/s  %wrqm w_await wareq-sz     d/s     dkB/s   drqm/s  %drqm d_await dareq-sz     f/s f_await  aqu-sz  %util
dm-1             0.00      0.00     0.00   0.00    0.00     0.00   55.00    240.00     0.00   0.00    9.35     4.36    0.00      0.00     0.00   0.00    0.00     0.00    0.00    0.00    0.51  21.00
sdb              0.00      0.00     0.00   0.00    0.00     0.00   59.00    328.00    13.00  18.06   10.25     5.56    0.00      0.00     0.00   0.00    0.00     0.00    0.00    0.00    0.60  51.90
sdc              0.00      0.00     0.00   0.00    0.00     0.00  119.00    496.00    13.00   9.85    7.18     4.17    0.00      0.00     0.00   0.00    0.00     0.00   37.00   18.46    1.54  61.90
sdd              0.00      0.00     0.00   0.00    0.00     0.00   55.00    240.00     0.00   0.00    5.55     4.36    0.00      0.00     0.00   0.00    0.00     0.00    0.00    0.00    0.30  21.00


avg-cpu:  %user   %nice %system %iowait  %steal   %idle
           0.00    0.00    0.50   24.87    0.00   74.62

Device            r/s     rkB/s   rrqm/s  %rrqm r_await rareq-sz     w/s     wkB/s   wrqm/s  %wrqm w_await wareq-sz     d/s     dkB/s   drqm/s  %drqm d_await dareq-sz     f/s f_await  aqu-sz  %util
sdb              0.00      0.00     0.00   0.00    0.00     0.00   96.00    580.00    12.00  11.11   11.20     6.04    0.00      0.00     0.00   0.00    0.00     0.00    0.00    0.00    1.07  71.20
sdc              0.00      0.00     0.00   0.00    0.00     0.00   66.00    360.00    21.00  24.14    9.86     5.45    0.00      0.00     0.00   0.00    0.00     0.00   31.00   13.35    1.06  40.90



--- sar -dp 1 2
    $ sar -dp 1 2
Linux 6.17.9-1-pve (pfv-tsys4) 	07/29/2026 	_x86_64_	(8 CPU)

05:13:47 AM       tps     rkB/s     wkB/s     dkB/s   areq-sz    aqu-sz     await     %util DEV
05:13:48 AM      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 sda
05:13:48 AM     38.00      0.00    212.00      0.00      5.58      0.45     11.71     36.50 sdb
05:13:48 AM     60.00      0.00    284.00      0.00      4.73      0.95      8.42     39.50 sdc
05:13:48 AM      4.00    512.00      0.00      0.00    128.00      0.01      2.25      1.00 sdd
05:13:48 AM      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 pve-swap
05:13:48 AM      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 pve-root
05:13:48 AM      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 pve-data_tmeta
05:13:48 AM      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 pve-data_tdata
05:13:48 AM      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 sde
05:13:48 AM      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 pve-data-tpool
05:13:48 AM      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 pve-data
05:13:48 AM      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 sdf
05:13:48 AM      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 pve-vm--400--disk--0

05:13:48 AM       tps     rkB/s     wkB/s     dkB/s   areq-sz    aqu-sz     await     %util DEV
05:13:49 AM      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 sda
05:13:49 AM     33.00      0.00    172.00      0.00      5.21      0.28      8.64     27.20 sdb
05:13:49 AM     56.00      0.00    284.00      0.00      5.07      0.99     10.57     38.50 sdc
05:13:49 AM      5.00      0.00     32.00      0.00      6.40      0.08      8.40      4.10 sdd
05:13:49 AM      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 pve-swap
05:13:49 AM      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 pve-root
05:13:49 AM      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 pve-data_tmeta
05:13:49 AM      5.00      0.00     32.00      0.00      6.40      0.04      8.20      4.10 pve-data_tdata
05:13:49 AM      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 sde
05:13:49 AM      5.00      0.00     32.00      0.00      6.40      0.04      8.20      4.10 pve-data-tpool
05:13:49 AM      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 pve-data
05:13:49 AM      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 sdf
05:13:49 AM      5.00      0.00     32.00      0.00      6.40      0.04      8.40      4.20 pve-vm--400--disk--0

Average:          tps     rkB/s     wkB/s     dkB/s   areq-sz    aqu-sz     await     %util DEV
Average:         0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 sda
Average:        35.50      0.00    192.00      0.00      5.41      0.37     10.28     31.85 sdb
Average:        58.00      0.00    284.00      0.00      4.90      0.97      9.46     39.00 sdc
Average:         4.50    256.00     16.00      0.00     60.44      0.05      5.67      2.55 sdd
Average:         0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 pve-swap
Average:         0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 pve-root
Average:         0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 pve-data_tmeta
Average:         2.50      0.00     16.00      0.00      6.40      0.02      8.20      2.05 pve-data_tdata
Average:         0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 sde
Average:         2.50      0.00     16.00      0.00      6.40      0.02      8.20      2.05 pve-data-tpool
Average:         0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 pve-data
Average:         0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 sdf
Average:         2.50      0.00     16.00      0.00      6.40      0.02      8.40      2.10 pve-vm--400--disk--0

--- sar -n DEV 1 2
    $ sar -n DEV 1 2
Linux 6.17.9-1-pve (pfv-tsys4) 	07/29/2026 	_x86_64_	(8 CPU)

05:13:49 AM     IFACE   rxpck/s   txpck/s    rxkB/s    txkB/s   rxcmp/s   txcmp/s  rxmcst/s   %ifutil
05:13:50 AM        lo      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
05:13:50 AM      nic0     36.00      6.00      5.23      0.89      0.00      0.00     10.00      0.00
05:13:50 AM enx8cae4ccda926    651.00    368.00    748.56     44.15      0.00      0.00      0.00      0.00
05:13:50 AM enx80ae4ccdec03      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
05:13:50 AM tailscale0      2.00      1.00      0.15      0.08      0.00      0.00      0.00      0.00
05:13:50 AM     vmbr0     26.00      3.00      3.16      0.26      0.00      0.00      2.00      0.00
05:13:50 AM   datanet    650.00    367.00    748.52     43.90      0.00      0.00      0.00      0.00
05:13:50 AM  tap400i0      2.00     26.00      0.35      3.73      0.00      0.00      0.00      0.00
05:13:50 AM fwbr400i0     23.00      0.00      2.82      0.00      0.00      0.00      2.00      0.00
05:13:50 AM fwpr400p0      3.00     26.00      0.59      3.73      0.00      0.00      0.00      0.00
05:13:50 AM fwln400i0     26.00      3.00      3.73      0.59      0.00      0.00      0.00      0.00

05:13:50 AM     IFACE   rxpck/s   txpck/s    rxkB/s    txkB/s   rxcmp/s   txcmp/s  rxmcst/s   %ifutil
05:13:51 AM        lo      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
05:13:51 AM      nic0     42.00      8.00      5.46      1.14      0.00      0.00     19.00      0.00
05:13:51 AM enx8cae4ccda926    766.00    415.00    886.79     52.86      0.00      0.00      0.00      0.00
05:13:51 AM enx80ae4ccdec03      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
05:13:51 AM tailscale0      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
05:13:51 AM     vmbr0     32.00      4.00      3.64      0.63      0.00      0.00     13.00      0.00
05:13:51 AM   datanet    766.00    417.00    886.79     52.99      0.00      0.00      1.00      0.00
05:13:51 AM  tap400i0      4.00     32.00      0.48      3.95      0.00      0.00      0.00      0.00
05:13:51 AM fwbr400i0     28.00      0.00      3.09      0.00      0.00      0.00     13.00      0.00
05:13:51 AM fwpr400p0      4.00     32.00      0.48      3.95      0.00      0.00      0.00      0.00
05:13:51 AM fwln400i0     32.00      4.00      3.95      0.48      0.00      0.00      0.00      0.00

Average:        IFACE   rxpck/s   txpck/s    rxkB/s    txkB/s   rxcmp/s   txcmp/s  rxmcst/s   %ifutil
Average:           lo      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
Average:         nic0     39.00      7.00      5.34      1.02      0.00      0.00     14.50      0.00
Average:    enx8cae4ccda926    708.50    391.50    817.68     48.51      0.00      0.00      0.00      0.00
Average:    enx80ae4ccdec03      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
Average:    tailscale0      1.00      0.50      0.08      0.04      0.00      0.00      0.00      0.00
Average:        vmbr0     29.00      3.50      3.40      0.45      0.00      0.00      7.50      0.00
Average:      datanet    708.00    392.00    817.65     48.45      0.00      0.00      0.50      0.00
Average:     tap400i0      3.00     29.00      0.41      3.84      0.00      0.00      0.00      0.00
Average:    fwbr400i0     25.50      0.00      2.96      0.00      0.00      0.00      7.50      0.00
Average:    fwpr400p0      3.50     29.00      0.54      3.84      0.00      0.00      0.00      0.00
Average:    fwln400i0     29.00      3.50      3.84      0.54      0.00      0.00      0.00      0.00

--- sar -n NFS,NFSD 1 2
    $ sar -n NFS,NFSD 1 2
Linux 6.17.9-1-pve (pfv-tsys4) 	07/29/2026 	_x86_64_	(8 CPU)

05:13:51 AM    call/s retrans/s    read/s   write/s  access/s  getatt/s
05:13:52 AM      0.00      0.00      0.00      0.00      0.00      0.00

05:13:51 AM   scall/s badcall/s  packet/s     udp/s     tcp/s     hit/s    miss/s   sread/s  swrite/s saccess/s sgetatt/s
05:13:52 AM    181.00      0.00    181.00      0.00    181.00      0.00      0.00      0.00    155.00      0.00     75.00

05:13:52 AM    call/s retrans/s    read/s   write/s  access/s  getatt/s
05:13:53 AM      0.00      0.00      0.00      0.00      0.00      0.00

05:13:52 AM   scall/s badcall/s  packet/s     udp/s     tcp/s     hit/s    miss/s   sread/s  swrite/s saccess/s sgetatt/s
05:13:53 AM     69.00      0.00     69.00      0.00     69.00      0.00      0.00      0.00     68.00      0.00     49.00

Average:       call/s retrans/s    read/s   write/s  access/s  getatt/s
Average:         0.00      0.00      0.00      0.00      0.00      0.00

Average:      scall/s badcall/s  packet/s     udp/s     tcp/s     hit/s    miss/s   sread/s  swrite/s saccess/s sgetatt/s
Average:       125.00      0.00    125.00      0.00    125.00      0.00      0.00      0.00    111.50      0.00     62.00

--- sar -n SOCK 1 1
    $ sar -n SOCK 1 1
Linux 6.17.9-1-pve (pfv-tsys4) 	07/29/2026 	_x86_64_	(8 CPU)

05:13:53 AM    totsck    tcpsck    udpsck    rawsck   ip-frag    tcp-tw
05:13:54 AM       389        58        10         0         0         1
Average:          389        58        10         0         0         1

--- sar -n TCP,ETCP 1 2
    $ sar -n TCP,ETCP 1 2
Linux 6.17.9-1-pve (pfv-tsys4) 	07/29/2026 	_x86_64_	(8 CPU)

05:13:54 AM  active/s passive/s    iseg/s    oseg/s
05:13:55 AM      0.00      6.00    477.00    268.00

05:13:54 AM  atmptf/s  estres/s retrans/s isegerr/s   orsts/s
05:13:55 AM      0.00      0.00      0.00      0.00      0.00

05:13:55 AM  active/s passive/s    iseg/s    oseg/s
05:13:56 AM      0.00      0.00    690.00    349.00

05:13:55 AM  atmptf/s  estres/s retrans/s isegerr/s   orsts/s
05:13:56 AM      0.00      0.00      0.00      0.00      0.00

Average:     active/s passive/s    iseg/s    oseg/s
Average:         0.00      3.00    583.50    308.50

Average:     atmptf/s  estres/s retrans/s isegerr/s   orsts/s
Average:         0.00      0.00      0.00      0.00      0.00

--- pidstat -d 1 2 (top disk)
    $ pidstat -d 1 2
Linux 6.17.9-1-pve (pfv-tsys4) 	07/29/2026 	_x86_64_	(8 CPU)

05:13:56 AM   UID       PID   kB_rd/s   kB_wr/s kB_ccwr/s iodelay  Command
05:13:57 AM     0      1578      0.00      3.96      0.00       0  nfsd
05:13:57 AM     0      1579      0.00     23.76      0.00       0  nfsd
05:13:57 AM     0      1580      0.00   1615.84      0.00       0  nfsd
05:13:57 AM     0      1581      0.00      3.96      0.00       0  nfsd
05:13:57 AM     0      1582      0.00     19.80      0.00       0  nfsd
05:13:57 AM     0      1583      0.00     47.52      0.00       0  nfsd
05:13:57 AM     0      1584      0.00   1552.48      0.00       0  nfsd
05:13:57 AM     0      1585      0.00      3.96      0.00       0  nfsd
05:13:57 AM     0      1586      0.00      3.96      0.00       0  nfsd
05:13:57 AM     0      1587      3.96   1619.80      0.00       0  nfsd
05:13:57 AM     0      1588      0.00     19.80      0.00       0  nfsd
05:13:57 AM     0      1589      0.00      3.96      0.00       0  nfsd
05:13:57 AM     0      1590      0.00    293.07      0.00       0  nfsd
05:13:57 AM     0      1591      0.00    768.32      0.00       0  nfsd
05:13:57 AM     0      1592      0.00     15.84      0.00       0  nfsd
05:13:57 AM     0      1593      0.00      7.92      0.00       0  nfsd

05:13:57 AM   UID       PID   kB_rd/s   kB_wr/s kB_ccwr/s iodelay  Command
05:13:58 AM     0      1465    512.00      0.00      0.00       0  pvestatd
05:13:58 AM     0      1578      0.00     48.00      0.00       0  nfsd
05:13:58 AM     0      1579      0.00     20.00      0.00       0  nfsd
05:13:58 AM     0      1580      0.00     36.00      0.00       0  nfsd
05:13:58 AM     0      1581      0.00    324.00      0.00       0  nfsd
05:13:58 AM     0      1582      0.00     76.00      0.00       0  nfsd
05:13:58 AM     0      1583      0.00     12.00      0.00       0  nfsd
05:13:58 AM     0      1584      0.00    272.00      0.00       0  nfsd
05:13:58 AM     0      1585      0.00    308.00      0.00       0  nfsd
05:13:58 AM     0      1586      0.00     36.00      0.00       0  nfsd
05:13:58 AM     0      1587      0.00     28.00      0.00       0  nfsd
05:13:58 AM     0      1588      0.00    572.00      0.00       0  nfsd
05:13:58 AM     0      1589      0.00     48.00      0.00       0  nfsd
05:13:58 AM     0      1590      0.00     12.00      0.00       0  nfsd
05:13:58 AM     0      1591      0.00     56.00      0.00       0  nfsd
05:13:58 AM     0      1592      0.00    300.00      0.00       0  nfsd
05:13:58 AM     0      1593      0.00    308.00      0.00       0  nfsd

Average:      UID       PID   kB_rd/s   kB_wr/s kB_ccwr/s iodelay  Command
Average:        0      1465    254.73      0.00      0.00       0  pvestatd
Average:        0      1578      0.00     25.87      0.00       0  nfsd
Average:        0      1579      0.00     21.89      0.00       0  nfsd
Average:        0      1580      0.00    829.85      0.00       0  nfsd
Average:        0      1581      0.00    163.18      0.00       0  nfsd
Average:        0      1582      0.00     47.76      0.00       0  nfsd
Average:        0      1583      0.00     29.85      0.00       0  nfsd
Average:        0      1584      0.00    915.42      0.00       0  nfsd
Average:        0      1585      0.00    155.22      0.00       0  nfsd
Average:        0      1586      0.00     19.90      0.00       0  nfsd
Average:        0      1587      1.99    827.86      0.00       0  nfsd
Average:        0      1588      0.00    294.53      0.00       0  nfsd
Average:        0      1589      0.00     25.87      0.00       0  nfsd
Average:        0      1590      0.00    153.23      0.00       0  nfsd
Average:        0      1591      0.00    413.93      0.00       0  nfsd
Average:        0      1592      0.00    157.21      0.00       0  nfsd
Average:        0      1593      0.00    157.21      0.00       0  nfsd

--- pidstat -u 1 2 (top cpu)
    $ pidstat -u 1 2
Linux 6.17.9-1-pve (pfv-tsys4) 	07/29/2026 	_x86_64_	(8 CPU)

05:13:58 AM   UID       PID    %usr %system  %guest   %wait    %CPU   CPU  Command
05:13:59 AM     0        94    0.00    1.00    0.00    0.00    1.00     7  kworker/7:1H-kblockd
05:13:59 AM     0      1580    0.00    1.00    0.00    0.00    1.00     7  nfsd
05:13:59 AM     0      1591    0.00    1.00    0.00    0.00    1.00     6  nfsd
05:13:59 AM     0      1622    0.00    0.00    1.00    0.00    1.00     4  kvm
05:13:59 AM     0   1248769    0.00    1.00    0.00    0.00    1.00     3  pidstat

05:13:59 AM   UID       PID    %usr %system  %guest   %wait    %CPU   CPU  Command
05:14:00 AM     0        94    0.00    1.00    0.00    0.00    1.00     7  kworker/7:1H-kblockd
05:14:00 AM     0       872    0.00    1.00    0.00    0.00    1.00     6  jbd2/sdb-8
05:14:00 AM     0       961    1.00    0.00    0.00    0.00    1.00     2  tailscaled
05:14:00 AM     0      1484    1.00    0.00    0.00    0.00    1.00     6  pvedaemon
05:14:00 AM     0      1578    0.00    1.00    0.00    1.00    1.00     4  nfsd
05:14:00 AM     0      1590    0.00    1.00    0.00    0.00    1.00     4  nfsd

Average:      UID       PID    %usr %system  %guest   %wait    %CPU   CPU  Command
Average:        0        94    0.00    1.00    0.00    0.00    1.00     -  kworker/7:1H-kblockd
Average:        0       872    0.00    0.50    0.00    0.00    0.50     -  jbd2/sdb-8
Average:        0       961    0.50    0.00    0.00    0.00    0.50     -  tailscaled
Average:        0      1484    0.50    0.00    0.00    0.00    0.50     -  pvedaemon
Average:        0      1578    0.00    0.50    0.00    0.50    0.50     -  nfsd
Average:        0      1580    0.00    0.50    0.00    0.00    0.50     -  nfsd
Average:        0      1590    0.00    0.50    0.00    0.00    0.50     -  nfsd
Average:        0      1591    0.00    0.50    0.00    0.00    0.50     -  nfsd
Average:        0      1622    0.00    0.00    0.50    0.00    0.50     -  kvm
Average:        0   1248769    0.00    0.50    0.00    0.00    0.50     -  pidstat

--- top (single snapshot, top 30)
    $ top -b -n 1
top - 05:14:00 up 4 days, 13:15,  3 users,  load average: 7.53, 6.71, 6.36
Tasks: 265 total,   1 running, 264 sleeping,   0 stopped,   0 zombie
%Cpu(s):  0.0 us,  0.0 sy,  0.0 ni, 82.3 id, 17.7 wa,  0.0 hi,  0.0 si,  0.0 st 
MiB Mem :  15901.1 total,  13101.9 free,   2098.4 used,   1021.0 buff/cache     
MiB Swap:   8192.0 total,   7359.2 free,    832.8 used.  13802.7 avail Mem 

    PID USER      PR  NI    VIRT    RES    SHR S  %CPU  %MEM     TIME+ COMMAND
      1 root      20   0   25816  12236   7752 S   0.0   0.1   0:29.80 systemd
      2 root      20   0       0      0      0 S   0.0   0.0   0:00.20 kthreadd
      3 root      20   0       0      0      0 S   0.0   0.0   0:00.00 pool_wo+
      4 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
      5 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
      6 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
      7 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
      8 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     10 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     13 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     14 root      20   0       0      0      0 S   0.0   0.0   0:01.79 ksoftir+
     15 root      20   0       0      0      0 I   0.0   0.0   4:37.81 rcu_pre+
     16 root      20   0       0      0      0 S   0.0   0.0   0:00.00 rcu_exp+
     17 root      20   0       0      0      0 S   0.0   0.0   0:00.00 rcu_exp+
     18 root      rt   0       0      0      0 S   0.0   0.0   0:00.51 migrati+
     19 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 idle_in+
     20 root      20   0       0      0      0 S   0.0   0.0   0:00.00 cpuhp/0
     21 root      20   0       0      0      0 S   0.0   0.0   0:00.00 cpuhp/1
     22 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 idle_in+
     23 root      rt   0       0      0      0 S   0.0   0.0   0:00.82 migrati+
     24 root      20   0       0      0      0 S   0.0   0.0   0:01.76 ksoftir+
     26 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     27 root      20   0       0      0      0 S   0.0   0.0   0:00.00 cpuhp/2
     28 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 idle_in+
     29 root      rt   0       0      0      0 S   0.0   0.0   0:00.77 migrati+
     30 root      20   0       0      0      0 S   0.0   0.0   0:01.06 ksoftir+
     32 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     33 root      20   0       0      0      0 S   0.0   0.0   0:00.00 cpuhp/3
     34 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 idle_in+
     35 root      rt   0       0      0      0 S   0.0   0.0   0:00.74 migrati+
     36 root      20   0       0      0      0 S   0.0   0.0   0:00.86 ksoftir+
     38 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     39 root      20   0       0      0      0 S   0.0   0.0   0:00.00 cpuhp/4
     40 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 idle_in+
     41 root      rt   0       0      0      0 S   0.0   0.0   0:01.00 migrati+
     42 root      20   0       0      0      0 S   0.0   0.0   0:33.67 ksoftir+
     44 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     45 root      20   0       0      0      0 S   0.0   0.0   0:00.00 cpuhp/5
     46 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 idle_in+
     47 root      rt   0       0      0      0 S   0.0   0.0   0:00.88 migrati+
     48 root      20   0       0      0      0 S   0.0   0.0   0:00.86 ksoftir+
     50 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     51 root      20   0       0      0      0 S   0.0   0.0   0:00.00 cpuhp/6
     52 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 idle_in+
     53 root      rt   0       0      0      0 S   0.0   0.0   0:00.87 migrati+
     54 root      20   0       0      0      0 S   0.0   0.0   0:00.92 ksoftir+
     56 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     57 root      20   0       0      0      0 S   0.0   0.0   0:00.00 cpuhp/7
     58 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 idle_in+
     59 root      rt   0       0      0      0 S   0.0   0.0   0:00.89 migrati+
     60 root      20   0       0      0      0 S   0.0   0.0   0:01.54 ksoftir+
     63 root      20   0       0      0      0 S   0.0   0.0   0:00.00 kdevtmp+
     64 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     65 root      20   0       0      0      0 I   0.0   0.0   0:00.00 rcu_tas+
     66 root      20   0       0      0      0 I   0.0   0.0   0:00.00 rcu_tas+
     67 root      20   0       0      0      0 I   0.0   0.0   0:00.00 rcu_tas+
     68 root      20   0       0      0      0 S   0.0   0.0   0:00.00 kauditd
     69 root      20   0       0      0      0 S   0.0   0.0   0:00.15 khungta+
     71 root      20   0       0      0      0 S   0.0   0.0   0:00.00 oom_rea+
     73 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     74 root      20   0       0      0      0 S   0.0   0.0   1:48.95 kcompac+
     75 root      25   5       0      0      0 S   0.0   0.0   0:00.00 ksmd
     76 root      39  19       0      0      0 S   0.0   0.0   0:01.61 khugepa+
     77 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     78 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     79 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     80 root     -51   0       0      0      0 S   0.0   0.0   0:02.37 irq/9-a+
     85 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     86 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     87 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     88 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     89 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     90 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     91 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 watchdo+
     93 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     94 root       0 -20       0      0      0 I   0.0   0.0  21:17.26 kworker+
     96 root      20   0       0      0      0 S   0.0   0.0   0:43.68 kswapd0
     97 root      20   0       0      0      0 S   0.0   0.0   0:00.00 ecryptf+
     98 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     99 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    100 root      20   0       0      0      0 S   0.0   0.0   0:00.00 scsi_eh+
    101 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    102 root      20   0       0      0      0 S   0.0   0.0   0:00.00 scsi_eh+
    103 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    105 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    107 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    108 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    111 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    122 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    123 root       0 -20       0      0      0 I   0.0   0.0   0:52.29 kworker+
    124 root       0 -20       0      0      0 I   0.0   0.0   0:48.97 kworker+
    126 root       0 -20       0      0      0 I   0.0   0.0   0:49.34 kworker+
    127 root       0 -20       0      0      0 I   0.0   0.0   0:48.25 kworker+
    159 root       0 -20       0      0      0 I   0.0   0.0   1:28.46 kworker+
    172 root       0 -20       0      0      0 I   0.0   0.0   0:50.98 kworker+
    174 root       0 -20       0      0      0 I   0.0   0.0   0:49.96 kworker+
    232 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    233 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    241 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    243 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    244 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    268 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    269 root      20   0       0      0      0 S   0.0   0.0   0:00.00 scsi_eh+
    270 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    279 root      20   0       0      0      0 S   0.0   0.0   0:00.00 scsi_eh+
    280 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    281 root      20   0       0      0      0 S   0.0   0.0   0:00.32 usb-sto+
    282 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    283 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    284 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    285 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    310 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    342 root      20   0       0      0      0 S   0.0   0.0   0:05.48 jbd2/dm+
    343 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    394 root      20   0   59712  25952  25392 S   0.0   0.2   0:06.42 systemd+
    433 root      20   0   77292  22296   9124 S   0.0   0.1   0:10.41 dmeventd
    434 root       0 -20       0      0      0 S   0.0   0.0   0:00.00 spl_sys+
    435 root       0 -20       0      0      0 S   0.0   0.0   0:00.00 spl_del+
    436 root       0 -20       0      0      0 S   0.0   0.0   0:00.00 spl_dyn+
    437 root       0 -20       0      0      0 S   0.0   0.0   0:00.00 spl_kme+
    445 root      20   0   36720   8188   5556 S   0.0   0.1   0:00.84 systemd+
    446 root       0 -20       0      0      0 S   0.0   0.0   0:00.00 zvol_tq+
    447 root       0 -20       0      0      0 S   0.0   0.0   0:00.00 zvol_tq+
    448 root      20   0       0      0      0 S   0.0   0.0   0:00.00 arc_pru+
    449 root      20   0       0      0      0 S   0.0   0.0   0:00.00 arc_evi+
    450 root      20   0       0      0      0 S   0.0   0.0   0:00.00 arc_evi+
    451 root      20   0       0      0      0 S   0.0   0.0   0:00.00 arc_evi+
    452 root      20   0       0      0      0 S   0.0   0.0   0:00.00 arc_flu+
    453 root      20   0       0      0      0 S   0.0   0.0   0:02.83 arc_evi+
    454 root      39  19       0      0      0 S   0.0   0.0   0:02.90 arc_reap
    455 root      20   0       0      0      0 S   0.0   0.0   0:00.00 dbu_evi+
    456 root      39  19       0      0      0 S   0.0   0.0   0:02.76 dbuf_ev+
    457 root      39  19       0      0      0 S   0.0   0.0   0:00.00 z_vdev_+
    458 root      20   0       0      0      0 S   0.0   0.0   0:03.40 l2arc_f+
    464 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    465 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    467 root      -2   0       0      0      0 S   0.0   0.0   0:00.00 psimon
    557 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 irq/38-+
    667 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    854 root      20   0       0      0      0 S   0.0   0.0   0:00.00 jbd2/sd+
    855 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    858 root      20   0       0      0      0 S   0.0   0.0   1:53.21 jbd2/sd+
    859 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    865 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    868 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 card0-c+
    869 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 card0-c+
    870 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 card0-c+
    872 root      20   0       0      0      0 S   0.0   0.0   1:27.44 jbd2/sd+
    876 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    897 root      20   0       0      0      0 S   0.0   0.0   0:00.00 jbd2/sd+
    898 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    934 _rpc      20   0    6664   3212   2800 S   0.0   0.0   3:37.20 rpcbind
    937 message+  20   0    8612   4968   4056 S   0.0   0.0   0:19.39 dbus-da+
    939 root      20   0    5460   3456   3144 S   0.0   0.0   0:00.00 fsidd
    945 root      20   0  276136   2804   2516 S   0.0   0.0   0:00.00 pve-lxc+
    948 root      20   0  404832   6556   5532 S   0.0   0.0   0:24.71 rrdcach+
    951 root      20   0   10592   6408   4568 S   0.0   0.0   0:00.47 smartd
    952 root      20   0   20676   8044   5736 S   0.0   0.0   0:01.11 systemd+
    961 root      20   0 1422028  96368  19112 S   0.0   0.6  11:36.91 tailsca+
    964 root      20   0  104412   3524   2868 S   0.0   0.0   0:00.01 zed
    968 root      20   0  159068   2260   1940 S   0.0   0.0   0:00.00 lxcfs
    995 root      20   0    5748   1688   1608 S   0.0   0.0   0:00.02 qmeventd
    996 root      20   0    7224   2080   1872 S   0.0   0.0   0:04.79 ksmtuned
    998 root      20   0    5260   1556   1356 S   0.0   0.0   0:00.00 blkmapd
   1012 root      20   0    5660   2420   2100 S   0.0   0.0   0:00.01 nfsdcld
   1036 _chrony   20   0   19932   3444   2672 S   0.0   0.0   0:00.37 chronyd
   1041 _chrony   20   0   11604   2144   1512 S   0.0   0.0   0:00.00 chronyd
   1104 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
   1144 root      20   0    5988   2732   2036 S   0.0   0.0   0:02.00 dhclient
   1206 beszel    20   0 2231516  13996   6220 S   0.0   0.1   1:03.92 beszel-+
   1207 root      20   0  513512  10376   4464 S   0.0   0.1   0:00.45 glances
   1208 _lldpd    20   0   21372   3888   2848 S   0.0   0.0   0:00.18 lldpd
   1209 root      20   0    5520   2444   2232 S   0.0   0.0   0:00.00 lxc-mon+
   1222 root      20   0  266300  17832   8920 S   0.0   0.1   0:36.90 tuned
   1233 root      20   0    2952   2068   1860 S   0.0   0.0   0:00.04 rpc.idm+
   1234 statd     20   0    4560   1692   1460 S   0.0   0.0   0:00.00 rpc.sta+
   1235 root      20   0    8832   3780   2840 S   0.0   0.0   1:52.99 rpc.mou+
   1242 root      20   0   11772   4860   4288 S   0.0   0.0   0:00.31 sshd
   1245 root      20   0  535024  26932  20912 S   0.0   0.2   2:40.67 pmxcfs
   1261 _lldpd    20   0   21372   2532   1504 S   0.0   0.0   0:04.12 lldpd
   1287 root      20   0    6868   2744   2504 S   0.0   0.0   0:00.70 cron
   1288 root      20   0   13808   2816   2124 S   0.0   0.0   0:20.32 proxmox+
   1411 root      20   0   43992   4436   4168 S   0.0   0.0   0:00.78 master
   1413 postfix   20   0   44524   6716   6500 S   0.0   0.0   0:00.14 qmgr
   1420 polkitd   20   0  306704   6568   5616 S   0.0   0.0   0:04.81 polkitd
   1449 root      20   0  177368  37724   6120 S   0.0   0.2  13:41.43 pve-fir+
   1465 root      20   0  180508  48272   9516 S   0.0   0.3  18:50.39 pvestatd
   1484 root      20   0  219064   7536   3212 S   0.0   0.0   0:03.11 pvedaem+
   1553 www-data  20   0  220336 179008  31864 S   0.0   1.1   0:07.55 pveproxy
   1562 www-data  20   0   92008  68352  16932 S   0.0   0.4   0:04.50 spicepr+
   1574 root      20   0       0      0      0 I   0.0   0.0   0:00.00 lockd
   1578 root      20   0       0      0      0 I   0.0   0.0   4:55.97 nfsd
   1579 root      20   0       0      0      0 I   0.0   0.0   5:02.95 nfsd
   1580 root      20   0       0      0      0 I   0.0   0.0   4:57.58 nfsd
   1581 root      20   0       0      0      0 I   0.0   0.0   4:57.52 nfsd
   1582 root      20   0       0      0      0 I   0.0   0.0   4:55.50 nfsd
   1583 root      20   0       0      0      0 I   0.0   0.0   4:59.58 nfsd
   1584 root      20   0       0      0      0 I   0.0   0.0   4:56.24 nfsd
   1585 root      20   0       0      0      0 I   0.0   0.0   4:58.01 nfsd
   1586 root      20   0       0      0      0 I   0.0   0.0   4:57.66 nfsd
   1587 root      20   0       0      0      0 I   0.0   0.0   4:56.04 nfsd
   1588 root      20   0       0      0      0 D   0.0   0.0   4:57.08 nfsd
   1589 root      20   0       0      0      0 I   0.0   0.0   4:59.77 nfsd
   1590 root      20   0       0      0      0 I   0.0   0.0   4:57.48 nfsd
   1591 root      20   0       0      0      0 I   0.0   0.0   4:58.86 nfsd
   1592 root      20   0       0      0      0 I   0.0   0.0   4:59.75 nfsd
   1593 root      20   0       0      0      0 I   0.0   0.0   4:58.69 nfsd
   1603 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
   1622 root      20   0 2862928 899060   4124 S   0.0   5.5  53:55.40 kvm
   1685 root      20   0       0      0      0 S   0.0   0.0   0:00.00 kvm-pit+
   1692 root      20   0  200848   9548   3368 S   0.0   0.1   0:23.15 pvesche+
   3656 root      20   0    8164   2392   2196 S   0.0   0.0   0:00.00 agetty
  13588 root      20   0   22572   7684   6204 S   0.0   0.0   0:00.50 systemd
  13590 root      20   0   24372   1676   1568 S   0.0   0.0   0:00.00 (sd-pam)
  13595 root      -2   0       0      0      0 S   0.0   0.0   0:00.00 psimon
  13647 root      20   0    7308   2172   1684 S   0.0   0.0   0:00.32 screen
  13721 root      20   0    7308   2092   1576 S   0.0   0.0   0:00.29 screen
  78155 root      20   0       0      0      0 S   0.0   0.0   0:00.00 jbd2/sd+
  78156 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
 551797 root      20   0    7176   1988   1660 S   0.0   0.0   0:00.55 screen
 553759 root      20   0    7176   2184   1648 S   0.0   0.0   0:05.68 screen
 980581 root      20   0  228236  17132   6176 S   0.0   0.1   0:02.85 pvedaem+
 981614 root      20   0  226964  16836   6188 S   0.0   0.1   0:02.61 pvedaem+
 986538 root      20   0  266928  64688  10144 S   0.0   0.4   0:05.06 pvedaem+
1137714 root      20   0    6360   3680   3208 S   0.0   0.0   0:04.13 ser2net
1137796 root      -2   0       0      0      0 S   0.0   0.0   0:00.00 psimon
1142324 root      20   0   84980   1996   1672 S   0.0   0.0   0:00.13 conmand
1197606 root      20   0   79616   2548   2340 S   0.0   0.0   0:00.85 pvefw-l+
1197625 www-data  20   0   92272  55488   3924 S   0.0   0.3   0:00.30 spicepr+
1197626 www-data  20   0  234784 166260  11788 S   0.0   1.0   0:01.07 pveprox+
1197627 www-data  20   0  269436 203864  16444 S   0.0   1.3   0:01.76 pveprox+
1197628 www-data  20   0  234780 166264  11792 S   0.0   1.0   0:01.04 pveprox+
1215464 root      20   0       0      0      0 I   0.0   0.0   0:00.32 kworker+
1221307 root      20   0       0      0      0 I   0.0   0.0   0:00.61 kworker+
1222609 root      20   0       0      0      0 I   0.0   0.0   0:00.65 kworker+
1227296 root      20   0       0      0      0 I   0.0   0.0   0:00.18 kworker+
1228901 root      20   0       0      0      0 I   0.0   0.0   0:00.15 kworker+
1230586 root      20   0       0      0      0 I   0.0   0.0   0:00.12 kworker+
1234192 root      20   0       0      0      0 I   0.0   0.0   0:00.35 kworker+
1237027 postfix   20   0   44472   7736   7052 S   0.0   0.0   0:00.00 pickup
1239353 root      20   0       0      0      0 I   0.0   0.0   0:00.05 kworker+
1240849 root      20   0       0      0      0 I   0.0   0.0   0:00.04 kworker+
1240950 root      20   0       0      0      0 I   0.0   0.0   0:00.04 kworker+
1240983 root      20   0       0      0      0 I   0.0   0.0   0:00.06 kworker+
1241760 root      20   0       0      0      0 I   0.0   0.0   0:00.06 kworker+
1241970 root      20   0       0      0      0 I   0.0   0.0   0:00.09 kworker+
1242331 root      20   0       0      0      0 I   0.0   0.0   0:00.04 kworker+
1243605 root      20   0       0      0      0 I   0.0   0.0   0:00.03 kworker+
1243644 root      20   0       0      0      0 I   0.0   0.0   0:00.06 kworker+
1244280 root      20   0       0      0      0 I   0.0   0.0   0:00.01 kworker+
1244451 root      20   0       0      0      0 I   0.0   0.0   0:00.04 kworker+
1244985 root      20   0       0      0      0 I   0.0   0.0   0:00.03 kworker+
1245212 root      20   0       0      0      0 I   0.0   0.0   0:00.02 kworker+
1245602 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1245652 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1245662 root      20   0   19636  11680   9908 S   0.0   0.1   0:00.00 sshd-se+
1245669 root      20   0   19892   7432   5384 S   0.0   0.0   0:00.00 sshd-se+
1245670 root      20   0    7328   3824   3292 S   0.0   0.0   0:00.29 bash
1246984 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1247815 root      20   0       0      0      0 I   0.0   0.0   0:00.01 kworker+
1247976 root      20   0    5584   1984   1880 S   0.0   0.0   0:00.00 sleep
1248049 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1248770 root      20   0    7328   2432   1900 S   0.0   0.0   0:00.00 bash
1248771 root      20   0    5592   2068   1952 S   0.0   0.0   0:00.00 head
1248772 root      20   0   10424   5408   3320 R   0.0   0.0   0:00.00 top

--- zpool iostat 1 2
    $ zpool iostat 1 2
no pools available
no pools available

--- arcstat 1 2
    $ arcstat 1 2
/root/check.sh: line 45: arcstat: command not found
    [exit=127 / not installed or not permitted]

--- /proc/net/dev delta (1s)
    $ awk '{print $1}' /proc/net/dev
echo "--- t0 ---"
cat /proc/net/dev
sleep 1
echo "--- t1 (1s later) ---"
cat /proc/net/dev
Inter-|
face
lo:
nic0:
enx8cae4ccda926:
enx80ae4ccdec03:
tailscale0:
vmbr0:
datanet:
tap400i0:
fwbr400i0:
fwpr400p0:
fwln400i0:
--- t0 ---
Inter-|   Receive                                                |  Transmit
 face |bytes    packets errs drop fifo frame compressed multicast|bytes    packets errs drop fifo colls carrier compressed
    lo: 9939151   59700    0    0    0     0          0         0  9939151   59700    0    0    0     0       0          0
  nic0: 5481243115 20033358    0 13115    0     0          0   9686165 4493389546 5449766    0    0    0     0       0          0
enx8cae4ccda926: 471075408771 511586764    0 13113    0     0          0         0 893495918681 693926619    0    6    0     0       0          0
enx80ae4ccdec03:       0       0    0    0    0     0          0         0        0       0    0    0    0     0       0          0
tailscale0: 28504167  243228    0    0    0     0          0         0 197177830  301112    0    0    0     0       0          0
 vmbr0: 4130812774 14857434    0    0    0     0          0   8097430 3984696888 1725723    0    0    0     0       0          0
datanet: 471069837195 511569187    0   15    0     0          0    328379 893492587523 693913529    0    0    0     0       0          0
tap400i0: 315652297 1189744    0    0    0     0          0         0 1817901913 13930897    0 5168    0     0       0          0
fwbr400i0: 1093610597 11970028    0 15594    0     0          0   8096391        0       0    0    0    0     0       0          0
fwpr400p0: 318915442 1202849    0 13105    0     0          0         0 1818426529 13936066    0    0    0     0       0          0
fwln400i0: 1818426529 13936066    0 13105    0     0          0         0 318915442 1202849    0    0    0     0       0          0
--- t1 (1s later) ---
Inter-|   Receive                                                |  Transmit
 face |bytes    packets errs drop fifo frame compressed multicast|bytes    packets errs drop fifo colls carrier compressed
    lo: 9939151   59700    0    0    0     0          0         0  9939151   59700    0    0    0     0       0          0
  nic0: 5481247086 20033382    0 13115    0     0          0   9686175 4493390748 5449771    0    0    0     0       0          0
enx8cae4ccda926: 471075877684 511587170    0 13113    0     0          0         0 893495949797 693926823    0    6    0     0       0          0
enx80ae4ccdec03:       0       0    0    0    0     0          0         0        0       0    0    0    0     0       0          0
tailscale0: 28504167  243228    0    0    0     0          0         0 197177830  301112    0    0    0     0       0          0
 vmbr0: 4130813726 14857449    0    0    0     0          0   8097435 3984697220 1725725    0    0    0     0       0          0
datanet: 471070306108 511569593    0   15    0     0          0    328380 893492616851 693913723    0    0    0     0       0          0
tap400i0: 315653147 1189747    0    0    0     0          0         0 1817903300 13930914    0 5168    0     0       0          0
fwbr400i0: 1093611273 11970041    0 15594    0     0          0   8096396        0       0    0    0    0     0       0          0
fwpr400p0: 318916292 1202852    0 13105    0     0          0         0 1818427916 13936083    0    0    0     0       0          0
fwln400i0: 1818427916 13936083    0 13105    0     0          0         0 318916292 1202852    0    0    0     0       0          0

###############################################################################
# 27. DNS / NTP / TIME
###############################################################################

--- /etc/resolv.conf
    --- /etc/resolv.conf ---
domain knel.net
search knel.net
nameserver 100.100.100.100

--- /etc/hosts
    --- /etc/hosts ---
127.0.0.1 localhost.localdomain localhost
192.168.100.2 pfv-tsys4.knel.net pfv-tsys4

# The following lines are desirable for IPv6 capable hosts

::1     ip6-localhost ip6-loopback
fe00::0 ip6-localnet
ff00::0 ip6-mcastprefix
ff02::1 ip6-allnodes
ff02::2 ip6-allrouters
ff02::3 ip6-allhosts

--- /etc/ntp.conf
    [missing: /etc/ntp.conf]

--- /etc/chrony/chrony.conf
    --- /etc/chrony/chrony.conf ---
# Welcome to the chrony configuration file. See chrony.conf(5) for more
# information about usable directives.

# Use Debian vendor zone.
pool 2.debian.pool.ntp.org iburst

# Use time sources from DHCP.
sourcedir /run/chrony-dhcp

# Use NTP sources found in /etc/chrony/sources.d.
sourcedir /etc/chrony/sources.d

# This directive specifies the location of the file containing ID/key pairs for
# NTP authentication.
keyfile /etc/chrony/chrony.keys

# This directive specifies the file into which chronyd will store the rate
# information.
driftfile /var/lib/chrony/chrony.drift

# Save NTS keys and cookies.
ntsdumpdir /var/lib/chrony

# Uncomment the following line to turn logging on.
#log tracking measurements statistics

# Log files location.
logdir /var/log/chrony

# Stop bad estimates upsetting machine clock.
maxupdateskew 100.0

# This directive enables kernel synchronisation (every 11 minutes) of the
# real-time clock. Note that it can't be used along with the 'rtcfile' directive.
rtcsync

# Step the system clock instead of slewing it if the adjustment is larger than
# one second, but only in the first three clock updates.
makestep 1 3

# Get TAI-UTC offset and leap seconds from the system tz database.
# This directive must be commented out when using time sources serving
# leap-smeared time.
leapseclist /usr/share/zoneinfo/leap-seconds.list

# Include configuration files found in /etc/chrony/conf.d.
confdir /etc/chrony/conf.d

--- timedatectl
    $ timedatectl
               Local time: Wed 2026-07-29 05:14:02 CDT
           Universal time: Wed 2026-07-29 10:14:02 UTC
                 RTC time: Wed 2026-07-29 10:14:02
                Time zone: America/Chicago (CDT, -0500)
System clock synchronized: yes
              NTP service: active
          RTC in local TZ: no

--- chronyc tracking
    $ chronyc tracking
Reference ID    : 178FC4CC (time-usw7.crimpac.net)
Stratum         : 3
Ref time (UTC)  : Wed Jul 29 10:11:58 2026
System time     : 0.001178914 seconds fast of NTP time
Last offset     : +0.000033258 seconds
RMS offset      : 0.000184320 seconds
Frequency       : 8.307 ppm slow
Residual freq   : -0.000 ppm
Skew            : 0.077 ppm
Root delay      : 0.046502136 seconds
Root dispersion : 0.001698966 seconds
Update interval : 1033.0 seconds
Leap status     : Normal

--- chronyc sources
    $ chronyc sources
MS Name/IP address         Stratum Poll Reach LastRx Last sample               
===============================================================================
^+ 66.85.78.80                   2  10   377   516  +5707us[+5740us] +/-   54ms
^- 23.172.120.58                 2  10   377    70  -6376us[-6376us] +/-   77ms
^+ ntp2.wiktel.com               1  10   377   144  +2281us[+2315us] +/-   32ms
^* time-usw7.crimpac.net         2  10   377   125  -7945us[-7912us] +/-   25ms

--- ntpq peers
    $ ntpq -pn
/root/check.sh: line 45: ntpq: command not found
    [exit=127 / not installed or not permitted]

###############################################################################
# 28. FIREWALL / SECURITY
###############################################################################

--- pve-firewall status
    $ pve-firewall status
Status: disabled/running

--- nft ruleset (count)
    $ nft list ruleset

--- nft ruleset (head)
    $ nft list ruleset

--- iptables-save (legacy)
    $ iptables-save
# Generated by iptables-save v1.8.11 on Wed Jul 29 05:14:03 2026
*mangle
:PREROUTING ACCEPT [521415512:473930132553]
:INPUT ACCEPT [513714282:472995202599]
:FORWARD ACCEPT [0:0]
:OUTPUT ACCEPT [166489644:860411515115]
:POSTROUTING ACCEPT [166489644:860411515115]
-A PREROUTING -m conntrack --ctstate RELATED,ESTABLISHED -j CONNMARK --restore-mark --nfmask 0xff0000 --ctmask 0xff0000
-A OUTPUT -m conntrack --ctstate NEW -m mark ! --mark 0x0/0xff0000 -j CONNMARK --save-mark --nfmask 0xff0000 --ctmask 0xff0000
COMMIT
# Completed on Wed Jul 29 05:14:03 2026
# Generated by iptables-save v1.8.11 on Wed Jul 29 05:14:03 2026
*raw
:PREROUTING ACCEPT [521415562:473930154387]
:OUTPUT ACCEPT [166489713:860411521379]
COMMIT
# Completed on Wed Jul 29 05:14:03 2026
# Generated by iptables-save v1.8.11 on Wed Jul 29 05:14:03 2026
*nat
:PREROUTING ACCEPT [9059602:1041464125]
:INPUT ACCEPT [1642179:170001088]
:OUTPUT ACCEPT [156660:13029706]
:POSTROUTING ACCEPT [156660:13029706]
:ts-postrouting - [0:0]
-A POSTROUTING -j ts-postrouting
-A ts-postrouting -m mark --mark 0x40000/0xff0000 -j MASQUERADE
COMMIT
# Completed on Wed Jul 29 05:14:03 2026
# Generated by iptables-save v1.8.11 on Wed Jul 29 05:14:03 2026
*filter
:INPUT ACCEPT [512632870:472842959520]
:FORWARD ACCEPT [0:0]
:OUTPUT ACCEPT [166490912:860411574598]
:ts-forward - [0:0]
:ts-input - [0:0]
-A INPUT -j ts-input
-A FORWARD -j ts-forward
-A ts-forward -i tailscale0 -j MARK --set-xmark 0x40000/0xff0000
-A ts-forward -m mark --mark 0x40000/0xff0000 -j ACCEPT
-A ts-forward -s 100.64.0.0/10 -o tailscale0 -j DROP
-A ts-forward -o tailscale0 -j ACCEPT
-A ts-input -s 100.70.77.93/32 -i lo -j ACCEPT
-A ts-input -i tailscale0 -j ACCEPT
-A ts-input -p udp -m udp --dport 41641 -j ACCEPT
-A ts-input -s 100.115.92.0/23 ! -i tailscale0 -j RETURN
-A ts-input -s 100.64.0.0/10 ! -i tailscale0 -j DROP
COMMIT
# Completed on Wed Jul 29 05:14:03 2026

--- ipset list (names)
    $ ipset list -n

--- apparmor status
    $ aa-status
apparmor module is loaded.
6 profiles are loaded.
6 profiles are in enforce mode.
   /usr/bin/lxc-copy
   /usr/bin/lxc-start
   lxc-container-default
   lxc-container-default-cgns
   lxc-container-default-with-mounting
   lxc-container-default-with-nesting
0 profiles are in complain mode.
0 profiles are in prompt mode.
0 profiles are in kill mode.
0 profiles are in unconfined mode.
0 processes have profiles defined.
0 processes are in enforce mode.
0 processes are in complain mode.
0 processes are in prompt mode.
0 processes are in kill mode.
0 processes are unconfined but have a profile defined.
0 processes are in mixed mode.

###############################################################################
# 29. TOP CONSUMERS
###############################################################################

--- top 10 memory hogs
    $ ps -eo pid,user,rss,vsz,pcpu,pmem,comm --sort=-rss | head -n 11
    PID USER       RSS    VSZ %CPU %MEM COMMAND
   1622 root     899060 2862928 0.8  5.5 kvm
1197627 www-data 203864 269436 0.0  1.2 pveproxy worker
   1553 www-data 179008 220336 0.0  1.0 pveproxy
1197628 www-data 166264 234780 0.0  1.0 pveproxy worker
1197626 www-data 166260 234784 0.0  1.0 pveproxy worker
    961 root     96372 1422028 0.1  0.5 tailscaled
   1562 www-data 68352  92008  0.0  0.4 spiceproxy
 986538 root     64696 266928  0.0  0.3 pvedaemon worke
1197625 www-data 55488  92272  0.0  0.3 spiceproxy work
   1465 root     48272 180508  0.2  0.2 pvestatd

--- top 10 CPU hogs
    $ ps -eo pid,user,pcpu,pmem,rss,comm --sort=-pcpu | head -n 11
    PID USER     %CPU %MEM   RSS COMMAND
1248786 root      2.7  0.0  7904 systemd-timedat
   1622 root      0.8  5.5 899060 kvm
     94 root      0.3  0.0     0 kworker/7:1H-kblockd
   1465 root      0.2  0.2 48272 pvestatd
   1449 root      0.2  0.2 37724 pve-firewall
    961 root      0.1  0.5 96372 tailscaled
1245670 root      0.0  0.0  3824 bash
   1579 root      0.0  0.0     0 nfsd
   1589 root      0.0  0.0     0 nfsd
   1592 root      0.0  0.0     0 nfsd

--- top file-handle holders
    $ for pid in $(ps -e -o pid= | head -n 200); do
    n="$(ls /proc/$pid/fd 2>/dev/null | wc -l)"
    [ "$n" -gt 50 ] && printf '%6d fd=%-6s %s\n' "$pid" "$n" "$(cat /proc/$pid/comm 2>/dev/null)"
done | sort -k2 -t= -nr | head -n 15
     1 fd=194    systemd
  1411 fd=94     master
   937 fd=58     dbus-daemon

--- largest files in /var/log (top 10)
    $ find /var/log -type f -size +10M -exec ls -lh {} \; 2>/dev/null | sort -k5 -h -r | head -n 10
-rw-r-----+ 1 root systemd-journal 72M May  5 12:03 /var/log/journal/baf5d201679e4e6bb6556b9e7bc72f8b/system@9de2491ca6204af4abc9a3bb70197495-00000000000c198f-0006509d05c54c92.journal
-rw-r-----+ 1 root systemd-journal 72M May 29 05:57 /var/log/journal/baf5d201679e4e6bb6556b9e7bc72f8b/system@9de2491ca6204af4abc9a3bb70197495-0000000000132172-0006527b0796e828.journal
-rw-r-----+ 1 root systemd-journal 72M May 23 07:10 /var/log/journal/baf5d201679e4e6bb6556b9e7bc72f8b/system@9de2491ca6204af4abc9a3bb70197495-000000000011647e-000652034bfe3eab.journal
-rw-r-----+ 1 root systemd-journal 72M May 17 08:19 /var/log/journal/baf5d201679e4e6bb6556b9e7bc72f8b/system@9de2491ca6204af4abc9a3bb70197495-00000000000fa101-0006518bee28b2c8.journal
-rw-r-----+ 1 root systemd-journal 72M May 11 09:54 /var/log/journal/baf5d201679e4e6bb6556b9e7bc72f8b/system@9de2491ca6204af4abc9a3bb70197495-00000000000dd53f-0006511506a65c06.journal
-rw-r-----+ 1 root systemd-journal 72M Jun  4 03:06 /var/log/journal/baf5d201679e4e6bb6556b9e7bc72f8b/system@9de2491ca6204af4abc9a3bb70197495-000000000014dd9c-000652f2b69faaee.journal
-rw-r-----+ 1 root systemd-journal 72M Jun 27 16:46 /var/log/journal/baf5d201679e4e6bb6556b9e7bc72f8b/system@9de2491ca6204af4abc9a3bb70197495-00000000001be603-000654ccc38f89f2.journal
-rw-r-----+ 1 root systemd-journal 72M Jun 21 19:31 /var/log/journal/baf5d201679e4e6bb6556b9e7bc72f8b/system@9de2491ca6204af4abc9a3bb70197495-00000000001a260d-00065456241fdf96.journal
-rw-r-----+ 1 root systemd-journal 72M Jun 15 22:00 /var/log/journal/baf5d201679e4e6bb6556b9e7bc72f8b/system@9de2491ca6204af4abc9a3bb70197495-000000000018639a-000653df589e3988.journal
-rw-r-----+ 1 root systemd-journal 72M Jun 10 00:16 /var/log/journal/baf5d201679e4e6bb6556b9e7bc72f8b/system@9de2491ca6204af4abc9a3bb70197495-000000000016a0e9-00065369063b5267.journal

###############################################################################
# 30. QUICK-LOOK SUSPECT SUMMARY
###############################################################################

Auto-detected performance anti-patterns (verify against full data above):


--- [A] Network interfaces < 10 Gbps and up
    $ hits=0
for ifc in $NETIFS; do
    s=$(cat "/sys/class/net/$ifc/speed" 2>/dev/null)
    c=$(cat "/sys/class/net/$ifc/carrier" 2>/dev/null)
    case "$s" in
        10|100|1000)
            if [ "$c" = "1" ]; then
                printf '  %s : %s Mbps (UP)  <-- sub-10GbE; suspect if this carries storage/migration\n' "$ifc" "$s"
                hits=$((hits+1))
            fi
            ;;
    esac
done
[ "$hits" = "0" ] && echo "  no <10GbE interfaces are UP (or speed unreadable)"
  nic0 : 1000 Mbps (UP)  <-- sub-10GbE; suspect if this carries storage/migration
    [exit=1]


--- [B] MTU not jumbo on carrier-up interfaces
    $ hits=0
for ifc in $NETIFS; do
    m=$(cat "/sys/class/net/$ifc/mtu" 2>/dev/null)
    c=$(cat "/sys/class/net/$ifc/carrier" 2>/dev/null)
    [ "$c" = "1" ] || continue
    if [ -n "$m" ] && [ "$m" != "9000" ]; then
        printf '  %s : mtu=%s\n' "$ifc" "$m"
        hits=$((hits+1))
    fi
done
[ "$hits" = "0" ] && echo "  all carrier-up interfaces have MTU 9000 (or none are up)"
  datanet : mtu=1500
  enx8cae4ccda926 : mtu=1500
  fwbr400i0 : mtu=1500
  fwln400i0 : mtu=1500
  fwpr400p0 : mtu=1500
  nic0 : mtu=1500
  tap400i0 : mtu=1500
  vmbr0 : mtu=1500
    [exit=1]


--- [C] CPU governor != performance
    $ g=$(cat /sys/devices/system/cpu/cpu0/cpufreq/scaling_governor 2>/dev/null)
if [ -z "$g" ]; then
    echo "  cpufreq driver not loaded (governor unknown)"
elif [ "$g" = "performance" ]; then
    echo "  OK: performance governor"
else
    echo "  <-- governor=$g  (recommend 'performance')"
fi
  OK: performance governor


--- [D] EPB / EPP not performance-bias
    $ epb=$(cat /sys/devices/system/cpu/cpu0/power/energy_perf_bias 2>/dev/null)
epp=$(cat /sys/devices/system/cpu/cpu0/cpufreq/energy_performance_preference 2>/dev/null)
echo "  EPB=$epb  EPP=$epp  (0=performance, 15=max-power on EPB; 'performance' on EPP)"
  EPB=0  EPP=  (0=performance, 15=max-power on EPB; 'performance' on EPP)


--- [E] vm.swappiness and dirty ratios
    $ sw=$(sysctl -n vm.swappiness 2>/dev/null)
dr=$(sysctl -n vm.dirty_ratio 2>/dev/null)
dbr=$(sysctl -n vm.dirty_background_ratio 2>/dev/null)
echo "  swappiness=$sw  dirty_ratio=$dr  dirty_background_ratio=$dbr"
[ "$sw" != "10" ] && [ -n "$sw" ] && echo "    <-- swappiness not 10 (Proxmox default)"
  swappiness=1  dirty_ratio=40  dirty_background_ratio=10
    <-- swappiness not 10 (Proxmox default)


--- [F] TCP congestion control
    $ cc=$(sysctl -n net.ipv4.tcp_congestion_control 2>/dev/null)
avail=$(sysctl -n net.ipv4.tcp_available_congestion_control 2>/dev/null)
echo "  active: $cc"
echo "  available: $avail"
[ "$cc" = "cubic" ] && echo "    <-- consider bbr (if available) for high-BDP NFS paths"
  active: bbr
  available: reno cubic bbr
    [exit=1]


--- [G] ZFS dataset red flags
    $ if ! command -v zfs >/dev/null 2>&1; then
    echo "  ZFS not present"
else
    zfs get -r -o name,property,value compression,atime,sync,recordsize,xattr 2>/dev/null \
      | awk '$2=="compression" && $3=="off" {print "  <-- "$1" has compression=off"}
             $2=="atime" && $3=="on"        {print "  <-- "$1" has atime=on"}
             $2=="sync" && $3=="always"     {print "  <-- "$1" has sync=always (slow without SLOG)"}
             $2=="xattr" && $3=="on"        {print "  <-- "$1" has xattr=on (use sa)"}'
fi


--- [H] ARC size vs RAM
    $ if [ -r /proc/spl/kstat/zfs/arcstats ]; then
    arc=$(awk '/^size /{print $3}' /proc/spl/kstat/zfs/arcstats 2>/dev/null)
    cmax=$(awk '/^c_max /{print $3}' /proc/spl/kstat/zfs/arcstats 2>/dev/null)
    ram=$(awk '/MemTotal/{print $2*1024}' /proc/meminfo)
    echo "  ARC current=$arc bytes  ARC max=$cmax bytes  RAM total=$ram bytes"
    if [ -n "$cmax" ] && [ -n "$ram" ] && [ "$ram" -gt 0 ]; then
        pct=$((cmax * 100 / ram))
        echo "  ARC max is ${pct}% of RAM (Proxmox default ~50%)"
    fi
    hits=$(awk '/^hits /{print $3}' /proc/spl/kstat/zfs/arcstats 2>/dev/null)
    miss=$(awk '/^misses /{print $3}' /proc/spl/kstat/zfs/arcstats 2>/dev/null)
    if [ -n "$hits" ] && [ -n "$miss" ] && [ "$((hits+miss))" -gt 0 ]; then
        hr=$((hits * 100 / (hits + miss)))
        echo "  ARC hit rate since boot: ${hr}% (hits=$hits misses=$miss)"
    fi
else
    echo "  ZFS ARC stats not available (ZFS not loaded?)"
fi
  ARC current=1920 bytes  ARC max=1667235840 bytes  RAM total=16673505280 bytes
  ARC max is 9% of RAM (Proxmox default ~50%)


--- [I] VMs with non-optimal storage/NIC models
    $ hits=0
for vmid in $(qm list 2>/dev/null | awk 'NR>1{print $1}'); do
    cfg=$(qm config "$vmid" 2>/dev/null)
    flags=""
    echo "$cfg" | grep -qE '^ide[0-9]'                 && flags="${flags}ide-disk "
    echo "$cfg" | grep -qE '^sata[0-9]'                && flags="${flags}sata-disk "
    echo "$cfg" | grep -qE '^scsi[0-9].*:,'            && echo "$cfg" | grep -E '^scsi[0-9]' | grep -qv 'virtio-scsi' && flags="${flags}scsi-no-virtio-scsi "
    echo "$cfg" | grep -qE '^scsihw: ' && ! echo "$cfg" | grep -qE '^scsihw: virtio-scsi-single' && flags="${flags}scsihw!=virtio-scsi-single "
    echo "$cfg" | grep -qE '^cpu: .*kvm64'             && flags="${flags}cpu=kvm64 "
    echo "$cfg" | grep -q '^iothread: 1'               || echo "$cfg" | grep -qE '^scsi[0-9].*iothread=1' || flags="${flags}no-iothread "
    echo "$cfg" | grep -qE '^net[0-9].*model=(e1000|rtl8139|vmxnet)' && flags="${flags}legacy-nic "
    echo "$cfg" | grep -qE '^net[0-9].*model=virtio' && ! echo "$cfg" | grep -qE 'multiqueue=|queues=' && flags="${flags}virtio-no-multiqueue "
    if [ -n "$flags" ]; then
        echo "  VM $vmid: $flags"
        hits=$((hits+1))
    fi
done
[ "$hits" = "0" ] && echo "  no obvious VM storage/NIC anti-patterns"
  VM 400: ide-disk 
  VM 4000: ide-disk no-iothread 
    [exit=1]


--- [J] NFS client mount option red flags
    $ if ! command -v nfsstat >/dev/null 2>&1; then
    echo "  nfsstat not available"
else
    nfsstat -m 2>/dev/null | awk '
        /^.*:/ {mp=$0; next}
        /Flags:/ {
            gsub(/Flags:|,/,"",$0)
            line=$0
            if (line !~ /noatime/)        print "  "mp" : missing noatime"
            if (line !~ /nconnect/)       print "  "mp" : missing nconnect (kernel >=5.3)"
            if (line !~ /rsize=1048576/)  print "  "mp" : rsize<1M"
            if (line !~ /wsize=1048576/)  print "  "mp" : wsize<1M"
            if (line ~ /sync/)            print "  "mp" : sync mount (slow)"
        }
    '
fi


--- [K] Softnet / NIC drops (non-zero)
    $ awk 'NR<=32 && ($2+0 > 0 || $4+0 > 0) {printf "  cpu%d: dropped=%d time_squeezed=%d\n", NR-1, $2, $4}' /proc/net/softnet_stat
echo "  (also check ethtool -S sections above for rx_dropped/rx_missed_errors)"
  (also check ethtool -S sections above for rx_dropped/rx_missed_errors)


--- [L] Failed systemd services
    $ failed=$(systemctl --failed --no-legend 2>/dev/null | head -n 10)
if [ -n "$failed" ]; then
    echo "$failed" | sed 's/^/  /'
else
    echo "  no failed services"
fi
  ● conman.service loaded failed failed serial console management program


--- [M] Filesystem usage > 80%
    $ df -h 2>/dev/null | awk 'NR>1 && $5+0 > 80 {print "  "$0}'


--- [N] SMART / NVMe health warnings
    $ if command -v nvme >/dev/null 2>&1; then
    for n in /dev/nvme[0-9]*; do
        [ -b "$n" ] || continue
        crit=$(nvme smart-log "$n" 2>/dev/null | grep -iE 'critical_warning|media_and_data_integrity|available_spare' | head -n 5)
        [ -n "$crit" ] && echo "  $n: $crit" | tr '\n' ' '
    done
fi
if command -v smartctl >/dev/null 2>&1; then
    for d in $(ls /sys/block/ 2>/dev/null | grep -E '^sd'); do
        dev="/dev/$d"
        [ -b "$dev" ] || continue
        chk=$(smartctl -H "$dev" 2>/dev/null | grep -iE 'result|health|passed|failed')
        echo "$chk" | grep -qi fail && echo "  $dev: $chk"
    done
fi
echo "  (see section 20 for full smartctl/nvme output)"
  (see section 20 for full smartctl/nvme output)

###############################################################################
# Collection complete: pfv-tsys4
# Output:  /root/pfv-tsys4.log
# Size:    632237 bytes / 11200 lines
# Elapsed: 301 seconds
###############################################################################
