==== sw-capture 2026-07-26 16:18:17 ====
device=/dev/ttyUSB2 baud=9600 cmds=/root/pfv-core-sw01.cmds n=52 per_cmd_timeout=45.0




[Kpfv-core-sw01> enable


pfv-core-sw01# terminal datadump

pfv-core-sw01# show version

SW version    2.0.0.46 ( date  14-Apr-2011 time  13:10:53 )
Boot version    2.0.0.0 ( date  12-Nov-2008 time  12:56:52 )
HW version    00.00.02
pfv-core-sw01# show system

System Description:                       PowerConnect 5448
System Up Time (days,hour:min:sec):       176,02:17:35
System Contact:                           coo@turnsys.com
System Name:                              pfv-core-sw01
System Location:                          SITER1-ServerRoom-SiteR-Pflugerville
System MAC Address:                       a4:ba:db:6f:ce:28
System Object ID:                         1.3.6.1.4.1.674.10895.3021
Type:                                     Ethernet Switch
Asset tag:                                 
Service tag:                              D5WVFH1

Main Power Supply Status:                 OK
Fan 1 Status:                             OK
Fan 2 Status:                             OK
Fan 3 Status:                             OK


          Unit            Temperature (Celsius)            Status          
------------------------ ------------------------ ------------------------ 
           1                        48                       OK            


pfv-core-sw01# show inventory

% Unrecognized command
pfv-core-sw01# show bootvar

Image  Filename   Version     Date                    Status
-----  ---------  ---------   ---------------------   -----------
1      image-1    2.0.0.35    27-Jan-2009  18:13:34   Not active
2      image-2    2.0.0.46    14-Apr-2011  13:10:53   Active* 

"*" designates that the image was selected for the next boot

pfv-core-sw01# 