=== iperf3: tsys7→tsys6 TCP single-stream ===
Client: pfv-tsys7  Server: pfv-tsys6 (10.100.100.6)
Date: 2026-07-26T21:34:35Z
Args: /home/reachableceo/projects/perfopt/returned-logs/iperf/tsys6-tsys7-03-tcp-single.log -t 20 -O 2

Connecting to host 10.100.100.6, port 5201
[  5] local 10.100.100.7 port 47496 connected to 10.100.100.6 port 5201
[ ID] Interval           Transfer     Bitrate         Retr  Cwnd
[  5]   0.00-1.00   sec   114 MBytes   952 Mbits/sec    0    243 KBytes       (omitted)
[  5]   1.00-1.00   sec   113 MBytes   472 Mbits/sec    0    238 KBytes       
[  5]   1.00-2.00   sec   112 MBytes   941 Mbits/sec    0    240 KBytes       
[  5]   2.00-3.00   sec   112 MBytes   944 Mbits/sec    0    240 KBytes       
[  5]   3.00-4.00   sec   112 MBytes   942 Mbits/sec    0    240 KBytes       
[  5]   4.00-5.00   sec   112 MBytes   936 Mbits/sec    0    243 KBytes       
[  5]   5.00-6.00   sec   112 MBytes   942 Mbits/sec    0    243 KBytes       
[  5]   6.00-7.00   sec   113 MBytes   946 Mbits/sec    0    240 KBytes       
[  5]   7.00-8.00   sec   111 MBytes   934 Mbits/sec    0   5.66 KBytes       
[  5]   8.00-9.00   sec  96.9 MBytes   813 Mbits/sec    0    243 KBytes       
[  5]   9.00-10.00  sec   112 MBytes   941 Mbits/sec    0    240 KBytes       
[  5]  10.00-11.00  sec   112 MBytes   943 Mbits/sec    0    240 KBytes       
[  5]  11.00-12.00  sec   112 MBytes   940 Mbits/sec    0    243 KBytes       
[  5]  12.00-13.00  sec   113 MBytes   947 Mbits/sec    0    240 KBytes       
[  5]  13.00-14.00  sec   112 MBytes   938 Mbits/sec    0    240 KBytes       
[  5]  14.00-15.00  sec   112 MBytes   942 Mbits/sec    0    240 KBytes       
[  5]  15.00-16.00  sec   112 MBytes   942 Mbits/sec    0    240 KBytes       
[  5]  16.00-17.00  sec   113 MBytes   948 Mbits/sec    0    240 KBytes       
[  5]  17.00-18.00  sec   111 MBytes   932 Mbits/sec    0    240 KBytes       
[  5]  18.00-19.00  sec  96.8 MBytes   812 Mbits/sec    0    240 KBytes       
[  5]  19.00-20.00  sec   112 MBytes   943 Mbits/sec    0    240 KBytes       
- - - - - - - - - - - - - - - - - - - - - - - - -
[ ID] Interval           Transfer     Bitrate         Retr
[  5]   0.00-20.00  sec  2.16 GBytes   928 Mbits/sec    0            sender
[  5]   0.00-20.00  sec  2.16 GBytes   927 Mbits/sec                  receiver

iperf Done.

=== END ===
