=== iperf3: UDP saturation (tsys7→tsys5 PCI) ===
Client: pfv-tsys7 (10.100.100.7)
Server: pfv-tsys5 (10.100.100.5)
Direction: udp
Date: 2026-07-26T21:08:21Z

warning: UDP block size 8972 exceeds TCP MSS 1448, may result in fragmentation / drops
Connecting to host 10.100.100.5, port 5201
[  5] local 10.100.100.7 port 44414 connected to 10.100.100.5 port 5201
[ ID] Interval           Transfer     Bitrate         Total Datagrams
[  5]   0.00-1.00   sec   239 MBytes  2.00 Gbits/sec  27893  
[  5]   1.00-2.00   sec   238 MBytes  2.00 Gbits/sec  27855  
[  5]   2.00-3.00   sec   238 MBytes  2.00 Gbits/sec  27863  
[  5]   3.00-4.00   sec   238 MBytes  2.00 Gbits/sec  27865  
[  5]   4.00-5.00   sec   238 MBytes  2.00 Gbits/sec  27863  
[  5]   5.00-6.00   sec   238 MBytes  2.00 Gbits/sec  27866  
[  5]   6.00-7.00   sec   238 MBytes  2.00 Gbits/sec  27864  
[  5]   7.00-8.00   sec   239 MBytes  2.00 Gbits/sec  27876  
[  5]   8.00-9.00   sec   238 MBytes  2.00 Gbits/sec  27852  
[  5]   9.00-10.00  sec   238 MBytes  2.00 Gbits/sec  27865  
- - - - - - - - - - - - - - - - - - - - - - - - -
[ ID] Interval           Transfer     Bitrate         Jitter    Lost/Total Datagrams
[  5]   0.00-10.00  sec  2.33 GBytes  2.00 Gbits/sec  0.000 ms  0/278662 (0%)  sender
[  5]   0.00-10.21  sec  61.3 KBytes  49.2 Kbits/sec  2.404 ms  0/7 (0%)  receiver

iperf Done.

=== END ===
