! #369/#394: Convert cross-rack trunk ch1 from static (mode=on) to LACP
! Switch: pfv-r3-tor-stor (Dell PowerConnect 5324 / "Neyland 24T", rack 3)
! WHEN: Friday maintenance window — BOTH switches must change together
! RISK: Brief storage-net outage during transition (seconds)
!
! Current: g20-g23 in ch1, mode=on (static, no failure detection)
! Target:  g20-g23 in ch1, LACP active
!
! Radlan CLI syntax (different from DNOS on core-sw01)
! Verify exact keywords on this switch first — 'show running-config'
! will show the current ch1 config to confirm syntax.
!
! IMPORTANT: Run this SIMULTANEOUSLY with core-sw01 change.
!
enable
configure
interface range ethernet g20-g23
  no channel-group
  channel-group 1 mode active
exit
exit
show interfaces status port-channel 1
show lacp port-channel 1
copy running-config startup-config
