###############################################################################
# Proxmox VE host performance assessment  (READ-ONLY)
# Host:      pfv-tsys6 (pfv-tsys6.knel.net)
# FQDN:      pfv-tsys6.knel.net
# All IPs:   192.168.3.169 100.73.35.111 10.251.2.6 10.100.100.6 fd7a:115c:a1e0::df3b:236f 
# Collected: 2026-07-29T10:09:07Z (UTC)
# Kernel:    7.0.14-6-pve
# Machine:   x86_64 GNU/Linux
# Caller:    root (uid=0)
# Script:    check.sh  -  strictly READ-ONLY
###############################################################################

###############################################################################
# 1. TOOL AVAILABILITY MATRIX
###############################################################################

--- command presence + path + version
    $ # Each line: name | present? | path | version
printf '%-22s %-8s %-30s %s\n' "TOOL" "PRESENT" "PATH" "VERSION/NOTE"
printf '%-22s %-8s %-30s %s\n' "----" "-------" "----" "------------"
for t in \
    pveversion pvecm qm pct pvesm pvesh pveperf proxmox-backup-client \
    ip ss ethtool bridge brctl nmcli \
    tcpdump mtr nstat netstat nicstat ifstat \
    dmidecode lscpu lshw hwinfo inxi lspci lsusb numactl numastat \
    cpupower turbostat x86_energy_perf_policy rdmsr \
    tuned-adm irqbalance \
    zpool zfs zdb arcstat arc_summary \
    lsblk blkid blockdev findmnt smartctl nvme hdparm \
    storcli storcli64 MegaCli MegaCli64 tw-cli arcconf \
    sas2ircu sas3ircu hpssacli ssacli perccli \
    multipath pvs vgs lvs lvdisplay \
    xfs_info dumpe2fs btrfs \
    fio iperf iperf3 sysbench bonnie++ iozone \
    iostat mpstat pidstat sar vmstat \
    top htop atop glances dstat nethogs iftop iotop smem pmap slabtop \
    perf strace lsof fatrace \
    dig host nslookup \
    chronyc ntpq timedatectl \
    nft iptables iptables-save ipset ufw \
    jq bc awk smartctl nvme \
    apt dpkg
do
    p="$(command -v "$t" 2>/dev/null)"
    if [ -n "$p" ]; then
        v=""
        case "$t" in
            zpool|zfs)        v="$(timeout 3 "$t" version 2>/dev/null | head -n 2 | tr '\n' ' ')" ;;
            iperf3|fio|sysbench|smartctl|nvme|tuned-adm|ethtool|cpupower)
                v="$(timeout 3 "$t" --version 2>&1 | head -n 1)" ;;
            pveversion)       v="$(timeout 3 "$t" 2>/dev/null)" ;;
            storcli64|storcli|MegaCli64|MegaCli|arcconf|sas2ircu|sas3ircu|ssacli|hpssacli)
                v="(storage HBA CLI - present)" ;;
        esac
        printf '%-22s %-8s %-30s %s\n' "$t" "yes" "$p" "$v"
    else
        printf '%-22s %-8s %-30s %s\n' "$t" "no" "-" "-"
    fi
done
TOOL                   PRESENT  PATH                           VERSION/NOTE
----                   -------  ----                           ------------
pveversion             yes      /usr/bin/pveversion            pve-manager/9.2.5/20242970da7fbcef (running kernel: 7.0.14-6-pve)
pvecm                  yes      /usr/bin/pvecm                 
qm                     yes      /usr/sbin/qm                   
pct                    yes      /usr/sbin/pct                  
pvesm                  yes      /usr/sbin/pvesm                
pvesh                  yes      /usr/bin/pvesh                 
pveperf                yes      /usr/bin/pveperf               
proxmox-backup-client  yes      /usr/bin/proxmox-backup-client 
ip                     yes      /usr/sbin/ip                   
ss                     yes      /usr/bin/ss                    
ethtool                yes      /usr/sbin/ethtool              ethtool version 6.14.2
bridge                 yes      /usr/sbin/bridge               
brctl                  yes      /usr/sbin/brctl                
nmcli                  no       -                              -
tcpdump                yes      /usr/bin/tcpdump               
mtr                    yes      /usr/bin/mtr                   
nstat                  yes      /usr/bin/nstat                 
netstat                no       -                              -
nicstat                no       -                              -
ifstat                 no       -                              -
dmidecode              yes      /usr/sbin/dmidecode            
lscpu                  yes      /usr/bin/lscpu                 
lshw                   no       -                              -
hwinfo                 no       -                              -
inxi                   no       -                              -
lspci                  yes      /usr/bin/lspci                 
lsusb                  yes      /usr/bin/lsusb                 
numactl                yes      /usr/bin/numactl               
numastat               yes      /usr/bin/numastat              
cpupower               yes      /usr/bin/cpupower              cpupower 6.12
turbostat              yes      /usr/sbin/turbostat            
x86_energy_perf_policy yes      /usr/sbin/x86_energy_perf_policy 
rdmsr                  no       -                              -
tuned-adm              yes      /usr/sbin/tuned-adm            tuned-adm 2.25.1
irqbalance             no       -                              -
zpool                  yes      /usr/sbin/zpool                zfs-2.4.3-pve1 zfs-kmod-2.4.3-pve1 
zfs                    yes      /usr/sbin/zfs                  zfs-2.4.3-pve1 zfs-kmod-2.4.3-pve1 
zdb                    yes      /usr/sbin/zdb                  
arcstat                yes      /usr/sbin/arcstat              
arc_summary            yes      /usr/sbin/arc_summary          
lsblk                  yes      /usr/bin/lsblk                 
blkid                  yes      /usr/sbin/blkid                
blockdev               yes      /usr/sbin/blockdev             
findmnt                yes      /usr/bin/findmnt               
smartctl               yes      /usr/sbin/smartctl             smartctl 7.5 2025-04-30 r5714 [x86_64-linux-7.0.14-6-pve] (local build)
nvme                   yes      /usr/sbin/nvme                 nvme version 2.13 (git 2.13)
hdparm                 yes      /usr/sbin/hdparm               
storcli                no       -                              -
storcli64              no       -                              -
MegaCli                no       -                              -
MegaCli64              no       -                              -
tw-cli                 no       -                              -
arcconf                no       -                              -
sas2ircu               no       -                              -
sas3ircu               no       -                              -
hpssacli               no       -                              -
ssacli                 no       -                              -
perccli                no       -                              -
multipath              no       -                              -
pvs                    yes      /usr/sbin/pvs                  
vgs                    yes      /usr/sbin/vgs                  
lvs                    yes      /usr/sbin/lvs                  
lvdisplay              yes      /usr/sbin/lvdisplay            
xfs_info               yes      /usr/sbin/xfs_info             
dumpe2fs               yes      /usr/sbin/dumpe2fs             
btrfs                  yes      /usr/bin/btrfs                 
fio                    no       -                              -
iperf                  no       -                              -
iperf3                 yes      /usr/bin/iperf3                iperf 3.18 (cJSON 1.7.15)
sysbench               no       -                              -
bonnie++               no       -                              -
iozone                 no       -                              -
iostat                 yes      /usr/bin/iostat                
mpstat                 yes      /usr/bin/mpstat                
pidstat                yes      /usr/bin/pidstat               
sar                    yes      /usr/bin/sar                   
vmstat                 yes      /usr/bin/vmstat                
top                    yes      /usr/bin/top                   
htop                   no       -                              -
atop                   no       -                              -
glances                no       -                              -
dstat                  no       -                              -
nethogs                no       -                              -
iftop                  no       -                              -
iotop                  no       -                              -
smem                   no       -                              -
pmap                   yes      /usr/bin/pmap                  
slabtop                yes      /usr/bin/slabtop               
perf                   yes      /usr/bin/perf                  
strace                 yes      /usr/bin/strace                
lsof                   yes      /usr/bin/lsof                  
fatrace                no       -                              -
dig                    yes      /usr/bin/dig                   
host                   yes      /usr/bin/host                  
nslookup               yes      /usr/bin/nslookup              
chronyc                yes      /usr/bin/chronyc               
ntpq                   no       -                              -
timedatectl            yes      /usr/bin/timedatectl           
nft                    yes      /usr/sbin/nft                  
iptables               yes      /usr/sbin/iptables             
iptables-save          yes      /usr/sbin/iptables-save        
ipset                  yes      /usr/sbin/ipset                
ufw                    no       -                              -
jq                     yes      /usr/bin/jq                    
bc                     yes      /usr/bin/bc                    
awk                    yes      /usr/bin/awk                   
smartctl               yes      /usr/sbin/smartctl             smartctl 7.5 2025-04-30 r5714 [x86_64-linux-7.0.14-6-pve] (local build)
nvme                   yes      /usr/sbin/nvme                 nvme version 2.13 (git 2.13)
apt                    yes      /usr/bin/apt                   
dpkg                   yes      /usr/bin/dpkg                  

--- Debian packages relevant to perf/storage/net
    $ dpkg -l 2>/dev/null | awk '/^ii/ && ($2 ~ /^(proxmox-|pve-|zfs|zfsutils|nfs|nfs-kernel-server|nfs-common|open-iscsi|ceph|tuned|irqbalance|sysstat|smartmontools|nvme-cli|ethtool|bridge-utils|ifenslave|fio|iperf3|sysbench|glances|htop|atop|lm-sensors|numactl|cpufrequtils|linux-image-|pve-kernel|qemu|libvirt|corosync|pacemaker)/) {print $2"  "$3}' | head -n 80
bridge-utils  1.7.1-4+b1
ceph-common  19.2.3-pve2
ceph-fuse  19.2.3-pve2
corosync  3.1.10-pve3
ethtool  1:6.14.2-1
iperf3  3.18-2+deb13u2
nfs-common  1:2.8.3-1
numactl  2.0.19-1
nvme-cli  2.13-2
open-iscsi  2.1.11-1+deb13u2
proxmox-archive-keyring  4.0
proxmox-backup-client  4.2.3-1
proxmox-backup-file-restore  4.2.3-1
proxmox-backup-restore-image  1.0.0
proxmox-default-kernel  2.1.0
proxmox-enterprise-support-keyring  1.0
proxmox-firewall  1.2.3
proxmox-kernel-6.17  6.17.13-19
proxmox-kernel-6.17.13-19-pve-signed  6.17.13-19
proxmox-kernel-6.17.2-1-pve-signed  6.17.2-1
proxmox-kernel-7.0  7.0.14-6
proxmox-kernel-7.0.14-6-pve-signed  7.0.14-6
proxmox-kernel-helper  9.2.0
proxmox-mail-forward  1.0.3
proxmox-mini-journalreader  1.7
proxmox-offline-mirror-docs  0.7.4
proxmox-offline-mirror-helper  0.7.4
proxmox-termproxy  2.1.0
proxmox-ve  9.2.0
proxmox-websocket-tunnel  1.0.0
proxmox-widget-toolkit  5.2.6
pve-cluster  9.1.6
pve-container  6.1.12
pve-docs  9.2.3
pve-edk2-firmware  4.2025.05-2
pve-edk2-firmware-legacy  4.2025.05-2
pve-edk2-firmware-ovmf  4.2025.05-2
pve-esxi-import-tools  1.0.1
pve-firewall  6.0.5
pve-firmware  3.18-5
pve-ha-manager  5.2.4
pve-i18n  3.9.0
pve-lxc-syscalld  2.0.2
pve-manager  9.2.5
pve-nvidia-vgpu-helper  0.3.1
pve-qemu-kvm  11.0.2-2
pve-xtermjs  6.0.0-2
pve-yew-mobile-gui  0.7.0
pve-yew-mobile-i18n  3.9.0
qemu-server  9.2.1
smartmontools  7.5-pve2
sysstat  12.7.5-2
tuned  2.25.1-1
zfs-initramfs  2.4.3-pve1
zfs-zed  2.4.3-pve1
zfsutils-linux  2.4.3-pve1

--- kernel modules available (relevant to perf)
    $ for m in kvm_intel kvm_amd \
         ixgbe i40e i40iw ice igb igc mlx4_en mlx5_core mlx4_core bnx2x bnx2 tg3 be2net qed qede virtio_net \
         nvme nvme-tcp nvme-fabrics sd_mod sr_mod \
         zfs spl znvpair zcommon zunicode zavl icp zlua \
         megaraid_sas mpt3sas hpsa aacraid smartpqi isci \
         dm_multipath multipath \
         tcp_dctcp tcp_bbr tcp_cubic tcp_htcp \
         8021q bonding bridge br_netfilter \
         vhost_net vhost_scsi target_core_mod \
         nfsv4 nfsv3 rpcsec_gss_krb5
do
    modinfo "$m" >/dev/null 2>&1 && printf 'available : %s (%s)\n' "$m" "$(modinfo -F version "$m" 2>/dev/null || echo built-in)"
done
available : kvm_intel ()
available : kvm_amd ()
available : ixgbe ()
available : i40e ()
available : i40iw ()
available : ice ()
available : igb ()
available : igc ()
available : mlx4_en (4.0-0)
available : mlx5_core ()
available : mlx4_core (4.0-0)
available : bnx2x ()
available : bnx2 ()
available : tg3 ()
available : be2net ()
available : qed ()
available : qede ()
available : virtio_net ()
available : nvme (1.0)
available : nvme-tcp ()
available : nvme-fabrics ()
available : sd_mod ()
available : sr_mod ()
available : zfs (2.4.3-pve1)
available : spl (2.4.3-pve1)
available : znvpair (2.4.3-pve1)
available : zcommon (2.4.3-pve1)
available : zunicode (2.4.3-pve1)
available : zavl (2.4.3-pve1)
available : icp (2.4.3-pve1)
available : zlua (2.4.3-pve1)
available : megaraid_sas (07.734.00.00-rc1)
available : mpt3sas (54.100.00.00)
available : hpsa (3.4.20-200)
available : aacraid (1.2.1[50983]-custom)
available : smartpqi (2.1.36-026)
available : isci (1.2.0)
available : dm_multipath ()
available : tcp_dctcp ()
available : tcp_bbr ()
available : tcp_cubic (2.3)
available : tcp_htcp ()
available : 8021q (1.8)
available : bonding ()
available : bridge (2.3)
available : br_netfilter ()
available : vhost_net (0.0.1)
available : vhost_scsi ()
available : target_core_mod ()
available : nfsv4 ()
available : nfsv3 ()
available : rpcsec_gss_krb5 ()

--- currently loaded modules (filtered)
    $ lsmod | awk 'NR==1 || $1 ~ /^(kvm|virtio|vhost|ixgb|i40e|ice|igb|mlx|bnx|tg3|be2|qed|nvme|zfs|spl|z|dm_|megaraid|mpt|hpsa|aacraid|smartpqi|8021q|bonding|bridge|nfsv|tcp_|rpc|sunrpc|loop)/{print}'
Module                  Size  Used by
tcp_diag               20480  0
rpcsec_gss_krb5        32768  0
nfsv4                1200128  2
8021q                  49152  0
sunrpc                815104  23 nfsv4,auth_rpcgss,lockd,rpcsec_gss_krb5,nfs
bonding               253952  0
kvm_intel             507904  18
kvm                  1445888  13 kvm_intel
zfs                  6258688  6
spl                   151552  1 zfs
vhost_net              36864  3
vhost                  69632  1 vhost_net
nvme_fabrics           36864  0
vhost_iotlb            16384  1 vhost
nvme_core             229376  1 nvme_fabrics
nvme_keyring           20480  2 nvme_core,nvme_fabrics
nvme_auth              28672  1 nvme_core
tcp_bbr                24576  29
dm_thin_pool           94208  1
dm_persistent_data    118784  1 dm_thin_pool
dm_bio_prison          24576  1 dm_thin_pool
dm_bufio               57344  1 dm_persistent_data
bnx2                  106496  0

###############################################################################
# 2. OS / DISTRO / UPTIME
###############################################################################

--- os-release
    --- /etc/os-release ---
PRETTY_NAME="Debian GNU/Linux 13 (trixie)"
NAME="Debian GNU/Linux"
VERSION_ID="13"
VERSION="13 (trixie)"
VERSION_CODENAME=trixie
DEBIAN_VERSION_FULL=13.6
ID=debian
HOME_URL="https://www.debian.org/"
SUPPORT_URL="https://www.debian.org/support"
BUG_REPORT_URL="https://bugs.debian.org/"

--- debian version
    $ cat /etc/debian_version
13.6

--- uptime
    $ uptime
 05:09:13 up 2 days, 11:49,  1 user,  load average: 0.48, 0.34, 0.29

--- uptime raw (since boot)
    $ cat /proc/uptime
215395.72 3341276.25

--- last reboot
    $ last -x reboot
reboot   system boot  7.0.14-6-pve     Sun Jul 26 17:19 - still running
reboot   system boot  6.17.2-1-pve     Sun Jul 26 16:17 - 17:14  (00:56)
shutdown system down  6.17.2-1-pve     Sun Jul 26 17:14 - 17:19  (00:04)
reboot   system boot  6.17.2-1-pve     Fri Jul 24 13:39 - 16:12 (2+02:33)
shutdown system down  6.17.2-1-pve     Sun Jul 26 16:12 - 16:17  (00:04)
reboot   system boot  6.17.2-1-pve     Thu Jul 23 10:58 - 10:45  (23:47)
shutdown system down  6.17.2-1-pve     Fri Jul 24 10:45 - 13:39  (02:53)
reboot   system boot  6.17.2-1-pve     Fri Jun 19 03:04 - 18:06 (33+15:02)
shutdown system down  6.17.2-1-pve     Wed Jul 22 18:06 - 10:58  (16:51)
reboot   system boot  6.17.2-1-pve     Fri Jun 19 03:00 - crash 
reboot   system boot  6.17.2-1-pve     Wed May 20 12:05 - crash 
reboot   system boot  6.17.2-1-pve     Wed May 20 11:28 - crash 
reboot   system boot  6.17.2-1-pve     Wed May 20 09:36 - crash 
reboot   system boot  6.17.2-1-pve     Wed May 20 08:39 - crash 
reboot   system boot  6.17.2-1-pve     Sun May 10 21:59 - crash 
reboot   system boot  6.17.2-1-pve     Sun May 10 21:55 - crash 
reboot   system boot  6.17.2-1-pve     Sun Apr  5 04:48 - crash 
reboot   system boot  6.17.2-1-pve     Sun Apr  5 04:27 - 04:46  (00:18)
shutdown system down  6.17.2-1-pve     Sun Apr  5 04:46 - 04:48  (00:01)
reboot   system boot  6.17.2-1-pve     Sat Apr  4 12:52 - 04:25  (15:32)
shutdown system down  6.17.2-1-pve     Sun Apr  5 04:25 - 04:27  (00:02)
reboot   system boot  6.17.2-1-pve     Sat Apr  4 12:46 - 12:50  (00:04)
shutdown system down  6.17.2-1-pve     Sat Apr  4 12:50 - 12:52  (00:01)

wtmpdb begins Sat Apr  4 12:46:05 2026

--- last logins
    $ last
root     pts/0        100.87.49.37     Mon Jul 27 08:43 - 08:43  (00:00)
reboot   system boot  7.0.14-6-pve     Sun Jul 26 17:19 - still running
root     pts/2        100.87.49.37     Sun Jul 26 17:12 - 17:12  (00:00)
root     pts/0        100.87.49.37     Sun Jul 26 17:10 - 17:14  (00:03)
reboot   system boot  6.17.2-1-pve     Sun Jul 26 16:17 - 17:14  (00:56)
root     pts/0        100.87.49.37     Sun Jul 26 12:22 - 12:25  (00:03)
root     pts/0        100.87.49.37     Sun Jul 26 11:51 - 11:54  (00:03)
root     pts/0        100.87.49.37     Sun Jul 26 09:30 - 09:33  (00:03)
root     pts/0        100.87.49.37     Sun Jul 26 09:21 - 09:28  (00:07)
root     pts/0        100.87.49.37     Sat Jul 25 11:35 - 11:37  (00:01)
root     pts/0        100.87.49.37     Sat Jul 25 01:24 - 01:29  (00:04)
reboot   system boot  6.17.2-1-pve     Fri Jul 24 13:39 - 16:12 (2+02:33)
root     pts/0        100.87.49.37     Fri Jul 24 10:45 - 10:45  (00:00)
root     pts/0        100.87.49.37     Thu Jul 23 13:55 - 13:55  (00:00)
root     pts/0        100.87.49.37     Thu Jul 23 13:51 - 13:52  (00:00)
reboot   system boot  6.17.2-1-pve     Thu Jul 23 10:58 - 10:45  (23:47)
root     pts/0        100.87.49.37     Wed Jul 22 17:40 - 17:44  (00:03)
root     pts/0        100.87.49.37     Wed Jul 22 17:24 - 17:25  (00:00)
root     pts/0        100.87.49.37     Wed Jul 22 17:01 - 17:20  (00:19)
root     pts/0        100.87.49.37     Mon Jul 20 19:02 - 19:04  (00:01)
root     pts/1        100.87.49.37     Mon Jul 20 12:28 - 12:28  (00:00)
root     pts/0        100.109.70.137   Mon Jul 20 12:26 - 17:16  (04:50)
root     pts/0        100.87.49.37     Mon Jul 20 11:29 - 11:29  (00:00)
root     pts/0        100.87.49.37     Mon Jul 20 11:29 - 11:29  (00:00)
root     pts/0        100.87.49.37     Mon Jul 20 11:13 - 11:13  (00:00)
root     pts/0        100.87.49.37     Mon Jul 20 10:58 - 10:58  (00:00)
root     pts/0        100.87.49.37     Mon Jul 20 10:51 - 10:52  (00:00)
reboot   system boot  6.17.2-1-pve     Fri Jun 19 03:04 - 18:06 (33+15:02)
reboot   system boot  6.17.2-1-pve     Fri Jun 19 03:00 - crash 
reboot   system boot  6.17.2-1-pve     Wed May 20 12:05 - crash 
reboot   system boot  6.17.2-1-pve     Wed May 20 11:28 - crash 
reboot   system boot  6.17.2-1-pve     Wed May 20 09:36 - crash 
reboot   system boot  6.17.2-1-pve     Wed May 20 08:39 - crash 
reboot   system boot  6.17.2-1-pve     Sun May 10 21:59 - crash 
reboot   system boot  6.17.2-1-pve     Sun May 10 21:55 - crash 
root     pts/0        100.118.91.16    Mon Apr 27 13:47 - 13:47  (00:00)
root     pts/0        100.118.91.16    Mon Apr 27 13:44 - 13:45  (00:00)
root     pts/0        100.118.91.16    Mon Apr 27 12:48 - 12:56  (00:07)
root     pts/0        100.118.91.16    Mon Apr  6 17:20 - 17:20  (00:00)
root     pts/0        100.118.91.16    Mon Apr  6 09:43 - 09:43  (00:00)
root     pts/0        100.118.91.16    Sun Apr  5 11:23 - 11:26  (00:02)
root     pts/0        192.168.3.32     Sun Apr  5 10:02 - 10:04  (00:02)
root     tty1                          Sun Apr  5 04:50 - 09:54  (05:04)
reboot   system boot  6.17.2-1-pve     Sun Apr  5 04:48 - crash 
root     tty2                          Sun Apr  5 04:45 - 04:46  (00:00)
root     tty1                          Sun Apr  5 04:30 - 04:46  (00:16)
reboot   system boot  6.17.2-1-pve     Sun Apr  5 04:27 - 04:46  (00:18)
root     tty1                          Sat Apr  4 12:57 - 04:25  (15:28)
reboot   system boot  6.17.2-1-pve     Sat Apr  4 12:52 - 04:25  (15:32)
root     tty1                          Sat Apr  4 12:48 - 12:50  (00:02)
reboot   system boot  6.17.2-1-pve     Sat Apr  4 12:46 - 12:50  (00:04)

wtmpdb begins Sat Apr  4 12:46:05 2026

--- uname
    $ uname -a
Linux pfv-tsys6 7.0.14-6-pve #1 SMP PREEMPT_DYNAMIC PMX 7.0.14-6 (2026-07-20T14:45Z) x86_64 GNU/Linux

--- /proc/cmdline (boot args)
    $ cat /proc/cmdline
BOOT_IMAGE=/boot/vmlinuz-7.0.14-6-pve root=/dev/mapper/pve-root ro intel_iommu=off quiet

###############################################################################
# 3. HARDWARE INVENTORY
###############################################################################

--- dmidecode -t system
    $ dmidecode -t system
# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 2.6 present.

Handle 0x0100, DMI type 1, 27 bytes
System Information
	Manufacturer: Dell Inc.
	Product Name: PowerEdge R610
	Version: Not Specified
	Serial Number: 3B5DSL1
	UUID: 4c4c4544-0042-3510-8044-b3c04f534c31
	Wake-up Type: Power Switch
	SKU Number: Not Specified
	Family: Not Specified

Handle 0x0C00, DMI type 12, 5 bytes
System Configuration Options
	Option 1: NVRAM_CLR:  Clear user settable NVRAM areas and set defaults
	Option 2: PWRD_EN:  Close to enable password

Handle 0x2000, DMI type 32, 11 bytes
System Boot Information
	Status: No errors detected


--- dmidecode -t baseboard
    $ dmidecode -t baseboard
# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 2.6 present.

Handle 0x0200, DMI type 2, 9 bytes
Base Board Information
	Manufacturer: Dell Inc.
	Product Name: 0XDN97
	Version: A09
	Serial Number: ..CN7016304R017M.
	Asset Tag: Not Specified

Handle 0x0A00, DMI type 10, 14 bytes
On Board Device 1 Information
	Type: Video
	Status: Enabled
	Description: Embedded Matrox G200 Video
On Board Device 2 Information
	Type: Ethernet
	Status: Enabled
	Description: Embedded Broadcom 5709C NIC 1
On Board Device 3 Information
	Type: Ethernet
	Status: Enabled
	Description: Embedded Broadcom 5709C NIC 2
On Board Device 4 Information
	Type: Ethernet
	Status: Enabled
	Description: Embedded Broadcom 5709C NIC 3
On Board Device 5 Information
	Type: Ethernet
	Status: Enabled
	Description: Embedded Broadcom 5709C NIC 4

Handle 0x2900, DMI type 41, 11 bytes
Onboard Device
	Reference Designation: Embedded NIC 1                          
	Type: Ethernet
	Status: Enabled
	Type Instance: 1
	Bus Address: 0000:01:00.0

Handle 0x2901, DMI type 41, 11 bytes
Onboard Device
	Reference Designation: Embedded NIC 2                          
	Type: Ethernet
	Status: Enabled
	Type Instance: 2
	Bus Address: 0000:01:00.1

Handle 0x2902, DMI type 41, 11 bytes
Onboard Device
	Reference Designation: Embedded NIC 3                          
	Type: Ethernet
	Status: Enabled
	Type Instance: 3
	Bus Address: 0000:02:00.0

Handle 0x2903, DMI type 41, 11 bytes
Onboard Device
	Reference Designation: Embedded NIC 4                          
	Type: Ethernet
	Status: Enabled
	Type Instance: 4
	Bus Address: 0000:02:00.1

Handle 0x2904, DMI type 41, 11 bytes
Onboard Device
	Reference Designation:                                         
	Type: SAS Controller
	Status: Disabled
	Type Instance: 4

Handle 0x2906, DMI type 41, 11 bytes
Onboard Device
	Reference Designation: Embedded Video                          
	Type: Video
	Status: Enabled
	Type Instance: 4
	Bus Address: 0000:06:03.0


--- dmidecode -t bios
    $ dmidecode -t bios
# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 2.6 present.

Handle 0x0000, DMI type 0, 24 bytes
BIOS Information
	Vendor: Dell Inc.
	Version: 2.0.13
	Release Date: 04/06/2010
	Address: 0xF0000
	Runtime Size: 64 kB
	ROM Size: 4 MB
	Characteristics:
		ISA is supported
		PCI is supported
		PNP is supported
		BIOS is upgradeable
		BIOS shadowing is allowed
		Boot from CD is supported
		Selectable boot is supported
		EDD is supported
		Japanese floppy for Toshiba 1.2 MB is supported (int 13h)
		5.25"/360 kB floppy services are supported (int 13h)
		5.25"/1.2 MB floppy services are supported (int 13h)
		3.5"/720 kB floppy services are supported (int 13h)
		8042 keyboard services are supported (int 9h)
		Serial services are supported (int 14h)
		CGA/mono video services are supported (int 10h)
		ACPI is supported
		USB legacy is supported
		BIOS boot specification is supported
		Function key-initiated network boot is supported
		Targeted content distribution is supported
	BIOS Revision: 2.0

Handle 0x0D00, DMI type 13, 22 bytes
BIOS Language Information
	Language Description Format: Long
	Installable Languages: 1
		en|US|iso8859-1
	Currently Installed Language: en|US|iso8859-1


--- dmidecode -t chassis
    $ dmidecode -t chassis
# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 2.6 present.

Handle 0x0300, DMI type 3, 21 bytes
Chassis Information
	Manufacturer: Dell Inc.
	Type: Rack Mount Chassis
	Lock: Present
	Version: Not Specified
	Serial Number: 3B5DSL1
	Asset Tag:           
	Boot-up State: Safe
	Power Supply State: Safe
	Thermal State: Safe
	Security Status: Unknown
	OEM Information: 0x00000000
	Height: 1 U
	Number Of Power Cords: Unspecified
	Contained Elements: 0


--- dmidecode -t processor
    $ dmidecode -t processor
# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 2.6 present.

Handle 0x0400, DMI type 4, 40 bytes
Processor Information
	Socket Designation: CPU1
	Type: Central Processor
	Family: Xeon
	Manufacturer: Intel
	ID: A5 06 01 00 FF FB EB BF
	Signature: Type 0, Family 6, Model 26, Stepping 5
	Flags:
		FPU (Floating-point unit on-chip)
		VME (Virtual mode extension)
		DE (Debugging extension)
		PSE (Page size extension)
		TSC (Time stamp counter)
		MSR (Model specific registers)
		PAE (Physical address extension)
		MCE (Machine check exception)
		CX8 (CMPXCHG8 instruction supported)
		APIC (On-chip APIC hardware supported)
		SEP (Fast system call)
		MTRR (Memory type range registers)
		PGE (Page global enable)
		MCA (Machine check architecture)
		CMOV (Conditional move instruction supported)
		PAT (Page attribute table)
		PSE-36 (36-bit page size extension)
		CLFSH (CLFLUSH instruction supported)
		DS (Debug store)
		ACPI (ACPI supported)
		MMX (MMX technology supported)
		FXSR (FXSAVE and FXSTOR instructions supported)
		SSE (Streaming SIMD extensions)
		SSE2 (Streaming SIMD extensions 2)
		SS (Self-snoop)
		HTT (Multi-threading)
		TM (Thermal monitor supported)
		PBE (Pending break enabled)
	Version: Intel(R) Xeon(R) CPU           E5530  @ 2.40GHz
	Voltage: 1.2 V
	External Clock: 5860 MHz
	Max Speed: 3600 MHz
	Current Speed: 2400 MHz
	Status: Populated, Enabled
	Upgrade: Socket LGA1366
	L1 Cache Handle: 0x0700
	L2 Cache Handle: 0x0701
	L3 Cache Handle: 0x0702
	Serial Number: Not Specified
	Asset Tag: Not Specified
	Part Number: Not Specified
	Core Count: 4
	Core Enabled: 4
	Thread Count: 8
	Characteristics:
		64-bit capable

Handle 0x0401, DMI type 4, 40 bytes
Processor Information
	Socket Designation: CPU2
	Type: Central Processor
	Family: Xeon
	Manufacturer: Intel
	ID: A5 06 01 00 FF FB EB BF
	Signature: Type 0, Family 6, Model 26, Stepping 5
	Flags:
		FPU (Floating-point unit on-chip)
		VME (Virtual mode extension)
		DE (Debugging extension)
		PSE (Page size extension)
		TSC (Time stamp counter)
		MSR (Model specific registers)
		PAE (Physical address extension)
		MCE (Machine check exception)
		CX8 (CMPXCHG8 instruction supported)
		APIC (On-chip APIC hardware supported)
		SEP (Fast system call)
		MTRR (Memory type range registers)
		PGE (Page global enable)
		MCA (Machine check architecture)
		CMOV (Conditional move instruction supported)
		PAT (Page attribute table)
		PSE-36 (36-bit page size extension)
		CLFSH (CLFLUSH instruction supported)
		DS (Debug store)
		ACPI (ACPI supported)
		MMX (MMX technology supported)
		FXSR (FXSAVE and FXSTOR instructions supported)
		SSE (Streaming SIMD extensions)
		SSE2 (Streaming SIMD extensions 2)
		SS (Self-snoop)
		HTT (Multi-threading)
		TM (Thermal monitor supported)
		PBE (Pending break enabled)
	Version: Intel(R) Xeon(R) CPU           E5530  @ 2.40GHz
	Voltage: 1.2 V
	External Clock: 5860 MHz
	Max Speed: 3600 MHz
	Current Speed: 2400 MHz
	Status: Populated, Idle
	Upgrade: Socket LGA1366
	L1 Cache Handle: 0x0703
	L2 Cache Handle: 0x0704
	L3 Cache Handle: 0x0705
	Serial Number: Not Specified
	Asset Tag: Not Specified
	Part Number: Not Specified
	Core Count: 4
	Core Enabled: 4
	Thread Count: 8
	Characteristics:
		64-bit capable


--- dmidecode -t memory
    $ dmidecode -t memory
# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 2.6 present.

Handle 0x1000, DMI type 16, 15 bytes
Physical Memory Array
	Location: System Board Or Motherboard
	Use: System Memory
	Error Correction Type: Multi-bit ECC
	Maximum Capacity: 192 GB
	Error Information Handle: Not Provided
	Number Of Devices: 12

Handle 0x1100, DMI type 17, 28 bytes
Memory Device
	Array Handle: 0x1000
	Error Information Handle: Not Provided
	Total Width: 72 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: 1
	Locator: DIMM_A1 
	Bank Locator: Not Specified
	Type: DDR3
	Type Detail: Synchronous Registered (Buffered)
	Speed: 1333 MT/s
	Manufacturer: 00CE00B380CE
	Serial Number: 352705DF
	Asset Tag: 02124963
	Part Number: M393B2G70BH0-YH9  
	Rank: 2

Handle 0x1101, DMI type 17, 28 bytes
Memory Device
	Array Handle: 0x1000
	Error Information Handle: Not Provided
	Total Width: 72 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: 1
	Locator: DIMM_A2 
	Bank Locator: Not Specified
	Type: DDR3
	Type Detail: Synchronous Registered (Buffered)
	Speed: 1333 MT/s
	Manufacturer: 00CE00B380CE
	Serial Number: 352703F3
	Asset Tag: 02124963
	Part Number: M393B2G70BH0-YH9  
	Rank: 2

Handle 0x1102, DMI type 17, 28 bytes
Memory Device
	Array Handle: 0x1000
	Error Information Handle: Not Provided
	Total Width: 72 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: 2
	Locator: DIMM_A3 
	Bank Locator: Not Specified
	Type: DDR3
	Type Detail: Synchronous Registered (Buffered)
	Speed: 1333 MT/s
	Manufacturer: 00CE00B380CE
	Serial Number: 353C3634
	Asset Tag: 02125163
	Part Number: M393B2G70BH0-YH9  
	Rank: 2

Handle 0x1103, DMI type 17, 28 bytes
Memory Device
	Array Handle: 0x1000
	Error Information Handle: Not Provided
	Total Width: 72 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: 2
	Locator: DIMM_A4 
	Bank Locator: Not Specified
	Type: DDR3
	Type Detail: Synchronous Registered (Buffered)
	Speed: 1333 MT/s
	Manufacturer: 00CE00B380CE
	Serial Number: 352708D9
	Asset Tag: 02124963
	Part Number: M393B2G70BH0-YH9  
	Rank: 2

Handle 0x1104, DMI type 17, 28 bytes
Memory Device
	Array Handle: 0x1000
	Error Information Handle: Not Provided
	Total Width: 72 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: 3
	Locator: DIMM_A5 
	Bank Locator: Not Specified
	Type: DDR3
	Type Detail: Synchronous Registered (Buffered)
	Speed: 1333 MT/s
	Manufacturer: 00CE00B380CE
	Serial Number: 352708D7
	Asset Tag: 02124963
	Part Number: M393B2G70BH0-YH9  
	Rank: 2

Handle 0x1105, DMI type 17, 28 bytes
Memory Device
	Array Handle: 0x1000
	Error Information Handle: Not Provided
	Total Width: 72 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: 3
	Locator: DIMM_A6 
	Bank Locator: Not Specified
	Type: DDR3
	Type Detail: Synchronous Registered (Buffered)
	Speed: 1333 MT/s
	Manufacturer: 00CE00B380CE
	Serial Number: 351F0E9A
	Asset Tag: 02124963
	Part Number: M393B2G70BH0-YH9  
	Rank: 2

Handle 0x1109, DMI type 17, 28 bytes
Memory Device
	Array Handle: 0x1000
	Error Information Handle: Not Provided
	Total Width: 72 bits
	Data Width: 64 bits
	Size: No Module Installed
	Form Factor: DIMM
	Set: 5
	Locator: DIMM_B1 
	Bank Locator: Not Specified
	Type: DDR3
	Type Detail: Synchronous

Handle 0x110A, DMI type 17, 28 bytes
Memory Device
	Array Handle: 0x1000
	Error Information Handle: Not Provided
	Total Width: 72 bits
	Data Width: 64 bits
	Size: No Module Installed
	Form Factor: DIMM
	Set: 6
	Locator: DIMM_B2 
	Bank Locator: Not Specified
	Type: DDR3
	Type Detail: Synchronous

Handle 0x110B, DMI type 17, 28 bytes
Memory Device
	Array Handle: 0x1000
	Error Information Handle: Not Provided
	Total Width: 72 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: 6
	Locator: DIMM_B3 
	Bank Locator: Not Specified
	Type: DDR3
	Type Detail: Synchronous Registered (Buffered)
	Speed: 1333 MT/s
	Manufacturer: 00CE00B380CE
	Serial Number: 353C3192
	Asset Tag: 02125163
	Part Number: M393B2G70BH0-YH9  
	Rank: 2

Handle 0x110C, DMI type 17, 28 bytes
Memory Device
	Array Handle: 0x1000
	Error Information Handle: Not Provided
	Total Width: 72 bits
	Data Width: 64 bits
	Size: No Module Installed
	Form Factor: DIMM
	Set: 4
	Locator: DIMM_B4 
	Bank Locator: Not Specified
	Type: DDR3
	Type Detail: Synchronous

Handle 0x110D, DMI type 17, 28 bytes
Memory Device
	Array Handle: 0x1000
	Error Information Handle: Not Provided
	Total Width: 72 bits
	Data Width: 64 bits
	Size: No Module Installed
	Form Factor: DIMM
	Set: 5
	Locator: DIMM_B5 
	Bank Locator: Not Specified
	Type: DDR3
	Type Detail: Synchronous

Handle 0x110E, DMI type 17, 28 bytes
Memory Device
	Array Handle: 0x1000
	Error Information Handle: Not Provided
	Total Width: 72 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: 6
	Locator: DIMM_B6 
	Bank Locator: Not Specified
	Type: DDR3
	Type Detail: Synchronous Registered (Buffered)
	Speed: 1333 MT/s
	Manufacturer: 00CE00B380CE
	Serial Number: 353C32B8
	Asset Tag: 02125163
	Part Number: M393B2G70BH0-YH9  
	Rank: 2


--- dmidecode -t cache
    $ dmidecode -t cache
# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 2.6 present.

Handle 0x0700, DMI type 7, 19 bytes
Cache Information
	Socket Designation: Not Specified
	Configuration: Enabled, Not Socketed, Level 1
	Operational Mode: Write Back
	Location: Internal
	Installed Size: 128 kB
	Maximum Size: 128 kB
	Supported SRAM Types:
		Unknown
	Installed SRAM Type: Unknown
	Speed: Unknown
	Error Correction Type: Single-bit ECC
	System Type: Data
	Associativity: 8-way Set-associative

Handle 0x0701, DMI type 7, 19 bytes
Cache Information
	Socket Designation: Not Specified
	Configuration: Enabled, Not Socketed, Level 2
	Operational Mode: Write Back
	Location: Internal
	Installed Size: 1 MB
	Maximum Size: 2 MB
	Supported SRAM Types:
		Unknown
	Installed SRAM Type: Unknown
	Speed: Unknown
	Error Correction Type: Single-bit ECC
	System Type: Unified
	Associativity: 8-way Set-associative

Handle 0x0702, DMI type 7, 19 bytes
Cache Information
	Socket Designation: Not Specified
	Configuration: Enabled, Not Socketed, Level 3
	Operational Mode: Write Back
	Location: Internal
	Installed Size: 8 MB
	Maximum Size: 8 MB
	Supported SRAM Types:
		Unknown
	Installed SRAM Type: Unknown
	Speed: Unknown
	Error Correction Type: Single-bit ECC
	System Type: Unified
	Associativity: 16-way Set-associative

Handle 0x0703, DMI type 7, 19 bytes
Cache Information
	Socket Designation: Not Specified
	Configuration: Enabled, Not Socketed, Level 1
	Operational Mode: Write Back
	Location: Internal
	Installed Size: 128 kB
	Maximum Size: 128 kB
	Supported SRAM Types:
		Unknown
	Installed SRAM Type: Unknown
	Speed: Unknown
	Error Correction Type: Single-bit ECC
	System Type: Data
	Associativity: 8-way Set-associative

Handle 0x0704, DMI type 7, 19 bytes
Cache Information
	Socket Designation: Not Specified
	Configuration: Enabled, Not Socketed, Level 2
	Operational Mode: Write Back
	Location: Internal
	Installed Size: 1 MB
	Maximum Size: 2 MB
	Supported SRAM Types:
		Unknown
	Installed SRAM Type: Unknown
	Speed: Unknown
	Error Correction Type: Single-bit ECC
	System Type: Unified
	Associativity: 8-way Set-associative

Handle 0x0705, DMI type 7, 19 bytes
Cache Information
	Socket Designation: Not Specified
	Configuration: Enabled, Not Socketed, Level 3
	Operational Mode: Write Back
	Location: Internal
	Installed Size: 8 MB
	Maximum Size: 8 MB
	Supported SRAM Types:
		Unknown
	Installed SRAM Type: Unknown
	Speed: Unknown
	Error Correction Type: Single-bit ECC
	System Type: Unified
	Associativity: 16-way Set-associative


--- dmidecode -t connector
    $ dmidecode -t connector
# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 2.6 present.

Handle 0x0800, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: Not Specified
	Internal Connector Type: None
	External Reference Designator: Not Specified
	External Connector Type: DB-15 female
	Port Type: Video Port

Handle 0x0801, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: Not Specified
	Internal Connector Type: None
	External Reference Designator: Not Specified
	External Connector Type: DB-15 female
	Port Type: Video Port

Handle 0x0802, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: Not Specified
	Internal Connector Type: None
	External Reference Designator: Not Specified
	External Connector Type: Access Bus (USB)
	Port Type: USB

Handle 0x0803, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: Not Specified
	Internal Connector Type: None
	External Reference Designator: Not Specified
	External Connector Type: Access Bus (USB)
	Port Type: USB

Handle 0x0808, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: Not Specified
	Internal Connector Type: None
	External Reference Designator: Not Specified
	External Connector Type: Access Bus (USB)
	Port Type: USB

Handle 0x0809, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: Not Specified
	Internal Connector Type: None
	External Reference Designator: Not Specified
	External Connector Type: Access Bus (USB)
	Port Type: USB

Handle 0x080A, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: INT_USB
	Internal Connector Type: Access Bus (USB)
	External Reference Designator: Not Specified
	External Connector Type: None
	Port Type: USB

Handle 0x080B, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: INT_SD
	Internal Connector Type: Other
	External Reference Designator: Not Specified
	External Connector Type: None
	Port Type: USB

Handle 0x080E, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: Not Specified
	Internal Connector Type: None
	External Reference Designator: Not Specified
	External Connector Type: RJ-45
	Port Type: Network Port

Handle 0x080F, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: Not Specified
	Internal Connector Type: None
	External Reference Designator: Not Specified
	External Connector Type: RJ-45
	Port Type: Network Port

Handle 0x0810, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: Not Specified
	Internal Connector Type: None
	External Reference Designator: Not Specified
	External Connector Type: RJ-45
	Port Type: Network Port

Handle 0x0811, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: Not Specified
	Internal Connector Type: None
	External Reference Designator: Not Specified
	External Connector Type: RJ-45
	Port Type: Network Port

Handle 0x0812, DMI type 8, 9 bytes
Port Connector Information
	Internal Reference Designator: Not Specified
	Internal Connector Type: None
	External Reference Designator: Not Specified
	External Connector Type: DB-9 male
	Port Type: Serial Port 16550A Compatible


--- dmidecode -t slot
    $ dmidecode -t slot
# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 2.6 present.

Handle 0x0900, DMI type 9, 17 bytes
System Slot Information
	Designation: PCI1
	Type: PCI Express 2
	Data Bus Width: 8x or x8
	Current Usage: In Use
	Length: Long
	ID: 1
	Characteristics:
		3.3 V is provided
		PME signal is supported
	Bus Address: 0000:04:00.0

Handle 0x0901, DMI type 9, 17 bytes
System Slot Information
	Designation: PCI2
	Type: PCI Express 2
	Data Bus Width: 8x or x8
	Current Usage: Available
	Length: Long
	ID: 2
	Characteristics:
		3.3 V is provided
		PME signal is supported


--- lscpu
    $ lscpu
Architecture:                            x86_64
CPU op-mode(s):                          32-bit, 64-bit
Address sizes:                           40 bits physical, 48 bits virtual
Byte Order:                              Little Endian
CPU(s):                                  16
On-line CPU(s) list:                     0-15
Vendor ID:                               GenuineIntel
Model name:                              Intel(R) Xeon(R) CPU           E5530  @ 2.40GHz
CPU family:                              6
Model:                                   26
Thread(s) per core:                      2
Core(s) per socket:                      4
Socket(s):                               2
Stepping:                                5
Frequency boost:                         enabled
CPU(s) scaling MHz:                      92%
CPU max MHz:                             2395.0000
CPU min MHz:                             1596.0000
BogoMIPS:                                4787.75
Flags:                                   fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush dts acpi mmx fxsr sse sse2 ht tm pbe syscall nx rdtscp lm constant_tsc arch_perfmon pebs bts rep_good nopl xtopology nonstop_tsc cpuid aperfmperf pni dtes64 monitor ds_cpl vmx est tm2 ssse3 cx16 xtpr pdcm dca sse4_1 sse4_2 popcnt lahf_lm pti ssbd ibrs ibpb stibp tpr_shadow flexpriority ept vpid dtherm ida vnmi flush_l1d
Virtualization:                          VT-x
L1d cache:                               256 KiB (8 instances)
L1i cache:                               256 KiB (8 instances)
L2 cache:                                2 MiB (8 instances)
L3 cache:                                16 MiB (2 instances)
NUMA node(s):                            2
NUMA node0 CPU(s):                       0,2,4,6,8,10,12,14
NUMA node1 CPU(s):                       1,3,5,7,9,11,13,15
Vulnerability Gather data sampling:      Not affected
Vulnerability Ghostwrite:                Not affected
Vulnerability Indirect target selection: Not affected
Vulnerability Itlb multihit:             KVM: Mitigation: Split huge pages
Vulnerability L1tf:                      Mitigation; PTE Inversion; VMX conditional cache flushes, SMT vulnerable
Vulnerability Mds:                       Vulnerable: Clear CPU buffers attempted, no microcode; SMT vulnerable
Vulnerability Meltdown:                  Mitigation; PTI
Vulnerability Mmio stale data:           Not affected
Vulnerability Old microcode:             Not affected
Vulnerability Reg file data sampling:    Not affected
Vulnerability Retbleed:                  Not affected
Vulnerability Spec rstack overflow:      Not affected
Vulnerability Spec store bypass:         Mitigation; Speculative Store Bypass disabled via prctl
Vulnerability Spectre v1:                Mitigation; usercopy/swapgs barriers and __user pointer sanitization
Vulnerability Spectre v2:                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP conditional; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected
Vulnerability Srbds:                     Not affected
Vulnerability Tsa:                       Not affected
Vulnerability Tsx async abort:           Not affected
Vulnerability Vmscape:                   Not affected

--- lscpu cache
    $ lscpu -C
NAME ONE-SIZE ALL-SIZE WAYS TYPE        LEVEL SETS PHY-LINE COHERENCY-SIZE
L1d       32K     256K    8 Data            1   64        1             64
L1i       32K     256K    4 Instruction     1  128        1             64
L2       256K       2M    8 Unified         2  512        1             64
L3         8M      16M   16 Unified         3 8192        1             64

--- numactl --hardware
    $ numactl --hardware
available: 2 nodes (0-1)
node 0 cpus: 0 2 4 6 8 10 12 14
node 0 size: 96763 MB
node 0 free: 92544 MB
node 1 cpus: 1 3 5 7 9 11 13 15
node 1 size: 32133 MB
node 1 free: 26557 MB
node distances:
node     0    1 
   0:   10   20 
   1:   20   10 

--- numactl --show
    $ numactl --show
policy: default
preferred node: current
physcpubind: 0 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 
cpubind: 0 1 
nodebind: 0 1 
membind: 0 1 
preferred: 

--- lspci -nnvv (verbose)
    $ lspci -nnvv
00:00.0 Host bridge [0600]: Intel Corporation 5500 I/O Hub to ESI Port [8086:3403] (rev 13)
	Subsystem: Dell PowerEdge R610 I/O Hub to ESI Port [1028:0236]
	Control: I/O- Mem- BusMaster- SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Interrupt: pin A routed to IRQ 15
	Capabilities: [60] MSI: Enable- Count=1/2 Maskable+ 64bit-
		Address: 00000000  Data: 0000
		Masking: 00000000  Pending: 00000000
	Capabilities: [90] Express (v2) Root Port (Slot-), IntMsgNum 0
		DevCap:	MaxPayload 128 bytes, PhantFunc 0
			ExtTag+ RBE+ TEE-IO-
		DevCtl:	CorrErr+ NonFatalErr+ FatalErr+ UnsupReq+
			RlxdOrd- ExtTag+ PhantFunc- AuxPwr- NoSnoop-
			MaxPayload 128 bytes, MaxReadReq 128 bytes
		DevSta:	CorrErr- NonFatalErr- FatalErr- UnsupReq- AuxPwr- TransPend-
		LnkCap:	Port #0, Speed 2.5GT/s, Width x4, ASPM L0s L1, Exit Latency L0s <512ns, L1 <64us
			ClockPM- Surprise+ LLActRep+ BwNot+ ASPMOptComp-
		LnkCtl:	ASPM Disabled; RCB 64 bytes, LnkDisable- CommClk-
			ExtSynch- ClockPM- AutWidDis- BWInt- AutBWInt-
		LnkSta:	Speed 2.5GT/s, Width x4
			TrErr- Train- SlotClk+ DLActive+ BWMgmt- ABWMgmt-
		RootCap: CRSVisible-
		RootCtl: ErrCorrectable- ErrNon-Fatal+ ErrFatal+ PMEIntEna- CRSVisible-
		RootSta: PME ReqID 0000, PMEStatus- PMEPending-
		DevCap2: Completion Timeout: Range BCD, TimeoutDis+ NROPrPrP- LTR-
			 10BitTagComp- 10BitTagReq- OBFF Not Supported, ExtFmt- EETLPPrefix-
			 EmergencyPowerReduction Not Supported, EmergencyPowerReductionInit-
			 FRS- LN System CLS Not Supported, TPHComp- ExtTPHComp- ARIFwd+
			 AtomicOpsCap: Routing- 32bit- 64bit- 128bitCAS-
		DevCtl2: Completion Timeout: 17s to 64s, TimeoutDis- ARIFwd-
			 AtomicOpsCtl: ReqEn- EgressBlck-
			 IDOReq- IDOCompl- LTR- EmergencyPowerReductionReq-
			 10BitTagReq- OBFF Disabled, EETLPPrefixBlk-
		LnkCtl2: Target Link Speed: 2.5GT/s, EnterCompliance- SpeedDis-
			 Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
			 Compliance Preset/De-emphasis: -6dB de-emphasis, 0dB preshoot
		LnkSta2: Current De-emphasis Level: -6dB, EqualizationComplete- EqualizationPhase1-
			 EqualizationPhase2- EqualizationPhase3- LinkEqualizationRequest-
			 Retimer- 2Retimers- CrosslinkRes: unsupported
	Capabilities: [e0] Power Management version 3
		Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
		Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=0 PME-
	Capabilities: [100 v1] Advanced Error Reporting
		UESta:	DLP- SDES- TLP- FCP- CmpltTO- CmpltAbrt- UnxCmplt- RxOF- MalfTLP-
			ECRC- UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		UEMsk:	DLP- SDES- TLP- FCP- CmpltTO- CmpltAbrt+ UnxCmplt+ RxOF- MalfTLP-
			ECRC- UnsupReq- ACSViol+ UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		UESvrt:	DLP+ SDES+ TLP+ FCP+ CmpltTO+ CmpltAbrt- UnxCmplt- RxOF+ MalfTLP+
			ECRC- UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		CESta:	RxErr- BadTLP- BadDLLP- Rollover- Timeout- AdvNonFatalErr- CorrIntErr- HeaderOF-
		CEMsk:	RxErr+ BadTLP+ BadDLLP+ Rollover+ Timeout+ AdvNonFatalErr+ CorrIntErr- HeaderOF-
		AERCap:	First Error Pointer: 00, ECRCGenCap- ECRCGenEn- ECRCChkCap- ECRCChkEn-
			MultHdrRecCap- MultHdrRecEn- TLPPfxPres- HdrLogCap-
		HeaderLog: 00000000 00000000 00000000 00000000
		RootCmd: CERptEn- NFERptEn- FERptEn-
		RootSta: CERcvd- MultCERcvd- UERcvd- MultUERcvd-
			 FirstFatal- NonFatalMsg- FatalMsg- IntMsgNum 0
		ErrorSrc: ERR_COR: 0000 ERR_FATAL/NONFATAL: 0000
	Capabilities: [150 v1] Access Control Services
		ACSCap:	SrcValid+ TransBlk+ ReqRedir+ CmpltRedir+ UpstreamFwd+ EgressCtrl- DirectTrans-
		ACSCtl:	SrcValid- TransBlk- ReqRedir- CmpltRedir- UpstreamFwd- EgressCtrl- DirectTrans-
	Capabilities: [160 v0] Vendor Specific Information: ID=0002 Rev=0 Len=00c <?>

00:01.0 PCI bridge [0604]: Intel Corporation 5520/5500/X58 I/O Hub PCI Express Root Port 1 [8086:3408] (rev 13) (prog-if 00 [Normal decode])
	Subsystem: Dell Device [1028:0236]
	Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr+ Stepping- SERR+ FastB2B- DisINTx+
	Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0, Cache Line Size: 64 bytes
	Interrupt: pin A routed to IRQ 25
	Bus: primary=00, secondary=01, subordinate=01, sec-latency=0
	I/O behind bridge: [disabled] [16-bit]
	Memory behind bridge: d2000000-d5ffffff [size=64M] [32-bit]
	Prefetchable memory behind bridge: [disabled] [64-bit]
	Secondary status: 66MHz- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- <SERR- <PERR-
	BridgeCtl: Parity+ SERR+ NoISA+ VGA- VGA16- MAbort- >Reset- FastB2B-
		PriDiscTmr- SecDiscTmr- DiscTmrStat- DiscTmrSERREn-
	Capabilities: [40] Subsystem: Dell Device [1028:0236]
	Capabilities: [60] MSI: Enable+ Count=1/2 Maskable+ 64bit-
		Address: fee00000  Data: 0020
		Masking: 00000002  Pending: 00000000
	Capabilities: [90] Express (v2) Root Port (Slot-), IntMsgNum 0
		DevCap:	MaxPayload 256 bytes, PhantFunc 0
			ExtTag+ RBE+ TEE-IO-
		DevCtl:	CorrErr+ NonFatalErr+ FatalErr+ UnsupReq+
			RlxdOrd- ExtTag+ PhantFunc- AuxPwr- NoSnoop-
			MaxPayload 256 bytes, MaxReadReq 128 bytes
		DevSta:	CorrErr- NonFatalErr- FatalErr- UnsupReq- AuxPwr- TransPend-
		LnkCap:	Port #1, Speed 5GT/s, Width x4, ASPM L0s L1, Exit Latency L0s <512ns, L1 <64us
			ClockPM- Surprise+ LLActRep+ BwNot+ ASPMOptComp-
		LnkCtl:	ASPM Disabled; RCB 64 bytes, LnkDisable- CommClk+
			ExtSynch- ClockPM- AutWidDis- BWInt+ AutBWInt+
		LnkSta:	Speed 2.5GT/s, Width x4
			TrErr- Train- SlotClk+ DLActive+ BWMgmt- ABWMgmt-
		RootCap: CRSVisible+
		RootCtl: ErrCorrectable- ErrNon-Fatal- ErrFatal- PMEIntEna+ CRSVisible+
		RootSta: PME ReqID 0000, PMEStatus- PMEPending-
		DevCap2: Completion Timeout: Range BCD, TimeoutDis+ NROPrPrP- LTR-
			 10BitTagComp- 10BitTagReq- OBFF Not Supported, ExtFmt- EETLPPrefix-
			 EmergencyPowerReduction Not Supported, EmergencyPowerReductionInit-
			 FRS- LN System CLS Not Supported, TPHComp- ExtTPHComp- ARIFwd+
			 AtomicOpsCap: Routing- 32bit- 64bit- 128bitCAS-
		DevCtl2: Completion Timeout: 1s to 3.5s, TimeoutDis- ARIFwd-
			 AtomicOpsCtl: ReqEn- EgressBlck-
			 IDOReq- IDOCompl- LTR- EmergencyPowerReductionReq-
			 10BitTagReq- OBFF Disabled, EETLPPrefixBlk-
		LnkCtl2: Target Link Speed: 5GT/s, EnterCompliance- SpeedDis-
			 Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
			 Compliance Preset/De-emphasis: -6dB de-emphasis, 0dB preshoot
		LnkSta2: Current De-emphasis Level: -6dB, EqualizationComplete- EqualizationPhase1-
			 EqualizationPhase2- EqualizationPhase3- LinkEqualizationRequest-
			 Retimer- 2Retimers- CrosslinkRes: unsupported
	Capabilities: [e0] Power Management version 3
		Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
		Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=0 PME-
	Capabilities: [100 v1] Advanced Error Reporting
		UESta:	DLP- SDES- TLP- FCP- CmpltTO- CmpltAbrt- UnxCmplt- RxOF- MalfTLP-
			ECRC- UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		UEMsk:	DLP- SDES- TLP- FCP- CmpltTO- CmpltAbrt+ UnxCmplt+ RxOF- MalfTLP-
			ECRC- UnsupReq- ACSViol+ UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		UESvrt:	DLP+ SDES+ TLP+ FCP+ CmpltTO+ CmpltAbrt- UnxCmplt- RxOF+ MalfTLP+
			ECRC- UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		CESta:	RxErr- BadTLP- BadDLLP- Rollover- Timeout- AdvNonFatalErr- CorrIntErr- HeaderOF-
		CEMsk:	RxErr+ BadTLP+ BadDLLP+ Rollover+ Timeout+ AdvNonFatalErr+ CorrIntErr- HeaderOF-
		AERCap:	First Error Pointer: 00, ECRCGenCap- ECRCGenEn- ECRCChkCap- ECRCChkEn-
			MultHdrRecCap- MultHdrRecEn- TLPPfxPres- HdrLogCap-
		HeaderLog: 00000000 00000000 00000000 00000000
		RootCmd: CERptEn+ NFERptEn+ FERptEn+
		RootSta: CERcvd- MultCERcvd- UERcvd- MultUERcvd-
			 FirstFatal- NonFatalMsg- FatalMsg- IntMsgNum 0
		ErrorSrc: ERR_COR: 0000 ERR_FATAL/NONFATAL: 0000
	Capabilities: [150 v1] Access Control Services
		ACSCap:	SrcValid+ TransBlk+ ReqRedir+ CmpltRedir+ UpstreamFwd+ EgressCtrl- DirectTrans-
		ACSCtl:	SrcValid- TransBlk- ReqRedir- CmpltRedir- UpstreamFwd- EgressCtrl- DirectTrans-
	Capabilities: [160 v0] Vendor Specific Information: ID=0002 Rev=0 Len=00c <?>
	Kernel driver in use: pcieport
	Kernel modules: shpchp

00:03.0 PCI bridge [0604]: Intel Corporation 5520/5500/X58 I/O Hub PCI Express Root Port 3 [8086:340a] (rev 13) (prog-if 00 [Normal decode])
	Subsystem: Dell Device [1028:0236]
	Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr+ Stepping- SERR+ FastB2B- DisINTx+
	Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0, Cache Line Size: 64 bytes
	Interrupt: pin A routed to IRQ 26
	Bus: primary=00, secondary=02, subordinate=02, sec-latency=0
	I/O behind bridge: [disabled] [16-bit]
	Memory behind bridge: d6000000-d9ffffff [size=64M] [32-bit]
	Prefetchable memory behind bridge: [disabled] [64-bit]
	Secondary status: 66MHz- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- <SERR- <PERR-
	BridgeCtl: Parity+ SERR+ NoISA+ VGA- VGA16- MAbort- >Reset- FastB2B-
		PriDiscTmr- SecDiscTmr- DiscTmrStat- DiscTmrSERREn-
	Capabilities: [40] Subsystem: Dell Device [1028:0236]
	Capabilities: [60] MSI: Enable+ Count=1/2 Maskable+ 64bit-
		Address: fee02000  Data: 0020
		Masking: 00000002  Pending: 00000000
	Capabilities: [90] Express (v2) Root Port (Slot-), IntMsgNum 0
		DevCap:	MaxPayload 256 bytes, PhantFunc 0
			ExtTag+ RBE+ TEE-IO-
		DevCtl:	CorrErr+ NonFatalErr+ FatalErr+ UnsupReq+
			RlxdOrd- ExtTag+ PhantFunc- AuxPwr- NoSnoop-
			MaxPayload 256 bytes, MaxReadReq 128 bytes
		DevSta:	CorrErr- NonFatalErr- FatalErr- UnsupReq- AuxPwr- TransPend-
		LnkCap:	Port #3, Speed 5GT/s, Width x4, ASPM L0s L1, Exit Latency L0s <512ns, L1 <64us
			ClockPM- Surprise+ LLActRep+ BwNot+ ASPMOptComp-
		LnkCtl:	ASPM Disabled; RCB 64 bytes, LnkDisable- CommClk+
			ExtSynch- ClockPM- AutWidDis- BWInt+ AutBWInt+
		LnkSta:	Speed 2.5GT/s, Width x4
			TrErr- Train- SlotClk+ DLActive+ BWMgmt- ABWMgmt-
		RootCap: CRSVisible+
		RootCtl: ErrCorrectable- ErrNon-Fatal- ErrFatal- PMEIntEna+ CRSVisible+
		RootSta: PME ReqID 0000, PMEStatus- PMEPending-
		DevCap2: Completion Timeout: Range BCD, TimeoutDis+ NROPrPrP- LTR-
			 10BitTagComp- 10BitTagReq- OBFF Not Supported, ExtFmt- EETLPPrefix-
			 EmergencyPowerReduction Not Supported, EmergencyPowerReductionInit-
			 FRS- LN System CLS Not Supported, TPHComp- ExtTPHComp- ARIFwd+
			 AtomicOpsCap: Routing- 32bit- 64bit- 128bitCAS-
		DevCtl2: Completion Timeout: 1s to 3.5s, TimeoutDis- ARIFwd-
			 AtomicOpsCtl: ReqEn- EgressBlck-
			 IDOReq- IDOCompl- LTR- EmergencyPowerReductionReq-
			 10BitTagReq- OBFF Disabled, EETLPPrefixBlk-
		LnkCtl2: Target Link Speed: 5GT/s, EnterCompliance- SpeedDis-
			 Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
			 Compliance Preset/De-emphasis: -6dB de-emphasis, 0dB preshoot
		LnkSta2: Current De-emphasis Level: -6dB, EqualizationComplete- EqualizationPhase1-
			 EqualizationPhase2- EqualizationPhase3- LinkEqualizationRequest-
			 Retimer- 2Retimers- CrosslinkRes: unsupported
	Capabilities: [e0] Power Management version 3
		Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
		Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=0 PME-
	Capabilities: [100 v1] Advanced Error Reporting
		UESta:	DLP- SDES- TLP- FCP- CmpltTO- CmpltAbrt- UnxCmplt- RxOF- MalfTLP-
			ECRC- UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		UEMsk:	DLP- SDES- TLP- FCP- CmpltTO- CmpltAbrt+ UnxCmplt+ RxOF- MalfTLP-
			ECRC- UnsupReq- ACSViol+ UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		UESvrt:	DLP+ SDES+ TLP+ FCP+ CmpltTO+ CmpltAbrt- UnxCmplt- RxOF+ MalfTLP+
			ECRC- UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		CESta:	RxErr- BadTLP- BadDLLP- Rollover- Timeout- AdvNonFatalErr- CorrIntErr- HeaderOF-
		CEMsk:	RxErr+ BadTLP+ BadDLLP+ Rollover+ Timeout+ AdvNonFatalErr+ CorrIntErr- HeaderOF-
		AERCap:	First Error Pointer: 00, ECRCGenCap- ECRCGenEn- ECRCChkCap- ECRCChkEn-
			MultHdrRecCap- MultHdrRecEn- TLPPfxPres- HdrLogCap-
		HeaderLog: 00000000 00000000 00000000 00000000
		RootCmd: CERptEn+ NFERptEn+ FERptEn+
		RootSta: CERcvd- MultCERcvd- UERcvd- MultUERcvd-
			 FirstFatal- NonFatalMsg- FatalMsg- IntMsgNum 0
		ErrorSrc: ERR_COR: 0000 ERR_FATAL/NONFATAL: 0000
	Capabilities: [150 v1] Access Control Services
		ACSCap:	SrcValid+ TransBlk+ ReqRedir+ CmpltRedir+ UpstreamFwd+ EgressCtrl- DirectTrans-
		ACSCtl:	SrcValid- TransBlk- ReqRedir- CmpltRedir- UpstreamFwd- EgressCtrl- DirectTrans-
	Capabilities: [160 v0] Vendor Specific Information: ID=0002 Rev=0 Len=00c <?>
	Kernel driver in use: pcieport
	Kernel modules: shpchp

00:07.0 PCI bridge [0604]: Intel Corporation 5520/5500/X58 I/O Hub PCI Express Root Port 7 [8086:340e] (rev 13) (prog-if 00 [Normal decode])
	Subsystem: Dell Device [1028:0236]
	Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr+ Stepping- SERR+ FastB2B- DisINTx+
	Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0, Cache Line Size: 64 bytes
	Interrupt: pin A routed to IRQ 27
	Bus: primary=00, secondary=04, subordinate=04, sec-latency=0
	I/O behind bridge: [disabled] [16-bit]
	Memory behind bridge: da000000-ddffffff [size=64M] [32-bit]
	Prefetchable memory behind bridge: [disabled] [64-bit]
	Secondary status: 66MHz- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- <SERR- <PERR-
	BridgeCtl: Parity+ SERR+ NoISA+ VGA- VGA16- MAbort- >Reset- FastB2B-
		PriDiscTmr- SecDiscTmr- DiscTmrStat- DiscTmrSERREn-
	Capabilities: [40] Subsystem: Dell Device [1028:0236]
	Capabilities: [60] MSI: Enable+ Count=1/2 Maskable+ 64bit-
		Address: fee14000  Data: 0020
		Masking: 00000002  Pending: 00000000
	Capabilities: [90] Express (v2) Root Port (Slot+), IntMsgNum 0
		DevCap:	MaxPayload 256 bytes, PhantFunc 0
			ExtTag+ RBE+ TEE-IO-
		DevCtl:	CorrErr+ NonFatalErr+ FatalErr+ UnsupReq+
			RlxdOrd- ExtTag+ PhantFunc- AuxPwr- NoSnoop-
			MaxPayload 256 bytes, MaxReadReq 128 bytes
		DevSta:	CorrErr- NonFatalErr- FatalErr- UnsupReq- AuxPwr- TransPend-
		LnkCap:	Port #7, Speed 5GT/s, Width x8, ASPM L0s L1, Exit Latency L0s <512ns, L1 <64us
			ClockPM- Surprise+ LLActRep+ BwNot+ ASPMOptComp-
		LnkCtl:	ASPM Disabled; RCB 64 bytes, LnkDisable- CommClk+
			ExtSynch- ClockPM- AutWidDis- BWInt+ AutBWInt+
		LnkSta:	Speed 2.5GT/s, Width x4
			TrErr- Train- SlotClk+ DLActive+ BWMgmt- ABWMgmt-
		SltCap:	AttnBtn- PwrCtrl- MRL- AttnInd- PwrInd- HotPlug- Surprise-
			Slot #1, PowerLimit 25W; Interlock- NoCompl-
		SltCtl:	Enable: AttnBtn- PwrFlt- MRL- PresDet- CmdCplt- HPIrq- LinkChg-
			Control: AttnInd Off, PwrInd Off, Power- Interlock-
		SltSta:	Status: AttnBtn- PowerFlt- MRL- CmdCplt- PresDet+ Interlock-
			Changed: MRL- PresDet+ LinkState+
		RootCap: CRSVisible+
		RootCtl: ErrCorrectable- ErrNon-Fatal- ErrFatal- PMEIntEna+ CRSVisible+
		RootSta: PME ReqID 0000, PMEStatus- PMEPending-
		DevCap2: Completion Timeout: Range BCD, TimeoutDis+ NROPrPrP- LTR-
			 10BitTagComp- 10BitTagReq- OBFF Not Supported, ExtFmt- EETLPPrefix-
			 EmergencyPowerReduction Not Supported, EmergencyPowerReductionInit-
			 FRS- LN System CLS Not Supported, TPHComp- ExtTPHComp- ARIFwd+
			 AtomicOpsCap: Routing- 32bit- 64bit- 128bitCAS-
		DevCtl2: Completion Timeout: 1s to 3.5s, TimeoutDis- ARIFwd-
			 AtomicOpsCtl: ReqEn- EgressBlck-
			 IDOReq- IDOCompl- LTR- EmergencyPowerReductionReq-
			 10BitTagReq- OBFF Disabled, EETLPPrefixBlk-
		LnkCtl2: Target Link Speed: 5GT/s, EnterCompliance- SpeedDis-
			 Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
			 Compliance Preset/De-emphasis: -6dB de-emphasis, 0dB preshoot
		LnkSta2: Current De-emphasis Level: -6dB, EqualizationComplete- EqualizationPhase1-
			 EqualizationPhase2- EqualizationPhase3- LinkEqualizationRequest-
			 Retimer- 2Retimers- CrosslinkRes: unsupported
	Capabilities: [e0] Power Management version 3
		Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
		Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=0 PME-
	Capabilities: [100 v1] Advanced Error Reporting
		UESta:	DLP- SDES- TLP- FCP- CmpltTO- CmpltAbrt- UnxCmplt- RxOF- MalfTLP-
			ECRC- UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		UEMsk:	DLP- SDES- TLP- FCP- CmpltTO- CmpltAbrt+ UnxCmplt+ RxOF- MalfTLP-
			ECRC- UnsupReq- ACSViol+ UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		UESvrt:	DLP+ SDES+ TLP+ FCP+ CmpltTO+ CmpltAbrt- UnxCmplt- RxOF+ MalfTLP+
			ECRC- UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		CESta:	RxErr- BadTLP- BadDLLP- Rollover- Timeout- AdvNonFatalErr- CorrIntErr- HeaderOF-
		CEMsk:	RxErr+ BadTLP+ BadDLLP+ Rollover+ Timeout+ AdvNonFatalErr+ CorrIntErr- HeaderOF-
		AERCap:	First Error Pointer: 00, ECRCGenCap- ECRCGenEn- ECRCChkCap- ECRCChkEn-
			MultHdrRecCap- MultHdrRecEn- TLPPfxPres- HdrLogCap-
		HeaderLog: 00000000 00000000 00000000 00000000
		RootCmd: CERptEn+ NFERptEn+ FERptEn+
		RootSta: CERcvd- MultCERcvd- UERcvd- MultUERcvd-
			 FirstFatal- NonFatalMsg- FatalMsg- IntMsgNum 0
		ErrorSrc: ERR_COR: 0000 ERR_FATAL/NONFATAL: 0000
	Capabilities: [150 v1] Access Control Services
		ACSCap:	SrcValid+ TransBlk+ ReqRedir+ CmpltRedir+ UpstreamFwd+ EgressCtrl- DirectTrans-
		ACSCtl:	SrcValid- TransBlk- ReqRedir- CmpltRedir- UpstreamFwd- EgressCtrl- DirectTrans-
	Capabilities: [160 v0] Vendor Specific Information: ID=0002 Rev=0 Len=00c <?>
	Kernel driver in use: pcieport
	Kernel modules: shpchp

00:09.0 PCI bridge [0604]: Intel Corporation 7500/5520/5500/X58 I/O Hub PCI Express Root Port 9 [8086:3410] (rev 13) (prog-if 00 [Normal decode])
	Subsystem: Dell Device [1028:0236]
	Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr+ Stepping- SERR+ FastB2B- DisINTx+
	Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0, Cache Line Size: 64 bytes
	Interrupt: pin A routed to IRQ 28
	Bus: primary=00, secondary=05, subordinate=05, sec-latency=0
	I/O behind bridge: [disabled] [16-bit]
	Memory behind bridge: [disabled] [32-bit]
	Prefetchable memory behind bridge: [disabled] [64-bit]
	Secondary status: 66MHz- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- <SERR- <PERR-
	BridgeCtl: Parity+ SERR+ NoISA+ VGA- VGA16- MAbort- >Reset- FastB2B-
		PriDiscTmr- SecDiscTmr- DiscTmrStat- DiscTmrSERREn-
	Capabilities: [40] Subsystem: Dell Device [1028:0236]
	Capabilities: [60] MSI: Enable+ Count=1/2 Maskable+ 64bit-
		Address: fee04000  Data: 0020
		Masking: 00000002  Pending: 00000000
	Capabilities: [90] Express (v2) Root Port (Slot+), IntMsgNum 0
		DevCap:	MaxPayload 256 bytes, PhantFunc 0
			ExtTag+ RBE+ TEE-IO-
		DevCtl:	CorrErr+ NonFatalErr+ FatalErr+ UnsupReq+
			RlxdOrd- ExtTag+ PhantFunc- AuxPwr- NoSnoop-
			MaxPayload 128 bytes, MaxReadReq 128 bytes
		DevSta:	CorrErr- NonFatalErr- FatalErr- UnsupReq- AuxPwr- TransPend-
		LnkCap:	Port #9, Speed 5GT/s, Width x8, ASPM L0s L1, Exit Latency L0s <512ns, L1 <64us
			ClockPM- Surprise+ LLActRep+ BwNot+ ASPMOptComp-
		LnkCtl:	ASPM Disabled; RCB 64 bytes, LnkDisable+ CommClk-
			ExtSynch- ClockPM- AutWidDis- BWInt+ AutBWInt+
		LnkSta:	Speed 2.5GT/s, Width x0
			TrErr- Train- SlotClk+ DLActive- BWMgmt- ABWMgmt-
		SltCap:	AttnBtn- PwrCtrl- MRL- AttnInd- PwrInd- HotPlug- Surprise-
			Slot #2, PowerLimit 25W; Interlock- NoCompl-
		SltCtl:	Enable: AttnBtn- PwrFlt- MRL- PresDet- CmdCplt- HPIrq- LinkChg-
			Control: AttnInd Off, PwrInd Off, Power- Interlock-
		SltSta:	Status: AttnBtn- PowerFlt- MRL- CmdCplt- PresDet- Interlock-
			Changed: MRL- PresDet+ LinkState-
		RootCap: CRSVisible+
		RootCtl: ErrCorrectable- ErrNon-Fatal- ErrFatal- PMEIntEna+ CRSVisible+
		RootSta: PME ReqID 0000, PMEStatus- PMEPending-
		DevCap2: Completion Timeout: Range BCD, TimeoutDis+ NROPrPrP- LTR-
			 10BitTagComp- 10BitTagReq- OBFF Not Supported, ExtFmt- EETLPPrefix-
			 EmergencyPowerReduction Not Supported, EmergencyPowerReductionInit-
			 FRS- LN System CLS Not Supported, TPHComp- ExtTPHComp- ARIFwd+
			 AtomicOpsCap: Routing- 32bit- 64bit- 128bitCAS-
		DevCtl2: Completion Timeout: 1s to 3.5s, TimeoutDis- ARIFwd-
			 AtomicOpsCtl: ReqEn- EgressBlck-
			 IDOReq- IDOCompl- LTR- EmergencyPowerReductionReq-
			 10BitTagReq- OBFF Disabled, EETLPPrefixBlk-
		LnkCtl2: Target Link Speed: 2.5GT/s, EnterCompliance- SpeedDis-
			 Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
			 Compliance Preset/De-emphasis: -6dB de-emphasis, 0dB preshoot
		LnkSta2: Current De-emphasis Level: -6dB, EqualizationComplete- EqualizationPhase1-
			 EqualizationPhase2- EqualizationPhase3- LinkEqualizationRequest-
			 Retimer- 2Retimers- CrosslinkRes: unsupported
	Capabilities: [e0] Power Management version 3
		Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
		Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=0 PME-
	Capabilities: [100 v1] Advanced Error Reporting
		UESta:	DLP- SDES- TLP- FCP- CmpltTO- CmpltAbrt- UnxCmplt- RxOF- MalfTLP-
			ECRC- UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		UEMsk:	DLP- SDES- TLP- FCP- CmpltTO- CmpltAbrt+ UnxCmplt+ RxOF- MalfTLP-
			ECRC- UnsupReq- ACSViol+ UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		UESvrt:	DLP+ SDES+ TLP+ FCP+ CmpltTO+ CmpltAbrt- UnxCmplt- RxOF+ MalfTLP+
			ECRC- UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		CESta:	RxErr- BadTLP- BadDLLP- Rollover- Timeout- AdvNonFatalErr- CorrIntErr- HeaderOF-
		CEMsk:	RxErr+ BadTLP+ BadDLLP+ Rollover+ Timeout+ AdvNonFatalErr+ CorrIntErr- HeaderOF-
		AERCap:	First Error Pointer: 00, ECRCGenCap- ECRCGenEn- ECRCChkCap- ECRCChkEn-
			MultHdrRecCap- MultHdrRecEn- TLPPfxPres- HdrLogCap-
		HeaderLog: 00000000 00000000 00000000 00000000
		RootCmd: CERptEn+ NFERptEn+ FERptEn+
		RootSta: CERcvd- MultCERcvd- UERcvd- MultUERcvd-
			 FirstFatal- NonFatalMsg- FatalMsg- IntMsgNum 0
		ErrorSrc: ERR_COR: 0000 ERR_FATAL/NONFATAL: 0000
	Capabilities: [150 v1] Access Control Services
		ACSCap:	SrcValid+ TransBlk+ ReqRedir+ CmpltRedir+ UpstreamFwd+ EgressCtrl- DirectTrans-
		ACSCtl:	SrcValid- TransBlk- ReqRedir- CmpltRedir- UpstreamFwd- EgressCtrl- DirectTrans-
	Kernel driver in use: pcieport
	Kernel modules: shpchp

00:14.0 PIC [0800]: Intel Corporation 7500/5520/5500/X58 I/O Hub System Management Registers [8086:342e] (rev 13) (prog-if 00 [8259])
	Control: I/O- Mem- BusMaster- SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Capabilities: [40] Express (v2) Root Complex Integrated Endpoint, IntMsgNum 0
		DevCap:	MaxPayload 128 bytes, PhantFunc 0
			ExtTag- RBE+ FLReset- TEE-IO-
		DevCtl:	CorrErr- NonFatalErr- FatalErr- UnsupReq-
			RlxdOrd- ExtTag- PhantFunc- AuxPwr- NoSnoop-
			MaxPayload 128 bytes, MaxReadReq 128 bytes
		DevSta:	CorrErr- NonFatalErr- FatalErr- UnsupReq- AuxPwr- TransPend-
		DevCap2: Completion Timeout: Not Supported, TimeoutDis- NROPrPrP- LTR-
			 10BitTagComp- 10BitTagReq- OBFF Not Supported, ExtFmt- EETLPPrefix-
			 EmergencyPowerReduction Not Supported, EmergencyPowerReductionInit-
			 FRS-
		DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis-
			 AtomicOpsCtl: ReqEn-
			 IDOReq- IDOCompl- LTR- EmergencyPowerReductionReq-
			 10BitTagReq- OBFF Disabled, EETLPPrefixBlk-
	Kernel driver in use: i7core_edac
	Kernel modules: i7core_edac

00:14.1 PIC [0800]: Intel Corporation 7500/5520/5500/X58 I/O Hub GPIO and Scratch Pad Registers [8086:3422] (rev 13) (prog-if 00 [8259])
	Control: I/O- Mem- BusMaster- SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Capabilities: [40] Express (v2) Root Complex Integrated Endpoint, IntMsgNum 0
		DevCap:	MaxPayload 128 bytes, PhantFunc 0
			ExtTag- RBE+ FLReset- TEE-IO-
		DevCtl:	CorrErr- NonFatalErr- FatalErr- UnsupReq-
			RlxdOrd- ExtTag- PhantFunc- AuxPwr- NoSnoop-
			MaxPayload 128 bytes, MaxReadReq 128 bytes
		DevSta:	CorrErr- NonFatalErr- FatalErr- UnsupReq- AuxPwr- TransPend-
		DevCap2: Completion Timeout: Not Supported, TimeoutDis- NROPrPrP- LTR-
			 10BitTagComp- 10BitTagReq- OBFF Not Supported, ExtFmt- EETLPPrefix-
			 EmergencyPowerReduction Not Supported, EmergencyPowerReductionInit-
			 FRS-
		DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis-
			 AtomicOpsCtl: ReqEn-
			 IDOReq- IDOCompl- LTR- EmergencyPowerReductionReq-
			 10BitTagReq- OBFF Disabled, EETLPPrefixBlk-

00:14.2 PIC [0800]: Intel Corporation 7500/5520/5500/X58 I/O Hub Control Status and RAS Registers [8086:3423] (rev 13) (prog-if 00 [8259])
	Control: I/O- Mem- BusMaster- SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Capabilities: [40] Express (v2) Root Complex Integrated Endpoint, IntMsgNum 0
		DevCap:	MaxPayload 128 bytes, PhantFunc 0
			ExtTag- RBE+ FLReset- TEE-IO-
		DevCtl:	CorrErr- NonFatalErr- FatalErr- UnsupReq-
			RlxdOrd- ExtTag- PhantFunc- AuxPwr- NoSnoop-
			MaxPayload 128 bytes, MaxReadReq 128 bytes
		DevSta:	CorrErr- NonFatalErr- FatalErr- UnsupReq- AuxPwr- TransPend-
		DevCap2: Completion Timeout: Not Supported, TimeoutDis- NROPrPrP- LTR-
			 10BitTagComp- 10BitTagReq- OBFF Not Supported, ExtFmt- EETLPPrefix-
			 EmergencyPowerReduction Not Supported, EmergencyPowerReductionInit-
			 FRS-
		DevCtl2: Completion Timeout: 50us to 50ms, TimeoutDis-
			 AtomicOpsCtl: ReqEn-
			 IDOReq- IDOCompl- LTR- EmergencyPowerReductionReq-
			 10BitTagReq- OBFF Disabled, EETLPPrefixBlk-

00:1a.0 USB controller [0c03]: Intel Corporation 82801I (ICH9 Family) USB UHCI Controller #4 [8086:2937] (rev 02) (prog-if 00 [UHCI])
	Subsystem: Dell PowerEdge R610 USB UHCI Controller [1028:0236]
	Control: I/O+ Mem- BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap+ 66MHz- UDF- FastB2B+ ParErr- DEVSEL=medium >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0
	Interrupt: pin A routed to IRQ 17
	Region 4: I/O ports at ec40 [size=32]
	Capabilities: [50] PCI Advanced Features
		AFCap: TP+ FLR+
		AFCtrl: FLR-
		AFStatus: TP-
	Kernel driver in use: uhci_hcd
	Kernel modules: uhci_hcd

00:1a.1 USB controller [0c03]: Intel Corporation 82801I (ICH9 Family) USB UHCI Controller #5 [8086:2938] (rev 02) (prog-if 00 [UHCI])
	Subsystem: Dell PowerEdge R610 USB UHCI Controller [1028:0236]
	Control: I/O+ Mem- BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap+ 66MHz- UDF- FastB2B+ ParErr- DEVSEL=medium >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0
	Interrupt: pin B routed to IRQ 18
	Region 4: I/O ports at ec60 [size=32]
	Capabilities: [50] PCI Advanced Features
		AFCap: TP+ FLR+
		AFCtrl: FLR-
		AFStatus: TP-
	Kernel driver in use: uhci_hcd
	Kernel modules: uhci_hcd

00:1a.7 USB controller [0c03]: Intel Corporation 82801I (ICH9 Family) USB2 EHCI Controller #2 [8086:293c] (rev 02) (prog-if 20 [EHCI])
	Subsystem: Dell PowerEdge R610 USB EHCI Controller [1028:0236]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr+ Stepping- SERR+ FastB2B- DisINTx-
	Status: Cap+ 66MHz- UDF- FastB2B+ ParErr- DEVSEL=medium >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0
	Interrupt: pin C routed to IRQ 19
	Region 0: Memory at df0ff800 (32-bit, non-prefetchable) [size=1K]
	Capabilities: [50] Power Management version 2
		Flags: PMEClk- DSI- D1- D2- AuxCurrent=375mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
		Status: D0 NoSoftRst- PME-Enable- DSel=0 DScale=0 PME-
	Capabilities: [58] Debug port: BAR=1 offset=00a0
	Capabilities: [98] PCI Advanced Features
		AFCap: TP+ FLR+
		AFCtrl: FLR-
		AFStatus: TP-
	Kernel driver in use: ehci-pci
	Kernel modules: ehci_pci

00:1c.0 PCI bridge [0604]: Intel Corporation 82801I (ICH9 Family) PCI Express Port 1 [8086:2940] (rev 02) (prog-if 00 [Normal decode])
	Subsystem: Dell Device [1028:0236]
	Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr+ Stepping- SERR+ FastB2B- DisINTx+
	Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0, Cache Line Size: 64 bytes
	Interrupt: pin A routed to IRQ 29
	Bus: primary=00, secondary=03, subordinate=03, sec-latency=0
	I/O behind bridge: f000-ffff [size=4K] [16-bit]
	Memory behind bridge: df100000-df2fffff [size=2M] [32-bit]
	Prefetchable memory behind bridge: [disabled] [64-bit]
	Secondary status: 66MHz- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- <SERR- <PERR-
	BridgeCtl: Parity+ SERR+ NoISA- VGA- VGA16- MAbort- >Reset- FastB2B-
		PriDiscTmr- SecDiscTmr- DiscTmrStat- DiscTmrSERREn-
	Capabilities: [40] Express (v1) Root Port (Slot-), IntMsgNum 0
		DevCap:	MaxPayload 128 bytes, PhantFunc 0
			ExtTag- RBE+ TEE-IO-
		DevCtl:	CorrErr- NonFatalErr+ FatalErr+ UnsupReq+
			RlxdOrd- ExtTag- PhantFunc- AuxPwr- NoSnoop-
			MaxPayload 128 bytes, MaxReadReq 128 bytes
		DevSta:	CorrErr- NonFatalErr- FatalErr- UnsupReq- AuxPwr+ TransPend-
		LnkCap:	Port #1, Speed 2.5GT/s, Width x4, ASPM L0s L1, Exit Latency L0s <256ns, L1 <4us
			ClockPM- Surprise- LLActRep+ BwNot- ASPMOptComp-
		LnkCtl:	ASPM Disabled; RCB 64 bytes, LnkDisable+ CommClk+
			ExtSynch- ClockPM- AutWidDis- BWInt- AutBWInt-
		LnkSta:	Speed 2.5GT/s, Width x4
			TrErr- Train- SlotClk+ DLActive- BWMgmt- ABWMgmt-
		RootCap: CRSVisible-
		RootCtl: ErrCorrectable- ErrNon-Fatal+ ErrFatal+ PMEIntEna+ CRSVisible-
		RootSta: PME ReqID 0000, PMEStatus- PMEPending-
	Capabilities: [80] MSI: Enable+ Count=1/1 Maskable- 64bit-
		Address: fee16000  Data: 0020
	Capabilities: [90] Subsystem: Dell Device [1028:0236]
	Capabilities: [a0] Power Management version 2
		Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
		Status: D0 NoSoftRst- PME-Enable- DSel=0 DScale=0 PME-
	Capabilities: [100 v1] Virtual Channel
		Caps:	LPEVC=0 RefClk=100ns PATEntryBits=1
		Arb:	Fixed+ WRR32- WRR64- WRR128-
		Ctrl:	ArbSelect=Fixed
		Status:	InProgress-
		VC0:	Caps:	PATOffset=00 MaxTimeSlots=1 RejSnoopTrans-
			Arb:	Fixed+ WRR32- WRR64- WRR128- TWRR128- WRR256-
			Ctrl:	Enable+ ID=0 ArbSelect=Fixed TC/VC=ff
			Status:	NegoPending- InProgress-
	Capabilities: [180 v1] Root Complex Link
		Desc:	PortNumber=01 ComponentID=02 EltType=Config
		Link0:	Desc:	TargetPort=00 TargetComponent=02 AssocRCRB- LinkType=MemMapped LinkValid+
			Addr:	00000000feda8000
	Kernel driver in use: pcieport
	Kernel modules: shpchp

00:1d.0 USB controller [0c03]: Intel Corporation 82801I (ICH9 Family) USB UHCI Controller #1 [8086:2934] (rev 02) (prog-if 00 [UHCI])
	Subsystem: Dell PowerEdge R610 USB UHCI Controller [1028:0236]
	Control: I/O+ Mem- BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap+ 66MHz- UDF- FastB2B+ ParErr- DEVSEL=medium >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0
	Interrupt: pin A routed to IRQ 21
	Region 4: I/O ports at ec80 [size=32]
	Capabilities: [50] PCI Advanced Features
		AFCap: TP+ FLR+
		AFCtrl: FLR-
		AFStatus: TP-
	Kernel driver in use: uhci_hcd
	Kernel modules: uhci_hcd

00:1d.1 USB controller [0c03]: Intel Corporation 82801I (ICH9 Family) USB UHCI Controller #2 [8086:2935] (rev 02) (prog-if 00 [UHCI])
	Subsystem: Dell PowerEdge R610 USB UHCI Controller [1028:0236]
	Control: I/O+ Mem- BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap+ 66MHz- UDF- FastB2B+ ParErr- DEVSEL=medium >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0
	Interrupt: pin B routed to IRQ 20
	Region 4: I/O ports at eca0 [size=32]
	Capabilities: [50] PCI Advanced Features
		AFCap: TP+ FLR+
		AFCtrl: FLR-
		AFStatus: TP-
	Kernel driver in use: uhci_hcd
	Kernel modules: uhci_hcd

00:1d.7 USB controller [0c03]: Intel Corporation 82801I (ICH9 Family) USB2 EHCI Controller #1 [8086:293a] (rev 02) (prog-if 20 [EHCI])
	Subsystem: Dell PowerEdge R610 USB EHCI Controller [1028:0236]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr+ Stepping- SERR+ FastB2B- DisINTx-
	Status: Cap+ 66MHz- UDF- FastB2B+ ParErr- DEVSEL=medium >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0
	Interrupt: pin A routed to IRQ 21
	Region 0: Memory at df0ffc00 (32-bit, non-prefetchable) [size=1K]
	Capabilities: [50] Power Management version 2
		Flags: PMEClk- DSI- D1- D2- AuxCurrent=375mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
		Status: D0 NoSoftRst- PME-Enable- DSel=0 DScale=0 PME-
	Capabilities: [58] Debug port: BAR=1 offset=00a0
	Capabilities: [98] PCI Advanced Features
		AFCap: TP+ FLR+
		AFCtrl: FLR-
		AFStatus: TP-
	Kernel driver in use: ehci-pci
	Kernel modules: ehci_pci

00:1e.0 PCI bridge [0604]: Intel Corporation 82801 PCI Bridge [8086:244e] (rev 92) (prog-if 01 [Subtractive decode])
	Subsystem: Dell Device [1028:0236]
	Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr+ Stepping- SERR+ FastB2B- DisINTx-
	Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0
	Bus: primary=00, secondary=06, subordinate=06, sec-latency=32
	I/O behind bridge: [disabled] [16-bit]
	Memory behind bridge: de000000-deffffff [size=16M] [32-bit]
	Prefetchable memory behind bridge: d1800000-d1ffffff [size=8M] [32-bit]
	Secondary status: 66MHz- FastB2B+ ParErr- DEVSEL=medium >TAbort- <TAbort- <MAbort+ <SERR- <PERR-
	BridgeCtl: Parity+ SERR+ NoISA- VGA+ VGA16- MAbort- >Reset- FastB2B-
		PriDiscTmr- SecDiscTmr- DiscTmrStat- DiscTmrSERREn-
	Capabilities: [50] Subsystem: Dell Device [1028:0236]

00:1f.0 ISA bridge [0601]: Intel Corporation 82801IB (ICH9) LPC Interface Controller [8086:2918] (rev 02)
	Subsystem: Dell PowerEdge R610 82801IB (ICH9) LPC Interface Controller [1028:0236]
	Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr+ Stepping- SERR+ FastB2B- DisINTx-
	Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=medium >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0
	Capabilities: [e0] Vendor Specific Information: Len=0c <?>
	Kernel driver in use: lpc_ich
	Kernel modules: lpc_ich

01:00.0 Ethernet controller [0200]: Broadcom Inc. and subsidiaries NetXtreme II BCM5709 Gigabit Ethernet [14e4:1639] (rev 20)
	DeviceName: Embedded NIC 1                          
	Subsystem: Dell PowerEdge R610 BCM5709 Gigabit Ethernet [1028:0236]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
	Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0, Cache Line Size: 64 bytes
	Interrupt: pin A routed to IRQ 30
	Region 0: Memory at d2000000 (64-bit, non-prefetchable) [size=32M]
	Capabilities: [48] Power Management version 3
		Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
		Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=1 PME-
	Capabilities: [50] Vital Product Data
		Product Name: Broadcom NetXtreme II Ethernet Controller
		Read-only fields:
			[PN] Part number: BCM95709C0
			[EC] Engineering changes: 220197-2
			[SN] Serial number: 0123456789
			[MN] Manufacture ID: 1028
			[V0] Vendor specific: 5.0.13
			[RV] Reserved: checksum good, 22 byte(s) reserved
		End
	Capabilities: [58] MSI: Enable- Count=1/16 Maskable- 64bit+
		Address: 0000000000000000  Data: 0000
	Capabilities: [a0] MSI-X: Enable+ Count=9 Masked-
		Vector table: BAR=0 offset=0000c000
		PBA: BAR=0 offset=0000e000
	Capabilities: [ac] Express (v2) Endpoint, IntMsgNum 0
		DevCap:	MaxPayload 512 bytes, PhantFunc 0, Latency L0s <4us, L1 <64us
			ExtTag- AttnBtn- AttnInd- PwrInd- RBE+ FLReset- SlotPowerLimit 0W TEE-IO-
		DevCtl:	CorrErr+ NonFatalErr+ FatalErr+ UnsupReq+
			RlxdOrd+ ExtTag- PhantFunc- AuxPwr+ NoSnoop+
			MaxPayload 256 bytes, MaxReadReq 512 bytes
		DevSta:	CorrErr+ NonFatalErr- FatalErr- UnsupReq+ AuxPwr+ TransPend-
		LnkCap:	Port #0, Speed 2.5GT/s, Width x4, ASPM L0s L1, Exit Latency L0s <2us, L1 <2us
			ClockPM- Surprise- LLActRep- BwNot- ASPMOptComp-
		LnkCtl:	ASPM Disabled; RCB 64 bytes, LnkDisable- CommClk+
			ExtSynch- ClockPM- AutWidDis- BWInt- AutBWInt-
		LnkSta:	Speed 2.5GT/s, Width x4
			TrErr- Train- SlotClk+ DLActive- BWMgmt- ABWMgmt-
		DevCap2: Completion Timeout: Range ABCD, TimeoutDis+ NROPrPrP- LTR-
			 10BitTagComp- 10BitTagReq- OBFF Not Supported, ExtFmt- EETLPPrefix-
			 EmergencyPowerReduction Not Supported, EmergencyPowerReductionInit-
			 FRS- TPHComp- ExtTPHComp-
			 AtomicOpsCap: 32bit- 64bit- 128bitCAS-
		DevCtl2: Completion Timeout: 65ms to 210ms, TimeoutDis-
			 AtomicOpsCtl: ReqEn-
			 IDOReq- IDOCompl- LTR- EmergencyPowerReductionReq-
			 10BitTagReq- OBFF Disabled, EETLPPrefixBlk-
		LnkCtl2: Target Link Speed: 2.5GT/s, EnterCompliance- SpeedDis-
			 Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
			 Compliance Preset/De-emphasis: -6dB de-emphasis, 0dB preshoot
		LnkSta2: Current De-emphasis Level: -6dB, EqualizationComplete- EqualizationPhase1-
			 EqualizationPhase2- EqualizationPhase3- LinkEqualizationRequest-
			 Retimer- 2Retimers- CrosslinkRes: unsupported
	Capabilities: [100 v1] Device Serial Number 00-21-9b-ff-fe-a2-7c-53
	Capabilities: [110 v1] Advanced Error Reporting
		UESta:	DLP- SDES- TLP- FCP- CmpltTO- CmpltAbrt- UnxCmplt- RxOF- MalfTLP-
			ECRC- UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		UEMsk:	DLP- SDES- TLP- FCP- CmpltTO- CmpltAbrt+ UnxCmplt+ RxOF- MalfTLP-
			ECRC- UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		UESvrt:	DLP+ SDES+ TLP+ FCP+ CmpltTO+ CmpltAbrt- UnxCmplt- RxOF+ MalfTLP+
			ECRC+ UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		CESta:	RxErr- BadTLP- BadDLLP- Rollover- Timeout- AdvNonFatalErr+ CorrIntErr- HeaderOF-
		CEMsk:	RxErr- BadTLP+ BadDLLP+ Rollover+ Timeout+ AdvNonFatalErr+ CorrIntErr- HeaderOF-
		AERCap:	First Error Pointer: 00, ECRCGenCap+ ECRCGenEn- ECRCChkCap+ ECRCChkEn-
			MultHdrRecCap- MultHdrRecEn- TLPPfxPres- HdrLogCap-
		HeaderLog: 00000000 00000000 00000000 00000000
	Capabilities: [150 v1] Power Budgeting <?>
	Capabilities: [160 v1] Virtual Channel
		Caps:	LPEVC=0 RefClk=100ns PATEntryBits=1
		Arb:	Fixed- WRR32- WRR64- WRR128-
		Ctrl:	ArbSelect=Fixed
		Status:	InProgress-
		VC0:	Caps:	PATOffset=00 MaxTimeSlots=1 RejSnoopTrans-
			Arb:	Fixed- WRR32- WRR64- WRR128- TWRR128- WRR256-
			Ctrl:	Enable+ ID=0 ArbSelect=Fixed TC/VC=ff
			Status:	NegoPending- InProgress-
	Kernel driver in use: bnx2
	Kernel modules: bnx2

01:00.1 Ethernet controller [0200]: Broadcom Inc. and subsidiaries NetXtreme II BCM5709 Gigabit Ethernet [14e4:1639] (rev 20)
	DeviceName: Embedded NIC 2                          
	Subsystem: Dell PowerEdge R610 BCM5709 Gigabit Ethernet [1028:0236]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
	Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0, Cache Line Size: 64 bytes
	Interrupt: pin B routed to IRQ 31
	Region 0: Memory at d4000000 (64-bit, non-prefetchable) [size=32M]
	Capabilities: [48] Power Management version 3
		Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
		Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=1 PME-
	Capabilities: [50] Vital Product Data
		Product Name: Broadcom NetXtreme II Ethernet Controller
		Read-only fields:
			[PN] Part number: BCM95709C0
			[EC] Engineering changes: 220197-2
			[SN] Serial number: 0123456789
			[MN] Manufacture ID: 1028
			[V0] Vendor specific: 5.0.13
			[RV] Reserved: checksum good, 22 byte(s) reserved
		End
	Capabilities: [58] MSI: Enable- Count=1/16 Maskable- 64bit+
		Address: 0000000000000000  Data: 0000
	Capabilities: [a0] MSI-X: Enable+ Count=9 Masked-
		Vector table: BAR=0 offset=0000c000
		PBA: BAR=0 offset=0000e000
	Capabilities: [ac] Express (v2) Endpoint, IntMsgNum 0
		DevCap:	MaxPayload 512 bytes, PhantFunc 0, Latency L0s <4us, L1 <64us
			ExtTag- AttnBtn- AttnInd- PwrInd- RBE+ FLReset- SlotPowerLimit 0W TEE-IO-
		DevCtl:	CorrErr+ NonFatalErr+ FatalErr+ UnsupReq+
			RlxdOrd+ ExtTag- PhantFunc- AuxPwr+ NoSnoop+
			MaxPayload 256 bytes, MaxReadReq 512 bytes
		DevSta:	CorrErr+ NonFatalErr- FatalErr- UnsupReq+ AuxPwr+ TransPend-
		LnkCap:	Port #0, Speed 2.5GT/s, Width x4, ASPM L0s L1, Exit Latency L0s <2us, L1 <2us
			ClockPM- Surprise- LLActRep- BwNot- ASPMOptComp-
		LnkCtl:	ASPM Disabled; RCB 64 bytes, LnkDisable- CommClk+
			ExtSynch- ClockPM- AutWidDis- BWInt- AutBWInt-
		LnkSta:	Speed 2.5GT/s, Width x4
			TrErr- Train- SlotClk+ DLActive- BWMgmt- ABWMgmt-
		DevCap2: Completion Timeout: Range ABCD, TimeoutDis+ NROPrPrP- LTR-
			 10BitTagComp- 10BitTagReq- OBFF Not Supported, ExtFmt- EETLPPrefix-
			 EmergencyPowerReduction Not Supported, EmergencyPowerReductionInit-
			 FRS- TPHComp- ExtTPHComp-
			 AtomicOpsCap: 32bit- 64bit- 128bitCAS-
		DevCtl2: Completion Timeout: 65ms to 210ms, TimeoutDis-
			 AtomicOpsCtl: ReqEn-
			 IDOReq- IDOCompl- LTR- EmergencyPowerReductionReq-
			 10BitTagReq- OBFF Disabled, EETLPPrefixBlk-
		LnkSta2: Current De-emphasis Level: -6dB, EqualizationComplete- EqualizationPhase1-
			 EqualizationPhase2- EqualizationPhase3- LinkEqualizationRequest-
			 Retimer- 2Retimers- CrosslinkRes: unsupported
	Capabilities: [100 v1] Device Serial Number 00-21-9b-ff-fe-a2-7c-55
	Capabilities: [110 v1] Advanced Error Reporting
		UESta:	DLP- SDES- TLP- FCP- CmpltTO- CmpltAbrt- UnxCmplt- RxOF- MalfTLP-
			ECRC- UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		UEMsk:	DLP- SDES- TLP- FCP- CmpltTO- CmpltAbrt+ UnxCmplt+ RxOF- MalfTLP-
			ECRC- UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		UESvrt:	DLP+ SDES+ TLP+ FCP+ CmpltTO+ CmpltAbrt- UnxCmplt- RxOF+ MalfTLP+
			ECRC+ UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		CESta:	RxErr- BadTLP- BadDLLP- Rollover- Timeout- AdvNonFatalErr+ CorrIntErr- HeaderOF-
		CEMsk:	RxErr- BadTLP+ BadDLLP+ Rollover+ Timeout+ AdvNonFatalErr+ CorrIntErr- HeaderOF-
		AERCap:	First Error Pointer: 00, ECRCGenCap+ ECRCGenEn- ECRCChkCap+ ECRCChkEn-
			MultHdrRecCap- MultHdrRecEn- TLPPfxPres- HdrLogCap-
		HeaderLog: 00000000 00000000 00000000 00000000
	Capabilities: [150 v1] Power Budgeting <?>
	Capabilities: [160 v1] Virtual Channel
		Caps:	LPEVC=0 RefClk=100ns PATEntryBits=1
		Arb:	Fixed- WRR32- WRR64- WRR128-
		Ctrl:	ArbSelect=Fixed
		Status:	InProgress-
		VC0:	Caps:	PATOffset=00 MaxTimeSlots=1 RejSnoopTrans-
			Arb:	Fixed- WRR32- WRR64- WRR128- TWRR128- WRR256-
			Ctrl:	Enable+ ID=0 ArbSelect=Fixed TC/VC=ff
			Status:	NegoPending- InProgress-
	Kernel driver in use: bnx2
	Kernel modules: bnx2

02:00.0 Ethernet controller [0200]: Broadcom Inc. and subsidiaries NetXtreme II BCM5709 Gigabit Ethernet [14e4:1639] (rev 20)
	DeviceName: Embedded NIC 3                          
	Subsystem: Dell PowerEdge R610 BCM5709 Gigabit Ethernet [1028:0236]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
	Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0, Cache Line Size: 64 bytes
	Interrupt: pin A routed to IRQ 32
	Region 0: Memory at d6000000 (64-bit, non-prefetchable) [size=32M]
	Capabilities: [48] Power Management version 3
		Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
		Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=1 PME-
	Capabilities: [50] Vital Product Data
		Product Name: Broadcom NetXtreme II Ethernet Controller
		Read-only fields:
			[PN] Part number: BCM95709C0
			[EC] Engineering changes: 220197-2
			[SN] Serial number: 0123456789
			[MN] Manufacture ID: 1028
			[V0] Vendor specific: 5.0.13
			[RV] Reserved: checksum good, 22 byte(s) reserved
		End
	Capabilities: [58] MSI: Enable- Count=1/16 Maskable- 64bit+
		Address: 0000000000000000  Data: 0000
	Capabilities: [a0] MSI-X: Enable+ Count=9 Masked-
		Vector table: BAR=0 offset=0000c000
		PBA: BAR=0 offset=0000e000
	Capabilities: [ac] Express (v2) Endpoint, IntMsgNum 0
		DevCap:	MaxPayload 512 bytes, PhantFunc 0, Latency L0s <4us, L1 <64us
			ExtTag- AttnBtn- AttnInd- PwrInd- RBE+ FLReset- SlotPowerLimit 0W TEE-IO-
		DevCtl:	CorrErr+ NonFatalErr+ FatalErr+ UnsupReq+
			RlxdOrd+ ExtTag- PhantFunc- AuxPwr+ NoSnoop+
			MaxPayload 256 bytes, MaxReadReq 512 bytes
		DevSta:	CorrErr+ NonFatalErr- FatalErr- UnsupReq+ AuxPwr+ TransPend-
		LnkCap:	Port #0, Speed 2.5GT/s, Width x4, ASPM L0s L1, Exit Latency L0s <2us, L1 <2us
			ClockPM- Surprise- LLActRep- BwNot- ASPMOptComp-
		LnkCtl:	ASPM Disabled; RCB 64 bytes, LnkDisable- CommClk+
			ExtSynch- ClockPM- AutWidDis- BWInt- AutBWInt-
		LnkSta:	Speed 2.5GT/s, Width x4
			TrErr- Train- SlotClk+ DLActive- BWMgmt- ABWMgmt-
		DevCap2: Completion Timeout: Range ABCD, TimeoutDis+ NROPrPrP- LTR-
			 10BitTagComp- 10BitTagReq- OBFF Not Supported, ExtFmt- EETLPPrefix-
			 EmergencyPowerReduction Not Supported, EmergencyPowerReductionInit-
			 FRS- TPHComp- ExtTPHComp-
			 AtomicOpsCap: 32bit- 64bit- 128bitCAS-
		DevCtl2: Completion Timeout: 65ms to 210ms, TimeoutDis-
			 AtomicOpsCtl: ReqEn-
			 IDOReq- IDOCompl- LTR- EmergencyPowerReductionReq-
			 10BitTagReq- OBFF Disabled, EETLPPrefixBlk-
		LnkCtl2: Target Link Speed: 2.5GT/s, EnterCompliance- SpeedDis-
			 Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
			 Compliance Preset/De-emphasis: -6dB de-emphasis, 0dB preshoot
		LnkSta2: Current De-emphasis Level: -6dB, EqualizationComplete- EqualizationPhase1-
			 EqualizationPhase2- EqualizationPhase3- LinkEqualizationRequest-
			 Retimer- 2Retimers- CrosslinkRes: unsupported
	Capabilities: [100 v1] Device Serial Number 00-21-9b-ff-fe-a2-7c-57
	Capabilities: [110 v1] Advanced Error Reporting
		UESta:	DLP- SDES- TLP- FCP- CmpltTO- CmpltAbrt- UnxCmplt- RxOF- MalfTLP-
			ECRC- UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		UEMsk:	DLP- SDES- TLP- FCP- CmpltTO- CmpltAbrt+ UnxCmplt+ RxOF- MalfTLP-
			ECRC- UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		UESvrt:	DLP+ SDES+ TLP+ FCP+ CmpltTO+ CmpltAbrt- UnxCmplt- RxOF+ MalfTLP+
			ECRC+ UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		CESta:	RxErr- BadTLP- BadDLLP- Rollover- Timeout- AdvNonFatalErr+ CorrIntErr- HeaderOF-
		CEMsk:	RxErr- BadTLP+ BadDLLP+ Rollover+ Timeout+ AdvNonFatalErr+ CorrIntErr- HeaderOF-
		AERCap:	First Error Pointer: 00, ECRCGenCap+ ECRCGenEn- ECRCChkCap+ ECRCChkEn-
			MultHdrRecCap- MultHdrRecEn- TLPPfxPres- HdrLogCap-
		HeaderLog: 00000000 00000000 00000000 00000000
	Capabilities: [150 v1] Power Budgeting <?>
	Capabilities: [160 v1] Virtual Channel
		Caps:	LPEVC=0 RefClk=100ns PATEntryBits=1
		Arb:	Fixed- WRR32- WRR64- WRR128-
		Ctrl:	ArbSelect=Fixed
		Status:	InProgress-
		VC0:	Caps:	PATOffset=00 MaxTimeSlots=1 RejSnoopTrans-
			Arb:	Fixed- WRR32- WRR64- WRR128- TWRR128- WRR256-
			Ctrl:	Enable+ ID=0 ArbSelect=Fixed TC/VC=ff
			Status:	NegoPending- InProgress-
	Kernel driver in use: bnx2
	Kernel modules: bnx2

02:00.1 Ethernet controller [0200]: Broadcom Inc. and subsidiaries NetXtreme II BCM5709 Gigabit Ethernet [14e4:1639] (rev 20)
	DeviceName: Embedded NIC 4                          
	Subsystem: Dell PowerEdge R610 BCM5709 Gigabit Ethernet [1028:0236]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx+
	Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0, Cache Line Size: 64 bytes
	Interrupt: pin B routed to IRQ 33
	Region 0: Memory at d8000000 (64-bit, non-prefetchable) [size=32M]
	Capabilities: [48] Power Management version 3
		Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
		Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=1 PME-
	Capabilities: [50] Vital Product Data
		Product Name: Broadcom NetXtreme II Ethernet Controller
		Read-only fields:
			[PN] Part number: BCM95709C0
			[EC] Engineering changes: 220197-2
			[SN] Serial number: 0123456789
			[MN] Manufacture ID: 1028
			[V0] Vendor specific: 5.0.13
			[RV] Reserved: checksum good, 22 byte(s) reserved
		End
	Capabilities: [58] MSI: Enable- Count=1/16 Maskable- 64bit+
		Address: 0000000000000000  Data: 0000
	Capabilities: [a0] MSI-X: Enable+ Count=9 Masked-
		Vector table: BAR=0 offset=0000c000
		PBA: BAR=0 offset=0000e000
	Capabilities: [ac] Express (v2) Endpoint, IntMsgNum 0
		DevCap:	MaxPayload 512 bytes, PhantFunc 0, Latency L0s <4us, L1 <64us
			ExtTag- AttnBtn- AttnInd- PwrInd- RBE+ FLReset- SlotPowerLimit 0W TEE-IO-
		DevCtl:	CorrErr+ NonFatalErr+ FatalErr+ UnsupReq+
			RlxdOrd+ ExtTag- PhantFunc- AuxPwr+ NoSnoop+
			MaxPayload 256 bytes, MaxReadReq 512 bytes
		DevSta:	CorrErr+ NonFatalErr- FatalErr- UnsupReq+ AuxPwr+ TransPend-
		LnkCap:	Port #0, Speed 2.5GT/s, Width x4, ASPM L0s L1, Exit Latency L0s <2us, L1 <2us
			ClockPM- Surprise- LLActRep- BwNot- ASPMOptComp-
		LnkCtl:	ASPM Disabled; RCB 64 bytes, LnkDisable- CommClk+
			ExtSynch- ClockPM- AutWidDis- BWInt- AutBWInt-
		LnkSta:	Speed 2.5GT/s, Width x4
			TrErr- Train- SlotClk+ DLActive- BWMgmt- ABWMgmt-
		DevCap2: Completion Timeout: Range ABCD, TimeoutDis+ NROPrPrP- LTR-
			 10BitTagComp- 10BitTagReq- OBFF Not Supported, ExtFmt- EETLPPrefix-
			 EmergencyPowerReduction Not Supported, EmergencyPowerReductionInit-
			 FRS- TPHComp- ExtTPHComp-
			 AtomicOpsCap: 32bit- 64bit- 128bitCAS-
		DevCtl2: Completion Timeout: 65ms to 210ms, TimeoutDis-
			 AtomicOpsCtl: ReqEn-
			 IDOReq- IDOCompl- LTR- EmergencyPowerReductionReq-
			 10BitTagReq- OBFF Disabled, EETLPPrefixBlk-
		LnkSta2: Current De-emphasis Level: -6dB, EqualizationComplete- EqualizationPhase1-
			 EqualizationPhase2- EqualizationPhase3- LinkEqualizationRequest-
			 Retimer- 2Retimers- CrosslinkRes: unsupported
	Capabilities: [100 v1] Device Serial Number 00-21-9b-ff-fe-a2-7c-59
	Capabilities: [110 v1] Advanced Error Reporting
		UESta:	DLP- SDES- TLP- FCP- CmpltTO- CmpltAbrt- UnxCmplt- RxOF- MalfTLP-
			ECRC- UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		UEMsk:	DLP- SDES- TLP- FCP- CmpltTO- CmpltAbrt+ UnxCmplt+ RxOF- MalfTLP-
			ECRC- UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		UESvrt:	DLP+ SDES+ TLP+ FCP+ CmpltTO+ CmpltAbrt- UnxCmplt- RxOF+ MalfTLP+
			ECRC+ UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		CESta:	RxErr- BadTLP- BadDLLP- Rollover- Timeout- AdvNonFatalErr+ CorrIntErr- HeaderOF-
		CEMsk:	RxErr- BadTLP+ BadDLLP+ Rollover+ Timeout+ AdvNonFatalErr+ CorrIntErr- HeaderOF-
		AERCap:	First Error Pointer: 00, ECRCGenCap+ ECRCGenEn- ECRCChkCap+ ECRCChkEn-
			MultHdrRecCap- MultHdrRecEn- TLPPfxPres- HdrLogCap-
		HeaderLog: 00000000 00000000 00000000 00000000
	Capabilities: [150 v1] Power Budgeting <?>
	Capabilities: [160 v1] Virtual Channel
		Caps:	LPEVC=0 RefClk=100ns PATEntryBits=1
		Arb:	Fixed- WRR32- WRR64- WRR128-
		Ctrl:	ArbSelect=Fixed
		Status:	InProgress-
		VC0:	Caps:	PATOffset=00 MaxTimeSlots=1 RejSnoopTrans-
			Arb:	Fixed- WRR32- WRR64- WRR128- TWRR128- WRR256-
			Ctrl:	Enable+ ID=0 ArbSelect=Fixed TC/VC=ff
			Status:	NegoPending- InProgress-
	Kernel driver in use: bnx2
	Kernel modules: bnx2

04:00.0 Ethernet controller [0200]: Broadcom Inc. and subsidiaries NetXtreme II BCM5709 Gigabit Ethernet [14e4:1639] (rev 20)
	Subsystem: Broadcom Inc. and subsidiaries Device [14e4:1917]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0, Cache Line Size: 64 bytes
	Interrupt: pin A routed to IRQ 34
	Region 0: Memory at da000000 (64-bit, non-prefetchable) [size=32M]
	Capabilities: [48] Power Management version 3
		Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
		Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=1 PME-
	Capabilities: [50] Vital Product Data
		Not readable
	Capabilities: [58] MSI: Enable- Count=1/16 Maskable- 64bit+
		Address: 0000000000000000  Data: 0000
	Capabilities: [a0] MSI-X: Enable- Count=9 Masked-
		Vector table: BAR=0 offset=0000c000
		PBA: BAR=0 offset=0000e000
	Capabilities: [ac] Express (v2) Endpoint, IntMsgNum 0
		DevCap:	MaxPayload 512 bytes, PhantFunc 0, Latency L0s <4us, L1 <64us
			ExtTag- AttnBtn- AttnInd- PwrInd- RBE+ FLReset- SlotPowerLimit 25W TEE-IO-
		DevCtl:	CorrErr+ NonFatalErr+ FatalErr+ UnsupReq+
			RlxdOrd+ ExtTag- PhantFunc- AuxPwr+ NoSnoop+
			MaxPayload 256 bytes, MaxReadReq 512 bytes
		DevSta:	CorrErr+ NonFatalErr- FatalErr- UnsupReq+ AuxPwr+ TransPend-
		LnkCap:	Port #0, Speed 2.5GT/s, Width x4, ASPM L0s L1, Exit Latency L0s <2us, L1 <2us
			ClockPM- Surprise- LLActRep- BwNot- ASPMOptComp-
		LnkCtl:	ASPM Disabled; RCB 64 bytes, LnkDisable- CommClk+
			ExtSynch- ClockPM- AutWidDis- BWInt- AutBWInt-
		LnkSta:	Speed 2.5GT/s, Width x4
			TrErr- Train- SlotClk+ DLActive- BWMgmt- ABWMgmt-
		DevCap2: Completion Timeout: Range ABCD, TimeoutDis+ NROPrPrP- LTR-
			 10BitTagComp- 10BitTagReq- OBFF Not Supported, ExtFmt- EETLPPrefix-
			 EmergencyPowerReduction Not Supported, EmergencyPowerReductionInit-
			 FRS- TPHComp- ExtTPHComp-
			 AtomicOpsCap: 32bit- 64bit- 128bitCAS-
		DevCtl2: Completion Timeout: 65ms to 210ms, TimeoutDis-
			 AtomicOpsCtl: ReqEn-
			 IDOReq- IDOCompl- LTR- EmergencyPowerReductionReq-
			 10BitTagReq- OBFF Disabled, EETLPPrefixBlk-
		LnkCtl2: Target Link Speed: 2.5GT/s, EnterCompliance- SpeedDis-
			 Transmit Margin: Normal Operating Range, EnterModifiedCompliance- ComplianceSOS-
			 Compliance Preset/De-emphasis: -6dB de-emphasis, 0dB preshoot
		LnkSta2: Current De-emphasis Level: -6dB, EqualizationComplete- EqualizationPhase1-
			 EqualizationPhase2- EqualizationPhase3- LinkEqualizationRequest-
			 Retimer- 2Retimers- CrosslinkRes: unsupported
	Capabilities: [100 v1] Device Serial Number 00-10-18-ff-fe-72-16-40
	Capabilities: [110 v1] Advanced Error Reporting
		UESta:	DLP- SDES- TLP- FCP- CmpltTO- CmpltAbrt- UnxCmplt- RxOF- MalfTLP-
			ECRC- UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		UEMsk:	DLP- SDES- TLP- FCP- CmpltTO- CmpltAbrt+ UnxCmplt+ RxOF- MalfTLP-
			ECRC- UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		UESvrt:	DLP+ SDES+ TLP+ FCP+ CmpltTO+ CmpltAbrt- UnxCmplt- RxOF+ MalfTLP+
			ECRC+ UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		CESta:	RxErr- BadTLP- BadDLLP- Rollover- Timeout- AdvNonFatalErr+ CorrIntErr- HeaderOF-
		CEMsk:	RxErr- BadTLP+ BadDLLP+ Rollover+ Timeout+ AdvNonFatalErr+ CorrIntErr- HeaderOF-
		AERCap:	First Error Pointer: 00, ECRCGenCap+ ECRCGenEn- ECRCChkCap+ ECRCChkEn-
			MultHdrRecCap- MultHdrRecEn- TLPPfxPres- HdrLogCap-
		HeaderLog: 00000000 00000000 00000000 00000000
	Capabilities: [150 v1] Power Budgeting <?>
	Capabilities: [160 v1] Virtual Channel
		Caps:	LPEVC=0 RefClk=100ns PATEntryBits=1
		Arb:	Fixed- WRR32- WRR64- WRR128-
		Ctrl:	ArbSelect=Fixed
		Status:	InProgress-
		VC0:	Caps:	PATOffset=00 MaxTimeSlots=1 RejSnoopTrans-
			Arb:	Fixed- WRR32- WRR64- WRR128- TWRR128- WRR256-
			Ctrl:	Enable+ ID=0 ArbSelect=Fixed TC/VC=ff
			Status:	NegoPending- InProgress-
	Kernel driver in use: bnx2
	Kernel modules: bnx2

04:00.1 Ethernet controller [0200]: Broadcom Inc. and subsidiaries NetXtreme II BCM5709 Gigabit Ethernet [14e4:1639] (rev 20)
	Subsystem: Broadcom Inc. and subsidiaries Device [14e4:1917]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap+ 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0, Cache Line Size: 64 bytes
	Interrupt: pin B routed to IRQ 35
	Region 0: Memory at dc000000 (64-bit, non-prefetchable) [size=32M]
	Capabilities: [48] Power Management version 3
		Flags: PMEClk- DSI- D1- D2- AuxCurrent=0mA PME(D0+,D1-,D2-,D3hot+,D3cold+)
		Status: D0 NoSoftRst+ PME-Enable- DSel=0 DScale=1 PME-
	Capabilities: [50] Vital Product Data
		Not readable
	Capabilities: [58] MSI: Enable- Count=1/16 Maskable- 64bit+
		Address: 0000000000000000  Data: 0000
	Capabilities: [a0] MSI-X: Enable- Count=9 Masked-
		Vector table: BAR=0 offset=0000c000
		PBA: BAR=0 offset=0000e000
	Capabilities: [ac] Express (v2) Endpoint, IntMsgNum 0
		DevCap:	MaxPayload 512 bytes, PhantFunc 0, Latency L0s <4us, L1 <64us
			ExtTag- AttnBtn- AttnInd- PwrInd- RBE+ FLReset- SlotPowerLimit 25W TEE-IO-
		DevCtl:	CorrErr+ NonFatalErr+ FatalErr+ UnsupReq+
			RlxdOrd+ ExtTag- PhantFunc- AuxPwr+ NoSnoop+
			MaxPayload 256 bytes, MaxReadReq 512 bytes
		DevSta:	CorrErr+ NonFatalErr- FatalErr- UnsupReq+ AuxPwr+ TransPend-
		LnkCap:	Port #0, Speed 2.5GT/s, Width x4, ASPM L0s L1, Exit Latency L0s <2us, L1 <2us
			ClockPM- Surprise- LLActRep- BwNot- ASPMOptComp-
		LnkCtl:	ASPM Disabled; RCB 64 bytes, LnkDisable- CommClk+
			ExtSynch- ClockPM- AutWidDis- BWInt- AutBWInt-
		LnkSta:	Speed 2.5GT/s, Width x4
			TrErr- Train- SlotClk+ DLActive- BWMgmt- ABWMgmt-
		DevCap2: Completion Timeout: Range ABCD, TimeoutDis+ NROPrPrP- LTR-
			 10BitTagComp- 10BitTagReq- OBFF Not Supported, ExtFmt- EETLPPrefix-
			 EmergencyPowerReduction Not Supported, EmergencyPowerReductionInit-
			 FRS- TPHComp- ExtTPHComp-
			 AtomicOpsCap: 32bit- 64bit- 128bitCAS-
		DevCtl2: Completion Timeout: 65ms to 210ms, TimeoutDis-
			 AtomicOpsCtl: ReqEn-
			 IDOReq- IDOCompl- LTR- EmergencyPowerReductionReq-
			 10BitTagReq- OBFF Disabled, EETLPPrefixBlk-
		LnkSta2: Current De-emphasis Level: -6dB, EqualizationComplete- EqualizationPhase1-
			 EqualizationPhase2- EqualizationPhase3- LinkEqualizationRequest-
			 Retimer- 2Retimers- CrosslinkRes: unsupported
	Capabilities: [100 v1] Device Serial Number 00-10-18-ff-fe-72-16-42
	Capabilities: [110 v1] Advanced Error Reporting
		UESta:	DLP- SDES- TLP- FCP- CmpltTO- CmpltAbrt- UnxCmplt- RxOF- MalfTLP-
			ECRC- UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		UEMsk:	DLP- SDES- TLP- FCP- CmpltTO- CmpltAbrt+ UnxCmplt+ RxOF- MalfTLP-
			ECRC- UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		UESvrt:	DLP+ SDES+ TLP+ FCP+ CmpltTO+ CmpltAbrt- UnxCmplt- RxOF+ MalfTLP+
			ECRC+ UnsupReq- ACSViol- UncorrIntErr- BlockedTLP- AtomicOpBlocked- TLPBlockedErr-
			PoisonTLPBlocked- DMWrReqBlocked- IDECheck- MisIDETLP- PCRC_CHECK- TLPXlatBlocked-
		CESta:	RxErr- BadTLP- BadDLLP- Rollover- Timeout- AdvNonFatalErr+ CorrIntErr- HeaderOF-
		CEMsk:	RxErr- BadTLP+ BadDLLP+ Rollover+ Timeout+ AdvNonFatalErr+ CorrIntErr- HeaderOF-
		AERCap:	First Error Pointer: 00, ECRCGenCap+ ECRCGenEn- ECRCChkCap+ ECRCChkEn-
			MultHdrRecCap- MultHdrRecEn- TLPPfxPres- HdrLogCap-
		HeaderLog: 00000000 00000000 00000000 00000000
	Capabilities: [150 v1] Power Budgeting <?>
	Capabilities: [160 v1] Virtual Channel
		Caps:	LPEVC=0 RefClk=100ns PATEntryBits=1
		Arb:	Fixed- WRR32- WRR64- WRR128-
		Ctrl:	ArbSelect=Fixed
		Status:	InProgress-
		VC0:	Caps:	PATOffset=00 MaxTimeSlots=1 RejSnoopTrans-
			Arb:	Fixed- WRR32- WRR64- WRR128- TWRR128- WRR256-
			Ctrl:	Enable+ ID=0 ArbSelect=Fixed TC/VC=ff
			Status:	NegoPending- InProgress-
	Kernel driver in use: bnx2
	Kernel modules: bnx2

06:03.0 VGA compatible controller [0300]: Matrox Electronics Systems Ltd. MGA G200eW WPCM450 [102b:0532] (rev 0a) (prog-if 00 [VGA controller])
	DeviceName: Embedded Video                          
	Subsystem: Dell PowerEdge R610 MGA G200eW WPCM450 [1028:0236]
	Control: I/O+ Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap+ 66MHz- UDF- FastB2B+ ParErr- DEVSEL=medium >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 32 (4000ns min, 8000ns max), Cache Line Size: 64 bytes
	Interrupt: pin A routed to IRQ 19
	Region 0: Memory at d1800000 (32-bit, prefetchable) [size=8M]
	Region 1: Memory at de7fc000 (32-bit, non-prefetchable) [size=16K]
	Region 2: Memory at de800000 (32-bit, non-prefetchable) [size=8M]
	Expansion ROM at 000c0000 [virtual] [disabled] [size=128K]
	Capabilities: [dc] Power Management version 1
		Flags: PMEClk- DSI+ D1- D2- AuxCurrent=0mA PME(D0-,D1-,D2-,D3hot-,D3cold-)
		Status: D0 NoSoftRst- PME-Enable- DSel=0 DScale=0 PME-
	Kernel driver in use: mgag200
	Kernel modules: matroxfb_base, mgag200

fe:00.0 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 QuickPath Architecture Generic Non-Core Registers [8086:2c40] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

fe:00.1 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 QuickPath Architecture System Address Decoder [8086:2c01] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

fe:02.0 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 QPI Link 0 [8086:2c10] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

fe:02.1 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 QPI Physical 0 [8086:2c11] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

fe:02.4 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 QPI Link 1 [8086:2c14] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

fe:02.5 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 QPI Physical 1 [8086:2c15] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

fe:03.0 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller [8086:2c18] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

fe:03.1 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Target Address Decoder [8086:2c19] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

fe:03.2 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller RAS Registers [8086:2c1a] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

fe:03.4 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Test Registers [8086:2c1c] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

fe:04.0 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 0 Control Registers [8086:2c20] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

fe:04.1 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 0 Address Registers [8086:2c21] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

fe:04.2 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 0 Rank Registers [8086:2c22] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

fe:04.3 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 0 Thermal Control Registers [8086:2c23] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

fe:05.0 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 1 Control Registers [8086:2c28] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

fe:05.1 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 1 Address Registers [8086:2c29] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

fe:05.2 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 1 Rank Registers [8086:2c2a] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

fe:05.3 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 1 Thermal Control Registers [8086:2c2b] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

fe:06.0 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 2 Control Registers [8086:2c30] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

fe:06.1 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 2 Address Registers [8086:2c31] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

fe:06.2 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 2 Rank Registers [8086:2c32] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

fe:06.3 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 2 Thermal Control Registers [8086:2c33] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

ff:00.0 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 QuickPath Architecture Generic Non-Core Registers [8086:2c40] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

ff:00.1 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 QuickPath Architecture System Address Decoder [8086:2c01] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

ff:02.0 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 QPI Link 0 [8086:2c10] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

ff:02.1 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 QPI Physical 0 [8086:2c11] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

ff:02.4 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 QPI Link 1 [8086:2c14] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

ff:02.5 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 QPI Physical 1 [8086:2c15] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

ff:03.0 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller [8086:2c18] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

ff:03.1 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Target Address Decoder [8086:2c19] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

ff:03.2 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller RAS Registers [8086:2c1a] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

ff:03.4 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Test Registers [8086:2c1c] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

ff:04.0 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 0 Control Registers [8086:2c20] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

ff:04.1 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 0 Address Registers [8086:2c21] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

ff:04.2 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 0 Rank Registers [8086:2c22] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

ff:04.3 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 0 Thermal Control Registers [8086:2c23] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

ff:05.0 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 1 Control Registers [8086:2c28] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

ff:05.1 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 1 Address Registers [8086:2c29] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

ff:05.2 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 1 Rank Registers [8086:2c2a] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

ff:05.3 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 1 Thermal Control Registers [8086:2c2b] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

ff:06.0 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 2 Control Registers [8086:2c30] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

ff:06.1 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 2 Address Registers [8086:2c31] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

ff:06.2 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 2 Rank Registers [8086:2c32] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0

ff:06.3 Host bridge [0600]: Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 2 Thermal Control Registers [8086:2c33] (rev 05)
	Subsystem: Intel Corporation Device [8086:8086]
	Control: I/O- Mem+ BusMaster+ SpecCycle- MemWINV- VGASnoop- ParErr- Stepping- SERR- FastB2B- DisINTx-
	Status: Cap- 66MHz- UDF- FastB2B- ParErr- DEVSEL=fast >TAbort- <TAbort- <MAbort- >SERR- <PERR- INTx-
	Latency: 0


--- lspci -tv (tree)
    $ lspci -tv
-+-[0000:00]-+-00.0  Intel Corporation 5500 I/O Hub to ESI Port
 |           +-01.0-[01]--+-00.0  Broadcom Inc. and subsidiaries NetXtreme II BCM5709 Gigabit Ethernet
 |           |            \-00.1  Broadcom Inc. and subsidiaries NetXtreme II BCM5709 Gigabit Ethernet
 |           +-03.0-[02]--+-00.0  Broadcom Inc. and subsidiaries NetXtreme II BCM5709 Gigabit Ethernet
 |           |            \-00.1  Broadcom Inc. and subsidiaries NetXtreme II BCM5709 Gigabit Ethernet
 |           +-07.0-[04]--+-00.0  Broadcom Inc. and subsidiaries NetXtreme II BCM5709 Gigabit Ethernet
 |           |            \-00.1  Broadcom Inc. and subsidiaries NetXtreme II BCM5709 Gigabit Ethernet
 |           +-09.0-[05]--
 |           +-14.0  Intel Corporation 7500/5520/5500/X58 I/O Hub System Management Registers
 |           +-14.1  Intel Corporation 7500/5520/5500/X58 I/O Hub GPIO and Scratch Pad Registers
 |           +-14.2  Intel Corporation 7500/5520/5500/X58 I/O Hub Control Status and RAS Registers
 |           +-1a.0  Intel Corporation 82801I (ICH9 Family) USB UHCI Controller #4
 |           +-1a.1  Intel Corporation 82801I (ICH9 Family) USB UHCI Controller #5
 |           +-1a.7  Intel Corporation 82801I (ICH9 Family) USB2 EHCI Controller #2
 |           +-1c.0-[03]--
 |           +-1d.0  Intel Corporation 82801I (ICH9 Family) USB UHCI Controller #1
 |           +-1d.1  Intel Corporation 82801I (ICH9 Family) USB UHCI Controller #2
 |           +-1d.7  Intel Corporation 82801I (ICH9 Family) USB2 EHCI Controller #1
 |           +-1e.0-[06]----03.0  Matrox Electronics Systems Ltd. MGA G200eW WPCM450
 |           \-1f.0  Intel Corporation 82801IB (ICH9) LPC Interface Controller
 +-[0000:fe]-+-00.0  Intel Corporation Xeon 5500/Core i7 QuickPath Architecture Generic Non-Core Registers
 |           +-00.1  Intel Corporation Xeon 5500/Core i7 QuickPath Architecture System Address Decoder
 |           +-02.0  Intel Corporation Xeon 5500/Core i7 QPI Link 0
 |           +-02.1  Intel Corporation Xeon 5500/Core i7 QPI Physical 0
 |           +-02.4  Intel Corporation Xeon 5500/Core i7 QPI Link 1
 |           +-02.5  Intel Corporation Xeon 5500/Core i7 QPI Physical 1
 |           +-03.0  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller
 |           +-03.1  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Target Address Decoder
 |           +-03.2  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller RAS Registers
 |           +-03.4  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Test Registers
 |           +-04.0  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 0 Control Registers
 |           +-04.1  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 0 Address Registers
 |           +-04.2  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 0 Rank Registers
 |           +-04.3  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 0 Thermal Control Registers
 |           +-05.0  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 1 Control Registers
 |           +-05.1  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 1 Address Registers
 |           +-05.2  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 1 Rank Registers
 |           +-05.3  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 1 Thermal Control Registers
 |           +-06.0  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 2 Control Registers
 |           +-06.1  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 2 Address Registers
 |           +-06.2  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 2 Rank Registers
 |           \-06.3  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 2 Thermal Control Registers
 \-[0000:ff]-+-00.0  Intel Corporation Xeon 5500/Core i7 QuickPath Architecture Generic Non-Core Registers
             +-00.1  Intel Corporation Xeon 5500/Core i7 QuickPath Architecture System Address Decoder
             +-02.0  Intel Corporation Xeon 5500/Core i7 QPI Link 0
             +-02.1  Intel Corporation Xeon 5500/Core i7 QPI Physical 0
             +-02.4  Intel Corporation Xeon 5500/Core i7 QPI Link 1
             +-02.5  Intel Corporation Xeon 5500/Core i7 QPI Physical 1
             +-03.0  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller
             +-03.1  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Target Address Decoder
             +-03.2  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller RAS Registers
             +-03.4  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Test Registers
             +-04.0  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 0 Control Registers
             +-04.1  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 0 Address Registers
             +-04.2  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 0 Rank Registers
             +-04.3  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 0 Thermal Control Registers
             +-05.0  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 1 Control Registers
             +-05.1  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 1 Address Registers
             +-05.2  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 1 Rank Registers
             +-05.3  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 1 Thermal Control Registers
             +-06.0  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 2 Control Registers
             +-06.1  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 2 Address Registers
             +-06.2  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 2 Rank Registers
             \-06.3  Intel Corporation Xeon 5500/Core i7 Integrated Memory Controller Channel 2 Thermal Control Registers

--- lspci numa nodes
    $ cat /sys/bus/pci/devices/0000:00:00.0/numa_node /sys/bus/pci/devices/0000:00:01.0/numa_node /sys/bus/pci/devices/0000:00:03.0/numa_node /sys/bus/pci/devices/0000:00:07.0/numa_node /sys/bus/pci/devices/0000:00:09.0/numa_node /sys/bus/pci/devices/0000:00:14.0/numa_node /sys/bus/pci/devices/0000:00:14.1/numa_node /sys/bus/pci/devices/0000:00:14.2/numa_node /sys/bus/pci/devices/0000:00:1a.0/numa_node /sys/bus/pci/devices/0000:00:1a.1/numa_node /sys/bus/pci/devices/0000:00:1a.7/numa_node /sys/bus/pci/devices/0000:00:1c.0/numa_node /sys/bus/pci/devices/0000:00:1d.0/numa_node /sys/bus/pci/devices/0000:00:1d.1/numa_node /sys/bus/pci/devices/0000:00:1d.7/numa_node /sys/bus/pci/devices/0000:00:1e.0/numa_node /sys/bus/pci/devices/0000:00:1f.0/numa_node /sys/bus/pci/devices/0000:01:00.0/numa_node /sys/bus/pci/devices/0000:01:00.1/numa_node /sys/bus/pci/devices/0000:02:00.0/numa_node /sys/bus/pci/devices/0000:02:00.1/numa_node /sys/bus/pci/devices/0000:04:00.0/numa_node /sys/bus/pci/devices/0000:04:00.1/numa_node /sys/bus/pci/devices/0000:06:03.0/numa_node /sys/bus/pci/devices/0000:fe:00.0/numa_node /sys/bus/pci/devices/0000:fe:00.1/numa_node /sys/bus/pci/devices/0000:fe:02.0/numa_node /sys/bus/pci/devices/0000:fe:02.1/numa_node /sys/bus/pci/devices/0000:fe:02.4/numa_node /sys/bus/pci/devices/0000:fe:02.5/numa_node /sys/bus/pci/devices/0000:fe:03.0/numa_node /sys/bus/pci/devices/0000:fe:03.1/numa_node /sys/bus/pci/devices/0000:fe:03.2/numa_node /sys/bus/pci/devices/0000:fe:03.4/numa_node /sys/bus/pci/devices/0000:fe:04.0/numa_node /sys/bus/pci/devices/0000:fe:04.1/numa_node /sys/bus/pci/devices/0000:fe:04.2/numa_node /sys/bus/pci/devices/0000:fe:04.3/numa_node /sys/bus/pci/devices/0000:fe:05.0/numa_node /sys/bus/pci/devices/0000:fe:05.1/numa_node /sys/bus/pci/devices/0000:fe:05.2/numa_node /sys/bus/pci/devices/0000:fe:05.3/numa_node /sys/bus/pci/devices/0000:fe:06.0/numa_node /sys/bus/pci/devices/0000:fe:06.1/numa_node /sys/bus/pci/devices/0000:fe:06.2/numa_node /sys/bus/pci/devices/0000:fe:06.3/numa_node /sys/bus/pci/devices/0000:ff:00.0/numa_node /sys/bus/pci/devices/0000:ff:00.1/numa_node /sys/bus/pci/devices/0000:ff:02.0/numa_node /sys/bus/pci/devices/0000:ff:02.1/numa_node /sys/bus/pci/devices/0000:ff:02.4/numa_node /sys/bus/pci/devices/0000:ff:02.5/numa_node /sys/bus/pci/devices/0000:ff:03.0/numa_node /sys/bus/pci/devices/0000:ff:03.1/numa_node /sys/bus/pci/devices/0000:ff:03.2/numa_node /sys/bus/pci/devices/0000:ff:03.4/numa_node /sys/bus/pci/devices/0000:ff:04.0/numa_node /sys/bus/pci/devices/0000:ff:04.1/numa_node /sys/bus/pci/devices/0000:ff:04.2/numa_node /sys/bus/pci/devices/0000:ff:04.3/numa_node /sys/bus/pci/devices/0000:ff:05.0/numa_node /sys/bus/pci/devices/0000:ff:05.1/numa_node /sys/bus/pci/devices/0000:ff:05.2/numa_node /sys/bus/pci/devices/0000:ff:05.3/numa_node /sys/bus/pci/devices/0000:ff:06.0/numa_node /sys/bus/pci/devices/0000:ff:06.1/numa_node /sys/bus/pci/devices/0000:ff:06.2/numa_node /sys/bus/pci/devices/0000:ff:06.3/numa_node
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1
-1

--- lsusb
    $ lsusb
Bus 001 Device 001: ID 1d6b:0002 Linux Foundation 2.0 root hub
Bus 001 Device 002: ID 0424:2514 Microchip Technology, Inc. (formerly SMSC) USB 2.0 Hub
Bus 001 Device 003: ID 1058:260d Western Digital Technologies, Inc. My Passport 260D
Bus 002 Device 001: ID 1d6b:0002 Linux Foundation 2.0 root hub
Bus 003 Device 001: ID 1d6b:0001 Linux Foundation 1.1 root hub
Bus 004 Device 001: ID 1d6b:0001 Linux Foundation 1.1 root hub
Bus 005 Device 001: ID 1d6b:0001 Linux Foundation 1.1 root hub
Bus 005 Device 002: ID 10d5:5a08 Uni Class Technology Co., Ltd Dual Bay Docking Station
Bus 005 Device 003: ID 0624:0248 Avocent Corp. Virtual Hub
Bus 006 Device 001: ID 1d6b:0001 Linux Foundation 1.1 root hub

--- lshw -short
    $ lshw -short
/root/check.sh: line 45: lshw: command not found
    [exit=127 / not installed or not permitted]

--- PCIe AER errors
    [missing: /sys/bus/pci/devices/0000:00:00.0/aer_dev_correctable]

--- PCIe AER summary (errors matter for NIC/NVMe stability)
    $ found=0
for d in /sys/bus/pci/devices/*; do
    [ -d "$d" ] || continue
    addr="$(basename "$d")"
    class="$(cat "$d/class" 2>/dev/null)"
    case "$class" in
        0x020000|0x010802|0x010700) ;;  # ethernet, nvme, raid
        *) continue ;;
    esac
    for f in "$d"/aer_dev_*; do
        [ -r "$f" ] || continue
        val="$(cat "$f" 2>/dev/null)"
        [ "$val" = "0" ] && continue
        [ "$val" = "" ] && continue
        printf '%s %s = %s\n' "$addr" "$(basename "$f")" "$val"
        found=1
    done
done
[ "$found" = "0" ] && echo "  no AER errors on NIC/NVMe/RAID devices"
0000:01:00.0 aer_dev_correctable = RxErr 0
BadTLP 0
BadDLLP 0
Rollover 0
Timeout 0
NonFatalErr 0
CorrIntErr 0
HeaderOF 0
TOTAL_ERR_COR 0
0000:01:00.0 aer_dev_fatal = Undefined 0
DLP 0
SDES 0
TLP 0
FCP 0
CmpltTO 0
CmpltAbrt 0
UnxCmplt 0
RxOF 0
MalfTLP 0
ECRC 0
UnsupReq 0
ACSViol 0
UncorrIntErr 0
BlockedTLP 0
AtomicOpBlocked 0
TLPBlockedErr 0
PoisonTLPBlocked 0
DMWrReqBlocked 0
IDECheck 0
MisIDETLP 0
PCRC_CHECK 0
TLPXlatBlocked 0
TOTAL_ERR_FATAL 0
0000:01:00.0 aer_dev_nonfatal = Undefined 0
DLP 0
SDES 0
TLP 0
FCP 0
CmpltTO 0
CmpltAbrt 0
UnxCmplt 0
RxOF 0
MalfTLP 0
ECRC 0
UnsupReq 0
ACSViol 0
UncorrIntErr 0
BlockedTLP 0
AtomicOpBlocked 0
TLPBlockedErr 0
PoisonTLPBlocked 0
DMWrReqBlocked 0
IDECheck 0
MisIDETLP 0
PCRC_CHECK 0
TLPXlatBlocked 0
TOTAL_ERR_NONFATAL 0
0000:01:00.1 aer_dev_correctable = RxErr 0
BadTLP 0
BadDLLP 0
Rollover 0
Timeout 0
NonFatalErr 0
CorrIntErr 0
HeaderOF 0
TOTAL_ERR_COR 0
0000:01:00.1 aer_dev_fatal = Undefined 0
DLP 0
SDES 0
TLP 0
FCP 0
CmpltTO 0
CmpltAbrt 0
UnxCmplt 0
RxOF 0
MalfTLP 0
ECRC 0
UnsupReq 0
ACSViol 0
UncorrIntErr 0
BlockedTLP 0
AtomicOpBlocked 0
TLPBlockedErr 0
PoisonTLPBlocked 0
DMWrReqBlocked 0
IDECheck 0
MisIDETLP 0
PCRC_CHECK 0
TLPXlatBlocked 0
TOTAL_ERR_FATAL 0
0000:01:00.1 aer_dev_nonfatal = Undefined 0
DLP 0
SDES 0
TLP 0
FCP 0
CmpltTO 0
CmpltAbrt 0
UnxCmplt 0
RxOF 0
MalfTLP 0
ECRC 0
UnsupReq 0
ACSViol 0
UncorrIntErr 0
BlockedTLP 0
AtomicOpBlocked 0
TLPBlockedErr 0
PoisonTLPBlocked 0
DMWrReqBlocked 0
IDECheck 0
MisIDETLP 0
PCRC_CHECK 0
TLPXlatBlocked 0
TOTAL_ERR_NONFATAL 0
0000:02:00.0 aer_dev_correctable = RxErr 0
BadTLP 0
BadDLLP 0
Rollover 0
Timeout 0
NonFatalErr 0
CorrIntErr 0
HeaderOF 0
TOTAL_ERR_COR 0
0000:02:00.0 aer_dev_fatal = Undefined 0
DLP 0
SDES 0
TLP 0
FCP 0
CmpltTO 0
CmpltAbrt 0
UnxCmplt 0
RxOF 0
MalfTLP 0
ECRC 0
UnsupReq 0
ACSViol 0
UncorrIntErr 0
BlockedTLP 0
AtomicOpBlocked 0
TLPBlockedErr 0
PoisonTLPBlocked 0
DMWrReqBlocked 0
IDECheck 0
MisIDETLP 0
PCRC_CHECK 0
TLPXlatBlocked 0
TOTAL_ERR_FATAL 0
0000:02:00.0 aer_dev_nonfatal = Undefined 0
DLP 0
SDES 0
TLP 0
FCP 0
CmpltTO 0
CmpltAbrt 0
UnxCmplt 0
RxOF 0
MalfTLP 0
ECRC 0
UnsupReq 0
ACSViol 0
UncorrIntErr 0
BlockedTLP 0
AtomicOpBlocked 0
TLPBlockedErr 0
PoisonTLPBlocked 0
DMWrReqBlocked 0
IDECheck 0
MisIDETLP 0
PCRC_CHECK 0
TLPXlatBlocked 0
TOTAL_ERR_NONFATAL 0
0000:02:00.1 aer_dev_correctable = RxErr 0
BadTLP 0
BadDLLP 0
Rollover 0
Timeout 0
NonFatalErr 0
CorrIntErr 0
HeaderOF 0
TOTAL_ERR_COR 0
0000:02:00.1 aer_dev_fatal = Undefined 0
DLP 0
SDES 0
TLP 0
FCP 0
CmpltTO 0
CmpltAbrt 0
UnxCmplt 0
RxOF 0
MalfTLP 0
ECRC 0
UnsupReq 0
ACSViol 0
UncorrIntErr 0
BlockedTLP 0
AtomicOpBlocked 0
TLPBlockedErr 0
PoisonTLPBlocked 0
DMWrReqBlocked 0
IDECheck 0
MisIDETLP 0
PCRC_CHECK 0
TLPXlatBlocked 0
TOTAL_ERR_FATAL 0
0000:02:00.1 aer_dev_nonfatal = Undefined 0
DLP 0
SDES 0
TLP 0
FCP 0
CmpltTO 0
CmpltAbrt 0
UnxCmplt 0
RxOF 0
MalfTLP 0
ECRC 0
UnsupReq 0
ACSViol 0
UncorrIntErr 0
BlockedTLP 0
AtomicOpBlocked 0
TLPBlockedErr 0
PoisonTLPBlocked 0
DMWrReqBlocked 0
IDECheck 0
MisIDETLP 0
PCRC_CHECK 0
TLPXlatBlocked 0
TOTAL_ERR_NONFATAL 0
0000:04:00.0 aer_dev_correctable = RxErr 0
BadTLP 0
BadDLLP 0
Rollover 0
Timeout 0
NonFatalErr 0
CorrIntErr 0
HeaderOF 0
TOTAL_ERR_COR 0
0000:04:00.0 aer_dev_fatal = Undefined 0
DLP 0
SDES 0
TLP 0
FCP 0
CmpltTO 0
CmpltAbrt 0
UnxCmplt 0
RxOF 0
MalfTLP 0
ECRC 0
UnsupReq 0
ACSViol 0
UncorrIntErr 0
BlockedTLP 0
AtomicOpBlocked 0
TLPBlockedErr 0
PoisonTLPBlocked 0
DMWrReqBlocked 0
IDECheck 0
MisIDETLP 0
PCRC_CHECK 0
TLPXlatBlocked 0
TOTAL_ERR_FATAL 0
0000:04:00.0 aer_dev_nonfatal = Undefined 0
DLP 0
SDES 0
TLP 0
FCP 0
CmpltTO 0
CmpltAbrt 0
UnxCmplt 0
RxOF 0
MalfTLP 0
ECRC 0
UnsupReq 0
ACSViol 0
UncorrIntErr 0
BlockedTLP 0
AtomicOpBlocked 0
TLPBlockedErr 0
PoisonTLPBlocked 0
DMWrReqBlocked 0
IDECheck 0
MisIDETLP 0
PCRC_CHECK 0
TLPXlatBlocked 0
TOTAL_ERR_NONFATAL 0
0000:04:00.1 aer_dev_correctable = RxErr 0
BadTLP 0
BadDLLP 0
Rollover 0
Timeout 0
NonFatalErr 0
CorrIntErr 0
HeaderOF 0
TOTAL_ERR_COR 0
0000:04:00.1 aer_dev_fatal = Undefined 0
DLP 0
SDES 0
TLP 0
FCP 0
CmpltTO 0
CmpltAbrt 0
UnxCmplt 0
RxOF 0
MalfTLP 0
ECRC 0
UnsupReq 0
ACSViol 0
UncorrIntErr 0
BlockedTLP 0
AtomicOpBlocked 0
TLPBlockedErr 0
PoisonTLPBlocked 0
DMWrReqBlocked 0
IDECheck 0
MisIDETLP 0
PCRC_CHECK 0
TLPXlatBlocked 0
TOTAL_ERR_FATAL 0
0000:04:00.1 aer_dev_nonfatal = Undefined 0
DLP 0
SDES 0
TLP 0
FCP 0
CmpltTO 0
CmpltAbrt 0
UnxCmplt 0
RxOF 0
MalfTLP 0
ECRC 0
UnsupReq 0
ACSViol 0
UncorrIntErr 0
BlockedTLP 0
AtomicOpBlocked 0
TLPBlockedErr 0
PoisonTLPBlocked 0
DMWrReqBlocked 0
IDECheck 0
MisIDETLP 0
PCRC_CHECK 0
TLPXlatBlocked 0
TOTAL_ERR_NONFATAL 0
    [exit=1]

###############################################################################
# 4. CPU POWER / FREQUENCY / IDLE STATES
###############################################################################

--- scaling_governor per cpu (counts)
    $ for c in /sys/devices/system/cpu/cpu*/cpufreq/scaling_governor; do
    [ -e "$c" ] || continue
    cat "$c"
done | sort | uniq -c
     16 performance

--- scaling_driver / available governors / freq limits
    $ for f in /sys/devices/system/cpu/cpu0/cpufreq/*; do
    [ -r "$f" ] || continue
    [ -d "$f" ] && continue
    printf '%-40s = %s\n' "$(basename "$f")" "$(cat "$f" 2>/dev/null)"
done
affected_cpus                            = 0
bios_limit                               = 2395000
boost                                    = 1
cpuinfo_avg_freq                         = 2359038
cpuinfo_cur_freq                         = 2395000
cpuinfo_max_freq                         = 2395000
cpuinfo_min_freq                         = 1596000
cpuinfo_transition_latency               = 10000
freqdomain_cpus                          = 0 2 4 6 8 10 12 14
related_cpus                             = 0
scaling_available_frequencies            = 2395000 2394000 2261000 2128000 1995000 1862000 1729000 1596000 
scaling_available_governors              = conservative ondemand userspace powersave performance schedutil 
scaling_boost_frequencies                = 
scaling_cur_freq                         = 1766059
scaling_driver                           = acpi-cpufreq
scaling_governor                         = performance
scaling_max_freq                         = 2395000
scaling_min_freq                         = 1596000
scaling_setspeed                         = <unsupported>

--- EPP / EPB / intel_pstate
    $ echo "intel_pstate status: $(cat /sys/devices/system/cpu/intel_pstate/status 2>/dev/null)"
echo "intel_pstate no_turbo: $(cat /sys/devices/system/cpu/intel_pstate/no_turbo 2>/dev/null)"
echo "intel_pstate turbo_pct: $(cat /sys/devices/system/cpu/intel_pstate/turbo_pct 2>/dev/null)"
echo "intel_pstate max_perf_pct: $(cat /sys/devices/system/cpu/intel_pstate/max_perf_pct 2>/dev/null)"
echo "intel_pstate min_perf_pct: $(cat /sys/devices/system/cpu/intel_pstate/min_perf_pct 2>/dev/null)"
echo "EPB (energy_perf_bias) per cpu:"
for c in /sys/devices/system/cpu/cpu*/power/energy_perf_bias; do
    [ -r "$c" ] || continue
    printf '  %s : %s\n' "$(echo "$c" | cut -d/ -f5)" "$(cat "$c" 2>/dev/null)"
done | sort | uniq -c
echo "EPP (energy_performance_preference) per cpu:"
for c in /sys/devices/system/cpu/cpu*/cpufreq/energy_performance_preference; do
    [ -r "$c" ] || continue
    printf '  %s : %s\n' "$(echo "$c" | cut -d/ -f5)" "$(cat "$c" 2>/dev/null)"
done | sort | uniq -c
echo "available EPP:"
cat /sys/devices/system/cpu/cpu0/cpufreq/energy_performance_available_preferences 2>/dev/null
intel_pstate status: 
intel_pstate no_turbo: 
intel_pstate turbo_pct: 
intel_pstate max_perf_pct: 
intel_pstate min_perf_pct: 
EPB (energy_perf_bias) per cpu:
EPP (energy_performance_preference) per cpu:
available EPP:
    [exit=1]

--- cpupower frequency-info
    $ cpupower frequency-info
analyzing CPU 2:
  driver: acpi-cpufreq
  CPUs which run at the same hardware frequency: 2
  CPUs which need to have their frequency coordinated by software: 2
  maximum transition latency: 10.0 us
  hardware limits: 1.60 GHz - 2.40 GHz
  available frequency steps:  2.40 GHz, 2.39 GHz, 2.26 GHz, 2.13 GHz, 2.00 GHz, 1.86 GHz, 1.73 GHz, 1.60 GHz
  available cpufreq governors: conservative ondemand userspace powersave performance schedutil
  current policy: frequency should be within 1.60 GHz and 2.40 GHz.
                  The governor "performance" may decide which speed to use
                  within this range.
  current CPU frequency: 2.40 GHz (asserted by call to hardware)
  boost state support:
    Supported: yes
    Active: yes
    2533 MHz max turbo 4 active cores
    2533 MHz max turbo 3 active cores
    2667 MHz max turbo 2 active cores
    2667 MHz max turbo 1 active cores

--- turbostat snapshot
    $ timeout 3 turbostat --quiet --show CPU,Core,Bzy_MHz,IRQ,Busy%,Bzy_MHz,TSC_MHz,CoreTmp,PkgTmp sleep 1
1.002855 sec
Core	CPU	Busy%	Bzy_MHz	TSC_MHz	IRQ	CoreTmp
-	-	0.56	1898	2394	1833	45
0	1	0.39	1912	2394	95	45
0	9	0.84	1829	2394	70
1	3	0.36	2027	2394	52	41
1	11	0.79	1992	2394	186
2	5	0.23	2253	2394	29	43
2	13	0.57	2145	2394	76
3	7	1.40	1654	2394	609	44
3	15	0.33	2003	2394	134
0	0	0.34	1891	2394	52	42
0	8	1.01	1890	2394	146
1	2	0.26	1940	2394	31	42
1	10	0.29	1841	2394	46
2	4	0.42	2019	2394	40	41
2	12	0.34	1794	2394	61
3	6	0.61	1921	2394	108	40
3	14	0.71	1907	2394	98

--- x86_energy_perf_policy -r
    $ x86_energy_perf_policy -r

--- C-states (idle) enabled per cpu0
    $ for s in /sys/devices/system/cpu/cpu0/cpuidle/state*; do
    [ -d "$s" ] || continue
    printf '  %s : %s disabled=%s  latency=%sus  residency=%sus\n' \
        "$(cat "$s/name" 2>/dev/null)" \
        "$(cat "$s/desc" 2>/dev/null)" \
        "$(cat "$s/disable" 2>/dev/null)" \
        "$(cat "$s/latency" 2>/dev/null)" \
        "$(cat "$s/time" 2>/dev/null)"
done
  POLL : CPUIDLE CORE POLL IDLE disabled=0  latency=0us  residency=5031906us
  C1 : MWAIT 0x00 disabled=0  latency=3us  residency=83783731us
  C1E : MWAIT 0x01 disabled=0  latency=10us  residency=212292799593us
  C3 : MWAIT 0x10 disabled=1  latency=20us  residency=0us
  C6 : MWAIT 0x20 disabled=0  latency=200us  residency=67917800us

--- THP enabled
    $ cat /sys/kernel/mm/transparent_hugepage/enabled
always [madvise] never

--- THP defrag
    $ cat /sys/kernel/mm/transparent_hugepage/defrag
always defer defer+madvise [madvise] never

--- THP khugepaged pages_to_scan
    $ cat /sys/kernel/mm/transparent_hugepage/khugepaged/pages_to_scan
4096

--- THP khugepaged defrag
    $ cat /sys/kernel/mm/transparent_hugepage/khugepaged/defrag
1

--- microcode
    $ dmesg
[215256.782997] Memory failure: 0x166dca: unhandlable page.
[215256.913265] mce: [Hardware Error]: Machine check events logged
[215256.913297] EDAC MC0: 147 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215257.353735] mce: [Hardware Error]: Machine check events logged
[215257.353761] RAS: Soft-offlining pfn: 0x80fb9c
[215257.353773] EDAC MC0: 594 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215257.353836] Memory failure: 0x80fb9c: unhandlable page.
[215257.372738] mce: [Hardware Error]: Machine check events logged
[215257.385185] mce: [Hardware Error]: Machine check events logged
[215257.385204] RAS: Soft-offlining pfn: 0x80fb98
[215257.385216] EDAC MC0: 425 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215257.388033] Memory failure: 0x80fb98: unhandlable page.
[215257.400628] mce: [Hardware Error]: Machine check events logged
[215257.420094] mce: [Hardware Error]: Machine check events logged
[215257.420129] EDAC MC0: 656 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215257.436469] mce: [Hardware Error]: Machine check events logged
[215257.454776] mce: [Hardware Error]: Machine check events logged
[215257.454808] EDAC MC0: 791 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215257.467925] mce: [Hardware Error]: Machine check events logged
[215257.467947] RAS: Soft-offlining pfn: 0x166dca
[215257.467959] EDAC MC0: 32714 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215257.468298] Memory failure: 0x166dca: unhandlable page.
[215257.512923] mce: [Hardware Error]: Machine check events logged
[215257.512948] EDAC MC0: 371 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215257.527741] mce: [Hardware Error]: Machine check events logged
[215257.527772] EDAC MC0: 161 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215257.561270] mce: [Hardware Error]: Machine check events logged
[215257.575024] mce: [Hardware Error]: Machine check events logged
[215257.575055] EDAC MC0: 1313 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215257.612156] mce: [Hardware Error]: Machine check events logged
[215257.683854] mce: [Hardware Error]: Machine check events logged
[215257.683870] RAS: Soft-offlining pfn: 0x80fd18
[215257.683882] EDAC MC0: 28500 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215257.684973] Memory failure: 0x80fd18: unhandlable page.
[215257.693698] mce: [Hardware Error]: Machine check events logged
[215257.693720] RAS: Soft-offlining pfn: 0x80fc30
[215257.693734] EDAC MC0: 383 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215257.695477] Memory failure: 0x80fc30: unhandlable page.
[215257.710377] mce: [Hardware Error]: Machine check events logged
[215257.731915] mce: [Hardware Error]: Machine check events logged
[215257.731951] EDAC MC0: 806 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215257.757464] mce: [Hardware Error]: Machine check events logged
[215257.757489] EDAC MC0: 589 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215257.784560] mce: [Hardware Error]: Machine check events logged
[215258.115200] mce: [Hardware Error]: Machine check events logged
[215258.115230] EDAC MC0: 545 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215258.265362] mce: [Hardware Error]: Machine check events logged
[215258.265382] RAS: Soft-offlining pfn: 0x165b9e
[215258.265394] EDAC MC0: 76 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215258.265927] Memory failure: 0x165b9e: unhandlable page.
[215258.316221] mce: [Hardware Error]: Machine check events logged
[215258.316238] EDAC MC0: 72 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215258.359292] mce: [Hardware Error]: Machine check events logged
[215258.636117] mce: [Hardware Error]: Machine check events logged
[215258.636156] EDAC MC0: 13697 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215258.777153] mce: [Hardware Error]: Machine check events logged
[215258.777181] EDAC MC0: 36 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215258.805221] mce: [Hardware Error]: Machine check events logged
[215258.809707] mce: [Hardware Error]: Machine check events logged
[215258.809726] EDAC MC0: 414 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215258.818747] mce: [Hardware Error]: Machine check events logged
[215258.824743] mce: [Hardware Error]: Machine check events logged
[215259.015950] mce: [Hardware Error]: Machine check events logged
[215259.015973] RAS: Soft-offlining pfn: 0x165a08
[215259.015986] EDAC MC0: 210 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215259.016228] Memory failure: 0x165a08: unhandlable page.
[215259.596081] mce: [Hardware Error]: Machine check events logged
[215259.596112] EDAC MC0: 25401 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215259.770977] mce: [Hardware Error]: Machine check events logged
[215259.770989] RAS: Soft-offlining pfn: 0x80fa98
[215259.770997] EDAC MC0: 153 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215259.774091] Memory failure: 0x80fa98: unhandlable page.
[215259.786694] EDID block 0 (tag 0x00) checksum is invalid, remainder is 125
[215259.788340] mce: [Hardware Error]: Machine check events logged
[215259.788355] RAS: Soft-offlining pfn: 0x165b98
[215259.788363] EDAC MC0: 32699 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215259.788388] Memory failure: 0x165b98: unhandlable page.
[215259.808875] mce: [Hardware Error]: Machine check events logged
[215260.063943] mce: [Hardware Error]: Machine check events logged
[215260.064044] RAS: Soft-offlining pfn: 0x80fa9c
[215260.064065] EDAC MC0: 975 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215260.064103] Memory failure: 0x80fa9c: unhandlable page.
[215260.610141] mce: [Hardware Error]: Machine check events logged
[215260.610171] EDAC MC0: 32061 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215260.620045] mce: [Hardware Error]: Machine check events logged
[215260.620069] EDAC MC0: 21026 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215260.643183] mce: [Hardware Error]: Machine check events logged
[215260.705759] mce: [Hardware Error]: Machine check events logged
[215260.705782] RAS: Soft-offlining pfn: 0x166dca
[215260.705796] EDAC MC0: 489 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215260.705988] Memory failure: 0x166dca: unhandlable page.
[215260.786511] mce: [Hardware Error]: Machine check events logged
[215260.786537] EDAC MC0: 32758 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215260.811932] mce: [Hardware Error]: Machine check events logged
[215260.811956] EDAC MC0: 45 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215261.360224] mce: [Hardware Error]: Machine check events logged
[215261.360251] EDAC MC0: 32731 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215261.580002] mce: [Hardware Error]: Machine check events logged
[215262.124082] mce: [Hardware Error]: Machine check events logged
[215262.124109] EDAC MC0: 8201 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215262.603969] mce: [Hardware Error]: Machine check events logged
[215262.767059] mce: [Hardware Error]: Machine check events logged
[215262.767084] EDAC MC0: 20087 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215262.788211] mce: [Hardware Error]: Machine check events logged
[215262.788240] EDAC MC0: 180 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215263.096847] mce: [Hardware Error]: Machine check events logged
[215263.096869] EDAC MC0: 205 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215263.108339] mce: [Hardware Error]: Machine check events logged
[215263.108367] EDAC MC0: 420 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215263.122594] mce: [Hardware Error]: Machine check events logged
[215263.122629] EDAC MC0: 745 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215263.136306] mce: [Hardware Error]: Machine check events logged
[215263.136331] RAS: Soft-offlining pfn: 0x80fb22
[215263.136346] EDAC MC0: 325 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215263.136971] Memory failure: 0x80fb22: unhandlable page.
[215263.149133] mce: [Hardware Error]: Machine check events logged
[215263.149152] RAS: Soft-offlining pfn: 0x80fa98
[215263.149163] EDAC MC0: 32691 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215263.149360] Memory failure: 0x80fa98: unhandlable page.
[215263.164059] mce: [Hardware Error]: Machine check events logged
[215263.164094] EDAC MC0: 493 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215263.176795] mce: [Hardware Error]: Machine check events logged
[215263.272692] mce: [Hardware Error]: Machine check events logged
[215263.272728] EDAC MC0: 651 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215263.625929] mce: [Hardware Error]: Machine check events logged
[215263.627930] mce: [Hardware Error]: Machine check events logged
[215263.627960] RAS: Soft-offlining pfn: 0x80fbb2
[215263.627972] EDAC MC0: 248 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215263.628293] Memory failure: 0x80fbb2: unhandlable page.
[215263.778119] mce: [Hardware Error]: Machine check events logged
[215263.783961] mce: [Hardware Error]: Machine check events logged
[215263.783992] EDAC MC0: 396 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215263.845571] mce: [Hardware Error]: Machine check events logged
[215264.220639] mce: [Hardware Error]: Machine check events logged
[215264.220678] EDAC MC0: 355 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215264.587966] mce: [Hardware Error]: Machine check events logged
[215264.587993] RAS: Soft-offlining pfn: 0x80fa18
[215264.588006] EDAC MC0: 16190 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215264.588198] Memory failure: 0x80fa18: unhandlable page.
[215264.779273] mce: [Hardware Error]: Machine check events logged
[215264.781831] EDAC MC0: 8950 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215264.827556] mce: [Hardware Error]: Machine check events logged
[215264.827576] EDAC MC0: 23898 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215265.237150] mce: [Hardware Error]: Machine check events logged
[215265.237178] EDAC MC0: 33 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215265.611875] mce: [Hardware Error]: Machine check events logged
[215265.611915] EDAC MC0: 12680 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215265.760087] mce: [Hardware Error]: Machine check events logged
[215265.986349] mce: [Hardware Error]: Machine check events logged
[215265.986382] EDAC MC0: 607 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215266.473158] mce: [Hardware Error]: Machine check events logged
[215266.635817] mce: [Hardware Error]: Machine check events logged
[215266.777176] mce: [Hardware Error]: Machine check events logged
[215266.777205] EDAC MC0: 11694 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215266.790129] mce: [Hardware Error]: Machine check events logged
[215266.790148] EDAC MC0: 32726 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215266.838653] mce: [Hardware Error]: Machine check events logged
[215266.838684] EDAC MC0: 79 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215267.287699] mce: [Hardware Error]: Machine check events logged
[215267.595794] mce: [Hardware Error]: Machine check events logged
[215267.595832] EDAC MC0: 12065 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215267.788733] mce: [Hardware Error]: Machine check events logged
[215267.788756] RAS: Soft-offlining pfn: 0x166dca
[215267.788774] EDAC MC0: 661 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215267.792393] Memory failure: 0x166dca: unhandlable page.
[215267.798625] mce: [Hardware Error]: Machine check events logged
[215267.798648] EDAC MC0: 32590 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215267.823619] mce: [Hardware Error]: Machine check events logged
[215267.823656] EDAC MC0: 869 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215267.838903] mce: [Hardware Error]: Machine check events logged
[215267.838926] RAS: Soft-offlining pfn: 0x80fab4
[215267.838939] EDAC MC0: 490 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215267.839136] Memory failure: 0x80fab4: unhandlable page.
[215267.855786] mce: [Hardware Error]: Machine check events logged
[215267.871268] mce: [Hardware Error]: Machine check events logged
[215267.884930] mce: [Hardware Error]: Machine check events logged
[215267.905762] mce: [Hardware Error]: Machine check events logged
[215267.905791] RAS: Soft-offlining pfn: 0x166dca
[215267.905807] EDAC MC0: 1285 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215267.906503] Memory failure: 0x166dca: unhandlable page.
[215267.917449] mce: [Hardware Error]: Machine check events logged
[215267.932229] mce: [Hardware Error]: Machine check events logged
[215267.932267] EDAC MC0: 536 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215267.946293] mce: [Hardware Error]: Machine check events logged
[215267.946316] RAS: Soft-offlining pfn: 0x166dca
[215267.946328] EDAC MC0: 572 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215267.953283] Memory failure: 0x166dca: unhandlable page.
[215267.960416] mce: [Hardware Error]: Machine check events logged
[215267.978227] mce: [Hardware Error]: Machine check events logged
[215267.978255] EDAC MC0: 599 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215268.001007] mce: [Hardware Error]: Machine check events logged
[215268.019769] mce: [Hardware Error]: Machine check events logged
[215268.019801] EDAC MC0: 753 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215268.034137] mce: [Hardware Error]: Machine check events logged
[215268.034173] EDAC MC0: 359 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215268.050568] mce: [Hardware Error]: Machine check events logged
[215268.081225] mce: [Hardware Error]: Machine check events logged
[215268.081252] EDAC MC0: 578 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215268.094216] mce: [Hardware Error]: Machine check events logged
[215268.094238] RAS: Soft-offlining pfn: 0x166dca
[215268.094248] EDAC MC0: 32682 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215268.094487] Memory failure: 0x166dca: unhandlable page.
[215268.135891] mce: [Hardware Error]: Machine check events logged
[215268.135915] EDAC MC0: 278 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215268.158022] mce: [Hardware Error]: Machine check events logged
[215268.158084] EDAC MC0: 558 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215268.520280] mce: [Hardware Error]: Machine check events logged
[215268.520315] EDAC MC0: 32642 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215268.619742] mce: [Hardware Error]: Machine check events logged
[215268.780957] mce: [Hardware Error]: Machine check events logged
[215268.780982] RAS: Soft-offlining pfn: 0x80fc98
[215268.780997] EDAC MC0: 5132 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215268.781263] Memory failure: 0x80fc98: unhandlable page.
[215268.797751] mce: [Hardware Error]: Machine check events logged
[215268.797782] EDAC MC0: 32675 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215269.217580] mce: [Hardware Error]: Machine check events logged
[215269.579713] mce: [Hardware Error]: Machine check events logged
[215269.579749] RAS: Soft-offlining pfn: 0x167e4e
[215269.579765] EDAC MC0: 13722 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215269.579940] Memory failure: 0x167e4e: unhandlable page.
[215269.902575] i2c i2c-0: sendbytes: NAK bailout.
[215269.905366] mce: [Hardware Error]: Machine check events logged
[215269.905390] EDAC MC0: 120 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215269.966156] i2c i2c-0: sendbytes: NAK bailout.
[215269.997388] i2c i2c-0: sendbytes: NAK bailout.
[215270.028450] EDID block 0 (tag 0x00) checksum is invalid, remainder is 125
[215270.044761] mce: [Hardware Error]: Machine check events logged
[215270.044872] RAS: Soft-offlining pfn: 0x165b98
[215270.044935] EDAC MC0: 110 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215270.045735] Memory failure: 0x165b98: unhandlable page.
[215270.084880] mce: [Hardware Error]: Machine check events logged
[215270.085072] RAS: Soft-offlining pfn: 0x165b9e
[215270.085083] EDAC MC0: 2179 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215270.085128] Memory failure: 0x165b9e: unhandlable page.
[215270.473188] mce: [Hardware Error]: Machine check events logged
[215270.473211] EDAC MC0: 31053 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215270.603679] mce: [Hardware Error]: Machine check events logged
[215270.603708] RAS: Soft-offlining pfn: 0x166dca
[215270.603720] EDAC MC0: 3271 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215270.603876] Memory failure: 0x166dca: unhandlable page.
[215270.663842] mce: [Hardware Error]: Machine check events logged
[215270.665101] EDAC MC0: 4497 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215270.696064] mce: [Hardware Error]: Machine check events logged
[215270.696092] EDAC MC0: 28899 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215270.781547] mce: [Hardware Error]: Machine check events logged
[215270.798883] mce: [Hardware Error]: Machine check events logged
[215270.798920] EDAC MC0: 1775 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215271.042356] mce: [Hardware Error]: Machine check events logged
[215271.374179] mce: [Hardware Error]: Machine check events logged
[215271.374204] RAS: Soft-offlining pfn: 0x166dca
[215271.374219] EDAC MC0: 32020 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215271.374439] Memory failure: 0x166dca: unhandlable page.
[215271.627655] mce: [Hardware Error]: Machine check events logged
[215271.799348] mce: [Hardware Error]: Machine check events logged
[215271.799376] EDAC MC0: 16050 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215271.997209] mce: [Hardware Error]: Machine check events logged
[215271.997241] EDAC MC0: 156 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215272.167459] mce: [Hardware Error]: Machine check events logged
[215272.167473] RAS: Soft-offlining pfn: 0x166dca
[215272.167484] EDAC MC0: 274 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215272.167637] Memory failure: 0x166dca: unhandlable page.
[215272.587602] mce: [Hardware Error]: Machine check events logged
[215272.788459] mce: [Hardware Error]: Machine check events logged
[215272.788491] EDAC MC0: 23541 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215272.852840] mce: [Hardware Error]: Machine check events logged
[215272.852869] EDAC MC0: 260 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215273.191500] mce: [Hardware Error]: Machine check events logged
[215273.203194] mce: [Hardware Error]: Machine check events logged
[215273.203212] RAS: Soft-offlining pfn: 0x80fb9c
[215273.203225] EDAC MC0: 460 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215273.203592] Memory failure: 0x80fb9c: unhandlable page.
[215273.216571] mce: [Hardware Error]: Machine check events logged
[215273.216593] EDAC MC0: 196 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215273.232251] mce: [Hardware Error]: Machine check events logged
[215273.232284] EDAC MC0: 510 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215273.245021] mce: [Hardware Error]: Machine check events logged
[215273.262304] mce: [Hardware Error]: Machine check events logged
[215273.262332] EDAC MC0: 531 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215273.273642] mce: [Hardware Error]: Machine check events logged
[215273.273679] EDAC MC0: 329 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215273.350837] mce: [Hardware Error]: Machine check events logged
[215273.611570] mce: [Hardware Error]: Machine check events logged
[215273.611607] RAS: Soft-offlining pfn: 0x100026
[215273.611624] EDAC MC0: 20935 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215273.612020] Memory failure: 0x100026: unhandlable page.
[215274.166632] mce: [Hardware Error]: Machine check events logged
[215274.166719] EDAC MC0: 529 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215274.635521] mce: [Hardware Error]: Machine check events logged
[215274.779449] mce: [Hardware Error]: Machine check events logged
[215274.801225] mce: [Hardware Error]: Machine check events logged
[215274.801247] RAS: Soft-offlining pfn: 0x80fb18
[215274.801262] EDAC MC0: 17068 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215274.801474] Memory failure: 0x80fb18: unhandlable page.
[215275.133960] mce: [Hardware Error]: Machine check events logged
[215275.133989] RAS: Soft-offlining pfn: 0x166dca
[215275.134005] EDAC MC0: 270 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215275.134213] Memory failure: 0x166dca: unhandlable page.
[215275.410966] mce: [Hardware Error]: Machine check events logged
[215275.410987] EDAC MC0: 65 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215275.595486] mce: [Hardware Error]: Machine check events logged
[215275.595529] EDAC MC0: 16538 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215275.771748] mce: [Hardware Error]: Machine check events logged
[215275.795389] mce: [Hardware Error]: Machine check events logged
[215276.125355] mce: [Hardware Error]: Machine check events logged
[215276.125387] RAS: Soft-offlining pfn: 0x80fc34
[215276.125408] EDAC MC0: 991 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215276.125638] Memory failure: 0x80fc34: unhandlable page.
[215276.535673] mce: [Hardware Error]: Machine check events logged
[215276.535697] EDAC MC0: 32701 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215276.619446] mce: [Hardware Error]: Machine check events logged
[215276.619491] EDAC MC0: 7240 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215276.779832] mce: [Hardware Error]: Machine check events logged
[215276.779850] RAS: Soft-offlining pfn: 0x80fb98
[215276.779861] EDAC MC0: 508 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215276.780058] Memory failure: 0x80fb98: unhandlable page.
[215276.799480] mce: [Hardware Error]: Machine check events logged
[215276.799502] RAS: Soft-offlining pfn: 0x166dca
[215276.799515] EDAC MC0: 201 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215276.799742] Memory failure: 0x166dca: unhandlable page.
[215277.154897] mce: [Hardware Error]: Machine check events logged
[215277.154923] EDAC MC0: 123 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215277.179251] mce: [Hardware Error]: Machine check events logged
[215277.195335] mce: [Hardware Error]: Machine check events logged
[215277.217535] mce: [Hardware Error]: Machine check events logged
[215277.217575] EDAC MC0: 1490 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215277.228254] mce: [Hardware Error]: Machine check events logged
[215277.228277] RAS: Soft-offlining pfn: 0x166dca
[215277.228290] EDAC MC0: 197 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215277.228883] Memory failure: 0x166dca: unhandlable page.
[215277.239822] mce: [Hardware Error]: Machine check events logged
[215277.239852] EDAC MC0: 314 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215277.344207] mce: [Hardware Error]: Machine check events logged
[215277.344227] EDAC MC0: 50 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215277.374039] mce: [Hardware Error]: Machine check events logged
[215277.374064] EDAC MC0: 32732 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215277.388831] mce: [Hardware Error]: Machine check events logged
[215277.389455] EDAC MC0: 1488 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215277.402525] mce: [Hardware Error]: Machine check events logged
[215277.402550] EDAC MC0: 31753 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215277.421829] mce: [Hardware Error]: Machine check events logged
[215277.421857] EDAC MC0: 323 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215277.441697] mce: [Hardware Error]: Machine check events logged
[215277.441725] EDAC MC0: 555 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215277.456757] mce: [Hardware Error]: Machine check events logged
[215277.498241] mce: [Hardware Error]: Machine check events logged
[215277.498294] EDAC MC0: 663 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215277.522296] mce: [Hardware Error]: Machine check events logged
[215277.522322] RAS: Soft-offlining pfn: 0x80fc30
[215277.522338] EDAC MC0: 573 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215277.523254] Memory failure: 0x80fc30: unhandlable page.
[215277.549892] mce: [Hardware Error]: Machine check events logged
[215277.574111] mce: [Hardware Error]: Machine check events logged
[215277.579404] mce: [Hardware Error]: Machine check events logged
[215277.609169] mce: [Hardware Error]: Machine check events logged
[215277.609197] EDAC MC0: 838 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215277.748698] mce: [Hardware Error]: Machine check events logged
[215277.748735] EDAC MC0: 295 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215278.040397] mce: [Hardware Error]: Machine check events logged
[215278.539473] mce: [Hardware Error]: Machine check events logged
[215278.603369] mce: [Hardware Error]: Machine check events logged
[215278.778319] mce: [Hardware Error]: Machine check events logged
[215278.780222] EDAC MC0: 10819 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215278.935263] mce: [Hardware Error]: Machine check events logged
[215278.935302] EDAC MC0: 26532 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215279.134311] mce: [Hardware Error]: Machine check events logged
[215279.134352] RAS: Soft-offlining pfn: 0x32000
[215279.134365] EDAC MC0: 238 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215279.134560] Memory failure: 0x32000: unhandlable page.
[215279.169405] mce: [Hardware Error]: Machine check events logged
[215279.169434] EDAC MC0: 32605 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215279.204509] mce: [Hardware Error]: Machine check events logged
[215279.204536] EDAC MC0: 16 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215279.242478] mce: [Hardware Error]: Machine check events logged
[215279.242501] RAS: Soft-offlining pfn: 0x165b98
[215279.242512] EDAC MC0: 372 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215279.242898] Memory failure: 0x165b98: unhandlable page.
[215279.275896] mce: [Hardware Error]: Machine check events logged
[215279.275915] RAS: Soft-offlining pfn: 0x166dca
[215279.275926] EDAC MC0: 31 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215279.276109] Memory failure: 0x166dca: unhandlable page.
[215279.314713] mce: [Hardware Error]: Machine check events logged
[215279.314741] EDAC MC0: 42 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215279.348784] mce: [Hardware Error]: Machine check events logged
[215279.348812] EDAC MC0: 4 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215279.378410] mce: [Hardware Error]: Machine check events logged
[215279.410828] mce: [Hardware Error]: Machine check events logged
[215279.446186] mce: [Hardware Error]: Machine check events logged
[215279.446208] RAS: Soft-offlining pfn: 0x80fa34
[215279.446222] EDAC MC0: 97 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215279.446263] Memory failure: 0x80fa34: unhandlable page.
[215279.480246] mce: [Hardware Error]: Machine check events logged
[215279.480268] RAS: Soft-offlining pfn: 0x80fa1c
[215279.480279] EDAC MC0: 10 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215279.480315] Memory failure: 0x80fa1c: unhandlable page.
[215279.512146] mce: [Hardware Error]: Machine check events logged
[215279.512164] RAS: Soft-offlining pfn: 0x165a1c
[215279.512173] EDAC MC0: 10 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215279.512204] Memory failure: 0x165a1c: unhandlable page.
[215279.552509] mce: [Hardware Error]: Machine check events logged
[215279.552531] RAS: Soft-offlining pfn: 0x165b9e
[215279.552541] EDAC MC0: 9 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215279.552574] Memory failure: 0x165b9e: unhandlable page.
[215279.588031] mce: [Hardware Error]: Machine check events logged
[215279.623733] mce: [Hardware Error]: Machine check events logged
[215279.627326] mce: [Hardware Error]: Machine check events logged
[215279.651244] mce: [Hardware Error]: Machine check events logged
[215279.651269] EDAC MC0: 4194 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215279.679935] mce: [Hardware Error]: Machine check events logged
[215279.706893] mce: [Hardware Error]: Machine check events logged
[215279.706922] EDAC MC0: 151 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215279.745229] mce: [Hardware Error]: Machine check events logged
[215279.745248] EDAC MC0: 37 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215279.774396] mce: [Hardware Error]: Machine check events logged
[215279.774418] RAS: Soft-offlining pfn: 0x166dca
[215279.774430] EDAC MC0: 155 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215279.774619] Memory failure: 0x166dca: unhandlable page.
[215279.785186] mce: [Hardware Error]: Machine check events logged
[215279.803235] mce: [Hardware Error]: Machine check events logged
[215279.803266] EDAC MC0: 417 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215279.834685] mce: [Hardware Error]: Machine check events logged
[215279.834705] RAS: Soft-offlining pfn: 0x165b98
[215279.834716] EDAC MC0: 32598 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215279.834779] Memory failure: 0x165b98: unhandlable page.
[215279.866599] mce: [Hardware Error]: Machine check events logged
[215279.866626] EDAC MC0: 40 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215279.898059] mce: [Hardware Error]: Machine check events logged
[215279.925334] mce: [Hardware Error]: Machine check events logged
[215279.925362] EDAC MC0: 106 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215279.949146] mce: [Hardware Error]: Machine check events logged
[215279.972858] mce: [Hardware Error]: Machine check events logged
[215279.972876] EDAC MC0: 92 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215280.003609] mce: [Hardware Error]: Machine check events logged
[215280.003633] EDAC MC0: 28 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215280.033876] mce: [Hardware Error]: Machine check events logged
[215280.033899] EDAC MC0: 54 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215280.065613] mce: [Hardware Error]: Machine check events logged
[215280.086312] mce: [Hardware Error]: Machine check events logged
[215280.086338] EDAC MC0: 156 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215280.113417] mce: [Hardware Error]: Machine check events logged
[215280.113437] RAS: Soft-offlining pfn: 0x166a1a
[215280.113447] EDAC MC0: 51 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215280.113514] Memory failure: 0x166a1a: unhandlable page.
[215280.141935] i2c i2c-0: sendbytes: NAK bailout.
[215280.143956] mce: [Hardware Error]: Machine check events logged
[215280.143975] EDAC MC0: 32747 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215280.170472] mce: [Hardware Error]: Machine check events logged
[215280.205697] i2c i2c-0: sendbytes: NAK bailout.
[215280.243879] mce: [Hardware Error]: Machine check events logged
[215280.243897] EDAC MC0: 453 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215280.267468] EDID has corrupt header
[215280.401394] mce: [Hardware Error]: Machine check events logged
[215280.401421] EDAC MC0: 219 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215280.587293] mce: [Hardware Error]: Machine check events logged
[215280.587327] RAS: Soft-offlining pfn: 0x80fdb4
[215280.587339] EDAC MC0: 8815 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215280.587672] Memory failure: 0x80fdb4: unhandlable page.
[215280.698469] mce: [Hardware Error]: Machine check events logged
[215280.698496] EDAC MC0: 89 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215280.717214] mce: [Hardware Error]: Machine check events logged
[215280.717238] EDAC MC0: 156 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215280.778610] mce: [Hardware Error]: Machine check events logged
[215280.778631] RAS: Soft-offlining pfn: 0x80fd9c
[215280.778642] EDAC MC0: 148 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215280.778833] Memory failure: 0x80fd9c: unhandlable page.
[215280.793479] mce: [Hardware Error]: Machine check events logged
[215280.990279] mce: [Hardware Error]: Machine check events logged
[215281.203493] mce: [Hardware Error]: Machine check events logged
[215281.203518] EDAC MC0: 54 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215281.611257] mce: [Hardware Error]: Machine check events logged
[215282.257455] mce: [Hardware Error]: Machine check events logged
[215282.257482] EDAC MC0: 29937 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215282.635223] mce: [Hardware Error]: Machine check events logged
[215282.635254] EDAC MC0: 10608 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215282.777434] mce: [Hardware Error]: Machine check events logged
[215282.777460] EDAC MC0: 250 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215282.790693] mce: [Hardware Error]: Machine check events logged
[215282.790715] EDAC MC0: 16300 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215283.232884] mce: [Hardware Error]: Machine check events logged
[215283.232905] RAS: Soft-offlining pfn: 0x165b98
[215283.232917] EDAC MC0: 32658 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215283.233110] Memory failure: 0x165b98: unhandlable page.
[215283.293517] mce: [Hardware Error]: Machine check events logged
[215283.293548] EDAC MC0: 248 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215283.308879] mce: [Hardware Error]: Machine check events logged
[215283.308902] RAS: Soft-offlining pfn: 0x166dca
[215283.308916] EDAC MC0: 458 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215283.315201] Memory failure: 0x166dca: unhandlable page.
[215283.328421] mce: [Hardware Error]: Machine check events logged
[215283.328456] EDAC MC0: 428 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215283.342066] mce: [Hardware Error]: Machine check events logged
[215283.361478] mce: [Hardware Error]: Machine check events logged
[215283.361505] EDAC MC0: 650 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215283.371986] mce: [Hardware Error]: Machine check events logged
[215283.448063] mce: [Hardware Error]: Machine check events logged
[215283.570396] mce: [Hardware Error]: Machine check events logged
[215283.570425] EDAC MC0: 668 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215283.595180] mce: [Hardware Error]: Machine check events logged
[215283.780731] mce: [Hardware Error]: Machine check events logged
[215283.780757] EDAC MC0: 9128 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215283.944416] mce: [Hardware Error]: Machine check events logged
[215283.944440] EDAC MC0: 153 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215284.440461] mce: [Hardware Error]: Machine check events logged
[215284.440490] EDAC MC0: 49 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215284.619142] mce: [Hardware Error]: Machine check events logged
[215284.619177] EDAC MC0: 4344 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215284.785019] mce: [Hardware Error]: Machine check events logged
[215284.976215] mce: [Hardware Error]: Machine check events logged
[215285.422179] mce: [Hardware Error]: Machine check events logged
[215285.422203] EDAC MC0: 143 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215285.579103] mce: [Hardware Error]: Machine check events logged
[215285.579138] EDAC MC0: 5937 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215285.862212] mce: [Hardware Error]: Machine check events logged
[215285.862243] EDAC MC0: 83 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215286.499146] mce: [Hardware Error]: Machine check events logged
[215286.499172] RAS: Soft-offlining pfn: 0x80fb18
[215286.499184] EDAC MC0: 87 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215286.499707] Memory failure: 0x80fb18: unhandlable page.
[215286.505184] audit: type=1400 audit(1785319652.624:2572): apparmor="DENIED" operation="create" class="net" info="failed protocol match" error=-13 profile="/{,usr/}sbin/dhclient" pid=1073 comm="dhclient" family="unix" sock_type="dgram" protocol=0 requested="create" denied="create" addr=none
[215286.506526] audit: type=1400 audit(1785319652.625:2573): apparmor="DENIED" operation="create" class="net" info="failed protocol match" error=-13 profile="/{,usr/}sbin/dhclient" pid=1073 comm="dhclient" family="unix" sock_type="dgram" protocol=0 requested="create" denied="create" addr=none
[215286.511997] mce: [Hardware Error]: Machine check events logged
[215286.512019] RAS: Soft-offlining pfn: 0x80fa18
[215286.512030] EDAC MC0: 293 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215286.513084] Memory failure: 0x80fa18: unhandlable page.
[215286.522975] mce: [Hardware Error]: Machine check events logged
[215286.522995] EDAC MC0: 555 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215286.535231] mce: [Hardware Error]: Machine check events logged
[215286.535253] EDAC MC0: 32726 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215286.545694] audit: type=1400 audit(1785319652.664:2574): apparmor="DENIED" operation="create" class="net" info="failed protocol match" error=-13 profile="/{,usr/}sbin/dhclient" pid=1073 comm="dhclient" family="unix" sock_type="dgram" protocol=0 requested="create" denied="create" addr=none
[215286.566832] mce: [Hardware Error]: Machine check events logged
[215286.566852] RAS: Soft-offlining pfn: 0x166dca
[215286.566866] EDAC MC0: 32753 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215286.567150] Memory failure: 0x166dca: unhandlable page.
[215286.603067] mce: [Hardware Error]: Machine check events logged
[215286.603094] RAS: Soft-offlining pfn: 0x165b9e
[215286.603105] EDAC MC0: 4194 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215286.603270] Memory failure: 0x165b9e: unhandlable page.
[215286.766100] mce: [Hardware Error]: Machine check events logged
[215286.766129] EDAC MC0: 125 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215286.775189] mce: [Hardware Error]: Machine check events logged
[215286.775597] RAS: Soft-offlining pfn: 0x80fc98
[215286.775606] EDAC MC0: 2450 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215286.775633] Memory failure: 0x80fc98: unhandlable page.
[215286.823018] mce: [Hardware Error]: Machine check events logged
[215286.823044] EDAC MC0: 30336 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215287.522837] mce: [Hardware Error]: Machine check events logged
[215287.627027] mce: [Hardware Error]: Machine check events logged
[215287.627875] EDAC MC0: 13239 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215287.651272] mce: [Hardware Error]: Machine check events logged
[215287.651308] EDAC MC0: 32298 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215287.674518] mce: [Hardware Error]: Machine check events logged
[215287.685392] mce: [Hardware Error]: Machine check events logged
[215287.717904] mce: [Hardware Error]: Machine check events logged
[215287.717928] EDAC MC0: 808 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215287.735600] mce: [Hardware Error]: Machine check events logged
[215287.735627] EDAC MC0: 885 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215287.760546] mce: [Hardware Error]: Machine check events logged
[215287.760621] RAS: Soft-offlining pfn: 0x80fa98
[215287.760633] EDAC MC0: 342 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215287.761044] Memory failure: 0x80fa98: unhandlable page.
[215287.771629] mce: [Hardware Error]: Machine check events logged
[215287.771653] EDAC MC0: 32361 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215287.793956] mce: [Hardware Error]: Machine check events logged
[215287.793979] EDAC MC0: 19 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215287.847817] mce: [Hardware Error]: Machine check events logged
[215287.847855] EDAC MC0: 482 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215287.868947] mce: [Hardware Error]: Machine check events logged
[215287.868974] RAS: Soft-offlining pfn: 0x80fd34
[215287.868991] EDAC MC0: 721 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215287.870040] Memory failure: 0x80fd34: unhandlable page.
[215287.883894] mce: [Hardware Error]: Machine check events logged
[215287.887032] EDAC MC0: 4785 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215287.899663] mce: [Hardware Error]: Machine check events logged
[215287.921899] mce: [Hardware Error]: Machine check events logged
[215287.921924] RAS: Soft-offlining pfn: 0x80fda2
[215287.921941] EDAC MC0: 29066 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215287.922833] Memory failure: 0x80fda2: unhandlable page.
[215287.938317] mce: [Hardware Error]: Machine check events logged
[215287.957477] mce: [Hardware Error]: Machine check events logged
[215287.967891] mce: [Hardware Error]: Machine check events logged
[215287.967928] EDAC MC0: 1134 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215287.982796] mce: [Hardware Error]: Machine check events logged
[215288.006866] mce: [Hardware Error]: Machine check events logged
[215288.031607] mce: [Hardware Error]: Machine check events logged
[215288.031639] EDAC MC0: 773 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215288.139027] mce: [Hardware Error]: Machine check events logged
[215288.344230] mce: [Hardware Error]: Machine check events logged
[215288.344256] RAS: Soft-offlining pfn: 0x165b98
[215288.344269] EDAC MC0: 194 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215288.344616] Memory failure: 0x165b98: unhandlable page.
[215288.586994] mce: [Hardware Error]: Machine check events logged
[215288.587031] EDAC MC0: 24337 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215288.780212] mce: [Hardware Error]: Machine check events logged
[215288.781039] EDAC MC0: 5320 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215288.796943] mce: [Hardware Error]: Machine check events logged
[215288.796966] EDAC MC0: 28307 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215289.156588] mce: [Hardware Error]: Machine check events logged
[215289.156611] RAS: Soft-offlining pfn: 0x166dca
[215289.156624] EDAC MC0: 32637 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215289.156816] Memory failure: 0x166dca: unhandlable page.
[215289.610973] mce: [Hardware Error]: Machine check events logged
[215289.611014] EDAC MC0: 24951 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215290.243423] mce: [Hardware Error]: Machine check events logged
[215290.379437] i2c i2c-0: sendbytes: NAK bailout.
[215290.379977] i2c i2c-0: sendbytes: NAK bailout.
[215290.385214] mce: [Hardware Error]: Machine check events logged
[215290.390934] EDAC MC0: 11418 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215290.506643] EDID block 0 (tag 0x00) checksum is invalid, remainder is 115
[215290.522646] mce: [Hardware Error]: Machine check events logged
[215290.522937] EDAC MC0: 22102 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215290.634918] mce: [Hardware Error]: Machine check events logged
[215290.634949] RAS: Soft-offlining pfn: 0x166dca
[215290.634962] EDAC MC0: 19334 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215290.635153] Memory failure: 0x166dca: unhandlable page.
[215290.739598] mce: [Hardware Error]: Machine check events logged
[215290.739629] EDAC MC0: 213 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215290.757783] mce: [Hardware Error]: Machine check events logged
[215290.777147] mce: [Hardware Error]: Machine check events logged
[215290.777174] EDAC MC0: 125 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215290.790468] mce: [Hardware Error]: Machine check events logged
[215290.856957] mce: [Hardware Error]: Machine check events logged
[215290.856977] EDAC MC0: 68 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215291.430802] mce: [Hardware Error]: Machine check events logged
[215291.594888] mce: [Hardware Error]: Machine check events logged
[215291.594925] RAS: Soft-offlining pfn: 0x80fa1c
[215291.594941] EDAC MC0: 8327 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215291.595234] Memory failure: 0x80fa1c: unhandlable page.
[215291.771177] mce: [Hardware Error]: Machine check events logged
[215291.771193] RAS: Soft-offlining pfn: 0x166dca
[215291.771203] EDAC MC0: 364 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215291.771405] Memory failure: 0x166dca: unhandlable page.
[215291.790248] mce: [Hardware Error]: Machine check events logged
[215291.790268] EDAC MC0: 17 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215292.132583] mce: [Hardware Error]: Machine check events logged
[215292.618847] mce: [Hardware Error]: Machine check events logged
[215292.783438] mce: [Hardware Error]: Machine check events logged
[215292.784527] RAS: Soft-offlining pfn: 0x80fc9c
[215292.784544] EDAC MC0: 27721 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215292.784608] Memory failure: 0x80fc9c: unhandlable page.
[215292.919026] mce: [Hardware Error]: Machine check events logged
[215292.919068] EDAC MC0: 28012 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215293.377519] mce: [Hardware Error]: Machine check events logged
[215293.380244] RAS: Soft-offlining pfn: 0x80fb18
[215293.380258] EDAC MC0: 9537 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215293.380849] Memory failure: 0x80fb18: unhandlable page.
[215293.387587] mce: [Hardware Error]: Machine check events logged
[215293.402706] mce: [Hardware Error]: Machine check events logged
[215293.404853] RAS: Soft-offlining pfn: 0x866dca
[215293.404866] EDAC MC0: 325 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215293.404873] Soft offline: 0x866dca: page already poisoned
[215293.412869] mce: [Hardware Error]: Machine check events logged
[215293.412900] EDAC MC0: 23663 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215293.426448] mce: [Hardware Error]: Machine check events logged
[215293.443372] mce: [Hardware Error]: Machine check events logged
[215293.455049] mce: [Hardware Error]: Machine check events logged
[215293.455082] EDAC MC0: 844 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215293.469277] mce: [Hardware Error]: Machine check events logged
[215293.469304] EDAC MC0: 332 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215293.578819] mce: [Hardware Error]: Machine check events logged
[215293.578855] EDAC MC0: 25770 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215294.039376] mce: [Hardware Error]: Machine check events logged
[215294.530856] mce: [Hardware Error]: Machine check events logged
[215294.602768] mce: [Hardware Error]: Machine check events logged
[215294.602805] EDAC MC0: 1915 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215294.784224] mce: [Hardware Error]: Machine check events logged
[215294.784241] RAS: Soft-offlining pfn: 0x80fb98
[215294.784251] EDAC MC0: 351 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215294.784569] Memory failure: 0x80fb98: unhandlable page.
[215294.800453] mce: [Hardware Error]: Machine check events logged
[215294.800476] EDAC MC0: 202 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215295.073606] mce: [Hardware Error]: Machine check events logged
[215295.073626] EDAC MC0: 81 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215295.536197] mce: [Hardware Error]: Machine check events logged
[215295.626737] mce: [Hardware Error]: Machine check events logged
[215295.626777] EDAC MC0: 4482 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215295.790416] mce: [Hardware Error]: Machine check events logged
[215295.790432] RAS: Soft-offlining pfn: 0x166dca
[215295.790440] EDAC MC0: 331 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215295.794732] Memory failure: 0x166dca: unhandlable page.
[215295.801863] mce: [Hardware Error]: Machine check events logged
[215295.801901] EDAC MC0: 36 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215296.192666] mce: [Hardware Error]: Machine check events logged
[215296.586688] mce: [Hardware Error]: Machine check events logged
[215296.785148] mce: [Hardware Error]: Machine check events logged
[215296.787698] EDAC MC0: 10067 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215296.799917] mce: [Hardware Error]: Machine check events logged
[215296.799937] EDAC MC0: 22523 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215297.053277] mce: [Hardware Error]: Machine check events logged
[215297.053306] EDAC MC0: 123 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215297.071466] mce: [Hardware Error]: Machine check events logged
[215297.071493] EDAC MC0: 253 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215297.091903] mce: [Hardware Error]: Machine check events logged
[215297.091933] EDAC MC0: 355 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215297.110784] mce: [Hardware Error]: Machine check events logged
[215297.110807] RAS: Soft-offlining pfn: 0x80fa98
[215297.110820] EDAC MC0: 154 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215297.111051] Memory failure: 0x80fa98: unhandlable page.
[215297.129682] mce: [Hardware Error]: Machine check events logged
[215297.129708] EDAC MC0: 32686 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215297.157044] mce: [Hardware Error]: Machine check events logged
[215297.157080] EDAC MC0: 322 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215297.173712] mce: [Hardware Error]: Machine check events logged
[215297.193548] mce: [Hardware Error]: Machine check events logged
[215297.193585] EDAC MC0: 1183 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215297.208506] mce: [Hardware Error]: Machine check events logged
[215297.209538] EDAC MC0: 1752 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215297.226887] mce: [Hardware Error]: Machine check events logged
[215297.226915] EDAC MC0: 31756 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215297.250582] mce: [Hardware Error]: Machine check events logged
[215297.250614] EDAC MC0: 467 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215297.273997] mce: [Hardware Error]: Machine check events logged
[215297.303807] mce: [Hardware Error]: Machine check events logged
[215297.328891] mce: [Hardware Error]: Machine check events logged
[215297.328916] EDAC MC0: 1497 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215297.352728] mce: [Hardware Error]: Machine check events logged
[215297.352750] RAS: Soft-offlining pfn: 0x166dca
[215297.352762] EDAC MC0: 555 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215297.353175] Memory failure: 0x166dca: unhandlable page.
[215297.381952] mce: [Hardware Error]: Machine check events logged
[215297.610654] mce: [Hardware Error]: Machine check events logged
[215297.610694] EDAC MC0: 23532 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215298.142509] mce: [Hardware Error]: Machine check events logged
[215298.142525] RAS: Soft-offlining pfn: 0x80fd98
[215298.142533] EDAC MC0: 72 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215298.142777] Memory failure: 0x80fd98: unhandlable page.
[215298.634615] mce: [Hardware Error]: Machine check events logged
[215298.778494] mce: [Hardware Error]: Machine check events logged
[215298.778516] RAS: Soft-offlining pfn: 0x80fb9c
[215298.778530] EDAC MC0: 29548 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215298.778758] Memory failure: 0x80fb9c: unhandlable page.
[215298.795638] mce: [Hardware Error]: Machine check events logged
[215298.795664] EDAC MC0: 73 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215299.304842] mce: [Hardware Error]: Machine check events logged
[215299.594585] mce: [Hardware Error]: Machine check events logged
[215299.594639] EDAC MC0: 14828 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215299.779939] mce: [Hardware Error]: Machine check events logged
[215299.779962] EDAC MC0: 155 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215300.022976] mce: [Hardware Error]: Machine check events logged
[215300.023003] EDAC MC0: 298 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215300.320314] mce: [Hardware Error]: Machine check events logged
[215300.320338] RAS: Soft-offlining pfn: 0x166dca
[215300.320351] EDAC MC0: 413 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215300.320575] Memory failure: 0x166dca: unhandlable page.
[215300.618558] mce: [Hardware Error]: Machine check events logged
[215300.618606] EDAC MC0: 30897 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215300.684266] i2c i2c-0: sendbytes: NAK bailout.
[215300.684792] i2c i2c-0: sendbytes: NAK bailout.
[215300.746618] EDID block 0 (tag 0x00) checksum is invalid, remainder is 18
[215300.757257] mce: [Hardware Error]: Machine check events logged
[215300.757546] RAS: Soft-offlining pfn: 0x165b98
[215300.757556] EDAC MC0: 143 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215300.758548] Memory failure: 0x165b98: unhandlable page.
[215300.788403] mce: [Hardware Error]: Machine check events logged
[215300.788550] EDAC MC0: 1284 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215300.795781] mce: [Hardware Error]: Machine check events logged
[215300.803572] mce: [Hardware Error]: Machine check events logged
[215300.815853] mce: [Hardware Error]: Machine check events logged
[215300.815877] RAS: Soft-offlining pfn: 0x80fa18
[215300.815888] EDAC MC0: 32266 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215300.816051] Memory failure: 0x80fa18: unhandlable page.
[215300.850343] mce: [Hardware Error]: Machine check events logged
[215301.284659] mce: [Hardware Error]: Machine check events logged
[215301.284693] EDAC MC0: 93 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215301.578520] mce: [Hardware Error]: Machine check events logged
[215302.317846] mce: [Hardware Error]: Machine check events logged
[215302.317872] RAS: Soft-offlining pfn: 0x166dca
[215302.317886] EDAC MC0: 19087 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215302.318071] Memory failure: 0x166dca: unhandlable page.
[215302.602501] mce: [Hardware Error]: Machine check events logged
[215302.602527] EDAC MC0: 23578 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215302.761014] mce: [Hardware Error]: Machine check events logged
[215302.904194] mce: [Hardware Error]: Machine check events logged
[215302.904231] EDAC MC0: 521 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215303.183884] mce: [Hardware Error]: Machine check events logged
[215303.198886] mce: [Hardware Error]: Machine check events logged
[215303.198912] EDAC MC0: 658 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215303.208423] mce: [Hardware Error]: Machine check events logged
[215303.216933] mce: [Hardware Error]: Machine check events logged
[215303.220075] mce: [Hardware Error]: Machine check events logged
[215303.223970] mce: [Hardware Error]: Machine check events logged
[215303.223991] RAS: Soft-offlining pfn: 0x80fd18
[215303.224002] EDAC MC0: 2164 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215303.225462] Memory failure: 0x80fd18: unhandlable page.
[215303.226748] mce: [Hardware Error]: Machine check events logged
[215303.226764] EDAC MC0: 32700 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215303.234098] mce: [Hardware Error]: Machine check events logged
[215303.234123] RAS: Soft-offlining pfn: 0x80fbb2
[215303.234132] EDAC MC0: 926 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215303.234468] Memory failure: 0x80fbb2: unhandlable page.
[215303.242551] mce: [Hardware Error]: Machine check events logged
[215303.242571] EDAC MC0: 10 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215303.247827] mce: [Hardware Error]: Machine check events logged
[215303.247844] RAS: Soft-offlining pfn: 0x80fc98
[215303.247853] EDAC MC0: 347 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215303.248481] Memory failure: 0x80fc98: unhandlable page.
[215303.255897] mce: [Hardware Error]: Machine check events logged
[215303.255916] RAS: Soft-offlining pfn: 0x166dca
[215303.255925] EDAC MC0: 673 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215303.256474] Memory failure: 0x166dca: unhandlable page.
[215303.259176] mce: [Hardware Error]: Machine check events logged
[215303.259189] RAS: Soft-offlining pfn: 0x80fdb0
[215303.259196] EDAC MC0: 42 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215303.259234] Memory failure: 0x80fdb0: unhandlable page.
[215303.275699] mce: [Hardware Error]: Machine check events logged
[215303.275729] EDAC MC0: 647 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215303.476475] mce: [Hardware Error]: Machine check events logged
[215303.476504] EDAC MC0: 182 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215303.489302] mce: [Hardware Error]: Machine check events logged
[215303.489332] EDAC MC0: 163 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215303.503011] mce: [Hardware Error]: Machine check events logged
[215303.515803] mce: [Hardware Error]: Machine check events logged
[215303.532460] mce: [Hardware Error]: Machine check events logged
[215303.532503] EDAC MC0: 1216 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215303.544243] mce: [Hardware Error]: Machine check events logged
[215303.544262] EDAC MC0: 228 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215303.556452] mce: [Hardware Error]: Machine check events logged
[215303.584901] mce: [Hardware Error]: Machine check events logged
[215303.626425] mce: [Hardware Error]: Machine check events logged
[215303.626449] RAS: Soft-offlining pfn: 0x166dca
[215303.626464] EDAC MC0: 13120 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215303.626980] Memory failure: 0x166dca: unhandlable page.
[215303.770231] mce: [Hardware Error]: Machine check events logged
[215303.770258] EDAC MC0: 534 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215303.788864] mce: [Hardware Error]: Machine check events logged
[215303.790541] EDAC MC0: 5040 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215304.064723] mce: [Hardware Error]: Machine check events logged
[215304.285087] mce: [Hardware Error]: Machine check events logged
[215304.586391] mce: [Hardware Error]: Machine check events logged
[215304.586431] EDAC MC0: 6462 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215304.776769] mce: [Hardware Error]: Machine check events logged
[215304.793253] mce: [Hardware Error]: Machine check events logged
[215305.006968] mce: [Hardware Error]: Machine check events logged
[215305.006992] RAS: Soft-offlining pfn: 0x166dca
[215305.007009] EDAC MC0: 1077 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215305.007205] Memory failure: 0x166dca: unhandlable page.
[215305.087732] mce: [Hardware Error]: Machine check events logged
[215305.463722] mce: [Hardware Error]: Machine check events logged
[215305.463754] EDAC MC0: 32735 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215305.610367] mce: [Hardware Error]: Machine check events logged
[215305.610400] EDAC MC0: 5617 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215305.846888] mce: [Hardware Error]: Machine check events logged
[215305.846922] EDAC MC0: 588 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215306.179795] mce: [Hardware Error]: Machine check events logged
[215306.179818] RAS: Soft-offlining pfn: 0x166dca
[215306.179832] EDAC MC0: 73 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215306.180029] Memory failure: 0x166dca: unhandlable page.
[215306.356607] mce: [Hardware Error]: Machine check events logged
[215306.356636] EDAC MC0: 62 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215306.528526] mce: [Hardware Error]: Machine check events logged
[215306.634317] mce: [Hardware Error]: Machine check events logged
[215306.634355] EDAC MC0: 11527 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215306.777576] mce: [Hardware Error]: Machine check events logged
[215306.777599] EDAC MC0: 290 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215306.793265] mce: [Hardware Error]: Machine check events logged
[215306.793290] EDAC MC0: 261 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215307.231584] mce: [Hardware Error]: Machine check events logged
[215307.412290] mce: [Hardware Error]: Machine check events logged
[215307.412317] RAS: Soft-offlining pfn: 0x166dca
[215307.412330] EDAC MC0: 842 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215307.417297] Memory failure: 0x166dca: unhandlable page.
[215307.421908] mce: [Hardware Error]: Machine check events logged
[215307.439930] mce: [Hardware Error]: Machine check events logged
[215307.455375] mce: [Hardware Error]: Machine check events logged
[215307.455399] RAS: Soft-offlining pfn: 0x80fc22
[215307.455412] EDAC MC0: 1173 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215307.458546] Memory failure: 0x80fc22: unhandlable page.
[215307.465747] mce: [Hardware Error]: Machine check events logged
[215307.465778] EDAC MC0: 132 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215307.486038] mce: [Hardware Error]: Machine check events logged
[215307.486074] EDAC MC0: 464 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215307.510692] mce: [Hardware Error]: Machine check events logged
[215307.510727] EDAC MC0: 453 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215307.525658] mce: [Hardware Error]: Machine check events logged
[215307.525696] EDAC MC0: 646 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215307.535467] mce: [Hardware Error]: Machine check events logged
[215307.547219] mce: [Hardware Error]: Machine check events logged
[215307.547248] EDAC MC0: 16135 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215307.583487] mce: [Hardware Error]: Machine check events logged
[215307.583503] RAS: Soft-offlining pfn: 0x80fd22
[215307.583511] EDAC MC0: 139 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215307.587302] Memory failure: 0x80fd22: unhandlable page.
[215307.594280] mce: [Hardware Error]: Machine check events logged
[215307.594310] EDAC MC0: 26367 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215307.631209] mce: [Hardware Error]: Machine check events logged
[215307.631231] EDAC MC0: 514 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215307.634665] mce: [Hardware Error]: Machine check events logged
[215307.634691] EDAC MC0: 290 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215307.649740] mce: [Hardware Error]: Machine check events logged
[215307.649768] RAS: Soft-offlining pfn: 0x80fc34
[215307.649784] EDAC MC0: 634 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215307.650760] Memory failure: 0x80fc34: unhandlable page.
[215307.668758] mce: [Hardware Error]: Machine check events logged
[215307.669081] RAS: Soft-offlining pfn: 0x166dca
[215307.669094] EDAC MC0: 1811 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215307.672571] Memory failure: 0x166dca: unhandlable page.
[215307.687876] mce: [Hardware Error]: Machine check events logged
[215307.687905] EDAC MC0: 31704 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215307.702178] mce: [Hardware Error]: Machine check events logged
[215307.702276] RAS: Soft-offlining pfn: 0x80fb1c
[215307.702289] EDAC MC0: 1385 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215307.703148] Memory failure: 0x80fb1c: unhandlable page.
[215307.729889] mce: [Hardware Error]: Machine check events logged
[215307.729913] EDAC MC0: 32016 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215307.769168] mce: [Hardware Error]: Machine check events logged
[215307.791122] mce: [Hardware Error]: Machine check events logged
[215307.791363] EDAC MC0: 2400 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215307.928695] mce: [Hardware Error]: Machine check events logged
[215307.928722] EDAC MC0: 30772 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215308.547347] mce: [Hardware Error]: Machine check events logged
[215308.547376] EDAC MC0: 117 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215308.618237] mce: [Hardware Error]: Machine check events logged
[215308.618266] RAS: Soft-offlining pfn: 0x80fab2
[215308.618278] EDAC MC0: 3786 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215308.618462] Memory failure: 0x80fab2: unhandlable page.
[215308.775301] mce: [Hardware Error]: Machine check events logged
[215308.777243] EDAC MC0: 5778 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215308.849446] mce: [Hardware Error]: Machine check events logged
[215309.450225] mce: [Hardware Error]: Machine check events logged
[215309.450247] RAS: Soft-offlining pfn: 0x166dca
[215309.450262] EDAC MC0: 27540 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215309.450436] Memory failure: 0x166dca: unhandlable page.
[215309.578204] mce: [Hardware Error]: Machine check events logged
[215309.578239] EDAC MC0: 5407 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215310.080985] mce: [Hardware Error]: Machine check events logged
[215310.409181] mce: [Hardware Error]: Machine check events logged
[215310.409212] EDAC MC0: 667 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215310.602165] mce: [Hardware Error]: Machine check events logged
[215310.786440] mce: [Hardware Error]: Machine check events logged
[215310.803784] mce: [Hardware Error]: Machine check events logged
[215310.804061] RAS: Soft-offlining pfn: 0x80fb84
[215310.804075] EDAC MC0: 29776 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215310.804181] Memory failure: 0x80fb84: unhandlable page.
[215310.849788] mce: [Hardware Error]: Machine check events logged
[215310.849816] EDAC MC0: 29551 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215310.860728] i2c i2c-0: sendbytes: NAK bailout.
[215310.861159] mce: [Hardware Error]: Machine check events logged
[215310.871161] EDAC MC0: 31085 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215310.873157] mce: [Hardware Error]: Machine check events logged
[215310.874154] EDAC MC0: 2782 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215310.902079] mce: [Hardware Error]: Machine check events logged
[215310.902151] RAS: Soft-offlining pfn: 0x80fc18
[215310.902160] EDAC MC0: 88 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215310.903157] Memory failure: 0x80fc18: unhandlable page.
[215310.928500] mce: [Hardware Error]: Machine check events logged
[215310.929152] EDAC MC0: 32428 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215310.955788] mce: [Hardware Error]: Machine check events logged
[215310.956151] EDAC MC0: 18 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215310.987862] EDID has corrupt header
[215310.993481] mce: [Hardware Error]: Machine check events logged
[215311.023644] mce: [Hardware Error]: Machine check events logged
[215311.024161] EDAC MC0: 148 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215311.044310] mce: [Hardware Error]: Machine check events logged
[215311.044342] EDAC MC0: 32428 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215311.085115] mce: [Hardware Error]: Machine check events logged
[215311.119367] mce: [Hardware Error]: Machine check events logged
[215311.151285] mce: [Hardware Error]: Machine check events logged
[215311.179509] mce: [Hardware Error]: Machine check events logged
[215311.204754] mce: [Hardware Error]: Machine check events logged
[215311.204785] EDAC MC0: 577 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215311.237943] mce: [Hardware Error]: Machine check events logged
[215311.237971] EDAC MC0: 32745 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215311.275053] mce: [Hardware Error]: Machine check events logged
[215311.275080] EDAC MC0: 16 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215311.313989] mce: [Hardware Error]: Machine check events logged
[215311.342254] mce: [Hardware Error]: Machine check events logged
[215311.342322] EDAC MC0: 417 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215311.378087] mce: [Hardware Error]: Machine check events logged
[215311.378117] EDAC MC0: 32626 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215311.408613] mce: [Hardware Error]: Machine check events logged
[215311.408639] EDAC MC0: 347 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215311.439135] mce: [Hardware Error]: Machine check events logged
[215311.439162] EDAC MC0: 72 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215311.475739] mce: [Hardware Error]: Machine check events logged
[215311.475761] RAS: Soft-offlining pfn: 0x165b98
[215311.475772] EDAC MC0: 424 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215311.475969] Memory failure: 0x165b98: unhandlable page.
[215311.512240] mce: [Hardware Error]: Machine check events logged
[215311.512259] EDAC MC0: 32618 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215311.548367] mce: [Hardware Error]: Machine check events logged
[215311.584533] mce: [Hardware Error]: Machine check events logged
[215311.613287] mce: [Hardware Error]: Machine check events logged
[215311.613315] EDAC MC0: 247 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215311.626125] mce: [Hardware Error]: Machine check events logged
[215311.626153] EDAC MC0: 15705 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215311.661609] mce: [Hardware Error]: Machine check events logged
[215311.661632] EDAC MC0: 145 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215311.691359] mce: [Hardware Error]: Machine check events logged
[215311.691386] EDAC MC0: 74 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215311.715273] mce: [Hardware Error]: Machine check events logged
[215311.715302] EDAC MC0: 39 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215311.743764] mce: [Hardware Error]: Machine check events logged
[215311.743790] EDAC MC0: 5 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215311.771257] mce: [Hardware Error]: Machine check events logged
[215311.771280] EDAC MC0: 247 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215311.785701] mce: [Hardware Error]: Machine check events logged
[215311.785728] EDAC MC0: 111 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215311.796200] mce: [Hardware Error]: Machine check events logged
[215311.796229] RAS: Soft-offlining pfn: 0x80fb1c
[215311.796243] EDAC MC0: 375 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215311.796495] Memory failure: 0x80fb1c: unhandlable page.
[215311.821306] mce: [Hardware Error]: Machine check events logged
[215311.854612] mce: [Hardware Error]: Machine check events logged
[215311.854633] RAS: Soft-offlining pfn: 0x166dca
[215311.854644] EDAC MC0: 80 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215311.854679] Memory failure: 0x166dca: unhandlable page.
[215311.879626] mce: [Hardware Error]: Machine check events logged
[215311.879655] EDAC MC0: 39 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215311.914242] mce: [Hardware Error]: Machine check events logged
[215311.914272] EDAC MC0: 924 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215311.961962] mce: [Hardware Error]: Machine check events logged
[215312.346599] mce: [Hardware Error]: Machine check events logged
[215312.346688] EDAC MC0: 32655 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215312.586087] mce: [Hardware Error]: Machine check events logged
[215312.586123] RAS: Soft-offlining pfn: 0x165b98
[215312.586135] EDAC MC0: 10756 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215312.586179] Memory failure: 0x165b98: unhandlable page.
[215312.779992] mce: [Hardware Error]: Machine check events logged
[215312.788260] mce: [Hardware Error]: Machine check events logged
[215312.788275] RAS: Soft-offlining pfn: 0x80fa98
[215312.788287] EDAC MC0: 526 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215312.788599] Memory failure: 0x80fa98: unhandlable page.
[215312.863927] mce: [Hardware Error]: Machine check events logged
[215312.863960] EDAC MC0: 109 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215313.570126] mce: [Hardware Error]: Machine check events logged
[215313.570146] RAS: Soft-offlining pfn: 0x165b98
[215313.570157] EDAC MC0: 381 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215313.571065] Memory failure: 0x165b98: unhandlable page.
[215313.581504] mce: [Hardware Error]: Machine check events logged
[215313.598115] mce: [Hardware Error]: Machine check events logged
[215313.598152] EDAC MC0: 418 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215313.610057] mce: [Hardware Error]: Machine check events logged
[215313.627496] mce: [Hardware Error]: Machine check events logged
[215313.638720] mce: [Hardware Error]: Machine check events logged
[215313.638754] EDAC MC0: 28904 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215313.651577] mce: [Hardware Error]: Machine check events logged
[215313.651606] EDAC MC0: 183 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215313.695799] mce: [Hardware Error]: Machine check events logged
[215313.695832] EDAC MC0: 273 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215314.102350] mce: [Hardware Error]: Machine check events logged
[215314.102380] EDAC MC0: 29 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215314.634014] mce: [Hardware Error]: Machine check events logged
[215314.774921] mce: [Hardware Error]: Machine check events logged
[215314.776603] EDAC MC0: 1720 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215314.967755] mce: [Hardware Error]: Machine check events logged
[215314.967794] EDAC MC0: 27287 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215315.441198] mce: [Hardware Error]: Machine check events logged
[215315.441224] RAS: Soft-offlining pfn: 0x80fb18
[215315.441236] EDAC MC0: 166 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215315.441745] Memory failure: 0x80fb18: unhandlable page.
[215315.593977] mce: [Hardware Error]: Machine check events logged
[215315.768986] mce: [Hardware Error]: Machine check events logged
[215315.769019] EDAC MC0: 10305 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215315.881849] mce: [Hardware Error]: Machine check events logged
[215315.995681] mce: [Hardware Error]: Machine check events logged
[215316.324560] mce: [Hardware Error]: Machine check events logged
[215316.324580] RAS: Soft-offlining pfn: 0x165b98
[215316.324593] EDAC MC0: 961 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215316.327178] Memory failure: 0x165b98: unhandlable page.
[215316.416742] mce: [Hardware Error]: Machine check events logged
[215316.416778] EDAC MC0: 216 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215316.617157] mce: [Hardware Error]: Machine check events logged
[215316.617178] EDAC MC0: 82 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215316.617941] mce: [Hardware Error]: Machine check events logged
[215316.617974] EDAC MC0: 1497 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215316.785293] mce: [Hardware Error]: Machine check events logged
[215316.785781] RAS: Soft-offlining pfn: 0x80fc04
[215316.785794] EDAC MC0: 3822 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215316.785835] Memory failure: 0x80fc04: unhandlable page.
[215316.859602] mce: [Hardware Error]: Machine check events logged
[215316.859636] EDAC MC0: 29396 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215317.059273] mce: [Hardware Error]: Machine check events logged
[215317.059288] RAS: Soft-offlining pfn: 0x2260c6
[215317.059298] EDAC MC0: 311 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215317.577907] mce: [Hardware Error]: Machine check events logged
[215317.577945] EDAC MC0: 28857 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215317.757514] mce: [Hardware Error]: Machine check events logged
[215317.757536] RAS: Soft-offlining pfn: 0x80fb98
[215317.757548] EDAC MC0: 87 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215317.757881] Memory failure: 0x80fb98: unhandlable page.
[215317.769870] mce: [Hardware Error]: Machine check events logged
[215317.786446] mce: [Hardware Error]: Machine check events logged
[215317.786468] RAS: Soft-offlining pfn: 0x32000
[215317.786480] EDAC MC0: 238 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215317.786661] Memory failure: 0x32000: unhandlable page.
[215317.818089] mce: [Hardware Error]: Machine check events logged
[215317.818121] EDAC MC0: 230 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215317.835499] mce: [Hardware Error]: Machine check events logged
[215317.835527] EDAC MC0: 222 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215317.863366] mce: [Hardware Error]: Machine check events logged
[215317.863391] EDAC MC0: 281 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215317.880052] mce: [Hardware Error]: Machine check events logged
[215317.897888] mce: [Hardware Error]: Machine check events logged
[215317.897914] EDAC MC0: 585 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215317.953851] mce: [Hardware Error]: Machine check events logged
[215317.953885] EDAC MC0: 536 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215317.979475] mce: [Hardware Error]: Machine check events logged
[215317.979508] EDAC MC0: 294 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215317.996335] mce: [Hardware Error]: Machine check events logged
[215318.013759] mce: [Hardware Error]: Machine check events logged
[215318.013789] EDAC MC0: 702 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215318.032087] mce: [Hardware Error]: Machine check events logged
[215318.032113] EDAC MC0: 670 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215318.048051] mce: [Hardware Error]: Machine check events logged
[215318.048103] RAS: Soft-offlining pfn: 0x165c88
[215318.048115] EDAC MC0: 1079 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215318.050041] Memory failure: 0x165c88: unhandlable page.
[215318.092561] mce: [Hardware Error]: Machine check events logged
[215318.092583] RAS: Soft-offlining pfn: 0x166dca
[215318.092595] EDAC MC0: 32247 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215318.092900] Memory failure: 0x166dca: unhandlable page.
[215318.107087] mce: [Hardware Error]: Machine check events logged
[215318.124717] mce: [Hardware Error]: Machine check events logged
[215318.137292] mce: [Hardware Error]: Machine check events logged
[215318.137320] EDAC MC0: 1376 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215318.149734] mce: [Hardware Error]: Machine check events logged
[215318.149766] EDAC MC0: 83 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215318.181879] mce: [Hardware Error]: Machine check events logged
[215318.601873] mce: [Hardware Error]: Machine check events logged
[215318.601907] EDAC MC0: 30464 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215318.782233] mce: [Hardware Error]: Machine check events logged
[215318.782262] EDAC MC0: 171 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215318.800072] mce: [Hardware Error]: Machine check events logged
[215318.800096] EDAC MC0: 139 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215318.823824] mce: [Hardware Error]: Machine check events logged
[215318.823853] EDAC MC0: 249 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215318.833404] mce: [Hardware Error]: Machine check events logged
[215318.837888] mce: [Hardware Error]: Machine check events logged
[215318.837913] EDAC MC0: 494 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215318.949860] mce: [Hardware Error]: Machine check events logged
[215318.949886] EDAC MC0: 32622 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215319.077146] mce: [Hardware Error]: Machine check events logged
[215319.077166] RAS: Soft-offlining pfn: 0x80fb22
[215319.077179] EDAC MC0: 485 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215319.077602] Memory failure: 0x80fb22: unhandlable page.
[215319.561844] mce: [Hardware Error]: Machine check events logged
[215319.561867] RAS: Soft-offlining pfn: 0x80fd98
[215319.561879] EDAC MC0: 98 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215319.562104] Memory failure: 0x80fd98: unhandlable page.
[215319.625846] mce: [Hardware Error]: Machine check events logged
[215319.625879] EDAC MC0: 2460 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215319.893080] mce: [Hardware Error]: Machine check events logged
[215320.383572] mce: [Hardware Error]: Machine check events logged
[215320.383591] RAS: Soft-offlining pfn: 0x80fb18
[215320.383601] EDAC MC0: 418 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215320.383796] Memory failure: 0x80fb18: unhandlable page.
[215320.585801] mce: [Hardware Error]: Machine check events logged
[215320.585986] EDAC MC0: 12762 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215320.786158] mce: [Hardware Error]: Machine check events logged
[215320.786177] RAS: Soft-offlining pfn: 0x165b9e
[215320.786190] EDAC MC0: 32472 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215320.786246] Memory failure: 0x165b9e: unhandlable page.
[215320.809715] mce: [Hardware Error]: Machine check events logged
[215320.809749] EDAC MC0: 379 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215320.895395] mce: [Hardware Error]: Machine check events logged
[215320.895421] EDAC MC0: 244 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215320.910748] mce: [Hardware Error]: Machine check events logged
[215320.961426] mce: [Hardware Error]: Machine check events logged
[215321.128771] mce: [Hardware Error]: Machine check events logged
[215321.128803] EDAC MC0: 638 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215321.162853] i2c i2c-0: sendbytes: NAK bailout.
[215321.224357] EDID block 0 (tag 0x00) checksum is invalid, remainder is 122
[215321.277060] mce: [Hardware Error]: Machine check events logged
[215321.609766] mce: [Hardware Error]: Machine check events logged
[215321.609803] EDAC MC0: 18315 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215322.288249] mce: [Hardware Error]: Machine check events logged
[215322.288271] EDAC MC0: 292 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215322.633719] mce: [Hardware Error]: Machine check events logged
[215322.633896] RAS: Soft-offlining pfn: 0x166dca
[215322.633906] EDAC MC0: 12402 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215322.634081] Memory failure: 0x166dca: unhandlable page.
[215322.771187] mce: [Hardware Error]: Machine check events logged
[215322.771216] EDAC MC0: 32330 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215322.785081] mce: [Hardware Error]: Machine check events logged
[215322.785113] EDAC MC0: 181 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215323.127103] mce: [Hardware Error]: Machine check events logged
[215323.127125] RAS: Soft-offlining pfn: 0x80fd34
[215323.127138] EDAC MC0: 21 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215323.127330] Memory failure: 0x80fd34: unhandlable page.
[215323.593682] mce: [Hardware Error]: Machine check events logged
[215323.674964] mce: [Hardware Error]: Machine check events logged
[215323.674991] EDAC MC0: 18756 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215323.684032] mce: [Hardware Error]: Machine check events logged
[215323.699640] mce: [Hardware Error]: Machine check events logged
[215323.713917] mce: [Hardware Error]: Machine check events logged
[215323.713945] EDAC MC0: 1018 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215323.726455] mce: [Hardware Error]: Machine check events logged
[215323.726473] RAS: Soft-offlining pfn: 0x80fb98
[215323.726483] EDAC MC0: 361 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215323.726687] Memory failure: 0x80fb98: unhandlable page.
[215323.743191] mce: [Hardware Error]: Machine check events logged
[215323.743221] EDAC MC0: 163 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215323.753842] mce: [Hardware Error]: Machine check events logged
[215323.753877] EDAC MC0: 415 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215323.780443] mce: [Hardware Error]: Machine check events logged
[215323.816856] mce: [Hardware Error]: Machine check events logged
[215323.816884] RAS: Soft-offlining pfn: 0x80fb9c
[215323.816901] EDAC MC0: 321 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215323.817240] Memory failure: 0x80fb9c: unhandlable page.
[215324.159016] mce: [Hardware Error]: Machine check events logged
[215324.159063] RAS: Soft-offlining pfn: 0x80fa98
[215324.159082] EDAC MC0: 179 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215324.159269] Memory failure: 0x80fa98: unhandlable page.
[215324.617647] mce: [Hardware Error]: Machine check events logged
[215324.617684] EDAC MC0: 24046 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215324.777183] mce: [Hardware Error]: Machine check events logged
[215324.777207] EDAC MC0: 340 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215324.912091] mce: [Hardware Error]: Machine check events logged
[215324.912129] EDAC MC0: 352 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215325.519618] mce: [Hardware Error]: Machine check events logged
[215325.519648] EDAC MC0: 95 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215325.577617] mce: [Hardware Error]: Machine check events logged
[215325.964016] mce: [Hardware Error]: Machine check events logged
[215326.117493] mce: [Hardware Error]: Machine check events logged
[215326.117530] EDAC MC0: 2659 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215326.601589] mce: [Hardware Error]: Machine check events logged
[215326.601619] RAS: Soft-offlining pfn: 0x165b98
[215326.601635] EDAC MC0: 26243 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215326.601926] Memory failure: 0x165b98: unhandlable page.
[215326.775635] mce: [Hardware Error]: Machine check events logged
[215326.792925] mce: [Hardware Error]: Machine check events logged
[215327.177141] mce: [Hardware Error]: Machine check events logged
[215327.207237] mce: [Hardware Error]: Machine check events logged
[215327.207261] RAS: Soft-offlining pfn: 0x166dca
[215327.207277] EDAC MC0: 1064 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215327.207454] Memory failure: 0x166dca: unhandlable page.
[215327.221526] mce: [Hardware Error]: Machine check events logged
[215327.238869] mce: [Hardware Error]: Machine check events logged
[215327.238888] RAS: Soft-offlining pfn: 0x166dca
[215327.238901] EDAC MC0: 1166 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215327.239554] Memory failure: 0x166dca: unhandlable page.
[215327.250905] mce: [Hardware Error]: Machine check events logged
[215327.250928] RAS: Soft-offlining pfn: 0x80fd34
[215327.250943] EDAC MC0: 199 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215327.251058] Memory failure: 0x80fd34: unhandlable page.
[215327.276431] mce: [Hardware Error]: Machine check events logged
[215327.276467] EDAC MC0: 391 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215327.290400] mce: [Hardware Error]: Machine check events logged
[215327.290431] RAS: Soft-offlining pfn: 0x80fa1c
[215327.290450] EDAC MC0: 382 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215327.290629] Memory failure: 0x80fa1c: unhandlable page.
[215327.328121] mce: [Hardware Error]: Machine check events logged
[215327.347043] mce: [Hardware Error]: Machine check events logged
[215327.347069] EDAC MC0: 436 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215327.386482] mce: [Hardware Error]: Machine check events logged
[215327.430118] mce: [Hardware Error]: Machine check events logged
[215327.453657] mce: [Hardware Error]: Machine check events logged
[215327.453696] EDAC MC0: 1030 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215327.477894] mce: [Hardware Error]: Machine check events logged
[215327.477924] RAS: Soft-offlining pfn: 0x80fca2
[215327.477942] EDAC MC0: 863 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215327.478554] Memory failure: 0x80fca2: unhandlable page.
[215327.512730] mce: [Hardware Error]: Machine check events logged
[215327.512748] RAS: Soft-offlining pfn: 0x80fc9e
[215327.512758] EDAC MC0: 1 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215327.512928] Memory failure: 0x80fc9e: unhandlable page.
[215327.530161] mce: [Hardware Error]: Machine check events logged
[215327.533732] EDAC MC0: 4127 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215327.550097] mce: [Hardware Error]: Machine check events logged
[215327.550128] EDAC MC0: 29584 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215327.625547] mce: [Hardware Error]: Machine check events logged
[215327.625583] RAS: Soft-offlining pfn: 0x166dca
[215327.625593] EDAC MC0: 22189 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215327.625842] Memory failure: 0x166dca: unhandlable page.
[215327.678890] mce: [Hardware Error]: Machine check events logged
[215327.753760] mce: [Hardware Error]: Machine check events logged
[215327.766679] mce: [Hardware Error]: Machine check events logged
[215327.787337] mce: [Hardware Error]: Machine check events logged
[215327.787383] RAS: Soft-offlining pfn: 0x166dca
[215327.787405] EDAC MC0: 1555 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215327.787572] Memory failure: 0x166dca: unhandlable page.
[215328.047650] mce: [Hardware Error]: Machine check events logged
[215328.047680] EDAC MC0: 32613 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215328.585495] mce: [Hardware Error]: Machine check events logged
[215328.585638] RAS: Soft-offlining pfn: 0x165b98
[215328.585648] EDAC MC0: 26792 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215328.585678] Memory failure: 0x165b98: unhandlable page.
[215328.785326] mce: [Hardware Error]: Machine check events logged
[215328.839216] mce: [Hardware Error]: Machine check events logged
[215329.609454] mce: [Hardware Error]: Machine check events logged
[215330.083078] mce: [Hardware Error]: Machine check events logged
[215330.083102] EDAC MC0: 344 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215330.132678] mce: [Hardware Error]: Machine check events logged
[215330.132699] EDAC MC0: 200 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215330.633415] mce: [Hardware Error]: Machine check events logged
[215330.633454] EDAC MC0: 31800 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215330.768727] mce: [Hardware Error]: Machine check events logged
[215330.768754] EDAC MC0: 390 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215330.785197] mce: [Hardware Error]: Machine check events logged
[215330.785343] EDAC MC0: 1336 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215330.948265] mce: [Hardware Error]: Machine check events logged
[215330.948289] RAS: Soft-offlining pfn: 0x165b9e
[215330.948299] EDAC MC0: 31904 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215330.950053] Memory failure: 0x165b9e: unhandlable page.
[215330.955299] mce: [Hardware Error]: Machine check events logged
[215330.955327] EDAC MC0: 142 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215330.968781] mce: [Hardware Error]: Machine check events logged
[215330.968799] RAS: Soft-offlining pfn: 0x166dca
[215330.968809] EDAC MC0: 288 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215330.969028] Memory failure: 0x166dca: unhandlable page.
[215331.084137] mce: [Hardware Error]: Machine check events logged
[215331.344150] mce: [Hardware Error]: Machine check events logged
[215331.344172] EDAC MC0: 275 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215331.433158] i2c i2c-0: sendbytes: NAK bailout.
[215331.463933] EDID block 0 (tag 0x00) checksum is invalid, remainder is 125
[215331.496848] mce: [Hardware Error]: Machine check events logged
[215331.496876] EDAC MC0: 40 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215331.593395] mce: [Hardware Error]: Machine check events logged
[215331.778011] mce: [Hardware Error]: Machine check events logged
[215331.778034] EDAC MC0: 16433 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215331.876056] mce: [Hardware Error]: Machine check events logged
[215332.274732] mce: [Hardware Error]: Machine check events logged
[215332.274750] RAS: Soft-offlining pfn: 0x165b98
[215332.274762] EDAC MC0: 626 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215332.274972] Memory failure: 0x165b98: unhandlable page.
[215332.617346] mce: [Hardware Error]: Machine check events logged
[215332.617380] RAS: Soft-offlining pfn: 0x166dca
[215332.617395] EDAC MC0: 15640 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215332.617645] Memory failure: 0x166dca: unhandlable page.
[215332.778635] mce: [Hardware Error]: Machine check events logged
[215332.778660] EDAC MC0: 304 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215332.796124] mce: [Hardware Error]: Machine check events logged
[215332.796156] EDAC MC0: 211 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215333.098607] mce: [Hardware Error]: Machine check events logged
[215333.577297] mce: [Hardware Error]: Machine check events logged
[215333.577330] EDAC MC0: 14273 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215333.766179] mce: [Hardware Error]: Machine check events logged
[215333.766212] EDAC MC0: 366 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215333.779521] mce: [Hardware Error]: Machine check events logged
[215333.779543] EDAC MC0: 146 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215333.792521] mce: [Hardware Error]: Machine check events logged
[215333.794902] RAS: Soft-offlining pfn: 0x80fa9c
[215333.794915] EDAC MC0: 5828 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215333.795108] Memory failure: 0x80fa9c: unhandlable page.
[215333.807143] mce: [Hardware Error]: Machine check events logged
[215333.807157] RAS: Soft-offlining pfn: 0x166dca
[215333.807165] EDAC MC0: 27386 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215333.807353] Memory failure: 0x166dca: unhandlable page.
[215333.822047] mce: [Hardware Error]: Machine check events logged
[215333.822070] RAS: Soft-offlining pfn: 0x80fa98
[215333.822084] EDAC MC0: 398 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215333.822309] Memory failure: 0x80fa98: unhandlable page.
[215333.833350] mce: [Hardware Error]: Machine check events logged
[215333.844078] mce: [Hardware Error]: Machine check events logged
[215333.844099] EDAC MC0: 202 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215333.895069] mce: [Hardware Error]: Machine check events logged
[215333.895084] RAS: Soft-offlining pfn: 0x80fa1c
[215333.895095] EDAC MC0: 233 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215333.895511] Memory failure: 0x80fa1c: unhandlable page.
[215334.129290] mce: [Hardware Error]: Machine check events logged
[215334.129319] EDAC MC0: 55 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215334.601271] mce: [Hardware Error]: Machine check events logged
[215334.601299] RAS: Soft-offlining pfn: 0x165a08
[215334.601312] EDAC MC0: 21820 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215334.601499] Memory failure: 0x165a08: unhandlable page.
[215334.780656] mce: [Hardware Error]: Machine check events logged
[215334.824383] mce: [Hardware Error]: Machine check events logged
[215335.397734] mce: [Hardware Error]: Machine check events logged
[215335.625237] mce: [Hardware Error]: Machine check events logged
[215335.625278] EDAC MC0: 29224 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215335.784834] mce: [Hardware Error]: Machine check events logged
[215335.784852] RAS: Soft-offlining pfn: 0x166dca
[215335.784864] EDAC MC0: 373 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215335.785095] Memory failure: 0x166dca: unhandlable page.
[215335.824318] mce: [Hardware Error]: Machine check events logged
[215335.957734] mce: [Hardware Error]: Machine check events logged
[215336.078252] mce: [Hardware Error]: Machine check events logged
[215336.305736] mce: [Hardware Error]: Machine check events logged
[215336.305762] RAS: Soft-offlining pfn: 0x166dca
[215336.305778] EDAC MC0: 16754 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215336.305904] Memory failure: 0x166dca: unhandlable page.
[215336.585195] mce: [Hardware Error]: Machine check events logged
[215336.781299] mce: [Hardware Error]: Machine check events logged
[215336.781509] RAS: Soft-offlining pfn: 0x80fd18
[215336.781522] EDAC MC0: 21458 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215336.781552] Memory failure: 0x80fd18: unhandlable page.
[215336.797575] mce: [Hardware Error]: Machine check events logged
[215337.170735] mce: [Hardware Error]: Machine check events logged
[215337.170759] RAS: Soft-offlining pfn: 0x80fb9c
[215337.170775] EDAC MC0: 32434 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215337.170970] Memory failure: 0x80fb9c: unhandlable page.
[215337.609375] mce: [Hardware Error]: Machine check events logged
[215337.609407] RAS: Soft-offlining pfn: 0x165b98
[215337.609419] EDAC MC0: 27044 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215337.609445] Memory failure: 0x165b98: unhandlable page.
[215337.711880] mce: [Hardware Error]: Machine check events logged
[215337.726244] mce: [Hardware Error]: Machine check events logged
[215337.726268] RAS: Soft-offlining pfn: 0x166dca
[215337.726284] EDAC MC0: 729 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215337.726552] Memory failure: 0x166dca: unhandlable page.
[215337.749468] mce: [Hardware Error]: Machine check events logged
[215337.771173] mce: [Hardware Error]: Machine check events logged
[215337.771214] EDAC MC0: 1218 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215337.788892] mce: [Hardware Error]: Machine check events logged
[215337.788924] EDAC MC0: 231 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215337.805473] mce: [Hardware Error]: Machine check events logged
[215337.805506] EDAC MC0: 930 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215337.811371] mce: [Hardware Error]: Machine check events logged
[215337.814551] EDAC MC0: 20977 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215337.829046] mce: [Hardware Error]: Machine check events logged
[215337.829080] EDAC MC0: 27800 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215337.847097] mce: [Hardware Error]: Machine check events logged
[215337.863872] mce: [Hardware Error]: Machine check events logged
[215337.883980] mce: [Hardware Error]: Machine check events logged
[215337.884014] EDAC MC0: 1335 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215337.901202] mce: [Hardware Error]: Machine check events logged
[215337.927330] mce: [Hardware Error]: Machine check events logged
[215337.939517] mce: [Hardware Error]: Machine check events logged
[215337.939545] EDAC MC0: 539 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215337.962487] mce: [Hardware Error]: Machine check events logged
[215337.962512] EDAC MC0: 864 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215337.984339] mce: [Hardware Error]: Machine check events logged
[215337.984368] RAS: Soft-offlining pfn: 0x166dca
[215337.984383] EDAC MC0: 32662 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215337.985165] Memory failure: 0x166dca: unhandlable page.
[215338.010867] mce: [Hardware Error]: Machine check events logged
[215338.010893] EDAC MC0: 386 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215338.026538] mce: [Hardware Error]: Machine check events logged
[215338.026569] EDAC MC0: 485 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215338.265124] mce: [Hardware Error]: Machine check events logged
[215338.265170] EDAC MC0: 176 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215338.633115] mce: [Hardware Error]: Machine check events logged
[215338.780117] mce: [Hardware Error]: Machine check events logged
[215338.780142] EDAC MC0: 27312 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215338.810325] mce: [Hardware Error]: Machine check events logged
[215338.810346] RAS: Soft-offlining pfn: 0x80fc18
[215338.810360] EDAC MC0: 303 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215338.810824] Memory failure: 0x80fc18: unhandlable page.
[215339.197692] mce: [Hardware Error]: Machine check events logged
[215339.593132] mce: [Hardware Error]: Machine check events logged
[215339.593164] RAS: Soft-offlining pfn: 0x166dca
[215339.593179] EDAC MC0: 13570 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215339.593378] Memory failure: 0x166dca: unhandlable page.
[215339.784251] mce: [Hardware Error]: Machine check events logged
[215339.948950] mce: [Hardware Error]: Machine check events logged
[215339.948994] EDAC MC0: 667 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215340.500786] mce: [Hardware Error]: Machine check events logged
[215340.500820] EDAC MC0: 314 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215340.617061] mce: [Hardware Error]: Machine check events logged
[215340.617093] RAS: Soft-offlining pfn: 0x166dca
[215340.617105] EDAC MC0: 16245 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215340.617199] Memory failure: 0x166dca: unhandlable page.
[215340.782117] mce: [Hardware Error]: Machine check events logged
[215340.782147] EDAC MC0: 308 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215340.800103] mce: [Hardware Error]: Machine check events logged
[215340.800131] EDAC MC0: 523 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215340.988908] mce: [Hardware Error]: Machine check events logged
[215341.000034] mce: [Hardware Error]: Machine check events logged
[215341.014923] mce: [Hardware Error]: Machine check events logged
[215341.014942] RAS: Soft-offlining pfn: 0x166dca
[215341.014954] EDAC MC0: 942 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215341.015158] Memory failure: 0x166dca: unhandlable page.
[215341.213026] mce: [Hardware Error]: Machine check events logged
[215341.213058] EDAC MC0: 83 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215341.576998] mce: [Hardware Error]: Machine check events logged
[215341.577035] EDAC MC0: 23115 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215341.577526] i2c i2c-0: sendbytes: NAK bailout.
[215341.579120] i2c i2c-0: sendbytes: NAK bailout.
[215341.581688] i2c i2c-0: sendbytes: NAK bailout.
[215341.704638] EDID block 0 (tag 0x00) checksum is invalid, remainder is 125
[215341.707138] mce: [Hardware Error]: Machine check events logged
[215341.707169] EDAC MC0: 32709 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215341.862483] mce: [Hardware Error]: Machine check events logged
[215341.862511] EDAC MC0: 247 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215342.421152] mce: [Hardware Error]: Machine check events logged
[215342.421186] EDAC MC0: 2 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215342.600958] mce: [Hardware Error]: Machine check events logged
[215342.637895] mce: [Hardware Error]: Machine check events logged
[215342.670248] mce: [Hardware Error]: Machine check events logged
[215342.670271] EDAC MC0: 7468 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215342.700870] mce: [Hardware Error]: Machine check events logged
[215342.700894] RAS: Soft-offlining pfn: 0x80fb18
[215342.700905] EDAC MC0: 66 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215342.701023] Memory failure: 0x80fb18: unhandlable page.
[215342.737062] mce: [Hardware Error]: Machine check events logged
[215342.737085] EDAC MC0: 32733 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215342.770797] mce: [Hardware Error]: Machine check events logged
[215342.770812] RAS: Soft-offlining pfn: 0x80fa18
[215342.770820] EDAC MC0: 142 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215342.771026] Memory failure: 0x80fa18: unhandlable page.
[215342.778490] mce: [Hardware Error]: Machine check events logged
[215342.778509] EDAC MC0: 190 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215342.791997] mce: [Hardware Error]: Machine check events logged
[215342.792048] EDAC MC0: 752 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215342.822430] mce: [Hardware Error]: Machine check events logged
[215342.852757] mce: [Hardware Error]: Machine check events logged
[215342.852778] RAS: Soft-offlining pfn: 0x166dca
[215342.852791] EDAC MC0: 32530 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215342.852864] Memory failure: 0x166dca: unhandlable page.
[215342.887035] mce: [Hardware Error]: Machine check events logged
[215342.926972] mce: [Hardware Error]: Machine check events logged
[215342.926991] RAS: Soft-offlining pfn: 0x80fb9c
[215342.927002] EDAC MC0: 98 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215342.927033] Memory failure: 0x80fb9c: unhandlable page.
[215342.962321] mce: [Hardware Error]: Machine check events logged
[215342.962341] RAS: Soft-offlining pfn: 0x80fd34
[215342.962351] EDAC MC0: 32738 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215342.962385] Memory failure: 0x80fd34: unhandlable page.
[215342.992406] mce: [Hardware Error]: Machine check events logged
[215342.992429] EDAC MC0: 278 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215343.030049] mce: [Hardware Error]: Machine check events logged
[215343.030071] RAS: Soft-offlining pfn: 0x80fab4
[215343.030083] EDAC MC0: 32735 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215343.030120] Memory failure: 0x80fab4: unhandlable page.
[215343.060881] mce: [Hardware Error]: Machine check events logged
[215343.092646] mce: [Hardware Error]: Machine check events logged
[215343.119907] mce: [Hardware Error]: Machine check events logged
[215343.119925] EDAC MC0: 190 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215343.159210] mce: [Hardware Error]: Machine check events logged
[215343.159229] RAS: Soft-offlining pfn: 0x80fc84
[215343.159240] EDAC MC0: 34 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215343.159275] Memory failure: 0x80fc84: unhandlable page.
[215343.188746] mce: [Hardware Error]: Machine check events logged
[215343.188775] EDAC MC0: 72 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215343.222896] mce: [Hardware Error]: Machine check events logged
[215343.222922] EDAC MC0: 44 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215343.248408] mce: [Hardware Error]: Machine check events logged
[215343.248435] EDAC MC0: 247 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215343.283534] mce: [Hardware Error]: Machine check events logged
[215343.283559] EDAC MC0: 53 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215343.327999] mce: [Hardware Error]: Machine check events logged
[215343.328021] EDAC MC0: 24 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215343.356909] mce: [Hardware Error]: Machine check events logged
[215343.356935] EDAC MC0: 23 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215343.389547] mce: [Hardware Error]: Machine check events logged
[215343.389569] EDAC MC0: 66 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215343.415430] mce: [Hardware Error]: Machine check events logged
[215343.415451] EDAC MC0: 32764 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215343.447811] mce: [Hardware Error]: Machine check events logged
[215343.447838] EDAC MC0: 27 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215343.473942] mce: [Hardware Error]: Machine check events logged
[215343.473962] EDAC MC0: 7 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215343.506291] mce: [Hardware Error]: Machine check events logged
[215343.506314] EDAC MC0: 84 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215343.624939] mce: [Hardware Error]: Machine check events logged
[215343.785373] mce: [Hardware Error]: Machine check events logged
[215343.785393] RAS: Soft-offlining pfn: 0x166dca
[215343.785405] EDAC MC0: 12415 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215343.785619] Memory failure: 0x166dca: unhandlable page.
[215343.860844] mce: [Hardware Error]: Machine check events logged
[215343.860873] EDAC MC0: 264 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215343.873245] mce: [Hardware Error]: Machine check events logged
[215343.873276] EDAC MC0: 339 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215343.887873] mce: [Hardware Error]: Machine check events logged
[215343.901330] mce: [Hardware Error]: Machine check events logged
[215343.901356] EDAC MC0: 632 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215343.917917] mce: [Hardware Error]: Machine check events logged
[215343.917953] EDAC MC0: 493 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215343.927959] mce: [Hardware Error]: Machine check events logged
[215343.939119] mce: [Hardware Error]: Machine check events logged
[215343.939144] EDAC MC0: 362 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215343.949924] mce: [Hardware Error]: Machine check events logged
[215343.949948] EDAC MC0: 326 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215344.200229] mce: [Hardware Error]: Machine check events logged
[215344.200262] EDAC MC0: 32721 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215344.584889] mce: [Hardware Error]: Machine check events logged
[215344.782881] mce: [Hardware Error]: Machine check events logged
[215344.782902] RAS: Soft-offlining pfn: 0x80fc22
[215344.782915] EDAC MC0: 21409 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215344.783311] Memory failure: 0x80fc22: unhandlable page.
[215344.867010] mce: [Hardware Error]: Machine check events logged
[215344.867045] EDAC MC0: 83 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215345.548210] mce: [Hardware Error]: Machine check events logged
[215345.548233] RAS: Soft-offlining pfn: 0x166dca
[215345.548247] EDAC MC0: 61 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215345.548459] Memory failure: 0x166dca: unhandlable page.
[215345.608887] mce: [Hardware Error]: Machine check events logged
[215345.608922] RAS: Soft-offlining pfn: 0x165b9e
[215345.608932] EDAC MC0: 4267 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215345.609137] Memory failure: 0x165b9e: unhandlable page.
[215346.023065] mce: [Hardware Error]: Machine check events logged
[215346.166619] mce: [Hardware Error]: Machine check events logged
[215346.619303] mce: [Hardware Error]: Machine check events logged
[215346.619336] EDAC MC0: 737 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215346.632806] mce: [Hardware Error]: Machine check events logged
[215346.632972] EDAC MC0: 4140 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215346.782719] mce: [Hardware Error]: Machine check events logged
[215346.782744] EDAC MC0: 32348 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215346.839076] mce: [Hardware Error]: Machine check events logged
[215346.839109] RAS: Soft-offlining pfn: 0x165b98
[215346.839123] EDAC MC0: 167 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215346.839321] Memory failure: 0x165b98: unhandlable page.
[215347.050883] mce: [Hardware Error]: Machine check events logged
[215347.052078] EDAC MC0: 8092 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215347.066955] mce: [Hardware Error]: Machine check events logged
[215347.083847] mce: [Hardware Error]: Machine check events logged
[215347.083956] EDAC MC0: 25600 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215347.119359] mce: [Hardware Error]: Machine check events logged
[215347.134226] mce: [Hardware Error]: Machine check events logged
[215347.134278] RAS: Soft-offlining pfn: 0x80fa9c
[215347.134291] EDAC MC0: 486 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215347.134469] Memory failure: 0x80fa9c: unhandlable page.
[215347.165466] mce: [Hardware Error]: Machine check events logged
[215347.165504] EDAC MC0: 143 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215347.185799] mce: [Hardware Error]: Machine check events logged
[215347.202740] mce: [Hardware Error]: Machine check events logged
[215347.218069] mce: [Hardware Error]: Machine check events logged
[215347.218110] EDAC MC0: 1268 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215347.233230] mce: [Hardware Error]: Machine check events logged
[215347.233255] EDAC MC0: 277 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215347.246835] mce: [Hardware Error]: Machine check events logged
[215347.246877] EDAC MC0: 547 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215347.262324] mce: [Hardware Error]: Machine check events logged
[215347.262353] EDAC MC0: 317 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215347.271362] mce: [Hardware Error]: Machine check events logged
[215347.271399] EDAC MC0: 370 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215347.288309] mce: [Hardware Error]: Machine check events logged
[215347.288341] EDAC MC0: 933 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215347.308950] mce: [Hardware Error]: Machine check events logged
[215347.353723] mce: [Hardware Error]: Machine check events logged
[215347.353752] EDAC MC0: 582 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215347.370252] mce: [Hardware Error]: Machine check events logged
[215347.370283] RAS: Soft-offlining pfn: 0x80fb98
[215347.370299] EDAC MC0: 898 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215347.371006] Memory failure: 0x80fb98: unhandlable page.
[215347.383842] mce: [Hardware Error]: Machine check events logged
[215347.403618] mce: [Hardware Error]: Machine check events logged
[215347.403642] RAS: Soft-offlining pfn: 0x166dca
[215347.403657] EDAC MC0: 974 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215347.403937] Memory failure: 0x166dca: unhandlable page.
[215347.432681] mce: [Hardware Error]: Machine check events logged
[215347.484236] mce: [Hardware Error]: Machine check events logged
[215347.592771] mce: [Hardware Error]: Machine check events logged
[215347.592810] EDAC MC0: 8279 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215347.787887] mce: [Hardware Error]: Machine check events logged
[215347.787921] EDAC MC0: 221 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215347.880127] mce: [Hardware Error]: Machine check events logged
[215347.880168] EDAC MC0: 304 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215348.201863] mce: [Hardware Error]: Machine check events logged
[215348.201895] EDAC MC0: 198 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215348.612305] mce: [Hardware Error]: Machine check events logged
[215348.612330] EDAC MC0: 245 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215348.616738] mce: [Hardware Error]: Machine check events logged
[215348.616766] EDAC MC0: 758 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215348.780719] mce: [Hardware Error]: Machine check events logged
[215348.780742] RAS: Soft-offlining pfn: 0x80fd98
[215348.780752] EDAC MC0: 484 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215348.780929] Memory failure: 0x80fd98: unhandlable page.
[215348.797196] mce: [Hardware Error]: Machine check events logged
[215348.797216] RAS: Soft-offlining pfn: 0x166dca
[215348.797228] EDAC MC0: 382 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215348.797451] Memory failure: 0x166dca: unhandlable page.
[215349.206069] mce: [Hardware Error]: Machine check events logged
[215349.206130] RAS: Soft-offlining pfn: 0x80fc18
[215349.206141] EDAC MC0: 84 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215349.206169] Memory failure: 0x80fc18: unhandlable page.
[215349.576840] mce: [Hardware Error]: Machine check events logged
[215349.576880] EDAC MC0: 19586 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215350.092409] mce: [Hardware Error]: Machine check events logged
[215350.600660] mce: [Hardware Error]: Machine check events logged
[215350.600688] EDAC MC0: 32694 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215350.772613] mce: [Hardware Error]: Machine check events logged
[215350.772632] RAS: Soft-offlining pfn: 0x166dca
[215350.772649] EDAC MC0: 351 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215350.772732] Memory failure: 0x166dca: unhandlable page.
[215350.793953] mce: [Hardware Error]: Machine check events logged
[215350.793977] EDAC MC0: 112 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215351.039714] mce: [Hardware Error]: Machine check events logged
[215351.048522] mce: [Hardware Error]: Machine check events logged
[215351.064377] mce: [Hardware Error]: Machine check events logged
[215351.064444] EDAC MC0: 1348 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215351.282753] mce: [Hardware Error]: Machine check events logged
[215351.624629] mce: [Hardware Error]: Machine check events logged
[215351.624667] EDAC MC0: 24839 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215351.792927] mce: [Hardware Error]: Machine check events logged
[215351.792957] EDAC MC0: 415 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215351.817150] i2c i2c-0: sendbytes: NAK bailout.
[215351.820040] mce: [Hardware Error]: Machine check events logged
[215351.821669] i2c i2c-0: sendbytes: NAK bailout.
[215351.898512] mce: [Hardware Error]: Machine check events logged
[215351.898531] RAS: Soft-offlining pfn: 0x166dca
[215351.898541] EDAC MC0: 442 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215351.898825] Memory failure: 0x166dca: unhandlable page.
[215351.944654] EDID block 0 (tag 0x00) checksum is invalid, remainder is 125
[215352.025283] mce: [Hardware Error]: Machine check events logged
[215352.584589] mce: [Hardware Error]: Machine check events logged
[215352.584630] EDAC MC0: 25794 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215352.783518] mce: [Hardware Error]: Machine check events logged
[215352.799935] mce: [Hardware Error]: Machine check events logged
[215352.956684] mce: [Hardware Error]: Machine check events logged
[215352.956711] EDAC MC0: 1155 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215352.969508] mce: [Hardware Error]: Machine check events logged
[215352.969539] EDAC MC0: 259 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215352.984341] mce: [Hardware Error]: Machine check events logged
[215352.984368] EDAC MC0: 334 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215352.999284] mce: [Hardware Error]: Machine check events logged
[215352.999581] EDAC MC0: 2049 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215353.014974] mce: [Hardware Error]: Machine check events logged
[215353.015002] EDAC MC0: 31434 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215353.025855] mce: [Hardware Error]: Machine check events logged
[215353.025879] EDAC MC0: 519 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215353.036586] mce: [Hardware Error]: Machine check events logged
[215353.036876] EDAC MC0: 2666 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215353.099850] mce: [Hardware Error]: Machine check events logged
[215353.099878] EDAC MC0: 30953 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215353.281031] mce: [Hardware Error]: Machine check events logged
[215353.281061] EDAC MC0: 32363 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215353.542409] mce: [Hardware Error]: Machine check events logged
[215353.542429] RAS: Soft-offlining pfn: 0x165b98
[215353.542437] EDAC MC0: 277 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215353.542833] Memory failure: 0x165b98: unhandlable page.
[215353.608549] mce: [Hardware Error]: Machine check events logged
[215354.452476] mce: [Hardware Error]: Machine check events logged
[215354.452496] EDAC MC0: 5693 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215354.632511] mce: [Hardware Error]: Machine check events logged
[215354.632543] EDAC MC0: 5352 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215354.769645] mce: [Hardware Error]: Machine check events logged
[215354.769662] RAS: Soft-offlining pfn: 0x166dca
[215354.769672] EDAC MC0: 404 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215354.769702] Memory failure: 0x166dca: unhandlable page.
[215354.785800] mce: [Hardware Error]: Machine check events logged
[215355.161194] mce: [Hardware Error]: Machine check events logged
[215355.161221] EDAC MC0: 319 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215355.592475] mce: [Hardware Error]: Machine check events logged
[215355.592512] EDAC MC0: 18013 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215355.789551] mce: [Hardware Error]: Machine check events logged
[215355.789577] EDAC MC0: 263 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215356.047245] mce: [Hardware Error]: Machine check events logged
[215356.047270] RAS: Soft-offlining pfn: 0x166dca
[215356.047287] EDAC MC0: 337 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215356.047528] Memory failure: 0x166dca: unhandlable page.
[215356.284154] mce: [Hardware Error]: Machine check events logged
[215356.284205] RAS: Soft-offlining pfn: 0x80fc9c
[215356.284223] EDAC MC0: 202 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215356.284324] Memory failure: 0x80fc9c: unhandlable page.
[215356.384993] mce: [Hardware Error]: Machine check events logged
[215356.616489] mce: [Hardware Error]: Machine check events logged
[215356.785128] mce: [Hardware Error]: Machine check events logged
[215356.901820] mce: [Hardware Error]: Machine check events logged
[215356.901845] EDAC MC0: 12434 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215357.450994] mce: [Hardware Error]: Machine check events logged
[215357.451018] RAS: Soft-offlining pfn: 0x165b98
[215357.451031] EDAC MC0: 188 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215357.451281] Memory failure: 0x165b98: unhandlable page.
[215357.473252] mce: [Hardware Error]: Machine check events logged
[215357.473275] EDAC MC0: 275 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215357.493599] mce: [Hardware Error]: Machine check events logged
[215357.493625] EDAC MC0: 532 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215357.512811] mce: [Hardware Error]: Machine check events logged
[215357.512830] RAS: Soft-offlining pfn: 0x80fb1c
[215357.512841] EDAC MC0: 395 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215357.513195] Memory failure: 0x80fb1c: unhandlable page.
[215357.530410] mce: [Hardware Error]: Machine check events logged
[215357.530433] RAS: Soft-offlining pfn: 0x166dca
[215357.530446] EDAC MC0: 301 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215357.531247] Memory failure: 0x166dca: unhandlable page.
[215357.548110] mce: [Hardware Error]: Machine check events logged
[215357.548141] EDAC MC0: 561 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215357.568318] mce: [Hardware Error]: Machine check events logged
[215357.576402] mce: [Hardware Error]: Machine check events logged
[215357.576431] RAS: Soft-offlining pfn: 0x166dca
[215357.576447] EDAC MC0: 15060 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215357.576717] Memory failure: 0x166dca: unhandlable page.
[215357.591460] mce: [Hardware Error]: Machine check events logged
[215357.614885] mce: [Hardware Error]: Machine check events logged
[215357.630761] mce: [Hardware Error]: Machine check events logged
[215357.680531] mce: [Hardware Error]: Machine check events logged
[215357.680569] EDAC MC0: 1599 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215357.696170] mce: [Hardware Error]: Machine check events logged
[215357.713856] mce: [Hardware Error]: Machine check events logged
[215357.730319] mce: [Hardware Error]: Machine check events logged
[215357.730344] EDAC MC0: 1074 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215357.761473] mce: [Hardware Error]: Machine check events logged
[215357.781407] mce: [Hardware Error]: Machine check events logged
[215357.781430] RAS: Soft-offlining pfn: 0x166dca
[215357.781444] EDAC MC0: 253 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215357.781939] Memory failure: 0x166dca: unhandlable page.
[215357.820688] mce: [Hardware Error]: Machine check events logged
[215357.820713] EDAC MC0: 31 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215357.962593] mce: [Hardware Error]: Machine check events logged
[215358.482190] mce: [Hardware Error]: Machine check events logged
[215358.482219] EDAC MC0: 136 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215358.600362] mce: [Hardware Error]: Machine check events logged
[215358.600392] RAS: Soft-offlining pfn: 0x80fa1c
[215358.600404] EDAC MC0: 12871 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215358.600561] Memory failure: 0x80fa1c: unhandlable page.
[215358.784172] mce: [Hardware Error]: Machine check events logged
[215358.800901] mce: [Hardware Error]: Machine check events logged
[215358.800925] EDAC MC0: 646 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215359.145661] mce: [Hardware Error]: Machine check events logged
[215359.145690] EDAC MC0: 29 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215359.624326] mce: [Hardware Error]: Machine check events logged
[215359.624369] EDAC MC0: 19027 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215359.795299] mce: [Hardware Error]: Machine check events logged
[215359.795331] EDAC MC0: 262 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215360.094756] mce: [Hardware Error]: Machine check events logged
[215360.584287] mce: [Hardware Error]: Machine check events logged
[215360.584332] EDAC MC0: 15800 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215360.786905] mce: [Hardware Error]: Machine check events logged
[215360.786925] RAS: Soft-offlining pfn: 0x166dca
[215360.786935] EDAC MC0: 282 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215360.787123] Memory failure: 0x166dca: unhandlable page.
[215360.832380] mce: [Hardware Error]: Machine check events logged
[215360.832412] EDAC MC0: 399 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215361.044293] mce: [Hardware Error]: Machine check events logged
[215361.090385] mce: [Hardware Error]: Machine check events logged
[215361.090414] EDAC MC0: 165 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215361.099010] mce: [Hardware Error]: Machine check events logged
[215361.099034] EDAC MC0: 272 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215361.115846] mce: [Hardware Error]: Machine check events logged
[215361.360453] mce: [Hardware Error]: Machine check events logged
[215361.360484] EDAC MC0: 480 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215361.584446] mce: [Hardware Error]: Machine check events logged
[215361.608248] mce: [Hardware Error]: Machine check events logged
[215362.064209] mce: [Hardware Error]: Machine check events logged
[215362.068231] RAS: Soft-offlining pfn: 0x80fb18
[215362.068242] EDAC MC0: 2359 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215362.068394] Memory failure: 0x80fb18: unhandlable page.
[215362.182824] EDID block 0 (tag 0x00) checksum is invalid, remainder is 78
[215362.221456] mce: [Hardware Error]: Machine check events logged
[215362.222232] EDAC MC0: 32270 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215362.632233] mce: [Hardware Error]: Machine check events logged
[215362.632272] EDAC MC0: 29929 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215362.774747] mce: [Hardware Error]: Machine check events logged
[215362.774769] EDAC MC0: 275 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215362.912301] mce: [Hardware Error]: Machine check events logged
[215362.912332] EDAC MC0: 534 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215363.055510] mce: [Hardware Error]: Machine check events logged
[215363.055526] RAS: Soft-offlining pfn: 0x165b98
[215363.055537] EDAC MC0: 87 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215363.056214] Memory failure: 0x165b98: unhandlable page.
[215363.068992] mce: [Hardware Error]: Machine check events logged
[215363.082985] mce: [Hardware Error]: Machine check events logged
[215363.083009] RAS: Soft-offlining pfn: 0x80fcb4
[215363.083025] EDAC MC0: 714 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215363.083880] Memory failure: 0x80fcb4: unhandlable page.
[215363.093458] mce: [Hardware Error]: Machine check events logged
[215363.093477] EDAC MC0: 32745 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215363.109109] mce: [Hardware Error]: Machine check events logged
[215363.120711] mce: [Hardware Error]: Machine check events logged
[215363.120734] EDAC MC0: 709 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215363.133250] mce: [Hardware Error]: Machine check events logged
[215363.133268] RAS: Soft-offlining pfn: 0x166dca
[215363.133279] EDAC MC0: 371 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215363.133914] Memory failure: 0x166dca: unhandlable page.
[215363.148188] mce: [Hardware Error]: Machine check events logged
[215363.148219] EDAC MC0: 32718 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215363.268309] mce: [Hardware Error]: Machine check events logged
[215363.284652] mce: [Hardware Error]: Machine check events logged
[215363.292723] mce: [Hardware Error]: Machine check events logged
[215363.299259] mce: [Hardware Error]: Machine check events logged
[215363.299288] EDAC MC0: 1833 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215363.302456] mce: [Hardware Error]: Machine check events logged
[215363.306275] mce: [Hardware Error]: Machine check events logged
[215363.306299] EDAC MC0: 457 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215363.309189] mce: [Hardware Error]: Machine check events logged
[215363.309207] EDAC MC0: 261 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215363.316440] mce: [Hardware Error]: Machine check events logged
[215363.316467] EDAC MC0: 523 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215363.325267] mce: [Hardware Error]: Machine check events logged
[215363.325290] RAS: Soft-offlining pfn: 0x165d34
[215363.325299] EDAC MC0: 505 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215363.326219] Memory failure: 0x165d34: unhandlable page.
[215363.330449] mce: [Hardware Error]: Machine check events logged
[215363.330469] EDAC MC0: 12 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215363.338267] mce: [Hardware Error]: Machine check events logged
[215363.338296] EDAC MC0: 924 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215363.341311] mce: [Hardware Error]: Machine check events logged
[215363.366871] mce: [Hardware Error]: Machine check events logged
[215363.366898] EDAC MC0: 333 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215363.592196] mce: [Hardware Error]: Machine check events logged
[215363.783515] mce: [Hardware Error]: Machine check events logged
[215363.783543] RAS: Soft-offlining pfn: 0x166dca
[215363.783557] EDAC MC0: 13985 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215363.783760] Memory failure: 0x166dca: unhandlable page.
[215363.895474] mce: [Hardware Error]: Machine check events logged
[215363.895511] RAS: Soft-offlining pfn: 0x80fa98
[215363.895521] EDAC MC0: 618 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215363.895695] Memory failure: 0x80fa98: unhandlable page.
[215364.335136] mce: [Hardware Error]: Machine check events logged
[215364.335162] EDAC MC0: 32475 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215364.616161] mce: [Hardware Error]: Machine check events logged
[215364.788866] mce: [Hardware Error]: Machine check events logged
[215364.870791] mce: [Hardware Error]: Machine check events logged
[215364.870826] EDAC MC0: 10982 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215365.576111] mce: [Hardware Error]: Machine check events logged
[215366.109519] mce: [Hardware Error]: Machine check events logged
[215366.109545] EDAC MC0: 32701 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215366.460603] mce: [Hardware Error]: Machine check events logged
[215366.600059] mce: [Hardware Error]: Machine check events logged
[215366.600097] RAS: Soft-offlining pfn: 0x165b98
[215366.600116] EDAC MC0: 16562 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215366.600319] Memory failure: 0x165b98: unhandlable page.
[215366.777911] mce: [Hardware Error]: Machine check events logged
[215366.777936] EDAC MC0: 495 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215366.921600] mce: [Hardware Error]: Machine check events logged
[215366.921630] EDAC MC0: 112 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215367.624029] mce: [Hardware Error]: Machine check events logged
[215367.797084] mce: [Hardware Error]: Machine check events logged
[215367.797103] RAS: Soft-offlining pfn: 0x166dca
[215367.797115] EDAC MC0: 22224 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215367.797297] Memory failure: 0x166dca: unhandlable page.
[215367.843792] mce: [Hardware Error]: Machine check events logged
[215367.843826] EDAC MC0: 630 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215367.863108] mce: [Hardware Error]: Machine check events logged
[215367.863125] RAS: Soft-offlining pfn: 0x80fb1c
[215367.863137] EDAC MC0: 267 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215367.863339] Memory failure: 0x80fb1c: unhandlable page.
[215367.882800] mce: [Hardware Error]: Machine check events logged
[215367.904369] mce: [Hardware Error]: Machine check events logged
[215367.904408] EDAC MC0: 711 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215367.926353] mce: [Hardware Error]: Machine check events logged
[215367.926383] EDAC MC0: 638 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215367.933498] mce: [Hardware Error]: Machine check events logged
[215367.933517] EDAC MC0: 236 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215367.961296] mce: [Hardware Error]: Machine check events logged
[215367.961323] EDAC MC0: 32446 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215367.975151] mce: [Hardware Error]: Machine check events logged
[215367.975180] EDAC MC0: 559 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215368.014866] mce: [Hardware Error]: Machine check events logged
[215368.032713] mce: [Hardware Error]: Machine check events logged
[215368.032737] EDAC MC0: 321 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215368.051867] mce: [Hardware Error]: Machine check events logged
[215368.051891] EDAC MC0: 391 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215368.076001] mce: [Hardware Error]: Machine check events logged
[215368.098668] mce: [Hardware Error]: Machine check events logged
[215368.098698] RAS: Soft-offlining pfn: 0x80fdb4
[215368.098715] EDAC MC0: 1205 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215368.099407] Memory failure: 0x80fdb4: unhandlable page.
[215368.123012] mce: [Hardware Error]: Machine check events logged
[215368.123032] RAS: Soft-offlining pfn: 0x166dca
[215368.123044] EDAC MC0: 160 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215368.123310] Memory failure: 0x166dca: unhandlable page.
[215368.138232] mce: [Hardware Error]: Machine check events logged
[215368.170140] mce: [Hardware Error]: Machine check events logged
[215368.170162] RAS: Soft-offlining pfn: 0x80fb1c
[215368.170178] EDAC MC0: 930 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215368.172019] Memory failure: 0x80fb1c: unhandlable page.
[215368.325362] mce: [Hardware Error]: Machine check events logged
[215368.584005] mce: [Hardware Error]: Machine check events logged
[215368.584041] EDAC MC0: 12908 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215368.776160] mce: [Hardware Error]: Machine check events logged
[215368.793692] mce: [Hardware Error]: Machine check events logged
[215368.793712] RAS: Soft-offlining pfn: 0x166dca
[215368.793725] EDAC MC0: 685 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215368.794036] Memory failure: 0x166dca: unhandlable page.
[215369.269972] mce: [Hardware Error]: Machine check events logged
[215369.607944] mce: [Hardware Error]: Machine check events logged
[215369.607985] EDAC MC0: 7198 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215370.631916] mce: [Hardware Error]: Machine check events logged
[215370.631941] RAS: Soft-offlining pfn: 0x166dca
[215370.631954] EDAC MC0: 32502 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215370.632135] Memory failure: 0x166dca: unhandlable page.
[215370.776807] mce: [Hardware Error]: Machine check events logged
[215370.776825] RAS: Soft-offlining pfn: 0x165a1c
[215370.776836] EDAC MC0: 337 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215370.776868] Memory failure: 0x165a1c: unhandlable page.
[215370.794031] mce: [Hardware Error]: Machine check events logged
[215370.794064] EDAC MC0: 1011 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215371.131619] mce: [Hardware Error]: Machine check events logged
[215371.131640] EDAC MC0: 32579 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215371.146469] mce: [Hardware Error]: Machine check events logged
[215371.146504] EDAC MC0: 566 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215371.163662] mce: [Hardware Error]: Machine check events logged
[215371.528014] mce: [Hardware Error]: Machine check events logged
[215371.591870] mce: [Hardware Error]: Machine check events logged
[215371.591906] EDAC MC0: 11354 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215371.784411] mce: [Hardware Error]: Machine check events logged
[215371.784450] EDAC MC0: 227 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215371.791627] mce: [Hardware Error]: Machine check events logged
[215371.794855] mce: [Hardware Error]: Machine check events logged
[215371.794878] RAS: Soft-offlining pfn: 0x80fb98
[215371.794891] EDAC MC0: 833 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215371.795776] Memory failure: 0x80fb98: unhandlable page.
[215371.799172] mce: [Hardware Error]: Machine check events logged
[215371.799194] EDAC MC0: 11 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215371.807954] mce: [Hardware Error]: Machine check events logged
[215371.812820] mce: [Hardware Error]: Machine check events logged
[215371.821699] mce: [Hardware Error]: Machine check events logged
[215371.821728] EDAC MC0: 197 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215372.115099] mce: [Hardware Error]: Machine check events logged
[215372.115123] RAS: Soft-offlining pfn: 0x166dca
[215372.115133] EDAC MC0: 260 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215372.115353] Memory failure: 0x166dca: unhandlable page.
[215372.299020] i2c i2c-0: sendbytes: NAK bailout.
[215372.299541] i2c i2c-0: sendbytes: NAK bailout.
[215372.303963] mce: [Hardware Error]: Machine check events logged
[215372.307843] EDAC MC0: 258 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215372.331879] i2c i2c-0: sendbytes: NAK bailout.
[215372.363492] i2c i2c-0: sendbytes: NAK bailout.
[215372.424949] EDID block 0 (tag 0x00) checksum is invalid, remainder is 125
[215372.495059] mce: [Hardware Error]: Machine check events logged
[215372.495087] EDAC MC0: 39 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215372.615856] mce: [Hardware Error]: Machine check events logged
[215372.781309] mce: [Hardware Error]: Machine check events logged
[215372.945223] mce: [Hardware Error]: Machine check events logged
[215372.945252] EDAC MC0: 6885 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215373.151076] mce: [Hardware Error]: Machine check events logged
[215373.151099] EDAC MC0: 410 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215373.165367] mce: [Hardware Error]: Machine check events logged
[215373.178530] mce: [Hardware Error]: Machine check events logged
[215373.193950] mce: [Hardware Error]: Machine check events logged
[215373.193975] RAS: Soft-offlining pfn: 0x166dca
[215373.193992] EDAC MC0: 938 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215373.196710] Memory failure: 0x166dca: unhandlable page.
[215373.214310] mce: [Hardware Error]: Machine check events logged
[215373.214342] EDAC MC0: 287 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215373.228085] mce: [Hardware Error]: Machine check events logged
[215373.306111] mce: [Hardware Error]: Machine check events logged
[215373.306142] EDAC MC0: 871 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215373.497945] mce: [Hardware Error]: Machine check events logged
[215373.497966] EDAC MC0: 353 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215373.575796] mce: [Hardware Error]: Machine check events logged
[215373.575836] EDAC MC0: 16324 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215373.865884] mce: [Hardware Error]: Machine check events logged
[215373.865913] EDAC MC0: 226 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215374.353456] mce: [Hardware Error]: Machine check events logged
[215374.353486] EDAC MC0: 34 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215374.389540] mce: [Hardware Error]: Machine check events logged
[215374.389558] RAS: Soft-offlining pfn: 0x80fc98
[215374.389569] EDAC MC0: 32766 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215374.389928] Memory failure: 0x80fc98: unhandlable page.
[215374.419538] mce: [Hardware Error]: Machine check events logged
[215374.419562] EDAC MC0: 673 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215374.449179] mce: [Hardware Error]: Machine check events logged
[215374.473763] mce: [Hardware Error]: Machine check events logged
[215374.473785] EDAC MC0: 32592 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215374.508932] mce: [Hardware Error]: Machine check events logged
[215374.508953] RAS: Soft-offlining pfn: 0x165b98
[215374.508961] EDAC MC0: 32749 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215374.509130] Memory failure: 0x165b98: unhandlable page.
[215374.546097] mce: [Hardware Error]: Machine check events logged
[215374.580027] mce: [Hardware Error]: Machine check events logged
[215374.599766] mce: [Hardware Error]: Machine check events logged
[215374.599794] EDAC MC0: 19368 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215374.639768] mce: [Hardware Error]: Machine check events logged
[215374.671997] mce: [Hardware Error]: Machine check events logged
[215374.672026] EDAC MC0: 436 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215374.704904] mce: [Hardware Error]: Machine check events logged
[215374.733642] mce: [Hardware Error]: Machine check events logged
[215374.733671] EDAC MC0: 1468 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215374.746171] mce: [Hardware Error]: Machine check events logged
[215374.770739] mce: [Hardware Error]: Machine check events logged
[215374.770765] EDAC MC0: 15302 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215374.777488] mce: [Hardware Error]: Machine check events logged
[215374.790133] mce: [Hardware Error]: Machine check events logged
[215374.790160] EDAC MC0: 357 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215374.815425] mce: [Hardware Error]: Machine check events logged
[215374.815448] RAS: Soft-offlining pfn: 0x165b9e
[215374.815459] EDAC MC0: 32686 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215374.815629] Memory failure: 0x165b9e: unhandlable page.
[215374.852714] mce: [Hardware Error]: Machine check events logged
[215374.852750] EDAC MC0: 32766 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215374.888327] mce: [Hardware Error]: Machine check events logged
[215374.888347] RAS: Soft-offlining pfn: 0x80fb18
[215374.888357] EDAC MC0: 18 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215374.888393] Memory failure: 0x80fb18: unhandlable page.
[215374.920057] mce: [Hardware Error]: Machine check events logged
[215374.947520] mce: [Hardware Error]: Machine check events logged
[215374.947541] EDAC MC0: 32757 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215374.980986] mce: [Hardware Error]: Machine check events logged
[215375.011535] mce: [Hardware Error]: Machine check events logged
[215375.039898] mce: [Hardware Error]: Machine check events logged
[215375.039921] RAS: Soft-offlining pfn: 0x80fa18
[215375.039932] EDAC MC0: 70 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215375.039991] Memory failure: 0x80fa18: unhandlable page.
[215375.069823] mce: [Hardware Error]: Machine check events logged
[215375.069850] EDAC MC0: 12 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215375.098264] mce: [Hardware Error]: Machine check events logged
[215375.098286] EDAC MC0: 899 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215375.128330] mce: [Hardware Error]: Machine check events logged
[215375.128348] RAS: Soft-offlining pfn: 0x80fd1c
[215375.128358] EDAC MC0: 32268 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215375.128458] Memory failure: 0x80fd1c: unhandlable page.
[215375.160127] mce: [Hardware Error]: Machine check events logged
[215375.160149] EDAC MC0: 32732 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215375.196514] mce: [Hardware Error]: Machine check events logged
[215375.230297] mce: [Hardware Error]: Machine check events logged
[215375.259928] mce: [Hardware Error]: Machine check events logged
[215375.259948] RAS: Soft-offlining pfn: 0x80fcb0
[215375.259959] EDAC MC0: 131 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215375.259998] Memory failure: 0x80fcb0: unhandlable page.
[215375.291397] mce: [Hardware Error]: Machine check events logged
[215375.348460] mce: [Hardware Error]: Machine check events logged
[215375.348480] RAS: Soft-offlining pfn: 0x80fc98
[215375.348490] EDAC MC0: 94 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215375.348527] Memory failure: 0x80fc98: unhandlable page.
[215375.623722] mce: [Hardware Error]: Machine check events logged
[215375.623762] EDAC MC0: 23163 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215375.778511] mce: [Hardware Error]: Machine check events logged
[215375.781716] EDAC MC0: 6582 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215375.795356] mce: [Hardware Error]: Machine check events logged
[215375.795381] EDAC MC0: 26398 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215375.846324] mce: [Hardware Error]: Machine check events logged
[215375.846345] RAS: Soft-offlining pfn: 0x80fb1c
[215375.846357] EDAC MC0: 488 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215375.846585] Memory failure: 0x80fb1c: unhandlable page.
[215376.142575] mce: [Hardware Error]: Machine check events logged
[215376.142611] EDAC MC0: 540 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215376.383782] mce: [Hardware Error]: Machine check events logged
[215376.383816] EDAC MC0: 32684 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215376.583687] mce: [Hardware Error]: Machine check events logged
[215376.773460] mce: [Hardware Error]: Machine check events logged
[215376.773483] RAS: Soft-offlining pfn: 0x166dca
[215376.773499] EDAC MC0: 10402 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215376.774002] Memory failure: 0x166dca: unhandlable page.
[215376.781260] mce: [Hardware Error]: Machine check events logged
[215376.781283] EDAC MC0: 67 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215376.854501] mce: [Hardware Error]: Machine check events logged
[215377.177354] mce: [Hardware Error]: Machine check events logged
[215377.205129] mce: [Hardware Error]: Machine check events logged
[215377.205159] EDAC MC0: 433 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215377.224812] mce: [Hardware Error]: Machine check events logged
[215377.224840] EDAC MC0: 619 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215377.344991] mce: [Hardware Error]: Machine check events logged
[215377.345021] RAS: Soft-offlining pfn: 0x166dca
[215377.345040] EDAC MC0: 430 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215377.351333] Memory failure: 0x166dca: unhandlable page.
[215377.365416] mce: [Hardware Error]: Machine check events logged
[215377.365450] EDAC MC0: 427 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215377.372550] mce: [Hardware Error]: Machine check events logged
[215377.372576] EDAC MC0: 32697 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215377.406786] mce: [Hardware Error]: Machine check events logged
[215377.409453] EDAC MC0: 2751 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215377.420043] mce: [Hardware Error]: Machine check events logged
[215377.420076] EDAC MC0: 30823 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215377.452729] mce: [Hardware Error]: Machine check events logged
[215377.468361] mce: [Hardware Error]: Machine check events logged
[215377.468423] EDAC MC0: 701 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215377.490514] mce: [Hardware Error]: Machine check events logged
[215377.493363] EDAC MC0: 2893 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215377.607670] mce: [Hardware Error]: Machine check events logged
[215377.607710] EDAC MC0: 25139 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215377.932225] mce: [Hardware Error]: Machine check events logged
[215377.932254] EDAC MC0: 172 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215378.136260] mce: [Hardware Error]: Machine check events logged
[215378.136295] EDAC MC0: 506 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215378.158273] mce: [Hardware Error]: Machine check events logged
[215378.178021] mce: [Hardware Error]: Machine check events logged
[215378.180631] EDAC MC0: 9403 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215378.188940] mce: [Hardware Error]: Machine check events logged
[215378.188954] RAS: Soft-offlining pfn: 0x166dca
[215378.188962] EDAC MC0: 24503 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215378.189571] Memory failure: 0x166dca: unhandlable page.
[215378.278560] mce: [Hardware Error]: Machine check events logged
[215378.278593] EDAC MC0: 206 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215378.308087] mce: [Hardware Error]: Machine check events logged
[215378.308119] EDAC MC0: 351 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215378.343671] mce: [Hardware Error]: Machine check events logged
[215378.343703] EDAC MC0: 676 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215378.631656] mce: [Hardware Error]: Machine check events logged
[215378.631686] EDAC MC0: 30927 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215378.772456] mce: [Hardware Error]: Machine check events logged
[215378.772487] EDAC MC0: 255 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215378.789768] mce: [Hardware Error]: Machine check events logged
[215378.789790] EDAC MC0: 218 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215378.840329] mce: [Hardware Error]: Machine check events logged
[215378.840347] RAS: Soft-offlining pfn: 0x166a1a
[215378.840357] EDAC MC0: 564 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215378.842434] Memory failure: 0x166a1a: unhandlable page.
[215378.845352] mce: [Hardware Error]: Machine check events logged
[215378.845380] EDAC MC0: 274 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215378.852769] mce: [Hardware Error]: Machine check events logged
[215378.852795] EDAC MC0: 32754 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215378.875750] mce: [Hardware Error]: Machine check events logged
[215379.054594] mce: [Hardware Error]: Machine check events logged
[215379.054610] RAS: Soft-offlining pfn: 0x80fb1c
[215379.054618] EDAC MC0: 154 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215379.054921] Memory failure: 0x80fb1c: unhandlable page.
[215379.563251] mce: [Hardware Error]: Machine check events logged
[215379.591569] mce: [Hardware Error]: Machine check events logged
[215379.591599] RAS: Soft-offlining pfn: 0x165b98
[215379.591612] EDAC MC0: 383 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215379.591761] Memory failure: 0x165b98: unhandlable page.
[215379.782746] mce: [Hardware Error]: Machine check events logged
[215379.782772] EDAC MC0: 32741 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215380.027132] mce: [Hardware Error]: Machine check events logged
[215380.027160] EDAC MC0: 164 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215380.469448] mce: [Hardware Error]: Machine check events logged
[215380.469471] EDAC MC0: 32744 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215380.480777] mce: [Hardware Error]: Machine check events logged
[215380.480807] RAS: Soft-offlining pfn: 0x80fa9c
[215380.480818] EDAC MC0: 496 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215380.481563] Memory failure: 0x80fa9c: unhandlable page.
[215380.496443] mce: [Hardware Error]: Machine check events logged
[215380.583971] mce: [Hardware Error]: Machine check events logged
[215380.583995] RAS: Soft-offlining pfn: 0x166dca
[215380.584011] EDAC MC0: 431 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215380.584635] Memory failure: 0x166dca: unhandlable page.
[215380.592182] mce: [Hardware Error]: Machine check events logged
[215380.592333] EDAC MC0: 407 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215380.607734] mce: [Hardware Error]: Machine check events logged
[215380.615532] mce: [Hardware Error]: Machine check events logged
[215380.615572] EDAC MC0: 9734 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215380.631098] mce: [Hardware Error]: Machine check events logged
[215380.631116] EDAC MC0: 103 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215380.641059] mce: [Hardware Error]: Machine check events logged
[215380.653981] mce: [Hardware Error]: Machine check events logged
[215380.654003] EDAC MC0: 376 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215380.657090] mce: [Hardware Error]: Machine check events logged
[215380.657119] EDAC MC0: 88 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215380.666921] mce: [Hardware Error]: Machine check events logged
[215380.666943] RAS: Soft-offlining pfn: 0x166dca
[215380.666956] EDAC MC0: 84 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215380.667420] Memory failure: 0x166dca: unhandlable page.
[215380.705436] mce: [Hardware Error]: Machine check events logged
[215380.753178] mce: [Hardware Error]: Machine check events logged
[215380.753206] EDAC MC0: 16522 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215380.763094] mce: [Hardware Error]: Machine check events logged
[215380.763126] EDAC MC0: 34 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215380.779709] mce: [Hardware Error]: Machine check events logged
[215380.779729] EDAC MC0: 127 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215380.785260] mce: [Hardware Error]: Machine check events logged
[215380.785275] RAS: Soft-offlining pfn: 0x80fb18
[215380.785285] EDAC MC0: 257 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215380.785564] Memory failure: 0x80fb18: unhandlable page.
[215380.798741] mce: [Hardware Error]: Machine check events logged
[215380.798761] EDAC MC0: 85 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.005289] mce: [Hardware Error]: Machine check events logged
[215381.015642] mce: [Hardware Error]: Machine check events logged
[215381.015671] EDAC MC0: 409 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.020153] mce: [Hardware Error]: Machine check events logged
[215381.033336] mce: [Hardware Error]: Machine check events logged
[215381.042040] mce: [Hardware Error]: Machine check events logged
[215381.042071] EDAC MC0: 430 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.055485] mce: [Hardware Error]: Machine check events logged
[215381.055800] RAS: Soft-offlining pfn: 0x80fb98
[215381.055812] EDAC MC0: 2085 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.056209] Memory failure: 0x80fb98: unhandlable page.
[215381.076437] mce: [Hardware Error]: Machine check events logged
[215381.076451] RAS: Soft-offlining pfn: 0x166dca
[215381.076460] EDAC MC0: 30960 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.077957] Memory failure: 0x166dca: unhandlable page.
[215381.091575] mce: [Hardware Error]: Machine check events logged
[215381.091596] EDAC MC0: 233 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.161340] mce: [Hardware Error]: Machine check events logged
[215381.161371] EDAC MC0: 188 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.188824] mce: [Hardware Error]: Machine check events logged
[215381.193317] mce: [Hardware Error]: Machine check events logged
[215381.193337] EDAC MC0: 334 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.201913] mce: [Hardware Error]: Machine check events logged
[215381.201939] EDAC MC0: 59 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.215319] mce: [Hardware Error]: Machine check events logged
[215381.226392] mce: [Hardware Error]: Machine check events logged
[215381.226415] EDAC MC0: 882 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.241877] mce: [Hardware Error]: Machine check events logged
[215381.241894] RAS: Soft-offlining pfn: 0x80fd18
[215381.241904] EDAC MC0: 73 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.242296] Memory failure: 0x80fd18: unhandlable page.
[215381.251077] mce: [Hardware Error]: Machine check events logged
[215381.271335] mce: [Hardware Error]: Machine check events logged
[215381.271368] EDAC MC0: 257 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.284535] mce: [Hardware Error]: Machine check events logged
[215381.284559] EDAC MC0: 308 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.369873] mce: [Hardware Error]: Machine check events logged
[215381.369906] EDAC MC0: 140 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.385222] mce: [Hardware Error]: Machine check events logged
[215381.385248] EDAC MC0: 206 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.401863] mce: [Hardware Error]: Machine check events logged
[215381.401887] EDAC MC0: 347 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.418625] mce: [Hardware Error]: Machine check events logged
[215381.427166] mce: [Hardware Error]: Machine check events logged
[215381.427190] EDAC MC0: 404 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.445962] mce: [Hardware Error]: Machine check events logged
[215381.445984] RAS: Soft-offlining pfn: 0x166dca
[215381.445995] EDAC MC0: 16398 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.447515] Memory failure: 0x166dca: unhandlable page.
[215381.457592] mce: [Hardware Error]: Machine check events logged
[215381.538137] mce: [Hardware Error]: Machine check events logged
[215381.538169] EDAC MC0: 312 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.554635] mce: [Hardware Error]: Machine check events logged
[215381.554662] EDAC MC0: 12 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.575771] mce: [Hardware Error]: Machine check events logged
[215381.575825] EDAC MC0: 432 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.576498] mce: [Hardware Error]: Machine check events logged
[215381.576519] EDAC MC0: 1509 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.588936] mce: [Hardware Error]: Machine check events logged
[215381.602181] mce: [Hardware Error]: Machine check events logged
[215381.622431] mce: [Hardware Error]: Machine check events logged
[215381.622455] EDAC MC0: 592 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.640740] mce: [Hardware Error]: Machine check events logged
[215381.640772] EDAC MC0: 61 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.666033] mce: [Hardware Error]: Machine check events logged
[215381.666059] EDAC MC0: 2 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.723324] mce: [Hardware Error]: Machine check events logged
[215381.723348] RAS: Soft-offlining pfn: 0x166dca
[215381.723361] EDAC MC0: 472 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.724510] Memory failure: 0x166dca: unhandlable page.
[215381.791071] mce: [Hardware Error]: Machine check events logged
[215381.799664] mce: [Hardware Error]: Machine check events logged
[215381.799686] RAS: Soft-offlining pfn: 0x80fd04
[215381.799700] EDAC MC0: 1077 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215381.800177] Memory failure: 0x80fd04: unhandlable page.
[215381.898886] mce: [Hardware Error]: Machine check events logged
[215382.026522] mce: [Hardware Error]: Machine check events logged
[215382.026638] EDAC MC0: 2593 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.063310] mce: [Hardware Error]: Machine check events logged
[215382.063341] EDAC MC0: 31517 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.180930] mce: [Hardware Error]: Machine check events logged
[215382.180964] EDAC MC0: 617 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.243481] mce: [Hardware Error]: Machine check events logged
[215382.255474] mce: [Hardware Error]: Machine check events logged
[215382.255496] RAS: Soft-offlining pfn: 0x80fd32
[215382.255508] EDAC MC0: 1077 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.256487] Memory failure: 0x80fd32: unhandlable page.
[215382.261263] mce: [Hardware Error]: Machine check events logged
[215382.261278] EDAC MC0: 32629 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.265265] mce: [Hardware Error]: Machine check events logged
[215382.265283] RAS: Soft-offlining pfn: 0x166dca
[215382.265291] EDAC MC0: 981 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.265734] Memory failure: 0x166dca: unhandlable page.
[215382.266058] mce: [Hardware Error]: Machine check events logged
[215382.266080] EDAC MC0: 54 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.266832] mce: [Hardware Error]: Machine check events logged
[215382.266854] EDAC MC0: 669 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.267590] mce: [Hardware Error]: Machine check events logged
[215382.268350] mce: [Hardware Error]: Machine check events logged
[215382.268382] EDAC MC0: 1468 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.269110] mce: [Hardware Error]: Machine check events logged
[215382.269140] EDAC MC0: 640 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.269873] mce: [Hardware Error]: Machine check events logged
[215382.270639] mce: [Hardware Error]: Machine check events logged
[215382.271403] mce: [Hardware Error]: Machine check events logged
[215382.272187] mce: [Hardware Error]: Machine check events logged
[215382.272214] RAS: Soft-offlining pfn: 0x80fc32
[215382.272229] EDAC MC0: 2617 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.272393] Memory failure: 0x80fc32: unhandlable page.
[215382.272938] mce: [Hardware Error]: Machine check events logged
[215382.272963] RAS: Soft-offlining pfn: 0x80fd9c
[215382.272973] EDAC MC0: 673 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.273017] Memory failure: 0x80fd9c: unhandlable page.
[215382.280116] mce: [Hardware Error]: Machine check events logged
[215382.280144] EDAC MC0: 32044 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.286964] mce: [Hardware Error]: Machine check events logged
[215382.286986] EDAC MC0: 363 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.290828] mce: [Hardware Error]: Machine check events logged
[215382.290847] EDAC MC0: 190 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.294735] mce: [Hardware Error]: Machine check events logged
[215382.294755] EDAC MC0: 322 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.298591] mce: [Hardware Error]: Machine check events logged
[215382.302322] mce: [Hardware Error]: Machine check events logged
[215382.306239] mce: [Hardware Error]: Machine check events logged
[215382.310186] mce: [Hardware Error]: Machine check events logged
[215382.313841] mce: [Hardware Error]: Machine check events logged
[215382.313863] EDAC MC0: 1460 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.317683] mce: [Hardware Error]: Machine check events logged
[215382.321786] mce: [Hardware Error]: Machine check events logged
[215382.321807] EDAC MC0: 504 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.328769] mce: [Hardware Error]: Machine check events logged
[215382.336312] mce: [Hardware Error]: Machine check events logged
[215382.336338] EDAC MC0: 633 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.343759] mce: [Hardware Error]: Machine check events logged
[215382.343778] RAS: Soft-offlining pfn: 0x80fda2
[215382.343787] EDAC MC0: 389 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.344480] Memory failure: 0x80fda2: unhandlable page.
[215382.351228] mce: [Hardware Error]: Machine check events logged
[215382.351249] EDAC MC0: 136 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.359238] mce: [Hardware Error]: Machine check events logged
[215382.359256] RAS: Soft-offlining pfn: 0x80fd18
[215382.359265] EDAC MC0: 405 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.359295] Memory failure: 0x80fd18: unhandlable page.
[215382.366801] mce: [Hardware Error]: Machine check events logged
[215382.366818] RAS: Soft-offlining pfn: 0x165b9e
[215382.366827] EDAC MC0: 280 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.366856] Memory failure: 0x165b9e: unhandlable page.
[215382.374236] mce: [Hardware Error]: Machine check events logged
[215382.374257] EDAC MC0: 272 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.381841] mce: [Hardware Error]: Machine check events logged
[215382.381864] EDAC MC0: 295 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.389280] mce: [Hardware Error]: Machine check events logged
[215382.397086] mce: [Hardware Error]: Machine check events logged
[215382.397110] EDAC MC0: 759 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.404736] mce: [Hardware Error]: Machine check events logged
[215382.411313] mce: [Hardware Error]: Machine check events logged
[215382.411330] RAS: Soft-offlining pfn: 0x80fa9c
[215382.411343] EDAC MC0: 737 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.411379] Memory failure: 0x80fa9c: unhandlable page.
[215382.417808] mce: [Hardware Error]: Machine check events logged
[215382.417830] EDAC MC0: 25 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.425499] mce: [Hardware Error]: Machine check events logged
[215382.425517] EDAC MC0: 242 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.433455] mce: [Hardware Error]: Machine check events logged
[215382.433478] EDAC MC0: 397 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.442161] mce: [Hardware Error]: Machine check events logged
[215382.442183] EDAC MC0: 292 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.449636] mce: [Hardware Error]: Machine check events logged
[215382.449661] EDAC MC0: 509 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.457497] mce: [Hardware Error]: Machine check events logged
[215382.465012] mce: [Hardware Error]: Machine check events logged
[215382.465038] EDAC MC0: 676 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.472535] mce: [Hardware Error]: Machine check events logged
[215382.478742] mce: [Hardware Error]: Machine check events logged
[215382.478775] RAS: Soft-offlining pfn: 0x80fbb4
[215382.478796] EDAC MC0: 2855 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.479437] mce: [Hardware Error]: Machine check events logged
[215382.479463] EDAC MC0: 31583 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.479482] Memory failure: 0x80fbb4: unhandlable page.
[215382.482549] mce: [Hardware Error]: Machine check events logged
[215382.485127] mce: [Hardware Error]: Machine check events logged
[215382.487662] mce: [Hardware Error]: Machine check events logged
[215382.487690] EDAC MC0: 1277 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.490105] mce: [Hardware Error]: Machine check events logged
[215382.490127] EDAC MC0: 278 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.492631] mce: [Hardware Error]: Machine check events logged
[215382.492655] EDAC MC0: 466 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.495149] mce: [Hardware Error]: Machine check events logged
[215382.495171] EDAC MC0: 327 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.497658] mce: [Hardware Error]: Machine check events logged
[215382.497681] EDAC MC0: 389 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.500197] mce: [Hardware Error]: Machine check events logged
[215382.500220] EDAC MC0: 358 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.527776] mce: [Hardware Error]: Machine check events logged
[215382.527807] EDAC MC0: 541 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.538061] i2c i2c-0: sendbytes: NAK bailout.
[215382.544095] mce: [Hardware Error]: Machine check events logged
[215382.544117] EDAC MC0: 32692 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.584993] mce: [Hardware Error]: Machine check events logged
[215382.585018] RAS: Soft-offlining pfn: 0x166dca
[215382.585029] EDAC MC0: 619 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.585476] Memory failure: 0x166dca: unhandlable page.
[215382.599451] mce: [Hardware Error]: Machine check events logged
[215382.642060] mce: [Hardware Error]: Machine check events logged
[215382.662379] EDID block 0 (tag 0x00) checksum is invalid, remainder is 125
[215382.675068] mce: [Hardware Error]: Machine check events logged
[215382.698654] mce: [Hardware Error]: Machine check events logged
[215382.698675] RAS: Soft-offlining pfn: 0x80fb98
[215382.698688] EDAC MC0: 16659 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.699066] Memory failure: 0x80fb98: unhandlable page.
[215382.722816] mce: [Hardware Error]: Machine check events logged
[215382.748160] mce: [Hardware Error]: Machine check events logged
[215382.748179] RAS: Soft-offlining pfn: 0x80fb84
[215382.748191] EDAC MC0: 776 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.748595] Memory failure: 0x80fb84: unhandlable page.
[215382.767622] mce: [Hardware Error]: Machine check events logged
[215382.770466] mce: [Hardware Error]: Machine check events logged
[215382.770485] EDAC MC0: 16373 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.785233] mce: [Hardware Error]: Machine check events logged
[215382.785254] EDAC MC0: 129 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.808366] mce: [Hardware Error]: Machine check events logged
[215382.808387] EDAC MC0: 171 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.843460] mce: [Hardware Error]: Machine check events logged
[215382.843481] RAS: Soft-offlining pfn: 0x165b98
[215382.843493] EDAC MC0: 721 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.843978] Memory failure: 0x165b98: unhandlable page.
[215382.877267] mce: [Hardware Error]: Machine check events logged
[215382.877287] RAS: Soft-offlining pfn: 0x80fb9c
[215382.877298] EDAC MC0: 210 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.877619] Memory failure: 0x80fb9c: unhandlable page.
[215382.910903] mce: [Hardware Error]: Machine check events logged
[215382.910921] RAS: Soft-offlining pfn: 0x80fc98
[215382.910932] EDAC MC0: 207 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.911250] Memory failure: 0x80fc98: unhandlable page.
[215382.921808] mce: [Hardware Error]: Machine check events logged
[215382.921828] EDAC MC0: 111 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.928199] mce: [Hardware Error]: Machine check events logged
[215382.928215] RAS: Soft-offlining pfn: 0x166dca
[215382.928224] EDAC MC0: 246 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.929461] Memory failure: 0x166dca: unhandlable page.
[215382.933547] mce: [Hardware Error]: Machine check events logged
[215382.933562] RAS: Soft-offlining pfn: 0x80fd34
[215382.933572] EDAC MC0: 46 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.933731] Memory failure: 0x80fd34: unhandlable page.
[215382.940038] mce: [Hardware Error]: Machine check events logged
[215382.946872] mce: [Hardware Error]: Machine check events logged
[215382.953339] mce: [Hardware Error]: Machine check events logged
[215382.953362] EDAC MC0: 483 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.960245] mce: [Hardware Error]: Machine check events logged
[215382.960265] EDAC MC0: 103 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.968287] mce: [Hardware Error]: Machine check events logged
[215382.968307] EDAC MC0: 161 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.975268] mce: [Hardware Error]: Machine check events logged
[215382.975293] EDAC MC0: 595 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.977962] mce: [Hardware Error]: Machine check events logged
[215382.980699] mce: [Hardware Error]: Machine check events logged
[215382.980724] EDAC MC0: 423 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.983383] mce: [Hardware Error]: Machine check events logged
[215382.986154] mce: [Hardware Error]: Machine check events logged
[215382.988922] mce: [Hardware Error]: Machine check events logged
[215382.988945] EDAC MC0: 631 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.991715] mce: [Hardware Error]: Machine check events logged
[215382.991740] EDAC MC0: 513 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.993000] mce: [Hardware Error]: Machine check events logged
[215382.993017] EDAC MC0: 104 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.994198] mce: [Hardware Error]: Machine check events logged
[215382.994220] EDAC MC0: 347 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.995587] mce: [Hardware Error]: Machine check events logged
[215382.996836] mce: [Hardware Error]: Machine check events logged
[215382.996869] EDAC MC0: 852 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.998248] mce: [Hardware Error]: Machine check events logged
[215382.998263] EDAC MC0: 32674 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215382.999696] mce: [Hardware Error]: Machine check events logged
[215383.001224] mce: [Hardware Error]: Machine check events logged
[215383.001248] EDAC MC0: 545 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.002693] mce: [Hardware Error]: Machine check events logged
[215383.004172] mce: [Hardware Error]: Machine check events logged
[215383.004189] RAS: Soft-offlining pfn: 0x80fc98
[215383.004202] EDAC MC0: 642 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.004458] Memory failure: 0x80fc98: unhandlable page.
[215383.017558] mce: [Hardware Error]: Machine check events logged
[215383.048025] mce: [Hardware Error]: Machine check events logged
[215383.048058] EDAC MC0: 1317 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.049828] mce: [Hardware Error]: Machine check events logged
[215383.049860] EDAC MC0: 861 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.050498] mce: [Hardware Error]: Machine check events logged
[215383.050527] EDAC MC0: 576 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.051117] mce: [Hardware Error]: Machine check events logged
[215383.051155] EDAC MC0: 1240 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.052488] mce: [Hardware Error]: Machine check events logged
[215383.052505] RAS: Soft-offlining pfn: 0x165c88
[215383.052514] EDAC MC0: 32092 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.052994] Memory failure: 0x165c88: unhandlable page.
[215383.053290] mce: [Hardware Error]: Machine check events logged
[215383.053305] RAS: Soft-offlining pfn: 0x166dca
[215383.053314] EDAC MC0: 966 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.053334] Memory failure: 0x166dca: unhandlable page.
[215383.053923] mce: [Hardware Error]: Machine check events logged
[215383.054677] mce: [Hardware Error]: Machine check events logged
[215383.054696] EDAC MC0: 326 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.056233] mce: [Hardware Error]: Machine check events logged
[215383.056253] EDAC MC0: 239 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.057054] mce: [Hardware Error]: Machine check events logged
[215383.057690] mce: [Hardware Error]: Machine check events logged
[215383.058383] mce: [Hardware Error]: Machine check events logged
[215383.059264] mce: [Hardware Error]: Machine check events logged
[215383.059899] mce: [Hardware Error]: Machine check events logged
[215383.060532] mce: [Hardware Error]: Machine check events logged
[215383.060575] EDAC MC0: 5461 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.061133] mce: [Hardware Error]: Machine check events logged
[215383.061157] EDAC MC0: 290 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.065648] mce: [Hardware Error]: Machine check events logged
[215383.079566] mce: [Hardware Error]: Machine check events logged
[215383.094793] mce: [Hardware Error]: Machine check events logged
[215383.106200] mce: [Hardware Error]: Machine check events logged
[215383.106222] RAS: Soft-offlining pfn: 0x80fa98
[215383.106238] EDAC MC0: 5 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.107157] Memory failure: 0x80fa98: unhandlable page.
[215383.127388] mce: [Hardware Error]: Machine check events logged
[215383.127410] RAS: Soft-offlining pfn: 0x166dca
[215383.127418] EDAC MC0: 32722 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.127575] Memory failure: 0x166dca: unhandlable page.
[215383.153772] mce: [Hardware Error]: Machine check events logged
[215383.153793] RAS: Soft-offlining pfn: 0x32000
[215383.153804] EDAC MC0: 40 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.153863] Memory failure: 0x32000: unhandlable page.
[215383.168722] mce: [Hardware Error]: Machine check events logged
[215383.198112] mce: [Hardware Error]: Machine check events logged
[215383.231452] mce: [Hardware Error]: Machine check events logged
[215383.244216] mce: [Hardware Error]: Machine check events logged
[215383.244242] EDAC MC0: 1339 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.252732] mce: [Hardware Error]: Machine check events logged
[215383.262762] mce: [Hardware Error]: Machine check events logged
[215383.262792] RAS: Soft-offlining pfn: 0x166dca
[215383.262811] EDAC MC0: 601 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.263768] Memory failure: 0x166dca: unhandlable page.
[215383.269434] mce: [Hardware Error]: Machine check events logged
[215383.278227] mce: [Hardware Error]: Machine check events logged
[215383.278446] EDAC MC0: 1294 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.286517] mce: [Hardware Error]: Machine check events logged
[215383.286543] EDAC MC0: 31974 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.294579] mce: [Hardware Error]: Machine check events logged
[215383.294621] EDAC MC0: 600 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.303263] mce: [Hardware Error]: Machine check events logged
[215383.303288] EDAC MC0: 32617 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.312805] mce: [Hardware Error]: Machine check events logged
[215383.312833] EDAC MC0: 81 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.322295] mce: [Hardware Error]: Machine check events logged
[215383.322324] EDAC MC0: 291 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.328325] mce: [Hardware Error]: Machine check events logged
[215383.342881] mce: [Hardware Error]: Machine check events logged
[215383.342896] RAS: Soft-offlining pfn: 0x166dca
[215383.342907] EDAC MC0: 382 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.343394] Memory failure: 0x166dca: unhandlable page.
[215383.363303] mce: [Hardware Error]: Machine check events logged
[215383.383177] mce: [Hardware Error]: Machine check events logged
[215383.404144] mce: [Hardware Error]: Machine check events logged
[215383.423669] mce: [Hardware Error]: Machine check events logged
[215383.423689] EDAC MC0: 238 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.448019] mce: [Hardware Error]: Machine check events logged
[215383.448040] EDAC MC0: 32751 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.471725] mce: [Hardware Error]: Machine check events logged
[215383.471749] RAS: Soft-offlining pfn: 0x166dca
[215383.471761] EDAC MC0: 68 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.471905] Memory failure: 0x166dca: unhandlable page.
[215383.500530] mce: [Hardware Error]: Machine check events logged
[215383.500544] RAS: Soft-offlining pfn: 0x80fb98
[215383.500551] EDAC MC0: 4 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.500835] Memory failure: 0x80fb98: unhandlable page.
[215383.522230] mce: [Hardware Error]: Machine check events logged
[215383.522254] EDAC MC0: 47 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.549908] mce: [Hardware Error]: Machine check events logged
[215383.573746] mce: [Hardware Error]: Machine check events logged
[215383.573810] EDAC MC0: 431 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.603776] mce: [Hardware Error]: Machine check events logged
[215383.603791] RAS: Soft-offlining pfn: 0x80fb98
[215383.603800] EDAC MC0: 32563 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.603990] Memory failure: 0x80fb98: unhandlable page.
[215383.623427] mce: [Hardware Error]: Machine check events logged
[215383.623462] EDAC MC0: 24915 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.646795] mce: [Hardware Error]: Machine check events logged
[215383.668673] mce: [Hardware Error]: Machine check events logged
[215383.689883] mce: [Hardware Error]: Machine check events logged
[215383.689900] RAS: Soft-offlining pfn: 0x80fcb0
[215383.689911] EDAC MC0: 520 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.690095] Memory failure: 0x80fcb0: unhandlable page.
[215383.718202] mce: [Hardware Error]: Machine check events logged
[215383.718221] EDAC MC0: 32730 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.746507] mce: [Hardware Error]: Machine check events logged
[215383.746533] EDAC MC0: 80 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.771274] mce: [Hardware Error]: Machine check events logged
[215383.780055] mce: [Hardware Error]: Machine check events logged
[215383.780081] RAS: Soft-offlining pfn: 0x80fa98
[215383.780096] EDAC MC0: 413 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.781450] Memory failure: 0x80fa98: unhandlable page.
[215383.790140] mce: [Hardware Error]: Machine check events logged
[215383.790159] RAS: Soft-offlining pfn: 0x80fb18
[215383.790173] EDAC MC0: 309 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.791439] Memory failure: 0x80fb18: unhandlable page.
[215383.799694] mce: [Hardware Error]: Machine check events logged
[215383.800293] EDAC MC0: 2981 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.804938] mce: [Hardware Error]: Machine check events logged
[215383.829902] mce: [Hardware Error]: Machine check events logged
[215383.829927] EDAC MC0: 13224 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.852603] mce: [Hardware Error]: Machine check events logged
[215383.852632] EDAC MC0: 61 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.877058] mce: [Hardware Error]: Machine check events logged
[215383.877079] RAS: Soft-offlining pfn: 0x166dca
[215383.877090] EDAC MC0: 116 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.877270] Memory failure: 0x166dca: unhandlable page.
[215383.901150] mce: [Hardware Error]: Machine check events logged
[215383.908819] mce: [Hardware Error]: Machine check events logged
[215383.908850] EDAC MC0: 381 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.923044] mce: [Hardware Error]: Machine check events logged
[215383.923067] RAS: Soft-offlining pfn: 0x80fb9c
[215383.923080] EDAC MC0: 61 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.923253] Memory failure: 0x80fb9c: unhandlable page.
[215383.941962] mce: [Hardware Error]: Machine check events logged
[215383.941988] EDAC MC0: 6 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.964799] mce: [Hardware Error]: Machine check events logged
[215383.964834] EDAC MC0: 271 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215383.988835] mce: [Hardware Error]: Machine check events logged
[215384.014900] mce: [Hardware Error]: Machine check events logged
[215384.014929] EDAC MC0: 82 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.040667] mce: [Hardware Error]: Machine check events logged
[215384.040693] EDAC MC0: 7 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.061077] mce: [Hardware Error]: Machine check events logged
[215384.092778] mce: [Hardware Error]: Machine check events logged
[215384.092797] EDAC MC0: 154 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.106617] mce: [Hardware Error]: Machine check events logged
[215384.106648] EDAC MC0: 150 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.135222] mce: [Hardware Error]: Machine check events logged
[215384.163905] mce: [Hardware Error]: Machine check events logged
[215384.191286] mce: [Hardware Error]: Machine check events logged
[215384.191300] RAS: Soft-offlining pfn: 0x80fdb0
[215384.191309] EDAC MC0: 286 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.191475] Memory failure: 0x80fdb0: unhandlable page.
[215384.213416] mce: [Hardware Error]: Machine check events logged
[215384.213439] EDAC MC0: 32743 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.240143] mce: [Hardware Error]: Machine check events logged
[215384.240160] RAS: Soft-offlining pfn: 0x165b98
[215384.240168] EDAC MC0: 744 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.241416] Memory failure: 0x165b98: unhandlable page.
[215384.241933] mce: [Hardware Error]: Machine check events logged
[215384.241949] EDAC MC0: 32604 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.246596] mce: [Hardware Error]: Machine check events logged
[215384.246619] EDAC MC0: 361 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.253100] mce: [Hardware Error]: Machine check events logged
[215384.253129] EDAC MC0: 685 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.260177] mce: [Hardware Error]: Machine check events logged
[215384.260201] RAS: Soft-offlining pfn: 0x166dca
[215384.260212] EDAC MC0: 864 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.260813] Memory failure: 0x166dca: unhandlable page.
[215384.266394] mce: [Hardware Error]: Machine check events logged
[215384.266412] EDAC MC0: 32581 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.270368] mce: [Hardware Error]: Machine check events logged
[215384.284406] mce: [Hardware Error]: Machine check events logged
[215384.284568] RAS: Soft-offlining pfn: 0x80fc22
[215384.284579] EDAC MC0: 879 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.286276] Memory failure: 0x80fc22: unhandlable page.
[215384.294017] mce: [Hardware Error]: Machine check events logged
[215384.294033] RAS: Soft-offlining pfn: 0x166dca
[215384.294041] EDAC MC0: 32174 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.294599] Memory failure: 0x166dca: unhandlable page.
[215384.306669] mce: [Hardware Error]: Machine check events logged
[215384.323171] mce: [Hardware Error]: Machine check events logged
[215384.323199] EDAC MC0: 328 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.340074] mce: [Hardware Error]: Machine check events logged
[215384.340099] EDAC MC0: 3 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.365356] mce: [Hardware Error]: Machine check events logged
[215384.365390] EDAC MC0: 32766 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.387644] mce: [Hardware Error]: Machine check events logged
[215384.387666] EDAC MC0: 36 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.405669] mce: [Hardware Error]: Machine check events logged
[215384.406153] EDAC MC0: 369 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.428126] mce: [Hardware Error]: Machine check events logged
[215384.429016] RAS: Soft-offlining pfn: 0x80fb18
[215384.429031] EDAC MC0: 6863 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.431386] Memory failure: 0x80fb18: unhandlable page.
[215384.436402] mce: [Hardware Error]: Machine check events logged
[215384.446631] mce: [Hardware Error]: Machine check events logged
[215384.446659] EDAC MC0: 26002 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.473199] mce: [Hardware Error]: Machine check events logged
[215384.473226] EDAC MC0: 2 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.493965] mce: [Hardware Error]: Machine check events logged
[215384.493987] EDAC MC0: 115 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.512404] mce: [Hardware Error]: Machine check events logged
[215384.512431] EDAC MC0: 22 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.532957] mce: [Hardware Error]: Machine check events logged
[215384.532982] EDAC MC0: 32759 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.558814] mce: [Hardware Error]: Machine check events logged
[215384.558836] EDAC MC0: 37 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.581596] mce: [Hardware Error]: Machine check events logged
[215384.581772] EDAC MC0: 1944 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.583383] mce: [Hardware Error]: Machine check events logged
[215384.604973] mce: [Hardware Error]: Machine check events logged
[215384.605001] EDAC MC0: 7220 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.630009] mce: [Hardware Error]: Machine check events logged
[215384.656772] mce: [Hardware Error]: Machine check events logged
[215384.681471] mce: [Hardware Error]: Machine check events logged
[215384.692064] mce: [Hardware Error]: Machine check events logged
[215384.692088] RAS: Soft-offlining pfn: 0x32000
[215384.692103] EDAC MC0: 677 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.692288] Memory failure: 0x32000: unhandlable page.
[215384.717050] mce: [Hardware Error]: Machine check events logged
[215384.717072] RAS: Soft-offlining pfn: 0x166dca
[215384.717083] EDAC MC0: 32685 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.717295] Memory failure: 0x166dca: unhandlable page.
[215384.738955] mce: [Hardware Error]: Machine check events logged
[215384.739097] EDAC MC0: 2739 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.741120] mce: [Hardware Error]: Machine check events logged
[215384.744656] mce: [Hardware Error]: Machine check events logged
[215384.744680] EDAC MC0: 31091 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.748413] mce: [Hardware Error]: Machine check events logged
[215384.751126] mce: [Hardware Error]: Machine check events logged
[215384.751150] EDAC MC0: 401 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.754123] mce: [Hardware Error]: Machine check events logged
[215384.756978] mce: [Hardware Error]: Machine check events logged
[215384.757004] EDAC MC0: 429 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.760314] mce: [Hardware Error]: Machine check events logged
[215384.760339] EDAC MC0: 258 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.764324] mce: [Hardware Error]: Machine check events logged
[215384.764349] EDAC MC0: 104 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.770011] mce: [Hardware Error]: Machine check events logged
[215384.770034] EDAC MC0: 32646 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.776125] mce: [Hardware Error]: Machine check events logged
[215384.777585] EDAC MC0: 13269 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.781755] mce: [Hardware Error]: Machine check events logged
[215384.793843] mce: [Hardware Error]: Machine check events logged
[215384.810197] mce: [Hardware Error]: Machine check events logged
[215384.810220] RAS: Soft-offlining pfn: 0x165b98
[215384.810235] EDAC MC0: 20053 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.810451] Memory failure: 0x165b98: unhandlable page.
[215384.829242] mce: [Hardware Error]: Machine check events logged
[215384.829263] EDAC MC0: 110 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.853955] mce: [Hardware Error]: Machine check events logged
[215384.880114] mce: [Hardware Error]: Machine check events logged
[215384.880143] EDAC MC0: 32744 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.906191] mce: [Hardware Error]: Machine check events logged
[215384.906212] EDAC MC0: 160 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.913806] mce: [Hardware Error]: Machine check events logged
[215384.913822] RAS: Soft-offlining pfn: 0x165b98
[215384.913831] EDAC MC0: 200 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.915405] Memory failure: 0x165b98: unhandlable page.
[215384.924558] mce: [Hardware Error]: Machine check events logged
[215384.924586] EDAC MC0: 32730 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.950404] mce: [Hardware Error]: Machine check events logged
[215384.950437] RAS: Soft-offlining pfn: 0x166dca
[215384.950452] EDAC MC0: 777 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215384.950506] Memory failure: 0x166dca: unhandlable page.
[215384.970498] mce: [Hardware Error]: Machine check events logged
[215384.991610] mce: [Hardware Error]: Machine check events logged
[215385.014114] mce: [Hardware Error]: Machine check events logged
[215385.037143] mce: [Hardware Error]: Machine check events logged
[215385.037181] EDAC MC0: 421 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.060660] mce: [Hardware Error]: Machine check events logged
[215385.060696] EDAC MC0: 32699 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.073313] mce: [Hardware Error]: Machine check events logged
[215385.073338] RAS: Soft-offlining pfn: 0x166dca
[215385.073367] EDAC MC0: 297 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.073537] Memory failure: 0x166dca: unhandlable page.
[215385.090665] mce: [Hardware Error]: Machine check events logged
[215385.090692] EDAC MC0: 32745 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.109899] mce: [Hardware Error]: Machine check events logged
[215385.109937] EDAC MC0: 744 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.130172] mce: [Hardware Error]: Machine check events logged
[215385.130202] RAS: Soft-offlining pfn: 0x165b98
[215385.130221] EDAC MC0: 32727 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.130299] Memory failure: 0x165b98: unhandlable page.
[215385.156898] mce: [Hardware Error]: Machine check events logged
[215385.156928] EDAC MC0: 563 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.167036] mce: [Hardware Error]: Machine check events logged
[215385.189210] mce: [Hardware Error]: Machine check events logged
[215385.216692] mce: [Hardware Error]: Machine check events logged
[215385.216719] EDAC MC0: 67 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.235831] mce: [Hardware Error]: Machine check events logged
[215385.235860] EDAC MC0: 170 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.259556] mce: [Hardware Error]: Machine check events logged
[215385.278783] mce: [Hardware Error]: Machine check events logged
[215385.278805] EDAC MC0: 577 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.296797] mce: [Hardware Error]: Machine check events logged
[215385.299220] EDAC MC0: 6075 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.316486] mce: [Hardware Error]: Machine check events logged
[215385.316512] EDAC MC0: 26819 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.343004] mce: [Hardware Error]: Machine check events logged
[215385.368886] mce: [Hardware Error]: Machine check events logged
[215385.368906] EDAC MC0: 68 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.395719] mce: [Hardware Error]: Machine check events logged
[215385.395743] RAS: Soft-offlining pfn: 0x166dca
[215385.395754] EDAC MC0: 177 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.396157] Memory failure: 0x166dca: unhandlable page.
[215385.422275] mce: [Hardware Error]: Machine check events logged
[215385.422296] RAS: Soft-offlining pfn: 0x80fdb4
[215385.422308] EDAC MC0: 5 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.422325] Memory failure: 0x80fdb4: unhandlable page.
[215385.444587] mce: [Hardware Error]: Machine check events logged
[215385.444619] EDAC MC0: 319 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.471262] mce: [Hardware Error]: Machine check events logged
[215385.498393] mce: [Hardware Error]: Machine check events logged
[215385.498428] EDAC MC0: 427 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.525528] mce: [Hardware Error]: Machine check events logged
[215385.525556] EDAC MC0: 953 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.551172] mce: [Hardware Error]: Machine check events logged
[215385.563904] mce: [Hardware Error]: Machine check events logged
[215385.563919] RAS: Soft-offlining pfn: 0x80fc98
[215385.563929] EDAC MC0: 32660 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.565370] Memory failure: 0x80fc98: unhandlable page.
[215385.584979] mce: [Hardware Error]: Machine check events logged
[215385.602925] mce: [Hardware Error]: Machine check events logged
[215385.602948] RAS: Soft-offlining pfn: 0x80fb30
[215385.602963] EDAC MC0: 97 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.605358] Memory failure: 0x80fb30: unhandlable page.
[215385.608338] mce: [Hardware Error]: Machine check events logged
[215385.608354] EDAC MC0: 18636 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.627580] mce: [Hardware Error]: Machine check events logged
[215385.627599] RAS: Soft-offlining pfn: 0x166dca
[215385.627611] EDAC MC0: 96 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.627701] Memory failure: 0x166dca: unhandlable page.
[215385.652652] mce: [Hardware Error]: Machine check events logged
[215385.652675] RAS: Soft-offlining pfn: 0x80fb34
[215385.652686] EDAC MC0: 36 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.652762] Memory failure: 0x80fb34: unhandlable page.
[215385.675039] mce: [Hardware Error]: Machine check events logged
[215385.675072] EDAC MC0: 209 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.700809] mce: [Hardware Error]: Machine check events logged
[215385.700833] RAS: Soft-offlining pfn: 0x165b98
[215385.700845] EDAC MC0: 109 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.705349] Memory failure: 0x165b98: unhandlable page.
[215385.711913] mce: [Hardware Error]: Machine check events logged
[215385.731702] mce: [Hardware Error]: Machine check events logged
[215385.731726] EDAC MC0: 409 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.756608] mce: [Hardware Error]: Machine check events logged
[215385.781295] mce: [Hardware Error]: Machine check events logged
[215385.781327] EDAC MC0: 289 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.802477] mce: [Hardware Error]: Machine check events logged
[215385.802508] EDAC MC0: 197 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.830156] mce: [Hardware Error]: Machine check events logged
[215385.857401] mce: [Hardware Error]: Machine check events logged
[215385.857442] EDAC MC0: 1146 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.878509] mce: [Hardware Error]: Machine check events logged
[215385.878537] EDAC MC0: 32505 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.905320] mce: [Hardware Error]: Machine check events logged
[215385.905351] EDAC MC0: 48 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.923451] mce: [Hardware Error]: Machine check events logged
[215385.938595] mce: [Hardware Error]: Machine check events logged
[215385.938618] RAS: Soft-offlining pfn: 0x32000
[215385.938632] EDAC MC0: 372 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.938796] Memory failure: 0x32000: unhandlable page.
[215385.958113] mce: [Hardware Error]: Machine check events logged
[215385.958133] EDAC MC0: 10 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.972902] mce: [Hardware Error]: Machine check events logged
[215385.972930] EDAC MC0: 151 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215385.993913] mce: [Hardware Error]: Machine check events logged
[215385.993938] EDAC MC0: 18 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.016900] mce: [Hardware Error]: Machine check events logged
[215386.038808] mce: [Hardware Error]: Machine check events logged
[215386.061604] mce: [Hardware Error]: Machine check events logged
[215386.061627] RAS: Soft-offlining pfn: 0x166dca
[215386.061641] EDAC MC0: 477 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.061922] Memory failure: 0x166dca: unhandlable page.
[215386.088395] mce: [Hardware Error]: Machine check events logged
[215386.088415] EDAC MC0: 10 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.108388] mce: [Hardware Error]: Machine check events logged
[215386.122360] mce: [Hardware Error]: Machine check events logged
[215386.122375] RAS: Soft-offlining pfn: 0x166dca
[215386.122387] EDAC MC0: 437 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.122574] Memory failure: 0x166dca: unhandlable page.
[215386.135449] mce: [Hardware Error]: Machine check events logged
[215386.155518] mce: [Hardware Error]: Machine check events logged
[215386.155537] RAS: Soft-offlining pfn: 0x80fca2
[215386.155553] EDAC MC0: 346 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.155708] Memory failure: 0x80fca2: unhandlable page.
[215386.182788] mce: [Hardware Error]: Machine check events logged
[215386.182819] EDAC MC0: 116 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.203044] mce: [Hardware Error]: Machine check events logged
[215386.223214] mce: [Hardware Error]: Machine check events logged
[215386.250652] mce: [Hardware Error]: Machine check events logged
[215386.250683] EDAC MC0: 1266 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.277596] mce: [Hardware Error]: Machine check events logged
[215386.277618] RAS: Soft-offlining pfn: 0x80fa98
[215386.277629] EDAC MC0: 32391 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.277915] Memory failure: 0x80fa98: unhandlable page.
[215386.294571] mce: [Hardware Error]: Machine check events logged
[215386.294599] EDAC MC0: 93 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.318171] mce: [Hardware Error]: Machine check events logged
[215386.318202] EDAC MC0: 737 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.344893] mce: [Hardware Error]: Machine check events logged
[215386.344915] RAS: Soft-offlining pfn: 0x165b98
[215386.344927] EDAC MC0: 361 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.345096] Memory failure: 0x165b98: unhandlable page.
[215386.363147] mce: [Hardware Error]: Machine check events logged
[215386.363171] EDAC MC0: 32626 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.374645] mce: [Hardware Error]: Machine check events logged
[215386.399999] mce: [Hardware Error]: Machine check events logged
[215386.400020] EDAC MC0: 191 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.421635] mce: [Hardware Error]: Machine check events logged
[215386.421654] RAS: Soft-offlining pfn: 0x166dca
[215386.421667] EDAC MC0: 370 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.423333] Memory failure: 0x166dca: unhandlable page.
[215386.454535] mce: [Hardware Error]: Machine check events logged
[215386.454560] EDAC MC0: 528 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.474451] mce: [Hardware Error]: Machine check events logged
[215386.474479] EDAC MC0: 32677 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.495315] mce: [Hardware Error]: Machine check events logged
[215386.495346] EDAC MC0: 281 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.517315] mce: [Hardware Error]: Machine check events logged
[215386.541186] mce: [Hardware Error]: Machine check events logged
[215386.541208] EDAC MC0: 188 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.565149] mce: [Hardware Error]: Machine check events logged
[215386.593563] mce: [Hardware Error]: Machine check events logged
[215386.605517] mce: [Hardware Error]: Machine check events logged
[215386.605544] RAS: Soft-offlining pfn: 0x166dca
[215386.605560] EDAC MC0: 567 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.605781] Memory failure: 0x166dca: unhandlable page.
[215386.629645] mce: [Hardware Error]: Machine check events logged
[215386.629673] RAS: Soft-offlining pfn: 0x80fd18
[215386.629685] EDAC MC0: 239 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.629739] Memory failure: 0x80fd18: unhandlable page.
[215386.631303] mce: [Hardware Error]: Machine check events logged
[215386.631320] RAS: Soft-offlining pfn: 0x117960
[215386.631329] EDAC MC0: 1941 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.631351] Memory failure: 0x117960: unhandlable page.
[215386.647979] mce: [Hardware Error]: Machine check events logged
[215386.648009] EDAC MC0: 167 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.672227] mce: [Hardware Error]: Machine check events logged
[215386.672246] EDAC MC0: 230 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.686726] mce: [Hardware Error]: Machine check events logged
[215386.686754] EDAC MC0: 33 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.707207] mce: [Hardware Error]: Machine check events logged
[215386.707228] RAS: Soft-offlining pfn: 0x80fc30
[215386.707237] EDAC MC0: 437 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.708420] Memory failure: 0x80fc30: unhandlable page.
[215386.725917] mce: [Hardware Error]: Machine check events logged
[215386.725942] EDAC MC0: 32594 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.750613] mce: [Hardware Error]: Machine check events logged
[215386.750634] RAS: Soft-offlining pfn: 0x80fb18
[215386.750646] EDAC MC0: 66 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.750726] Memory failure: 0x80fb18: unhandlable page.
[215386.765178] mce: [Hardware Error]: Machine check events logged
[215386.771235] mce: [Hardware Error]: Machine check events logged
[215386.771260] EDAC MC0: 550 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.779820] mce: [Hardware Error]: Machine check events logged
[215386.787160] mce: [Hardware Error]: Machine check events logged
[215386.787181] EDAC MC0: 229 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.803526] mce: [Hardware Error]: Machine check events logged
[215386.803554] EDAC MC0: 387 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.824257] mce: [Hardware Error]: Machine check events logged
[215386.844443] mce: [Hardware Error]: Machine check events logged
[215386.844463] EDAC MC0: 265 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.852017] mce: [Hardware Error]: Machine check events logged
[215386.852033] RAS: Soft-offlining pfn: 0x80fc1c
[215386.852041] EDAC MC0: 137 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.852264] Memory failure: 0x80fc1c: unhandlable page.
[215386.873579] mce: [Hardware Error]: Machine check events logged
[215386.873599] RAS: Soft-offlining pfn: 0x80fb18
[215386.873611] EDAC MC0: 68 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.873667] Memory failure: 0x80fb18: unhandlable page.
[215386.897103] mce: [Hardware Error]: Machine check events logged
[215386.897130] EDAC MC0: 32688 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.912483] mce: [Hardware Error]: Machine check events logged
[215386.912510] EDAC MC0: 202 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.936108] mce: [Hardware Error]: Machine check events logged
[215386.936124] EDAC MC0: 99 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.949908] mce: [Hardware Error]: Machine check events logged
[215386.949927] EDAC MC0: 173 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215386.975001] mce: [Hardware Error]: Machine check events logged
[215386.990400] mce: [Hardware Error]: Machine check events logged
[215387.014403] mce: [Hardware Error]: Machine check events logged
[215387.014424] RAS: Soft-offlining pfn: 0x80fcb4
[215387.014438] EDAC MC0: 361 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.014591] Memory failure: 0x80fcb4: unhandlable page.
[215387.032973] mce: [Hardware Error]: Machine check events logged
[215387.033000] EDAC MC0: 140 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.053390] mce: [Hardware Error]: Machine check events logged
[215387.053411] RAS: Soft-offlining pfn: 0x166dca
[215387.053422] EDAC MC0: 66 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.053521] Memory failure: 0x166dca: unhandlable page.
[215387.076198] mce: [Hardware Error]: Machine check events logged
[215387.076217] EDAC MC0: 228 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.095887] mce: [Hardware Error]: Machine check events logged
[215387.095909] EDAC MC0: 292 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.120775] mce: [Hardware Error]: Machine check events logged
[215387.120794] RAS: Soft-offlining pfn: 0x165b98
[215387.120804] EDAC MC0: 20 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.121002] Memory failure: 0x165b98: unhandlable page.
[215387.141657] mce: [Hardware Error]: Machine check events logged
[215387.141712] EDAC MC0: 205 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.153921] mce: [Hardware Error]: Machine check events logged
[215387.177139] mce: [Hardware Error]: Machine check events logged
[215387.177169] EDAC MC0: 99 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.194418] mce: [Hardware Error]: Machine check events logged
[215387.194494] EDAC MC0: 861 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.224172] mce: [Hardware Error]: Machine check events logged
[215387.224198] EDAC MC0: 32283 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.252309] mce: [Hardware Error]: Machine check events logged
[215387.252338] RAS: Soft-offlining pfn: 0x80fd22
[215387.252347] EDAC MC0: 229 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.252622] Memory failure: 0x80fd22: unhandlable page.
[215387.274815] mce: [Hardware Error]: Machine check events logged
[215387.274841] EDAC MC0: 32730 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.298073] mce: [Hardware Error]: Machine check events logged
[215387.298217] EDAC MC0: 1231 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.324597] mce: [Hardware Error]: Machine check events logged
[215387.324626] EDAC MC0: 31700 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.349749] mce: [Hardware Error]: Machine check events logged
[215387.349765] RAS: Soft-offlining pfn: 0x166dca
[215387.349774] EDAC MC0: 226 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.350206] Memory failure: 0x166dca: unhandlable page.
[215387.363195] mce: [Hardware Error]: Machine check events logged
[215387.363218] EDAC MC0: 89 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.374683] mce: [Hardware Error]: Machine check events logged
[215387.374703] EDAC MC0: 103 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.384295] mce: [Hardware Error]: Machine check events logged
[215387.392273] mce: [Hardware Error]: Machine check events logged
[215387.392296] EDAC MC0: 508 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.404697] mce: [Hardware Error]: Machine check events logged
[215387.415614] mce: [Hardware Error]: Machine check events logged
[215387.422744] mce: [Hardware Error]: Machine check events logged
[215387.422770] EDAC MC0: 838 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.428473] mce: [Hardware Error]: Machine check events logged
[215387.428493] EDAC MC0: 180 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.438305] mce: [Hardware Error]: Machine check events logged
[215387.438324] EDAC MC0: 182 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.462687] mce: [Hardware Error]: Machine check events logged
[215387.462706] RAS: Soft-offlining pfn: 0x80fa9c
[215387.462718] EDAC MC0: 52 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.463454] Memory failure: 0x80fa9c: unhandlable page.
[215387.480739] mce: [Hardware Error]: Machine check events logged
[215387.480761] EDAC MC0: 5 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.497267] mce: [Hardware Error]: Machine check events logged
[215387.497287] RAS: Soft-offlining pfn: 0x166a1c
[215387.497299] EDAC MC0: 85 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.497481] Memory failure: 0x166a1c: unhandlable page.
[215387.511824] mce: [Hardware Error]: Machine check events logged
[215387.511842] EDAC MC0: 191 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.519310] mce: [Hardware Error]: Machine check events logged
[215387.540910] mce: [Hardware Error]: Machine check events logged
[215387.540933] EDAC MC0: 925 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.558719] mce: [Hardware Error]: Machine check events logged
[215387.558735] RAS: Soft-offlining pfn: 0x80fa9c
[215387.558745] EDAC MC0: 53 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.559126] Memory failure: 0x80fa9c: unhandlable page.
[215387.581026] mce: [Hardware Error]: Machine check events logged
[215387.581050] RAS: Soft-offlining pfn: 0x166dca
[215387.581059] EDAC MC0: 451 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.581204] Memory failure: 0x166dca: unhandlable page.
[215387.591268] mce: [Hardware Error]: Machine check events logged
[215387.592929] mce: [Hardware Error]: Machine check events logged
[215387.592958] EDAC MC0: 32723 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.600594] mce: [Hardware Error]: Machine check events logged
[215387.600615] EDAC MC0: 632 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.609805] mce: [Hardware Error]: Machine check events logged
[215387.609833] EDAC MC0: 44 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.618117] mce: [Hardware Error]: Machine check events logged
[215387.618135] EDAC MC0: 13 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.631154] mce: [Hardware Error]: Machine check events logged
[215387.631182] EDAC MC0: 172 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.645930] mce: [Hardware Error]: Machine check events logged
[215387.648285] EDAC MC0: 10805 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.671033] mce: [Hardware Error]: Machine check events logged
[215387.692776] mce: [Hardware Error]: Machine check events logged
[215387.708277] mce: [Hardware Error]: Machine check events logged
[215387.708300] EDAC MC0: 22731 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.727289] mce: [Hardware Error]: Machine check events logged
[215387.730267] EDAC MC0: 3194 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.749961] mce: [Hardware Error]: Machine check events logged
[215387.749996] EDAC MC0: 30257 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.766500] mce: [Hardware Error]: Machine check events logged
[215387.773628] mce: [Hardware Error]: Machine check events logged
[215387.779560] mce: [Hardware Error]: Machine check events logged
[215387.779576] RAS: Soft-offlining pfn: 0x80fa98
[215387.779590] EDAC MC0: 969 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.782300] Memory failure: 0x80fa98: unhandlable page.
[215387.782915] mce: [Hardware Error]: Machine check events logged
[215387.782935] EDAC MC0: 766 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.790350] mce: [Hardware Error]: Machine check events logged
[215387.790373] EDAC MC0: 32538 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.800853] mce: [Hardware Error]: Machine check events logged
[215387.808442] mce: [Hardware Error]: Machine check events logged
[215387.820209] mce: [Hardware Error]: Machine check events logged
[215387.820241] EDAC MC0: 861 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.830214] mce: [Hardware Error]: Machine check events logged
[215387.830239] EDAC MC0: 394 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.841570] mce: [Hardware Error]: Machine check events logged
[215387.841599] EDAC MC0: 2 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.861265] mce: [Hardware Error]: Machine check events logged
[215387.861290] EDAC MC0: 62 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.883311] mce: [Hardware Error]: Machine check events logged
[215387.883340] EDAC MC0: 221 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.903785] mce: [Hardware Error]: Machine check events logged
[215387.903803] EDAC MC0: 34 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.914460] mce: [Hardware Error]: Machine check events logged
[215387.914642] EDAC MC0: 1229 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.925270] mce: [Hardware Error]: Machine check events logged
[215387.925298] EDAC MC0: 32140 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.938787] mce: [Hardware Error]: Machine check events logged
[215387.939258] RAS: Soft-offlining pfn: 0x80fc18
[215387.939270] EDAC MC0: 1072 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.941280] Memory failure: 0x80fc18: unhandlable page.
[215387.952589] mce: [Hardware Error]: Machine check events logged
[215387.952607] RAS: Soft-offlining pfn: 0x80fb98
[215387.952616] EDAC MC0: 31988 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.952853] Memory failure: 0x80fb98: unhandlable page.
[215387.959768] mce: [Hardware Error]: Machine check events logged
[215387.959792] RAS: Soft-offlining pfn: 0x80fca2
[215387.959802] EDAC MC0: 1104 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.959846] Memory failure: 0x80fca2: unhandlable page.
[215387.965439] mce: [Hardware Error]: Machine check events logged
[215387.965466] RAS: Soft-offlining pfn: 0x166a1a
[215387.965483] EDAC MC0: 42 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.965667] Memory failure: 0x166a1a: unhandlable page.
[215387.982478] mce: [Hardware Error]: Machine check events logged
[215387.982501] RAS: Soft-offlining pfn: 0x166dca
[215387.982513] EDAC MC0: 32652 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215387.982672] Memory failure: 0x166dca: unhandlable page.
[215388.006322] mce: [Hardware Error]: Machine check events logged
[215388.030648] mce: [Hardware Error]: Machine check events logged
[215388.050937] mce: [Hardware Error]: Machine check events logged
[215388.050966] EDAC MC0: 806 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215388.071358] mce: [Hardware Error]: Machine check events logged
[215388.071380] EDAC MC0: 126 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215388.090921] mce: [Hardware Error]: Machine check events logged
[215388.090951] EDAC MC0: 32755 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215388.112076] mce: [Hardware Error]: Machine check events logged
[215388.112105] EDAC MC0: 20 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215388.134188] mce: [Hardware Error]: Machine check events logged
[215388.134216] EDAC MC0: 32 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215388.147964] mce: [Hardware Error]: Machine check events logged
[215388.147993] EDAC MC0: 60 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215388.172276] mce: [Hardware Error]: Machine check events logged
[215388.172305] EDAC MC0: 21 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215388.194785] mce: [Hardware Error]: Machine check events logged
[215388.194814] EDAC MC0: 27 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215388.217349] mce: [Hardware Error]: Machine check events logged
[215388.217377] EDAC MC0: 32762 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215388.240332] mce: [Hardware Error]: Machine check events logged
[215388.240359] EDAC MC0: 59 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215388.271399] mce: [Hardware Error]: Machine check events logged
[215388.302907] mce: [Hardware Error]: Machine check events logged
[215388.302936] EDAC MC0: 802 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215388.439242] bnx2 0000:04:00.0: VPD access failed.  This is likely a firmware bug on this device.  Contact the card vendor for a firmware update
[215388.445670] mce: [Hardware Error]: Machine check events logged
[215388.445690] EDAC MC0: 83 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215388.565235] bnx2 0000:04:00.1: VPD access failed.  This is likely a firmware bug on this device.  Contact the card vendor for a firmware update
[215388.583535] mce: [Hardware Error]: Machine check events logged
[215388.607504] mce: [Hardware Error]: Machine check events logged
[215388.607524] EDAC MC0: 96 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215388.615239] mce: [Hardware Error]: Machine check events logged
[215388.615272] RAS: Soft-offlining pfn: 0x165a08
[215388.615285] EDAC MC0: 18988 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215388.615612] Memory failure: 0x165a08: unhandlable page.
[215388.637011] mce: [Hardware Error]: Machine check events logged
[215388.637040] EDAC MC0: 23 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215388.674033] mce: [Hardware Error]: Machine check events logged
[215388.694305] mce: [Hardware Error]: Machine check events logged
[215388.716307] mce: [Hardware Error]: Machine check events logged
[215388.716330] EDAC MC0: 612 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215388.738773] mce: [Hardware Error]: Machine check events logged
[215388.738866] EDAC MC0: 504 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215388.765030] mce: [Hardware Error]: Machine check events logged
[215388.765066] EDAC MC0: 32625 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215388.786080] mce: [Hardware Error]: Machine check events logged
[215388.794757] mce: [Hardware Error]: Machine check events logged
[215388.794787] EDAC MC0: 636 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215388.809644] mce: [Hardware Error]: Machine check events logged
[215388.809676] EDAC MC0: 321 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215388.828736] mce: [Hardware Error]: Machine check events logged
[215388.847908] mce: [Hardware Error]: Machine check events logged
[215388.847935] EDAC MC0: 647 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215388.868297] mce: [Hardware Error]: Machine check events logged
[215388.868321] EDAC MC0: 217 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215388.891408] mce: [Hardware Error]: Machine check events logged
[215388.891432] EDAC MC0: 244 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215388.915240] mce: [Hardware Error]: Machine check events logged
[215388.915258] RAS: Soft-offlining pfn: 0x166dca
[215388.915269] EDAC MC0: 627 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215388.916233] Memory failure: 0x166dca: unhandlable page.
[215388.932542] mce: [Hardware Error]: Machine check events logged
[215388.948906] mce: [Hardware Error]: Machine check events logged
[215388.969613] mce: [Hardware Error]: Machine check events logged
[215388.969638] EDAC MC0: 398 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215388.985844] mce: [Hardware Error]: Machine check events logged
[215388.985876] EDAC MC0: 237 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215389.002867] mce: [Hardware Error]: Machine check events logged
[215389.004252] RAS: Soft-offlining pfn: 0x166dca
[215389.004268] EDAC MC0: 17305 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215389.005347] Memory failure: 0x166dca: unhandlable page.
[215389.007872] mce: [Hardware Error]: Machine check events logged
[215389.007888] EDAC MC0: 15766 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215389.026654] mce: [Hardware Error]: Machine check events logged
[215389.026678] EDAC MC0: 277 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215389.050074] mce: [Hardware Error]: Machine check events logged
[215389.050108] EDAC MC0: 416 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215389.067173] mce: [Hardware Error]: Machine check events logged
[215389.067194] EDAC MC0: 77 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215389.079486] mce: [Hardware Error]: Machine check events logged
[215389.095746] mce: [Hardware Error]: Machine check events logged
[215389.095911] EDAC MC0: 859 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215389.108224] mce: [Hardware Error]: Machine check events logged
[215389.141346] mce: [Hardware Error]: Machine check events logged
[215389.141363] RAS: Soft-offlining pfn: 0x80fb98
[215389.141372] EDAC MC0: 32452 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215389.143393] Memory failure: 0x80fb98: unhandlable page.
[215389.191620] mce: [Hardware Error]: Machine check events logged
[215389.191652] EDAC MC0: 36 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215389.232653] mce: [Hardware Error]: Machine check events logged
[215389.232681] EDAC MC0: 29 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215389.264832] mce: [Hardware Error]: Machine check events logged
[215389.264854] RAS: Soft-offlining pfn: 0x80fa9c
[215389.264865] EDAC MC0: 35 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215389.265009] Memory failure: 0x80fa9c: unhandlable page.
[215389.465823] mce: [Hardware Error]: Machine check events logged
[215389.465852] EDAC MC0: 45 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215389.575197] mce: [Hardware Error]: Machine check events logged
[215390.075337] mce: [Hardware Error]: Machine check events logged
[215390.075359] RAS: Soft-offlining pfn: 0x80fb18
[215390.075373] EDAC MC0: 8975 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215390.075554] Memory failure: 0x80fb18: unhandlable page.
[215390.151600] mce: [Hardware Error]: Machine check events logged
[215390.151629] EDAC MC0: 100 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215390.174598] mce: [Hardware Error]: Machine check events logged
[215390.191312] mce: [Hardware Error]: Machine check events logged
[215390.191331] EDAC MC0: 185 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215390.212310] mce: [Hardware Error]: Machine check events logged
[215390.212331] RAS: Soft-offlining pfn: 0x166dca
[215390.212344] EDAC MC0: 379 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215390.212653] Memory failure: 0x166dca: unhandlable page.
[215390.230016] mce: [Hardware Error]: Machine check events logged
[215390.230044] EDAC MC0: 43 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)
[215390.244550] mce: [Hardware Error]: Machine check events logged
[215390.244576] EDAC MC0: 268 CE error on CPU#0Channel#0_DIMM#0 (channel:0 slot:0 page:0x0 offset:0x0 grain:8 syndrome:0x0)

--- cpu MHz (live snapshot)
    $ grep -c ^processor /proc/cpuinfo
16

###############################################################################
# 5. MEMORY / NUMA / SWAP
###############################################################################

--- free -h
    $ free -h
               total        used        free      shared  buff/cache   available
Mem:           125Gi       8.0Gi       116Gi        55Mi       2.3Gi       117Gi
Swap:          8.0Gi          0B       8.0Gi

--- free -b
    $ free -b
               total        used        free      shared  buff/cache   available
Mem:     135158845440  8561524736 124873990144    58138624  2517229568 126597320704
Swap:     8589930496           0  8589930496

--- swapon
    $ swapon --show
NAME      TYPE      SIZE USED PRIO
/dev/dm-0 partition   8G   0B   -1

--- /proc/meminfo highlights
    $ grep -E MemTotal|MemFree|MemAvailable|Buffers|^Cached|SwapTotal|SwapFree|Hugepagesize|HugePages_Total|HugePages_Free|AnonHugePages|DirectMap|Slab|SReclaimable|SUnreclaim|Dirty|Writeback|AnonPages|Mapped|Shmem|KernelStack|PageTables|NFS_Unstable /proc/meminfo
MemTotal:       131991060 kB
MemFree:        121947160 kB
MemAvailable:   123630100 kB
Buffers:          176592 kB
Cached:          2221716 kB
SwapTotal:       8388604 kB
SwapFree:        8388604 kB
Dirty:             21864 kB
Writeback:             0 kB
AnonPages:       6831492 kB
Mapped:           246944 kB
Shmem:             56776 kB
Slab:             242492 kB
SReclaimable:      59924 kB
SUnreclaim:       182568 kB
KernelStack:        7280 kB
PageTables:        26672 kB
SecPageTables:      1148 kB
NFS_Unstable:          0 kB
WritebackTmp:          0 kB
AnonHugePages:   5349376 kB
ShmemHugePages:        0 kB
ShmemPmdMapped:        0 kB
FilePmdMapped:         0 kB
HugePages_Total:       0
HugePages_Free:        0
Hugepagesize:       2048 kB
DirectMap4k:      233956 kB
DirectMap2M:    133974016 kB

--- numa stat
    $ cat /proc/sys/vm/numa_stat
1

--- numa_balancing
    $ cat /proc/sys/kernel/numa_balancing
1

--- zone reclaim
    $ cat /proc/sys/vm/zone_reclaim_mode
0

--- slab top (top 20)
    $ slabtop -o -s c
 Active / Total Objects (% used)    : 744627 / 827427 (90.0%)
 Active / Total Slabs (% used)      : 19984 / 19984 (100.0%)
 Active / Total Caches (% used)     : 361 / 472 (76.5%)
 Active / Total Size (% used)       : 174823.59K / 196700.60K (88.9%)
 Minimum / Average / Maximum Object : 0.01K / 0.24K / 16.00K

  OBJS ACTIVE  USE OBJ SIZE  SLABS OBJ/SLAB CACHE SIZE NAME                   
170937 170908  99%    0.10K   4383       39     17532K buffer_head            
  8128   5348  65%    2.00K    508       16     16256K kmalloc-rnd-08-2k      
 11745  11702  99%    1.10K    405       29     12960K ext4_inode_cache       
 15596  15564  99%    0.57K    557       28      8912K radix_tree_node        
 58080  57118  98%    0.13K   1936       30      7744K kernfs_node_cache      
 34104  34089  99%    0.19K    812       42      6496K dentry                 
   543    541  99%   10.31K    181        3      5792K task_struct            
  7618   7604  99%    0.60K    293       26      4688K inode_cache            
 20832  18319  87%    0.19K    496       42      3968K vm_area_struct         
  7648   7646  99%    0.50K    239       32      3824K kmalloc-rnd-06-512     
  5452   4803  88%    0.67K    116       47      3712K proc_inode_cache       
  7360   7331  99%    0.50K    230       32      3680K kmalloc-rnd-02-512     
  1744    878  50%    2.00K    109       16      3488K kmalloc-cg-2k          
 29578  29481  99%    0.09K    643       46      2572K lsm_inode_cache        
  2240   2123  94%    1.00K     70       32      2240K kmalloc-rnd-03-1k      
 27888  22043  79%    0.07K    498       56      1992K vmap_area              
 31296  27249  87%    0.06K    489       64      1956K kmalloc-cg-64          
  2478   2267  91%    0.75K     59       42      1888K shmem_inode_cache      
   432    283  65%    4.00K     54        8      1728K kmalloc-cg-4k          
   400    393  98%    4.00K     50        8      1600K kmalloc-rnd-10-4k      
   765    756  98%    1.88K     45       17      1440K mem_cgroup_per_node    
  2848   2618  91%    0.50K     89       32      1424K kmalloc-rnd-03-512     
  2200   2093  95%    0.62K     88       25      1408K debugfs_inode_cache    
  1344   1308  97%    1.00K     42       32      1344K kmalloc-rnd-15-1k      
  5312   3476  65%    0.25K    166       32      1328K maple_node             
 18368  15228  82%    0.06K    287       64      1148K anon_vma_chain         
   560    552  98%    2.00K     35       16      1120K kmalloc-rnd-05-2k      
 10842   9302  85%    0.10K    278       39      1112K anon_vma               
   510    445  87%    2.06K     34       15      1088K sighand_cache          
   924    834  90%    1.12K     33       28      1056K signal_cache           
  1056    926  87%    1.00K     33       32      1056K kmalloc-cg-1k          
   512    456  89%    2.00K     32       16      1024K kmalloc-rnd-12-2k      
  1170    943  80%    0.81K     30       39       960K sock_inode_cache       
   420    410  97%    2.25K     30       14       960K mem_cgroup             
  1920   1697  88%    0.50K     60       32       960K pool_workqueue         
   112    112 100%    8.00K     28        4       896K kmalloc-8k             
  3488   3477  99%    0.25K    109       32       872K kmalloc-rnd-02-256     
  3456   1776  51%    0.25K    108       32       864K kmalloc-rnd-06-256     
  4452   3787  85%    0.19K    106       42       848K filp                   
   100     79  79%    8.00K     25        4       800K kmalloc-rnd-15-8k      
    96     86  89%    8.00K     24        4       768K kmalloc-cg-8k          
    96     94  97%    8.00K     24        4       768K kmalloc-rnd-10-8k      
   184    161  87%    4.00K     23        8       736K biovec-max             
   352    326  92%    2.00K     22       16       704K kmalloc-rnd-04-2k      
   168    148  88%    4.00K     21        8       672K kmalloc-rnd-04-4k      
  1280   1194  93%    0.50K     40       32       640K kmalloc-512            
   152    127  83%    4.00K     19        8       608K kmalloc-rnd-15-4k      
   152     86  56%    4.00K     19        8       608K kmalloc-rnd-13-4k      
  4800   2045  42%    0.12K    150       32       600K bio_integrity_data     
  2368   1879  79%    0.25K     74       32       592K bio-200                
   612    541  88%    0.94K     18       34       576K nfs_read_data          
   414    380  91%    1.38K     18       23       576K RAWv6                  
   216    129  59%    2.50K     18       12       576K TCPv6                  
   234    162  69%    2.38K     18       13       576K TCP                    
   576    508  88%    1.00K     18       32       576K kmalloc-rnd-04-1k      
  1120    814  72%    0.50K     35       32       560K kmalloc-cg-512         
  2940   1221  41%    0.19K     70       42       560K kmalloc-cg-192         
    51     49  96%    9.19K     17        3       544K kvm_vcpu               
   272    225  82%    2.00K     17       16       544K kmalloc-rnd-09-2k      
   272    246  90%    2.00K     17       16       544K kmalloc-2k             
    64     64 100%    8.00K     16        4       512K kmalloc-rnd-11-8k      
    64     64 100%    8.00K     16        4       512K kmalloc-rnd-08-8k      
    64     64 100%    8.00K     16        4       512K kmalloc-rnd-05-8k      
   390    376  96%    1.19K     15       26       480K RAW                    
   240    212  88%    2.00K     15       16       480K biovec-128             
   240    184  76%    2.00K     15       16       480K kmalloc-rnd-15-2k      
   120    120 100%    4.00K     15        8       480K kmalloc-rnd-07-4k      
   240    206  85%    2.00K     15       16       480K kmalloc-rnd-07-2k      
   960    762  79%    0.50K     30       32       480K kmalloc-rnd-07-512     
    60     56  93%    8.00K     15        4       480K kmalloc-rnd-04-8k      
  3808   1498  39%    0.12K    119       32       476K kmalloc-cg-128         
  2394   1296  54%    0.19K     57       42       456K kmalloc-rnd-11-192     
  4746   4642  97%    0.09K    113       42       452K kmalloc-rnd-01-96      
   252    174  69%    1.75K     14       18       448K mm_struct              
    56     51  91%    8.00K     14        4       448K kmalloc-rnd-12-8k      
  4620   4221  91%    0.09K    110       42       440K kmalloc-cg-96          
  1134   1106  97%    0.38K     27       42       432K mnt_cache              
  7884   7848  99%    0.05K    108       73       432K ftrace_event_field     
  1696    972  57%    0.25K     53       32       424K kmalloc-rnd-12-256     
   416    362  87%    1.00K     13       32       416K kmalloc-rnd-14-1k      
   208    183  87%    2.00K     13       16       416K kmalloc-rnd-13-2k      
   208    130  62%    2.00K     13       16       416K kmalloc-rnd-10-2k      
   416    311  74%    1.00K     13       32       416K kmalloc-rnd-07-1k      
   208    183  87%    2.00K     13       16       416K kmalloc-rnd-06-2k      
    52     52 100%    8.00K     13        4       416K kmalloc-rnd-02-8k      
   504    444  88%    0.75K     12       42       384K nfs_commit_data        
   192    192 100%    2.00K     12       16       384K memdup_user-2k         
   288    228  79%    1.32K     12       24       384K perf_event             
    96     92  95%    4.00K     12        8       384K kmalloc-rnd-08-4k      
   384    336  87%    1.00K     12       32       384K kmalloc-rnd-06-1k      
   192    124  64%    2.00K     12       16       384K kmalloc-rnd-03-2k      
   192    180  93%    2.00K     12       16       384K kmalloc-rnd-02-2k      
   192    192 100%    2.00K     12       16       384K kmalloc-rnd-01-2k      
  3008   2866  95%    0.12K     94       32       376K kmalloc-rnd-02-128     
  3822   3780  98%    0.09K     91       42       364K trace_event_file       
   121    118  97%    2.75K     11       11       352K x86_emulator           
   396    324  81%    0.88K     11       36       352K fuse_inode             
   506    296  58%    0.69K     11       46       352K skbuff_small_head      
  1848   1207  65%    0.19K     44       42       352K file_lock_cache        
   506    261  51%    0.69K     11       46       352K files_cache            
  1848   1598  86%    0.19K     44       42       352K pid                    
   352    344  97%    1.00K     11       32       352K kmalloc-rnd-11-1k      
   352    318  90%    1.00K     11       32       352K kmalloc-rnd-09-1k      
    88     83  94%    4.00K     11        8       352K kmalloc-rnd-05-4k      
   352    264  75%    1.00K     11       32       352K kmalloc-rnd-02-1k      
  2784   2032  72%    0.12K     87       32       348K eventpoll_epi          
   672    639  95%    0.50K     21       32       336K kmalloc-rnd-13-512     
  5248   4788  91%    0.06K     82       64       328K kmalloc-rnd-10-64      
   220    177  80%    1.44K     10       22       320K UDPv6                  
   470    385  81%    0.67K     10       47       320K taskstats              
   460    348  75%    0.69K     10       46       320K task_group             
   640    603  94%    0.50K     20       32       320K kmalloc-rnd-15-512     
   320    239  74%    1.00K     10       32       320K kmalloc-rnd-13-1k      
   320    256  80%    1.00K     10       32       320K kmalloc-rnd-10-1k      
    40     40 100%    8.00K     10        4       320K kmalloc-rnd-07-8k      
    80     74  92%    4.00K     10        8       320K kmalloc-rnd-06-4k      
   640    596  93%    0.50K     20       32       320K kmalloc-rnd-04-512     
  1716   1451  84%    0.18K     39       44       312K kvm_mmu_page_header    
  1184   1125  95%    0.25K     37       32       296K kmalloc-rnd-10-256     
   252    222  88%    1.12K      9       28       288K nfs_inode_cache        
   504    497  98%    0.56K     18       28       288K kioctx                 
   216    132  61%    1.31K      9       24       288K UDP                    
  1512   1473  97%    0.19K     36       42       288K proc_dir_entry         
    72     67  93%    4.00K      9        8       288K kmalloc-rnd-12-4k      
   576    500  86%    0.50K     18       32       288K kmalloc-rnd-10-512     
  1512   1459  96%    0.19K     36       42       288K kmalloc-rnd-07-192     
    72     64  88%    4.00K      9        8       288K kmalloc-rnd-02-4k      
    72     60  83%    4.00K      9        8       288K kmalloc-rnd-01-4k      
   288    262  90%    1.00K      9       32       288K kmalloc-rnd-01-1k      
  7038   6928  98%    0.04K     69      102       276K extent_status          
   544    480  88%    0.50K     17       32       272K kmalloc-rnd-09-512     
   544    308  56%    0.50K     17       32       272K kmalloc-rnd-05-512     
  1386   1304  94%    0.19K     33       42       264K kmalloc-192            
  1024    692  67%    0.25K     32       32       256K io_kiocb               
    64     64 100%    4.00K      8        8       256K memdup_user-4k         
   256    143  55%    1.00K      8       32       256K iommu_iova_magazine    
    64     62  96%    4.00K      8        8       256K kmalloc-rnd-14-4k      
   128    106  82%    2.00K      8       16       256K kmalloc-rnd-14-2k      
   256    239  93%    1.00K      8       32       256K kmalloc-rnd-12-1k      
    64     64 100%    4.00K      8        8       256K kmalloc-rnd-11-4k      
    64     64 100%    4.00K      8        8       256K kmalloc-rnd-09-4k      
   256    227  88%    1.00K      8       32       256K kmalloc-rnd-08-1k      
   256    216  84%    1.00K      8       32       256K kmalloc-rnd-05-1k      
   512    444  86%    0.50K     16       32       256K kmalloc-rnd-01-512     
    64     62  96%    4.00K      8        8       256K kmalloc-4k             
  1380    913  66%    0.17K     30       46       240K fuse_request           
   375    364  97%    0.63K     15       25       240K tracefs_inode_cache    
   480    447  93%    0.50K     15       32       240K kmalloc-rnd-12-512     
  2478   1972  79%    0.09K     59       42       236K kmalloc-rnd-02-96      
   928    746  80%    0.25K     29       32       232K nf_conntrack           
  2394   1946  81%    0.09K     57       42       228K kmalloc-rnd-10-96      
  1036    994  95%    0.21K     28       37       224K nfs_direct_cache       
   322    276  85%    0.69K      7       46       224K rpc_inode_cache        
   448    448 100%    0.50K     14       32       224K memdup_user-512        
   322    278  86%    0.69K      7       46       224K uts_namespace          
   448    421  93%    0.50K     14       32       224K kmalloc-rnd-11-512     
   896    760  84%    0.25K     28       32       224K kmalloc-rnd-04-256     
  1134   1076  94%    0.19K     27       42       216K kmalloc-rnd-15-192     
  1134    905  79%    0.19K     27       42       216K kmalloc-rnd-12-192     
  1134   1037  91%    0.19K     27       42       216K kmalloc-rnd-10-192     
  1092    809  74%    0.19K     26       42       208K jbd2_transaction_s     
   338    308  91%    0.61K     13       26       208K hugetlbfs_inode_cache  
   416    389  93%    0.50K     13       32       208K kmalloc-rnd-14-512     
   832    804  96%    0.25K     26       32       208K kmalloc-rnd-09-256     
   725    659  90%    0.27K     25       29       200K tw_sock_TCP            
  2100   2085  99%    0.09K     50       42       200K kmalloc-rcl-96         
   192    166  86%    1.00K      6       32       192K memdup_user-1k         
  1008    960  95%    0.19K     24       42       192K memdup_user-192        
   216    196  90%    0.88K      6       36       192K user_namespace         
   768    651  84%    0.25K     24       32       192K kmalloc-rnd-15-256     
  1008    960  95%    0.19K     24       42       192K kmalloc-rnd-14-192     
   384    290  75%    0.50K     12       32       192K kmalloc-rnd-08-512     
  1008    960  95%    0.19K     24       42       192K kmalloc-rnd-08-192     
  1008    970  96%    0.19K     24       42       192K kmalloc-rnd-06-192     
  1008    882  87%    0.19K     24       42       192K kmalloc-rnd-04-192     
   575    518  90%    0.31K     23       25       184K bio-256                
   966    675  69%    0.19K     23       42       184K kmalloc-rnd-13-192     
   966    914  94%    0.19K     23       42       184K kmalloc-rnd-03-192     
   924    758  82%    0.19K     22       42       176K bio-136                
   528    402  76%    0.32K     22       24       176K request_sock_TCP       
   704    564  80%    0.25K     22       32       176K key_jar                
   924    731  79%    0.19K     22       42       176K kmalloc-rnd-09-192     
   924    886  95%    0.19K     22       42       176K kmalloc-rnd-01-192     
  1376   1287  93%    0.12K     43       32       172K kmalloc-rnd-06-128     
   672    604  89%    0.25K     21       32       168K kmalloc-rnd-13-256     
   672    540  80%    0.25K     21       32       168K kmalloc-rnd-05-256     
   882    840  95%    0.19K     21       42       168K kmalloc-rnd-05-192     
   672    670  99%    0.25K     21       32       168K kmalloc-rnd-01-256     
  2688   2632  97%    0.06K     42       64       168K kmalloc-64             
   960    960 100%    0.16K     40       24       160K ext4_allocation_context
    20     19  95%    8.00K      5        4       160K kmalloc-rnd-14-8k      
  2560   2414  94%    0.06K     40       64       160K kmalloc-rnd-01-64      
  4992   4808  96%    0.03K     39      128       156K kmalloc-rnd-06-32      
   475    417  87%    0.31K     19       25       152K bio-264                
   608    365  60%    0.25K     19       32       152K skbuff_head_cache      
  1216   1116  91%    0.12K     38       32       152K kmalloc-rnd-09-128     
   798    571  71%    0.19K     19       42       152K kmalloc-rnd-02-192     
  2368   1792  75%    0.06K     37       64       148K kmalloc-rnd-06-64      
  2368   2262  95%    0.06K     37       64       148K kmalloc-rnd-02-64      
  1152   1135  98%    0.12K     36       32       144K kmalloc-rnd-07-128     
  1120   1031  92%    0.12K     35       32       140K kmalloc-rcl-128        
  1470   1455  98%    0.09K     35       42       140K kmalloc-96             
   493    415  84%    0.27K     17       29       136K tw_sock_TCPv6          
   544    543  99%    0.25K     17       32       136K kmalloc-cg-256         
   544    519  95%    0.25K     17       32       136K kmalloc-rnd-03-256     
   544    541  99%    0.25K     17       32       136K kmalloc-256            
   544    472  86%    0.25K     17       32       136K kmem_cache             
  1386   1317  95%    0.09K     33       42       132K kmalloc-rnd-07-96      
  8448   8072  95%    0.02K     33      256       132K kmalloc-rnd-06-16      
     8      8 100%   16.00K      4        2       128K zio_buf_comb_16384     
    76     60  78%    1.62K      4       19       128K bdev_cache             
   672    329  48%    0.19K     16       42       128K names_cache            
    64     48  75%    2.00K      4       16       128K kmalloc-rnd-11-2k      
   512    479  93%    0.25K     16       32       128K kmalloc-rnd-11-256     
   512    360  70%    0.25K     16       32       128K kmalloc-rnd-07-256     
   128     96  75%    1.00K      4       32       128K kmalloc-1k             
  1024    852  83%    0.12K     32       32       128K kmalloc-128            
   992    940  94%    0.12K     31       32       124K kmalloc-rnd-10-128     
   780    780 100%    0.15K     30       26       120K ext4_groupinfo_4k      
   960    923  96%    0.12K     30       32       120K kmalloc-rnd-14-128     
   960    934  97%    0.12K     30       32       120K kmalloc-rnd-11-128     
  1260   1012  80%    0.09K     30       42       120K kmalloc-rnd-09-96      
   960    888  92%    0.12K     30       32       120K kmalloc-rnd-04-128     
   960    949  98%    0.12K     30       32       120K kmalloc-rnd-03-128     
   960    944  98%    0.12K     30       32       120K kmem_cache_node        
  4930   3689  74%    0.02K     29      170       116K lsm_file_cache         
   928    900  96%    0.12K     29       32       116K kmalloc-rnd-15-128     
   928    892  96%    0.12K     29       32       116K kmalloc-rnd-01-128     
   448    448 100%    0.25K     14       32       112K ip6_dst_cache          
   952    778  81%    0.12K     28       34       112K jbd2_journal_head      
  1008    953  94%    0.11K     28       36       112K ext4_prealloc_space    
   952    676  71%    0.12K     28       34       112K seq_file               
  1428    916  64%    0.08K     28       51       112K sigqueue               
   448    389  86%    0.25K     14       32       112K kmalloc-rnd-14-256     
   448    405  90%    0.25K     14       32       112K kmalloc-rnd-08-256     
   896    723  80%    0.12K     28       32       112K kmalloc-rnd-05-128     
  1134   1080  95%    0.09K     27       42       108K kmalloc-rnd-06-96      
  1134   1079  95%    0.09K     27       42       108K kmalloc-rnd-05-96      
  1092    953  87%    0.09K     26       42       104K kmalloc-rnd-11-96      
   832    711  85%    0.12K     26       32       104K kmalloc-rnd-08-128     
  1050   1020  97%    0.09K     25       42       100K kmalloc-rnd-15-96      
  1050    914  87%    0.09K     25       42       100K kmalloc-rnd-04-96      
    45     36  80%    2.12K      3       15        96K MPTCPv6                
    99     84  84%    0.97K      3       33        96K request_queue          
    12     12 100%    8.00K      3        4        96K memdup_user-8k         
   384    336  87%    0.25K     12       32        96K memdup_user-256        
    15     11  73%    6.19K      3        5        96K net_namespace          
  1008    890  88%    0.09K     24       42        96K kmalloc-rnd-14-96      
  1008    953  94%    0.09K     24       42        96K kmalloc-rnd-12-96      
    12     12 100%    8.00K      3        4        96K kmalloc-rnd-09-8k      
  1008    936  92%    0.09K     24       42        96K kmalloc-rnd-03-96      
   966    686  71%    0.09K     23       42        92K kmalloc-rnd-13-96      
   736    540  73%    0.12K     23       32        92K kmalloc-rnd-12-128     
  1408   1007  71%    0.06K     22       64        88K kmalloc-rcl-64         
   462    420  90%    0.19K     11       42        88K kmalloc-rcl-192        
  1408   1302  92%    0.06K     22       64        88K kmalloc-rnd-14-64      
  1408   1259  89%    0.06K     22       64        88K kmalloc-rnd-07-64      
  1408   1255  89%    0.06K     22       64        88K kmalloc-rnd-05-64      
  1071    942  87%    0.08K     21       51        84K Acpi-State             
   672    596  88%    0.12K     21       32        84K kmalloc-rnd-13-128     
  1344   1270  94%    0.06K     21       64        84K kmalloc-rnd-09-64      
  1344   1202  89%    0.06K     21       64        84K kmalloc-rnd-08-64      
  1344   1176  87%    0.06K     21       64        84K kmalloc-rnd-04-64      
   125    112  89%    0.62K      5       25        80K netfs_request          
   840    824  98%    0.09K     20       42        80K kmalloc-rnd-08-96      
  2432   1955  80%    0.03K     19      128        76K kmalloc-cg-32          
  2432   1788  73%    0.03K     19      128        76K kmalloc-rnd-15-32      
   756    720  95%    0.09K     18       42        72K memdup_user-96         
   702    659  93%    0.10K     18       39        72K Acpi-ParseExt          
  1530   1487  97%    0.05K     18       85        72K shared_policy_node     
  1152   1093  94%    0.06K     18       64        72K kmalloc-rnd-12-64      
  1152    982  85%    0.06K     18       64        72K kmalloc-rnd-11-64      
  1152   1087  94%    0.06K     18       64        72K kmalloc-rnd-03-64      
  1088    587  53%    0.06K     17       64        68K dmaengine-unmap-2      
  1088    856  78%    0.06K     17       64        68K pidfs_attr_cache       
  1088    966  88%    0.06K     17       64        68K kmalloc-rnd-15-64      
  2176   1879  86%    0.03K     17      128        68K kmalloc-rnd-02-32      
    20     12  60%    3.16K      2       10        64K kcopyd_job             
    32     24  75%    2.00K      2       16        64K MPTCP                  
    84     56  66%    0.75K      2       42        64K dax_cache              
  1024    959  93%    0.06K     16       64        64K memdup_user-64         
    16     15  93%    4.00K      2        8        64K kmalloc-rnd-03-4k      
   960    761  79%    0.06K     15       64        60K ext4_io_end            
   960    900  93%    0.06K     15       64        60K kmalloc-rnd-13-64      
  7680   2641  34%    0.01K     15      512        60K kmalloc-rnd-12-8       
  1022    964  94%    0.05K     14       73        56K mb_cache_entry         
   784    707  90%    0.07K     14       56        56K nsproxy                
  1792   1704  95%    0.03K     14      128        56K kmalloc-rnd-13-32      
  1326   1279  96%    0.04K     13      102        52K fsnotify_inode_mark_connector
  6656   5891  88%    0.01K     13      512        52K kmalloc-rnd-06-8       
  1536   1469  95%    0.03K     12      128        48K kmalloc-rnd-14-32      
  1536   1023  66%    0.03K     12      128        48K kmalloc-rnd-01-32      
  2816   2498  88%    0.02K     11      256        44K kmalloc-rnd-13-16      
  1020    906  88%    0.04K     10      102        40K pde_opener             
  1280   1064  83%    0.03K     10      128        40K kmalloc-rnd-03-32      
  1152    880  76%    0.03K      9      128        36K ext4_io_end_vec        
  1152   1074  93%    0.03K      9      128        36K kmalloc-rnd-10-32      
  1152   1079  93%    0.03K      9      128        36K kmalloc-rnd-08-32      
  1152    896  77%    0.03K      9      128        36K kmalloc-rnd-07-32      
  1152   1018  88%    0.03K      9      128        36K kmalloc-rnd-05-32      
  1152    825  71%    0.03K      9      128        36K kmalloc-rnd-04-32      
  1152    958  83%    0.03K      9      128        36K kmalloc-32             
    50     28  56%    0.62K      2       25        32K kvm_gmem_inode_cache   
    34     28  82%    0.94K      1       34        32K mqueue_inode_cache     
   584    477  81%    0.05K      8       73        32K ip_fib_alias           
  1024    960  93%    0.03K      8      128        32K memdup_user-32         
    15     12  80%    2.06K      1       15        32K dmaengine-unmap-256    
    30     12  40%    1.06K      1       30        32K dmaengine-unmap-128    
  1024    914  89%    0.03K      8      128        32K kmalloc-rnd-12-32      
  1024    960  93%    0.03K      8      128        32K kmalloc-rnd-11-32      
  1024    976  95%    0.03K      8      128        32K kmalloc-rnd-09-32      
     4      4 100%    8.00K      1        4        32K kmalloc-rnd-03-8k      
     4      4 100%    8.00K      1        4        32K kmalloc-rnd-01-8k      
  1792   1154  64%    0.02K      7      256        28K kmalloc-cg-16          
   126    120  95%    0.19K      3       42        24K bio-176                
   768    637  82%    0.03K      6      128        24K pending_reservation    
   510    477  93%    0.05K      6       85        24K ip_fib_trie            
    75     56  74%    0.31K      3       25        24K bio-280                
  1536    779  50%    0.02K      6      256        24K ep_head                
  1536   1207  78%    0.02K      6      256        24K kmalloc-rnd-01-16      
  3072   1885  61%    0.01K      6      512        24K kmalloc-rnd-01-8       
  1280    960  75%    0.02K      5      256        20K memdup_user-16         
  1280    936  73%    0.02K      5      256        20K kmalloc-rnd-15-16      
  1280   1079  84%    0.02K      5      256        20K kmalloc-rnd-12-16      
  1280   1140  89%    0.02K      5      256        20K kmalloc-rnd-08-16      
  2560   2107  82%    0.01K      5      512        20K kmalloc-8              
    68     60  88%    0.23K      2       34        16K arc_buf_hdr_t_full     
    42     28  66%    0.38K      1       42        16K bio-328                
    36     28  77%    0.44K      1       36        16K bio-392                
    36     28  77%    0.44K      1       36        16K bio-408                
    36     28  77%    0.44K      1       36        16K bio-424                
  2048   1351  65%    0.01K      4      512        16K kmalloc-cg-8           
  1024    816  79%    0.02K      4      256        16K kmalloc-rnd-14-16      
  2048   1254  61%    0.01K      4      512        16K kmalloc-rnd-13-8       
  1024    959  93%    0.02K      4      256        16K kmalloc-rnd-11-16      
  1024    961  93%    0.02K      4      256        16K kmalloc-rnd-10-16      
  1024    928  90%    0.02K      4      256        16K kmalloc-rnd-09-16      
  2048    884  43%    0.01K      4      512        16K kmalloc-rnd-09-8       
  1024    958  93%    0.02K      4      256        16K kmalloc-rnd-07-16      
  1024    960  93%    0.02K      4      256        16K kmalloc-rnd-05-16      
  1024    780  76%    0.02K      4      256        16K kmalloc-rnd-04-16      
  1024    878  85%    0.02K      4      256        16K kmalloc-rnd-03-16      
  1024    959  93%    0.02K      4      256        16K kmalloc-rnd-02-16      
  1024    812  79%    0.02K      4      256        16K kmalloc-16             
    75     60  80%    0.16K      3       25        12K dm_bufio_buffer-16-1   
  1536    948  61%    0.01K      3      512        12K kmalloc-rnd-15-8       
  1536    918  59%    0.01K      3      512        12K kmalloc-rnd-03-8       
    84     60  71%    0.09K      2       42         8K abd_t                  
    64     64 100%    0.12K      2       32         8K scsi_sense_cache       
  1024    955  93%    0.01K      2      512         8K memdup_user-8          
    28     28 100%    0.28K      1       28         8K numa_policy            
    72     60  83%    0.11K      2       36         8K kmalloc_buckets        
  1024    890  86%    0.01K      2      512         8K kmalloc-rnd-14-8       
  1024    480  46%    0.01K      2      512         8K kmalloc-rnd-11-8       
  1024    957  93%    0.01K      2      512         8K kmalloc-rnd-10-8       
  1024    742  72%    0.01K      2      512         8K kmalloc-rnd-08-8       
  1024    960  93%    0.01K      2      512         8K kmalloc-rnd-07-8       
  1024    960  93%    0.01K      2      512         8K kmalloc-rnd-05-8       
  1024    771  75%    0.01K      2      512         8K kmalloc-rnd-04-8       
  1024    900  87%    0.01K      2      512         8K kmalloc-rnd-02-8       
   256     60  23%    0.02K      1      256         4K jbd2_revoke_table_s    
     0      0   0%    2.08K      0       15         0K nfs4_xattr_cache_cache 
     0      0   0%    0.23K      0       35         0K nf_conntrack_expect    
     0      0   0%    0.09K      0       46         0K zfs_znode_hold_cache   
     0      0   0%    1.08K      0       29         0K zfs_znode_cache        
     0      0   0%    1.03K      0       31         0K zap_attr_long_cache    
     0      0   0%    1.07K      0       29         0K zap_name_long          
     0      0   0%    0.28K      0       28         0K zap_attr_cache         
     0      0   0%    0.32K      0       24         0K zap_name               
     0      0   0%    0.16K      0       24         0K sio_cache_2            
     0      0   0%    0.15K      0       26         0K sio_cache_1            
     0      0   0%    0.13K      0       30         0K sio_cache_0            
     0      0   0%    0.15K      0       26         0K zil_zcw_cache          
     0      0   0%    0.38K      0       41         0K zil_lwb_cache          
     0      0   0%    0.37K      0       43         0K dbuf_dirty_record_t    
     0      0   0%    0.36K      0       44         0K dmu_buf_impl_t         
     0      0   0%    0.03K      0      128         0K arc_buf_t              
     0      0   0%    0.09K      0       42         0K arc_buf_hdr_t_l2only   
     0      0   0%    0.91K      0       35         0K dnode_t                
     0      0   0%    0.25K      0       32         0K sa_cache               
     0      0   0%   16.00K      0        2         0K lz4_cache              
     0      0   0%   12.00K      0        2         0K zio_buf_comb_12288     
     0      0   0%    8.00K      0        4         0K zio_buf_comb_8192      
     0      0   0%    6.00K      0        5         0K zio_buf_comb_6144      
     0      0   0%    4.00K      0        8         0K zio_buf_comb_4096      
     0      0   0%    3.00K      0       10         0K zio_buf_comb_3072      
     0      0   0%    2.00K      0       16         0K zio_buf_comb_2048      
     0      0   0%    1.50K      0       21         0K zio_buf_comb_1536      
     0      0   0%    1.00K      0       32         0K zio_buf_comb_1024      
     0      0   0%    0.50K      0       32         0K zio_buf_comb_512       
     0      0   0%    0.05K      0       85         0K zio_link_cache         
     0      0   0%    1.12K      0       28         0K zio_cache              
     0      0   0%    0.32K      0       24         0K ddt_log_entry_trad_cache
     0      0   0%    0.14K      0       28         0K ddt_log_entry_flat_cache
     0      0   0%    0.41K      0       38         0K ddt_entry_trad_cache   
     0      0   0%    0.23K      0       34         0K ddt_entry_flat_cache   
     0      0   0%    0.16K      0       24         0K brt_entry_cache        
     0      0   0%    0.07K      0       56         0K metaslab_alloc_trace_cache
     0      0   0%    4.00K      0        8         0K zfs_btree_leaf_cache   
     0      0   0%    0.06K      0       64         0K kcf_context_cache      
     0      0   0%    0.30K      0       26         0K btrfs_delayed_node     
     0      0   0%    0.41K      0       39         0K btrfs_ordered_extent   
     0      0   0%    0.23K      0       34         0K btrfs_extent_buffer    
     0      0   0%    0.98K      0       32         0K btrfs_inode            
     0      0   0%    0.27K      0       30         0K fsverity_info          
     0      0   0%    0.12K      0       32         0K fscrypt_inode_info     
     0      0   0%    0.39K      0       40         0K request_sock_subflow_v6
     0      0   0%    0.18K      0       44         0K ip6-frags              
     0      0   0%    1.38K      0       23         0K PINGv6                 
     0      0   0%    0.32K      0       24         0K request_sock_TCPv6     
     0      0   0%    2.82K      0       11         0K dm_uevent              
     0      0   0%    1.00K      0       32         0K ecryptfs_inode_cache   
     0      0   0%    0.02K      0      256         0K ecryptfs_file_cache    
     0      0   0%    0.75K      0       42         0K fat_inode_cache        
     0      0   0%    0.04K      0      102         0K fat_cache              
     0      0   0%    0.69K      0       46         0K squashfs_inode_cache   
     0      0   0%    0.19K      0       42         0K userfaultfd_ctx_cache  
     0      0   0%    0.11K      0       36         0K fanotify_perm_event    
     0      0   0%    0.03K      0      128         0K dnotify_struct         
     0      0   0%    0.62K      0       25         0K dio                    
     0      0   0%    0.01K      0      512         0K zs_handle              
     0      0   0%    0.56K      0       28         0K pid_namespace          
     0      0   0%    0.20K      0       40         0K ip4-frags              
     0      0   0%    0.39K      0       40         0K request_sock_subflow_v4
     0      0   0%    0.31K      0       25         0K xfrm_dst               
     0      0   0%    0.81K      0       39         0K xfrm_state             
     0      0   0%    1.06K      0       30         0K PING                   
     0      0   0%    0.25K      0       32         0K dquot                  
     0      0   0%    8.00K      0        4         0K msg_msg-8k             
     0      0   0%    4.00K      0        8         0K msg_msg-4k             
     0      0   0%    2.00K      0       16         0K msg_msg-2k             
     0      0   0%    1.00K      0       32         0K msg_msg-1k             
     0      0   0%    0.50K      0       32         0K msg_msg-512            
     0      0   0%    0.25K      0       32         0K msg_msg-256            
     0      0   0%    0.12K      0       32         0K msg_msg-128            
     0      0   0%    0.06K      0       64         0K msg_msg-64             
     0      0   0%    0.03K      0      128         0K msg_msg-32             
     0      0   0%    0.02K      0      256         0K msg_msg-16             
     0      0   0%    0.01K      0      512         0K msg_msg-8              
     0      0   0%    0.19K      0       42         0K msg_msg-192            
     0      0   0%    0.09K      0       42         0K msg_msg-96             
     0      0   0%    0.12K      0       32         0K memdup_user-128        
     0      0   0%    0.16K      0       25         0K file_lease_cache       
     0      0   0%    0.36K      0       44         0K task_delay_info        
     0      0   0%    0.02K      0      256         0K pidfs_xattr_cache      
     0      0   0%    0.25K      0       32         0K bfilp                  
     0      0   0%    0.10K      0       39         0K ima_iint_cache         
     0      0   0%    0.34K      0       47         0K apparmor_auditcache    
     0      0   0%    8.00K      0        4         0K dma-kmalloc-8k         
     0      0   0%    4.00K      0        8         0K dma-kmalloc-4k         
     0      0   0%    2.00K      0       16         0K dma-kmalloc-2k         
     0      0   0%    1.00K      0       32         0K dma-kmalloc-1k         
     0      0   0%    0.50K      0       32         0K dma-kmalloc-512        
     0      0   0%    0.25K      0       32         0K dma-kmalloc-256        
     0      0   0%    0.12K      0       32         0K dma-kmalloc-128        
     0      0   0%    0.06K      0       64         0K dma-kmalloc-64         
     0      0   0%    0.03K      0      128         0K dma-kmalloc-32         
     0      0   0%    0.02K      0      256         0K dma-kmalloc-16         
     0      0   0%    0.01K      0      512         0K dma-kmalloc-8          
     0      0   0%    0.19K      0       42         0K dma-kmalloc-192        
     0      0   0%    0.09K      0       42         0K dma-kmalloc-96         
     0      0   0%    8.00K      0        4         0K kmalloc-rcl-8k         
     0      0   0%    4.00K      0        8         0K kmalloc-rcl-4k         
     0      0   0%    2.00K      0       16         0K kmalloc-rcl-2k         
     0      0   0%    1.00K      0       32         0K kmalloc-rcl-1k         
     0      0   0%    0.50K      0       32         0K kmalloc-rcl-512        
     0      0   0%    0.25K      0       32         0K kmalloc-rcl-256        
     0      0   0%    0.03K      0      128         0K kmalloc-rcl-32         
     0      0   0%    0.02K      0      256         0K kmalloc-rcl-16         
     0      0   0%    0.01K      0      512         0K kmalloc-rcl-8          
     0      0   0%    8.00K      0        4         0K kmalloc-rnd-13-8k      
     0      0   0%    8.00K      0        4         0K kmalloc-rnd-06-8k      

--- kswapd stats
    $ grep -E kswapd|pgmigrate|pgmigrate_failed|compact_ /proc/vmstat
pgdemote_kswapd 0
pgsteal_kswapd 0
pgscan_kswapd 0
kswapd_inodesteal 0
kswapd_low_wmark_hit_quickly 0
kswapd_high_wmark_hit_quickly 0
pgmigrate_success 6439698
pgmigrate_fail 4132
compact_migrate_scanned 0
compact_free_scanned 0
compact_isolated 0
compact_stall 0
compact_fail 0
compact_success 0
compact_daemon_wake 0
compact_daemon_migrate_scanned 0
compact_daemon_free_scanned 0

###############################################################################
# 6. KERNEL TUNABLES / SYSCTL
###############################################################################

--- vm.* tunables
    $ sysctl -a 2>/dev/null | grep -E '^vm\.(dirty_(ratio|background_ratio|bytes|background_bytes|expire_centisecs|writeback_centisecs)|swappiness|vfs_cache_pressure|min_free_kbytes|watermark_scale_factor|overcommit_memory|overcommit_ratio|nr_hugepages|nr_overcommit_hugepages|zone_reclaim_mode|compact_unevictable_allowed|stat_interval|admin_reserve_kbytes|user_reserve_kbytes)'
vm.admin_reserve_kbytes = 8192
vm.compact_unevictable_allowed = 1
vm.dirty_background_bytes = 0
vm.dirty_background_ratio = 5
vm.dirty_bytes = 0
vm.dirty_expire_centisecs = 3000
vm.dirty_ratio = 40
vm.dirty_writeback_centisecs = 500
vm.min_free_kbytes = 90112
vm.nr_hugepages = 0
vm.nr_hugepages_mempolicy = 0
vm.nr_overcommit_hugepages = 0
vm.overcommit_memory = 0
vm.overcommit_ratio = 50
vm.stat_interval = 1
vm.swappiness = 10
vm.user_reserve_kbytes = 131072
vm.vfs_cache_pressure = 100
vm.vfs_cache_pressure_denom = 100
vm.watermark_scale_factor = 10
vm.zone_reclaim_mode = 0

--- fs.* tunables
    $ sysctl -a 2>/dev/null | grep -E '^fs\.(file-max|file-nr|aio-max-nr|aio-nr|nr_open|pipe-max-size|epoll/max_user_watches|lease-break-time|mqueue|max_user_ns)'
fs.aio-max-nr = 1048576
fs.aio-nr = 0
fs.file-max = 9223372036854775807
fs.file-nr = 3143	0	9223372036854775807
fs.lease-break-time = 45
fs.mqueue.msg_default = 10
fs.mqueue.msg_max = 10
fs.mqueue.msgsize_default = 8192
fs.mqueue.msgsize_max = 8192
fs.mqueue.queues_max = 256
fs.nr_open = 1073741816
fs.pipe-max-size = 1048576

--- kernel.* perf-relevant
    $ sysctl -a 2>/dev/null | grep -E '^kernel\.(sched_(child_runs_first|migration_cost|domain|rt_period|rt_runtime|idle)|numa_balancing|watchdog|nmi_watchdog|hung_task|randomize_va_space|max_pid|threads-max|sched_time_avg)'
kernel.hung_task_all_cpu_backtrace = 0
kernel.hung_task_check_count = 4194304
kernel.hung_task_check_interval_secs = 0
kernel.hung_task_detect_count = 0
kernel.hung_task_panic = 0
kernel.hung_task_sys_info = 
kernel.hung_task_timeout_secs = 120
kernel.hung_task_warnings = 10
kernel.nmi_watchdog = 1
kernel.numa_balancing = 1
kernel.numa_balancing_promote_rate_limit_MBps = 65536
kernel.randomize_va_space = 2
kernel.sched_rt_period_us = 1000000
kernel.sched_rt_runtime_us = 950000
kernel.threads-max = 959160
kernel.watchdog = 1
kernel.watchdog_cpumask = 0-15
kernel.watchdog_thresh = 10

###############################################################################
# 7. NETWORK SYSCTL / TCP
###############################################################################

--- net.core.* tunables
    $ sysctl -a 2>/dev/null | grep -E '^net\.core\.(rmem_default|rmem_max|wmem_default|wmem_max|optmem_max|somaxconn|netdev_max_backlog|netdev_budget|netdev_budget_usecs|netdev_tstamp_prequeue|rps_flow_cnt|busy_poll|busy_read|default_qdisc|dev_weight|xfrm)'
net.core.busy_poll = 0
net.core.busy_read = 0
net.core.default_qdisc = fq
net.core.dev_weight = 64
net.core.dev_weight_rx_bias = 1
net.core.dev_weight_tx_bias = 1
net.core.netdev_budget = 300
net.core.netdev_budget_usecs = 2000
net.core.netdev_max_backlog = 250000
net.core.netdev_tstamp_prequeue = 1
net.core.optmem_max = 131072
net.core.rmem_default = 26214400
net.core.rmem_max = 134217728
net.core.somaxconn = 65535
net.core.wmem_default = 26214400
net.core.wmem_max = 134217728
net.core.xfrm_acq_expires = 30
net.core.xfrm_aevent_etime = 10
net.core.xfrm_aevent_rseqth = 2
net.core.xfrm_larval_drop = 1

--- net.ipv4.tcp.* tunables
    $ sysctl -a 2>/dev/null | grep -E '^net\.ipv4\.tcp_(rmem|wmem|congestion_control|available_congestion_control|mtu_probing|slow_start_after_idle|no_metrics_save|timestamps|window_scaling|sack|low_latency|fastopen|ecn|ecn_fallback|syncookies|max_syn_backlog|tw_reuse|fin_timeout|keepalive_time|keepalive_probes|keepalive_intvl|thp_linear_timeouts|pacing|pacing_ss_ratio|pacing_ca_ratio|no_ssthresh_metrics_save|md5sig|abort_on_overflow|buffer_split)'
net.ipv4.tcp_abort_on_overflow = 0
net.ipv4.tcp_available_congestion_control = reno cubic bbr
net.ipv4.tcp_congestion_control = bbr
net.ipv4.tcp_ecn = 2
net.ipv4.tcp_ecn_fallback = 1
net.ipv4.tcp_ecn_option = 2
net.ipv4.tcp_ecn_option_beacon = 3
net.ipv4.tcp_fastopen = 1
net.ipv4.tcp_fastopen_blackhole_timeout_sec = 0
net.ipv4.tcp_fastopen_key = 00000000-00000000-00000000-00000000
net.ipv4.tcp_fin_timeout = 60
net.ipv4.tcp_keepalive_intvl = 75
net.ipv4.tcp_keepalive_probes = 9
net.ipv4.tcp_keepalive_time = 7200
net.ipv4.tcp_low_latency = 0
net.ipv4.tcp_max_syn_backlog = 4096
net.ipv4.tcp_mtu_probing = 0
net.ipv4.tcp_no_metrics_save = 0
net.ipv4.tcp_no_ssthresh_metrics_save = 1
net.ipv4.tcp_pacing_ca_ratio = 120
net.ipv4.tcp_pacing_ss_ratio = 200
net.ipv4.tcp_rmem = 4096	87380	134217728
net.ipv4.tcp_sack = 1
net.ipv4.tcp_slow_start_after_idle = 1
net.ipv4.tcp_syncookies = 1
net.ipv4.tcp_timestamps = 1
net.ipv4.tcp_tw_reuse = 2
net.ipv4.tcp_tw_reuse_delay = 1000
net.ipv4.tcp_window_scaling = 1
net.ipv4.tcp_wmem = 4096	65536	134217728

--- other net.* sysctls
    $ sysctl -a 2>/dev/null | grep -E '^net\.(ipv4\.ip_(local_port_range|local_reserved_ports|no_pmtu_disc|forwarding)|ipv4\.conf\.all\.(rp_filter|accept_redirects|send_redirects)|ipv4\.conf\.default\.forwarding|core\.netdev_budget|ipv6\.conf\.all\.disable_ipv6)'
net.core.netdev_budget = 300
net.core.netdev_budget_usecs = 2000
net.ipv4.conf.all.accept_redirects = 1
net.ipv4.conf.all.rp_filter = 2
net.ipv4.conf.all.send_redirects = 1
net.ipv4.conf.default.forwarding = 0
net.ipv4.ip_local_port_range = 32768	60999
net.ipv4.ip_local_reserved_ports = 
net.ipv4.ip_no_pmtu_disc = 0
net.ipv6.conf.all.disable_ipv6 = 0

--- sysctl.d
total 16
drwxr-xr-x   2 root root 4096 Jul 26 15:44 .
drwxr-xr-x 107 root root 4096 Jul 29 05:07 ..
-rw-r--r--   1 root root  499 Jul 26 15:45 99-perfopt.conf
-rw-r--r--   1 root root  269 Jul 30  2025 README.sysctl

--- /etc/sysctl.conf
    [missing: /etc/sysctl.conf]

--- non-default sysctl values (sorted, filtered)
    $ # Show only sysctls that differ from running state vs an empty config;
# too noisy to dump all of /proc/sys. Just show /etc/sysctl.d content.
for f in /etc/sysctl.d/*.conf /etc/sysctl.conf; do
    [ -r "$f" ] || continue
    echo "=== $f ==="
    grep -vE '^\s*#|^\s*$' "$f" 2>/dev/null
done
=== /etc/sysctl.d/99-perfopt.conf ===
vm.swappiness = 10
net.ipv4.tcp_congestion_control = bbr
net.core.default_qdisc = fq
net.core.rmem_max = 134217728
net.core.wmem_max = 134217728
net.core.rmem_default = 26214400
net.core.wmem_default = 26214400
net.core.netdev_max_backlog = 250000
net.core.somaxconn = 65535
net.ipv4.tcp_rmem = 4096 87380 134217728
net.ipv4.tcp_wmem = 4096 65536 134217728

###############################################################################
# 8. tuned / irqbalance / udev
###############################################################################

--- tuned-adm active
    $ tuned-adm active
Current active profile: virtual-host

--- tuned-adm list
    $ tuned-adm list
Available profiles:
- accelerator-performance     - Throughput performance based tuning with disabled higher latency STOP states
- atomic-guest                - Optimize virtual guests based on the Atomic variant
- atomic-host                 - Optimize bare metal systems running the Atomic variant
- aws                         - Optimize for aws ec2 instances
- balanced                    - General non-specialized tuned profile
- balanced-battery            - Balanced profile biased towards power savings changes for battery
- cpu-partitioning            - Optimize for CPU partitioning
- cpu-partitioning-powersave  - Optimize for CPU partitioning with additional powersave
- default                     - Legacy default tuned profile
- desktop                     - Optimize for the desktop use-case
- desktop-powersave           - Optmize for the desktop use-case with power saving
- enterprise-storage          - Legacy profile for RHEL6, for RHEL7, please use throughput-performance profile
- hpc-compute                 - Optimize for HPC compute workloads
- intel-sst                   - Configure for Intel Speed Select Base Frequency
- laptop-ac-powersave         - Optimize for laptop with power savings
- laptop-battery-powersave    - Optimize laptop profile with more aggressive power saving
- latency-performance         - Optimize for deterministic performance at the cost of increased power consumption
- mssql                       - Optimize for Microsoft SQL Server
- network-latency             - Optimize for deterministic performance at the cost of increased power consumption, focused on low latency network performance
- network-throughput          - Optimize for streaming network throughput, generally only necessary on older CPUs or 40G+ networks
- openshift                   - Optimize systems running OpenShift (parent profile)
- openshift-control-plane     - Optimize systems running OpenShift control plane
- openshift-node              - Optimize systems running OpenShift nodes
- optimize-serial-console     - Optimize for serial console use.
- oracle                      - Optimize for Oracle RDBMS
- postgresql                  - Optimize for PostgreSQL server
- powersave                   - Optimize for low power consumption
- realtime                    - Optimize for realtime workloads
- realtime-virtual-guest      - Optimize for realtime workloads running within a KVM guest
- realtime-virtual-host       - Optimize for KVM guests running realtime workloads
- sap-hana                    - Optimize for SAP HANA
- sap-hana-kvm-guest          - Optimize for running SAP HANA on KVM inside a virtual guest
- sap-netweaver               - Optimize for SAP NetWeaver
- server-powersave            - Optimize for server power savings
- spectrumscale-ece           - Optimized for Spectrum Scale Erasure Code Edition Servers
- spindown-disk               - Optimize for power saving by spinning-down rotational disks
- throughput-performance      - Broadly applicable tuning that provides excellent performance across a variety of common server workloads
- virtual-guest               - Optimize for running inside a virtual guest
- virtual-host                - Optimize for running KVM guests
Current active profile: virtual-host

--- systemctl is-active tuned
    $ systemctl is-active tuned
active

--- irqbalance status
    $ systemctl is-active irqbalance
inactive
    [exit=4 / not installed or not permitted]

--- irqbalance config
    [missing: /etc/default/irqbalance]
    [missing: /etc/irqbalance.conf]

--- modprobe.d
total 20
drwxr-xr-x   2 root root 4096 Jul 26 17:13 .
drwxr-xr-x 107 root root 4096 Jul 29 05:07 ..
-rw-r--r--   1 root root  154 Oct 18  2025 intel-microcode-blacklist.conf
-rw-r--r--   1 root root  172 Nov 18  2025 pve-blacklist.conf
-rw-r--r--   1 root root    0 Apr  6 09:43 tuned.conf
-rw-r--r--   1 root root   36 Apr  4 12:32 zfs.conf

--- udev rules.d
total 8
drwxr-xr-x 2 root root 4096 Apr  4 12:31 .
drwxr-xr-x 4 root root 4096 Jul 26 11:25 ..
lrwxrwxrwx 1 root root    9 Apr  4 12:31 60-bridge-network-interface.rules -> /dev/null

--- modprobe.d files
    --- /etc/modprobe.d/intel-microcode-blacklist.conf ---
# The microcode module attempts to apply a microcode update when
# it autoloads.  This is not always safe, so we block it by default.
blacklist microcode
    --- /etc/modprobe.d/pve-blacklist.conf ---
# This file contains a list of modules which are not supported by Proxmox VE 

# nvidiafb see bugreport https://bugzilla.proxmox.com/show_bug.cgi?id=701
blacklist nvidiafb
    --- /etc/modprobe.d/tuned.conf ---
    --- /etc/modprobe.d/zfs.conf ---
options zfs zfs_arc_max=13515096064

--- module params: kvm_intel
    $ for p in /sys/module/kvm_intel/parameters/*; do
    [ -e "$p" ] && printf '  %s = %s\n' "$(basename "$p")" "$(cat "$p" 2>/dev/null)"
done
  allow_smaller_maxphyaddr = N
  dump_invalid_vmcs = N
  emulate_invalid_guest_state = Y
  enable_apicv = N
  enable_device_posted_irqs = N
  enable_ipiv = N
  enable_mediated_pmu = N
  enable_shadow_vmcs = N
  enlightened_vmcs = N
  ept = Y
  eptad = N
  error_on_inconsistent_vmcs_config = Y
  fasteoi = Y
  flexpriority = Y
  mbec = N
  nested = Y
  ple_gap = 0
  ple_window = 0
  ple_window_grow = 0
  ple_window_max = 0
  ple_window_shrink = 0
  pml = N
  preemption_timer = N
  sgx = N
  tdx = N
  unrestricted_guest = N
  vmentry_l1d_flush = cond
  vnmi = Y
  vpid = Y
  warn_on_missed_cc = N

--- module params: kvm_amd
    $ for p in /sys/module/kvm_amd/parameters/*; do
    [ -e "$p" ] && printf '  %s = %s\n' "$(basename "$p")" "$(cat "$p" 2>/dev/null)"
done
    [exit=1]

--- module params: relevant net drivers
    $ for mod in i40e ixgbe mlx5_core igb ice bnx2x virtio_net; do
    [ -d "/sys/module/$mod/parameters" ] || continue
    echo "=== $mod ==="
    for p in /sys/module/$mod/parameters/*; do
        [ -e "$p" ] && printf '  %s = %s\n' "$(basename "$p")" "$(cat "$p" 2>/dev/null)"
    done
done
=== virtio_net ===
  csum = Y
  gso = Y
  napi_tx = Y
  napi_weight = 64

###############################################################################
# 9. PROXMOX VERSION & CLUSTER
###############################################################################

--- pveversion
    $ pveversion
pve-manager/9.2.5/20242970da7fbcef (running kernel: 7.0.14-6-pve)

--- pveversion -v
    $ pveversion -v
proxmox-ve: 9.2.0 (running kernel: 7.0.14-6-pve)
pve-manager: 9.2.5 (running version: 9.2.5/20242970da7fbcef)
proxmox-kernel-helper: 9.2.0
proxmox-kernel-7.0.14-6-pve-signed: 7.0.14-6
proxmox-kernel-7.0: 7.0.14-6
proxmox-kernel-6.17.13-19-pve-signed: 6.17.13-19
proxmox-kernel-6.17: 6.17.13-19
proxmox-kernel-6.17.2-1-pve-signed: 6.17.2-1
ceph-fuse: 19.2.3-pve2
corosync: 3.1.10-pve3
criu: 4.1.1-1
frr-pythontools: 10.6.1-1+pve2
ifupdown2: 3.3.0-1+pmx12
intel-microcode: 3.20251111.1~deb13u1
ksm-control-daemon: 1.5-1
libjs-extjs: 7.0.0-5
libproxmox-acme-perl: 1.7.1
libproxmox-backup-qemu0: 2.0.2
libproxmox-rs-perl: 0.4.1
libpve-access-control: 9.1.1
libpve-apiclient-perl: 3.4.2
libpve-cluster-api-perl: 9.1.6
libpve-cluster-perl: 9.1.6
libpve-common-perl: 9.1.19
libpve-guest-common-perl: 6.0.5
libpve-http-server-perl: 6.0.5
libpve-network-perl: 1.6.7
libpve-notify-perl: 9.1.6
libpve-rs-perl: 0.15.3
libpve-storage-perl: 9.1.6
libspice-server1: 0.15.2-1+b1
lvm2: 2.03.31-2+pmx1
lxc-pve: 7.0.0-2
lxcfs: 7.0.0-pve1
novnc-pve: 1.7.0-2
proxmox-backup-client: 4.2.3-1
proxmox-backup-file-restore: 4.2.3-1
proxmox-backup-restore-image: 1.0.0
proxmox-firewall: 1.2.3
proxmox-kernel-helper: 9.2.0
proxmox-mail-forward: 1.0.3
proxmox-mini-journalreader: 1.7
proxmox-offline-mirror-helper: 0.7.4
proxmox-widget-toolkit: 5.2.6
pve-cluster: 9.1.6
pve-container: 6.1.12
pve-docs: 9.2.3
pve-edk2-firmware: 4.2025.05-2
pve-esxi-import-tools: 1.0.1
pve-firewall: 6.0.5
pve-firmware: 3.18-5
pve-ha-manager: 5.2.4
pve-i18n: 3.9.0
pve-qemu-kvm: 11.0.2-2
pve-xtermjs: 6.0.0-2
qemu-server: 9.2.1
smartmontools: 7.5-pve2
spiceterm: 3.4.2
swtpm: 0.8.0+pve3
vncterm: 1.9.2
zfsutils-linux: 2.4.3-pve1

--- pvecm status
    $ pvecm status
Error: Corosync config '/etc/pve/corosync.conf' does not exist - is this node part of a cluster?
    [exit=2 / not installed or not permitted]

--- pvecm nodes
    $ pvecm nodes
Error: Corosync config '/etc/pve/corosync.conf' does not exist - is this node part of a cluster?
    [exit=2 / not installed or not permitted]

--- pvecm expected
    $ pvecm expected
400 not enough arguments
pvecm expected <expected>
    [exit=255 / not installed or not permitted]

--- pveperf
    $ timeout 15 pveperf
CPU BOGOMIPS:      76604.00
REGEX/SECOND:      1558527
HD SIZE:           93.93 GB (/dev/mapper/pve-root)
BUFFERED READS:    11.17 MB/sec
AVERAGE SEEK TIME: 36.46 ms
FSYNCS/SECOND:     2.33
    [exit=124 / not installed or not permitted]

--- corosync.conf
    [missing: /etc/pve/corosync.conf]

--- datacenter.cfg
    --- /etc/pve/datacenter.cfg ---
keyboard: en-us

--- storage.cfg
    --- /etc/pve/storage.cfg ---
dir: local
	path /var/lib/vz
	content iso,vztmpl,backup,import

lvmthin: local-lvm
	thinpool data
	vgname pve
	content rootdir,images


nfs: D2
	options nconnect=4,noatime
        export /mnt/tsys4/D2
        path /mnt/pve/D2
        server pfv-tsys4-nfs-stor
        content images
        prune-backups keep-all=1

nfs: D3
	options nconnect=4,noatime
        export /mnt/tsys4/D3
        path /mnt/pve/D3
        server pfv-tsys4-nfs-stor
        content images
        prune-backups keep-all=1

nfs: D5
	options nconnect=4,noatime
        export /mnt/tsys4/D5
        path /mnt/pve/D5
        server pfv-tsys4-nfs-stor
        content images
        prune-backups keep-all=1

nfs: S2
	options nconnect=4,noatime
        export /mnt/pfv-tsys5/S2
        path /mnt/pve/S2
        server pfv-tsys5-nfs-stor
        content images
        prune-backups keep-all=1

nfs: S3
	options nconnect=4,noatime
        export /mnt/pfv-tsys5/S3
        path /mnt/pve/S3
        server pfv-tsys5-nfs-stor
        content images
        prune-backups keep-all=1

nfs: S4
	options nconnect=4,noatime
        export /mnt/pfv-tsys5/S4
        path /mnt/pve/S4
        server pfv-tsys5-nfs-stor
        content images
        prune-backups keep-all=1

nfs: T5-SSD
	options nconnect=4,noatime
        export /mnt/pfv-tsys5/ssd
        path /mnt/pve/T5-SSD
        server pfv-tsys5-nfs-stor
        content images
        prune-backups keep-all=1


--- user.cfg
    --- /etc/pve/user.cfg ---
user:root@pam:1:0:::coo@turnsys.com::x:
token:root@pam!pdm-admin-tsys-proxmox-datacenter:0:0:auto-generated by PDM host 'tsys-proxmox-datacenter' on Mon, 06 Apr 2026 10%3A36%3A34 -0500:





--- domains.cfg
    [missing: /etc/pve/domains.cfg]

--- cluster resources (compact)
    $ pvesh get /cluster/resources --type node --output-format json 2>/dev/null \
  | jq -r '.[] | "\(.node)\tcpu=\(.cpu)\tmem=\(.mem)\tmaxmem=\(.maxmem)\tmaxdisk=\(.maxdisk)\tstatus=\(.status)\tssl_fingerprint=\(.ssl_fingerprint)"' 2>/dev/null \
  || pvesh get /cluster/resources --type node 2>/dev/null
pfv-tsys6	cpu=0.0118144592871048	mem=8510283776	maxmem=135158845440	maxdisk=100861726720	status=online	ssl_fingerprint=null

###############################################################################
# 10. NETWORK: INTERFACES
###############################################################################

--- ip -d link
    $ ip -d link
1: lo: <LOOPBACK,UP,LOWER_UP> mtu 65536 qdisc noqueue state UNKNOWN mode DEFAULT group default qlen 1000
    link/loopback 00:00:00:00:00:00 brd 00:00:00:00:00:00 promiscuity 0 allmulti 0 minmtu 0 maxmtu 0 addrgenmode eui64 numtxqueues 1 numrxqueues 1 gso_max_size 65536 gso_max_segs 65535 tso_max_size 524280 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 
2: nic0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc mq master vmbr0 state UP mode DEFAULT group default qlen 1000
    link/ether 00:21:9b:a2:7c:53 brd ff:ff:ff:ff:ff:ff promiscuity 1 allmulti 1 minmtu 46 maxmtu 9000 
    bridge_slave state forwarding priority 32 cost 5 hairpin off guard off root_block off fastleave off learning on flood on port_id 0x8001 port_no 0x1 designated_port 32769 designated_cost 0 designated_bridge 8000.0:21:9b:a2:7c:53 designated_root 8000.0:21:9b:a2:7c:53 hold_timer    0.00 message_age_timer    0.00 forward_delay_timer    0.00 topology_change_ack 0 config_pending 0 proxy_arp off proxy_arp_wifi off mcast_router 1 mcast_fast_leave off mcast_flood on bcast_flood on mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off group_fwd_mask 0 group_fwd_mask_str 0x0 vlan_tunnel off isolated off locked off mab off addrgenmode eui64 numtxqueues 8 numrxqueues 8 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 parentbus pci parentdev 0000:01:00.0 
    altname enp1s0f0
    altname enx00219ba27c53
3: nic1: <BROADCAST,MULTICAST,SLAVE,UP,LOWER_UP> mtu 1500 qdisc mq master bond0 state UP mode DEFAULT group default qlen 1000
    link/ether 00:21:9b:a2:7c:55 brd ff:ff:ff:ff:ff:ff promiscuity 1 allmulti 1 minmtu 46 maxmtu 9000 
    bond_slave state ACTIVE mii_status UP link_failure_count 0 perm_hwaddr 00:21:9b:a2:7c:55 queue_id 0 prio 0 ad_aggregator_id 1 ad_actor_oper_port_state 61 ad_actor_oper_port_state_str <active,aggregating,in_sync,collecting,distributing> ad_partner_oper_port_state 61 ad_partner_oper_port_state_str <active,aggregating,in_sync,collecting,distributing> addrgenmode eui64 numtxqueues 8 numrxqueues 8 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 parentbus pci parentdev 0000:01:00.1 
    altname enp1s0f1
    altname enx00219ba27c55
4: nic2: <BROADCAST,MULTICAST,SLAVE,UP,LOWER_UP> mtu 1500 qdisc mq master bond0 state UP mode DEFAULT group default qlen 1000
    link/ether 00:21:9b:a2:7c:55 brd ff:ff:ff:ff:ff:ff permaddr 00:21:9b:a2:7c:57 promiscuity 1 allmulti 1 minmtu 46 maxmtu 9000 
    bond_slave state ACTIVE mii_status UP link_failure_count 0 perm_hwaddr 00:21:9b:a2:7c:57 queue_id 0 prio 0 ad_aggregator_id 1 ad_actor_oper_port_state 61 ad_actor_oper_port_state_str <active,aggregating,in_sync,collecting,distributing> ad_partner_oper_port_state 61 ad_partner_oper_port_state_str <active,aggregating,in_sync,collecting,distributing> addrgenmode eui64 numtxqueues 8 numrxqueues 8 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 parentbus pci parentdev 0000:02:00.0 
    altname enp2s0f0
    altname enx00219ba27c57
5: nic3: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc mq state UP mode DEFAULT group default qlen 1000
    link/ether 00:21:9b:a2:7c:59 brd ff:ff:ff:ff:ff:ff promiscuity 1 allmulti 1 minmtu 46 maxmtu 9000 addrgenmode eui64 numtxqueues 8 numrxqueues 8 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 parentbus pci parentdev 0000:02:00.1 
    altname enp2s0f1
    altname enx00219ba27c59
6: nic4: <BROADCAST,MULTICAST> mtu 1500 qdisc noop state DOWN mode DEFAULT group default qlen 1000
    link/ether 00:10:18:72:16:40 brd ff:ff:ff:ff:ff:ff promiscuity 0 allmulti 0 minmtu 46 maxmtu 9000 addrgenmode eui64 numtxqueues 8 numrxqueues 8 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 parentbus pci parentdev 0000:04:00.0 
    altname enx001018721640
7: nic5: <BROADCAST,MULTICAST> mtu 1500 qdisc noop state DOWN mode DEFAULT group default qlen 1000
    link/ether 00:10:18:72:16:42 brd ff:ff:ff:ff:ff:ff promiscuity 0 allmulti 0 minmtu 46 maxmtu 9000 addrgenmode eui64 numtxqueues 8 numrxqueues 8 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 parentbus pci parentdev 0000:04:00.1 
    altname enx001018721642
8: vmbr0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000
    link/ether 00:21:9b:a2:7c:53 brd ff:ff:ff:ff:ff:ff promiscuity 0 allmulti 0 minmtu 68 maxmtu 65535 
    bridge forward_delay 0 hello_time 200 max_age 2000 ageing_time 30000 stp_state 0 priority 32768 vlan_filtering 0 vlan_protocol 802.1Q bridge_id 8000.0:21:9b:a2:7c:53 designated_root 8000.0:21:9b:a2:7c:53 root_port 0 root_path_cost 0 topology_change 0 topology_change_detected 0 hello_timer    0.00 tcn_timer    0.00 topology_change_timer    0.00 gc_timer    0.00 fdb_n_learned 106 fdb_max_learned 0 vlan_default_pvid 1 vlan_stats_enabled 0 vlan_stats_per_port 0 group_fwd_mask 0 group_address 01:80:c2:00:00:00 mcast_snooping 1 no_linklocal_learn 0 mcast_vlan_snooping 0 mst_enabled 0 mcast_router 1 mcast_query_use_ifaddr 0 mcast_querier 0 mcast_querier_ipv4_addr 0.0.0.0 mcast_querier_ipv4_port 2 mcast_querier_ipv4_other_timer 19.7us mcast_hash_elasticity 16 mcast_hash_max 4096 mcast_last_member_count 2 mcast_startup_query_count 2 mcast_last_member_interval 100 mcast_membership_interval 26000 mcast_querier_interval 25500 mcast_query_interval 12500 mcast_query_response_interval 1000 mcast_startup_query_interval 3125 mcast_stats_enabled 0 mcast_igmp_version 2 mcast_mld_version 1 nf_call_iptables 0 nf_call_ip6tables 0 nf_call_arptables 0 addrgenmode eui64 numtxqueues 1 numrxqueues 1 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 
9: tailscale0: <POINTOPOINT,MULTICAST,NOARP,UP,LOWER_UP> mtu 1280 qdisc fq state UNKNOWN mode DEFAULT group default qlen 500
    link/none  promiscuity 0 allmulti 0 minmtu 68 maxmtu 65535 
    tun type tun pi off vnet_hdr on persist off addrgenmode random numtxqueues 1 numrxqueues 1 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 
10: nic3.2@nic3: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master br-rr-mgmt state UP mode DEFAULT group default qlen 1000
    link/ether 00:21:9b:a2:7c:59 brd ff:ff:ff:ff:ff:ff promiscuity 1 allmulti 1 minmtu 0 maxmtu 65535 
    vlan protocol 802.1Q id 2 <REORDER_HDR> 
    bridge_slave state forwarding priority 32 cost 19 hairpin off guard off root_block off fastleave off learning on flood on port_id 0x8001 port_no 0x1 designated_port 32769 designated_cost 0 designated_bridge 8000.0:21:9b:a2:7c:59 designated_root 8000.0:21:9b:a2:7c:59 hold_timer    0.00 message_age_timer    0.00 forward_delay_timer    0.00 topology_change_ack 0 config_pending 0 proxy_arp off proxy_arp_wifi off mcast_router 1 mcast_fast_leave off mcast_flood on bcast_flood on mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off group_fwd_mask 0 group_fwd_mask_str 0x0 vlan_tunnel off isolated off locked off mab off addrgenmode eui64 numtxqueues 1 numrxqueues 1 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 
11: br-rr-mgmt: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000
    link/ether 00:21:9b:a2:7c:59 brd ff:ff:ff:ff:ff:ff promiscuity 0 allmulti 0 minmtu 68 maxmtu 65535 
    bridge forward_delay 0 hello_time 200 max_age 2000 ageing_time 30000 stp_state 0 priority 32768 vlan_filtering 0 vlan_protocol 802.1Q bridge_id 8000.0:21:9b:a2:7c:59 designated_root 8000.0:21:9b:a2:7c:59 root_port 0 root_path_cost 0 topology_change 0 topology_change_detected 0 hello_timer    0.00 tcn_timer    0.00 topology_change_timer    0.00 gc_timer  222.37 fdb_n_learned 0 fdb_max_learned 0 vlan_default_pvid 1 vlan_stats_enabled 0 vlan_stats_per_port 0 group_fwd_mask 0 group_address 01:80:c2:00:00:00 mcast_snooping 1 no_linklocal_learn 0 mcast_vlan_snooping 0 mst_enabled 0 mcast_router 1 mcast_query_use_ifaddr 0 mcast_querier 0 mcast_hash_elasticity 16 mcast_hash_max 4096 mcast_last_member_count 2 mcast_startup_query_count 2 mcast_last_member_interval 100 mcast_membership_interval 26000 mcast_querier_interval 25500 mcast_query_interval 12500 mcast_query_response_interval 1000 mcast_startup_query_interval 3125 mcast_stats_enabled 0 mcast_igmp_version 2 mcast_mld_version 1 nf_call_iptables 0 nf_call_ip6tables 0 nf_call_arptables 0 addrgenmode eui64 numtxqueues 1 numrxqueues 1 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 
12: bond0: <BROADCAST,MULTICAST,MASTER,UP,LOWER_UP> mtu 1500 qdisc noqueue master storagenet state UP mode DEFAULT group default qlen 1000
    link/ether 00:21:9b:a2:7c:55 brd ff:ff:ff:ff:ff:ff promiscuity 1 allmulti 1 minmtu 68 maxmtu 65535 
    bond mode 802.3ad miimon 100 updelay 0 downdelay 0 peer_notify_delay 0 use_carrier 1 arp_interval 0 arp_missed_max 2 arp_validate none arp_all_targets any primary_reselect always fail_over_mac none xmit_hash_policy layer3+4 resend_igmp 1 num_grat_arp 1 all_slaves_active 0 min_links 0 lp_interval 1 packets_per_slave 1 lacp_active on lacp_rate slow coupled_control on ad_select stable ad_aggregator 1 ad_num_ports 2 ad_actor_key 9 ad_partner_key 26 ad_partner_mac 00:13:72:46:95:e4 ad_actor_sys_prio 65535 ad_user_port_key 0 ad_actor_system 00:00:00:00:00:00 tlb_dynamic_lb 1 
    bridge_slave state forwarding priority 32 cost 5 hairpin off guard off root_block off fastleave off learning on flood on port_id 0x8001 port_no 0x1 designated_port 32769 designated_cost 0 designated_bridge 8000.0:21:9b:a2:7c:55 designated_root 8000.0:21:9b:a2:7c:55 hold_timer    0.00 message_age_timer    0.00 forward_delay_timer    0.00 topology_change_ack 0 config_pending 0 proxy_arp off proxy_arp_wifi off mcast_router 1 mcast_fast_leave off mcast_flood on bcast_flood on mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off group_fwd_mask 0 group_fwd_mask_str 0x0 vlan_tunnel off isolated off locked off mab off addrgenmode eui64 numtxqueues 16 numrxqueues 16 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 
13: storagenet: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000
    link/ether 00:21:9b:a2:7c:55 brd ff:ff:ff:ff:ff:ff promiscuity 0 allmulti 0 minmtu 68 maxmtu 65535 
    bridge forward_delay 0 hello_time 200 max_age 2000 ageing_time 30000 stp_state 0 priority 32768 vlan_filtering 0 vlan_protocol 802.1Q bridge_id 8000.0:21:9b:a2:7c:55 designated_root 8000.0:21:9b:a2:7c:55 root_port 0 root_path_cost 0 topology_change 0 topology_change_detected 0 hello_timer    0.00 tcn_timer    0.00 topology_change_timer    0.00 gc_timer   34.62 fdb_n_learned 7 fdb_max_learned 0 vlan_default_pvid 1 vlan_stats_enabled 0 vlan_stats_per_port 0 group_fwd_mask 0 group_address 01:80:c2:00:00:00 mcast_snooping 1 no_linklocal_learn 0 mcast_vlan_snooping 0 mst_enabled 0 mcast_router 1 mcast_query_use_ifaddr 0 mcast_querier 0 mcast_hash_elasticity 16 mcast_hash_max 4096 mcast_last_member_count 2 mcast_startup_query_count 2 mcast_last_member_interval 100 mcast_membership_interval 26000 mcast_querier_interval 25500 mcast_query_interval 12500 mcast_query_response_interval 1000 mcast_startup_query_interval 3125 mcast_stats_enabled 0 mcast_igmp_version 2 mcast_mld_version 1 nf_call_iptables 0 nf_call_ip6tables 0 nf_call_arptables 0 addrgenmode eui64 numtxqueues 1 numrxqueues 1 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 
46: tap100i0: <BROADCAST,MULTICAST,PROMISC,UP,LOWER_UP> mtu 1500 qdisc fq master fwbr100i0 state UNKNOWN mode DEFAULT group default qlen 1000
    link/ether 86:4a:ba:ce:74:cb brd ff:ff:ff:ff:ff:ff promiscuity 2 allmulti 1 minmtu 68 maxmtu 65521 
    tun type tap pi off vnet_hdr on persist off 
    bridge_slave state forwarding priority 32 cost 2 hairpin off guard off root_block off fastleave off learning on flood on port_id 0x8002 port_no 0x2 designated_port 32770 designated_cost 0 designated_bridge 8000.1a:fa:65:4c:65:9d designated_root 8000.1a:fa:65:4c:65:9d hold_timer    0.00 message_age_timer    0.00 forward_delay_timer    0.00 topology_change_ack 0 config_pending 0 proxy_arp off proxy_arp_wifi off mcast_router 1 mcast_fast_leave off mcast_flood on bcast_flood on mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off group_fwd_mask 0 group_fwd_mask_str 0x0 vlan_tunnel off isolated off locked off mab off addrgenmode eui64 numtxqueues 1 numrxqueues 1 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 
47: fwbr100i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000
    link/ether 1a:fa:65:4c:65:9d brd ff:ff:ff:ff:ff:ff promiscuity 0 allmulti 0 minmtu 68 maxmtu 65535 
    bridge forward_delay 0 hello_time 200 max_age 2000 ageing_time 30000 stp_state 0 priority 32768 vlan_filtering 0 vlan_protocol 802.1Q bridge_id 8000.1a:fa:65:4c:65:9d designated_root 8000.1a:fa:65:4c:65:9d root_port 0 root_path_cost 0 topology_change 0 topology_change_detected 0 hello_timer    0.00 tcn_timer    0.00 topology_change_timer    0.00 gc_timer    8.46 fdb_n_learned 78 fdb_max_learned 0 vlan_default_pvid 1 vlan_stats_enabled 0 vlan_stats_per_port 0 group_fwd_mask 0 group_address 01:80:c2:00:00:00 mcast_snooping 1 no_linklocal_learn 0 mcast_vlan_snooping 0 mst_enabled 0 mcast_router 1 mcast_query_use_ifaddr 0 mcast_querier 0 mcast_querier_ipv4_addr 0.0.0.0 mcast_querier_ipv4_port 49 mcast_querier_ipv4_other_timer 19.7us mcast_hash_elasticity 16 mcast_hash_max 4096 mcast_last_member_count 2 mcast_startup_query_count 2 mcast_last_member_interval 100 mcast_membership_interval 26000 mcast_querier_interval 25500 mcast_query_interval 12500 mcast_query_response_interval 1000 mcast_startup_query_interval 3125 mcast_stats_enabled 0 mcast_igmp_version 2 mcast_mld_version 1 nf_call_iptables 0 nf_call_ip6tables 0 nf_call_arptables 0 addrgenmode eui64 numtxqueues 1 numrxqueues 1 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 
48: fwpr100p0@fwln100i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master vmbr0 state UP mode DEFAULT group default qlen 1000
    link/ether c2:2f:59:b1:8b:a8 brd ff:ff:ff:ff:ff:ff promiscuity 1 allmulti 1 minmtu 68 maxmtu 65535 
    veth 
    bridge_slave state forwarding priority 32 cost 2 hairpin off guard off root_block off fastleave off learning on flood on port_id 0x8002 port_no 0x2 designated_port 32770 designated_cost 0 designated_bridge 8000.0:21:9b:a2:7c:53 designated_root 8000.0:21:9b:a2:7c:53 hold_timer    0.00 message_age_timer    0.00 forward_delay_timer    0.00 topology_change_ack 0 config_pending 0 proxy_arp off proxy_arp_wifi off mcast_router 1 mcast_fast_leave off mcast_flood on bcast_flood on mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off group_fwd_mask 0 group_fwd_mask_str 0x0 vlan_tunnel off isolated off locked off mab off addrgenmode eui64 numtxqueues 16 numrxqueues 16 gso_max_size 65536 gso_max_segs 65535 tso_max_size 524280 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 
49: fwln100i0@fwpr100p0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master fwbr100i0 state UP mode DEFAULT group default qlen 1000
    link/ether 1a:fa:65:4c:65:9d brd ff:ff:ff:ff:ff:ff promiscuity 1 allmulti 1 minmtu 68 maxmtu 65535 
    veth 
    bridge_slave state forwarding priority 32 cost 2 hairpin off guard off root_block off fastleave off learning on flood on port_id 0x8001 port_no 0x1 designated_port 32769 designated_cost 0 designated_bridge 8000.1a:fa:65:4c:65:9d designated_root 8000.1a:fa:65:4c:65:9d hold_timer    0.00 message_age_timer    0.00 forward_delay_timer    0.00 topology_change_ack 0 config_pending 0 proxy_arp off proxy_arp_wifi off mcast_router 1 mcast_fast_leave off mcast_flood on bcast_flood on mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off group_fwd_mask 0 group_fwd_mask_str 0x0 vlan_tunnel off isolated off locked off mab off addrgenmode eui64 numtxqueues 16 numrxqueues 16 gso_max_size 65536 gso_max_segs 65535 tso_max_size 524280 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 
50: tap600i0: <BROADCAST,MULTICAST,PROMISC,UP,LOWER_UP> mtu 1500 qdisc fq master fwbr600i0 state UNKNOWN mode DEFAULT group default qlen 1000
    link/ether 46:3a:47:c7:38:66 brd ff:ff:ff:ff:ff:ff promiscuity 2 allmulti 1 minmtu 68 maxmtu 65521 
    tun type tap pi off vnet_hdr on persist off 
    bridge_slave state forwarding priority 32 cost 2 hairpin off guard off root_block off fastleave off learning on flood on port_id 0x8002 port_no 0x2 designated_port 32770 designated_cost 0 designated_bridge 8000.62:c5:35:11:4b:3c designated_root 8000.62:c5:35:11:4b:3c hold_timer    0.00 message_age_timer    0.00 forward_delay_timer    0.00 topology_change_ack 0 config_pending 0 proxy_arp off proxy_arp_wifi off mcast_router 1 mcast_fast_leave off mcast_flood on bcast_flood on mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off group_fwd_mask 0 group_fwd_mask_str 0x0 vlan_tunnel off isolated off locked off mab off addrgenmode eui64 numtxqueues 1 numrxqueues 1 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 
51: fwbr600i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000
    link/ether 62:c5:35:11:4b:3c brd ff:ff:ff:ff:ff:ff promiscuity 0 allmulti 0 minmtu 68 maxmtu 65535 
    bridge forward_delay 0 hello_time 200 max_age 2000 ageing_time 30000 stp_state 0 priority 32768 vlan_filtering 0 vlan_protocol 802.1Q bridge_id 8000.62:c5:35:11:4b:3c designated_root 8000.62:c5:35:11:4b:3c root_port 0 root_path_cost 0 topology_change 0 topology_change_detected 0 hello_timer    0.00 tcn_timer    0.00 topology_change_timer    0.00 gc_timer    8.46 fdb_n_learned 78 fdb_max_learned 0 vlan_default_pvid 1 vlan_stats_enabled 0 vlan_stats_per_port 0 group_fwd_mask 0 group_address 01:80:c2:00:00:00 mcast_snooping 1 no_linklocal_learn 0 mcast_vlan_snooping 0 mst_enabled 0 mcast_router 1 mcast_query_use_ifaddr 0 mcast_querier 0 mcast_querier_ipv4_addr 0.0.0.0 mcast_querier_ipv4_port 53 mcast_querier_ipv4_other_timer 19.7us mcast_hash_elasticity 16 mcast_hash_max 4096 mcast_last_member_count 2 mcast_startup_query_count 2 mcast_last_member_interval 100 mcast_membership_interval 26000 mcast_querier_interval 25500 mcast_query_interval 12500 mcast_query_response_interval 1000 mcast_startup_query_interval 3125 mcast_stats_enabled 0 mcast_igmp_version 2 mcast_mld_version 1 nf_call_iptables 0 nf_call_ip6tables 0 nf_call_arptables 0 addrgenmode eui64 numtxqueues 1 numrxqueues 1 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 
52: fwpr600p0@fwln600i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master vmbr0 state UP mode DEFAULT group default qlen 1000
    link/ether 82:f1:c8:d9:02:f3 brd ff:ff:ff:ff:ff:ff promiscuity 1 allmulti 1 minmtu 68 maxmtu 65535 
    veth 
    bridge_slave state forwarding priority 32 cost 2 hairpin off guard off root_block off fastleave off learning on flood on port_id 0x8003 port_no 0x3 designated_port 32771 designated_cost 0 designated_bridge 8000.0:21:9b:a2:7c:53 designated_root 8000.0:21:9b:a2:7c:53 hold_timer    0.00 message_age_timer    0.00 forward_delay_timer    0.00 topology_change_ack 0 config_pending 0 proxy_arp off proxy_arp_wifi off mcast_router 1 mcast_fast_leave off mcast_flood on bcast_flood on mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off group_fwd_mask 0 group_fwd_mask_str 0x0 vlan_tunnel off isolated off locked off mab off addrgenmode eui64 numtxqueues 16 numrxqueues 16 gso_max_size 65536 gso_max_segs 65535 tso_max_size 524280 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 
53: fwln600i0@fwpr600p0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master fwbr600i0 state UP mode DEFAULT group default qlen 1000
    link/ether 62:c5:35:11:4b:3c brd ff:ff:ff:ff:ff:ff promiscuity 1 allmulti 1 minmtu 68 maxmtu 65535 
    veth 
    bridge_slave state forwarding priority 32 cost 2 hairpin off guard off root_block off fastleave off learning on flood on port_id 0x8001 port_no 0x1 designated_port 32769 designated_cost 0 designated_bridge 8000.62:c5:35:11:4b:3c designated_root 8000.62:c5:35:11:4b:3c hold_timer    0.00 message_age_timer    0.00 forward_delay_timer    0.00 topology_change_ack 0 config_pending 0 proxy_arp off proxy_arp_wifi off mcast_router 1 mcast_fast_leave off mcast_flood on bcast_flood on mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off group_fwd_mask 0 group_fwd_mask_str 0x0 vlan_tunnel off isolated off locked off mab off addrgenmode eui64 numtxqueues 16 numrxqueues 16 gso_max_size 65536 gso_max_segs 65535 tso_max_size 524280 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 
54: tap601i0: <BROADCAST,MULTICAST,PROMISC,UP,LOWER_UP> mtu 1500 qdisc fq master fwbr601i0 state UNKNOWN mode DEFAULT group default qlen 1000
    link/ether b6:0f:0a:05:bb:7f brd ff:ff:ff:ff:ff:ff promiscuity 2 allmulti 1 minmtu 68 maxmtu 65521 
    tun type tap pi off vnet_hdr on persist off 
    bridge_slave state forwarding priority 32 cost 2 hairpin off guard off root_block off fastleave off learning on flood on port_id 0x8002 port_no 0x2 designated_port 32770 designated_cost 0 designated_bridge 8000.d6:d7:f0:f5:2f:c designated_root 8000.d6:d7:f0:f5:2f:c hold_timer    0.00 message_age_timer    0.00 forward_delay_timer    0.00 topology_change_ack 0 config_pending 0 proxy_arp off proxy_arp_wifi off mcast_router 1 mcast_fast_leave off mcast_flood on bcast_flood on mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off group_fwd_mask 0 group_fwd_mask_str 0x0 vlan_tunnel off isolated off locked off mab off addrgenmode eui64 numtxqueues 1 numrxqueues 1 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 
55: fwbr601i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000
    link/ether d6:d7:f0:f5:2f:0c brd ff:ff:ff:ff:ff:ff promiscuity 0 allmulti 0 minmtu 68 maxmtu 65535 
    bridge forward_delay 0 hello_time 200 max_age 2000 ageing_time 30000 stp_state 0 priority 32768 vlan_filtering 0 vlan_protocol 802.1Q bridge_id 8000.d6:d7:f0:f5:2f:c designated_root 8000.d6:d7:f0:f5:2f:c root_port 0 root_path_cost 0 topology_change 0 topology_change_detected 0 hello_timer    0.00 tcn_timer    0.00 topology_change_timer    0.00 gc_timer    8.46 fdb_n_learned 78 fdb_max_learned 0 vlan_default_pvid 1 vlan_stats_enabled 0 vlan_stats_per_port 0 group_fwd_mask 0 group_address 01:80:c2:00:00:00 mcast_snooping 1 no_linklocal_learn 0 mcast_vlan_snooping 0 mst_enabled 0 mcast_router 1 mcast_query_use_ifaddr 0 mcast_querier 0 mcast_querier_ipv4_addr 0.0.0.0 mcast_querier_ipv4_port 57 mcast_querier_ipv4_other_timer 19.7us mcast_hash_elasticity 16 mcast_hash_max 4096 mcast_last_member_count 2 mcast_startup_query_count 2 mcast_last_member_interval 100 mcast_membership_interval 26000 mcast_querier_interval 25500 mcast_query_interval 12500 mcast_query_response_interval 1000 mcast_startup_query_interval 3125 mcast_stats_enabled 0 mcast_igmp_version 2 mcast_mld_version 1 nf_call_iptables 0 nf_call_ip6tables 0 nf_call_arptables 0 addrgenmode eui64 numtxqueues 1 numrxqueues 1 gso_max_size 65536 gso_max_segs 65535 tso_max_size 65536 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 
56: fwpr601p0@fwln601i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master vmbr0 state UP mode DEFAULT group default qlen 1000
    link/ether 5a:b3:90:81:99:9b brd ff:ff:ff:ff:ff:ff promiscuity 1 allmulti 1 minmtu 68 maxmtu 65535 
    veth 
    bridge_slave state forwarding priority 32 cost 2 hairpin off guard off root_block off fastleave off learning on flood on port_id 0x8004 port_no 0x4 designated_port 32772 designated_cost 0 designated_bridge 8000.0:21:9b:a2:7c:53 designated_root 8000.0:21:9b:a2:7c:53 hold_timer    0.00 message_age_timer    0.00 forward_delay_timer    0.00 topology_change_ack 0 config_pending 0 proxy_arp off proxy_arp_wifi off mcast_router 1 mcast_fast_leave off mcast_flood on bcast_flood on mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off group_fwd_mask 0 group_fwd_mask_str 0x0 vlan_tunnel off isolated off locked off mab off addrgenmode eui64 numtxqueues 16 numrxqueues 16 gso_max_size 65536 gso_max_segs 65535 tso_max_size 524280 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 
57: fwln601i0@fwpr601p0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master fwbr601i0 state UP mode DEFAULT group default qlen 1000
    link/ether d6:d7:f0:f5:2f:0c brd ff:ff:ff:ff:ff:ff promiscuity 1 allmulti 1 minmtu 68 maxmtu 65535 
    veth 
    bridge_slave state forwarding priority 32 cost 2 hairpin off guard off root_block off fastleave off learning on flood on port_id 0x8001 port_no 0x1 designated_port 32769 designated_cost 0 designated_bridge 8000.d6:d7:f0:f5:2f:c designated_root 8000.d6:d7:f0:f5:2f:c hold_timer    0.00 message_age_timer    0.00 forward_delay_timer    0.00 topology_change_ack 0 config_pending 0 proxy_arp off proxy_arp_wifi off mcast_router 1 mcast_fast_leave off mcast_flood on bcast_flood on mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off group_fwd_mask 0 group_fwd_mask_str 0x0 vlan_tunnel off isolated off locked off mab off addrgenmode eui64 numtxqueues 16 numrxqueues 16 gso_max_size 65536 gso_max_segs 65535 tso_max_size 524280 tso_max_segs 65535 gro_max_size 65536 gso_ipv4_max_size 65536 gro_ipv4_max_size 65536 

--- ip -o link
    $ ip -o link
1: lo: <LOOPBACK,UP,LOWER_UP> mtu 65536 qdisc noqueue state UNKNOWN mode DEFAULT group default qlen 1000\    link/loopback 00:00:00:00:00:00 brd 00:00:00:00:00:00
2: nic0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc mq master vmbr0 state UP mode DEFAULT group default qlen 1000\    link/ether 00:21:9b:a2:7c:53 brd ff:ff:ff:ff:ff:ff\    altname enp1s0f0\    altname enx00219ba27c53
3: nic1: <BROADCAST,MULTICAST,SLAVE,UP,LOWER_UP> mtu 1500 qdisc mq master bond0 state UP mode DEFAULT group default qlen 1000\    link/ether 00:21:9b:a2:7c:55 brd ff:ff:ff:ff:ff:ff\    altname enp1s0f1\    altname enx00219ba27c55
4: nic2: <BROADCAST,MULTICAST,SLAVE,UP,LOWER_UP> mtu 1500 qdisc mq master bond0 state UP mode DEFAULT group default qlen 1000\    link/ether 00:21:9b:a2:7c:55 brd ff:ff:ff:ff:ff:ff permaddr 00:21:9b:a2:7c:57\    altname enp2s0f0\    altname enx00219ba27c57
5: nic3: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc mq state UP mode DEFAULT group default qlen 1000\    link/ether 00:21:9b:a2:7c:59 brd ff:ff:ff:ff:ff:ff\    altname enp2s0f1\    altname enx00219ba27c59
6: nic4: <BROADCAST,MULTICAST> mtu 1500 qdisc noop state DOWN mode DEFAULT group default qlen 1000\    link/ether 00:10:18:72:16:40 brd ff:ff:ff:ff:ff:ff\    altname enx001018721640
7: nic5: <BROADCAST,MULTICAST> mtu 1500 qdisc noop state DOWN mode DEFAULT group default qlen 1000\    link/ether 00:10:18:72:16:42 brd ff:ff:ff:ff:ff:ff\    altname enx001018721642
8: vmbr0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000\    link/ether 00:21:9b:a2:7c:53 brd ff:ff:ff:ff:ff:ff
9: tailscale0: <POINTOPOINT,MULTICAST,NOARP,UP,LOWER_UP> mtu 1280 qdisc fq state UNKNOWN mode DEFAULT group default qlen 500\    link/none 
10: nic3.2@nic3: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master br-rr-mgmt state UP mode DEFAULT group default qlen 1000\    link/ether 00:21:9b:a2:7c:59 brd ff:ff:ff:ff:ff:ff
11: br-rr-mgmt: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000\    link/ether 00:21:9b:a2:7c:59 brd ff:ff:ff:ff:ff:ff
12: bond0: <BROADCAST,MULTICAST,MASTER,UP,LOWER_UP> mtu 1500 qdisc noqueue master storagenet state UP mode DEFAULT group default qlen 1000\    link/ether 00:21:9b:a2:7c:55 brd ff:ff:ff:ff:ff:ff
13: storagenet: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000\    link/ether 00:21:9b:a2:7c:55 brd ff:ff:ff:ff:ff:ff
46: tap100i0: <BROADCAST,MULTICAST,PROMISC,UP,LOWER_UP> mtu 1500 qdisc fq master fwbr100i0 state UNKNOWN mode DEFAULT group default qlen 1000\    link/ether 86:4a:ba:ce:74:cb brd ff:ff:ff:ff:ff:ff
47: fwbr100i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000\    link/ether 1a:fa:65:4c:65:9d brd ff:ff:ff:ff:ff:ff
48: fwpr100p0@fwln100i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master vmbr0 state UP mode DEFAULT group default qlen 1000\    link/ether c2:2f:59:b1:8b:a8 brd ff:ff:ff:ff:ff:ff
49: fwln100i0@fwpr100p0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master fwbr100i0 state UP mode DEFAULT group default qlen 1000\    link/ether 1a:fa:65:4c:65:9d brd ff:ff:ff:ff:ff:ff
50: tap600i0: <BROADCAST,MULTICAST,PROMISC,UP,LOWER_UP> mtu 1500 qdisc fq master fwbr600i0 state UNKNOWN mode DEFAULT group default qlen 1000\    link/ether 46:3a:47:c7:38:66 brd ff:ff:ff:ff:ff:ff
51: fwbr600i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000\    link/ether 62:c5:35:11:4b:3c brd ff:ff:ff:ff:ff:ff
52: fwpr600p0@fwln600i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master vmbr0 state UP mode DEFAULT group default qlen 1000\    link/ether 82:f1:c8:d9:02:f3 brd ff:ff:ff:ff:ff:ff
53: fwln600i0@fwpr600p0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master fwbr600i0 state UP mode DEFAULT group default qlen 1000\    link/ether 62:c5:35:11:4b:3c brd ff:ff:ff:ff:ff:ff
54: tap601i0: <BROADCAST,MULTICAST,PROMISC,UP,LOWER_UP> mtu 1500 qdisc fq master fwbr601i0 state UNKNOWN mode DEFAULT group default qlen 1000\    link/ether b6:0f:0a:05:bb:7f brd ff:ff:ff:ff:ff:ff
55: fwbr601i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000\    link/ether d6:d7:f0:f5:2f:0c brd ff:ff:ff:ff:ff:ff
56: fwpr601p0@fwln601i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master vmbr0 state UP mode DEFAULT group default qlen 1000\    link/ether 5a:b3:90:81:99:9b brd ff:ff:ff:ff:ff:ff
57: fwln601i0@fwpr601p0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master fwbr601i0 state UP mode DEFAULT group default qlen 1000\    link/ether d6:d7:f0:f5:2f:0c brd ff:ff:ff:ff:ff:ff

--- ip -o -4 addr
    $ ip -o -4 addr
1: lo    inet 127.0.0.1/8 scope host lo\       valid_lft forever preferred_lft forever
8: vmbr0    inet 192.168.3.169/22 brd 192.168.3.255 scope global dynamic vmbr0\       valid_lft 460sec preferred_lft 460sec
9: tailscale0    inet 100.73.35.111/32 scope global tailscale0\       valid_lft forever preferred_lft forever
11: br-rr-mgmt    inet 10.251.2.6/24 scope global br-rr-mgmt\       valid_lft forever preferred_lft forever
13: storagenet    inet 10.100.100.6/24 scope global storagenet\       valid_lft forever preferred_lft forever

--- ip -o -6 addr (link-local filter)
    $ ip -o -6 addr
1: lo    inet6 ::1/128 scope host noprefixroute \       valid_lft forever preferred_lft forever
5: nic3    inet6 fe80::221:9bff:fea2:7c59/64 scope link proto kernel_ll \       valid_lft forever preferred_lft forever
8: vmbr0    inet6 fe80::221:9bff:fea2:7c53/64 scope link proto kernel_ll \       valid_lft forever preferred_lft forever
9: tailscale0    inet6 fd7a:115c:a1e0::df3b:236f/128 scope global \       valid_lft forever preferred_lft forever
9: tailscale0    inet6 fe80::1f97:7375:575c:fc8e/64 scope link stable-privacy proto kernel_ll \       valid_lft forever preferred_lft forever
11: br-rr-mgmt    inet6 fe80::221:9bff:fea2:7c59/64 scope link proto kernel_ll \       valid_lft forever preferred_lft forever
13: storagenet    inet6 fe80::221:9bff:fea2:7c55/64 scope link proto kernel_ll \       valid_lft forever preferred_lft forever

--- ip addr
    $ ip addr
1: lo: <LOOPBACK,UP,LOWER_UP> mtu 65536 qdisc noqueue state UNKNOWN group default qlen 1000
    link/loopback 00:00:00:00:00:00 brd 00:00:00:00:00:00
    inet 127.0.0.1/8 scope host lo
       valid_lft forever preferred_lft forever
    inet6 ::1/128 scope host noprefixroute 
       valid_lft forever preferred_lft forever
2: nic0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc mq master vmbr0 state UP group default qlen 1000
    link/ether 00:21:9b:a2:7c:53 brd ff:ff:ff:ff:ff:ff
    altname enp1s0f0
    altname enx00219ba27c53
3: nic1: <BROADCAST,MULTICAST,SLAVE,UP,LOWER_UP> mtu 1500 qdisc mq master bond0 state UP group default qlen 1000
    link/ether 00:21:9b:a2:7c:55 brd ff:ff:ff:ff:ff:ff
    altname enp1s0f1
    altname enx00219ba27c55
4: nic2: <BROADCAST,MULTICAST,SLAVE,UP,LOWER_UP> mtu 1500 qdisc mq master bond0 state UP group default qlen 1000
    link/ether 00:21:9b:a2:7c:55 brd ff:ff:ff:ff:ff:ff permaddr 00:21:9b:a2:7c:57
    altname enp2s0f0
    altname enx00219ba27c57
5: nic3: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc mq state UP group default qlen 1000
    link/ether 00:21:9b:a2:7c:59 brd ff:ff:ff:ff:ff:ff
    altname enp2s0f1
    altname enx00219ba27c59
    inet6 fe80::221:9bff:fea2:7c59/64 scope link proto kernel_ll 
       valid_lft forever preferred_lft forever
6: nic4: <BROADCAST,MULTICAST> mtu 1500 qdisc noop state DOWN group default qlen 1000
    link/ether 00:10:18:72:16:40 brd ff:ff:ff:ff:ff:ff
    altname enx001018721640
7: nic5: <BROADCAST,MULTICAST> mtu 1500 qdisc noop state DOWN group default qlen 1000
    link/ether 00:10:18:72:16:42 brd ff:ff:ff:ff:ff:ff
    altname enx001018721642
8: vmbr0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP group default qlen 1000
    link/ether 00:21:9b:a2:7c:53 brd ff:ff:ff:ff:ff:ff
    inet 192.168.3.169/22 brd 192.168.3.255 scope global dynamic vmbr0
       valid_lft 460sec preferred_lft 460sec
    inet6 fe80::221:9bff:fea2:7c53/64 scope link proto kernel_ll 
       valid_lft forever preferred_lft forever
9: tailscale0: <POINTOPOINT,MULTICAST,NOARP,UP,LOWER_UP> mtu 1280 qdisc fq state UNKNOWN group default qlen 500
    link/none 
    inet 100.73.35.111/32 scope global tailscale0
       valid_lft forever preferred_lft forever
    inet6 fd7a:115c:a1e0::df3b:236f/128 scope global 
       valid_lft forever preferred_lft forever
    inet6 fe80::1f97:7375:575c:fc8e/64 scope link stable-privacy proto kernel_ll 
       valid_lft forever preferred_lft forever
10: nic3.2@nic3: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master br-rr-mgmt state UP group default qlen 1000
    link/ether 00:21:9b:a2:7c:59 brd ff:ff:ff:ff:ff:ff
11: br-rr-mgmt: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP group default qlen 1000
    link/ether 00:21:9b:a2:7c:59 brd ff:ff:ff:ff:ff:ff
    inet 10.251.2.6/24 scope global br-rr-mgmt
       valid_lft forever preferred_lft forever
    inet6 fe80::221:9bff:fea2:7c59/64 scope link proto kernel_ll 
       valid_lft forever preferred_lft forever
12: bond0: <BROADCAST,MULTICAST,MASTER,UP,LOWER_UP> mtu 1500 qdisc noqueue master storagenet state UP group default qlen 1000
    link/ether 00:21:9b:a2:7c:55 brd ff:ff:ff:ff:ff:ff
13: storagenet: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP group default qlen 1000
    link/ether 00:21:9b:a2:7c:55 brd ff:ff:ff:ff:ff:ff
    inet 10.100.100.6/24 scope global storagenet
       valid_lft forever preferred_lft forever
    inet6 fe80::221:9bff:fea2:7c55/64 scope link proto kernel_ll 
       valid_lft forever preferred_lft forever
46: tap100i0: <BROADCAST,MULTICAST,PROMISC,UP,LOWER_UP> mtu 1500 qdisc fq master fwbr100i0 state UNKNOWN group default qlen 1000
    link/ether 86:4a:ba:ce:74:cb brd ff:ff:ff:ff:ff:ff
47: fwbr100i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP group default qlen 1000
    link/ether 1a:fa:65:4c:65:9d brd ff:ff:ff:ff:ff:ff
48: fwpr100p0@fwln100i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master vmbr0 state UP group default qlen 1000
    link/ether c2:2f:59:b1:8b:a8 brd ff:ff:ff:ff:ff:ff
49: fwln100i0@fwpr100p0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master fwbr100i0 state UP group default qlen 1000
    link/ether 1a:fa:65:4c:65:9d brd ff:ff:ff:ff:ff:ff
50: tap600i0: <BROADCAST,MULTICAST,PROMISC,UP,LOWER_UP> mtu 1500 qdisc fq master fwbr600i0 state UNKNOWN group default qlen 1000
    link/ether 46:3a:47:c7:38:66 brd ff:ff:ff:ff:ff:ff
51: fwbr600i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP group default qlen 1000
    link/ether 62:c5:35:11:4b:3c brd ff:ff:ff:ff:ff:ff
52: fwpr600p0@fwln600i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master vmbr0 state UP group default qlen 1000
    link/ether 82:f1:c8:d9:02:f3 brd ff:ff:ff:ff:ff:ff
53: fwln600i0@fwpr600p0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master fwbr600i0 state UP group default qlen 1000
    link/ether 62:c5:35:11:4b:3c brd ff:ff:ff:ff:ff:ff
54: tap601i0: <BROADCAST,MULTICAST,PROMISC,UP,LOWER_UP> mtu 1500 qdisc fq master fwbr601i0 state UNKNOWN group default qlen 1000
    link/ether b6:0f:0a:05:bb:7f brd ff:ff:ff:ff:ff:ff
55: fwbr601i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP group default qlen 1000
    link/ether d6:d7:f0:f5:2f:0c brd ff:ff:ff:ff:ff:ff
56: fwpr601p0@fwln601i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master vmbr0 state UP group default qlen 1000
    link/ether 5a:b3:90:81:99:9b brd ff:ff:ff:ff:ff:ff
57: fwln601i0@fwpr601p0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master fwbr601i0 state UP group default qlen 1000
    link/ether d6:d7:f0:f5:2f:0c brd ff:ff:ff:ff:ff:ff

--- ip route
    $ ip route
default via 192.168.3.254 dev vmbr0 
10.100.100.0/24 dev storagenet proto kernel scope link src 10.100.100.6 
10.251.2.0/24 dev br-rr-mgmt proto kernel scope link src 10.251.2.6 
192.168.0.0/22 dev vmbr0 proto kernel scope link src 192.168.3.169 

--- ip rule
    $ ip rule
0:	from all lookup local
5210:	from all fwmark 0x80000/0xff0000 lookup main
5230:	from all fwmark 0x80000/0xff0000 lookup default
5250:	from all fwmark 0x80000/0xff0000 unreachable
5270:	from all lookup 52
32766:	from all lookup main
32767:	from all lookup default

--- ip -s -s link (counters/errors)
    $ ip -s -s link
1: lo: <LOOPBACK,UP,LOWER_UP> mtu 65536 qdisc noqueue state UNKNOWN mode DEFAULT group default qlen 1000
    link/loopback 00:00:00:00:00:00 brd 00:00:00:00:00:00
    RX:  bytes packets errors dropped  missed   mcast           
      61315931  378561      0       0       0       0 
    RX errors:  length    crc   frame    fifo overrun
                     0      0       0       0       0 
    TX:  bytes packets errors dropped carrier collsns           
      61315931  378561      0       0       0       0 
    TX errors: aborted   fifo  window heartbt transns
                     0      0       0       0       0 
2: nic0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc mq master vmbr0 state UP mode DEFAULT group default qlen 1000
    link/ether 00:21:9b:a2:7c:53 brd ff:ff:ff:ff:ff:ff
    RX:  bytes  packets errors dropped  missed   mcast           
    3350233895 12198574      0    7182       1 5084318 
    RX errors:   length    crc   frame    fifo overrun
                      0      0       0       0       0 
    TX:  bytes  packets errors dropped carrier collsns           
    5306247835  6212008      0       3       0       0 
    TX errors:  aborted   fifo  window heartbt transns
                      0      0       0       0       2 
    altname enp1s0f0
    altname enx00219ba27c53
3: nic1: <BROADCAST,MULTICAST,SLAVE,UP,LOWER_UP> mtu 1500 qdisc mq master bond0 state UP mode DEFAULT group default qlen 1000
    link/ether 00:21:9b:a2:7c:55 brd ff:ff:ff:ff:ff:ff
    RX:   bytes  packets errors dropped  missed   mcast           
    99924305026 70595086      0       0     175  147009 
    RX errors:    length    crc   frame    fifo overrun
                       0      0       0       0       0 
    TX:   bytes  packets errors dropped carrier collsns           
    23560468511 33694852      0       0       0       0 
    TX errors:   aborted   fifo  window heartbt transns
                       0      0       0       0       2 
    altname enp1s0f1
    altname enx00219ba27c55
4: nic2: <BROADCAST,MULTICAST,SLAVE,UP,LOWER_UP> mtu 1500 qdisc mq master bond0 state UP mode DEFAULT group default qlen 1000
    link/ether 00:21:9b:a2:7c:55 brd ff:ff:ff:ff:ff:ff permaddr 00:21:9b:a2:7c:57
    RX:   bytes  packets errors dropped  missed   mcast           
    22572716408 16421058      0       0       0   60090 
    RX errors:    length    crc   frame    fifo overrun
                       0      0       0       0       0 
    TX:   bytes  packets errors dropped carrier collsns           
     5686269766  6976654      0       0       0       0 
    TX errors:   aborted   fifo  window heartbt transns
                       0      0       0       0       2 
    altname enp2s0f0
    altname enx00219ba27c57
5: nic3: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc mq state UP mode DEFAULT group default qlen 1000
    link/ether 00:21:9b:a2:7c:59 brd ff:ff:ff:ff:ff:ff
    RX:  bytes packets errors dropped  missed   mcast           
      24123415  239733      0       0       0  214489 
    RX errors:  length    crc   frame    fifo overrun
                     0      0       0       0       0 
    TX:  bytes packets errors dropped carrier collsns           
       2045720    7862      0       0       0       0 
    TX errors: aborted   fifo  window heartbt transns
                     0      0       0       0       2 
    altname enp2s0f1
    altname enx00219ba27c59
6: nic4: <BROADCAST,MULTICAST> mtu 1500 qdisc noop state DOWN mode DEFAULT group default qlen 1000
    link/ether 00:10:18:72:16:40 brd ff:ff:ff:ff:ff:ff
    RX:  bytes packets errors dropped  missed   mcast           
             0       0      0       0       0       0 
    RX errors:  length    crc   frame    fifo overrun
                     0      0       0       0       0 
    TX:  bytes packets errors dropped carrier collsns           
             0       0      0       0       0       0 
    TX errors: aborted   fifo  window heartbt transns
                     0      0       0       0       0 
    altname enx001018721640
7: nic5: <BROADCAST,MULTICAST> mtu 1500 qdisc noop state DOWN mode DEFAULT group default qlen 1000
    link/ether 00:10:18:72:16:42 brd ff:ff:ff:ff:ff:ff
    RX:  bytes packets errors dropped  missed   mcast           
             0       0      0       0       0       0 
    RX errors:  length    crc   frame    fifo overrun
                     0      0       0       0       0 
    TX:  bytes packets errors dropped carrier collsns           
             0       0      0       0       0       0 
    TX errors: aborted   fifo  window heartbt transns
                     0      0       0       0       0 
    altname enx001018721642
8: vmbr0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000
    link/ether 00:21:9b:a2:7c:53 brd ff:ff:ff:ff:ff:ff
    RX:  bytes packets errors dropped  missed   mcast           
    1076025001 7927410      0       0       0 4217692 
    RX errors:  length    crc   frame    fifo overrun
                     0      0       0       0       0 
    TX:  bytes packets errors dropped carrier collsns           
    4826879122 1451133      0       3       0       0 
    TX errors: aborted   fifo  window heartbt transns
                     0      0       0       0       4 
9: tailscale0: <POINTOPOINT,MULTICAST,NOARP,UP,LOWER_UP> mtu 1280 qdisc fq state UNKNOWN mode DEFAULT group default qlen 500
    link/none 
    RX:  bytes packets errors dropped  missed   mcast           
     163474125 1146444      0       0       0       0 
    RX errors:  length    crc   frame    fifo overrun
                     0      0       0       0       0 
    TX:  bytes packets errors dropped carrier collsns           
    8056225151  978816      0       0       0       0 
    TX errors: aborted   fifo  window heartbt transns
                     0      0       0       0       0 
10: nic3.2@nic3: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master br-rr-mgmt state UP mode DEFAULT group default qlen 1000
    link/ether 00:21:9b:a2:7c:59 brd ff:ff:ff:ff:ff:ff
    RX:  bytes packets errors dropped  missed   mcast           
             0       0      0       0       0       0 
    RX errors:  length    crc   frame    fifo overrun
                     0      0       0       0       0 
    TX:  bytes packets errors dropped carrier collsns           
           906       7      0       0       0       0 
    TX errors: aborted   fifo  window heartbt transns
                     0      0       0       0       1 
11: br-rr-mgmt: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000
    link/ether 00:21:9b:a2:7c:59 brd ff:ff:ff:ff:ff:ff
    RX:  bytes packets errors dropped  missed   mcast           
             0       0      0       0       0       0 
    RX errors:  length    crc   frame    fifo overrun
                     0      0       0       0       0 
    TX:  bytes packets errors dropped carrier collsns           
           906       7      0       0       0       0 
    TX errors: aborted   fifo  window heartbt transns
                     0      0       0       0       2 
12: bond0: <BROADCAST,MULTICAST,MASTER,UP,LOWER_UP> mtu 1500 qdisc noqueue master storagenet state UP mode DEFAULT group default qlen 1000
    link/ether 00:21:9b:a2:7c:55 brd ff:ff:ff:ff:ff:ff
    RX:    bytes  packets errors dropped  missed   mcast           
    122497021434 87016144      0   14362     175  207099 
    RX errors:     length    crc   frame    fifo overrun
                        0      0       0       0       0 
    TX:    bytes  packets errors dropped carrier collsns           
     29246738277 40671506      0       0       0       0 
    TX errors:    aborted   fifo  window heartbt transns
                        0      0       0       0       2 
13: storagenet: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000
    link/ether 00:21:9b:a2:7c:55 brd ff:ff:ff:ff:ff:ff
    RX:    bytes  packets errors dropped  missed   mcast           
    118054783660 31981665      0       5       0  178369 
    RX errors:     length    crc   frame    fifo overrun
                        0      0       0       0       0 
    TX:    bytes  packets errors dropped carrier collsns           
     28189424191 27053335      0       0       0       0 
    TX errors:    aborted   fifo  window heartbt transns
                        0      0       0       0       2 
46: tap100i0: <BROADCAST,MULTICAST,PROMISC,UP,LOWER_UP> mtu 1500 qdisc fq master fwbr100i0 state UNKNOWN mode DEFAULT group default qlen 1000
    link/ether 86:4a:ba:ce:74:cb brd ff:ff:ff:ff:ff:ff
    RX:  bytes packets errors dropped  missed   mcast           
        918971    9300      0       0       0       0 
    RX errors:  length    crc   frame    fifo overrun
                     0      0       0       0       0 
    TX:  bytes packets errors dropped carrier collsns           
     476741485 4413496      0       0       0       0 
    TX errors: aborted   fifo  window heartbt transns
                     0      0       0       0       0 
47: fwbr100i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000
    link/ether 1a:fa:65:4c:65:9d brd ff:ff:ff:ff:ff:ff
    RX:  bytes packets errors dropped  missed   mcast           
     412699863 4399535      0    6271       0 2963679 
    RX errors:  length    crc   frame    fifo overrun
                     0      0       0       0       0 
    TX:  bytes packets errors dropped carrier collsns           
             0       0      0       0       0       0 
    TX errors: aborted   fifo  window heartbt transns
                     0      0       0       0       2 
48: fwpr100p0@fwln100i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master vmbr0 state UP mode DEFAULT group default qlen 1000
    link/ether c2:2f:59:b1:8b:a8 brd ff:ff:ff:ff:ff:ff
    RX:  bytes packets errors dropped  missed   mcast           
       2245643   14628      0    5328       0       0 
    RX errors:  length    crc   frame    fifo overrun
                     0      0       0       0       0 
    TX:  bytes packets errors dropped carrier collsns           
     476746813 4413496      0       0       0       0 
    TX errors: aborted   fifo  window heartbt transns
                     0      0       0       0       2 
49: fwln100i0@fwpr100p0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master fwbr100i0 state UP mode DEFAULT group default qlen 1000
    link/ether 1a:fa:65:4c:65:9d brd ff:ff:ff:ff:ff:ff
    RX:  bytes packets errors dropped  missed   mcast           
     476746813 4413496      0    5328       0       0 
    RX errors:  length    crc   frame    fifo overrun
                     0      0       0       0       0 
    TX:  bytes packets errors dropped carrier collsns           
       2245643   14628      0       0       0       0 
    TX errors: aborted   fifo  window heartbt transns
                     0      0       0       0       2 
50: tap600i0: <BROADCAST,MULTICAST,PROMISC,UP,LOWER_UP> mtu 1500 qdisc fq master fwbr600i0 state UNKNOWN mode DEFAULT group default qlen 1000
    link/ether 46:3a:47:c7:38:66 brd ff:ff:ff:ff:ff:ff
    RX:  bytes packets errors dropped  missed   mcast           
      90214677  426674      0       0       0       0 
    RX errors:  length    crc   frame    fifo overrun
                     0      0       0       0       0 
    TX:  bytes packets errors dropped carrier collsns           
     676443159 5109206      0       0       0       0 
    TX errors: aborted   fifo  window heartbt transns
                     0      0       0       0       0 
51: fwbr600i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000
    link/ether 62:c5:35:11:4b:3c brd ff:ff:ff:ff:ff:ff
    RX:  bytes packets errors dropped  missed   mcast           
     412689435 4399415      0    6270       0 2963609 
    RX errors:  length    crc   frame    fifo overrun
                     0      0       0       0       0 
    TX:  bytes packets errors dropped carrier collsns           
             0       0      0       0       0       0 
    TX errors: aborted   fifo  window heartbt transns
                     0      0       0       0       2 
52: fwpr600p0@fwln600i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master vmbr0 state UP mode DEFAULT group default qlen 1000
    link/ether 82:f1:c8:d9:02:f3 brd ff:ff:ff:ff:ff:ff
    RX:  bytes packets errors dropped  missed   mcast           
      91541349  432002      0    5328       0       0 
    RX errors:  length    crc   frame    fifo overrun
                     0      0       0       0       0 
    TX:  bytes packets errors dropped carrier collsns           
     676448701 5109207      0       0       0       0 
    TX errors: aborted   fifo  window heartbt transns
                     0      0       0       0       2 
53: fwln600i0@fwpr600p0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master fwbr600i0 state UP mode DEFAULT group default qlen 1000
    link/ether 62:c5:35:11:4b:3c brd ff:ff:ff:ff:ff:ff
    RX:  bytes packets errors dropped  missed   mcast           
     676448701 5109207      0    5328       0       0 
    RX errors:  length    crc   frame    fifo overrun
                     0      0       0       0       0 
    TX:  bytes packets errors dropped carrier collsns           
      91541349  432002      0       0       0       0 
    TX errors: aborted   fifo  window heartbt transns
                     0      0       0       0       2 
54: tap601i0: <BROADCAST,MULTICAST,PROMISC,UP,LOWER_UP> mtu 1500 qdisc fq master fwbr601i0 state UNKNOWN mode DEFAULT group default qlen 1000
    link/ether b6:0f:0a:05:bb:7f brd ff:ff:ff:ff:ff:ff
    RX:  bytes packets errors dropped  missed   mcast           
      89307849  438886      0       0       0       0 
    RX errors:  length    crc   frame    fifo overrun
                     0      0       0       0       0 
    TX:  bytes packets errors dropped carrier collsns           
    1008239703 5140324      0       0       0       0 
    TX errors: aborted   fifo  window heartbt transns
                     0      0       0       0       0 
55: fwbr601i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP mode DEFAULT group default qlen 1000
    link/ether d6:d7:f0:f5:2f:0c brd ff:ff:ff:ff:ff:ff
    RX:  bytes packets errors dropped  missed   mcast           
     412674723 4399278      0    6270       0 2963540 
    RX errors:  length    crc   frame    fifo overrun
                     0      0       0       0       0 
    TX:  bytes packets errors dropped carrier collsns           
             0       0      0       0       0       0 
    TX errors: aborted   fifo  window heartbt transns
                     0      0       0       0       2 
56: fwpr601p0@fwln601i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master vmbr0 state UP mode DEFAULT group default qlen 1000
    link/ether 5a:b3:90:81:99:9b brd ff:ff:ff:ff:ff:ff
    RX:  bytes packets errors dropped  missed   mcast           
      90634272  444213      0    5327       0       0 
    RX errors:  length    crc   frame    fifo overrun
                     0      0       0       0       0 
    TX:  bytes packets errors dropped carrier collsns           
    1008245030 5140324      0       0       0       0 
    TX errors: aborted   fifo  window heartbt transns
                     0      0       0       0       2 
57: fwln601i0@fwpr601p0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue master fwbr601i0 state UP mode DEFAULT group default qlen 1000
    link/ether d6:d7:f0:f5:2f:0c brd ff:ff:ff:ff:ff:ff
    RX:  bytes packets errors dropped  missed   mcast           
    1008245030 5140324      0    5327       0       0 
    RX errors:  length    crc   frame    fifo overrun
                     0      0       0       0       0 
    TX:  bytes packets errors dropped carrier collsns           
      90634272  444213      0       0       0       0 
    TX errors: aborted   fifo  window heartbt transns
                     0      0       0       0       2 

--- ip neigh
    $ ip neigh
192.168.3.58 dev vmbr0 lladdr a4:bb:6d:e3:56:86 STALE 
10.100.100.5 dev storagenet lladdr 00:1b:78:5c:e9:ce REACHABLE 
10.100.100.4 dev storagenet lladdr 8c:ae:4c:cd:a9:26 REACHABLE 
10.100.100.7 dev storagenet lladdr f8:bc:12:34:e0:75 STALE 
192.168.3.99 dev vmbr0 lladdr 00:a0:de:a2:81:87 STALE 
192.168.3.55 dev vmbr0 lladdr 54:e4:bd:d3:da:78 STALE 
192.168.3.250 dev vmbr0 lladdr 00:15:5d:64:e8:1e REACHABLE 
192.168.0.21 dev vmbr0 lladdr ca:fe:0f:0e:b0:75 REACHABLE 
192.168.2.44 dev vmbr0 lladdr bc:24:11:e6:03:2d REACHABLE 
10.100.100.9 dev storagenet lladdr 9c:69:d3:6a:5b:6c STALE 
192.168.3.254 dev vmbr0 lladdr 6c:4b:b4:10:40:61 REACHABLE 
192.168.3.32 dev vmbr0 lladdr a0:4a:5e:ca:46:f3 DELAY 
192.168.3.78 dev vmbr0 lladdr bc:24:11:1a:8f:6f REACHABLE 
192.168.0.1 dev vmbr0 lladdr a0:d0:dc:38:3b:41 STALE 
192.168.3.16 dev vmbr0 lladdr bc:24:11:8a:69:04 STALE 
192.168.1.119 dev vmbr0 lladdr 68:db:f5:1c:e8:8f STALE 
192.168.3.12 dev vmbr0 lladdr 02:5a:39:38:3e:9f STALE 
192.168.1.166 dev vmbr0 lladdr 00:00:c0:34:0c:dc REACHABLE 
192.168.3.173 dev vmbr0 lladdr 96:86:dd:1b:81:5a STALE 
192.168.3.153 dev vmbr0 lladdr c6:39:21:93:cd:e5 STALE 
192.168.0.250 dev vmbr0 lladdr f8:bc:12:34:e0:74 STALE 
fe80::2053:681c:dbc9:6350 dev vmbr0 lladdr bc:24:11:ee:08:c9 STALE 
fe80::8d8c:54c7:7a35:50a5 dev vmbr0 lladdr 2c:54:91:2a:0d:59 STALE 
fe80::be24:11ff:fecb:f7aa dev vmbr0 lladdr bc:24:11:cb:f7:aa STALE 
fe80::1041:575c:79d7:c3f3 dev vmbr0 lladdr c6:39:21:93:cd:e5 STALE 
fe80::436f:cf31:df06:ba90 dev vmbr0 lladdr bc:24:11:5e:dc:44 STALE 
fe80::7f67:9446:ea86:eb01 dev vmbr0 lladdr 68:ec:8a:0e:36:69 router STALE 
fe80::5ee7:53ff:fead:95c dev vmbr0 lladdr 5c:e7:53:ad:09:5c STALE 
fe80::be24:11ff:fe86:ea1a dev vmbr0 lladdr bc:24:11:86:ea:1a STALE 
fe80::907a:3764:9b08:16f3 dev vmbr0 lladdr bc:24:11:94:71:07 STALE 
fe80::eae9:e541:ea1f:9987 dev vmbr0 lladdr 9c:c8:e9:63:4b:95 STALE 
fe80::21b:78ff:fe5c:e9ce dev storagenet lladdr 00:1b:78:5c:e9:ce STALE 
fe80::6ae7:a88a:4305:7761 dev vmbr0 lladdr e8:4e:06:af:b8:92 STALE 
fe80::be5d:167b:45a7:5d73 dev vmbr0 lladdr bc:24:11:96:f7:b9 STALE 
fe80::be24:11ff:fee4:3753 dev vmbr0 lladdr bc:24:11:e4:37:53 STALE 
fe80::c0e:c2d8:9069:af43 dev vmbr0 lladdr 5a:cc:23:39:ec:f7 STALE 
fe80::be24:11ff:fec7:1171 dev vmbr0 lladdr bc:24:11:c7:11:71 STALE 
fe80::238a:7296:ce20:940f dev vmbr0 lladdr bc:24:11:8a:69:04 STALE 
fe80::a311:54:4085:c6b8 dev vmbr0 lladdr bc:24:11:32:d0:36 STALE 
fe80::65f9:f271:9449:32fc dev vmbr0 lladdr bc:24:11:2e:5a:d6 STALE 
fe80::10e8:fff4:c9c7:c57b dev vmbr0 lladdr ba:71:00:a6:a3:12 STALE 
fe80::be24:11ff:feee:67e2 dev vmbr0 lladdr bc:24:11:ee:67:e2 STALE 
fe80::31a5:b7f8:2ff3:6959 dev vmbr0 lladdr 2c:54:91:2a:0d:59 STALE 
fe80::86b:90fc:88ab:7eee dev vmbr0 lladdr 2a:cc:df:57:21:d2 STALE 
fe80::be24:11ff:feee:2bb6 dev vmbr0 lladdr bc:24:11:ee:2b:b6 STALE 
fe80::be24:11ff:fe65:b2ac dev vmbr0 lladdr bc:24:11:65:b2:ac STALE 
fe80::bb7f:ace0:50d5:690b dev vmbr0 lladdr bc:24:11:40:25:f8 STALE 
fe80::5ee7:53ff:fecf:45fa dev vmbr0 lladdr 5c:e7:53:cf:45:fa STALE 
fe80::109b:d06f:f2be:1dc4 dev vmbr0 lladdr 16:bc:55:38:d3:7f STALE 
fe80::ec58:8902:551a:c823 dev vmbr0 lladdr bc:24:11:1e:61:cf STALE 
fe80::4924:f822:d560:bc2f dev vmbr0 lladdr bc:24:11:f6:74:e8 STALE 
fe80::7172:40ba:b966:69df dev vmbr0 lladdr 2c:54:91:2a:0d:5b STALE 
fe80::b6f4:eaa:36af:1d47 dev vmbr0 lladdr f0:6e:0b:cf:c7:55 STALE 
fe80::ae76:5582:7949:6783 dev vmbr0 lladdr 2c:54:91:2a:0d:5b STALE 
fe80::be24:11ff:fec3:dc75 dev vmbr0 lladdr bc:24:11:c3:dc:75 STALE 
fe80::b40f:d2ff:fe8b:6aec dev vmbr0 lladdr b6:0f:d2:8b:6a:ec STALE 
fe80::ef5a:24f4:f260:2b1e dev vmbr0 lladdr bc:24:11:44:73:92 STALE 
fe80::ac15:1b59:37bb:96f5 dev vmbr0 lladdr 9c:6b:00:9d:1c:48 STALE 
fe80::be24:11ff:febb:6af dev vmbr0 lladdr bc:24:11:bb:06:af STALE 
fe80::afa2:9f93:a83a:8815 dev vmbr0 lladdr bc:24:11:eb:f0:0f STALE 
fe80::be24:11ff:fef6:74e8 dev vmbr0 lladdr bc:24:11:f6:74:e8 STALE 
fe80::966:b4b8:282d:dff8 dev vmbr0 lladdr bc:24:11:27:4f:1c STALE 
fe80::562b:57ff:fe4b:7c72 dev vmbr0 lladdr 54:2b:57:4b:7c:72 STALE 
fe80::54f2:477f:64f3:562c dev vmbr0 lladdr bc:24:11:5c:96:1e STALE 
fe80::1d:8fb:68fc:746 dev vmbr0 lladdr 74:29:59:27:3a:b7 STALE 
fe80::466:5100:c752:a95d dev vmbr0 lladdr ca:c3:35:a4:7f:c4 STALE 
fe80::30b4:e59a:dbc:6700 dev vmbr0 lladdr bc:24:11:e4:37:53 STALE 
fe80::6e4b:b4ff:fe10:4061 dev vmbr0 lladdr 6c:4b:b4:10:40:61 router STALE 
fe80::be24:11ff:fee6:32d dev vmbr0 lladdr bc:24:11:e6:03:2d STALE 
fe80::1175:ecfd:44b2:57cb dev vmbr0 lladdr bc:24:11:38:c0:58 STALE 
fe80::2e8d:48ff:fe22:31c dev vmbr0 lladdr 2c:8d:48:22:03:1c STALE 
fe80::54e4:4111:b359:b994 dev vmbr0 lladdr 96:86:dd:1b:81:5a STALE 
fe80::eb49:b5fa:c882:b02c dev vmbr0 lladdr bc:24:11:ee:7e:7b STALE 
fe80::36bd:c8ff:fe2d:18c5 dev vmbr0 lladdr 34:bd:c8:2d:18:c5 STALE 
fe80::6bea:ca7:4c8c:182f dev vmbr0 lladdr bc:24:11:80:0d:16 STALE 
fe80::be24:11ff:fea3:8761 dev vmbr0 lladdr bc:24:11:a3:87:61 STALE 

--- /proc/net/dev (counters)
    $ cat /proc/net/dev
Inter-|   Receive                                                |  Transmit
 face |bytes    packets errs drop fifo frame compressed multicast|bytes    packets errs drop fifo colls carrier compressed
    lo: 61315931  378561    0    0    0     0          0         0 61315931  378561    0    0    0     0       0          0
  nic0: 3350233895 12198574    0 7183    0     0          0   5084318 5306247835 6212008    0    3    0     0       0          0
  nic1: 99924305026 70595086    0  175    0     0          0    147009 23560468511 33694852    0    0    0     0       0          0
  nic2: 22572716408 16421058    0    0    0     0          0     60090 5686269766 6976654    0    0    0     0       0          0
  nic3: 24123415  239733    0    0    0     0          0    214489  2045720    7862    0    0    0     0       0          0
  nic4:       0       0    0    0    0     0          0         0        0       0    0    0    0     0       0          0
  nic5:       0       0    0    0    0     0          0         0        0       0    0    0    0     0       0          0
 vmbr0: 1076025001 7927410    0    0    0     0          0   4217692 4826879122 1451133    0    3    0     0       0          0
tailscale0: 163474125 1146444    0    0    0     0          0         0 8056225151  978816    0    0    0     0       0          0
nic3.2:       0       0    0    0    0     0          0         0      906       7    0    0    0     0       0          0
br-rr-mgmt:       0       0    0    0    0     0          0         0      906       7    0    0    0     0       0          0
 bond0: 122497021434 87016144    0 14537    0     0          0    207099 29246738277 40671506    0    0    0     0       0          0
storagenet: 118054783660 31981665    0    5    0     0          0    178369 28189424191 27053335    0    0    0     0       0          0
tap100i0:  918971    9300    0    0    0     0          0         0 476741485 4413496    0    0    0     0       0          0
fwbr100i0: 412699863 4399535    0 6271    0     0          0   2963679        0       0    0    0    0     0       0          0
fwpr100p0: 2245643   14628    0 5328    0     0          0         0 476746813 4413496    0    0    0     0       0          0
fwln100i0: 476746813 4413496    0 5328    0     0          0         0  2245643   14628    0    0    0     0       0          0
tap600i0: 90214677  426674    0    0    0     0          0         0 676443159 5109206    0    0    0     0       0          0
fwbr600i0: 412689435 4399415    0 6270    0     0          0   2963609        0       0    0    0    0     0       0          0
fwpr600p0: 91541349  432002    0 5328    0     0          0         0 676448701 5109207    0    0    0     0       0          0
fwln600i0: 676448701 5109207    0 5328    0     0          0         0 91541349  432002    0    0    0     0       0          0
tap601i0: 89307849  438886    0    0    0     0          0         0 1008239703 5140324    0    0    0     0       0          0
fwbr601i0: 412674723 4399278    0 6270    0     0          0   2963540        0       0    0    0    0     0       0          0
fwpr601p0: 90634272  444213    0 5327    0     0          0         0 1008245030 5140324    0    0    0     0       0          0
fwln601i0: 1008245030 5140324    0 5327    0     0          0         0 90634272  444213    0    0    0     0       0          0

--- ip -6 route (brief)
    $ ip -6 route
fd7a:115c:a1e0::df3b:236f dev tailscale0 proto kernel metric 256 pref medium
fe80::/64 dev vmbr0 proto kernel metric 256 pref medium
fe80::/64 dev tailscale0 proto kernel metric 256 pref medium
fe80::/64 dev nic3 proto kernel metric 256 pref medium
fe80::/64 dev br-rr-mgmt proto kernel metric 256 pref medium
fe80::/64 dev storagenet proto kernel metric 256 pref medium

--- sysfs interface attributes
    $ for ifc in $NETIFS; do
    d="/sys/class/net/$ifc"
    [ -d "$d" ] || continue
    printf '%-16s speed=%-8s duplex=%-8s mtu=%-6s carrier=%-3s tx_queue_len=%-5s qlen=%-5s type=%s\n' \
        "$ifc" \
        "$(cat "$d/speed" 2>/dev/null)" \
        "$(cat "$d/duplex" 2>/dev/null)" \
        "$(cat "$d/mtu" 2>/dev/null)" \
        "$(cat "$d/carrier" 2>/dev/null)" \
        "$(cat "$d/tx_queue_len" 2>/dev/null)" \
        "$(cat "$d/tx_queue_len" 2>/dev/null)" \
        "$(cat "$d/type" 2>/dev/null)"
done
bond0            speed=2000     duplex=full     mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
br-rr-mgmt       speed=100      duplex=unknown  mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
fwbr100i0        speed=10000    duplex=unknown  mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
fwbr600i0        speed=10000    duplex=unknown  mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
fwbr601i0        speed=10000    duplex=unknown  mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
fwln100i0        speed=10000    duplex=full     mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
fwln600i0        speed=10000    duplex=full     mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
fwln601i0        speed=10000    duplex=full     mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
fwpr100p0        speed=10000    duplex=full     mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
fwpr600p0        speed=10000    duplex=full     mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
fwpr601p0        speed=10000    duplex=full     mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
nic0             speed=1000     duplex=full     mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
nic1             speed=1000     duplex=full     mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
nic2             speed=1000     duplex=full     mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
nic3             speed=100      duplex=full     mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
nic3.2           speed=100      duplex=full     mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
nic4             speed=         duplex=         mtu=1500   carrier=    tx_queue_len=1000  qlen=1000  type=1
nic5             speed=         duplex=         mtu=1500   carrier=    tx_queue_len=1000  qlen=1000  type=1
storagenet       speed=2000     duplex=unknown  mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
tap100i0         speed=10000    duplex=full     mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
tap600i0         speed=10000    duplex=full     mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
tap601i0         speed=10000    duplex=full     mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1
vmbr0            speed=10000    duplex=unknown  mtu=1500   carrier=1   tx_queue_len=1000  qlen=1000  type=1

--- ethtool per-interface deep dump
    $ for ifc in $NETIFS; do
    [ -e "/sys/class/net/$ifc" ] || continue
    echo ""
    echo "----- ethtool: $ifc -----"
    echo "[driver/version/firmware/bus-info -i]"
    ethtool -i "$ifc" 2>&1
    echo "[settings - speed/duplex/autoneg/port]"
    ethtool "$ifc" 2>&1
    echo "[channels -l (RX/TX/combined queue counts)]"
    ethtool -l "$ifc" 2>&1
    echo "[coalesce -c (interrupt moderation)]"
    ethtool -c "$ifc" 2>&1
    echo "[ring -g (descriptor counts)]"
    ethtool -g "$ifc" 2>&1
    echo "[pause / flow-control -a]"
    ethtool -a "$ifc" 2>&1
    echo "[offload features -k]"
    ethtool -k "$ifc" 2>&1
    echo "[private flags --show-priv-flags]"
    ethtool --show-priv-flags "$ifc" 2>&1
    echo "[ntuple/RSS -n]"
    ethtool -n "$ifc" 2>&1 | head -n 40
    echo "[SFP/DOM transceiver -m]"
    ethtool -m "$ifc" 2>&1
    echo "[statistics -S (key error/drop counters only)]"
    ethtool -S "$ifc" 2>/dev/null \
        | grep -iE 'drop|discard|error|crc|miss|pause|fifo|no_buff|rx_no_|_err|fw_|_bad|oversiz|undersize|frag|jabber|length_err|alignment' \
        | head -n 60
    echo "[statistics -S (throughput counters)]"
    ethtool -S "$ifc" 2>/dev/null \
        | grep -iE 'rx_(octets|bytes|packets)|tx_(octets|bytes|packets)|rx_(unicast|multicast|broadcast)|tx_(unicast|multicast|broadcast)' \
        | head -n 30
done

----- ethtool: bond0 -----
[driver/version/firmware/bus-info -i]
driver: bonding
version: 7.0.14-6-pve
firmware-version: 2
expansion-rom-version: 
bus-info: 
supports-statistics: no
supports-test: no
supports-eeprom-access: no
supports-register-dump: no
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for bond0:
	Supported ports: [  ]
	Supported link modes:   Not reported
	Supported pause frame use: No
	Supports auto-negotiation: No
	Supported FEC modes: Not reported
	Advertised link modes:  Not reported
	Advertised pause frame use: No
	Advertised auto-negotiation: No
	Advertised FEC modes: Not reported
	Speed: 2000Mb/s
	Duplex: Full
	Auto-negotiation: off
	Port: Other
	PHYAD: 0
	Transceiver: internal
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
netlink error: Operation not supported
[coalesce -c (interrupt moderation)]
netlink error: Operation not supported
[ring -g (descriptor counts)]
netlink error: Operation not supported
[pause / flow-control -a]
netlink error: Operation not supported
[offload features -k]
Features for bond0:
rx-checksumming: off [fixed]
tx-checksumming: on
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: on
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: off [fixed]
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: off [requested on]
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: on
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: off [requested on]
generic-segmentation-offload: on
generic-receive-offload: on
large-receive-offload: off
rx-vlan-offload: on
tx-vlan-offload: on [fixed]
ntuple-filters: off [fixed]
receive-hashing: off [fixed]
highdma: on
rx-vlan-filter: on
vlan-challenged: off [fixed]
tx-gso-robust: off [fixed]
tx-fcoe-segmentation: off [fixed]
tx-gre-segmentation: on
tx-gre-csum-segmentation: on
tx-ipxip4-segmentation: on
tx-ipxip6-segmentation: on
tx-udp_tnl-segmentation: on
tx-udp_tnl-csum-segmentation: on
tx-gso-partial: on [fixed]
tx-tunnel-remcsum-segmentation: off [fixed]
tx-sctp-segmentation: off [requested on]
tx-esp-segmentation: off
tx-udp-segmentation: off [requested on]
tx-gso-list: off [requested on]
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: on [fixed]
rx-vlan-stag-hw-parse: on
rx-vlan-stag-filter: on
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off
esp-tx-csum-hw-offload: off
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
[statistics -S (throughput counters)]

----- ethtool: br-rr-mgmt -----
[driver/version/firmware/bus-info -i]
driver: bridge
version: 2.3
firmware-version: N/A
expansion-rom-version: 
bus-info: N/A
supports-statistics: no
supports-test: no
supports-eeprom-access: no
supports-register-dump: no
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for br-rr-mgmt:
	Supported ports: [  ]
	Supported link modes:   Not reported
	Supported pause frame use: No
	Supports auto-negotiation: No
	Supported FEC modes: Not reported
	Advertised link modes:  Not reported
	Advertised pause frame use: No
	Advertised auto-negotiation: No
	Advertised FEC modes: Not reported
	Speed: 100Mb/s
	Duplex: Unknown! (255)
	Auto-negotiation: off
	Port: Other
	PHYAD: 0
	Transceiver: internal
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
netlink error: Operation not supported
[coalesce -c (interrupt moderation)]
netlink error: Operation not supported
[ring -g (descriptor counts)]
netlink error: Operation not supported
[pause / flow-control -a]
netlink error: Operation not supported
[offload features -k]
Features for br-rr-mgmt:
rx-checksumming: off [fixed]
tx-checksumming: on
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: on
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: off [fixed]
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: off [requested on]
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: on
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: on
generic-segmentation-offload: on
generic-receive-offload: on
large-receive-offload: off [fixed]
rx-vlan-offload: off [fixed]
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: off [fixed]
highdma: on
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [requested on]
tx-fcoe-segmentation: off [requested on]
tx-gre-segmentation: on
tx-gre-csum-segmentation: on
tx-ipxip4-segmentation: on
tx-ipxip6-segmentation: on
tx-udp_tnl-segmentation: on
tx-udp_tnl-csum-segmentation: on
tx-gso-partial: on
tx-tunnel-remcsum-segmentation: on
tx-sctp-segmentation: on
tx-esp-segmentation: on
tx-udp-segmentation: on
tx-gso-list: on
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: on
rx-vlan-stag-hw-parse: off [fixed]
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
[statistics -S (throughput counters)]

----- ethtool: fwbr100i0 -----
[driver/version/firmware/bus-info -i]
driver: bridge
version: 2.3
firmware-version: N/A
expansion-rom-version: 
bus-info: N/A
supports-statistics: no
supports-test: no
supports-eeprom-access: no
supports-register-dump: no
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for fwbr100i0:
	Supported ports: [  ]
	Supported link modes:   Not reported
	Supported pause frame use: No
	Supports auto-negotiation: No
	Supported FEC modes: Not reported
	Advertised link modes:  Not reported
	Advertised pause frame use: No
	Advertised auto-negotiation: No
	Advertised FEC modes: Not reported
	Speed: 10000Mb/s
	Duplex: Unknown! (255)
	Auto-negotiation: off
	Port: Other
	PHYAD: 0
	Transceiver: internal
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
netlink error: Operation not supported
[coalesce -c (interrupt moderation)]
netlink error: Operation not supported
[ring -g (descriptor counts)]
netlink error: Operation not supported
[pause / flow-control -a]
netlink error: Operation not supported
[offload features -k]
Features for fwbr100i0:
rx-checksumming: off [fixed]
tx-checksumming: on
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: on
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: off [fixed]
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: on
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: on
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: on
generic-segmentation-offload: on
generic-receive-offload: on
large-receive-offload: off [fixed]
rx-vlan-offload: off [fixed]
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: off [fixed]
highdma: on
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [requested on]
tx-fcoe-segmentation: off [requested on]
tx-gre-segmentation: on
tx-gre-csum-segmentation: on
tx-ipxip4-segmentation: on
tx-ipxip6-segmentation: on
tx-udp_tnl-segmentation: on
tx-udp_tnl-csum-segmentation: on
tx-gso-partial: on
tx-tunnel-remcsum-segmentation: on
tx-sctp-segmentation: on
tx-esp-segmentation: on
tx-udp-segmentation: on
tx-gso-list: on
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: on
rx-vlan-stag-hw-parse: off [fixed]
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
[statistics -S (throughput counters)]

----- ethtool: fwbr600i0 -----
[driver/version/firmware/bus-info -i]
driver: bridge
version: 2.3
firmware-version: N/A
expansion-rom-version: 
bus-info: N/A
supports-statistics: no
supports-test: no
supports-eeprom-access: no
supports-register-dump: no
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for fwbr600i0:
	Supported ports: [  ]
	Supported link modes:   Not reported
	Supported pause frame use: No
	Supports auto-negotiation: No
	Supported FEC modes: Not reported
	Advertised link modes:  Not reported
	Advertised pause frame use: No
	Advertised auto-negotiation: No
	Advertised FEC modes: Not reported
	Speed: 10000Mb/s
	Duplex: Unknown! (255)
	Auto-negotiation: off
	Port: Other
	PHYAD: 0
	Transceiver: internal
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
netlink error: Operation not supported
[coalesce -c (interrupt moderation)]
netlink error: Operation not supported
[ring -g (descriptor counts)]
netlink error: Operation not supported
[pause / flow-control -a]
netlink error: Operation not supported
[offload features -k]
Features for fwbr600i0:
rx-checksumming: off [fixed]
tx-checksumming: on
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: on
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: off [fixed]
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: on
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: on
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: on
generic-segmentation-offload: on
generic-receive-offload: on
large-receive-offload: off [fixed]
rx-vlan-offload: off [fixed]
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: off [fixed]
highdma: on
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [requested on]
tx-fcoe-segmentation: off [requested on]
tx-gre-segmentation: on
tx-gre-csum-segmentation: on
tx-ipxip4-segmentation: on
tx-ipxip6-segmentation: on
tx-udp_tnl-segmentation: on
tx-udp_tnl-csum-segmentation: on
tx-gso-partial: on
tx-tunnel-remcsum-segmentation: on
tx-sctp-segmentation: on
tx-esp-segmentation: on
tx-udp-segmentation: on
tx-gso-list: on
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: on
rx-vlan-stag-hw-parse: off [fixed]
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
[statistics -S (throughput counters)]

----- ethtool: fwbr601i0 -----
[driver/version/firmware/bus-info -i]
driver: bridge
version: 2.3
firmware-version: N/A
expansion-rom-version: 
bus-info: N/A
supports-statistics: no
supports-test: no
supports-eeprom-access: no
supports-register-dump: no
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for fwbr601i0:
	Supported ports: [  ]
	Supported link modes:   Not reported
	Supported pause frame use: No
	Supports auto-negotiation: No
	Supported FEC modes: Not reported
	Advertised link modes:  Not reported
	Advertised pause frame use: No
	Advertised auto-negotiation: No
	Advertised FEC modes: Not reported
	Speed: 10000Mb/s
	Duplex: Unknown! (255)
	Auto-negotiation: off
	Port: Other
	PHYAD: 0
	Transceiver: internal
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
netlink error: Operation not supported
[coalesce -c (interrupt moderation)]
netlink error: Operation not supported
[ring -g (descriptor counts)]
netlink error: Operation not supported
[pause / flow-control -a]
netlink error: Operation not supported
[offload features -k]
Features for fwbr601i0:
rx-checksumming: off [fixed]
tx-checksumming: on
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: on
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: off [fixed]
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: on
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: on
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: on
generic-segmentation-offload: on
generic-receive-offload: on
large-receive-offload: off [fixed]
rx-vlan-offload: off [fixed]
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: off [fixed]
highdma: on
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [requested on]
tx-fcoe-segmentation: off [requested on]
tx-gre-segmentation: on
tx-gre-csum-segmentation: on
tx-ipxip4-segmentation: on
tx-ipxip6-segmentation: on
tx-udp_tnl-segmentation: on
tx-udp_tnl-csum-segmentation: on
tx-gso-partial: on
tx-tunnel-remcsum-segmentation: on
tx-sctp-segmentation: on
tx-esp-segmentation: on
tx-udp-segmentation: on
tx-gso-list: on
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: on
rx-vlan-stag-hw-parse: off [fixed]
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
[statistics -S (throughput counters)]

----- ethtool: fwln100i0 -----
[driver/version/firmware/bus-info -i]
driver: veth
version: 1.0
firmware-version: 
expansion-rom-version: 
bus-info: 
supports-statistics: yes
supports-test: no
supports-eeprom-access: no
supports-register-dump: no
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for fwln100i0:
	Supported ports: [  ]
	Supported link modes:   Not reported
	Supported pause frame use: No
	Supports auto-negotiation: No
	Supported FEC modes: Not reported
	Advertised link modes:  Not reported
	Advertised pause frame use: No
	Advertised auto-negotiation: No
	Advertised FEC modes: Not reported
	Speed: 10000Mb/s
	Duplex: Full
	Auto-negotiation: off
	Port: Twisted Pair
	PHYAD: 0
	Transceiver: internal
	MDI-X: Unknown
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
Channel parameters for fwln100i0:
Pre-set maximums:
RX:		16
TX:		16
Other:		n/a
Combined:	n/a
Current hardware settings:
RX:		1
TX:		1
Other:		n/a
Combined:	n/a
[coalesce -c (interrupt moderation)]
netlink error: Operation not supported
[ring -g (descriptor counts)]
netlink error: Operation not supported
[pause / flow-control -a]
netlink error: Operation not supported
[offload features -k]
Features for fwln100i0:
rx-checksumming: on
tx-checksumming: on
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: on
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: on
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: on
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: on
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: on
generic-segmentation-offload: on
generic-receive-offload: off
large-receive-offload: off [fixed]
rx-vlan-offload: on
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: off [fixed]
highdma: on
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [fixed]
tx-fcoe-segmentation: off [fixed]
tx-gre-segmentation: on
tx-gre-csum-segmentation: on
tx-ipxip4-segmentation: on
tx-ipxip6-segmentation: on
tx-udp_tnl-segmentation: on
tx-udp_tnl-csum-segmentation: on
tx-gso-partial: off [fixed]
tx-tunnel-remcsum-segmentation: off [fixed]
tx-sctp-segmentation: on
tx-esp-segmentation: off [fixed]
tx-udp-segmentation: on
tx-gso-list: on
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: on
rx-vlan-stag-hw-parse: on
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
     rx_queue_0_drops: 0
     rx_queue_0_xdp_drops: 0
     rx_queue_0_xdp_tx_errors: 0
     tx_queue_0_xdp_xmit_errors: 0
[statistics -S (throughput counters)]

----- ethtool: fwln600i0 -----
[driver/version/firmware/bus-info -i]
driver: veth
version: 1.0
firmware-version: 
expansion-rom-version: 
bus-info: 
supports-statistics: yes
supports-test: no
supports-eeprom-access: no
supports-register-dump: no
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for fwln600i0:
	Supported ports: [  ]
	Supported link modes:   Not reported
	Supported pause frame use: No
	Supports auto-negotiation: No
	Supported FEC modes: Not reported
	Advertised link modes:  Not reported
	Advertised pause frame use: No
	Advertised auto-negotiation: No
	Advertised FEC modes: Not reported
	Speed: 10000Mb/s
	Duplex: Full
	Auto-negotiation: off
	Port: Twisted Pair
	PHYAD: 0
	Transceiver: internal
	MDI-X: Unknown
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
Channel parameters for fwln600i0:
Pre-set maximums:
RX:		16
TX:		16
Other:		n/a
Combined:	n/a
Current hardware settings:
RX:		1
TX:		1
Other:		n/a
Combined:	n/a
[coalesce -c (interrupt moderation)]
netlink error: Operation not supported
[ring -g (descriptor counts)]
netlink error: Operation not supported
[pause / flow-control -a]
netlink error: Operation not supported
[offload features -k]
Features for fwln600i0:
rx-checksumming: on
tx-checksumming: on
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: on
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: on
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: on
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: on
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: on
generic-segmentation-offload: on
generic-receive-offload: off
large-receive-offload: off [fixed]
rx-vlan-offload: on
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: off [fixed]
highdma: on
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [fixed]
tx-fcoe-segmentation: off [fixed]
tx-gre-segmentation: on
tx-gre-csum-segmentation: on
tx-ipxip4-segmentation: on
tx-ipxip6-segmentation: on
tx-udp_tnl-segmentation: on
tx-udp_tnl-csum-segmentation: on
tx-gso-partial: off [fixed]
tx-tunnel-remcsum-segmentation: off [fixed]
tx-sctp-segmentation: on
tx-esp-segmentation: off [fixed]
tx-udp-segmentation: on
tx-gso-list: on
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: on
rx-vlan-stag-hw-parse: on
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
     rx_queue_0_drops: 0
     rx_queue_0_xdp_drops: 0
     rx_queue_0_xdp_tx_errors: 0
     tx_queue_0_xdp_xmit_errors: 0
[statistics -S (throughput counters)]

----- ethtool: fwln601i0 -----
[driver/version/firmware/bus-info -i]
driver: veth
version: 1.0
firmware-version: 
expansion-rom-version: 
bus-info: 
supports-statistics: yes
supports-test: no
supports-eeprom-access: no
supports-register-dump: no
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for fwln601i0:
	Supported ports: [  ]
	Supported link modes:   Not reported
	Supported pause frame use: No
	Supports auto-negotiation: No
	Supported FEC modes: Not reported
	Advertised link modes:  Not reported
	Advertised pause frame use: No
	Advertised auto-negotiation: No
	Advertised FEC modes: Not reported
	Speed: 10000Mb/s
	Duplex: Full
	Auto-negotiation: off
	Port: Twisted Pair
	PHYAD: 0
	Transceiver: internal
	MDI-X: Unknown
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
Channel parameters for fwln601i0:
Pre-set maximums:
RX:		16
TX:		16
Other:		n/a
Combined:	n/a
Current hardware settings:
RX:		1
TX:		1
Other:		n/a
Combined:	n/a
[coalesce -c (interrupt moderation)]
netlink error: Operation not supported
[ring -g (descriptor counts)]
netlink error: Operation not supported
[pause / flow-control -a]
netlink error: Operation not supported
[offload features -k]
Features for fwln601i0:
rx-checksumming: on
tx-checksumming: on
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: on
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: on
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: on
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: on
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: on
generic-segmentation-offload: on
generic-receive-offload: off
large-receive-offload: off [fixed]
rx-vlan-offload: on
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: off [fixed]
highdma: on
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [fixed]
tx-fcoe-segmentation: off [fixed]
tx-gre-segmentation: on
tx-gre-csum-segmentation: on
tx-ipxip4-segmentation: on
tx-ipxip6-segmentation: on
tx-udp_tnl-segmentation: on
tx-udp_tnl-csum-segmentation: on
tx-gso-partial: off [fixed]
tx-tunnel-remcsum-segmentation: off [fixed]
tx-sctp-segmentation: on
tx-esp-segmentation: off [fixed]
tx-udp-segmentation: on
tx-gso-list: on
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: on
rx-vlan-stag-hw-parse: on
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
     rx_queue_0_drops: 0
     rx_queue_0_xdp_drops: 0
     rx_queue_0_xdp_tx_errors: 0
     tx_queue_0_xdp_xmit_errors: 0
[statistics -S (throughput counters)]

----- ethtool: fwpr100p0 -----
[driver/version/firmware/bus-info -i]
driver: veth
version: 1.0
firmware-version: 
expansion-rom-version: 
bus-info: 
supports-statistics: yes
supports-test: no
supports-eeprom-access: no
supports-register-dump: no
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for fwpr100p0:
	Supported ports: [  ]
	Supported link modes:   Not reported
	Supported pause frame use: No
	Supports auto-negotiation: No
	Supported FEC modes: Not reported
	Advertised link modes:  Not reported
	Advertised pause frame use: No
	Advertised auto-negotiation: No
	Advertised FEC modes: Not reported
	Speed: 10000Mb/s
	Duplex: Full
	Auto-negotiation: off
	Port: Twisted Pair
	PHYAD: 0
	Transceiver: internal
	MDI-X: Unknown
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
Channel parameters for fwpr100p0:
Pre-set maximums:
RX:		16
TX:		16
Other:		n/a
Combined:	n/a
Current hardware settings:
RX:		1
TX:		1
Other:		n/a
Combined:	n/a
[coalesce -c (interrupt moderation)]
netlink error: Operation not supported
[ring -g (descriptor counts)]
netlink error: Operation not supported
[pause / flow-control -a]
netlink error: Operation not supported
[offload features -k]
Features for fwpr100p0:
rx-checksumming: on
tx-checksumming: on
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: on
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: on
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: on
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: on
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: on
generic-segmentation-offload: on
generic-receive-offload: off
large-receive-offload: off [fixed]
rx-vlan-offload: on
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: off [fixed]
highdma: on
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [fixed]
tx-fcoe-segmentation: off [fixed]
tx-gre-segmentation: on
tx-gre-csum-segmentation: on
tx-ipxip4-segmentation: on
tx-ipxip6-segmentation: on
tx-udp_tnl-segmentation: on
tx-udp_tnl-csum-segmentation: on
tx-gso-partial: off [fixed]
tx-tunnel-remcsum-segmentation: off [fixed]
tx-sctp-segmentation: on
tx-esp-segmentation: off [fixed]
tx-udp-segmentation: on
tx-gso-list: on
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: on
rx-vlan-stag-hw-parse: on
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
     rx_queue_0_drops: 0
     rx_queue_0_xdp_drops: 0
     rx_queue_0_xdp_tx_errors: 0
     tx_queue_0_xdp_xmit_errors: 0
[statistics -S (throughput counters)]

----- ethtool: fwpr600p0 -----
[driver/version/firmware/bus-info -i]
driver: veth
version: 1.0
firmware-version: 
expansion-rom-version: 
bus-info: 
supports-statistics: yes
supports-test: no
supports-eeprom-access: no
supports-register-dump: no
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for fwpr600p0:
	Supported ports: [  ]
	Supported link modes:   Not reported
	Supported pause frame use: No
	Supports auto-negotiation: No
	Supported FEC modes: Not reported
	Advertised link modes:  Not reported
	Advertised pause frame use: No
	Advertised auto-negotiation: No
	Advertised FEC modes: Not reported
	Speed: 10000Mb/s
	Duplex: Full
	Auto-negotiation: off
	Port: Twisted Pair
	PHYAD: 0
	Transceiver: internal
	MDI-X: Unknown
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
Channel parameters for fwpr600p0:
Pre-set maximums:
RX:		16
TX:		16
Other:		n/a
Combined:	n/a
Current hardware settings:
RX:		1
TX:		1
Other:		n/a
Combined:	n/a
[coalesce -c (interrupt moderation)]
netlink error: Operation not supported
[ring -g (descriptor counts)]
netlink error: Operation not supported
[pause / flow-control -a]
netlink error: Operation not supported
[offload features -k]
Features for fwpr600p0:
rx-checksumming: on
tx-checksumming: on
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: on
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: on
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: on
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: on
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: on
generic-segmentation-offload: on
generic-receive-offload: off
large-receive-offload: off [fixed]
rx-vlan-offload: on
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: off [fixed]
highdma: on
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [fixed]
tx-fcoe-segmentation: off [fixed]
tx-gre-segmentation: on
tx-gre-csum-segmentation: on
tx-ipxip4-segmentation: on
tx-ipxip6-segmentation: on
tx-udp_tnl-segmentation: on
tx-udp_tnl-csum-segmentation: on
tx-gso-partial: off [fixed]
tx-tunnel-remcsum-segmentation: off [fixed]
tx-sctp-segmentation: on
tx-esp-segmentation: off [fixed]
tx-udp-segmentation: on
tx-gso-list: on
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: on
rx-vlan-stag-hw-parse: on
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
     rx_queue_0_drops: 0
     rx_queue_0_xdp_drops: 0
     rx_queue_0_xdp_tx_errors: 0
     tx_queue_0_xdp_xmit_errors: 0
[statistics -S (throughput counters)]

----- ethtool: fwpr601p0 -----
[driver/version/firmware/bus-info -i]
driver: veth
version: 1.0
firmware-version: 
expansion-rom-version: 
bus-info: 
supports-statistics: yes
supports-test: no
supports-eeprom-access: no
supports-register-dump: no
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for fwpr601p0:
	Supported ports: [  ]
	Supported link modes:   Not reported
	Supported pause frame use: No
	Supports auto-negotiation: No
	Supported FEC modes: Not reported
	Advertised link modes:  Not reported
	Advertised pause frame use: No
	Advertised auto-negotiation: No
	Advertised FEC modes: Not reported
	Speed: 10000Mb/s
	Duplex: Full
	Auto-negotiation: off
	Port: Twisted Pair
	PHYAD: 0
	Transceiver: internal
	MDI-X: Unknown
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
Channel parameters for fwpr601p0:
Pre-set maximums:
RX:		16
TX:		16
Other:		n/a
Combined:	n/a
Current hardware settings:
RX:		1
TX:		1
Other:		n/a
Combined:	n/a
[coalesce -c (interrupt moderation)]
netlink error: Operation not supported
[ring -g (descriptor counts)]
netlink error: Operation not supported
[pause / flow-control -a]
netlink error: Operation not supported
[offload features -k]
Features for fwpr601p0:
rx-checksumming: on
tx-checksumming: on
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: on
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: on
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: on
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: on
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: on
generic-segmentation-offload: on
generic-receive-offload: off
large-receive-offload: off [fixed]
rx-vlan-offload: on
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: off [fixed]
highdma: on
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [fixed]
tx-fcoe-segmentation: off [fixed]
tx-gre-segmentation: on
tx-gre-csum-segmentation: on
tx-ipxip4-segmentation: on
tx-ipxip6-segmentation: on
tx-udp_tnl-segmentation: on
tx-udp_tnl-csum-segmentation: on
tx-gso-partial: off [fixed]
tx-tunnel-remcsum-segmentation: off [fixed]
tx-sctp-segmentation: on
tx-esp-segmentation: off [fixed]
tx-udp-segmentation: on
tx-gso-list: on
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: on
rx-vlan-stag-hw-parse: on
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
     rx_queue_0_drops: 0
     rx_queue_0_xdp_drops: 0
     rx_queue_0_xdp_tx_errors: 0
     tx_queue_0_xdp_xmit_errors: 0
[statistics -S (throughput counters)]

----- ethtool: nic0 -----
[driver/version/firmware/bus-info -i]
driver: bnx2
version: 7.0.14-6-pve
firmware-version: 5.0.13 bc 5.0.11
expansion-rom-version: 
bus-info: 0000:01:00.0
supports-statistics: yes
supports-test: yes
supports-eeprom-access: yes
supports-register-dump: yes
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for nic0:
	Supported ports: [ TP ]
	Supported link modes:   10baseT/Half 10baseT/Full
	                        100baseT/Half 100baseT/Full
	                        1000baseT/Full
	Supported pause frame use: No
	Supports auto-negotiation: Yes
	Supported FEC modes: Not reported
	Advertised link modes:  10baseT/Half 10baseT/Full
	                        100baseT/Half 100baseT/Full
	                        1000baseT/Full
	Advertised pause frame use: No
	Advertised auto-negotiation: Yes
	Advertised FEC modes: Not reported
	Speed: 1000Mb/s
	Duplex: Full
	Auto-negotiation: on
	Port: Twisted Pair
	PHYAD: 1
	Transceiver: internal
	MDI-X: off
	Supports Wake-on: g
	Wake-on: d
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
Channel parameters for nic0:
Pre-set maximums:
RX:		8
TX:		8
Other:		n/a
Combined:	n/a
Current hardware settings:
RX:		5
TX:		4
Other:		n/a
Combined:	n/a
[coalesce -c (interrupt moderation)]
Coalesce parameters for nic0:
Adaptive RX: n/a  TX: n/a
stats-block-usecs:	999936
sample-interval:	n/a
pkt-rate-low:		n/a
pkt-rate-high:		n/a

rx-usecs:	18
rx-frames:	12
rx-usecs-irq:	18
rx-frames-irq:	2

tx-usecs:	80
tx-frames:	20
tx-usecs-irq:	18
tx-frames-irq:	2

rx-usecs-low:	n/a
rx-frame-low:	n/a
tx-usecs-low:	n/a
tx-frame-low:	n/a

rx-usecs-high:	n/a
rx-frame-high:	n/a
tx-usecs-high:	n/a
tx-frame-high:	n/a

CQE mode RX: n/a  TX: n/a

tx-aggr-max-bytes:	n/a
tx-aggr-max-frames:	n/a
tx-aggr-time-usecs:	n/a

[ring -g (descriptor counts)]
Ring parameters for nic0:
Pre-set maximums:
RX:			2040
RX Mini:		n/a
RX Jumbo:		8160
TX:			255
TX push buff len:	n/a
Current hardware settings:
RX:			255
RX Mini:		n/a
RX Jumbo:		0
TX:			255
RX Buf Len:		n/a
CQE Size:		n/a
TX Push:		off
RX Push:		off
TX push buff len:	n/a
TCP data split:		n/a
[pause / flow-control -a]
Pause parameters for nic0:
Autonegotiate:	on
RX:		off
TX:		off

[offload features -k]
Features for nic0:
rx-checksumming: on
tx-checksumming: on
	tx-checksum-ipv4: on
	tx-checksum-ip-generic: off [fixed]
	tx-checksum-ipv6: on
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: off [fixed]
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: off [fixed]
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: off
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: off [fixed]
generic-segmentation-offload: on
generic-receive-offload: on
large-receive-offload: off [fixed]
rx-vlan-offload: on
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: on
highdma: on [fixed]
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [fixed]
tx-fcoe-segmentation: off [fixed]
tx-gre-segmentation: off [fixed]
tx-gre-csum-segmentation: off [fixed]
tx-ipxip4-segmentation: off [fixed]
tx-ipxip6-segmentation: off [fixed]
tx-udp_tnl-segmentation: off [fixed]
tx-udp_tnl-csum-segmentation: off [fixed]
tx-gso-partial: off [fixed]
tx-tunnel-remcsum-segmentation: off [fixed]
tx-sctp-segmentation: off [fixed]
tx-esp-segmentation: off [fixed]
tx-udp-segmentation: off [fixed]
tx-gso-list: off [fixed]
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: off [fixed]
rx-vlan-stag-hw-parse: off [fixed]
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
     rx_error_bytes: 0
     tx_error_bytes: 0
     tx_mac_errors: 0
     tx_carrier_errors: 0
     rx_crc_errors: 0
     rx_align_errors: 0
     rx_fragments: 0
     rx_jabbers: 0
     rx_undersize_packets: 0
     rx_oversize_packets: 0
     rx_ftq_discards: 0
     rx_discards: 0
     rx_fw_discards: 1
[statistics -S (throughput counters)]
     rx_bytes: 3350261178
     tx_bytes: 5306269926

----- ethtool: nic1 -----
[driver/version/firmware/bus-info -i]
driver: bnx2
version: 7.0.14-6-pve
firmware-version: 5.0.13 bc 5.0.11 NCSI 2.0.5
expansion-rom-version: 
bus-info: 0000:01:00.1
supports-statistics: yes
supports-test: yes
supports-eeprom-access: yes
supports-register-dump: yes
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for nic1:
	Supported ports: [ TP ]
	Supported link modes:   10baseT/Half 10baseT/Full
	                        100baseT/Half 100baseT/Full
	                        1000baseT/Full
	Supported pause frame use: No
	Supports auto-negotiation: Yes
	Supported FEC modes: Not reported
	Advertised link modes:  10baseT/Half 10baseT/Full
	                        100baseT/Half 100baseT/Full
	                        1000baseT/Full
	Advertised pause frame use: No
	Advertised auto-negotiation: Yes
	Advertised FEC modes: Not reported
	Speed: 1000Mb/s
	Duplex: Full
	Auto-negotiation: on
	Port: Twisted Pair
	PHYAD: 1
	Transceiver: internal
	MDI-X: off
	Supports Wake-on: g
	Wake-on: d
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
Channel parameters for nic1:
Pre-set maximums:
RX:		8
TX:		8
Other:		n/a
Combined:	n/a
Current hardware settings:
RX:		5
TX:		4
Other:		n/a
Combined:	n/a
[coalesce -c (interrupt moderation)]
Coalesce parameters for nic1:
Adaptive RX: n/a  TX: n/a
stats-block-usecs:	999936
sample-interval:	n/a
pkt-rate-low:		n/a
pkt-rate-high:		n/a

rx-usecs:	18
rx-frames:	12
rx-usecs-irq:	18
rx-frames-irq:	2

tx-usecs:	80
tx-frames:	20
tx-usecs-irq:	18
tx-frames-irq:	2

rx-usecs-low:	n/a
rx-frame-low:	n/a
tx-usecs-low:	n/a
tx-frame-low:	n/a

rx-usecs-high:	n/a
rx-frame-high:	n/a
tx-usecs-high:	n/a
tx-frame-high:	n/a

CQE mode RX: n/a  TX: n/a

tx-aggr-max-bytes:	n/a
tx-aggr-max-frames:	n/a
tx-aggr-time-usecs:	n/a

[ring -g (descriptor counts)]
Ring parameters for nic1:
Pre-set maximums:
RX:			2040
RX Mini:		n/a
RX Jumbo:		8160
TX:			255
TX push buff len:	n/a
Current hardware settings:
RX:			255
RX Mini:		n/a
RX Jumbo:		0
TX:			255
RX Buf Len:		n/a
CQE Size:		n/a
TX Push:		off
RX Push:		off
TX push buff len:	n/a
TCP data split:		n/a
[pause / flow-control -a]
Pause parameters for nic1:
Autonegotiate:	on
RX:		off
TX:		off

[offload features -k]
Features for nic1:
rx-checksumming: on
tx-checksumming: on
	tx-checksum-ipv4: on
	tx-checksum-ip-generic: off [fixed]
	tx-checksum-ipv6: on
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: off [fixed]
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: off [fixed]
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: off
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: off [fixed]
generic-segmentation-offload: on
generic-receive-offload: on
large-receive-offload: off [fixed]
rx-vlan-offload: on [fixed]
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: on
highdma: on [fixed]
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [fixed]
tx-fcoe-segmentation: off [fixed]
tx-gre-segmentation: off [fixed]
tx-gre-csum-segmentation: off [fixed]
tx-ipxip4-segmentation: off [fixed]
tx-ipxip6-segmentation: off [fixed]
tx-udp_tnl-segmentation: off [fixed]
tx-udp_tnl-csum-segmentation: off [fixed]
tx-gso-partial: off [fixed]
tx-tunnel-remcsum-segmentation: off [fixed]
tx-sctp-segmentation: off [fixed]
tx-esp-segmentation: off [fixed]
tx-udp-segmentation: off [fixed]
tx-gso-list: off [fixed]
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: off [fixed]
rx-vlan-stag-hw-parse: off [fixed]
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
     rx_error_bytes: 0
     tx_error_bytes: 0
     tx_mac_errors: 0
     tx_carrier_errors: 0
     rx_crc_errors: 0
     rx_align_errors: 0
     rx_fragments: 0
     rx_jabbers: 0
     rx_undersize_packets: 0
     rx_oversize_packets: 0
     rx_ftq_discards: 0
     rx_discards: 0
     rx_fw_discards: 175
[statistics -S (throughput counters)]
     rx_bytes: 99924310944
     tx_bytes: 23560482805

----- ethtool: nic2 -----
[driver/version/firmware/bus-info -i]
driver: bnx2
version: 7.0.14-6-pve
firmware-version: 5.0.13 bc 5.0.11 NCSI 2.0.5
expansion-rom-version: 
bus-info: 0000:02:00.0
supports-statistics: yes
supports-test: yes
supports-eeprom-access: yes
supports-register-dump: yes
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for nic2:
	Supported ports: [ TP ]
	Supported link modes:   10baseT/Half 10baseT/Full
	                        100baseT/Half 100baseT/Full
	                        1000baseT/Full
	Supported pause frame use: No
	Supports auto-negotiation: Yes
	Supported FEC modes: Not reported
	Advertised link modes:  10baseT/Half 10baseT/Full
	                        100baseT/Half 100baseT/Full
	                        1000baseT/Full
	Advertised pause frame use: No
	Advertised auto-negotiation: Yes
	Advertised FEC modes: Not reported
	Speed: 1000Mb/s
	Duplex: Full
	Auto-negotiation: on
	Port: Twisted Pair
	PHYAD: 1
	Transceiver: internal
	MDI-X: on
	Supports Wake-on: g
	Wake-on: d
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
Channel parameters for nic2:
Pre-set maximums:
RX:		8
TX:		8
Other:		n/a
Combined:	n/a
Current hardware settings:
RX:		5
TX:		4
Other:		n/a
Combined:	n/a
[coalesce -c (interrupt moderation)]
Coalesce parameters for nic2:
Adaptive RX: n/a  TX: n/a
stats-block-usecs:	999936
sample-interval:	n/a
pkt-rate-low:		n/a
pkt-rate-high:		n/a

rx-usecs:	18
rx-frames:	12
rx-usecs-irq:	18
rx-frames-irq:	2

tx-usecs:	80
tx-frames:	20
tx-usecs-irq:	18
tx-frames-irq:	2

rx-usecs-low:	n/a
rx-frame-low:	n/a
tx-usecs-low:	n/a
tx-frame-low:	n/a

rx-usecs-high:	n/a
rx-frame-high:	n/a
tx-usecs-high:	n/a
tx-frame-high:	n/a

CQE mode RX: n/a  TX: n/a

tx-aggr-max-bytes:	n/a
tx-aggr-max-frames:	n/a
tx-aggr-time-usecs:	n/a

[ring -g (descriptor counts)]
Ring parameters for nic2:
Pre-set maximums:
RX:			2040
RX Mini:		n/a
RX Jumbo:		8160
TX:			255
TX push buff len:	n/a
Current hardware settings:
RX:			255
RX Mini:		n/a
RX Jumbo:		0
TX:			255
RX Buf Len:		n/a
CQE Size:		n/a
TX Push:		off
RX Push:		off
TX push buff len:	n/a
TCP data split:		n/a
[pause / flow-control -a]
Pause parameters for nic2:
Autonegotiate:	on
RX:		off
TX:		off

[offload features -k]
Features for nic2:
rx-checksumming: on
tx-checksumming: on
	tx-checksum-ipv4: on
	tx-checksum-ip-generic: off [fixed]
	tx-checksum-ipv6: on
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: off [fixed]
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: off [fixed]
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: off
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: off [fixed]
generic-segmentation-offload: on
generic-receive-offload: on
large-receive-offload: off [fixed]
rx-vlan-offload: on [fixed]
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: on
highdma: on [fixed]
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [fixed]
tx-fcoe-segmentation: off [fixed]
tx-gre-segmentation: off [fixed]
tx-gre-csum-segmentation: off [fixed]
tx-ipxip4-segmentation: off [fixed]
tx-ipxip6-segmentation: off [fixed]
tx-udp_tnl-segmentation: off [fixed]
tx-udp_tnl-csum-segmentation: off [fixed]
tx-gso-partial: off [fixed]
tx-tunnel-remcsum-segmentation: off [fixed]
tx-sctp-segmentation: off [fixed]
tx-esp-segmentation: off [fixed]
tx-udp-segmentation: off [fixed]
tx-gso-list: off [fixed]
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: off [fixed]
rx-vlan-stag-hw-parse: off [fixed]
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
     rx_error_bytes: 0
     tx_error_bytes: 0
     tx_mac_errors: 0
     tx_carrier_errors: 0
     rx_crc_errors: 0
     rx_align_errors: 0
     rx_fragments: 0
     rx_jabbers: 0
     rx_undersize_packets: 0
     rx_oversize_packets: 0
     rx_ftq_discards: 0
     rx_discards: 0
     rx_fw_discards: 0
[statistics -S (throughput counters)]
     rx_bytes: 22572718080
     tx_bytes: 5686270846

----- ethtool: nic3 -----
[driver/version/firmware/bus-info -i]
driver: bnx2
version: 7.0.14-6-pve
firmware-version: 5.0.13 bc 5.0.11 NCSI 2.0.5
expansion-rom-version: 
bus-info: 0000:02:00.1
supports-statistics: yes
supports-test: yes
supports-eeprom-access: yes
supports-register-dump: yes
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for nic3:
	Supported ports: [ TP ]
	Supported link modes:   10baseT/Half 10baseT/Full
	                        100baseT/Half 100baseT/Full
	                        1000baseT/Full
	Supported pause frame use: No
	Supports auto-negotiation: Yes
	Supported FEC modes: Not reported
	Advertised link modes:  10baseT/Half 10baseT/Full
	                        100baseT/Half 100baseT/Full
	                        1000baseT/Full
	Advertised pause frame use: No
	Advertised auto-negotiation: Yes
	Advertised FEC modes: Not reported
	Speed: 100Mb/s
	Duplex: Full
	Auto-negotiation: on
	Port: Twisted Pair
	PHYAD: 1
	Transceiver: internal
	MDI-X: on
	Supports Wake-on: g
	Wake-on: d
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
Channel parameters for nic3:
Pre-set maximums:
RX:		8
TX:		8
Other:		n/a
Combined:	n/a
Current hardware settings:
RX:		5
TX:		4
Other:		n/a
Combined:	n/a
[coalesce -c (interrupt moderation)]
Coalesce parameters for nic3:
Adaptive RX: n/a  TX: n/a
stats-block-usecs:	999936
sample-interval:	n/a
pkt-rate-low:		n/a
pkt-rate-high:		n/a

rx-usecs:	18
rx-frames:	12
rx-usecs-irq:	18
rx-frames-irq:	2

tx-usecs:	80
tx-frames:	20
tx-usecs-irq:	18
tx-frames-irq:	2

rx-usecs-low:	n/a
rx-frame-low:	n/a
tx-usecs-low:	n/a
tx-frame-low:	n/a

rx-usecs-high:	n/a
rx-frame-high:	n/a
tx-usecs-high:	n/a
tx-frame-high:	n/a

CQE mode RX: n/a  TX: n/a

tx-aggr-max-bytes:	n/a
tx-aggr-max-frames:	n/a
tx-aggr-time-usecs:	n/a

[ring -g (descriptor counts)]
Ring parameters for nic3:
Pre-set maximums:
RX:			2040
RX Mini:		n/a
RX Jumbo:		8160
TX:			255
TX push buff len:	n/a
Current hardware settings:
RX:			255
RX Mini:		n/a
RX Jumbo:		0
TX:			255
RX Buf Len:		n/a
CQE Size:		n/a
TX Push:		off
RX Push:		off
TX push buff len:	n/a
TCP data split:		n/a
[pause / flow-control -a]
Pause parameters for nic3:
Autonegotiate:	on
RX:		on
TX:		on

[offload features -k]
Features for nic3:
rx-checksumming: on
tx-checksumming: on
	tx-checksum-ipv4: on
	tx-checksum-ip-generic: off [fixed]
	tx-checksum-ipv6: on
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: off [fixed]
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: off [fixed]
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: off
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: off [fixed]
generic-segmentation-offload: on
generic-receive-offload: on
large-receive-offload: off [fixed]
rx-vlan-offload: on [fixed]
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: on
highdma: on [fixed]
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [fixed]
tx-fcoe-segmentation: off [fixed]
tx-gre-segmentation: off [fixed]
tx-gre-csum-segmentation: off [fixed]
tx-ipxip4-segmentation: off [fixed]
tx-ipxip6-segmentation: off [fixed]
tx-udp_tnl-segmentation: off [fixed]
tx-udp_tnl-csum-segmentation: off [fixed]
tx-gso-partial: off [fixed]
tx-tunnel-remcsum-segmentation: off [fixed]
tx-sctp-segmentation: off [fixed]
tx-esp-segmentation: off [fixed]
tx-udp-segmentation: off [fixed]
tx-gso-list: off [fixed]
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: off [fixed]
rx-vlan-stag-hw-parse: off [fixed]
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
     rx_error_bytes: 0
     tx_error_bytes: 0
     tx_mac_errors: 0
     tx_carrier_errors: 0
     rx_crc_errors: 0
     rx_align_errors: 0
     rx_fragments: 0
     rx_jabbers: 0
     rx_undersize_packets: 0
     rx_oversize_packets: 0
     rx_ftq_discards: 0
     rx_discards: 0
     rx_fw_discards: 0
[statistics -S (throughput counters)]
     rx_bytes: 24123415
     tx_bytes: 2045720

----- ethtool: nic3.2 -----
[driver/version/firmware/bus-info -i]
driver: 802.1Q VLAN Support
version: 1.8
firmware-version: N/A
expansion-rom-version: 
bus-info: 
supports-statistics: no
supports-test: no
supports-eeprom-access: no
supports-register-dump: no
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for nic3.2:
	Supported ports: [ TP ]
	Supported link modes:   10baseT/Half 10baseT/Full
	                        100baseT/Half 100baseT/Full
	                        1000baseT/Full
	Supported pause frame use: No
	Supports auto-negotiation: Yes
	Supported FEC modes: Not reported
	Advertised link modes:  10baseT/Half 10baseT/Full
	                        100baseT/Half 100baseT/Full
	                        1000baseT/Full
	Advertised pause frame use: No
	Advertised auto-negotiation: Yes
	Advertised FEC modes: Not reported
	Speed: 100Mb/s
	Duplex: Full
	Auto-negotiation: on
	Port: Twisted Pair
	PHYAD: 1
	Transceiver: internal
	MDI-X: on
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
netlink error: Operation not supported
[coalesce -c (interrupt moderation)]
netlink error: Operation not supported
[ring -g (descriptor counts)]
netlink error: Operation not supported
[pause / flow-control -a]
netlink error: Operation not supported
[offload features -k]
Features for nic3.2:
rx-checksumming: off [fixed]
tx-checksumming: on
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: on
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [requested on]
	tx-checksum-sctp: off [requested on]
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: off [requested on]
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: on
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: on
generic-segmentation-offload: on
generic-receive-offload: on
large-receive-offload: off [fixed]
rx-vlan-offload: off [fixed]
tx-vlan-offload: off [fixed]
ntuple-filters: off [fixed]
receive-hashing: off [fixed]
highdma: on
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [fixed]
tx-fcoe-segmentation: off [requested on]
tx-gre-segmentation: off [requested on]
tx-gre-csum-segmentation: off [requested on]
tx-ipxip4-segmentation: off [requested on]
tx-ipxip6-segmentation: off [requested on]
tx-udp_tnl-segmentation: off [requested on]
tx-udp_tnl-csum-segmentation: off [requested on]
tx-gso-partial: off [fixed]
tx-tunnel-remcsum-segmentation: off [fixed]
tx-sctp-segmentation: on
tx-esp-segmentation: off [fixed]
tx-udp-segmentation: on
tx-gso-list: on
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: off [fixed]
rx-vlan-stag-hw-parse: off [fixed]
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
[statistics -S (throughput counters)]

----- ethtool: nic4 -----
[driver/version/firmware/bus-info -i]
driver: bnx2
version: 7.0.14-6-pve
firmware-version: 5.0.13 bc 5.0.11
expansion-rom-version: 
bus-info: 0000:04:00.0
supports-statistics: yes
supports-test: yes
supports-eeprom-access: yes
supports-register-dump: yes
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for nic4:
	Supported ports: [ TP ]
	Supported link modes:   10baseT/Half 10baseT/Full
	                        100baseT/Half 100baseT/Full
	                        1000baseT/Full
	Supported pause frame use: No
	Supports auto-negotiation: Yes
	Supported FEC modes: Not reported
	Advertised link modes:  10baseT/Half 10baseT/Full
	                        100baseT/Half 100baseT/Full
	                        1000baseT/Full
	Advertised pause frame use: No
	Advertised auto-negotiation: Yes
	Advertised FEC modes: Not reported
	Speed: Unknown!
	Duplex: Half
	Auto-negotiation: on
	Port: Twisted Pair
	PHYAD: 1
	Transceiver: internal
	MDI-X: off
	Supports Wake-on: g
	Wake-on: d
	Link detected: no
[channels -l (RX/TX/combined queue counts)]
Channel parameters for nic4:
Pre-set maximums:
RX:		8
TX:		8
Other:		n/a
Combined:	n/a
Current hardware settings:
RX:		0
TX:		0
Other:		n/a
Combined:	n/a
[coalesce -c (interrupt moderation)]
Coalesce parameters for nic4:
Adaptive RX: n/a  TX: n/a
stats-block-usecs:	999936
sample-interval:	n/a
pkt-rate-low:		n/a
pkt-rate-high:		n/a

rx-usecs:	18
rx-frames:	12
rx-usecs-irq:	18
rx-frames-irq:	2

tx-usecs:	80
tx-frames:	20
tx-usecs-irq:	18
tx-frames-irq:	2

rx-usecs-low:	n/a
rx-frame-low:	n/a
tx-usecs-low:	n/a
tx-frame-low:	n/a

rx-usecs-high:	n/a
rx-frame-high:	n/a
tx-usecs-high:	n/a
tx-frame-high:	n/a

CQE mode RX: n/a  TX: n/a

tx-aggr-max-bytes:	n/a
tx-aggr-max-frames:	n/a
tx-aggr-time-usecs:	n/a

[ring -g (descriptor counts)]
Ring parameters for nic4:
Pre-set maximums:
RX:			2040
RX Mini:		n/a
RX Jumbo:		8160
TX:			255
TX push buff len:	n/a
Current hardware settings:
RX:			255
RX Mini:		n/a
RX Jumbo:		0
TX:			255
RX Buf Len:		n/a
CQE Size:		n/a
TX Push:		off
RX Push:		off
TX push buff len:	n/a
TCP data split:		n/a
[pause / flow-control -a]
Pause parameters for nic4:
Autonegotiate:	on
RX:		off
TX:		off

[offload features -k]
Features for nic4:
rx-checksumming: on
tx-checksumming: on
	tx-checksum-ipv4: on
	tx-checksum-ip-generic: off [fixed]
	tx-checksum-ipv6: on
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: off [fixed]
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: off [fixed]
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: off
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: off [fixed]
generic-segmentation-offload: on
generic-receive-offload: on
large-receive-offload: off [fixed]
rx-vlan-offload: on [fixed]
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: on
highdma: on [fixed]
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [fixed]
tx-fcoe-segmentation: off [fixed]
tx-gre-segmentation: off [fixed]
tx-gre-csum-segmentation: off [fixed]
tx-ipxip4-segmentation: off [fixed]
tx-ipxip6-segmentation: off [fixed]
tx-udp_tnl-segmentation: off [fixed]
tx-udp_tnl-csum-segmentation: off [fixed]
tx-gso-partial: off [fixed]
tx-tunnel-remcsum-segmentation: off [fixed]
tx-sctp-segmentation: off [fixed]
tx-esp-segmentation: off [fixed]
tx-udp-segmentation: off [fixed]
tx-gso-list: off [fixed]
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: off [fixed]
rx-vlan-stag-hw-parse: off [fixed]
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
     rx_error_bytes: 0
     tx_error_bytes: 0
     tx_mac_errors: 0
     tx_carrier_errors: 0
     rx_crc_errors: 0
     rx_align_errors: 0
     rx_fragments: 0
     rx_jabbers: 0
     rx_undersize_packets: 0
     rx_oversize_packets: 0
     rx_ftq_discards: 0
     rx_discards: 0
     rx_fw_discards: 0
[statistics -S (throughput counters)]
     rx_bytes: 0
     tx_bytes: 0

----- ethtool: nic5 -----
[driver/version/firmware/bus-info -i]
driver: bnx2
version: 7.0.14-6-pve
firmware-version: 5.0.13 bc 5.0.11
expansion-rom-version: 
bus-info: 0000:04:00.1
supports-statistics: yes
supports-test: yes
supports-eeprom-access: yes
supports-register-dump: yes
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for nic5:
	Supported ports: [ TP ]
	Supported link modes:   10baseT/Half 10baseT/Full
	                        100baseT/Half 100baseT/Full
	                        1000baseT/Full
	Supported pause frame use: No
	Supports auto-negotiation: Yes
	Supported FEC modes: Not reported
	Advertised link modes:  10baseT/Half 10baseT/Full
	                        100baseT/Half 100baseT/Full
	                        1000baseT/Full
	Advertised pause frame use: No
	Advertised auto-negotiation: Yes
	Advertised FEC modes: Not reported
	Speed: Unknown!
	Duplex: Half
	Auto-negotiation: on
	Port: Twisted Pair
	PHYAD: 1
	Transceiver: internal
	MDI-X: off
	Supports Wake-on: g
	Wake-on: d
	Link detected: no
[channels -l (RX/TX/combined queue counts)]
Channel parameters for nic5:
Pre-set maximums:
RX:		8
TX:		8
Other:		n/a
Combined:	n/a
Current hardware settings:
RX:		0
TX:		0
Other:		n/a
Combined:	n/a
[coalesce -c (interrupt moderation)]
Coalesce parameters for nic5:
Adaptive RX: n/a  TX: n/a
stats-block-usecs:	999936
sample-interval:	n/a
pkt-rate-low:		n/a
pkt-rate-high:		n/a

rx-usecs:	18
rx-frames:	12
rx-usecs-irq:	18
rx-frames-irq:	2

tx-usecs:	80
tx-frames:	20
tx-usecs-irq:	18
tx-frames-irq:	2

rx-usecs-low:	n/a
rx-frame-low:	n/a
tx-usecs-low:	n/a
tx-frame-low:	n/a

rx-usecs-high:	n/a
rx-frame-high:	n/a
tx-usecs-high:	n/a
tx-frame-high:	n/a

CQE mode RX: n/a  TX: n/a

tx-aggr-max-bytes:	n/a
tx-aggr-max-frames:	n/a
tx-aggr-time-usecs:	n/a

[ring -g (descriptor counts)]
Ring parameters for nic5:
Pre-set maximums:
RX:			2040
RX Mini:		n/a
RX Jumbo:		8160
TX:			255
TX push buff len:	n/a
Current hardware settings:
RX:			255
RX Mini:		n/a
RX Jumbo:		0
TX:			255
RX Buf Len:		n/a
CQE Size:		n/a
TX Push:		off
RX Push:		off
TX push buff len:	n/a
TCP data split:		n/a
[pause / flow-control -a]
Pause parameters for nic5:
Autonegotiate:	on
RX:		off
TX:		off

[offload features -k]
Features for nic5:
rx-checksumming: on
tx-checksumming: on
	tx-checksum-ipv4: on
	tx-checksum-ip-generic: off [fixed]
	tx-checksum-ipv6: on
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: off [fixed]
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: off [fixed]
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: off
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: off [fixed]
generic-segmentation-offload: on
generic-receive-offload: on
large-receive-offload: off [fixed]
rx-vlan-offload: on
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: on
highdma: on [fixed]
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [fixed]
tx-fcoe-segmentation: off [fixed]
tx-gre-segmentation: off [fixed]
tx-gre-csum-segmentation: off [fixed]
tx-ipxip4-segmentation: off [fixed]
tx-ipxip6-segmentation: off [fixed]
tx-udp_tnl-segmentation: off [fixed]
tx-udp_tnl-csum-segmentation: off [fixed]
tx-gso-partial: off [fixed]
tx-tunnel-remcsum-segmentation: off [fixed]
tx-sctp-segmentation: off [fixed]
tx-esp-segmentation: off [fixed]
tx-udp-segmentation: off [fixed]
tx-gso-list: off [fixed]
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: off [fixed]
rx-vlan-stag-hw-parse: off [fixed]
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
     rx_error_bytes: 0
     tx_error_bytes: 0
     tx_mac_errors: 0
     tx_carrier_errors: 0
     rx_crc_errors: 0
     rx_align_errors: 0
     rx_fragments: 0
     rx_jabbers: 0
     rx_undersize_packets: 0
     rx_oversize_packets: 0
     rx_ftq_discards: 0
     rx_discards: 0
     rx_fw_discards: 0
[statistics -S (throughput counters)]
     rx_bytes: 0
     tx_bytes: 0

----- ethtool: storagenet -----
[driver/version/firmware/bus-info -i]
driver: bridge
version: 2.3
firmware-version: N/A
expansion-rom-version: 
bus-info: N/A
supports-statistics: no
supports-test: no
supports-eeprom-access: no
supports-register-dump: no
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for storagenet:
	Supported ports: [  ]
	Supported link modes:   Not reported
	Supported pause frame use: No
	Supports auto-negotiation: No
	Supported FEC modes: Not reported
	Advertised link modes:  Not reported
	Advertised pause frame use: No
	Advertised auto-negotiation: No
	Advertised FEC modes: Not reported
	Speed: 2000Mb/s
	Duplex: Unknown! (255)
	Auto-negotiation: off
	Port: Other
	PHYAD: 0
	Transceiver: internal
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
netlink error: Operation not supported
[coalesce -c (interrupt moderation)]
netlink error: Operation not supported
[ring -g (descriptor counts)]
netlink error: Operation not supported
[pause / flow-control -a]
netlink error: Operation not supported
[offload features -k]
Features for storagenet:
rx-checksumming: off [fixed]
tx-checksumming: on
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: on
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: off [fixed]
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: off [requested on]
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: on
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: off [requested on]
generic-segmentation-offload: on
generic-receive-offload: on
large-receive-offload: off [fixed]
rx-vlan-offload: off [fixed]
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: off [fixed]
highdma: on
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [requested on]
tx-fcoe-segmentation: off [requested on]
tx-gre-segmentation: on
tx-gre-csum-segmentation: on
tx-ipxip4-segmentation: on
tx-ipxip6-segmentation: on
tx-udp_tnl-segmentation: on
tx-udp_tnl-csum-segmentation: on
tx-gso-partial: on
tx-tunnel-remcsum-segmentation: on
tx-sctp-segmentation: off [requested on]
tx-esp-segmentation: on
tx-udp-segmentation: off [requested on]
tx-gso-list: off [requested on]
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: on
rx-vlan-stag-hw-parse: off [fixed]
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
[statistics -S (throughput counters)]

----- ethtool: tap100i0 -----
[driver/version/firmware/bus-info -i]
driver: tun
version: 1.6
firmware-version: 
expansion-rom-version: 
bus-info: tap
supports-statistics: no
supports-test: no
supports-eeprom-access: no
supports-register-dump: no
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for tap100i0:
	Supported ports: [  ]
	Supported link modes:   Not reported
	Supported pause frame use: No
	Supports auto-negotiation: No
	Supported FEC modes: Not reported
	Advertised link modes:  Not reported
	Advertised pause frame use: No
	Advertised auto-negotiation: No
	Advertised FEC modes: Not reported
	Speed: 10000Mb/s
	Duplex: Full
	Auto-negotiation: off
	Port: Twisted Pair
	PHYAD: 0
	Transceiver: internal
	MDI-X: Unknown
        Current message level: 0x00000000 (0)
                              
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
Channel parameters for tap100i0:
Pre-set maximums:
RX:		n/a
TX:		n/a
Other:		n/a
Combined:	1
Current hardware settings:
RX:		n/a
TX:		n/a
Other:		n/a
Combined:	1
[coalesce -c (interrupt moderation)]
Coalesce parameters for tap100i0:
Adaptive RX: n/a  TX: n/a
stats-block-usecs:	n/a
sample-interval:	n/a
pkt-rate-low:		n/a
pkt-rate-high:		n/a

rx-usecs:	n/a
rx-frames:	0
rx-usecs-irq:	n/a
rx-frames-irq:	n/a

tx-usecs:	n/a
tx-frames:	n/a
tx-usecs-irq:	n/a
tx-frames-irq:	n/a

rx-usecs-low:	n/a
rx-frame-low:	n/a
tx-usecs-low:	n/a
tx-frame-low:	n/a

rx-usecs-high:	n/a
rx-frame-high:	n/a
tx-usecs-high:	n/a
tx-frame-high:	n/a

CQE mode RX: n/a  TX: n/a

tx-aggr-max-bytes:	n/a
tx-aggr-max-frames:	n/a
tx-aggr-time-usecs:	n/a

[ring -g (descriptor counts)]
netlink error: Operation not supported
[pause / flow-control -a]
netlink error: Operation not supported
[offload features -k]
Features for tap100i0:
rx-checksumming: off [fixed]
tx-checksumming: on
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: on
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: off [fixed]
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: on
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: off
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: off [fixed]
generic-segmentation-offload: on
generic-receive-offload: on
large-receive-offload: off [fixed]
rx-vlan-offload: off [fixed]
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: off [fixed]
highdma: off [fixed]
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [fixed]
tx-fcoe-segmentation: off [fixed]
tx-gre-segmentation: off [fixed]
tx-gre-csum-segmentation: off [fixed]
tx-ipxip4-segmentation: off [fixed]
tx-ipxip6-segmentation: off [fixed]
tx-udp_tnl-segmentation: off
tx-udp_tnl-csum-segmentation: off
tx-gso-partial: off [fixed]
tx-tunnel-remcsum-segmentation: off [fixed]
tx-sctp-segmentation: off [fixed]
tx-esp-segmentation: off [fixed]
tx-udp-segmentation: on
tx-gso-list: off [fixed]
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: on
rx-vlan-stag-hw-parse: off [fixed]
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
[statistics -S (throughput counters)]

----- ethtool: tap600i0 -----
[driver/version/firmware/bus-info -i]
driver: tun
version: 1.6
firmware-version: 
expansion-rom-version: 
bus-info: tap
supports-statistics: no
supports-test: no
supports-eeprom-access: no
supports-register-dump: no
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for tap600i0:
	Supported ports: [  ]
	Supported link modes:   Not reported
	Supported pause frame use: No
	Supports auto-negotiation: No
	Supported FEC modes: Not reported
	Advertised link modes:  Not reported
	Advertised pause frame use: No
	Advertised auto-negotiation: No
	Advertised FEC modes: Not reported
	Speed: 10000Mb/s
	Duplex: Full
	Auto-negotiation: off
	Port: Twisted Pair
	PHYAD: 0
	Transceiver: internal
	MDI-X: Unknown
        Current message level: 0x00000000 (0)
                              
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
Channel parameters for tap600i0:
Pre-set maximums:
RX:		n/a
TX:		n/a
Other:		n/a
Combined:	1
Current hardware settings:
RX:		n/a
TX:		n/a
Other:		n/a
Combined:	1
[coalesce -c (interrupt moderation)]
Coalesce parameters for tap600i0:
Adaptive RX: n/a  TX: n/a
stats-block-usecs:	n/a
sample-interval:	n/a
pkt-rate-low:		n/a
pkt-rate-high:		n/a

rx-usecs:	n/a
rx-frames:	0
rx-usecs-irq:	n/a
rx-frames-irq:	n/a

tx-usecs:	n/a
tx-frames:	n/a
tx-usecs-irq:	n/a
tx-frames-irq:	n/a

rx-usecs-low:	n/a
rx-frame-low:	n/a
tx-usecs-low:	n/a
tx-frame-low:	n/a

rx-usecs-high:	n/a
rx-frame-high:	n/a
tx-usecs-high:	n/a
tx-frame-high:	n/a

CQE mode RX: n/a  TX: n/a

tx-aggr-max-bytes:	n/a
tx-aggr-max-frames:	n/a
tx-aggr-time-usecs:	n/a

[ring -g (descriptor counts)]
netlink error: Operation not supported
[pause / flow-control -a]
netlink error: Operation not supported
[offload features -k]
Features for tap600i0:
rx-checksumming: off [fixed]
tx-checksumming: on
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: on
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: off [fixed]
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: on
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: off
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: off [fixed]
generic-segmentation-offload: on
generic-receive-offload: on
large-receive-offload: off [fixed]
rx-vlan-offload: off [fixed]
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: off [fixed]
highdma: off [fixed]
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [fixed]
tx-fcoe-segmentation: off [fixed]
tx-gre-segmentation: off [fixed]
tx-gre-csum-segmentation: off [fixed]
tx-ipxip4-segmentation: off [fixed]
tx-ipxip6-segmentation: off [fixed]
tx-udp_tnl-segmentation: off
tx-udp_tnl-csum-segmentation: off
tx-gso-partial: off [fixed]
tx-tunnel-remcsum-segmentation: off [fixed]
tx-sctp-segmentation: off [fixed]
tx-esp-segmentation: off [fixed]
tx-udp-segmentation: on
tx-gso-list: off [fixed]
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: on
rx-vlan-stag-hw-parse: off [fixed]
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
[statistics -S (throughput counters)]

----- ethtool: tap601i0 -----
[driver/version/firmware/bus-info -i]
driver: tun
version: 1.6
firmware-version: 
expansion-rom-version: 
bus-info: tap
supports-statistics: no
supports-test: no
supports-eeprom-access: no
supports-register-dump: no
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for tap601i0:
	Supported ports: [  ]
	Supported link modes:   Not reported
	Supported pause frame use: No
	Supports auto-negotiation: No
	Supported FEC modes: Not reported
	Advertised link modes:  Not reported
	Advertised pause frame use: No
	Advertised auto-negotiation: No
	Advertised FEC modes: Not reported
	Speed: 10000Mb/s
	Duplex: Full
	Auto-negotiation: off
	Port: Twisted Pair
	PHYAD: 0
	Transceiver: internal
	MDI-X: Unknown
        Current message level: 0x00000000 (0)
                              
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
Channel parameters for tap601i0:
Pre-set maximums:
RX:		n/a
TX:		n/a
Other:		n/a
Combined:	1
Current hardware settings:
RX:		n/a
TX:		n/a
Other:		n/a
Combined:	1
[coalesce -c (interrupt moderation)]
Coalesce parameters for tap601i0:
Adaptive RX: n/a  TX: n/a
stats-block-usecs:	n/a
sample-interval:	n/a
pkt-rate-low:		n/a
pkt-rate-high:		n/a

rx-usecs:	n/a
rx-frames:	0
rx-usecs-irq:	n/a
rx-frames-irq:	n/a

tx-usecs:	n/a
tx-frames:	n/a
tx-usecs-irq:	n/a
tx-frames-irq:	n/a

rx-usecs-low:	n/a
rx-frame-low:	n/a
tx-usecs-low:	n/a
tx-frame-low:	n/a

rx-usecs-high:	n/a
rx-frame-high:	n/a
tx-usecs-high:	n/a
tx-frame-high:	n/a

CQE mode RX: n/a  TX: n/a

tx-aggr-max-bytes:	n/a
tx-aggr-max-frames:	n/a
tx-aggr-time-usecs:	n/a

[ring -g (descriptor counts)]
netlink error: Operation not supported
[pause / flow-control -a]
netlink error: Operation not supported
[offload features -k]
Features for tap601i0:
rx-checksumming: off [fixed]
tx-checksumming: on
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: on
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: off [fixed]
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: on
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: off
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: off [fixed]
generic-segmentation-offload: on
generic-receive-offload: on
large-receive-offload: off [fixed]
rx-vlan-offload: off [fixed]
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: off [fixed]
highdma: off [fixed]
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [fixed]
tx-fcoe-segmentation: off [fixed]
tx-gre-segmentation: off [fixed]
tx-gre-csum-segmentation: off [fixed]
tx-ipxip4-segmentation: off [fixed]
tx-ipxip6-segmentation: off [fixed]
tx-udp_tnl-segmentation: off
tx-udp_tnl-csum-segmentation: off
tx-gso-partial: off [fixed]
tx-tunnel-remcsum-segmentation: off [fixed]
tx-sctp-segmentation: off [fixed]
tx-esp-segmentation: off [fixed]
tx-udp-segmentation: on
tx-gso-list: off [fixed]
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: on
rx-vlan-stag-hw-parse: off [fixed]
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
[statistics -S (throughput counters)]

----- ethtool: vmbr0 -----
[driver/version/firmware/bus-info -i]
driver: bridge
version: 2.3
firmware-version: N/A
expansion-rom-version: 
bus-info: N/A
supports-statistics: no
supports-test: no
supports-eeprom-access: no
supports-register-dump: no
supports-priv-flags: no
[settings - speed/duplex/autoneg/port]
Settings for vmbr0:
	Supported ports: [  ]
	Supported link modes:   Not reported
	Supported pause frame use: No
	Supports auto-negotiation: No
	Supported FEC modes: Not reported
	Advertised link modes:  Not reported
	Advertised pause frame use: No
	Advertised auto-negotiation: No
	Advertised FEC modes: Not reported
	Speed: 10000Mb/s
	Duplex: Unknown! (255)
	Auto-negotiation: off
	Port: Other
	PHYAD: 0
	Transceiver: internal
	Link detected: yes
[channels -l (RX/TX/combined queue counts)]
netlink error: Operation not supported
[coalesce -c (interrupt moderation)]
netlink error: Operation not supported
[ring -g (descriptor counts)]
netlink error: Operation not supported
[pause / flow-control -a]
netlink error: Operation not supported
[offload features -k]
Features for vmbr0:
rx-checksumming: off [fixed]
tx-checksumming: on
	tx-checksum-ipv4: off [fixed]
	tx-checksum-ip-generic: on
	tx-checksum-ipv6: off [fixed]
	tx-checksum-fcoe-crc: off [fixed]
	tx-checksum-sctp: off [fixed]
scatter-gather: on
	tx-scatter-gather: on
	tx-scatter-gather-fraglist: on
tcp-segmentation-offload: on
	tx-tcp-segmentation: on
	tx-tcp-ecn-segmentation: on
	tx-tcp-mangleid-segmentation: on
	tx-tcp6-segmentation: on
	tx-tcp-accecn-segmentation: on
generic-segmentation-offload: on
generic-receive-offload: on
large-receive-offload: off [fixed]
rx-vlan-offload: off [fixed]
tx-vlan-offload: on
ntuple-filters: off [fixed]
receive-hashing: off [fixed]
highdma: on
rx-vlan-filter: off [fixed]
vlan-challenged: off [fixed]
tx-gso-robust: off [requested on]
tx-fcoe-segmentation: off [requested on]
tx-gre-segmentation: on
tx-gre-csum-segmentation: on
tx-ipxip4-segmentation: on
tx-ipxip6-segmentation: on
tx-udp_tnl-segmentation: on
tx-udp_tnl-csum-segmentation: on
tx-gso-partial: on
tx-tunnel-remcsum-segmentation: on
tx-sctp-segmentation: on
tx-esp-segmentation: on
tx-udp-segmentation: on
tx-gso-list: on
tx-nocache-copy: off
loopback: off [fixed]
rx-fcs: off [fixed]
rx-all: off [fixed]
tx-vlan-stag-hw-insert: on
rx-vlan-stag-hw-parse: off [fixed]
rx-vlan-stag-filter: off [fixed]
l2-fwd-offload: off [fixed]
hw-tc-offload: off [fixed]
esp-hw-offload: off [fixed]
esp-tx-csum-hw-offload: off [fixed]
rx-udp_tunnel-port-offload: off [fixed]
tls-hw-tx-offload: off [fixed]
tls-hw-rx-offload: off [fixed]
rx-gro-hw: off [fixed]
tls-hw-record: off [fixed]
rx-gro-list: off
macsec-hw-offload: off [fixed]
rx-udp-gro-forwarding: off
hsr-tag-ins-offload: off [fixed]
hsr-tag-rm-offload: off [fixed]
hsr-fwd-offload: off [fixed]
hsr-dup-offload: off [fixed]
[private flags --show-priv-flags]
netlink error: Operation not supported
[ntuple/RSS -n]
Cannot get RX rings: Operation not supported
rxclass: Cannot get RX class rule count: Operation not supported
RX classification rule retrieval failed
[SFP/DOM transceiver -m]
netlink error: Operation not supported
[statistics -S (key error/drop counters only)]
[statistics -S (throughput counters)]

###############################################################################
# 11. NETWORK: BRIDGES / BONDS / VLANS
###############################################################################

--- bridge link
    $ bridge link
2: nic0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 master vmbr0 state forwarding priority 32 cost 5 
10: nic3.2@nic3: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 master br-rr-mgmt state forwarding priority 32 cost 19 
12: bond0: <BROADCAST,MULTICAST,MASTER,UP,LOWER_UP> mtu 1500 master storagenet state forwarding priority 32 cost 5 
46: tap100i0: <BROADCAST,MULTICAST,PROMISC,UP,LOWER_UP> mtu 1500 master fwbr100i0 state forwarding priority 32 cost 2 
48: fwpr100p0@fwln100i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 master vmbr0 state forwarding priority 32 cost 2 
49: fwln100i0@fwpr100p0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 master fwbr100i0 state forwarding priority 32 cost 2 
50: tap600i0: <BROADCAST,MULTICAST,PROMISC,UP,LOWER_UP> mtu 1500 master fwbr600i0 state forwarding priority 32 cost 2 
52: fwpr600p0@fwln600i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 master vmbr0 state forwarding priority 32 cost 2 
53: fwln600i0@fwpr600p0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 master fwbr600i0 state forwarding priority 32 cost 2 
54: tap601i0: <BROADCAST,MULTICAST,PROMISC,UP,LOWER_UP> mtu 1500 master fwbr601i0 state forwarding priority 32 cost 2 
56: fwpr601p0@fwln601i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 master vmbr0 state forwarding priority 32 cost 2 
57: fwln601i0@fwpr601p0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 master fwbr601i0 state forwarding priority 32 cost 2 

--- bridge -d link
    $ bridge -d link
2: nic0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 master vmbr0 state forwarding priority 32 cost 5 
    hairpin off guard off root_block off fastleave off learning on flood on mcast_flood on bcast_flood on mcast_router 1 mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off vlan_tunnel off isolated off locked off mab off mcast_n_groups 54 mcast_max_groups 0 
10: nic3.2@nic3: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 master br-rr-mgmt state forwarding priority 32 cost 19 
    hairpin off guard off root_block off fastleave off learning on flood on mcast_flood on bcast_flood on mcast_router 1 mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off vlan_tunnel off isolated off locked off mab off mcast_n_groups 0 mcast_max_groups 0 
12: bond0: <BROADCAST,MULTICAST,MASTER,UP,LOWER_UP> mtu 1500 master storagenet state forwarding priority 32 cost 5 
    hairpin off guard off root_block off fastleave off learning on flood on mcast_flood on bcast_flood on mcast_router 1 mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off vlan_tunnel off isolated off locked off mab off mcast_n_groups 2 mcast_max_groups 0 
46: tap100i0: <BROADCAST,MULTICAST,PROMISC,UP,LOWER_UP> mtu 1500 master fwbr100i0 state forwarding priority 32 cost 2 
    hairpin off guard off root_block off fastleave off learning on flood on mcast_flood on bcast_flood on mcast_router 1 mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off vlan_tunnel off isolated off locked off mab off mcast_n_groups 0 mcast_max_groups 0 
48: fwpr100p0@fwln100i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 master vmbr0 state forwarding priority 32 cost 2 
    hairpin off guard off root_block off fastleave off learning on flood on mcast_flood on bcast_flood on mcast_router 1 mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off vlan_tunnel off isolated off locked off mab off mcast_n_groups 0 mcast_max_groups 0 
49: fwln100i0@fwpr100p0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 master fwbr100i0 state forwarding priority 32 cost 2 
    hairpin off guard off root_block off fastleave off learning on flood on mcast_flood on bcast_flood on mcast_router 1 mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off vlan_tunnel off isolated off locked off mab off mcast_n_groups 50 mcast_max_groups 0 
50: tap600i0: <BROADCAST,MULTICAST,PROMISC,UP,LOWER_UP> mtu 1500 master fwbr600i0 state forwarding priority 32 cost 2 
    hairpin off guard off root_block off fastleave off learning on flood on mcast_flood on bcast_flood on mcast_router 1 mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off vlan_tunnel off isolated off locked off mab off mcast_n_groups 0 mcast_max_groups 0 
52: fwpr600p0@fwln600i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 master vmbr0 state forwarding priority 32 cost 2 
    hairpin off guard off root_block off fastleave off learning on flood on mcast_flood on bcast_flood on mcast_router 1 mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off vlan_tunnel off isolated off locked off mab off mcast_n_groups 0 mcast_max_groups 0 
53: fwln600i0@fwpr600p0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 master fwbr600i0 state forwarding priority 32 cost 2 
    hairpin off guard off root_block off fastleave off learning on flood on mcast_flood on bcast_flood on mcast_router 1 mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off vlan_tunnel off isolated off locked off mab off mcast_n_groups 50 mcast_max_groups 0 
54: tap601i0: <BROADCAST,MULTICAST,PROMISC,UP,LOWER_UP> mtu 1500 master fwbr601i0 state forwarding priority 32 cost 2 
    hairpin off guard off root_block off fastleave off learning on flood on mcast_flood on bcast_flood on mcast_router 1 mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off vlan_tunnel off isolated off locked off mab off mcast_n_groups 0 mcast_max_groups 0 
56: fwpr601p0@fwln601i0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 master vmbr0 state forwarding priority 32 cost 2 
    hairpin off guard off root_block off fastleave off learning on flood on mcast_flood on bcast_flood on mcast_router 1 mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off vlan_tunnel off isolated off locked off mab off mcast_n_groups 0 mcast_max_groups 0 
57: fwln601i0@fwpr601p0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 master fwbr601i0 state forwarding priority 32 cost 2 
    hairpin off guard off root_block off fastleave off learning on flood on mcast_flood on bcast_flood on mcast_router 1 mcast_to_unicast off neigh_suppress off neigh_vlan_suppress off vlan_tunnel off isolated off locked off mab off mcast_n_groups 50 mcast_max_groups 0 

--- bridge vlan
    $ bridge vlan
port              vlan-id  
nic0              1 PVID Egress Untagged
vmbr0             1 PVID Egress Untagged
nic3.2            1 PVID Egress Untagged
br-rr-mgmt        1 PVID Egress Untagged
bond0             1 PVID Egress Untagged
storagenet        1 PVID Egress Untagged
tap100i0          1 PVID Egress Untagged
fwbr100i0         1 PVID Egress Untagged
fwpr100p0         1 PVID Egress Untagged
fwln100i0         1 PVID Egress Untagged
tap600i0          1 PVID Egress Untagged
fwbr600i0         1 PVID Egress Untagged
fwpr600p0         1 PVID Egress Untagged
fwln600i0         1 PVID Egress Untagged
tap601i0          1 PVID Egress Untagged
fwbr601i0         1 PVID Egress Untagged
fwpr601p0         1 PVID Egress Untagged
fwln601i0         1 PVID Egress Untagged

--- bridge vlan show
    $ bridge vlan show
port              vlan-id  
nic0              1 PVID Egress Untagged
vmbr0             1 PVID Egress Untagged
nic3.2            1 PVID Egress Untagged
br-rr-mgmt        1 PVID Egress Untagged
bond0             1 PVID Egress Untagged
storagenet        1 PVID Egress Untagged
tap100i0          1 PVID Egress Untagged
fwbr100i0         1 PVID Egress Untagged
fwpr100p0         1 PVID Egress Untagged
fwln100i0         1 PVID Egress Untagged
tap600i0          1 PVID Egress Untagged
fwbr600i0         1 PVID Egress Untagged
fwpr600p0         1 PVID Egress Untagged
fwln600i0         1 PVID Egress Untagged
tap601i0          1 PVID Egress Untagged
fwbr601i0         1 PVID Egress Untagged
fwpr601p0         1 PVID Egress Untagged
fwln601i0         1 PVID Egress Untagged

--- brctl show
    $ brctl show
bridge name	bridge id		STP enabled	interfaces
br-rr-mgmt		8000.00219ba27c59	no		nic3.2
fwbr100i0		8000.1afa654c659d	no		fwln100i0
							tap100i0
fwbr600i0		8000.62c535114b3c	no		fwln600i0
							tap600i0
fwbr601i0		8000.d6d7f0f52f0c	no		fwln601i0
							tap601i0
storagenet		8000.00219ba27c55	no		bond0
vmbr0		8000.00219ba27c53	no		fwpr100p0
							fwpr600p0
							fwpr601p0
							nic0

--- bonding state
    --- /proc/net/bonding/bond0 ---
Ethernet Channel Bonding Driver: v7.0.14-6-pve

Bonding Mode: IEEE 802.3ad Dynamic link aggregation
Transmit Hash Policy: layer3+4 (1)
MII Status: up
MII Polling Interval (ms): 100
Up Delay (ms): 0
Down Delay (ms): 0
Peer Notification Delay (ms): 0

802.3ad info
LACP active: on
LACP rate: slow
Min links: 0
Aggregator selection policy (ad_select): stable
System priority: 65535
System MAC address: 00:21:9b:a2:7c:55
Active Aggregator Info:
	Aggregator ID: 1
	Number of ports: 2
	Actor Key: 9
	Partner Key: 26
	Partner Mac Address: 00:13:72:46:95:e4

Slave Interface: nic1
MII Status: up
Speed: 1000 Mbps
Duplex: full
Link Failure Count: 0
Permanent HW addr: 00:21:9b:a2:7c:55
Slave queue ID: 0
Aggregator ID: 1
Actor Churn State: none
Partner Churn State: none
Actor Churned Count: 0
Partner Churned Count: 0
details actor lacp pdu:
    system priority: 65535
    system mac address: 00:21:9b:a2:7c:55
    port key: 9
    port priority: 255
    port number: 1
    port state: 61
details partner lacp pdu:
    system priority: 1
    system mac address: 00:13:72:46:95:e4
    oper key: 26
    port priority: 1
    port number: 8
    port state: 61

Slave Interface: nic2
MII Status: up
Speed: 1000 Mbps
Duplex: full
Link Failure Count: 0
Permanent HW addr: 00:21:9b:a2:7c:57
Slave queue ID: 0
Aggregator ID: 1
Actor Churn State: none
Partner Churn State: none
Actor Churned Count: 0
Partner Churned Count: 0
details actor lacp pdu:
    system priority: 65535
    system mac address: 00:21:9b:a2:7c:55
    port key: 9
    port priority: 255
    port number: 2
    port state: 61
details partner lacp pdu:
    system priority: 1
    system mac address: 00:13:72:46:95:e4
    oper key: 26
    port priority: 1
    port number: 9
    port state: 61

--- vlan config
    $ cat /proc/net/vlan/config
VLAN Dev name	 | VLAN ID
Name-Type: VLAN_NAME_TYPE_RAW_PLUS_VID_NO_PAD
nic3.2         | 2  | nic3

--- /proc/net/vlan
total 0
dr-xr-xr-x  4 root root 0 Jul 29 05:09 .
dr-xr-xr-x 62 root root 0 Jul 29 05:09 ..
-rw-------  1 root root 0 Jul 29 05:09 config
-rw-------  1 root root 0 Jul 29 05:09 nic3.2

--- /etc/network/interfaces
    --- /etc/network/interfaces ---
# network interface settings; autogenerated
# Please do NOT modify this file directly, unless you know what
# you're doing.
#
# If you want to manage parts of the network configuration manually,
# please utilize the 'source' or 'source-directory' directives to do
# so.
# PVE will preserve these directives, but will NOT read its network
# configuration from sourced files, so do not attempt to move any of
# the PVE managed interfaces into external files!

auto lo
iface lo inet loopback

iface nic0 inet manual

auto nic1
iface nic1 inet manual
#PortID:       ifname g8

auto nic2
iface nic2 inet manual
#PortID:       ifname g9

iface nic3 inet manual

iface nic3.2 inet manual

iface nic4 inet manual

iface nic5 inet manual

auto bond0
iface bond0 inet manual
	bond-slaves nic1 nic2
	bond-miimon 100
	bond-mode 802.3ad
	bond-xmit-hash-policy layer3+4

auto vmbr0
iface vmbr0 inet dhcp
	bridge-ports nic0
	bridge-stp off
	bridge-fd 0

auto br-rr-mgmt
iface br-rr-mgmt inet static
	address 10.251.2.6/24
	bridge-ports nic3.2
	bridge-stp off
	bridge-fd 0

auto storagenet
iface storagenet inet static
	address 10.100.100.6/24
	bridge-ports bond0
	bridge-stp off
	bridge-fd 0

source /etc/network/interfaces.d/*

--- interfaces.d (per file)
    $ for f in /etc/network/interfaces.d/*; do
    [ -r "$f" ] || continue
    echo "--- $f ---"
    cat "$f"
done
--- /etc/network/interfaces.d/sdn ---

###############################################################################
# 12. NETWORK: IRQ / RPS / XPS / aRFS / SOFTNET
###############################################################################

--- /proc/interrupts
    $ cat /proc/interrupts
            CPU0       CPU1       CPU2       CPU3       CPU4       CPU5       CPU6       CPU7       CPU8       CPU9       CPU10      CPU11      CPU12      CPU13      CPU14      CPU15      
   0:      25428          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0  IO-APIC    2-edge      timer
   1:          0          0          0          0          0          0          0          0          0          0          4          0          0          0          0          0  IO-APIC    1-edge      i8042
   8:          0          0          0          0          0          0          0          0          0          0          0          0          1          0          0          0  IO-APIC    8-edge      rtc0
   9:          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0  IO-APIC    9-fasteoi   acpi
  12:          0          0          0          0          0          0          0          0          6          0          0          0          0          0          0          0  IO-APIC   12-edge      i8042
  17:          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0  IO-APIC   17-fasteoi   uhci_hcd:usb3
  18:          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0  IO-APIC   18-fasteoi   uhci_hcd:usb4
  19:          0          0          0          0          0          0          0    6334597          0          0          0          0          0          0          0          0  IO-APIC   19-fasteoi   ehci_hcd:usb1
  20:          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0  IO-APIC   20-fasteoi   uhci_hcd:usb6
  21:          0          0          0          0          0          0          0          0          0         89          0          0          0          0          0          0  IO-APIC   21-fasteoi   ehci_hcd:usb2, uhci_hcd:usb5
  25:          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0 PCI-MSI-0000:00:01.0    0-edge      PCIe PME, aerdrv, PCIe bwctrl
  26:          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0 PCI-MSI-0000:00:03.0    0-edge      PCIe PME, aerdrv, PCIe bwctrl
  27:          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0 PCI-MSI-0000:00:07.0    0-edge      PCIe PME, aerdrv, PCIe bwctrl
  28:          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0 PCI-MSI-0000:00:09.0    0-edge      PCIe PME, aerdrv, PCIe bwctrl
  29:          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0 PCI-MSI-0000:00:1c.0    0-edge      PCIe PME
  36:          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0    5456512 PCI-MSIX-0000:01:00.0    0-edge      nic0-0
  37:    1638691          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0 PCI-MSIX-0000:01:00.0    1-edge      nic0-1
  38:          0    3177156          0          0          0          0          0          0          0          0          0          0          0          0          0          0 PCI-MSIX-0000:01:00.0    2-edge      nic0-2
  39:          0          0    1999663          0          0          0          0          0          0          0          0          0          0          0          0          0 PCI-MSIX-0000:01:00.0    3-edge      nic0-3
  40:          0          0          0    1392413          0          0          0          0          0          0          0          0          0          0          0          0 PCI-MSIX-0000:01:00.0    4-edge      nic0-4
  42:          0          0          0          0     216585          0          0          0          0          0          0          0          0          0          0          0 PCI-MSIX-0000:02:00.1    0-edge      nic3-0
  43:          0          0          0          0          0         64          0          0          0          0          0          0          0          0          0          0 PCI-MSIX-0000:02:00.1    1-edge      nic3-1
  44:          0          0          0          0          0          0          6          0          0          0          0          0          0          0          0          0 PCI-MSIX-0000:02:00.1    2-edge      nic3-2
  45:          0          0          0          0          0          0          0       7852          0          0          0          0          0          0          0          0 PCI-MSIX-0000:02:00.1    3-edge      nic3-3
  46:          0          0          0          0          0          0          0          0      23090          0          0          0          0          0          0          0 PCI-MSIX-0000:02:00.1    4-edge      nic3-4
  48:          0          0          0          0          0          0          0          0          0    4660203          0          0          0          0          0          0 PCI-MSIX-0000:01:00.1    0-edge      nic1-0
  49:          0          0          0          0          0          0          0          0          0          0    3682875          0          0          0          0          0 PCI-MSIX-0000:01:00.1    1-edge      nic1-1
  50:          0          0          0          0          0          0          0          0          0          0          0    3847411          0          0          0          0 PCI-MSIX-0000:01:00.1    2-edge      nic1-2
  51:          0          0          0          0          0          0          0          0          0          0          0          0   11894128          0          0          0 PCI-MSIX-0000:01:00.1    3-edge      nic1-3
  52:          0          0          0          0          0          0          0          0          0          0          0          0          0     359983          0          0 PCI-MSIX-0000:01:00.1    4-edge      nic1-4
  54:          0          0          0          0          0          0          0          0          0          0          0          0          0          0     896715          0 PCI-MSIX-0000:02:00.0    0-edge      nic2-0
  55:          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0    1273192 PCI-MSIX-0000:02:00.0    1-edge      nic2-1
  56:    2426718          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0 PCI-MSIX-0000:02:00.0    2-edge      nic2-2
  57:          0    1352521          0          0          0          0          0          0          0          0          0          0          0          0          0          0 PCI-MSIX-0000:02:00.0    3-edge      nic2-3
  58:          0          0     143230          0          0          0          0          0          0          0          0          0          0          0          0          0 PCI-MSIX-0000:02:00.0    4-edge      nic2-4
 NMI:       3468       3206      12376       2696       9447       2616       6521       2761       3258       2604       4556       2516       4765       2438       3426       2779   Non-maskable interrupts
 LOC:   17742936   18156273   25321793   17567585   23664758   18231386   21522367   20054113   19239654   19049224   19521268   18820201   19635468   18372327   18162349   29165538   Local timer interrupts
 SPU:          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0   Spurious interrupts
 PMI:       3468       3206      12376       2696       9447       2616       6521       2761       3258       2604       4556       2516       4765       2438       3426       2779   Performance monitoring interrupts
 IWI:        949     419481       1213        522        704        543        640        395        498       1236        757       1073       1214        859        550        508   IRQ work interrupts
 RTR:          7          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0   APIC ICR read retries
 RES:     275400     330851     274663     323073     302543     366144     333707     390099     367538     399569     351879     376471     320089     375799     338029     279405   Rescheduling interrupts
 CAL:    1782573     722464     544616     441499     602888     343577     447759     348459     470773     332981     467054     319933     431230     304419     440807     363453   Function call interrupts
 TLB:      79011      77634      78988      83285      79525      84279      79754      82275      77521      79211      76706      76717      74732      73920      73789      71940   TLB shootdowns
 TRM:          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0   Thermal event interrupts
 THR:          0     291699          0     291699          0     291699          0     291699          0     291699          0     291699          0     291699          0     291699   Threshold APIC interrupts
 DFR:          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0   Deferred Error APIC interrupts
 MCE:          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0   Machine check exceptions
 MCP:        660     370861        661     292361        662     292360        662     292362        662     292360        661     292361        660     292363        662     292363   Machine check polls
 ERR:          0
 MIS:          0
 PIN:          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0   Posted-interrupt notification event
 NPI:          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0   Nested posted-interrupt event
 PIW:          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0   Posted-interrupt wakeup event
VPMI:          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0          0  Perf Guest Mediated PMI

--- NIC IRQ affinities (which CPUs handle which queue)
    $ for ifc in $NETIFS; do
    [ -d "/sys/class/net/$ifc/device/msi_irqs" ] || continue
    echo "=== $ifc IRQ list (first 40) ==="
    ls "/sys/class/net/$ifc/device/msi_irqs" 2>/dev/null | head -n 40
done
=== nic0 IRQ list (first 40) ===
36
37
38
39
40
41
=== nic1 IRQ list (first 40) ===
48
49
50
51
52
53
=== nic2 IRQ list (first 40) ===
54
55
56
57
58
59
=== nic3 IRQ list (first 40) ===
42
43
44
45
46
47

--- RPS masks (non-zero only)
    $ for q in /sys/class/net/*/queues/rx-*/rps_cpus; do
    [ -e "$q" ] || continue
    val=$(cat "$q")
    [ "$val" != "0" ] && printf '  %s = %s\n' "$q" "$val"
done | head -n 60
  /sys/class/net/bond0/queues/rx-0/rps_cpus = 0000
  /sys/class/net/bond0/queues/rx-10/rps_cpus = 0000
  /sys/class/net/bond0/queues/rx-11/rps_cpus = 0000
  /sys/class/net/bond0/queues/rx-12/rps_cpus = 0000
  /sys/class/net/bond0/queues/rx-13/rps_cpus = 0000
  /sys/class/net/bond0/queues/rx-14/rps_cpus = 0000
  /sys/class/net/bond0/queues/rx-15/rps_cpus = 0000
  /sys/class/net/bond0/queues/rx-1/rps_cpus = 0000
  /sys/class/net/bond0/queues/rx-2/rps_cpus = 0000
  /sys/class/net/bond0/queues/rx-3/rps_cpus = 0000
  /sys/class/net/bond0/queues/rx-4/rps_cpus = 0000
  /sys/class/net/bond0/queues/rx-5/rps_cpus = 0000
  /sys/class/net/bond0/queues/rx-6/rps_cpus = 0000
  /sys/class/net/bond0/queues/rx-7/rps_cpus = 0000
  /sys/class/net/bond0/queues/rx-8/rps_cpus = 0000
  /sys/class/net/bond0/queues/rx-9/rps_cpus = 0000
  /sys/class/net/br-rr-mgmt/queues/rx-0/rps_cpus = 0000
  /sys/class/net/fwbr100i0/queues/rx-0/rps_cpus = 0000
  /sys/class/net/fwbr600i0/queues/rx-0/rps_cpus = 0000
  /sys/class/net/fwbr601i0/queues/rx-0/rps_cpus = 0000
  /sys/class/net/fwln100i0/queues/rx-0/rps_cpus = 0000
  /sys/class/net/fwln600i0/queues/rx-0/rps_cpus = 0000
  /sys/class/net/fwln601i0/queues/rx-0/rps_cpus = 0000
  /sys/class/net/fwpr100p0/queues/rx-0/rps_cpus = 0000
  /sys/class/net/fwpr600p0/queues/rx-0/rps_cpus = 0000
  /sys/class/net/fwpr601p0/queues/rx-0/rps_cpus = 0000
  /sys/class/net/lo/queues/rx-0/rps_cpus = 0000
  /sys/class/net/nic0/queues/rx-0/rps_cpus = 0000
  /sys/class/net/nic0/queues/rx-1/rps_cpus = 0000
  /sys/class/net/nic0/queues/rx-2/rps_cpus = 0000
  /sys/class/net/nic0/queues/rx-3/rps_cpus = 0000
  /sys/class/net/nic0/queues/rx-4/rps_cpus = 0000
  /sys/class/net/nic1/queues/rx-0/rps_cpus = 0000
  /sys/class/net/nic1/queues/rx-1/rps_cpus = 0000
  /sys/class/net/nic1/queues/rx-2/rps_cpus = 0000
  /sys/class/net/nic1/queues/rx-3/rps_cpus = 0000
  /sys/class/net/nic1/queues/rx-4/rps_cpus = 0000
  /sys/class/net/nic2/queues/rx-0/rps_cpus = 0000
  /sys/class/net/nic2/queues/rx-1/rps_cpus = 0000
  /sys/class/net/nic2/queues/rx-2/rps_cpus = 0000
  /sys/class/net/nic2/queues/rx-3/rps_cpus = 0000
  /sys/class/net/nic2/queues/rx-4/rps_cpus = 0000
  /sys/class/net/nic3.2/queues/rx-0/rps_cpus = 0000
  /sys/class/net/nic3/queues/rx-0/rps_cpus = 0000
  /sys/class/net/nic3/queues/rx-1/rps_cpus = 0000
  /sys/class/net/nic3/queues/rx-2/rps_cpus = 0000
  /sys/class/net/nic3/queues/rx-3/rps_cpus = 0000
  /sys/class/net/nic3/queues/rx-4/rps_cpus = 0000
  /sys/class/net/nic4/queues/rx-0/rps_cpus = 0000
  /sys/class/net/nic4/queues/rx-1/rps_cpus = 0000
  /sys/class/net/nic4/queues/rx-2/rps_cpus = 0000
  /sys/class/net/nic4/queues/rx-3/rps_cpus = 0000
  /sys/class/net/nic4/queues/rx-4/rps_cpus = 0000
  /sys/class/net/nic4/queues/rx-5/rps_cpus = 0000
  /sys/class/net/nic4/queues/rx-6/rps_cpus = 0000
  /sys/class/net/nic4/queues/rx-7/rps_cpus = 0000
  /sys/class/net/nic5/queues/rx-0/rps_cpus = 0000
  /sys/class/net/nic5/queues/rx-1/rps_cpus = 0000
  /sys/class/net/nic5/queues/rx-2/rps_cpus = 0000
  /sys/class/net/nic5/queues/rx-3/rps_cpus = 0000

--- XPS masks (non-zero only)
    $ for q in /sys/class/net/*/queues/tx-*/xps_cpus; do
    [ -e "$q" ] || continue
    val=$(cat "$q")
    [ "$val" != "0" ] && printf '  %s = %s\n' "$q" "$val"
done | head -n 60
cat: /sys/class/net/br-rr-mgmt/queues/tx-0/xps_cpus: No such file or directory
cat: /sys/class/net/fwbr100i0/queues/tx-0/xps_cpus: No such file or directory
cat: /sys/class/net/fwbr600i0/queues/tx-0/xps_cpus: No such file or directory
cat: /sys/class/net/fwbr601i0/queues/tx-0/xps_cpus: No such file or directory
cat: /sys/class/net/lo/queues/tx-0/xps_cpus: No such file or directory
cat: /sys/class/net/nic3.2/queues/tx-0/xps_cpus: No such file or directory
  /sys/class/net/bond0/queues/tx-0/xps_cpus = 0000
  /sys/class/net/bond0/queues/tx-10/xps_cpus = 0000
  /sys/class/net/bond0/queues/tx-11/xps_cpus = 0000
  /sys/class/net/bond0/queues/tx-12/xps_cpus = 0000
  /sys/class/net/bond0/queues/tx-13/xps_cpus = 0000
  /sys/class/net/bond0/queues/tx-14/xps_cpus = 0000
  /sys/class/net/bond0/queues/tx-15/xps_cpus = 0000
  /sys/class/net/bond0/queues/tx-1/xps_cpus = 0000
  /sys/class/net/bond0/queues/tx-2/xps_cpus = 0000
  /sys/class/net/bond0/queues/tx-3/xps_cpus = 0000
  /sys/class/net/bond0/queues/tx-4/xps_cpus = 0000
  /sys/class/net/bond0/queues/tx-5/xps_cpus = 0000
  /sys/class/net/bond0/queues/tx-6/xps_cpus = 0000
  /sys/class/net/bond0/queues/tx-7/xps_cpus = 0000
  /sys/class/net/bond0/queues/tx-8/xps_cpus = 0000
  /sys/class/net/bond0/queues/tx-9/xps_cpus = 0000
  /sys/class/net/br-rr-mgmt/queues/tx-0/xps_cpus = 
  /sys/class/net/fwbr100i0/queues/tx-0/xps_cpus = 
  /sys/class/net/fwbr600i0/queues/tx-0/xps_cpus = 
  /sys/class/net/fwbr601i0/queues/tx-0/xps_cpus = 
  /sys/class/net/fwln100i0/queues/tx-0/xps_cpus = 0000
  /sys/class/net/fwln600i0/queues/tx-0/xps_cpus = 0000
  /sys/class/net/fwln601i0/queues/tx-0/xps_cpus = 0000
  /sys/class/net/fwpr100p0/queues/tx-0/xps_cpus = 0000
  /sys/class/net/fwpr600p0/queues/tx-0/xps_cpus = 0000
  /sys/class/net/fwpr601p0/queues/tx-0/xps_cpus = 0000
  /sys/class/net/lo/queues/tx-0/xps_cpus = 
  /sys/class/net/nic0/queues/tx-0/xps_cpus = 0000
  /sys/class/net/nic0/queues/tx-1/xps_cpus = 0000
  /sys/class/net/nic0/queues/tx-2/xps_cpus = 0000
  /sys/class/net/nic0/queues/tx-3/xps_cpus = 0000
  /sys/class/net/nic1/queues/tx-0/xps_cpus = 0000
  /sys/class/net/nic1/queues/tx-1/xps_cpus = 0000
  /sys/class/net/nic1/queues/tx-2/xps_cpus = 0000
  /sys/class/net/nic1/queues/tx-3/xps_cpus = 0000
  /sys/class/net/nic2/queues/tx-0/xps_cpus = 0000
  /sys/class/net/nic2/queues/tx-1/xps_cpus = 0000
  /sys/class/net/nic2/queues/tx-2/xps_cpus = 0000
  /sys/class/net/nic2/queues/tx-3/xps_cpus = 0000
  /sys/class/net/nic3.2/queues/tx-0/xps_cpus = 
  /sys/class/net/nic3/queues/tx-0/xps_cpus = 0000
  /sys/class/net/nic3/queues/tx-1/xps_cpus = 0000
  /sys/class/net/nic3/queues/tx-2/xps_cpus = 0000
  /sys/class/net/nic3/queues/tx-3/xps_cpus = 0000
  /sys/class/net/nic4/queues/tx-0/xps_cpus = 0000
  /sys/class/net/nic4/queues/tx-1/xps_cpus = 0000
  /sys/class/net/nic4/queues/tx-2/xps_cpus = 0000
  /sys/class/net/nic4/queues/tx-3/xps_cpus = 0000
  /sys/class/net/nic4/queues/tx-4/xps_cpus = 0000
  /sys/class/net/nic4/queues/tx-5/xps_cpus = 0000
  /sys/class/net/nic4/queues/tx-6/xps_cpus = 0000
  /sys/class/net/nic4/queues/tx-7/xps_cpus = 0000
  /sys/class/net/nic5/queues/tx-0/xps_cpus = 0000
  /sys/class/net/nic5/queues/tx-1/xps_cpus = 0000
  /sys/class/net/nic5/queues/tx-2/xps_cpus = 0000
  /sys/class/net/nic5/queues/tx-3/xps_cpus = 0000
  /sys/class/net/nic5/queues/tx-4/xps_cpus = 0000
  /sys/class/net/nic5/queues/tx-5/xps_cpus = 0000
  /sys/class/net/nic5/queues/tx-6/xps_cpus = 0000
  /sys/class/net/nic5/queues/tx-7/xps_cpus = 0000
cat: /sys/class/net/storagenet/queues/tx-0/xps_cpus: No such file or directory

--- RFS flow counts
    $ for q in /sys/class/net/*/queues/rx-*/rps_flow_cnt; do
    [ -e "$q" ] || continue
    printf '  %s = %s\n' "$q" "$(cat "$q")"
done | head -n 60
  /sys/class/net/bond0/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/bond0/queues/rx-10/rps_flow_cnt = 0
  /sys/class/net/bond0/queues/rx-11/rps_flow_cnt = 0
  /sys/class/net/bond0/queues/rx-12/rps_flow_cnt = 0
  /sys/class/net/bond0/queues/rx-13/rps_flow_cnt = 0
  /sys/class/net/bond0/queues/rx-14/rps_flow_cnt = 0
  /sys/class/net/bond0/queues/rx-15/rps_flow_cnt = 0
  /sys/class/net/bond0/queues/rx-1/rps_flow_cnt = 0
  /sys/class/net/bond0/queues/rx-2/rps_flow_cnt = 0
  /sys/class/net/bond0/queues/rx-3/rps_flow_cnt = 0
  /sys/class/net/bond0/queues/rx-4/rps_flow_cnt = 0
  /sys/class/net/bond0/queues/rx-5/rps_flow_cnt = 0
  /sys/class/net/bond0/queues/rx-6/rps_flow_cnt = 0
  /sys/class/net/bond0/queues/rx-7/rps_flow_cnt = 0
  /sys/class/net/bond0/queues/rx-8/rps_flow_cnt = 0
  /sys/class/net/bond0/queues/rx-9/rps_flow_cnt = 0
  /sys/class/net/br-rr-mgmt/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/fwbr100i0/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/fwbr600i0/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/fwbr601i0/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/fwln100i0/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/fwln600i0/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/fwln601i0/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/fwpr100p0/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/fwpr600p0/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/fwpr601p0/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/lo/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/nic0/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/nic0/queues/rx-1/rps_flow_cnt = 0
  /sys/class/net/nic0/queues/rx-2/rps_flow_cnt = 0
  /sys/class/net/nic0/queues/rx-3/rps_flow_cnt = 0
  /sys/class/net/nic0/queues/rx-4/rps_flow_cnt = 0
  /sys/class/net/nic1/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/nic1/queues/rx-1/rps_flow_cnt = 0
  /sys/class/net/nic1/queues/rx-2/rps_flow_cnt = 0
  /sys/class/net/nic1/queues/rx-3/rps_flow_cnt = 0
  /sys/class/net/nic1/queues/rx-4/rps_flow_cnt = 0
  /sys/class/net/nic2/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/nic2/queues/rx-1/rps_flow_cnt = 0
  /sys/class/net/nic2/queues/rx-2/rps_flow_cnt = 0
  /sys/class/net/nic2/queues/rx-3/rps_flow_cnt = 0
  /sys/class/net/nic2/queues/rx-4/rps_flow_cnt = 0
  /sys/class/net/nic3.2/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/nic3/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/nic3/queues/rx-1/rps_flow_cnt = 0
  /sys/class/net/nic3/queues/rx-2/rps_flow_cnt = 0
  /sys/class/net/nic3/queues/rx-3/rps_flow_cnt = 0
  /sys/class/net/nic3/queues/rx-4/rps_flow_cnt = 0
  /sys/class/net/nic4/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/nic4/queues/rx-1/rps_flow_cnt = 0
  /sys/class/net/nic4/queues/rx-2/rps_flow_cnt = 0
  /sys/class/net/nic4/queues/rx-3/rps_flow_cnt = 0
  /sys/class/net/nic4/queues/rx-4/rps_flow_cnt = 0
  /sys/class/net/nic4/queues/rx-5/rps_flow_cnt = 0
  /sys/class/net/nic4/queues/rx-6/rps_flow_cnt = 0
  /sys/class/net/nic4/queues/rx-7/rps_flow_cnt = 0
  /sys/class/net/nic5/queues/rx-0/rps_flow_cnt = 0
  /sys/class/net/nic5/queues/rx-1/rps_flow_cnt = 0
  /sys/class/net/nic5/queues/rx-2/rps_flow_cnt = 0
  /sys/class/net/nic5/queues/rx-3/rps_flow_cnt = 0

--- /proc/net/softnet_stat (drops/backlog)
    $ cat /proc/net/softnet_stat
00f9d304 00000000 0000001c 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000
00cb68ec 00000000 00000008 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000001 00000000 00000000
00ce6643 00000000 000004b9 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000002 00000000 00000000
009ab420 00000000 00000005 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000003 00000000 00000000
00082afe 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000004 00000000 00000000
0005fc11 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000005 00000000 00000000
00034908 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000006 00000000 00000000
0003ee27 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000007 00000000 00000000
00026c90 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000008 00000000 00000000
00099225 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000009 00000000 00000000
000eda01 00000000 00000003 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 0000000a 00000000 00000000
0014d7b5 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 0000000b 00000000 00000000
04e09cf6 00000000 0000003f 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 0000000c 00000000 00000000
0014ba8b 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 0000000d 00000000 00000000
0002c06d 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 0000000e 00000000 00000000
01856ac7 00000000 00000008 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 00000000 0000000f 00000000 00000000

--- softnet_stat decoded
    $ # columns: TOTAL DROPPED DROPPED_BY_NETRX TIME_SQUEEZED CPU_COLLISIONS RPS_RECEIVED_FLOW_LIMIT
awk '{ printf "cpu%-2d total=%-8s dropped=%-6s time_squeezed=%-6s cpu_collision=%-4s rps_received=%-6s flow_limit=%s\n",
       NR-1, $1, $2, $4, $5, $6, $7 }' /proc/net/softnet_stat
cpu0  total=00f9d304 dropped=00000000 time_squeezed=00000000 cpu_collision=00000000 rps_received=00000000 flow_limit=00000000
cpu1  total=00cb68ec dropped=00000000 time_squeezed=00000000 cpu_collision=00000000 rps_received=00000000 flow_limit=00000000
cpu2  total=00ce6643 dropped=00000000 time_squeezed=00000000 cpu_collision=00000000 rps_received=00000000 flow_limit=00000000
cpu3  total=009ab420 dropped=00000000 time_squeezed=00000000 cpu_collision=00000000 rps_received=00000000 flow_limit=00000000
cpu4  total=00082afe dropped=00000000 time_squeezed=00000000 cpu_collision=00000000 rps_received=00000000 flow_limit=00000000
cpu5  total=0005fc11 dropped=00000000 time_squeezed=00000000 cpu_collision=00000000 rps_received=00000000 flow_limit=00000000
cpu6  total=00034908 dropped=00000000 time_squeezed=00000000 cpu_collision=00000000 rps_received=00000000 flow_limit=00000000
cpu7  total=0003ee27 dropped=00000000 time_squeezed=00000000 cpu_collision=00000000 rps_received=00000000 flow_limit=00000000
cpu8  total=00026c90 dropped=00000000 time_squeezed=00000000 cpu_collision=00000000 rps_received=00000000 flow_limit=00000000
cpu9  total=00099225 dropped=00000000 time_squeezed=00000000 cpu_collision=00000000 rps_received=00000000 flow_limit=00000000
cpu10 total=000eda01 dropped=00000000 time_squeezed=00000000 cpu_collision=00000000 rps_received=00000000 flow_limit=00000000
cpu11 total=0014d7b5 dropped=00000000 time_squeezed=00000000 cpu_collision=00000000 rps_received=00000000 flow_limit=00000000
cpu12 total=04e09cf6 dropped=00000000 time_squeezed=00000000 cpu_collision=00000000 rps_received=00000000 flow_limit=00000000
cpu13 total=0014ba8b dropped=00000000 time_squeezed=00000000 cpu_collision=00000000 rps_received=00000000 flow_limit=00000000
cpu14 total=0002c06d dropped=00000000 time_squeezed=00000000 cpu_collision=00000000 rps_received=00000000 flow_limit=00000000
cpu15 total=01856ac7 dropped=00000000 time_squeezed=00000000 cpu_collision=00000000 rps_received=00000000 flow_limit=00000000

--- netstat drop counters (significant ones)
    $ nstat -az 2>/dev/null | grep -iE '(Drop|Retrans|Fail|Abort|Overflow|Loss|ListenDrop|EmbryonicRsts|InErrs|OutErrs)' || \
netstat -s 2>/dev/null | grep -iE '(drop|retrans|fail|abort|overflow|loss|listen|error)' | head -n 60
IpReasmFails                    0                  0.0
IpFragFails                     0                  0.0
TcpAttemptFails                 9724               0.0
TcpRetransSegs                  758508             0.0
TcpInErrs                       6                  0.0
Ip6ReasmFails                   0                  0.0
Ip6FragFails                    0                  0.0
TcpExtSyncookiesFailed          0                  0.0
TcpExtEmbryonicRsts             0                  0.0
TcpExtLockDroppedIcmps          0                  0.0
TcpExtListenOverflows           0                  0.0
TcpExtListenDrops               0                  0.0
TcpExtTCPLossUndo               12                 0.0
TcpExtTCPLostRetransmit         175111             0.0
TcpExtTCPRenoFailures           0                  0.0
TcpExtTCPSackFailures           17                 0.0
TcpExtTCPLossFailures           19                 0.0
TcpExtTCPFastRetrans            635840             0.0
TcpExtTCPSlowStartRetrans       54718              0.0
TcpExtTCPLossProbes             65408              0.0
TcpExtTCPLossProbeRecovery      478                0.0
TcpExtTCPRenoRecoveryFail       0                  0.0
TcpExtTCPSackRecoveryFail       594                0.0
TcpExtTCPAbortOnData            2432               0.0
TcpExtTCPAbortOnClose           21                 0.0
TcpExtTCPAbortOnMemory          0                  0.0
TcpExtTCPAbortOnTimeout         14                 0.0
TcpExtTCPAbortOnLinger          0                  0.0
TcpExtTCPAbortFailed            0                  0.0
TcpExtTCPMD5Failure             0                  0.0
TcpExtTCPBacklogDrop            0                  0.0
TcpExtPFMemallocDrop            0                  0.0
TcpExtTCPMinTTLDrop             0                  0.0
TcpExtTCPDeferAcceptDrop        0                  0.0
TcpExtTCPTimeWaitOverflow       0                  0.0
TcpExtTCPReqQFullDrop           0                  0.0
TcpExtTCPRetransFail            0                  0.0
TcpExtTCPOFODrop                0                  0.0
TcpExtTCPFastOpenActiveFail     0                  0.0
TcpExtTCPFastOpenPassiveFail    0                  0.0
TcpExtTCPFastOpenListenOverflow 0                  0.0
TcpExtTCPSynRetrans             5250               0.0
TcpExtTCPMTUPFail               0                  0.0
TcpExtTCPZeroWindowDrop         0                  0.0
TcpExtTCPRcvQDrop               0                  0.0
TcpExtTCPMigrateReqFailure      0                  0.0
TcpExtTCPAODroppedIcmps         0                  0.0
MPTcpExtMPCapableSYNTXDrop      0                  0.0
MPTcpExtMPTCPRetrans            0                  0.0
MPTcpExtMPJoinSynAckHMacFailure 0                  0.0
MPTcpExtMPJoinAckHMacFailure    0                  0.0
MPTcpExtAddAddrTxDrop           0                  0.0
MPTcpExtEchoAddTxDrop           0                  0.0
MPTcpExtAddAddrDrop             0                  0.0
MPTcpExtRmAddrDrop              0                  0.0
MPTcpExtRmAddrTxDrop            0                  0.0
MPTcpExtMPFailTx                0                  0.0
MPTcpExtMPFailRx                0                  0.0
MPTcpExtFallbackFailed          0                  0.0

###############################################################################
# 13. NETWORK: SOCKET / TCP STATE
###############################################################################

--- ss -s
    $ ss -s
Total: 368
TCP:   175 (estab 19, closed 145, orphaned 0, timewait 144)

Transport Total     IP        IPv6
RAW	  0         0         0        
UDP	  7         4         3        
TCP	  30        20        10       
INET	  37        24        13       
FRAG	  0         0         0        


--- ss -t -m (top TCP with skmem/cwnd/rto)
    $ ss -tno state established ( dport != :22 and sport != :22 ) -m
Recv-Q Send-Q          Local Address:Port             Peer Address:Port                                                                                      
0      0               192.168.3.169:43780         199.165.136.101:443   timer:(keepalive,21sec,0)
	 skmem:(r0,rb807913,t0,tb130560,f0,w0,o0,bl0,d0)         
0      0               192.168.3.169:57504           152.53.37.179:443   timer:(keepalive,9.606sec,0)
	 skmem:(r0,rb87380,t0,tb130560,f0,w0,o0,bl0,d2)       
0      0               192.168.3.169:49820          209.177.156.94:443   timer:(keepalive,12sec,0)
	 skmem:(r0,rb807230,t0,tb130560,f0,w0,o0,bl0,d0)         
0      0               192.168.3.169:37082           192.200.0.116:443   timer:(keepalive,9.358sec,0)
	 skmem:(r0,rb104670,t0,tb130560,f0,w0,o0,bl0,d0)      
0      0                10.100.100.6:753              10.100.100.4:2049  timer:(keepalive,29sec,0)
	 skmem:(r0,rb4079894,t0,tb17782272,f0,w0,o0,bl0,d196)    
0      0                10.100.100.6:808              10.100.100.4:2049  timer:(keepalive,39sec,0)
	 skmem:(r0,rb7175536,t0,tb13212672,f0,w0,o0,bl0,d196)    
0      0                10.100.100.6:964              10.100.100.4:2049  timer:(keepalive,1min23sec,0)
	 skmem:(r0,rb5048990,t0,tb13186560,f0,w0,o0,bl0,d195)
0      0                10.100.100.6:972              10.100.100.4:2049  timer:(keepalive,1min10sec,0)
	 skmem:(r0,rb9053412,t0,tb15823872,f0,w0,o0,bl0,d145)
0      0                10.100.100.6:810              10.100.100.5:2049  timer:(keepalive,49sec,0)
	 skmem:(r0,rb1758483,t0,tb8199168,f0,w0,o0,bl0,d9)       
0      0                10.100.100.6:814              10.100.100.5:2049  timer:(keepalive,29sec,0)
	 skmem:(r0,rb1416963,t0,tb4595712,f0,w0,o0,bl0,d12)      
0      0                10.100.100.6:825              10.100.100.5:2049  timer:(keepalive,8.867sec,0)
	 skmem:(r0,rb1390036,t0,tb4882944,f0,w0,o0,bl0,d11)   
0      0                10.100.100.6:951              10.100.100.5:2049  timer:(keepalive,19sec,0)
	 skmem:(r0,rb4796174,t0,tb6397440,f0,w0,o0,bl0,d6)       
0      0                   127.0.0.1:59046               127.0.0.1:5900 
	 skmem:(r0,rb399451,t0,tb3939840,f0,w0,o0,bl0,d0)                                  
0      0                   127.0.0.1:5900                127.0.0.1:59046
	 skmem:(r0,rb87380,t0,tb3939840,f0,w0,o0,bl0,d0)                                   
0      0      [::ffff:100.73.35.111]:8006  [::ffff:100.109.70.137]:26831
	 skmem:(r0,rb1247438,t0,tb69120,f0,w0,o0,bl0,d0)                                   
0      0      [::ffff:100.73.35.111]:8006  [::ffff:100.109.70.137]:10582
	 skmem:(r0,rb87380,t0,tb69120,f0,w0,o0,bl0,d0)                                     
0      0      [::ffff:100.73.35.111]:8006  [::ffff:100.125.183.68]:60052
	 skmem:(r0,rb87380,t0,tb69120,f0,w0,o0,bl0,d0)                                     
0      0      [::ffff:100.73.35.111]:8006  [::ffff:100.109.70.137]:12306
	 skmem:(r0,rb87380,t0,tb69120,f0,w0,o0,bl0,d0)                                     

--- ss -ti (TCP internals)
    $ ss -ti
State Recv-Q Send-Q          Local Address:Port             Peer Address:Port                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           
ESTAB 0      0               192.168.3.169:43780         199.165.136.101:https
	 bbr wscale:7,12 rto:266 rtt:65.257/11.443 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:25 bytes_sent:7963208 bytes_retrans:541 bytes_acked:7962668 bytes_received:1514646 segs_out:31089 segs_in:24651 data_segs_out:15562 data_segs_in:15532 bbr:(bw:1.54Mbps,mrtt:39.517,pacing_gain:2.88672,cwnd_gain:2.88672) send 4.44Mbps lastsnd:5547 lastrcv:5469 lastack:5469 pacing_rate 4.41Mbps delivery_rate 785kbps delivered:15563 app_limited busy:980420ms retrans:0/5 dsack_dups:1 rcv_rtt:19257.8 rcv_space:46527 rcv_ssthresh:129040 minrtt:39.517 snd_wnd:73088 rcv_wnd:131072 rehash:4                                                                                                 
ESTAB 0      0               192.168.3.169:57504           152.53.37.179:https
	 bbr wscale:11,12 rto:248 rtt:47.67/0.449 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:18 bytes_sent:636128 bytes_retrans:1470 bytes_acked:634659 bytes_received:26652 segs_out:2514 segs_in:2972 data_segs_out:762 data_segs_in:593 bbr:(bw:914kbps,mrtt:46.824,pacing_gain:2.88672,cwnd_gain:2.88672) send 4.37Mbps lastsnd:51498 lastrcv:51501 lastack:5378 pacing_rate 2.61Mbps delivery_rate 914kbps delivered:761 app_limited busy:30774ms retrans:0/2 rcv_space:14480 rcv_ssthresh:53172 minrtt:46.298 snd_wnd:57344 rcv_wnd:53248 rehash:1                                                                                                                                            
ESTAB 0      0               192.168.3.169:49820          209.177.156.94:https
	 bbr wscale:7,12 rto:218 rtt:17.609/11.944 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:4 bytes_sent:1153984 bytes_acked:1153985 bytes_received:898021 segs_out:12915 segs_in:11717 data_segs_out:5915 data_segs_in:5380 bbr:(bw:4Mbps,mrtt:11.062,pacing_gain:1,cwnd_gain:1) send 2.63Mbps lastsnd:17551 lastrcv:17535 lastack:17535 pacing_rate 23.5Mbps delivery_rate 4Mbps delivered:5916 app_limited busy:49423ms rcv_rtt:15 rcv_space:46509 rcv_ssthresh:503078 minrtt:10.578 snd_wnd:203136 rcv_wnd:503808                                                                                                                                                                             
ESTAB 0      0               192.168.3.169:37082           192.200.0.116:https
	 bbr wscale:10,12 rto:337 rtt:135.289/1.683 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:18 bytes_sent:3718 bytes_acked:3719 bytes_received:102759 segs_out:1509 segs_in:1521 data_segs_out:21 data_segs_in:788 bbr:(bw:348kbps,mrtt:132.97,pacing_gain:2.88672,cwnd_gain:2.88672) send 1.54Mbps lastsnd:1319374 lastrcv:20672 lastack:20672 pacing_rate 2.44Mbps delivery_rate 348kbps delivered:22 app_limited busy:2058ms rcv_rtt:133 rcv_space:19429 rcv_ssthresh:63978 minrtt:132.97 snd_wnd:76800 rcv_wnd:65536                                                                                                                                                                         
ESTAB 0      0                10.100.100.6:753              10.100.100.4:nfs  
	 bbr wscale:9,12 rto:208 rtt:7.721/12.02 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:58 ssthresh:709 bytes_sent:3866725120 bytes_retrans:40900864 bytes_acked:3825824257 bytes_received:18283767132 segs_out:6801290 segs_in:13626711 data_segs_out:2780731 data_segs_in:12930333 bbr:(bw:100Mbps,mrtt:0.937,pacing_gain:1.25,cwnd_gain:2) send 87Mbps lastsnd:1237 lastrcv:928 lastack:928 pacing_rate 124Mbps delivery_rate 100Mbps delivered:2764074 app_limited busy:1943369ms rwnd_limited:1688ms(0.1%) retrans:0/31575 dsack_dups:14927 rcv_rtt:1 rcv_space:714584 rcv_ssthresh:2549933 minrtt:0.251 rcv_ooopack:379 snd_wnd:11141120 rcv_wnd:2551808 rehash:47                        
ESTAB 0      0                10.100.100.6:808              10.100.100.4:nfs  
	 bbr wscale:9,12 rto:204 rtt:3.464/2.824 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:34 ssthresh:402 bytes_sent:3844311068 bytes_retrans:36936244 bytes_acked:3807374825 bytes_received:18333655248 segs_out:6801172 segs_in:13658685 data_segs_out:2765117 data_segs_in:12964860 bbr:(bw:71.3Mbps,mrtt:0.327,pacing_gain:1.25,cwnd_gain:2) send 114Mbps lastsnd:1354 lastrcv:1350 lastack:1350 pacing_rate 88.2Mbps delivery_rate 71.3Mbps delivered:2751114 app_limited busy:1928061ms rwnd_limited:1387ms(0.1%) retrans:0/28739 dsack_dups:14746 rcv_rtt:16.37 rcv_space:714584 rcv_ssthresh:4344562 minrtt:0.206 rcv_ooopack:937 snd_wnd:10406912 rcv_wnd:4345856 rehash:47              
ESTAB 0      0                10.100.100.6:964              10.100.100.4:nfs  
	 bbr wscale:9,12 rto:211 rtt:10.712/15.875 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:32 ssthresh:720 bytes_sent:3874354012 bytes_retrans:37995512 bytes_acked:3836358501 bytes_received:18157558864 segs_out:6788643 segs_in:13537723 data_segs_out:2785784 data_segs_in:12843393 bbr:(bw:58.4Mbps,mrtt:0.563,pacing_gain:1.25,cwnd_gain:2) send 34.6Mbps lastsnd:1298 lastrcv:1238 lastack:1238 pacing_rate 72.2Mbps delivery_rate 58.4Mbps delivered:2771145 app_limited busy:1910086ms rwnd_limited:1107ms(0.1%) retrans:0/29438 dsack_dups:14798 rcv_rtt:1.125 rcv_space:588608 rcv_ssthresh:3155618 minrtt:0.362 rcv_ooopack:605 snd_wnd:11141120 rcv_wnd:3158016 rehash:42           
ESTAB 0      0                10.100.100.6:972              10.100.100.4:nfs  
	 bbr wscale:9,12 rto:204 rtt:3.974/5.179 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:64 ssthresh:583 bytes_sent:3885030348 bytes_retrans:36045236 bytes_acked:3848985113 bytes_received:18288296588 segs_out:6820306 segs_in:13627986 data_segs_out:2793148 data_segs_in:12933316 bbr:(bw:123Mbps,mrtt:0.9,pacing_gain:1.25,cwnd_gain:2) send 187Mbps lastsnd:998 lastrcv:996 lastack:996 pacing_rate 152Mbps delivery_rate 123Mbps delivered:2779823 app_limited busy:1913705ms rwnd_limited:692ms(0.0%) retrans:0/28040 dsack_dups:14719 rcv_rtt:3.625 rcv_space:836216 rcv_ssthresh:5481558 minrtt:0.277 rcv_ooopack:657 snd_wnd:10136064 rcv_wnd:5484544 rehash:41                       
ESTAB 0      0                10.100.100.6:810              10.100.100.5:nfs  
	 bbr wscale:12,12 rto:201 rtt:0.321/0.088 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:138 ssthresh:441 bytes_sent:1698692520 bytes_retrans:188449632 bytes_acked:1510242889 bytes_received:8485470964 segs_out:1807647 segs_in:5989637 data_segs_out:1205537 data_segs_in:5894083 bbr:(bw:375Mbps,mrtt:0.225,pacing_gain:1.25,cwnd_gain:2) send 4.98Gbps lastsnd:1334 lastrcv:1333 lastack:1333 pacing_rate 464Mbps delivery_rate 375Mbps delivered:1075350 app_limited busy:150471ms rwnd_limited:5ms(0.0%) retrans:0/130599 dsack_dups:411 rcv_rtt:1 rcv_space:341756 rcv_ssthresh:1097611 minrtt:0.223 snd_wnd:6840320 rcv_wnd:1097728 rehash:176                                         
ESTAB 0      0                10.100.100.6:814              10.100.100.5:nfs  
	 bbr wscale:12,12 rto:203 rtt:2.172/3.77 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:122 ssthresh:756 bytes_sent:1789134444 bytes_retrans:176189224 bytes_acked:1612945221 bytes_received:8471989648 segs_out:1869865 segs_in:5988807 data_segs_out:1268397 data_segs_in:5885011 bbr:(bw:338Mbps,mrtt:0.22,pacing_gain:1.25,cwnd_gain:2) send 651Mbps lastsnd:970 lastrcv:970 lastack:970 pacing_rate 419Mbps delivery_rate 338Mbps delivered:1146609 app_limited busy:128199ms rwnd_limited:2ms(0.0%) retrans:0/122235 dsack_dups:447 rcv_rtt:1 rcv_space:356208 rcv_ssthresh:884161 minrtt:0.196 snd_wnd:6688768 rcv_wnd:884736 rehash:53                                                  
ESTAB 0      0                10.100.100.6:825              10.100.100.5:nfs  
	 bbr wscale:12,12 rto:201 rtt:0.414/0.313 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:136 ssthresh:525 bytes_sent:1843354360 bytes_retrans:355945364 bytes_acked:1487408997 bytes_received:8482367296 segs_out:1907832 segs_in:6004199 data_segs_out:1305917 data_segs_in:5892187 bbr:(bw:387Mbps,mrtt:0.182,pacing_gain:1.25,cwnd_gain:2) send 3.81Gbps lastsnd:10531 lastrcv:10530 lastack:10530 pacing_rate 479Mbps delivery_rate 387Mbps delivered:1059832 app_limited busy:159907ms rwnd_limited:7ms(0.0%) retrans:0/246453 dsack_dups:367 rcv_rtt:1 rcv_space:355480 rcv_ssthresh:867332 minrtt:0.167 snd_wnd:5279744 rcv_wnd:868352 rehash:191                                        
ESTAB 0      0                10.100.100.6:951              10.100.100.5:nfs  
	 bbr wscale:12,12 rto:201 rtt:0.618/0.659 ato:40 mss:1448 pmtu:1500 rcvmss:1448 advmss:1448 cwnd:154 ssthresh:676 bytes_sent:1689009644 bytes_retrans:186317108 bytes_acked:1502692537 bytes_received:8487078660 segs_out:1797858 segs_in:5990520 data_segs_out:1198803 data_segs_in:5895217 bbr:(bw:454Mbps,mrtt:0.189,pacing_gain:1.25,cwnd_gain:2) send 2.89Gbps lastsnd:1209 lastrcv:1208 lastack:1208 pacing_rate 562Mbps delivery_rate 454Mbps delivered:1070161 app_limited busy:147515ms rwnd_limited:2ms(0.0%) retrans:0/129089 dsack_dups:446 reordering:87 reord_seen:2 rcv_rtt:1 rcv_space:436568 rcv_ssthresh:2996168 minrtt:0.131 rcv_ooopack:1 snd_wnd:9240576 rcv_wnd:2998272 rehash:150
ESTAB 0      0                   127.0.0.1:59046               127.0.0.1:5900 
	 bbr wscale:12,12 rto:201 rtt:0.031/0.002 ato:40 mss:22528 pmtu:65535 rcvmss:603 advmss:65483 cwnd:18 bytes_sent:40890 bytes_acked:40891 bytes_received:101506 segs_out:4122 segs_in:8131 data_segs_out:4081 data_segs_in:4054 bbr:(bw:8.19Gbps,mrtt:0.022,pacing_gain:2.88672,cwnd_gain:2.88672) send 105Gbps lastsnd:102 lastrcv:107 lastack:102 pacing_rate 135Gbps delivery_rate 8.19Gbps delivered:4082 app_limited busy:629ms rcv_rtt:355069 rcv_space:45087 rcv_ssthresh:33450 minrtt:0.022 snd_wnd:45056 rcv_wnd:45056                                                                                                                                                                          
ESTAB 0      0                   127.0.0.1:5900                127.0.0.1:59046
	 bbr wscale:12,12 rto:206 rtt:5.282/1.456 ato:40 mss:22528 pmtu:65535 rcvmss:536 advmss:65483 cwnd:18 bytes_sent:101506 bytes_acked:101506 bytes_received:40890 segs_out:8130 segs_in:4122 data_segs_out:4054 data_segs_in:4081 bbr:(bw:7.84Gbps,mrtt:0.023,pacing_gain:2.88672,cwnd_gain:2.88672) send 614Mbps lastsnd:108 lastrcv:103 lastack:103 pacing_rate 178Gbps delivery_rate 7.84Gbps delivered:4055 app_limited busy:17757ms rcv_space:43690 rcv_ssthresh:43690 minrtt:0.023 snd_wnd:45056 rcv_wnd:45056                                                                                                                                                                                      
ESTAB 0      0               100.73.35.111:ssh           100.101.187.119:60286
	 bbr wscale:7,12 rto:205 rtt:4.597/7.27 ato:40 mss:1228 pmtu:1280 rcvmss:1228 advmss:1228 cwnd:26 bytes_sent:5369 bytes_acked:5369 bytes_received:3941 segs_out:23 segs_in:23 data_segs_out:16 data_segs_in:14 bbr:(bw:26.8Mbps,mrtt:0.594,pacing_gain:2.88672,cwnd_gain:2.88672) send 55.6Mbps lastsnd:8277 lastrcv:8278 lastack:8277 pacing_rate 473Mbps delivery_rate 26.8Mbps delivered:17 app_limited busy:61ms rcv_rtt:8 rcv_space:12280 rcv_ssthresh:58024 minrtt:0.594 snd_wnd:76544 rcv_wnd:61440                                                                                                                                                                                              
ESTAB 0      0      [::ffff:100.73.35.111]:8006  [::ffff:100.109.70.137]:26831
	 bbr wscale:8,12 rto:205 rtt:4.835/1.464 ato:40 mss:1240 pmtu:1280 rcvmss:1240 advmss:1240 cwnd:44 bytes_sent:202439 bytes_acked:202439 bytes_received:158749 segs_out:8128 segs_in:4097 data_segs_out:4059 data_segs_in:4086 bbr:(bw:10.2Mbps,mrtt:1.429,pacing_gain:2.88672,cwnd_gain:2.88672) send 90.3Mbps lastsnd:119 lastrcv:115 lastack:115 pacing_rate 136Mbps delivery_rate 10.2Mbps delivered:4060 app_limited busy:17406ms rcv_rtt:218187 rcv_space:45433 rcv_ssthresh:40276 minrtt:1.429 snd_wnd:65024 rcv_wnd:45056                                                                                                                                                                        
ESTAB 0      0      [::ffff:100.73.35.111]:8006  [::ffff:100.109.70.137]:10582
	 bbr wscale:8,12 rto:209 rtt:8.162/12.428 ato:40 mss:1240 pmtu:1280 rcvmss:1240 advmss:1240 cwnd:16 bytes_sent:4866 bytes_acked:4866 bytes_received:2956 segs_out:7 segs_in:8 data_segs_out:6 data_segs_in:3 bbr:(bw:11.2Mbps,mrtt:1.887,pacing_gain:2.88672,cwnd_gain:2.88672) send 19.4Mbps lastsnd:1642 lastrcv:1645 lastack:1593 pacing_rate 143Mbps delivery_rate 11.2Mbps delivered:7 app_limited busy:55ms rcv_space:12400 rcv_ssthresh:35839 minrtt:1.887 snd_wnd:65280 rcv_wnd:45056                                                                                                                                                                                                           
ESTAB 0      0      [::ffff:100.73.35.111]:8006  [::ffff:100.125.183.68]:60052
	 bbr wscale:8,12 rto:201 rtt:0.609/0.216 ato:40 mss:1228 pmtu:1280 rcvmss:1228 advmss:1228 cwnd:25 bytes_sent:14565 bytes_acked:14565 bytes_received:2676 segs_out:16 segs_in:13 data_segs_out:15 data_segs_in:6 bbr:(bw:49.4Mbps,mrtt:0.451,pacing_gain:2.88672,cwnd_gain:2.88672) send 403Mbps lastsnd:2819 lastrcv:2823 lastack:2818 pacing_rate 623Mbps delivery_rate 49.4Mbps delivered:16 app_limited busy:3ms rcv_rtt:1 rcv_space:12280 rcv_ssthresh:55924 minrtt:0.451 snd_wnd:85248 rcv_wnd:57344                                                                                                                                                                                              
ESTAB 0      0      [::ffff:100.73.35.111]:8006  [::ffff:100.109.70.137]:12306
	 bbr wscale:8,12 rto:203 rtt:2.362/1.635 ato:40 mss:1240 pmtu:1280 rcvmss:1240 advmss:1240 cwnd:15 bytes_sent:4681 bytes_acked:4681 bytes_received:3231 segs_out:6 segs_in:7 data_segs_out:5 data_segs_in:3 bbr:(bw:13.6Mbps,mrtt:1.454,pacing_gain:2.88672,cwnd_gain:2.88672) send 63Mbps lastsnd:1636 lastrcv:1640 lastack:1634 pacing_rate 160Mbps delivery_rate 13.6Mbps delivered:6 app_limited busy:8ms rcv_space:12400 rcv_ssthresh:41300 minrtt:1.454 snd_wnd:65280 rcv_wnd:45056                                                                                                                                                                                                               

--- /proc/net/snmp (TCP summary)
    $ grep -A1 ^Tcp: /proc/net/snmp
Tcp: RtoAlgorithm RtoMin RtoMax MaxConn ActiveOpens PassiveOpens AttemptFails EstabResets CurrEstab InSegs OutSegs RetransSegs InErrs OutRsts InCsumErrors
Tcp: 1 200 120000 -1 323034 52300 9724 32 19 32723027 44231629 758508 6 5787 0
Udp: InDatagrams NoPorts InErrors OutDatagrams RcvbufErrors SndbufErrors InCsumErrors IgnoredMulti MemErrors

--- TCP retrans stats
    $ grep -A1 ^Tcp: /proc/net/snmp
Tcp: RtoAlgorithm RtoMin RtoMax MaxConn ActiveOpens PassiveOpens AttemptFails EstabResets CurrEstab InSegs OutSegs RetransSegs InErrs OutRsts InCsumErrors
Tcp: 1 200 120000 -1 323034 52300 9724 32 19 32723027 44231629 758508 6 5787 0
Udp: InDatagrams NoPorts InErrors OutDatagrams RcvbufErrors SndbufErrors InCsumErrors IgnoredMulti MemErrors

--- nstat TCP summary
    $ nstat -az Tcp_RetransSegs Tcp_InErrs Tcp_OutRsts Tcp_ActiveOpens Tcp_PassiveOpens
#kernel

###############################################################################
# 14. STORAGE: BLOCK DEVICES
###############################################################################

--- lsblk (key cols)
    $ lsblk -o NAME,SIZE,TYPE,MOUNTPOINT,FSTYPE,MODEL,SERIAL,STATE,ROTA,DISC-GRAN,DISC-MAX
NAME                SIZE TYPE MOUNTPOINT FSTYPE      MODEL                SERIAL          STATE   ROTA DISC-GRAN DISC-MAX
sda                 1.8T disk                        WDC WD20SDRM-59A4DS1 WD-WXL2A232X5RX running    1        0B       0B
├─sda1             1007K part                                                                        1        0B       0B
├─sda2                1G part            vfat                                                        1        0B       0B
└─sda3              1.8T part            LVM2_member                                                 1        0B       0B
  ├─pve-swap          8G lvm  [SWAP]     swap                                             running    1        0B       0B
  ├─pve-root         96G lvm  /          ext4                                             running    1        0B       0B
  ├─pve-data_tmeta 15.9G lvm                                                              running    1        0B       0B
  │ └─pve-data      1.7T lvm                                                              running    1        0B       0B
  └─pve-data_tdata  1.7T lvm                                                              running    1        0B       0B
    └─pve-data      1.7T lvm                                                              running    1        0B       0B

--- lsblk -t
    $ lsblk -t
NAME               ALIGNMENT MIN-IO OPT-IO PHY-SEC LOG-SEC ROTA SCHED       RQ-SIZE   RA WSAME
sda                        0    512      0     512     512    1 mq-deadline       2 4096    0B
├─sda1                     0    512      0     512     512    1 mq-deadline       2 4096    0B
├─sda2                     0    512      0     512     512    1 mq-deadline       2 4096    0B
└─sda3                     0    512      0     512     512    1 mq-deadline       2 4096    0B
  ├─pve-swap               0    512      0     512     512    1                     4096    0B
  ├─pve-root               0    512      0     512     512    1                     4096    0B
  ├─pve-data_tmeta         0    512      0     512     512    1                     4096    0B
  │ └─pve-data             0  65536  65536     512     512    1                     4096    0B
  └─pve-data_tdata         0    512      0     512     512    1                     4096    0B
    └─pve-data             0  65536  65536     512     512    1                     4096    0B

--- lsblk -O (everything, capped)
    $ lsblk -O
ALIGNMENT ID-LINK                      ID                       DISC-ALN DAX DISC-GRAN DISK-SEQ DISC-MAX DISC-ZERO FSAVAIL FSROOTS FSSIZE FSTYPE      FSUSED FSUSE% FSVER    GROUP HCTL       HOTPLUG KNAME LABEL LOG-SEC MAJ:MIN MAJ MIN MIN-IO MODE       MODEL                 MQ NAME               OPT-IO OWNER PARTFLAGS PARTLABEL PARTN PARTTYPE                             PARTTYPENAME PARTUUID                             PATH                       PHY-SEC PKNAME PTTYPE PTUUID                                 RA RAND      REV RM RO ROTA RQ-SIZE SCHED       SERIAL           SIZE   START STATE   SUBSYSTEMS         MOUNTPOINT MOUNTPOINTS TRAN TYPE UUID                                   VENDOR   WSAME WWN                ZONED ZONE-SZ ZONE-WGRAN ZONE-APP ZONE-NR ZONE-OMAX ZONE-AMAX
        0 wwn-0x50014ee215a96feb       0x50014ee215a96feb              0   0        0B        9       0B         0                                                           disk  0:0:0:0          0 sda             512   8:0   8   0      512 brw-rw---- WDC WD20SDRM-59A4DS1   1 sda                     0 root                                                                                                                   /dev/sda                       512        gpt    025e5938-0803-4136-bae5-7dcb01e5165d 4096    1 01.01A01  0  0    1       2 mq-deadline WD-WXL2A232X5RX  1.8T         running block:scsi:usb:pci                        usb  disk                                        WD          0B 0x50014ee215a96feb none       0B         0B       0B       0         0         0
        0 wwn-0x50014ee215a96feb-part1 0x50014ee215a96feb-part1        0   0        0B        9       0B         0                                                           disk                   0 sda1            512   8:1   8   1      512 brw-rw----                        1 ├─sda1                  0 root                          1 21686148-6449-6e6f-744e-656564454649 BIOS boot    8d928c72-cd89-456f-9c5b-29761e8e1be6 /dev/sda1                      512 sda    gpt    025e5938-0803-4136-bae5-7dcb01e5165d 4096    1           0  0    1       2 mq-deadline                 1007K      34         block:scsi:usb:pci                             part                                                    0B 0x50014ee215a96feb none       0B         0B       0B       0         0         0
        0 wwn-0x50014ee215a96feb-part2 0x50014ee215a96feb-part2        0   0        0B        9       0B         0                        vfat                      FAT32    disk                   0 sda2            512   8:2   8   2      512 brw-rw----                        1 ├─sda2                  0 root                          2 c12a7328-f81f-11d2-ba4b-00a0c93ec93b EFI System   827007c4-8d16-445e-a1b0-40fadc814747 /dev/sda2                      512 sda    gpt    025e5938-0803-4136-bae5-7dcb01e5165d 4096    1           0  0    1       2 mq-deadline                    1G    2048         block:scsi:usb:pci                             part 9E38-EF37                                          0B 0x50014ee215a96feb none       0B         0B       0B       0         0         0
        0 wwn-0x50014ee215a96feb-part3 0x50014ee215a96feb-part3        0   0        0B        9       0B         0                        LVM2_member               LVM2 001 disk                   0 sda3            512   8:3   8   3      512 brw-rw----                        1 └─sda3                  0 root                          3 e6d6d379-f507-44c2-a23c-238f2a3df928 Linux LVM    f534b537-a35f-4721-a245-669bcd1fc02e /dev/sda3                      512 sda    gpt    025e5938-0803-4136-bae5-7dcb01e5165d 4096    1           0  0    1       2 mq-deadline                  1.8T 2099200         block:scsi:usb:pci                             part aBoPok-Y20Z-3hHs-Buu6-ybpQ-KwCM-fbOoLy             0B 0x50014ee215a96feb none       0B         0B       0B       0         0         0
        0 dm-name-pve-swap             name-pve-swap                   0   0        0B       10       0B         0                        swap                      1        disk                   0 dm-0            512 252:0   252 0      512 brw-rw----                        1   ├─pve-swap            0 root                                                                                                                   /dev/mapper/pve-swap           512 sda3                                               4096    0           0  0    1                                        8G         running block              [SWAP]     [SWAP]           lvm  d75fe8d2-f4a5-4bb1-b6e1-75f0459945e7               0B                    none       0B         0B       0B       0         0         0
        0 dm-name-pve-root             name-pve-root                   0   0        0B       11       0B         0   77.9G /        93.9G ext4         11.3G    12% 1.0      disk                   0 dm-1            512 252:1   252 1      512 brw-rw----                        1   ├─pve-root            0 root                                                                                                                   /dev/mapper/pve-root           512 sda3                                               4096    0           0  0    1                                       96G         running block              /          /                lvm  8f69bbb5-3cdd-4b0b-97d0-f1c2541d8e83               0B                    none       0B         0B       0B       0         0         0
        0                                                              0   0        0B       12       0B         0                                                           disk                   0 dm-2            512 252:2   252 2      512 brw-rw----                        1   ├─pve-data_tmeta      0 root                                                                                                                   /dev/mapper/pve-data_tmeta     512 sda3                                               4096    0           0  0    1                                     15.9G         running block                                          lvm                                                     0B                    none       0B         0B       0B       0         0         0
        0                                                              0   0        0B       14       0B         0                                                           disk                   0 dm-4            512 252:4   252 4    65536 brw-rw----                        1   │ └─pve-data      65536 root                                                                                                                   /dev/mapper/pve-data           512 dm-2                                               4096    0           0  0    1                                      1.7T         running block                                          lvm                                                     0B                    none       0B         0B       0B       0         0         0
        0                                                              0   0        0B       13       0B         0                                                           disk                   0 dm-3            512 252:3   252 3      512 brw-rw----                        1   └─pve-data_tdata      0 root                                                                                                                   /dev/mapper/pve-data_tdata     512 sda3                                               4096    0           0  0    1                                      1.7T         running block                                          lvm                                                     0B                    none       0B         0B       0B       0         0         0
        0                                                              0   0        0B       14       0B         0                                                           disk                   0 dm-4            512 252:4   252 4    65536 brw-rw----                        1     └─pve-data      65536 root                                                                                                                   /dev/mapper/pve-data           512 dm-3                                               4096    0           0  0    1                                      1.7T         running block                                          lvm                                                     0B                    none       0B         0B       0B       0         0         0

--- blkid
    $ blkid
/dev/mapper/pve-root: UUID="8f69bbb5-3cdd-4b0b-97d0-f1c2541d8e83" BLOCK_SIZE="4096" TYPE="ext4"
/dev/mapper/pve-swap: UUID="d75fe8d2-f4a5-4bb1-b6e1-75f0459945e7" TYPE="swap"
/dev/sda2: UUID="9E38-EF37" BLOCK_SIZE="512" TYPE="vfat" PARTUUID="827007c4-8d16-445e-a1b0-40fadc814747"
/dev/sda3: UUID="aBoPok-Y20Z-3hHs-Buu6-ybpQ-KwCM-fbOoLy" TYPE="LVM2_member" PARTUUID="f534b537-a35f-4721-a245-669bcd1fc02e"
/dev/sda1: PARTUUID="8d928c72-cd89-456f-9c5b-29761e8e1be6"

--- /proc/partitions
    $ cat /proc/partitions
major minor  #blocks  name

   8        0 1953481728 sda
   8        1       1007 sda1
   8        2    1048576 sda2
   8        3 1952432111 sda3
 252        0    8388608 dm-0
 252        1  100663296 dm-1
 252        2   16650240 dm-2
 252        3 1793044480 dm-3
 252        4 1793044480 dm-4

--- fdisk -l
    $ fdisk -l
Disk /dev/sda: 1.82 TiB, 2000365289472 bytes, 3906963456 sectors
Disk model: My Passport 260D
Units: sectors of 1 * 512 = 512 bytes
Sector size (logical/physical): 512 bytes / 512 bytes
I/O size (minimum/optimal): 512 bytes / 512 bytes
Disklabel type: gpt
Disk identifier: 025E5938-0803-4136-BAE5-7DCB01E5165D

Device       Start        End    Sectors  Size Type
/dev/sda1       34       2047       2014 1007K BIOS boot
/dev/sda2     2048    2099199    2097152    1G EFI System
/dev/sda3  2099200 3906963422 3904864223  1.8T Linux LVM


Disk /dev/mapper/pve-swap: 8 GiB, 8589934592 bytes, 16777216 sectors
Units: sectors of 1 * 512 = 512 bytes
Sector size (logical/physical): 512 bytes / 512 bytes
I/O size (minimum/optimal): 512 bytes / 512 bytes


Disk /dev/mapper/pve-root: 96 GiB, 103079215104 bytes, 201326592 sectors
Units: sectors of 1 * 512 = 512 bytes
Sector size (logical/physical): 512 bytes / 512 bytes
I/O size (minimum/optimal): 512 bytes / 512 bytes

--- parted -l
    $ parted -l
/root/check.sh: line 45: parted: command not found
    [exit=127 / not installed or not permitted]

--- block device queue settings (per device)
    $ for d in $(ls /sys/block/ 2>/dev/null | grep -vE '^(loop|ram|md|dm-|sr|fd)'); do
    q="/sys/block/$d/queue"
    [ -d "$q" ] || continue
    printf '----- %s -----\n' "$d"
    for k in scheduler rotational nr_requests read_ahead_kb max_sectors_kb max_hw_sectors_kb \
             logical_block_size physical_block_size discard_granularity discard_max_hw_bytes \
             rq_affinity nomerges wbt_lat_usec write_cache stable_writes io_poll io_poll_delay \
             fua rot_stable_writes add_random zoned dma_alignment iostats;
    do
        f="$q/$k"
        [ -r "$f" ] && printf '  %-22s = %s\n' "$k" "$(cat "$f" 2>/dev/null)"
    done
    # NVMe-specific
    for f in /sys/block/$d/device/model /sys/block/$d/device/serial /sys/block/$d/device/transport /sys/block/$d/device/queue_count; do
        [ -r "$f" ] && printf '  %s = %s\n' "$(echo "$f" | sed "s|/sys/block/$d/device/||")" "$(cat "$f")"
    done
done
/root/check.sh: line 62: printf: --: invalid option
printf: usage: printf [-v var] format [arguments]
  scheduler              = none [mq-deadline] 
  rotational             = 1
  nr_requests            = 2
  read_ahead_kb          = 4096
  max_sectors_kb         = 120
  max_hw_sectors_kb      = 120
  logical_block_size     = 512
  physical_block_size    = 512
  discard_granularity    = 0
  discard_max_hw_bytes   = 0
  rq_affinity            = 1
  nomerges               = 0
  wbt_lat_usec           = 75000
  write_cache            = write through
  stable_writes          = 0
  io_poll                = 0
  io_poll_delay          = -1
  fua                    = 0
  add_random             = 1
  zoned                  = none
  dma_alignment          = 511
  iostats                = 1
  model = My Passport 260D
    [exit=1]

--- df -h (filesystem usage)
    $ df -h
Filesystem                             Size  Used Avail Use% Mounted on
udev                                    59G     0   59G   0% /dev
tmpfs                                   13G  3.5M   13G   1% /run
/dev/mapper/pve-root                    94G   12G   78G  13% /
tmpfs                                   63G   49M   63G   1% /dev/shm
tmpfs                                  1.0M     0  1.0M   0% /run/credentials/systemd-journald.service
tmpfs                                  5.0M     0  5.0M   0% /run/lock
tmpfs                                   63G   24K   63G   1% /tmp
/dev/fuse                              128M   20K  128M   1% /etc/pve
tmpfs                                  1.0M     0  1.0M   0% /run/credentials/getty@tty1.service
pfv-tsys5-nfs-stor:/mnt/pfv-tsys5/S2   916G   26G  844G   3% /mnt/pve/S2
pfv-tsys4-nfs-stor:/mnt/tsys4/D5       1.8T  210G  1.5T  13% /mnt/pve/D5
pfv-tsys5-nfs-stor:/mnt/pfv-tsys5/S4   458G  2.4G  432G   1% /mnt/pve/S4
pfv-tsys5-nfs-stor:/mnt/pfv-tsys5/ssd  234G  131G   91G  59% /mnt/pve/T5-SSD
pfv-tsys4-nfs-stor:/mnt/tsys4/D2       2.7T  189G  2.4T   8% /mnt/pve/D2
pfv-tsys5-nfs-stor:/mnt/pfv-tsys5/S3   916G   13G  857G   2% /mnt/pve/S3
pfv-tsys4-nfs-stor:/mnt/tsys4/D3       469G  2.0M  445G   1% /mnt/pve/D3
tmpfs                                   13G  4.0K   13G   1% /run/user/0

--- df -i (inode usage)
    $ df -i
Filesystem                               Inodes IUsed     IFree IUse% Mounted on
udev                                   15346505   603  15345902    1% /dev
tmpfs                                  16498882  1117  16497765    1% /run
/dev/mapper/pve-root                    6291456 82271   6209185    2% /
tmpfs                                  16498882   114  16498768    1% /dev/shm
tmpfs                                      1024     1      1023    1% /run/credentials/systemd-journald.service
tmpfs                                  16498882    22  16498860    1% /run/lock
tmpfs                                   1048576    14   1048562    1% /tmp
/dev/fuse                                262144    37    262107    1% /etc/pve
tmpfs                                      1024     1      1023    1% /run/credentials/getty@tty1.service
pfv-tsys5-nfs-stor:/mnt/pfv-tsys5/S2   61054976    21  61054955    1% /mnt/pve/S2
pfv-tsys4-nfs-stor:/mnt/tsys4/D5      122101760    56 122101704    1% /mnt/pve/D5
pfv-tsys5-nfs-stor:/mnt/pfv-tsys5/S4   30531584    15  30531569    1% /mnt/pve/S4
pfv-tsys5-nfs-stor:/mnt/pfv-tsys5/ssd  15630336    15  15630321    1% /mnt/pve/T5-SSD
pfv-tsys4-nfs-stor:/mnt/tsys4/D2      183148544    54 183148490    1% /mnt/pve/D2
pfv-tsys5-nfs-stor:/mnt/pfv-tsys5/S3   61054976    21  61054955    1% /mnt/pve/S3
pfv-tsys4-nfs-stor:/mnt/tsys4/D3       31260672    13  31260659    1% /mnt/pve/D3
tmpfs                                   3299776    26   3299750    1% /run/user/0

###############################################################################
# 15. STORAGE: MOUNTS & FILESYSTEMS
###############################################################################

--- mount (filtered)
    $ mount
sysfs on /sys type sysfs (rw,nosuid,nodev,noexec,relatime)
proc on /proc type proc (rw,relatime)
udev on /dev type devtmpfs (rw,nosuid,relatime,size=61386020k,nr_inodes=15346505,mode=755,inode64)
devpts on /dev/pts type devpts (rw,nosuid,noexec,relatime,gid=5,mode=600,ptmxmode=000)
tmpfs on /run type tmpfs (rw,nosuid,nodev,noexec,relatime,size=13199108k,mode=755,inode64)
/dev/mapper/pve-root on / type ext4 (rw,relatime,errors=remount-ro)
securityfs on /sys/kernel/security type securityfs (rw,nosuid,nodev,noexec,relatime)
tmpfs on /dev/shm type tmpfs (rw,nosuid,nodev,inode64)
cgroup2 on /sys/fs/cgroup type cgroup2 (rw,nosuid,nodev,noexec,relatime,nsdelegate,memory_recursiveprot)
none on /sys/fs/pstore type pstore (rw,nosuid,nodev,noexec,relatime)
bpf on /sys/fs/bpf type bpf (rw,nosuid,nodev,noexec,relatime,mode=700)
systemd-1 on /proc/sys/fs/binfmt_misc type autofs (rw,relatime,fd=37,pgrp=1,timeout=0,minproto=5,maxproto=5,direct,pipe_ino=12792)
tmpfs on /run/credentials/systemd-journald.service type tmpfs (ro,nosuid,nodev,noexec,relatime,nosymfollow,size=1024k,nr_inodes=1024,mode=700,inode64,noswap)
configfs on /sys/kernel/config type configfs (rw,nosuid,nodev,noexec,relatime)
tmpfs on /run/lock type tmpfs (rw,nosuid,nodev,noexec,relatime,size=5120k,inode64)
tracefs on /sys/kernel/tracing type tracefs (rw,nosuid,nodev,noexec,relatime)
fusectl on /sys/fs/fuse/connections type fusectl (rw,nosuid,nodev,noexec,relatime)
debugfs on /sys/kernel/debug type debugfs (rw,nosuid,nodev,noexec,relatime)
mqueue on /dev/mqueue type mqueue (rw,nosuid,nodev,noexec,relatime)
hugetlbfs on /dev/hugepages type hugetlbfs (rw,nosuid,nodev,relatime,pagesize=2M)
tmpfs on /tmp type tmpfs (rw,nosuid,nodev,size=65995532k,nr_inodes=1048576,inode64)
binfmt_misc on /proc/sys/fs/binfmt_misc type binfmt_misc (rw,nosuid,nodev,noexec,relatime)
sunrpc on /run/rpc_pipefs type rpc_pipefs (rw,relatime)
lxcfs on /var/lib/lxcfs type fuse.lxcfs (rw,nosuid,nodev,relatime,user_id=0,group_id=0,allow_other)
/dev/fuse on /etc/pve type fuse (rw,nosuid,nodev,relatime,user_id=0,group_id=0,default_permissions,allow_other)
tmpfs on /run/credentials/getty@tty1.service type tmpfs (ro,nosuid,nodev,noexec,relatime,nosymfollow,size=1024k,nr_inodes=1024,mode=700,inode64,noswap)
pfv-tsys5-nfs-stor:/mnt/pfv-tsys5/S2 on /mnt/pve/S2 type nfs4 (rw,noatime,vers=4.2,rsize=1048576,wsize=1048576,namlen=255,hard,fatal_neterrors=none,proto=tcp,nconnect=4,timeo=600,retrans=2,sec=sys,clientaddr=10.100.100.6,local_lock=none,addr=10.100.100.5)
pfv-tsys4-nfs-stor:/mnt/tsys4/D5 on /mnt/pve/D5 type nfs4 (rw,noatime,vers=4.2,rsize=1048576,wsize=1048576,namlen=255,hard,fatal_neterrors=none,proto=tcp,nconnect=4,timeo=600,retrans=2,sec=sys,clientaddr=10.100.100.6,local_lock=none,addr=10.100.100.4)
pfv-tsys5-nfs-stor:/mnt/pfv-tsys5/S4 on /mnt/pve/S4 type nfs4 (rw,noatime,vers=4.2,rsize=1048576,wsize=1048576,namlen=255,hard,fatal_neterrors=none,proto=tcp,nconnect=4,timeo=600,retrans=2,sec=sys,clientaddr=10.100.100.6,local_lock=none,addr=10.100.100.5)
pfv-tsys5-nfs-stor:/mnt/pfv-tsys5/ssd on /mnt/pve/T5-SSD type nfs4 (rw,noatime,vers=4.2,rsize=1048576,wsize=1048576,namlen=255,hard,fatal_neterrors=none,proto=tcp,nconnect=4,timeo=600,retrans=2,sec=sys,clientaddr=10.100.100.6,local_lock=none,addr=10.100.100.5)
pfv-tsys4-nfs-stor:/mnt/tsys4/D2 on /mnt/pve/D2 type nfs4 (rw,noatime,vers=4.2,rsize=1048576,wsize=1048576,namlen=255,hard,fatal_neterrors=none,proto=tcp,nconnect=4,timeo=600,retrans=2,sec=sys,clientaddr=10.100.100.6,local_lock=none,addr=10.100.100.4)
pfv-tsys5-nfs-stor:/mnt/pfv-tsys5/S3 on /mnt/pve/S3 type nfs4 (rw,noatime,vers=4.2,rsize=1048576,wsize=1048576,namlen=255,hard,fatal_neterrors=none,proto=tcp,nconnect=4,timeo=600,retrans=2,sec=sys,clientaddr=10.100.100.6,local_lock=none,addr=10.100.100.5)
pfv-tsys4-nfs-stor:/mnt/tsys4/D3 on /mnt/pve/D3 type nfs4 (rw,noatime,vers=4.2,rsize=1048576,wsize=1048576,namlen=255,hard,fatal_neterrors=none,proto=tcp,nconnect=4,timeo=600,retrans=2,sec=sys,clientaddr=10.100.100.6,local_lock=none,addr=10.100.100.4)
tmpfs on /run/user/0 type tmpfs (rw,nosuid,nodev,relatime,size=13199104k,nr_inodes=3299776,mode=700,inode64)

--- findmnt (tree)
    $ findmnt -t nfs,nfs4,zfs,ext4,xfs,btrfs
TARGET            SOURCE                                FSTYPE OPTIONS
/                 /dev/mapper/pve-root                  ext4   rw,relatime,errors=remount-ro
├─/mnt/pve/S2     pfv-tsys5-nfs-stor:/mnt/pfv-tsys5/S2  nfs4   rw,noatime,vers=4.2,rsize=1048576,wsize=1048576,namlen=255,hard,fatal_neterrors=none,proto=tcp,nconnect=4,timeo=600,retrans=2,sec=sys,clientaddr=10.100.100.6,local_lock=none,addr=10.100.100.5
├─/mnt/pve/D5     pfv-tsys4-nfs-stor:/mnt/tsys4/D5      nfs4   rw,noatime,vers=4.2,rsize=1048576,wsize=1048576,namlen=255,hard,fatal_neterrors=none,proto=tcp,nconnect=4,timeo=600,retrans=2,sec=sys,clientaddr=10.100.100.6,local_lock=none,addr=10.100.100.4
├─/mnt/pve/S4     pfv-tsys5-nfs-stor:/mnt/pfv-tsys5/S4  nfs4   rw,noatime,vers=4.2,rsize=1048576,wsize=1048576,namlen=255,hard,fatal_neterrors=none,proto=tcp,nconnect=4,timeo=600,retrans=2,sec=sys,clientaddr=10.100.100.6,local_lock=none,addr=10.100.100.5
├─/mnt/pve/T5-SSD pfv-tsys5-nfs-stor:/mnt/pfv-tsys5/ssd nfs4   rw,noatime,vers=4.2,rsize=1048576,wsize=1048576,namlen=255,hard,fatal_neterrors=none,proto=tcp,nconnect=4,timeo=600,retrans=2,sec=sys,clientaddr=10.100.100.6,local_lock=none,addr=10.100.100.5
├─/mnt/pve/D2     pfv-tsys4-nfs-stor:/mnt/tsys4/D2      nfs4   rw,noatime,vers=4.2,rsize=1048576,wsize=1048576,namlen=255,hard,fatal_neterrors=none,proto=tcp,nconnect=4,timeo=600,retrans=2,sec=sys,clientaddr=10.100.100.6,local_lock=none,addr=10.100.100.4
├─/mnt/pve/S3     pfv-tsys5-nfs-stor:/mnt/pfv-tsys5/S3  nfs4   rw,noatime,vers=4.2,rsize=1048576,wsize=1048576,namlen=255,hard,fatal_neterrors=none,proto=tcp,nconnect=4,timeo=600,retrans=2,sec=sys,clientaddr=10.100.100.6,local_lock=none,addr=10.100.100.5
└─/mnt/pve/D3     pfv-tsys4-nfs-stor:/mnt/tsys4/D3      nfs4   rw,noatime,vers=4.2,rsize=1048576,wsize=1048576,namlen=255,hard,fatal_neterrors=none,proto=tcp,nconnect=4,timeo=600,retrans=2,sec=sys,clientaddr=10.100.100.6,local_lock=none,addr=10.100.100.4

--- /etc/fstab
    --- /etc/fstab ---
# <file system> <mount point> <type> <options> <dump> <pass>
/dev/pve/root / ext4 errors=remount-ro 0 1
/dev/pve/swap none swap sw 0 0
proc /proc proc defaults 0 0

--- ext4 reserved block % (per fs)
    $ for dev in $(awk '$3=="ext4"{print $1}' /proc/mounts 2>/dev/null); do
    echo "=== $dev ==="
    dumpe2fs -h "$dev" 2>/dev/null | grep -E 'Reserved|Block count|Free blocks|Block size|Mount count|Maximum mount|Last'
done
=== /dev/mapper/pve-root ===
Last mounted on:          /
Block count:              25165824
Reserved block count:     1258291
Free blocks:              21677447
Block size:               4096
Reserved GDT blocks:      1024
Last mount time:          Sun Jul 26 17:19:37 2026
Last write time:          Wed Jul 29 04:21:52 2026
Mount count:              17
Maximum mount count:      -1
Last checked:             Sat Apr  4 12:26:59 2026
Reserved blocks uid:      0 (user root)
Reserved blocks gid:      0 (group root)

--- xfs info (per fs)
    $ for mp in $(awk '$3=="xfs"{print $2}' /proc/mounts 2>/dev/null); do
    echo "=== $mp ==="
    xfs_info "$mp" 2>/dev/null
done

###############################################################################
# 16. STORAGE: NFS (CLIENT + SERVER)
###############################################################################

--- nfsstat -m (mount options)
    $ nfsstat -m
/mnt/pve/S2 from pfv-tsys5-nfs-stor:/mnt/pfv-tsys5/S2
 Flags:	rw,noatime,vers=4.2,rsize=1048576,wsize=1048576,namlen=255,hard,fatal_neterrors=none,proto=tcp,nconnect=4,timeo=600,retrans=2,sec=sys,clientaddr=10.100.100.6,local_lock=none,addr=10.100.100.5

/mnt/pve/D5 from pfv-tsys4-nfs-stor:/mnt/tsys4/D5
 Flags:	rw,noatime,vers=4.2,rsize=1048576,wsize=1048576,namlen=255,hard,fatal_neterrors=none,proto=tcp,nconnect=4,timeo=600,retrans=2,sec=sys,clientaddr=10.100.100.6,local_lock=none,addr=10.100.100.4

/mnt/pve/S4 from pfv-tsys5-nfs-stor:/mnt/pfv-tsys5/S4
 Flags:	rw,noatime,vers=4.2,rsize=1048576,wsize=1048576,namlen=255,hard,fatal_neterrors=none,proto=tcp,nconnect=4,timeo=600,retrans=2,sec=sys,clientaddr=10.100.100.6,local_lock=none,addr=10.100.100.5

/mnt/pve/T5-SSD from pfv-tsys5-nfs-stor:/mnt/pfv-tsys5/ssd
 Flags:	rw,noatime,vers=4.2,rsize=1048576,wsize=1048576,namlen=255,hard,fatal_neterrors=none,proto=tcp,nconnect=4,timeo=600,retrans=2,sec=sys,clientaddr=10.100.100.6,local_lock=none,addr=10.100.100.5

/mnt/pve/D2 from pfv-tsys4-nfs-stor:/mnt/tsys4/D2
 Flags:	rw,noatime,vers=4.2,rsize=1048576,wsize=1048576,namlen=255,hard,fatal_neterrors=none,proto=tcp,nconnect=4,timeo=600,retrans=2,sec=sys,clientaddr=10.100.100.6,local_lock=none,addr=10.100.100.4

/mnt/pve/S3 from pfv-tsys5-nfs-stor:/mnt/pfv-tsys5/S3
 Flags:	rw,noatime,vers=4.2,rsize=1048576,wsize=1048576,namlen=255,hard,fatal_neterrors=none,proto=tcp,nconnect=4,timeo=600,retrans=2,sec=sys,clientaddr=10.100.100.6,local_lock=none,addr=10.100.100.5

/mnt/pve/D3 from pfv-tsys4-nfs-stor:/mnt/tsys4/D3
 Flags:	rw,noatime,vers=4.2,rsize=1048576,wsize=1048576,namlen=255,hard,fatal_neterrors=none,proto=tcp,nconnect=4,timeo=600,retrans=2,sec=sys,clientaddr=10.100.100.6,local_lock=none,addr=10.100.100.4


--- nfsstat -c (client stats)
    $ nfsstat -c
Client rpc stats:
calls      retrans    authrefrsh
1639888    4          1642849 

Client nfs v4:
null             read             write            commit           open             
2         0%     190663   11%     1080419  65%     74253     4%     2         0%     
open_conf        open_noat        open_dgrd        close            setattr          
0         0%     95        0%     0         0%     64        0%     0         0%     
fsinfo           renew            setclntid        confirm          lock             
28        0%     0         0%     0         0%     0         0%     0         0%     
lockt            locku            access           getattr          lookup           
0         0%     0         0%     171       0%     45516     2%     79        0%     
lookup_root      remove           rename           link             symlink          
7         0%     8         0%     0         0%     0         0%     0         0%     
create           pathconf         statfs           readlink         readdir          
2         0%     28        0%     146696    8%     0         0%     61        0%     
server_caps      delegreturn      getacl           setacl           fs_locations     
56        0%     26        0%     0         0%     0         0%     0         0%     
rel_lkowner      secinfo          fsid_present     exchange_id      create_session   
0         0%     0         0%     0         0%     4         0%     2         0%     
destroy_session  sequence         get_lease_time   reclaim_comp     layoutget        
0         0%     350       0%     0         0%     2         0%     0         0%     
getdevinfo       layoutcommit     layoutreturn     secinfo_no       test_stateid     
0         0%     0         0%     0         0%     7         0%     0         0%     
free_stateid     getdevicelist    bind_conn_to_ses destroy_clientid seek             
0         0%     0         0%     8         0%     0         0%     99983     6%     
allocate         deallocate       layoutstats      clone            
0         0%     0         0%     2500      0%     0         0%     


--- nfsstat -s (server stats)
    $ nfsstat -s
Error: No Server Stats (/proc/net/rpc/nfsd: No such file or directory). 
    [exit=2 / not installed or not permitted]

--- nfsstat -234 (version stats)
    $ nfsstat -234
Client rpc stats:
calls      retrans    authrefrsh
1639888    4          1642849 

Client nfs v2:
null             getattr          setattr          root             lookup           
0         0%     0         0%     0         0%     0         0%     0         0%     
readlink         read             wrcache          write            create           
0         0%     0         0%     0         0%     0         0%     0         0%     
remove           rename           link             symlink          mkdir            
0         0%     0         0%     0         0%     0         0%     0         0%     
rmdir            readdir          fsstat           
0         0%     0         0%     0         0%     

Client nfs v3:
null             getattr          setattr          lookup           access           
0         0%     0         0%     0         0%     0         0%     0         0%     
readlink         read             write            create           mkdir            
0         0%     0         0%     0         0%     0         0%     0         0%     
symlink          mknod            remove           rmdir            rename           
0         0%     0         0%     0         0%     0         0%     0         0%     
link             readdir          readdirplus      fsstat           fsinfo           
0         0%     0         0%     0         0%     0         0%     0         0%     
pathconf         commit           
0         0%     0         0%     

Client nfs v4:
null             read             write            commit           open             
2         0%     190663   11%     1080419  65%     74253     4%     2         0%     
open_conf        open_noat        open_dgrd        close            setattr          
0         0%     95        0%     0         0%     64        0%     0         0%     
fsinfo           renew            setclntid        confirm          lock             
28        0%     0         0%     0         0%     0         0%     0         0%     
lockt            locku            access           getattr          lookup           
0         0%     0         0%     171       0%     45516     2%     79        0%     
lookup_root      remove           rename           link             symlink          
7         0%     8         0%     0         0%     0         0%     0         0%     
create           pathconf         statfs           readlink         readdir          
2         0%     28        0%     146696    8%     0         0%     61        0%     
server_caps      delegreturn      getacl           setacl           fs_locations     
56        0%     26        0%     0         0%     0         0%     0         0%     
rel_lkowner      secinfo          fsid_present     exchange_id      create_session   
0         0%     0         0%     0         0%     4         0%     2         0%     
destroy_session  sequence         get_lease_time   reclaim_comp     layoutget        
0         0%     350       0%     0         0%     2         0%     0         0%     
getdevinfo       layoutcommit     layoutreturn     secinfo_no       test_stateid     
0         0%     0         0%     0         0%     7         0%     0         0%     
free_stateid     getdevicelist    bind_conn_to_ses destroy_clientid seek             
0         0%     0         0%     8         0%     0         0%     99983     6%     
allocate         deallocate       layoutstats      clone            
0         0%     0         0%     2500      0%     0         0%     


--- showmount -e (exports)
    $ showmount -e
clnt_create: RPC: Timed out
    [exit=1 / not installed or not permitted]

--- /proc/net/rpc/nfs
    $ cat /proc/net/rpc/nfs
net 0 0 0 0
rpc 1640780 4 1643743
proc4 71 2 190663 1081080 74310 2 0 95 0 64 0 28 0 0 0 0 0 0 171 45557 79 7 8 0 0 0 2 28 146829 0 61 56 26 0 0 0 0 0 0 4 2 0 350 0 2 0 0 0 0 7 0 0 0 8 0 99983 0 0 2500 0 0 0 0 0 0 0 0 0 0 0 0 0

--- /proc/net/rpc/nfsd
    $ cat /proc/net/rpc/nfsd
cat: /proc/net/rpc/nfsd: No such file or directory
    [exit=1 / not installed or not permitted]

--- exports
    [missing: /etc/exports]
    [missing: /etc/exports.d/*.exports]

--- nfs.conf
    --- /etc/nfs.conf ---
#
# This is a general configuration for the
# NFS daemons and tools
#
[general]
pipefs-directory=/run/rpc_pipefs
#
[nfsrahead]
# nfs=15000
# nfs4=16000
#
[exports]
# rootdir=/export
#
[exportfs]
# debug=0
#
[gssd]
# verbosity=0
# rpc-verbosity=0
# use-memcache=0
# use-machine-creds=1
# use-gss-proxy=0
# avoid-dns=1
# limit-to-legacy-enctypes=0
# allowed-enctypes=aes256-cts-hmac-sha384-192,aes128-cts-hmac-sha256-128,camellia256-cts-cmac,camellia128-cts-cmac,aes256-cts-hmac-sha1-96,aes128-cts-hmac-sha1-96
# context-timeout=0
# rpc-timeout=5
# keytab-file=/etc/krb5.keytab
# cred-cache-directory=
# preferred-realm=
# set-home=1
# upcall-timeout=30
# cancel-timed-out-upcalls=0
#
[lockd]
# port=0
# udp-port=0
#
[exportd]
# debug="all|auth|call|general|parse"
# manage-gids=n
# state-directory-path=/var/lib/nfs
# threads=1
# cache-use-ipaddr=n
# ttl=1800
[mountd]
# debug="all|auth|call|general|parse"
manage-gids=y
# descriptors=0
# port=0
# threads=1
# reverse-lookup=n
# state-directory-path=/var/lib/nfs
# ha-callout=
# cache-use-ipaddr=n
# ttl=1800
#
[nfsdcld]
# debug=0
# storagedir=/var/lib/nfs/nfsdcld
#
[nfsd]
# debug=0
# threads=16
# host=
# port=0
# grace-time=90
# lease-time=90
# udp=n
# tcp=y
# vers3=y
# vers4=y
# vers4.0=y
# vers4.1=y
# vers4.2=y
# rdma=n
# rdma-port=20049

[statd]
# debug=0
# port=0
# outgoing-port=0
# name=
# state-directory-path=/var/lib/nfs/statd
# ha-callout=
# no-notify=0
#
[sm-notify]
# debug=0
# force=0
# retry-time=900
# outgoing-port=
# outgoing-addr=
# lift-grace=y
#
[svcgssd]
# principal=
    [missing: /etc/nfs.conf.d/*.conf]

--- nfs defaults
    [missing: /etc/default/nfs-kernel-server]
    --- /etc/default/nfs-common ---
# If you do not set values for the NEED_ options, they will be attempted
# autodetected; this should be sufficient for most people. Valid alternatives
# for the NEED_ options are "yes" and "no".

# Do you want to start the statd daemon? It is not needed for NFSv4.
NEED_STATD=

# Do you want to start the idmapd daemon? It is only needed for NFSv4.
NEED_IDMAPD=

# Do you want to start the gssd daemon? It is required for Kerberos mounts.
NEED_GSSD=

--- idmapd.conf
    --- /etc/idmapd.conf ---
[General]

Verbosity = 0
# set your own domain here, if it differs from FQDN minus hostname
# Domain = localdomain

[Mapping]

Nobody-User = nobody
Nobody-Group = nogroup

--- pvesm status
    $ pvesm status
Name             Type     Status     Total (KiB)      Used (KiB) Available (KiB)        %
D2                nfs     active      2883130368       197245952      2539354112    6.84%
D3                nfs     active       491133952            2048       466110464    0.00%
D5                nfs     active      1921726464       219219968      1604814848   11.41%
S2                nfs     active       960304128        26530816       884918272    2.76%
S3                nfs     active       960304128        13431808       898018304    1.40%
S4                nfs     active       479597568         2460672       452701184    0.51%
T5-SSD            nfs     active       245023744       137123840        95380480   55.96%
local             dir     active        98497780        11770696        81677536   11.95%
local-lvm     lvmthin     active      1793044480               0      1793044480    0.00%

--- pvesm list per storage
    $ for s in $(pvesm status 2>/dev/null | awk 'NR>1 && $3=="active"{print $1}'); do
    echo "--- storage: $s ---"
    pvesm list "$s" 2>/dev/null | head -n 30
    echo "--- pvesm config $s ---"
    pvesm config "$s" 2>/dev/null
done
--- storage: D2 ---
Volid                          Format  Type              Size VMID
D2:100/vm-100-disk-0.raw       raw     images     34359738368 100
D2:100/vm-100-disk-1.raw       raw     images          540672 100
D2:101/vm-101-disk-0.qcow2     qcow2   images     34359738368 101
D2:104/vm-104-disk-0.qcow2     qcow2   images     53687091200 104
D2:105/vm-105-disk-0.qcow2     qcow2   images     34359738368 105
D2:108/vm-108-disk-0.qcow2     qcow2   images     34359738368 108
D2:109/vm-109-disk-0.qcow2     qcow2   images     26843545600 109
D2:114/vm-114-disk-0.qcow2     qcow2   images     34359738368 114
D2:117/vm-117-disk-0.qcow2     qcow2   images     34359738368 117
D2:3000/base-3000-disk-0.qcow2 qcow2   images     34359738368 3000
D2:500/vm-500-disk-0.qcow2     qcow2   images          540672 500
D2:509/vm-509-disk-0.qcow2     qcow2   images     34359738368 509
D2:600/vm-600-disk-1.qcow2     qcow2   images     34359738368 600
D2:601/vm-601-disk-0.qcow2     qcow2   images     34359738368 601
D2:702/vm-702-disk-0.qcow2     qcow2   images    107374182400 702
D2:703/vm-703-disk-0.qcow2     qcow2   images     34359738368 703
D2:704/vm-704-disk-0.qcow2     qcow2   images     34359738368 704
D2:705/vm-705-disk-0.qcow2     qcow2   images     34359738368 705
D2:901/vm-901-disk-0.qcow2     qcow2   images    141733920768 901
D2:904/vm-904-disk-0.qcow2     qcow2   images     34359738368 904
--- pvesm config D2 ---
--- storage: D3 ---
Volid Format  Type      Size VMID
--- pvesm config D3 ---
--- storage: D5 ---
Volid                      Format  Type              Size VMID
D5:106/vm-106-disk-0.qcow2 qcow2   images     34359738368 106
D5:313/vm-313-disk-0.qcow2 qcow2   images     34359738368 313
D5:530/vm-101-disk-0.qcow2 qcow2   images     34359738368 530
D5:531/vm-103-disk-0.qcow2 qcow2   images     34359738368 531
D5:532/vm-102-disk-0.qcow2 qcow2   images     34359738368 532
D5:533/vm-103-disk-0.qcow2 qcow2   images     34359738368 533
D5:534/vm-104-disk-0.qcow2 qcow2   images     34359738368 534
D5:535/vm-105-disk-0.qcow2 qcow2   images     34359738368 535
D5:536/vm-106-disk-0.qcow2 qcow2   images     34359738368 536
D5:537/vm-800-disk-0.qcow2 qcow2   images     34359738368 537
D5:538/vm-812-disk-0.qcow2 qcow2   images          540672 538
D5:538/vm-812-disk-2.raw   raw     images    429496729600 538
D5:541/vm-109-disk-0.qcow2 qcow2   images     34359738368 541
D5:903/vm-903-disk-0.qcow2 qcow2   images     34359738368 903
--- pvesm config D5 ---
--- storage: S2 ---
Volid                      Format  Type             Size VMID
S2:103/vm-103-disk-0.qcow2 qcow2   images    34359738368 103
S2:706/vm-706-disk-0.qcow2 qcow2   images    34359738368 706
S2:902/vm-902-disk-0.qcow2 qcow2   images    53687091200 902
S2:905/vm-905-disk-0.qcow2 qcow2   images    34359738368 905
--- pvesm config S2 ---
--- storage: S3 ---
Volid                      Format  Type             Size VMID
S3:102/vm-102-disk-0.qcow2 qcow2   images    34359738368 102
S3:701/vm-701-disk-0.qcow2 qcow2   images    34359738368 701
S3:905/vm-905-disk-0.qcow2 qcow2   images    34359738368 905
S3:906/vm-906-disk-0.qcow2 qcow2   images    34359738368 906
--- pvesm config S3 ---
--- storage: S4 ---
Volid                      Format  Type             Size VMID
S4:100/vm-100-disk-0.qcow2 qcow2   images    34359738368 100
--- pvesm config S4 ---
--- storage: T5-SSD ---
Volid                            Format  Type              Size VMID
T5-SSD:5111/vm-5111-disk-0.qcow2 qcow2   images    309237645312 5111
--- pvesm config T5-SSD ---
--- storage: local ---
Volid                Format  Type           Size VMID
local:iso/debian.iso iso     iso       791674880
--- pvesm config local ---
--- storage: local-lvm ---
Volid Format  Type      Size VMID
--- pvesm config local-lvm ---
    [exit=255]

###############################################################################
# 17. STORAGE: LVM
###############################################################################

--- pvs
    $ pvs -v
  PV         VG  Fmt  Attr PSize  PFree  DevSize PV UUID                               
  /dev/sda3  pve lvm2 a--  <1.82t 16.24g  <1.82t aBoPok-Y20Z-3hHs-Buu6-ybpQ-KwCM-fbOoLy

--- vgs
    $ vgs -v
  VG  Attr   Ext   #PV #LV #SN VSize  VFree  VG UUID                                VProfile
  pve wz--n- 4.00m   1   3   0 <1.82t 16.24g VLhH9x-Y3yB-zA1O-LhK8-fOtL-oW3X-8xjxcq         

--- lvs
    $ lvs -o +lv_layout,role,pool_lv,data_percent,metadata_percent --units b
  LV   VG  Attr       LSize          Pool Origin Data%  Meta%  Move Log Cpy%Sync Convert Layout     Role       Pool Data%  Meta% 
  data pve twi-a-tz-- 1836077547520B             0.00   0.15                             thin,pool  private         0.00   0.15  
  root pve -wi-ao----  103079215104B                                                     linear     public                       
  swap pve -wi-ao----    8589934592B                                                     linear     public                       

--- pvdisplay
    $ pvdisplay
  --- Physical volume ---
  PV Name               /dev/sda3
  VG Name               pve
  PV Size               <1.82 TiB / not usable 3.98 MiB
  Allocatable           yes 
  PE Size               4.00 MiB
  Total PE              476667
  Free PE               4158
  Allocated PE          472509
  PV UUID               aBoPok-Y20Z-3hHs-Buu6-ybpQ-KwCM-fbOoLy
   

--- vgdisplay
    $ vgdisplay
  --- Volume group ---
  VG Name               pve
  System ID             
  Format                lvm2
  Metadata Areas        1
  Metadata Sequence No  7
  VG Access             read/write
  VG Status             resizable
  MAX LV                0
  Cur LV                3
  Open LV               2
  Max PV                0
  Cur PV                1
  Act PV                1
  VG Size               <1.82 TiB
  PE Size               4.00 MiB
  Total PE              476667
  Alloc PE / Size       472509 / 1.80 TiB
  Free  PE / Size       4158 / 16.24 GiB
  VG UUID               VLhH9x-Y3yB-zA1O-LhK8-fOtL-oW3X-8xjxcq
   

--- lvdisplay
    $ lvdisplay
  --- Logical volume ---
  LV Name                data
  VG Name                pve
  LV UUID                A2o3em-JGs9-FRfH-vqsz-yVy7-XucO-CeWKPW
  LV Write Access        read/write
  LV Creation host, time proxmox, 2026-04-04 12:08:10 -0500
  LV Pool metadata       data_tmeta
  LV Pool data           data_tdata
  LV Status              available
  # open                 0
  LV Size                <1.67 TiB
  Allocated pool data    0.00%
  Allocated metadata     0.15%
  Current LE             437755
  Segments               1
  Allocation             inherit
  Read ahead sectors     auto
  - currently set to     8192
  Block device           252:4
   
  --- Logical volume ---
  LV Path                /dev/pve/swap
  LV Name                swap
  VG Name                pve
  LV UUID                A1dQoM-c3cN-o10U-aTrf-E6xE-9qlY-qvi56O
  LV Write Access        read/write
  LV Creation host, time proxmox, 2026-04-04 12:08:09 -0500
  LV Status              available
  # open                 1
  LV Size                8.00 GiB
  Current LE             2048
  Segments               1
  Allocation             inherit
  Read ahead sectors     auto
  - currently set to     8192
  Block device           252:0
   
  --- Logical volume ---
  LV Path                /dev/pve/root
  LV Name                root
  VG Name                pve
  LV UUID                BcScYG-321V-uPMn-mVoW-g7hS-ln1B-0uOD3j
  LV Write Access        read/write
  LV Creation host, time proxmox, 2026-04-04 12:08:10 -0500
  LV Status              available
  # open                 1
  LV Size                96.00 GiB
  Current LE             24576
  Segments               1
  Allocation             inherit
  Read ahead sectors     auto
  - currently set to     8192
  Block device           252:1
   

--- lvm/lvm.conf (filters only)
    --- /etc/lvm/lvm.conf ---
# This is an example configuration file for the LVM2 system.
# It contains the default settings that would be used if there was no
# /etc/lvm/lvm.conf file.
#
# Refer to 'man lvm.conf' for further information including the file layout.
#
# Refer to 'man lvm.conf' for information about how settings configured in
# this file are combined with built-in values and command line options to
# arrive at the final values used by LVM.
#
# Refer to 'man lvmconfig' for information about displaying the built-in
# and configured values used by LVM.
#
# If a default value is set in this file (not commented out), then a
# new version of LVM using this file will continue using that value,
# even if the new version of LVM changes the built-in default value.
#
# To put this file in a different directory and override /etc/lvm set
# the environment variable LVM_SYSTEM_DIR before running the tools.
#
# N.B. Take care that each setting only appears once if uncommenting
# example settings in this file.


# Configuration section config.
# How LVM configuration settings are handled.
config {

	# Configuration option config/checks.
	# If enabled, any LVM configuration mismatch is reported.
	# This implies checking that the configuration key is understood by
	# LVM and that the value of the key is the proper type. If disabled,
	# any configuration mismatch is ignored and the default value is used
	# without any warning (a message about the configuration key not being
	# found is issued in verbose mode only).
	# This configuration option has an automatic default value.
	# checks = 1

	# Configuration option config/validate_metadata.
	# Allows to select the level of validation after metadata transformation.
	# Validation takes extra CPU time to verify internal consistency.
	# Accepted values:
	#   full
	#     Do a full metadata validation before disk write.
	#   none
	#     Skip any checks (unrecommended, slightly faster).
	#
	# This configuration option is advanced.
	# This configuration option has an automatic default value.
	# validate_metadata = "full"

	# Configuration option config/abort_on_errors.
	# Abort the LVM process if a configuration mismatch is found.
	# This configuration option has an automatic default value.
	# abort_on_errors = 0

	# Configuration option config/profile_dir.
	# Directory where LVM looks for configuration profiles.
	# This configuration option has an automatic default value.
	# profile_dir = "/etc/lvm/profile"
}

# Configuration section devices.
# How LVM uses block devices.
devices {

	# Configuration option devices/dir.
	# Directory in which to create volume group device nodes.
	# Commands also accept this as a prefix on volume group names.
	# This configuration option is advanced.
	# This configuration option has an automatic default value.
	# dir = "/dev"

	# Configuration option devices/scan.
	# Directories containing device nodes to use with LVM.
	# This configuration option is advanced.
	# This configuration option has an automatic default value.
	# scan = [ "/dev" ]

	# Configuration option devices/obtain_device_list_from_udev.
	# Obtain the list of available devices from udev.
	# This avoids opening or using any inapplicable non-block devices or
	# subdirectories found in the udev directory. Any device node or
	# symlink not managed by udev in the udev directory is ignored. This
	# setting applies only to the udev-managed device directory; other
	# directories will be scanned fully. LVM needs to be compiled with
	# udev support for this setting to apply.
	# This configuration option has an automatic default value.
	# obtain_device_list_from_udev = 0

	# Configuration option devices/external_device_info_source.
	# Enable device information from udev.
	# If set to "udev", lvm will supplement its own native device information
	# with information from libudev. This can potentially improve the detection
	# of MD component devices and multipath component devices.
	# This configuration option has an automatic default value.
	# external_device_info_source = "none"

	# Configuration option devices/hints.
	# Use a local file to remember which devices have PVs on them.
	# Some commands will use this as an optimization to reduce device
	# scanning, and will only scan the listed PVs. Removing the hint file
	# will cause lvm to generate a new one. Disable hints if PVs will
	# be copied onto devices using non-lvm commands, like dd.
	#
	# Accepted values:
	#   all
	#     Use all hints.
	#   none
	#     Use no hints.
	#
	# This configuration option has an automatic default value.
	# hints = "all"

	# Configuration option devices/preferred_names.
	# Select which path name to display for a block device.
	# If multiple path names exist for a block device, and LVM needs to
	# display a name for the device, the path names are matched against
	# each item in this list of regular expressions. The first match is
	# used. Try to avoid using undescriptive /dev/dm-N names, if present.
	# If no preferred name matches, or if preferred_names are not defined,
	# the following built-in preferences are applied in order until one
	# produces a preferred name:
	# Prefer names with path prefixes in the order of:
	# /dev/mapper, /dev/disk, /dev/dm-*, /dev/block.
	# Prefer the name with the least number of slashes.
	# Prefer a name that is a symlink.
	# Prefer the path with least value in lexicographical order.
	#
	# Example
	# preferred_names = [ "^/dev/mpath/", "^/dev/mapper/mpath", "^/dev/[hs]d" ]
	#
	# This configuration option does not have a default value defined.

	# Configuration option devices/use_devicesfile.
	# Enable or disable the use of a devices file.
	# When enabled, lvm will only use devices that
	# are listed in the devices file. A devices file will
	# be used, regardless of this setting, when the --devicesfile
	# option is set to a specific file name.
	# This configuration option has an automatic default value.
	# use_devicesfile = 0

	# Configuration option devices/devicesfile.
	# The name of the system devices file, listing devices that LVM should use.
	# This should not be used to select a non-system devices file.
	# The --devicesfile option is intended for alternative devices files.
	# This configuration option has an automatic default value.
	# devicesfile = "system.devices"

	# Configuration option devices/devicesfile_backup_limit.
	# The max number of backup files to keep in /etc/lvm/devices/backup.
	# LVM creates a backup of the devices file each time a new
	# version is created, or each time a modification is detected.
	# When the max number of backups is reached, the oldest are
	# removed to remain at the limit. Set to 0 to disable backups.
	# Only the system devices file is backed up.
	# This configuration option has an automatic default value.
	# devicesfile_backup_limit = 50

	# Configuration option devices/search_for_devnames.
	# Look outside of the devices file for missing devname entries.
	# A devname entry is used for a device that does not have a stable
	# device id, e.g. wwid, so the unstable device name is used as
	# the device id. After reboot, or if the device is reattached,
	# the device name may change, in which case lvm will not find
	# the expected PV on the device listed in the devices file.
	# This setting controls whether lvm will search other devices,
	# outside the devices file, to look for the missing PV on a
	# renamed device. If "none", lvm will not look at other devices,
	# and the PV may appear to be missing. If "auto", lvm will look
	# at other devices, but only those that are likely to have the PV.
	# If "all", lvm will look at all devices on the system.
	# This configuration option has an automatic default value.
	# search_for_devnames = "all"

	# Configuration option devices/device_ids_refresh.
	# Find PVs on new devices and update the device IDs in the devices file.
	# If PVs are restored or moved to a new system with new devices, but
	# an old system.devices remains with old device IDs, then search for
	# the PVIDs on new devices and update the device IDs in system.devices.
	# The original device IDs must also not be found on the new system.
	# See device_ids_refresh_check for conditions that trigger the refresh.
	# This configuration option has an automatic default value.
	# device_ids_refresh = 1

	# Configuration option devices/device_ids_refresh_checks.
	# Conditions that trigger device_ids_refresh to locate PVIDs on new devices.
	# product_uuid: refresh if /sys/devices/virtual/dmi/id/product_uuid does not
	# match the value saved in system.devices.
	# hostname: refresh if hostname does not match the value saved in system.devices.
	# (hostname is used if product_uuid is not available.)
	# Remove values from this list to prevent lvm from using them.
	# This configuration option has an automatic default value.
	# device_ids_refresh_checks = [ "product_uuid", "hostname" ]

	# Configuration option devices/filter.
	# Limit the block devices that are used by LVM commands.
	# This is a list of regular expressions used to accept or reject block
	# device path names. Each regex is delimited by a vertical bar '|'
	# (or any character) and is preceded by 'a' to accept the path, or
	# by 'r' to reject the path. The first regex in the list to match the
	# path is used, producing the 'a' or 'r' result for the device.
	# When multiple path names exist for a block device, if any path name
	# matches an 'a' pattern before an 'r' pattern, then the device is
	# accepted. If all the path names match an 'r' pattern first, then the
	# device is rejected. Unmatching path names do not affect the accept
	# or reject decision. If no path names for a device match a pattern,
	# then the device is accepted. Be careful mixing 'a' and 'r' patterns,
	# as the combination might produce unexpected results (test changes.)
	# Run vgscan after changing the filter to regenerate the cache.
	#
	# Example
	# Accept every block device:
	# filter = [ "a|.*|" ]
	# Reject the cdrom drive:
	# filter = [ "r|/dev/cdrom|" ]
	# Work with just loopback devices, e.g. for testing:
	# filter = [ "a|loop|", "r|.*|" ]
	# Accept all loop devices and ide drives except hdc:
	# filter = [ "a|loop|", "r|/dev/hdc|", "a|/dev/ide|", "r|.*|" ]
	# Use anchors to be very specific:
	# filter = [ "a|^/dev/hda8$|", "r|.*|" ]
	#
	# This configuration option has an automatic default value.
	# filter = [ "a|.*|" ]

	# Configuration option devices/global_filter.
	# Limit the block devices that are used by LVM system components.
	# Because devices/filter may be overridden from the command line, it is
	# not suitable for system-wide device filtering, e.g. udev.
	# Use global_filter to hide devices from these LVM system components.
	# The syntax is the same as devices/filter. Devices rejected by
	# global_filter are not opened by LVM.
	# This configuration option has an automatic default value.
	# global_filter = [ "a|.*|" ]

	# Configuration option devices/types.
	# List of additional acceptable block device types.
	# These are of device type names from /proc/devices, followed by the
	# maximum number of partitions.
	#
	# Example
	# types = [ "fd", 16 ]
	#
	# This configuration option is advanced.
	# This configuration option does not have a default value defined.

	# Configuration option devices/sysfs_scan.
	# Restrict device scanning to block devices appearing in sysfs.
	# This is a quick way of filtering out block devices that are not
	# present on the system. sysfs must be part of the kernel and mounted.)
	# This configuration option has an automatic default value.
	# sysfs_scan = 1

	# Configuration option devices/scan_lvs.
	# Allow LVM LVs to be used as PVs. When enabled, LVM commands will
	# scan active LVs to look for other PVs. Caution is required to
	# avoid using PVs that belong to guest images stored on LVs.
	# When enabled, the LVs scanned should be restricted using the
	# devices file or the filter. This option does not enable autoactivation
	# of layered VGs, which requires editing LVM udev rules (see LVM_PVSCAN_ON_LVS.)
	# This configuration option has an automatic default value.
	# scan_lvs = 0

	# Configuration option devices/multipath_component_detection.
	# Ignore devices that are components of DM multipath devices.
	# This configuration option has an automatic default value.
	# multipath_component_detection = 1

	# Configuration option devices/multipath_wwids_file.
	# The path to the multipath wwids file used for multipath component detection.
	# Set this to an empty string to disable the use of the multipath wwids file.
	# This configuration option has an automatic default value.
	# multipath_wwids_file = "/etc/multipath/wwids"

	# Configuration option devices/md_component_detection.
	# Enable detection and exclusion of MD component devices.
	# An MD component device is a block device that MD uses as part
	# of a software RAID virtual device. When an LVM PV is created
	# on an MD device, LVM must only use the top level MD device as
	# the PV, and should ignore the underlying component devices.
	# In cases where the MD superblock is located at the end of the
	# component devices, it is more difficult for LVM to consistently
	# identify an MD component, see the md_component_checks setting.
	# This configuration option has an automatic default value.
	# md_component_detection = 1

	# Configuration option devices/md_component_checks.
	# The checks LVM should use to detect MD component devices.
	# MD component devices are block devices used by MD software RAID.
	#
	# Accepted values:
	#   auto
	#     LVM will skip scanning the end of devices when it has other
	#     indications that the device is not an MD component.
	#   start
	#     LVM will only scan the start of devices for MD superblocks.
	#     This does not incur extra I/O by LVM.
	#   full

--- lvm.conf active filter
    $ grep -E '^\s*(filter|global_filter|use_devicesfile|obtain_device_list_from_udev)' /etc/lvm/lvm.conf 2>/dev/null
     global_filter=["r|/dev/zd.*|","r|/dev/rbd.*|"]

###############################################################################
# 18. STORAGE: MULTIPATH
###############################################################################

--- multipath -ll
    $ multipath -ll
/root/check.sh: line 45: multipath: command not found
    [exit=127 / not installed or not permitted]

--- multipath -v3 -ll (verbose, capped)
    $ multipath -v3 -ll
/root/check.sh: line 45: multipath: command not found
    [exit=127 / not installed or not permitted]

--- multipath.conf
    [missing: /etc/multipath.conf]

--- systemctl is-active multipathd
    $ systemctl is-active multipathd
inactive
    [exit=4 / not installed or not permitted]

###############################################################################
# 19. STORAGE: ZFS
###############################################################################

--- zfs version (userland)
    $ zfs version
zfs-2.4.3-pve1
zfs-kmod-2.4.3-pve1

--- zpool version
    $ zpool version
zfs-2.4.3-pve1
zfs-kmod-2.4.3-pve1

--- zpool list -v
    $ zpool list -v
no pools available

--- zpool status -v
    $ zpool status -v
no pools available

--- zpool key properties
    $ zpool get name,size,alloc,free,expandsize,fragmentation,capacity,health,ashift,autotrim,autoreplace,cachefile,comment,listsnapshots,multihost,version,bootfs,delegation,failmode,freeing,leaked,readonly

--- zfs per-dataset key properties
    $ zfs get -r -o name,property,value,source \
    compression,atime,recordsize,volblocksize,sync,primarycache,secondarycache,checksum,xattr,acltype,aclinherit,copies,logbias,refreservation,reservation,quota,used,avail,refer,mountpoint,mounted,canmount,relative_path,snapdir,version,primarycache,redundant_metadata,encryption 2>/dev/null
    [exit=2]

--- ARC stats
    $ cat /proc/spl/kstat/zfs/arcstats
22 1 0x01 148 40256 23315364464 215648583830468
name                            type data
hits                            4    0
iohits                          4    0
misses                          4    0
demand_data_hits                4    0
demand_data_iohits              4    0
demand_data_misses              4    0
demand_metadata_hits            4    0
demand_metadata_iohits          4    0
demand_metadata_misses          4    0
prefetch_data_hits              4    0
prefetch_data_iohits            4    0
prefetch_data_misses            4    0
prefetch_metadata_hits          4    0
prefetch_metadata_iohits        4    0
prefetch_metadata_misses        4    0
mru_hits                        4    0
mru_ghost_hits                  4    0
mfu_hits                        4    0
mfu_ghost_hits                  4    0
uncached_hits                   4    0
deleted                         4    0
mutex_miss                      4    0
access_skip                     4    0
evict_skip                      4    0
evict_not_enough                4    0
evict_l2_cached                 4    0
evict_l2_eligible               4    0
evict_l2_eligible_mfu           4    0
evict_l2_eligible_mru           4    0
evict_l2_ineligible             4    0
evict_l2_skip                   4    0
hash_elements                   4    0
hash_elements_max               4    0
hash_collisions                 4    0
hash_chains                     4    0
hash_chain_max                  4    0
meta                            4    1073741824
pd                              4    2147483648
pm                              4    2147483648
c                               4    4223713920
c_min                           4    4223713920
c_max                           4    13515096064
size                            4    3840
compressed_size                 4    0
uncompressed_size               4    0
overhead_size                   4    0
hdr_size                        4    3840
data_size                       4    0
metadata_size                   4    0
dbuf_size                       4    0
dnode_size                      4    0
bonus_size                      4    0
anon_size                       4    0
anon_data                       4    0
anon_metadata                   4    0
anon_evictable_data             4    0
anon_evictable_metadata         4    0
mru_size                        4    0
mru_data                        4    0
mru_metadata                    4    0
mru_evictable_data              4    0
mru_evictable_metadata          4    0
mru_ghost_size                  4    0
mru_ghost_data                  4    0
mru_ghost_metadata              4    0
mru_ghost_evictable_data        4    0
mru_ghost_evictable_metadata    4    0
mfu_size                        4    0
mfu_data                        4    0
mfu_metadata                    4    0
mfu_evictable_data              4    0
mfu_evictable_metadata          4    0
mfu_ghost_size                  4    0
mfu_ghost_data                  4    0
mfu_ghost_metadata              4    0
mfu_ghost_evictable_data        4    0
mfu_ghost_evictable_metadata    4    0
uncached_size                   4    0
uncached_data                   4    0
uncached_metadata               4    0
uncached_evictable_data         4    0
uncached_evictable_metadata     4    0
l2_ndev                         4    0
l2_hits                         4    0
l2_misses                       4    0
l2_prefetch_asize               4    0
l2_mru_asize                    4    0
l2_mfu_asize                    4    0
l2_bufc_data_asize              4    0
l2_bufc_metadata_asize          4    0
l2_feeds                        4    0
l2_rw_clash                     4    0
l2_read_bytes                   4    0
l2_write_bytes                  4    0
l2_writes_sent                  4    0
l2_writes_done                  4    0
l2_writes_error                 4    0
l2_writes_lock_retry            4    0
l2_evict_lock_retry             4    0
l2_evict_reading                4    0
l2_evict_l1cached               4    0
l2_free_on_write                4    0
l2_abort_lowmem                 4    0
l2_cksum_bad                    4    0
l2_io_error                     4    0
l2_size                         4    0
l2_asize                        4    0
l2_hdr_size                     4    0
l2_log_blk_writes               4    0
l2_log_blk_avg_asize            4    0
l2_log_blk_asize                4    0
l2_log_blk_count                4    0
l2_data_to_meta_ratio           4    0
l2_rebuild_success              4    0
l2_rebuild_unsupported          4    0
l2_rebuild_io_errors            4    0
l2_rebuild_dh_errors            4    0
l2_rebuild_cksum_lb_errors      4    0
l2_rebuild_lowmem               4    0
l2_rebuild_size                 4    0
l2_rebuild_asize                4    0
l2_rebuild_bufs                 4    0
l2_rebuild_bufs_precached       4    0
l2_rebuild_log_blks             4    0
memory_throttle_count           4    0
memory_direct_count             4    0
memory_indirect_count           4    0
memory_all_bytes                4    135158845440
memory_free_bytes               4    126865047552
memory_available_bytes          3    122288406912
arc_no_grow                     4    0
arc_tempreserve                 4    0
arc_loaned_bytes                4    0
arc_prune                       4    0
arc_meta_used                   4    3840
arc_dnode_limit                 4    1351509606
async_upgrade_sync              4    0
predictive_prefetch             4    0
demand_hit_predictive_prefetch  4    0
demand_iohit_predictive_prefetch 4    0
prescient_prefetch              4    0
demand_hit_prescient_prefetch   4    0
demand_iohit_prescient_prefetch 4    0
arc_need_free                   4    0
arc_sys_free                    4    4576640640
arc_raw_size                    4    0
cached_only_in_progress         4    0
abd_chunk_waste_size            4    0

--- dmu_tx
    $ cat /proc/spl/kstat/zfs/dmu_tx
18 1 0x01 13 3536 23288375463 215648585390183
name                            type data
dmu_tx_assigned                 4    0
dmu_tx_delay                    4    0
dmu_tx_error                    4    0
dmu_tx_suspended                4    0
dmu_tx_group                    4    0
dmu_tx_memory_reserve           4    0
dmu_tx_memory_reclaim           4    0
dmu_tx_dirty_throttle           4    0
dmu_tx_dirty_delay              4    0
dmu_tx_dirty_over_max           4    0
dmu_tx_dirty_frees_delay        4    0
dmu_tx_wrlog_delay              4    0
dmu_tx_quota                    4    0

--- zfetchstats
    $ cat /proc/spl/kstat/zfs/zfetchstats
17 1 0x01 8 2176 23288374118 215648586814153
name                            type data
hits                            4    0
future                          4    0
stride                          4    0
past                            4    0
misses                          4    0
max_streams                     4    0
io_issued                       4    0
io_active                       4    0

--- vdev_cache_stats
    $ cat /proc/spl/kstat/zfs/vdev_cache_stats
cat: /proc/spl/kstat/zfs/vdev_cache_stats: No such file or directory
    [exit=1 / not installed or not permitted]

--- abdstats
    $ cat /proc/spl/kstat/zfs/abdstats
15 1 0x01 20 5440 23288199024 215648589910979
name                            type data
struct_size                     4    96
linear_cnt                      4    0
linear_data_size                4    0
scatter_cnt                     4    1
scatter_data_size               4    4096
scatter_chunk_waste             4    0
scatter_order_0                 4    0
scatter_order_1                 4    0
scatter_order_2                 4    0
scatter_order_3                 4    0
scatter_order_4                 4    0
scatter_order_5                 4    0
scatter_order_6                 4    0
scatter_order_7                 4    0
scatter_order_8                 4    0
scatter_order_9                 4    0
scatter_page_multi_chunk        4    1
scatter_page_multi_zone         4    0
scatter_page_alloc_retry        4    0
scatter_sg_table_retry          4    0

--- ZFS module parameters (perf-relevant)
    $ for f in /sys/module/zfs/parameters/*; do
    [ -r "$f" ] || continue
    name="$(basename "$f")"
    case "$name" in
        zfs_arc_*|zfs_abd_*|zfs_dbuf_*|zfs_txg_*|zfs_vdev_*|zfs_sync_*|zfs_dirty_*|zfs_*io_*|zvol_*|l2arc_*|zfs_prefetch_*|zfs_*max_active|zfs_*_taskq*) ;;
        *) continue ;;
    esac
    printf '  %-50s = %s\n' "$name" "$(cat "$f")"
done
  l2arc_exclude_special                              = 0
  l2arc_feed_again                                   = 1
  l2arc_feed_min_ms                                  = 200
  l2arc_feed_secs                                    = 1
  l2arc_headroom                                     = 8
  l2arc_headroom_boost                               = 200
  l2arc_meta_percent                                 = 33
  l2arc_mfuonly                                      = 0
  l2arc_noprefetch                                   = 1
  l2arc_norw                                         = 0
  l2arc_rebuild_blocks_min_l2size                    = 1073741824
  l2arc_rebuild_enabled                              = 1
  l2arc_trim_ahead                                   = 0
  l2arc_write_boost                                  = 33554432
  l2arc_write_max                                    = 33554432
  zfs_abd_scatter_enabled                            = 1
  zfs_abd_scatter_max_order                          = 9
  zfs_abd_scatter_min_size                           = 1536
  zfs_arc_average_blocksize                          = 8192
  zfs_arc_dnode_limit                                = 0
  zfs_arc_dnode_limit_percent                        = 10
  zfs_arc_dnode_reduce_percent                       = 10
  zfs_arc_evict_batches_limit                        = 5
  zfs_arc_evict_batch_limit                          = 10
  zfs_arc_eviction_pct                               = 200
  zfs_arc_evict_threads                              = 4
  zfs_arc_grow_retry                                 = 0
  zfs_arc_lotsfree_percent                           = 10
  zfs_arc_max                                        = 13515096064
  zfs_arc_meta_balance                               = 500
  zfs_arc_min                                        = 0
  zfs_arc_min_prefetch_ms                            = 0
  zfs_arc_min_prescient_prefetch_ms                  = 0
  zfs_arc_pc_percent                                 = 0
  zfs_arc_prune_task_threads                         = 1
  zfs_arc_shrinker_limit                             = 0
  zfs_arc_shrinker_seeks                             = 2
  zfs_arc_shrink_shift                               = 0
  zfs_arc_sys_free                                   = 0
  zfs_async_free_zio_wait_interval                   = 2000
  zfs_dbuf_state_index                               = 0
  zfs_dio_enabled                                    = 1
  zfs_dio_strict                                     = 0
  zfs_dio_write_verify_events_per_second             = 20
  zfs_dirty_data_max                                 = 4294967296
  zfs_dirty_data_max_max                             = 4294967296
  zfs_dirty_data_max_max_percent                     = 25
  zfs_dirty_data_max_percent                         = 10
  zfs_dirty_data_sync_percent                        = 20
  zfs_prefetch_disable                               = 0
  zfs_slow_io_events_per_second                      = 20
  zfs_sync_pass_deferred_free                        = 2
  zfs_sync_pass_dont_compress                        = 8
  zfs_sync_pass_rewrite                              = 2
  zfs_txg_history                                    = 100
  zfs_txg_timeout                                    = 5
  zfs_vdev_aggregation_limit                         = 1048576
  zfs_vdev_aggregation_limit_non_rotating            = 131072
  zfs_vdev_async_read_max_active                     = 3
  zfs_vdev_async_read_min_active                     = 1
  zfs_vdev_async_write_active_max_dirty_percent      = 60
  zfs_vdev_async_write_active_min_dirty_percent      = 30
  zfs_vdev_async_write_max_active                    = 10
  zfs_vdev_async_write_min_active                    = 2
  zfs_vdev_default_ms_count                          = 200
  zfs_vdev_default_ms_shift                          = 29
  zfs_vdev_direct_write_verify                       = 1
  zfs_vdev_disk_max_segs                             = 0
  zfs_vdev_failfast_mask                             = 1
  zfs_vdev_initializing_max_active                   = 1
  zfs_vdev_initializing_min_active                   = 1
  zfs_vdev_max_active                                = 1000
  zfs_vdev_max_auto_ashift                           = 14
  zfs_vdev_max_ms_shift                              = 34
  zfs_vdev_min_auto_ashift                           = 9
  zfs_vdev_min_ms_count                              = 16
  zfs_vdev_mirror_non_rotating_inc                   = 0
  zfs_vdev_mirror_non_rotating_seek_inc              = 1
  zfs_vdev_mirror_rotating_inc                       = 0
  zfs_vdev_mirror_rotating_seek_inc                  = 5
  zfs_vdev_mirror_rotating_seek_offset               = 1048576
  zfs_vdev_ms_count_limit                            = 131072
  zfs_vdev_nia_credit                                = 5
  zfs_vdev_nia_delay                                 = 5
  zfs_vdev_open_timeout_ms                           = 1000
  zfs_vdev_raidz_impl                                = cycle [fastest] original scalar sse2 ssse3 
  zfs_vdev_read_gap_limit                            = 32768
  zfs_vdev_rebuild_max_active                        = 3
  zfs_vdev_rebuild_min_active                        = 1
  zfs_vdev_removal_max_active                        = 2
  zfs_vdev_removal_min_active                        = 1
  zfs_vdev_scrub_max_active                          = 3
  zfs_vdev_scrub_min_active                          = 1
  zfs_vdev_sync_read_max_active                      = 10
  zfs_vdev_sync_read_min_active                      = 10
  zfs_vdev_sync_write_max_active                     = 10
  zfs_vdev_sync_write_min_active                     = 10
  zfs_vdev_trim_max_active                           = 2
  zfs_vdev_trim_min_active                           = 1
  zfs_vdev_write_gap_limit                           = 4096
  zfs_zil_clean_taskq_maxalloc                       = 1048576
  zfs_zil_clean_taskq_minalloc                       = 1024
  zfs_zil_clean_taskq_nthr_pct                       = 100
  zvol_blk_mq_blocks_per_thread                      = 8
  zvol_blk_mq_queue_depth                            = 128
  zvol_enforce_quotas                                = 1
  zvol_inhibit_dev                                   = 0
  zvol_major                                         = 230
  zvol_max_discard_blocks                            = 16384
  zvol_num_taskqs                                    = 0
  zvol_open_timeout_ms                               = 1000
  zvol_prefetch_bytes                                = 131072
  zvol_request_sync                                  = 0
  zvol_threads                                       = 0
  zvol_use_blk_mq                                    = 0
  zvol_volmode                                       = 1

--- zpool iostat snapshot
    $ zpool iostat 1 1
no pools available

--- arc_summary (if present)
    $ arc_summary

------------------------------------------------------------------------
ZFS Subsystem Report                            Wed Jul 29 05:13:37 2026
Linux 7.0.14-6-pve                                            2.4.3-pve1
Machine: pfv-tsys6 (x86_64)                                   2.4.3-pve1

ARC status:
        Total memory size:                                     125.9 GiB
        Min target size:                                3.1 %    3.9 GiB
        Max target size:                               10.0 %   12.6 GiB
        Target size (adaptive):                       < 0.1 %    3.9 GiB
        Current size:                                 < 0.1 %    3.8 KiB
        Free memory size:                                      118.2 GiB
        Available memory size:                                 113.9 GiB

ARC structural breakdown (current size):                         3.8 KiB
        Compressed size:                                0.0 %    0 Bytes
        Overhead size:                                  0.0 %    0 Bytes
        Bonus size:                                     0.0 %    0 Bytes
        Dnode size:                                     0.0 %    0 Bytes
        Dbuf size:                                      0.0 %    0 Bytes
        Header size:                                  100.0 %    3.8 KiB
        L2 header size:                                 0.0 %    0 Bytes
        ABD chunk waste size:                           0.0 %    0 Bytes

ARC types breakdown (compressed + overhead):                     0 Bytes
        Data size:                                        n/a    0 Bytes
        Metadata size:                                    n/a    0 Bytes

ARC states breakdown (compressed + overhead):                    0 Bytes
        Anonymous data size:                              n/a    0 Bytes
        Anonymous metadata size:                          n/a    0 Bytes
        MFU data target:                               37.5 %    0 Bytes
        MFU data size:                                    n/a    0 Bytes
        MFU evictable data size:                          n/a    0 Bytes
        MFU ghost data size:                                     0 Bytes
        MFU metadata target:                           12.5 %    0 Bytes
        MFU metadata size:                                n/a    0 Bytes
        MFU evictable metadata size:                      n/a    0 Bytes
        MFU ghost metadata size:                                 0 Bytes
        MRU data target:                               37.5 %    0 Bytes
        MRU data size:                                    n/a    0 Bytes
        MRU evictable data size:                          n/a    0 Bytes
        MRU ghost data size:                                     0 Bytes
        MRU metadata target:                           12.5 %    0 Bytes
        MRU metadata size:                                n/a    0 Bytes
        MRU evictable metadata size:                      n/a    0 Bytes
        MRU ghost metadata size:                                 0 Bytes
        Uncached data size:                               n/a    0 Bytes
        Uncached metadata size:                           n/a    0 Bytes

ARC hash breakdown:
        Elements:                                                      0
        Collisions:                                                    0
        Chain max:                                                     0
        Chains:                                                        0

ARC misc:
        Uncompressed size:                                n/a    0 Bytes
        Memory throttles:                                              0
        Memory direct reclaims:                                        0
        Memory indirect reclaims:                                      0
        Deleted:                                                       0
        Mutex misses:                                                  0
        Eviction skips:                                                0
        Eviction skips due to L2 writes:                               0
        L2 cached evictions:                                     0 Bytes
        L2 eligible evictions:                                   0 Bytes
        L2 eligible MFU evictions:                        n/a    0 Bytes
        L2 eligible MRU evictions:                        n/a    0 Bytes
        L2 ineligible evictions:                                 0 Bytes

ARC total accesses:                                                    0
        Total hits:                                       n/a          0
        Total I/O hits:                                   n/a          0
        Total misses:                                     n/a          0

ARC demand data accesses:                                 n/a          0
        Demand data hits:                                 n/a          0
        Demand data I/O hits:                             n/a          0
        Demand data misses:                               n/a          0

ARC demand metadata accesses:                             n/a          0
        Demand metadata hits:                             n/a          0
        Demand metadata I/O hits:                         n/a          0
        Demand metadata misses:                           n/a          0

ARC prefetch data accesses:                               n/a          0
        Prefetch data hits:                               n/a          0
        Prefetch data I/O hits:                           n/a          0
        Prefetch data misses:                             n/a          0

ARC prefetch metadata accesses:                           n/a          0
        Prefetch metadata hits:                           n/a          0
        Prefetch metadata I/O hits:                       n/a          0
        Prefetch metadata misses:                         n/a          0

ARC predictive prefetches:                                n/a          0
        Demand hits after predictive:                     n/a          0
        Demand I/O hits after predictive:                 n/a          0
        Never demanded after predictive:                  n/a          0

ARC prescient prefetches:                                 n/a          0
        Demand hits after prescient:                      n/a          0
        Demand I/O hits after prescient:                  n/a          0
        Never demanded after prescient:                   n/a          0

ARC states hits of all accesses:
        Most frequently used (MFU):                       n/a          0
        Most recently used (MRU):                         n/a          0
        Most frequently used (MFU) ghost:                 n/a          0
        Most recently used (MRU) ghost:                   n/a          0
        Uncached:                                         n/a          0

DMU predictive prefetcher calls:                                       0
        Stream hits:                                      n/a          0
        Hits ahead of stream:                             n/a          0
        Hits behind stream:                               n/a          0
        Stream misses:                                    n/a          0
        Streams limit reached:                            n/a          0
        Stream strides:                                                0
        Prefetches issued                                              0

L2ARC not detected, skipping section

Solaris Porting Layer (SPL):
        spl_hostid                                                     0
        spl_hostid_path                                      /etc/hostid
        spl_kmem_alloc_max                                       1048576
        spl_kmem_alloc_warn                                        65536
        spl_kmem_cache_kmem_threads                                    4
        spl_kmem_cache_magazine_size                                   0
        spl_kmem_cache_max_size                                       32
        spl_kmem_cache_obj_per_slab                                    8
        spl_kmem_cache_slab_limit                                  16384
        spl_panic_halt                                                 0
        spl_schedule_hrtimeout_slack_us                                0
        spl_taskq_kick                                                 0
        spl_taskq_thread_bind                                          0
        spl_taskq_thread_dynamic                                       1
        spl_taskq_thread_priority                                      1
        spl_taskq_thread_sequential                                    4
        spl_taskq_thread_timeout_ms                                 5000

Tunables:
        brt_zap_default_bs                                            13
        brt_zap_default_ibs                                           13
        brt_zap_prefetch                                               1
        dbuf_cache_hiwater_pct                                        10
        dbuf_cache_lowater_pct                                        10
        dbuf_cache_max_bytes                        18446744073709551615
        dbuf_cache_shift                                               5
        dbuf_metadata_cache_max_bytes               18446744073709551615
        dbuf_metadata_cache_shift                                      6
        dbuf_mutex_cache_shift                                         0
        ddt_zap_default_bs                                            15
        ddt_zap_default_ibs                                           15
        dmu_ddt_copies                                                 0
        dmu_object_alloc_chunk_shift                                   7
        dmu_prefetch_max                                       134217728
        icp_aes_impl                      cycle [fastest] generic x86_64
        icp_gcm_avx_chunk_size                                     32736
        icp_gcm_impl                             cycle [fastest] generic
        l2arc_exclude_special                                          0
        l2arc_feed_again                                               1
        l2arc_feed_min_ms                                            200
        l2arc_feed_secs                                                1
        l2arc_headroom                                                 8
        l2arc_headroom_boost                                         200
        l2arc_meta_percent                                            33
        l2arc_mfuonly                                                  0
        l2arc_noprefetch                                               1
        l2arc_norw                                                     0
        l2arc_rebuild_blocks_min_l2size                       1073741824
        l2arc_rebuild_enabled                                          1
        l2arc_trim_ahead                                               0
        l2arc_write_boost                                       33554432
        l2arc_write_max                                         33554432
        metaslab_aliquot                                         2097152
        metaslab_bias_enabled                                          1
        metaslab_debug_load                                            0
        metaslab_debug_unload                                          0
        metaslab_df_max_search                                  16777216
        metaslab_df_use_largest_segment                                0
        metaslab_force_ganging                                  16777217
        metaslab_force_ganging_pct                                     3
        metaslab_fragmentation_factor_enabled                          1
        metaslab_lba_weighting_enabled                                 1
        metaslab_perf_bias                                             1
        metaslab_preload_enabled                                       1
        metaslab_preload_limit                                        10
        metaslab_preload_pct                                          50
        metaslab_unload_delay                                         32
        metaslab_unload_delay_ms                                  600000
        raidz_expand_max_copy_bytes                            167772160
        raidz_expand_max_reflow_bytes                                  0
        raidz_io_aggregate_rows                                        4
        send_holes_without_birth_time                                  1
        spa_asize_inflation                                           24
        spa_config_path                             /etc/zfs/zpool.cache
        spa_cpus_per_allocator                                         4
        spa_flush_txg_time                                           600
        spa_load_print_vdev_tree                                       0
        spa_load_verify_data                                           1
        spa_load_verify_metadata                                       1
        spa_load_verify_shift                                          4
        spa_note_txg_time                                            600
        spa_num_allocators                                             4
        spa_slop_shift                                                 5
        spa_upgrade_errlog_limit                                       0
        vdev_file_logical_ashift                                       9
        vdev_file_physical_ashift                                      9
        vdev_raidz_outlier_check_interval_ms                        1000
        vdev_raidz_outlier_insensitivity                              50
        vdev_read_sit_out_secs                                       600
        vdev_removal_max_span                                      32768
        vdev_validate_skip                                             0
        zap_iterate_prefetch                                           1
        zap_micro_max_size                                        131072
        zap_shrink_enabled                                             1
        zfetch_hole_shift                                              2
        zfetch_max_distance                                     67108864
        zfetch_max_idistance                                   134217728
        zfetch_max_reorder                                      16777216
        zfetch_max_sec_reap                                            2
        zfetch_max_streams                                             8
        zfetch_min_distance                                      4194304
        zfetch_min_sec_reap                                            1
        zfs_abd_scatter_enabled                                        1
        zfs_abd_scatter_max_order                                      9
        zfs_abd_scatter_min_size                                    1536
        zfs_active_allocator                                     dynamic
        zfs_admin_snapshot                                             0
        zfs_allow_redacted_dataset_mount                               0
        zfs_arc_average_blocksize                                   8192
        zfs_arc_dnode_limit                                            0
        zfs_arc_dnode_limit_percent                                   10
        zfs_arc_dnode_reduce_percent                                  10
        zfs_arc_evict_batch_limit                                     10
        zfs_arc_evict_batches_limit                                    5
        zfs_arc_evict_threads                                          4
        zfs_arc_eviction_pct                                         200
        zfs_arc_grow_retry                                             0
        zfs_arc_lotsfree_percent                                      10
        zfs_arc_max                                          13515096064
        zfs_arc_meta_balance                                         500
        zfs_arc_min                                                    0
        zfs_arc_min_prefetch_ms                                        0
        zfs_arc_min_prescient_prefetch_ms                              0
        zfs_arc_pc_percent                                             0
        zfs_arc_prune_task_threads                                     1
        zfs_arc_shrink_shift                                           0
        zfs_arc_shrinker_limit                                         0
        zfs_arc_shrinker_seeks                                         2
        zfs_arc_sys_free                                               0
        zfs_async_block_max_blocks                  18446744073709551615
        zfs_async_free_zio_wait_interval                            2000
        zfs_bclone_enabled                                             1
        zfs_bclone_wait_dirty                                          1
        zfs_blake3_impl               cycle [fastest] generic sse2 sse41
        zfs_btree_verify_intensity                                     0
        zfs_checksum_events_per_second                                20
        zfs_commit_timeout_pct                                        10
        zfs_compressed_arc_enabled                                     1
        zfs_condense_indirect_commit_entry_delay_ms                    0
        zfs_condense_indirect_obsolete_pct                            25
        zfs_condense_indirect_vdevs_enable                             1
        zfs_condense_max_obsolete_bytes                       1073741824
        zfs_condense_min_mapping_bytes                            131072
        zfs_dbgmsg_enable                                              1
        zfs_dbgmsg_maxsize                                       4194304
        zfs_dbuf_state_index                                           0
        zfs_ddt_data_is_special                                        1
        zfs_deadman_checktime_ms                                   60000
        zfs_deadman_enabled                                            1
        zfs_deadman_events_per_second                                  1
        zfs_deadman_failmode                                        wait
        zfs_deadman_synctime_ms                                   600000
        zfs_deadman_ziotime_ms                                    300000
        zfs_dedup_log_cap                                     4294967295
        zfs_dedup_log_flush_entries_max                       4294967295
        zfs_dedup_log_flush_entries_min                              200
        zfs_dedup_log_flush_flow_rate_txgs                            10
        zfs_dedup_log_flush_min_time_ms                             1000
        zfs_dedup_log_flush_txgs                                     100
        zfs_dedup_log_hard_cap                                         0
        zfs_dedup_log_mem_max                                 1351588454
        zfs_dedup_log_mem_max_percent                                  1
        zfs_dedup_log_txg_max                                          8
        zfs_dedup_prefetch                                             0
        zfs_default_bs                                                 9
        zfs_default_ibs                                               17
        zfs_delay_min_dirty_percent                                   60
        zfs_delay_scale                                           500000
        zfs_delete_blocks                                          20480
        zfs_delete_dentry                                              0
        zfs_delete_inode                                               0
        zfs_dio_enabled                                                1
        zfs_dio_strict                                                 0
        zfs_dio_write_verify_events_per_second                        20
        zfs_dirty_data_max                                    4294967296
        zfs_dirty_data_max_max                                4294967296
        zfs_dirty_data_max_max_percent                                25
        zfs_dirty_data_max_percent                                    10
        zfs_dirty_data_sync_percent                                   20
        zfs_disable_ivset_guid_check                                   0
        zfs_dmu_offset_next_sync                                       1
        zfs_embedded_slog_min_ms                                      64
        zfs_expire_snapshot                                          300
        zfs_fallocate_reserve_percent                                110
        zfs_flags                                                      0
        zfs_fletcher_4_impl [fastest] scalar superscalar superscalar4 sse2 ssse3
        zfs_free_bpobj_enabled                                         1
        zfs_free_leak_on_eio                                           0
        zfs_free_min_time_ms                                         500
        zfs_history_output_max                                   1048576
        zfs_immediate_write_sz                                     32768
        zfs_import_defer_txgs                                          5
        zfs_initialize_chunk_size                                1048576
        zfs_initialize_value                        16045690984833335022
        zfs_keep_log_spacemaps_at_export                               0
        zfs_key_max_salt_uses                                  400000000
        zfs_livelist_condense_new_alloc                                0
        zfs_livelist_condense_sync_cancel                              0
        zfs_livelist_condense_sync_pause                               0
        zfs_livelist_condense_zthr_cancel                              0
        zfs_livelist_condense_zthr_pause                               0
        zfs_livelist_max_entries                                  500000
        zfs_livelist_min_percent_shared                               75
        zfs_lua_max_instrlimit                                 100000000
        zfs_lua_max_memlimit                                   104857600
        zfs_max_async_dedup_frees                                 250000
        zfs_max_dataset_nesting                                       50
        zfs_max_log_walking                                            5
        zfs_max_logsm_summary_length                                  10
        zfs_max_missing_tvds                                           0
        zfs_max_nvlist_src_size                                        0
        zfs_max_recordsize                                      16777216
        zfs_metaslab_find_max_tries                                  100
        zfs_metaslab_fragmentation_threshold                          77
        zfs_metaslab_max_size_cache_sec                             3600
        zfs_metaslab_mem_limit                                        25
        zfs_metaslab_segment_weight_enabled                            1
        zfs_metaslab_switch_threshold                                  2
        zfs_metaslab_try_hard_before_gang                              0
        zfs_mg_fragmentation_threshold                                95
        zfs_mg_noalloc_threshold                                       0
        zfs_min_metaslabs_to_flush                                     1
        zfs_multihost_fail_intervals                                  10
        zfs_multihost_history                                          0
        zfs_multihost_import_intervals                                20
        zfs_multihost_interval                                      1000
        zfs_multilist_num_sublists                                     0
        zfs_no_scrub_io                                                0
        zfs_no_scrub_prefetch                                          0
        zfs_nocacheflush                                               0
        zfs_nopwrite_enabled                                           1
        zfs_object_mutex_size                                         64
        zfs_obsolete_min_time_ms                                     500
        zfs_override_estimate_recordsize                               0
        zfs_pd_bytes_max                                        52428800
        zfs_per_txg_dirty_frees_percent                               30
        zfs_prefetch_disable                                           0
        zfs_read_history                                               0
        zfs_read_history_hits                                          0
        zfs_rebuild_max_segment                                  1048576
        zfs_rebuild_scrub_enabled                                      1
        zfs_rebuild_vdev_limit                                  67108864
        zfs_reconstruct_indirect_combinations_max                   4096
        zfs_recover                                                    0
        zfs_recv_best_effort_corrective                                0
        zfs_recv_queue_ff                                             20
        zfs_recv_queue_length                                   16777216
        zfs_recv_write_batch_size                                1048576
        zfs_removal_ignore_errors                                      0
        zfs_removal_suspend_progress                                   0
        zfs_remove_max_segment                                  16777216
        zfs_resilver_defer_percent                                    10
        zfs_resilver_disable_defer                                     0
        zfs_resilver_min_time_ms                                    1500
        zfs_scan_blkstats                                              0
        zfs_scan_checkpoint_intval                                  7200
        zfs_scan_fill_weight                                           3
        zfs_scan_ignore_errors                                         0
        zfs_scan_issue_strategy                                        0
        zfs_scan_legacy                                                0
        zfs_scan_max_ext_gap                                     2097152
        zfs_scan_mem_lim_fact                                         20
        zfs_scan_mem_lim_soft_fact                                    20
        zfs_scan_report_txgs                                           0
        zfs_scan_strict_mem_lim                                        0
        zfs_scan_suspend_progress                                      0
        zfs_scan_vdev_limit                                     16777216
        zfs_scrub_after_expand                                         1
        zfs_scrub_error_blocks_per_txg                              4096
        zfs_scrub_min_time_ms                                        750
        zfs_send_corrupt_data                                          0
        zfs_send_no_prefetch_queue_ff                                 20
        zfs_send_no_prefetch_queue_length                        1048576
        zfs_send_queue_ff                                             20
        zfs_send_queue_length                                   16777216
        zfs_send_unmodified_spill_blocks                               1
        zfs_sha256_impl                cycle [fastest] generic x64 ssse3
        zfs_sha512_impl                      cycle [fastest] generic x64
        zfs_slow_io_events_per_second                                 20
        zfs_snapshot_history_enabled                                   1
        zfs_snapshot_no_setuid                                         0
        zfs_spa_discard_memory_limit                            16777216
        zfs_special_class_metadata_reserve_pct                        25
        zfs_sync_pass_deferred_free                                    2
        zfs_sync_pass_dont_compress                                    8
        zfs_sync_pass_rewrite                                          2
        zfs_traverse_indirect_prefetch_limit                          32
        zfs_trim_extent_bytes_max                              134217728
        zfs_trim_extent_bytes_min                                  32768
        zfs_trim_metaslab_skip                                         0
        zfs_trim_queue_limit                                          10
        zfs_trim_txg_batch                                            32
        zfs_txg_history                                              100
        zfs_txg_timeout                                                5
        zfs_unflushed_log_block_max                               131072
        zfs_unflushed_log_block_min                                 1000
        zfs_unflushed_log_block_pct                                  400
        zfs_unflushed_log_txg_max                                   1000
        zfs_unflushed_max_mem_amt                             1073741824
        zfs_unflushed_max_mem_ppm                                   1000
        zfs_unlink_suspend_progress                                    0
        zfs_user_indirect_is_special                                   1
        zfs_vdev_aggregation_limit                               1048576
        zfs_vdev_aggregation_limit_non_rotating                   131072
        zfs_vdev_async_read_max_active                                 3
        zfs_vdev_async_read_min_active                                 1
        zfs_vdev_async_write_active_max_dirty_percent                 60
        zfs_vdev_async_write_active_min_dirty_percent                 30
        zfs_vdev_async_write_max_active                               10
        zfs_vdev_async_write_min_active                                2
        zfs_vdev_default_ms_count                                    200
        zfs_vdev_default_ms_shift                                     29
        zfs_vdev_direct_write_verify                                   1
        zfs_vdev_disk_max_segs                                         0
        zfs_vdev_failfast_mask                                         1
        zfs_vdev_initializing_max_active                               1
        zfs_vdev_initializing_min_active                               1
        zfs_vdev_max_active                                         1000
        zfs_vdev_max_auto_ashift                                      14
        zfs_vdev_max_ms_shift                                         34
        zfs_vdev_min_auto_ashift                                       9
        zfs_vdev_min_ms_count                                         16
        zfs_vdev_mirror_non_rotating_inc                               0
        zfs_vdev_mirror_non_rotating_seek_inc                          1
        zfs_vdev_mirror_rotating_inc                                   0
        zfs_vdev_mirror_rotating_seek_inc                              5
        zfs_vdev_mirror_rotating_seek_offset                     1048576
        zfs_vdev_ms_count_limit                                   131072
        zfs_vdev_nia_credit                                            5
        zfs_vdev_nia_delay                                             5
        zfs_vdev_open_timeout_ms                                    1000
        zfs_vdev_raidz_impl   cycle [fastest] original scalar sse2 ssse3
        zfs_vdev_read_gap_limit                                    32768
        zfs_vdev_rebuild_max_active                                    3
        zfs_vdev_rebuild_min_active                                    1
        zfs_vdev_removal_max_active                                    2
        zfs_vdev_removal_min_active                                    1
        zfs_vdev_scrub_max_active                                      3
        zfs_vdev_scrub_min_active                                      1
        zfs_vdev_sync_read_max_active                                 10
        zfs_vdev_sync_read_min_active                                 10
        zfs_vdev_sync_write_max_active                                10
        zfs_vdev_sync_write_min_active                                10
        zfs_vdev_trim_max_active                                       2
        zfs_vdev_trim_min_active                                       1
        zfs_vdev_write_gap_limit                                    4096
        zfs_vnops_read_chunk_size                               33554432
        zfs_wrlog_data_max                                    8589934592
        zfs_xattr_compat                                               0
        zfs_zevent_len_max                                           512
        zfs_zevent_retain_expire_secs                                900
        zfs_zevent_retain_max                                       2000
        zfs_zil_clean_taskq_maxalloc                             1048576
        zfs_zil_clean_taskq_minalloc                                1024
        zfs_zil_clean_taskq_nthr_pct                                 100
        zfs_zil_saxattr                                                1
        zil_maxblocksize                                          131072
        zil_maxcopied                                               7680
        zil_nocacheflush                                               0
        zil_replay_disable                                             0
        zil_slog_bulk                                           67108864
        zil_special_is_slog                                            1
        zio_deadman_log_all                                            0
        zio_dva_throttle_enabled                                       1
        zio_requeue_io_start_cut_in_line                               1
        zio_slow_io_ms                                             30000
        zio_taskq_batch_pct                                           80
        zio_taskq_batch_tpq                                            0
        zio_taskq_free                      scale,32 null fixed,1,1 null
        zio_taskq_read                         fixed,1,8 null scale null
        zio_taskq_write                             sync null scale null
        zio_taskq_write_tpq                                           16
        zstd_abort_size                                           131072
        zstd_earlyabort_pass                                           1
        zvol_blk_mq_blocks_per_thread                                  8
        zvol_blk_mq_queue_depth                                      128
        zvol_enforce_quotas                                            1
        zvol_inhibit_dev                                               0
        zvol_major                                                   230
        zvol_max_discard_blocks                                    16384
        zvol_num_taskqs                                                0
        zvol_open_timeout_ms                                        1000
        zvol_prefetch_bytes                                       131072
        zvol_request_sync                                              0
        zvol_threads                                                   0
        zvol_use_blk_mq                                                0
        zvol_volmode                                                   1

ZIL committed transactions:                                            0
        Commit requests:                                               0
        Flushes to stable storage:                                     0
        Transactions to SLOG storage pool:            0 Bytes          0
        Transactions to non-SLOG storage pool:        0 Bytes          0


--- zpool events -v (recent)
    $ zpool events -v
TIME                           CLASS

--- zpool history (last 30 events)
    $ zpool history -il 2>/dev/null | tail -n 30

###############################################################################
# 20. STORAGE: DRIVE HEALTH
###############################################################################

--- nvme list
    $ nvme list
Node                  Generic               SN                   Model                                    Namespace  Usage                      Format           FW Rev  
--------------------- --------------------- -------------------- ---------------------------------------- ---------- -------------------------- ---------------- --------

--- nvme smart-log per device
    $ for n in /dev/nvme[0-9]*; do
    [ -b "$n" ] || continue
    echo "--- $n smart-log ---"
    nvme smart-log "$n" 2>&1
    echo "--- $n error-log (first 5) ---"
    nvme error-log "$n" 2>&1 | head -n 80
done

--- nvme id-ctrl per device (key fields)
    $ for n in /dev/nvme[0-9]*; do
    [ -b "$n" ] || continue
    echo "--- $n id-ctrl (filtered) ---"
    nvme id-ctrl "$n" 2>&1 | grep -E '^(mn|sn|fn|fr|tnvmcap|vid|IEEE|cntlid|ver|rab|lpa|elpe|npdg|mdts|hmpre|hmmin|cap|frmw|lba|ws|awun|awupf|acwu|apsta)'
done

--- smartctl -a per disk
    $ for d in $(ls /sys/block/ 2>/dev/null | grep -E '^(sd|vd)'); do
    dev="/dev/$d"
    [ -b "$dev" ] || continue
    echo "--- smartctl -a $dev ---"
    smartctl -a "$dev" 2>&1 | head -n 200
done
--- smartctl -a /dev/sda ---
smartctl 7.5 2025-04-30 r5714 [x86_64-linux-7.0.14-6-pve] (local build)
Copyright (C) 2002-25, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Device Model:     WDC WD20SDRM-59A4DS1
Serial Number:    WD-WXL2A232X5RX
LU WWN Device Id: 5 0014ee 215a96feb
Firmware Version: 01.01A01
User Capacity:    2,000,365,379,584 bytes [2.00 TB]
Sector Sizes:     512 bytes logical, 4096 bytes physical
Rotation Rate:    5400 rpm
Form Factor:      2.5 inches
TRIM Command:     Available, deterministic
Device is:        Not in smartctl database 7.5/5706
ATA Version is:   ACS-3 T13/2161-D revision 5
SATA Version is:  SATA 3.1, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Wed Jul 29 05:13:37 2026 CDT
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		( 2100) seconds.
Offline data collection
capabilities: 			 (0x51) SMART execute Offline immediate.
					No Auto Offline data collection support.
					Suspend Offline collection upon new
					command.
					No Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 ( 100) minutes.
SCT capabilities: 	       (0x7035)	SCT Status supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAG     VALUE WORST THRESH TYPE      UPDATED  WHEN_FAILED RAW_VALUE
  1 Raw_Read_Error_Rate     0x002f   200   200   051    Pre-fail  Always       -       0
  3 Spin_Up_Time            0x0027   196   190   021    Pre-fail  Always       -       3158
  4 Start_Stop_Count        0x0032   094   094   000    Old_age   Always       -       6737
  5 Reallocated_Sector_Ct   0x0033   200   200   140    Pre-fail  Always       -       0
  7 Seek_Error_Rate         0x002e   200   200   000    Old_age   Always       -       0
  9 Power_On_Hours          0x0032   078   078   000    Old_age   Always       -       16350
 10 Spin_Retry_Count        0x0032   100   100   000    Old_age   Always       -       0
 11 Calibration_Retry_Count 0x0032   100   100   000    Old_age   Always       -       0
 12 Power_Cycle_Count       0x0032   100   100   000    Old_age   Always       -       372
192 Power-Off_Retract_Count 0x0032   200   200   000    Old_age   Always       -       266
193 Load_Cycle_Count        0x0032   190   190   000    Old_age   Always       -       30414
194 Temperature_Celsius     0x0022   117   091   000    Old_age   Always       -       30
196 Reallocated_Event_Count 0x0032   200   200   000    Old_age   Always       -       0
197 Current_Pending_Sector  0x0032   200   200   000    Old_age   Always       -       0
198 Offline_Uncorrectable   0x0030   100   253   000    Old_age   Offline      -       0
199 UDMA_CRC_Error_Count    0x0032   200   200   000    Old_age   Always       -       0
200 Multi_Zone_Error_Rate   0x0008   100   253   000    Old_age   Offline      -       0

SMART Error Log Version: 1
No Errors Logged

SMART Self-test log structure revision number 1
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

The above only provides legacy SMART information - try 'smartctl -x' for more


###############################################################################
# 21. STORAGE: HBA / RAID CONTROLLERS
###############################################################################

###############################################################################
# 22. VIRTUAL MACHINES (qm)
###############################################################################

--- qm list
    $ qm list
      VMID NAME                 STATUS     MEM(MB)    BOOTDISK(GB) PID       
       100 pfv-k8s-wnode-tsys6  running    32000             32.00 283375    
       600 tsys-awx             running    12000             32.00 283519    
       601 pfv-k8s-cnode4       running    4096              32.00 283674    

--- qm config per VM
    $ for vmid in $(qm list 2>/dev/null | awk 'NR>1{print $1}'); do
    echo "--- VM $vmid ---"
    qm config "$vmid" 2>&1
    echo ""
done
--- VM 100 ---
balloon: 0
boot: order=scsi0
cores: 2
cpu: host
ide2: local:iso/debian.iso,media=cdrom,size=755M
memory: 32000
meta: creation-qemu=10.1.2,ctime=1785085054
name: pfv-k8s-wnode-tsys6
net0: virtio=BC:24:11:F6:74:E8,bridge=vmbr0,firewall=1
numa: 0
onboot: 1
ostype: l26
scsi0: S4:100/vm-100-disk-0.qcow2,iothread=1,size=32G
scsihw: virtio-scsi-single
smbios1: uuid=03709518-2933-4764-8006-f3946ce59063
sockets: 2
vmgenid: 5a31db88-9ad1-4a8d-95cc-156eea8e87ae

--- VM 600 ---
agent: 1
balloon: 0
boot: order=scsi0
cores: 2
cpu: host
ide2: none,media=cdrom
memory: 12000
meta: creation-qemu=10.1.2,ctime=1771904766
name: tsys-awx
net0: virtio=BC:24:11:80:0D:16,bridge=vmbr0,firewall=1
numa: 0
onboot: 1
ostype: l26
scsi0: D2:600/vm-600-disk-1.qcow2,cache=writethrough,format=qcow2,iothread=1,size=32G
scsihw: virtio-scsi-single
smbios1: uuid=3f480575-849f-421c-8a53-0d46fcce3154
sockets: 2
vmgenid: b62bf796-cde6-4697-9df0-66cdb313e63d

--- VM 601 ---
agent: 1
balloon: 0
boot: order=scsi0;ide2;net0
cores: 4
cpu: host
ide2: none,media=cdrom
memory: 4096
meta: creation-qemu=10.1.2,ctime=1771904766
name: pfv-k8s-cnode4
net0: virtio=BC:24:11:27:4F:1C,bridge=vmbr0,firewall=1
numa: 0
onboot: 1
ostype: l26
scsi0: D2:601/vm-601-disk-0.qcow2,cache=writethrough,format=qcow2,iothread=1,size=32G
scsihw: virtio-scsi-single
smbios1: uuid=b9ef082b-3eb8-474d-a1b6-5a947433aa98
sockets: 1
vmgenid: c533aceb-c8c2-46e0-b3ff-cb547d6d9669


--- VM runtime status (qm guest agent if running)
    $ for vmid in $(qm list 2>/dev/null | awk 'NR>1{print $1}'); do
    echo "--- VM $vmid runtime ---"
    qm guest cmd "$vmid" network-get-interfaces 2>/dev/null | head -n 40 || echo "  [no agent or VM not running]"
done
--- VM 100 runtime ---
--- VM 600 runtime ---
[
   {
      "hardware-address" : "00:00:00:00:00:00",
      "ip-addresses" : [
         {
            "ip-address" : "127.0.0.1",
            "ip-address-type" : "ipv4",
            "prefix" : 8
         },
         {
            "ip-address" : "::1",
            "ip-address-type" : "ipv6",
            "prefix" : 128
         }
      ],
      "name" : "lo",
      "statistics" : {
         "rx-bytes" : 100698,
         "rx-dropped" : 0,
         "rx-errs" : 0,
         "rx-packets" : 1123,
         "tx-bytes" : 100698,
         "tx-dropped" : 0,
         "tx-errs" : 0,
         "tx-packets" : 1123
      }
   },
   {
      "hardware-address" : "bc:24:11:80:0d:16",
      "ip-addresses" : [
         {
            "ip-address" : "192.168.3.200",
            "ip-address-type" : "ipv4",
            "prefix" : 22
         },
         {
            "ip-address" : "2600:1700:1d1:eb00:7e75:979:903:add1",
            "ip-address-type" : "ipv6",
            "prefix" : 64
         },
--- VM 601 runtime ---
[
   {
      "hardware-address" : "00:00:00:00:00:00",
      "ip-addresses" : [
         {
            "ip-address" : "127.0.0.1",
            "ip-address-type" : "ipv4",
            "prefix" : 8
         },
         {
            "ip-address" : "::1",
            "ip-address-type" : "ipv6",
            "prefix" : 128
         }
      ],
      "name" : "lo",
      "statistics" : {
         "rx-bytes" : 71528538,
         "rx-dropped" : 0,
         "rx-errs" : 0,
         "rx-packets" : 130517,
         "tx-bytes" : 71528538,
         "tx-dropped" : 0,
         "tx-errs" : 0,
         "tx-packets" : 130517
      }
   },
   {
      "hardware-address" : "bc:24:11:27:4f:1c",
      "ip-addresses" : [
         {
            "ip-address" : "192.168.3.157",
            "ip-address-type" : "ipv4",
            "prefix" : 22
         },
         {
            "ip-address" : "2600:1700:1d1:eb00:66c4:2494:db49:b5f1",
            "ip-address-type" : "ipv6",
            "prefix" : 64
         },

--- /etc/pve/qemu-server
lrwxr-xr-x 1 root www-data 27 Dec 31  1969 /etc/pve/qemu-server -> nodes/pfv-tsys6/qemu-server

--- /etc/pve/firewall
total 0
drwxr-xr-x 2 root www-data 0 Apr  4 12:47 .
drwxr-xr-x 2 root www-data 0 Dec 31  1969 ..

###############################################################################
# 23. CONTAINERS (pct)
###############################################################################

--- pct list
    $ pct list

--- pct config per CT
    $ for ctid in $(pct list 2>/dev/null | awk 'NR>1{print $1}'); do
    echo "--- CT $ctid ---"
    pct config "$ctid" 2>&1
    echo ""
done

###############################################################################
# 24. SERVICES / FAILED UNITS
###############################################################################

--- running services
    $ systemctl list-units --type=service --state=running --no-pager
  UNIT                     LOAD   ACTIVE SUB     DESCRIPTION
  beszel-agent.service     loaded active running Beszel Agent Service
  chrony.service           loaded active running chrony, an NTP client/server
  cron.service             loaded active running Regular background program processing daemon
  dbus.service             loaded active running D-Bus System Message Bus
  dm-event.service         loaded active running Device-mapper event daemon
  getty@tty1.service       loaded active running Getty on tty1
  ksmtuned.service         loaded active running Kernel Samepage Merging (KSM) Tuning Daemon
  lldpd.service            loaded active running LLDP daemon
  lxc-monitord.service     loaded active running LXC Container Monitoring Daemon
  lxcfs.service            loaded active running FUSE filesystem for LXC
  nfs-blkmap.service       loaded active running pNFS block layout mapping daemon
  polkit.service           loaded active running Authorization Manager
  postfix.service          loaded active running Postfix Mail Transport Agent (main/default instance)
  proxmox-firewall.service loaded active running Proxmox nftables firewall
  pve-cluster.service      loaded active running The Proxmox VE cluster filesystem
  pve-firewall.service     loaded active running Proxmox VE firewall
  pve-ha-crm.service       loaded active running PVE Cluster HA Resource Manager Daemon
  pve-ha-lrm.service       loaded active running PVE Local HA Resource Manager Daemon
  pve-lxc-syscalld.service loaded active running Proxmox VE LXC Syscall Daemon
  pvedaemon.service        loaded active running PVE API Daemon
  pvefw-logger.service     loaded active running Proxmox VE firewall logger
  pveproxy.service         loaded active running PVE API Proxy Server
  pvescheduler.service     loaded active running Proxmox VE scheduler
  pvestatd.service         loaded active running PVE Status Daemon
  qmeventd.service         loaded active running PVE Qemu Event Daemon
  rpcbind.service          loaded active running RPC bind portmap service
  rrdcached.service        loaded active running Data caching daemon for rrdtool
  smartmontools.service    loaded active running Self Monitoring and Reporting Technology (SMART) Daemon
  spiceproxy.service       loaded active running PVE SPICE Proxy Server
  ssh.service              loaded active running OpenBSD Secure Shell server
  systemd-journald.service loaded active running Journal Service
  systemd-logind.service   loaded active running User Login Management
  systemd-udevd.service    loaded active running Rule-based Manager for Device Events and Files
  tailscaled.service       loaded active running Tailscale node agent
  tuned.service            loaded active running Dynamic System Tuning Daemon
  user@0.service           loaded active running User Manager for UID 0
  watchdog-mux.service     loaded active running Proxmox VE watchdog multiplexer
  zfs-zed.service          loaded active running ZFS Event Daemon (zed)

Legend: LOAD   → Reflects whether the unit definition was properly loaded.
        ACTIVE → The high-level unit activation state, i.e. generalization of SUB.
        SUB    → The low-level unit activation state, values depend on unit type.

38 loaded units listed.

--- failed services
    $ systemctl --failed --no-pager
  UNIT LOAD ACTIVE SUB DESCRIPTION

0 loaded units listed.

--- enabled services
    $ systemctl list-unit-files --state=enabled --no-pager
UNIT FILE                              STATE   PRESET
apparmor.service                       enabled enabled
beszel-agent.service                   enabled enabled
blk-availability.service               enabled enabled
chrony.service                         enabled enabled
console-setup.service                  enabled enabled
corosync.service                       enabled enabled
cron.service                           enabled enabled
e2scrub_reap.service                   enabled enabled
getty@.service                         enabled enabled
grub-common.service                    enabled enabled
keyboard-setup.service                 enabled enabled
ksmtuned.service                       enabled enabled
lldpd.service                          enabled enabled
lvm2-monitor.service                   enabled enabled
lxc-monitord.service                   enabled enabled
lxc-net.service                        enabled enabled
lxc.service                            enabled enabled
lxcfs.service                          enabled enabled
netavark-dhcp-proxy.service            enabled enabled
netavark-firewalld-reload.service      enabled enabled
networking.service                     enabled enabled
nfs-blkmap.service                     enabled enabled
nvmefc-boot-connections.service        enabled enabled
nvmf-autoconnect.service               enabled enabled
open-iscsi.service                     enabled enabled
postfix.service                        enabled enabled
proxmox-boot-cleanup.service           enabled enabled
proxmox-firewall.service               enabled enabled
pve-cluster.service                    enabled enabled
pve-firewall-commit.service            enabled enabled
pve-firewall.service                   enabled enabled
pve-guests.service                     enabled enabled
pve-ha-crm.service                     enabled enabled
pve-ha-lrm.service                     enabled enabled
pve-lxc-syscalld.service               enabled enabled
pve-query-machine-capabilities.service enabled enabled
pve-sdn-commit.service                 enabled enabled
pvebanner.service                      enabled enabled
pvedaemon.service                      enabled enabled
pvefw-logger.service                   enabled enabled
pvenetcommit.service                   enabled enabled
pveproxy.service                       enabled enabled
pvescheduler.service                   enabled enabled
pvestatd.service                       enabled enabled
qmeventd.service                       enabled enabled
rbdmap.service                         enabled enabled
rpcbind.service                        enabled enabled
rrdcached.service                      enabled enabled
smartmontools.service                  enabled enabled
spiceproxy.service                     enabled enabled
ssh.service                            enabled enabled
sshd-keygen.service                    enabled enabled
sysstat.service                        enabled enabled
systemd-pstore.service                 enabled enabled
tailscaled.service                     enabled enabled
tuned.service                          enabled enabled
wtmpdb-update-boot.service             enabled enabled
zfs-import-cache.service               enabled enabled
zfs-mount.service                      enabled enabled
zfs-share.service                      enabled enabled
zfs-volume-wait.service                enabled enabled
zfs-zed.service                        enabled enabled
system-xfs_scrub.slice                 enabled enabled
dm-event.socket                        enabled enabled
iscsid.socket                          enabled enabled
lvm2-lvmpolld.socket                   enabled enabled
netavark-dhcp-proxy.socket             enabled enabled
rpcbind.socket                         enabled enabled
rrdcached.socket                       enabled enabled
uuidd.socket                           enabled enabled
ceph-fuse.target                       enabled enabled
ceph.target                            enabled enabled
nfs-client.target                      enabled enabled
remote-fs.target                       enabled enabled
zfs-import.target                      enabled enabled
zfs-volumes.target                     enabled enabled
zfs.target                             enabled enabled
apt-daily-upgrade.timer                enabled enabled
apt-daily.timer                        enabled enabled
beszel-agent-update.timer              enabled enabled
dpkg-db-backup.timer                   enabled enabled
e2scrub_all.timer                      enabled enabled
fstrim.timer                           enabled enabled
logrotate.timer                        enabled enabled
man-db.timer                           enabled enabled
pve-daily-update.timer                 enabled enabled
sysstat-collect.timer                  enabled enabled
sysstat-rotate.timer                   enabled enabled
sysstat-summary.timer                  enabled enabled
xfs_scrub_all.timer                    enabled enabled

90 unit files listed.

--- pve-* service status
    $ systemctl status pve-cluster pvedaemon pveproxy pve-firewall pve-ha-crm pve-ha-lrm pvestatd pvebanner --no-pager 2>&1 | head -n 120
● pve-cluster.service - The Proxmox VE cluster filesystem
     Loaded: loaded (/usr/lib/systemd/system/pve-cluster.service; enabled; preset: enabled)
     Active: active (running) since Sun 2026-07-26 17:20:30 CDT; 2 days ago
 Invocation: 62b694216e044c82810cf98c43af9e8e
    Process: 1206 ExecStart=/usr/bin/pmxcfs (code=exited, status=0/SUCCESS)
   Main PID: 1317 (pmxcfs)
      Tasks: 7 (limit: 143874)
     Memory: 65.9M (peak: 82.9M)
        CPU: 2min 36.375s
     CGroup: /system.slice/pve-cluster.service
             └─1317 /usr/bin/pmxcfs

Jul 26 17:20:26 pfv-tsys6 systemd[1]: Starting pve-cluster.service - The Proxmox VE cluster filesystem...
Jul 26 17:20:27 pfv-tsys6 pmxcfs[1206]: [main] notice: resolved node name 'pfv-tsys6' to '192.168.100.2' for default node IP address
Jul 26 17:20:27 pfv-tsys6 pmxcfs[1206]: [main] notice: resolved node name 'pfv-tsys6' to '192.168.100.2' for default node IP address
Jul 26 17:20:30 pfv-tsys6 systemd[1]: Started pve-cluster.service - The Proxmox VE cluster filesystem.

● pvedaemon.service - PVE API Daemon
     Loaded: loaded (/usr/lib/systemd/system/pvedaemon.service; enabled; preset: enabled)
     Active: active (running) since Sun 2026-07-26 17:20:39 CDT; 2 days ago
 Invocation: e69e9d2d1910454d86a2b1833e6f8f00
    Process: 1371 ExecStart=/usr/bin/pvedaemon start (code=exited, status=0/SUCCESS)
   Main PID: 1517 (pvedaemon)
      Tasks: 6 (limit: 143874)
     Memory: 325.6M (peak: 508.4M)
        CPU: 6min 5.788s
     CGroup: /system.slice/pvedaemon.service
             ├─   1517 pvedaemon
             ├─ 947600 "pvedaemon worker"
             ├─ 949449 "pvedaemon worker"
             ├─ 949846 "pvedaemon worker"
             ├─1073219 "task UPID:pfv-tsys6:00106043:01477713:6A69CE35:vncproxy:100:root@pam:"
             └─1073221 /usr/bin/perl /usr/sbin/qm vncproxy 100

Jul 28 22:04:16 pfv-tsys6 pvedaemon[1517]: starting 1 worker(s)
Jul 28 22:04:16 pfv-tsys6 pvedaemon[1517]: worker 949846 started
Jul 28 22:17:39 pfv-tsys6 pvedaemon[947600]: <root@pam> successful auth for user 'root@pam'
Jul 29 04:55:38 pfv-tsys6 IPCC.xs[1073059]: pam_unix(proxmox-ve-auth:auth): authentication failure; logname= uid=0 euid=0 tty= ruser= rhost=::ffff:100.109.70.137  user=root
Jul 29 04:55:40 pfv-tsys6 pvedaemon[949449]: authentication failure; rhost=::ffff:100.109.70.137 user=root@pam msg=Authentication failure
Jul 29 04:55:56 pfv-tsys6 pvedaemon[947600]: <root@pam> successful auth for user 'root@pam'
Jul 29 04:55:58 pfv-tsys6 pvedaemon[949449]: <root@pam> successful auth for user 'root@pam'
Jul 29 04:56:05 pfv-tsys6 pvedaemon[1073219]: starting vnc proxy UPID:pfv-tsys6:00106043:01477713:6A69CE35:vncproxy:100:root@pam:
Jul 29 04:56:05 pfv-tsys6 pvedaemon[949449]: <root@pam> starting task UPID:pfv-tsys6:00106043:01477713:6A69CE35:vncproxy:100:root@pam:
Jul 29 05:10:54 pfv-tsys6 pvedaemon[949449]: <root@pam> successful auth for user 'root@pam'

● pveproxy.service - PVE API Proxy Server
     Loaded: loaded (/usr/lib/systemd/system/pveproxy.service; enabled; preset: enabled)
     Active: active (running) since Sun 2026-07-26 17:20:42 CDT; 2 days ago
 Invocation: a1defebf6fe74ec5a01683e481a413b4
    Process: 1523 ExecStartPre=/usr/bin/pvecm updatecerts --silent (code=exited, status=0/SUCCESS)
    Process: 1526 ExecStart=/usr/bin/pveproxy start (code=exited, status=0/SUCCESS)
    Process: 1537 ExecStartPost=sh -c [ ! -e /var/log/pveam.log ] && /usr/bin/pveupdate (code=exited, status=1/FAILURE)
    Process: 993498 ExecReload=/usr/bin/pveproxy restart (code=exited, status=0/SUCCESS)
   Main PID: 1532 (pveproxy)
      Tasks: 4 (limit: 143874)
     Memory: 270.4M (peak: 457.3M)
        CPU: 7min 46.035s
     CGroup: /system.slice/pveproxy.service
             ├─  1532 pveproxy
             ├─993540 "pveproxy worker"
             ├─993541 "pveproxy worker"
             └─993542 "pveproxy worker"

Jul 29 00:30:17 pfv-tsys6 pveproxy[1532]: worker 947403 finished
Jul 29 00:30:17 pfv-tsys6 pveproxy[1532]: worker 949113 finished
Jul 29 04:55:38 pfv-tsys6 pveproxy[993542]: authentication failure: 401 permission denied - invalid PVE ticket
Jul 29 04:55:38 pfv-tsys6 pveproxy[993541]: authentication failure: 401 permission denied - invalid PVE ticket
Jul 29 04:55:38 pfv-tsys6 pveproxy[993542]: authentication failure: 401 permission denied - invalid PVE ticket
Jul 29 04:55:38 pfv-tsys6 pveproxy[993542]: authentication failure: 401 permission denied - invalid PVE ticket
Jul 29 04:55:48 pfv-tsys6 pveproxy[993541]: authentication failure: 401 permission denied - invalid PVE ticket
Jul 29 04:55:48 pfv-tsys6 pveproxy[993542]: authentication failure: 401 permission denied - invalid PVE ticket
Jul 29 04:55:50 pfv-tsys6 pveproxy[993541]: authentication failure: 401 permission denied - invalid PVE ticket
Jul 29 04:55:50 pfv-tsys6 pveproxy[993542]: authentication failure: 401 permission denied - invalid PVE ticket

● pve-firewall.service - Proxmox VE firewall
     Loaded: loaded (/usr/lib/systemd/system/pve-firewall.service; enabled; preset: enabled)
     Active: active (running) since Sun 2026-07-26 17:20:37 CDT; 2 days ago
 Invocation: cbd6b10dfd9b48708a8a387d99c9f4fa
    Process: 1369 ExecStartPre=/usr/bin/update-alternatives --set ebtables /usr/sbin/ebtables-legacy (code=exited, status=0/SUCCESS)
    Process: 1378 ExecStartPre=/usr/bin/update-alternatives --set iptables /usr/sbin/iptables-legacy (code=exited, status=0/SUCCESS)
    Process: 1379 ExecStartPre=/usr/bin/update-alternatives --set ip6tables /usr/sbin/ip6tables-legacy (code=exited, status=0/SUCCESS)
    Process: 1381 ExecStart=/usr/sbin/pve-firewall start (code=exited, status=0/SUCCESS)
   Main PID: 1491 (pve-firewall)
      Tasks: 1 (limit: 143874)
     Memory: 112M (peak: 133.2M)
        CPU: 36min 25.294s
     CGroup: /system.slice/pve-firewall.service
             └─1491 pve-firewall

Jul 26 17:20:30 pfv-tsys6 systemd[1]: Starting pve-firewall.service - Proxmox VE firewall...
Jul 26 17:20:37 pfv-tsys6 pve-firewall[1491]: starting server
Jul 26 17:20:37 pfv-tsys6 systemd[1]: Started pve-firewall.service - Proxmox VE firewall.
Jul 29 05:09:35 pfv-tsys6 pve-firewall[1491]: firewall update time (5.830 seconds)

● pve-ha-crm.service - PVE Cluster HA Resource Manager Daemon
     Loaded: loaded (/usr/lib/systemd/system/pve-ha-crm.service; enabled; preset: enabled)
     Active: active (running) since Sun 2026-07-26 17:20:41 CDT; 2 days ago
 Invocation: a45e9bc718fe471cb8812f371058b06b
    Process: 1522 ExecStart=/usr/sbin/pve-ha-crm start (code=exited, status=0/SUCCESS)
   Main PID: 1527 (pve-ha-crm)
      Tasks: 1 (limit: 143874)
     Memory: 118.7M (peak: 138M)
        CPU: 21.107s
     CGroup: /system.slice/pve-ha-crm.service
             └─1527 pve-ha-crm

Jul 26 17:20:39 pfv-tsys6 systemd[1]: Starting pve-ha-crm.service - PVE Cluster HA Resource Manager Daemon...
Jul 26 17:20:40 pfv-tsys6 pve-ha-crm[1527]: starting server
Jul 26 17:20:40 pfv-tsys6 pve-ha-crm[1527]: status change startup => wait_for_quorum
Jul 26 17:20:41 pfv-tsys6 systemd[1]: Started pve-ha-crm.service - PVE Cluster HA Resource Manager Daemon.

● pve-ha-lrm.service - PVE Local HA Resource Manager Daemon
     Loaded: loaded (/usr/lib/systemd/system/pve-ha-lrm.service; enabled; preset: enabled)
     Active: active (running) since Sun 2026-07-26 17:20:44 CDT; 2 days ago
 Invocation: 9f02f9ebd30f4b7abf8b01afdc566212
    Process: 1539 ExecStart=/usr/sbin/pve-ha-lrm start (code=exited, status=0/SUCCESS)
   Main PID: 1545 (pve-ha-lrm)
      Tasks: 1 (limit: 143874)
     Memory: 117.4M (peak: 136.5M)
        CPU: 30.994s

--- storage-related service status
    $ systemctl status nfs-kernel-server nfs-server rpcbind rpc-statd zfs-import zfs-mount zfs-target smartd nvme-stat multipathd --no-pager 2>&1 | head -n 80
Unit nfs-kernel-server.service could not be found.
Unit nfs-server.service could not be found.
Unit zfs-target.service could not be found.
Unit nvme-stat.service could not be found.
Unit multipathd.service could not be found.
● rpcbind.service - RPC bind portmap service
     Loaded: loaded (/usr/lib/systemd/system/rpcbind.service; enabled; preset: enabled)
     Active: active (running) since Sun 2026-07-26 17:20:06 CDT; 2 days ago
 Invocation: c7c150a4ea78423ca300cc4b4b2e3100
TriggeredBy: ● rpcbind.socket
       Docs: man:rpcbind(8)
   Main PID: 868 (rpcbind)
      Tasks: 1 (limit: 143874)
     Memory: 616K (peak: 2M)
        CPU: 214ms
     CGroup: /system.slice/rpcbind.service
             └─868 /usr/sbin/rpcbind -f -w

Jul 26 17:20:05 pfv-tsys6 systemd[1]: Starting rpcbind.service - RPC bind portmap service...
Jul 26 17:20:06 pfv-tsys6 systemd[1]: Started rpcbind.service - RPC bind portmap service.

○ rpc-statd.service - NFS status monitor for NFSv2/3 locking.
     Loaded: loaded (/usr/lib/systemd/system/rpc-statd.service; static)
     Active: inactive (dead)
       Docs: man:rpc.statd(8)

○ zfs-import.service
     Loaded: masked (Reason: Unit zfs-import.service is masked.)
     Active: inactive (dead)

● zfs-mount.service - Mount ZFS filesystems
     Loaded: loaded (/usr/lib/systemd/system/zfs-mount.service; enabled; preset: enabled)
     Active: active (exited) since Sun 2026-07-26 17:19:48 CDT; 2 days ago
 Invocation: b08d997c988b4f8f889d900a9953595e
       Docs: man:zfs(8)
    Process: 696 ExecStart=/usr/sbin/zfs mount -a (code=exited, status=0/SUCCESS)
   Main PID: 696 (code=exited, status=0/SUCCESS)
   Mem peak: 1.7M
        CPU: 15ms

Jul 26 17:19:48 pfv-tsys6 systemd[1]: Starting zfs-mount.service - Mount ZFS filesystems...
Jul 26 17:19:48 pfv-tsys6 systemd[1]: Finished zfs-mount.service - Mount ZFS filesystems.

● smartmontools.service - Self Monitoring and Reporting Technology (SMART) Daemon
     Loaded: loaded (/usr/lib/systemd/system/smartmontools.service; enabled; preset: enabled)
     Active: active (running) since Sun 2026-07-26 17:20:10 CDT; 2 days ago
 Invocation: bdb4bd1ac72f4a6980f0372dac77c132
       Docs: man:smartd(8)
             man:smartd.conf(5)
   Main PID: 886 (smartd)
     Status: "Next check of 1 device will start at 05:20:10"
      Tasks: 1 (limit: 143874)
     Memory: 3.5M (peak: 5M)
        CPU: 180ms
     CGroup: /system.slice/smartmontools.service
             └─886 /usr/sbin/smartd -n -q never

Jul 28 17:20:10 pfv-tsys6 smartd[886]: Device: /dev/sda [SAT], SMART Usage Attribute: 194 Temperature_Celsius changed from 116 to 117
Jul 28 18:50:10 pfv-tsys6 smartd[886]: Device: /dev/sda [SAT], SMART Usage Attribute: 194 Temperature_Celsius changed from 117 to 116
Jul 28 19:20:10 pfv-tsys6 smartd[886]: Device: /dev/sda [SAT], SMART Usage Attribute: 194 Temperature_Celsius changed from 116 to 117
Jul 28 20:50:10 pfv-tsys6 smartd[886]: Device: /dev/sda [SAT], SMART Usage Attribute: 194 Temperature_Celsius changed from 117 to 118
Jul 28 21:20:10 pfv-tsys6 smartd[886]: Device: /dev/sda [SAT], SMART Usage Attribute: 194 Temperature_Celsius changed from 118 to 117
Jul 29 00:20:11 pfv-tsys6 smartd[886]: Device: /dev/sda [SAT], SMART Usage Attribute: 194 Temperature_Celsius changed from 117 to 118
Jul 29 00:50:10 pfv-tsys6 smartd[886]: Device: /dev/sda [SAT], SMART Usage Attribute: 194 Temperature_Celsius changed from 118 to 117
Jul 29 01:50:10 pfv-tsys6 smartd[886]: Device: /dev/sda [SAT], SMART Usage Attribute: 194 Temperature_Celsius changed from 117 to 118
Jul 29 03:20:10 pfv-tsys6 smartd[886]: Device: /dev/sda [SAT], SMART Usage Attribute: 194 Temperature_Celsius changed from 118 to 117
Jul 29 03:50:10 pfv-tsys6 smartd[886]: Device: /dev/sda [SAT], SMART Usage Attribute: 194 Temperature_Celsius changed from 117 to 118

###############################################################################
# 25. TIMERS / CRON
###############################################################################

--- systemctl list-timers
    $ systemctl list-timers --all --no-pager
NEXT                          LEFT LAST                              PASSED UNIT                         ACTIVATES
Wed 2026-07-29 05:20:00 CDT   5min Wed 2026-07-29 05:10:10 CDT 4min 29s ago sysstat-collect.timer        sysstat-collect.service
Wed 2026-07-29 06:13:25 CDT  58min Tue 2026-07-28 06:27:10 CDT      22h ago apt-daily-upgrade.timer      apt-daily-upgrade.service
Wed 2026-07-29 15:46:37 CDT    10h Wed 2026-07-29 04:55:08 CDT    19min ago apt-daily.timer              apt-daily.service
Wed 2026-07-29 17:34:47 CDT    12h Tue 2026-07-28 17:34:47 CDT      11h ago systemd-tmpfiles-clean.timer systemd-tmpfiles-clean.service
Thu 2026-07-30 00:00:00 CDT    18h Wed 2026-07-29 00:00:03 CDT 5h 14min ago dpkg-db-backup.timer         dpkg-db-backup.service
Thu 2026-07-30 00:00:00 CDT    18h Wed 2026-07-29 00:00:03 CDT 5h 14min ago sysstat-rotate.timer         sysstat-rotate.service
Thu 2026-07-30 00:07:00 CDT    18h Wed 2026-07-29 00:07:20 CDT  5h 7min ago sysstat-summary.timer        sysstat-summary.service
Thu 2026-07-30 00:12:52 CDT    18h Wed 2026-07-29 03:44:32 CDT 1h 30min ago beszel-agent-update.timer    beszel-agent-update.service
Thu 2026-07-30 00:17:29 CDT    19h Wed 2026-07-29 00:30:07 CDT 4h 44min ago logrotate.timer              logrotate.service
Thu 2026-07-30 02:57:45 CDT    21h Wed 2026-07-29 00:54:36 CDT 4h 20min ago man-db.timer                 man-db.service
Thu 2026-07-30 03:27:53 CDT    22h Wed 2026-07-29 02:42:42 CDT 2h 31min ago pve-daily-update.timer       pve-daily-update.service
Sun 2026-08-02 03:10:33 CDT 3 days Sun 2026-07-26 03:10:43 CDT            - e2scrub_all.timer            e2scrub_all.service
Sun 2026-08-02 03:10:49 CDT 3 days Sun 2026-07-26 03:11:00 CDT            - xfs_scrub_all.timer          xfs_scrub_all.service
Mon 2026-08-03 01:34:59 CDT 4 days Mon 2026-07-27 00:54:07 CDT   2 days ago fstrim.timer                 fstrim.service

14 timers listed.

--- /etc/cron.d
total 24
drwxr-xr-x   2 root root 4096 Jul 26 17:12 .
drwxr-xr-x 107 root root 4096 Jul 29 05:11 ..
-rw-r--r--   1 root root  188 Jul 30  2025 e2scrub_all
-rw-r--r--   1 root root  102 Jun 13  2025 .placeholder
-rw-r--r--   1 root root  400 Jan 15  2024 sysstat
lrwxrwxrwx   1 root root   20 Apr  4 12:47 vzdump -> /etc/pve/vzdump.cron
-rw-r--r--   1 root root  377 Aug 26  2025 zfsutils-linux

--- /etc/cron.daily
total 32
drwxr-xr-x   2 root root 4096 Jul 26 16:27 .
drwxr-xr-x 107 root root 4096 Jul 29 05:11 ..
-rwxr-xr-x   1 root root 1478 Jun 24  2025 apt-compat
-rwxr-xr-x   1 root root  123 May 27  2025 dpkg
-rwxr-xr-x   1 root root  377 Jul 14  2024 logrotate
-rwxr-xr-x   1 root root 1395 May  2  2025 man-db
-rw-r--r--   1 root root  102 Jun 13  2025 .placeholder
-rwxr-xr-x   1 root root  526 Jan 15  2024 sysstat

--- /etc/cron.hourly
total 12
drwxr-xr-x   2 root root 4096 Apr  4 12:31 .
drwxr-xr-x 107 root root 4096 Jul 29 05:11 ..
-rw-r--r--   1 root root  102 Jun 13  2025 .placeholder

--- /etc/cron.weekly
total 16
drwxr-xr-x   2 root root 4096 Apr  4 12:31 .
drwxr-xr-x 107 root root 4096 Jul 29 05:11 ..
-rwxr-xr-x   1 root root 1055 May  2  2025 man-db
-rw-r--r--   1 root root  102 Jun 13  2025 .placeholder

--- crontabs
    --- /etc/crontab ---
# /etc/crontab: system-wide crontab
# Unlike any other crontab you don't have to run the `crontab'
# command to install the new version when you edit this file
# and files in /etc/cron.d. These files also have username fields,
# that none of the other crontabs do.

SHELL=/bin/sh
PATH=/usr/local/sbin:/usr/local/bin:/usr/sbin:/usr/bin:/sbin:/bin

# Example of job definition:
# .---------------- minute (0 - 59)
# |  .------------- hour (0 - 23)
# |  |  .---------- day of month (1 - 31)
# |  |  |  .------- month (1 - 12) OR jan,feb,mar,apr ...
# |  |  |  |  .---- day of week (0 - 6) (Sunday=0 or 7) OR sun,mon,tue,wed,thu,fri,sat
# |  |  |  |  |
# *  *  *  *  * user-name command to be executed
17 *	* * *	root	cd / && run-parts --report /etc/cron.hourly
25 6	* * *	root	test -x /usr/sbin/anacron || { cd / && run-parts --report /etc/cron.daily; }
47 6	* * 7	root	test -x /usr/sbin/anacron || { cd / && run-parts --report /etc/cron.weekly; }
52 6	1 * *	root	test -x /usr/sbin/anacron || { cd / && run-parts --report /etc/cron.monthly; }
#

--- root crontab
    $ crontab -l 2>/dev/null || echo "  [no root crontab]"
  [no root crontab]

###############################################################################
# 26. LIVE PERFORMANCE SNAPSHOT
###############################################################################

--- /proc/loadavg
    $ cat /proc/loadavg
1.39 0.85 0.54 1/428 1081674

--- vmstat 1 3
    $ vmstat 1 3
procs -----------memory---------- ---swap-- -----io---- -system-- -------cpu-------
 r  b   swpd   free   buff  cache   si   so    bi    bo   in   cs us sy id wa st gu
 1  1      0 122726864  16464 1629092    0    0    66   118 1830    1  0  0 97  1  0  1
 0  0      0 122727832  16464 1629132    0    0     0  1220 1712 3398  0  0 99  1  0  0
 0  0      0 122728588  16464 1629132    0    0     0     0  769 1485  0  0 100  0  0  0

--- mpstat 1 3 (per-cpu)
    $ mpstat 1 3
Linux 7.0.14-6-pve (pfv-tsys6) 	07/29/2026 	_x86_64_	(16 CPU)

05:14:42 AM  CPU    %usr   %nice    %sys %iowait    %irq   %soft  %steal  %guest  %gnice   %idle
05:14:43 AM  all    0.44    0.00    0.13    0.00    0.00    0.00    0.00    0.00    0.00   99.44
05:14:44 AM  all    0.81    0.00    1.56    0.06    0.00    0.00    0.00    0.06    0.00   97.44
05:14:45 AM  all    0.56    0.00    0.00    0.31    0.00    0.00    0.00    0.06    0.00   99.00
Average:     all    0.60    0.00    0.56    0.13    0.00    0.00    0.00    0.04    0.00   98.67

--- iostat -xz 1 3
    $ iostat -xz 1 3
Linux 7.0.14-6-pve (pfv-tsys6) 	07/29/2026 	_x86_64_	(16 CPU)

avg-cpu:  %user   %nice %system %iowait  %steal   %idle
           1.08    0.00    0.42    1.41    0.00   97.09

Device            r/s     rkB/s   rrqm/s  %rrqm r_await rareq-sz     w/s     wkB/s   wrqm/s  %wrqm w_await wareq-sz     d/s     dkB/s   drqm/s  %drqm d_await dareq-sz     f/s f_await  aqu-sz  %util
dm-0             0.00      0.01     0.00   0.00   22.80    16.58    0.00      0.00     0.00   0.00    0.00     0.00    0.00      0.00     0.00   0.00    0.00     0.00    0.00    0.00    0.00   0.00
dm-1             0.15     15.83     0.00   0.00   29.85   105.97    9.16    118.47     0.00   0.00    2.76    12.94    0.00      0.00     0.00   0.00    0.00     0.00    0.00    0.00    0.03   1.34
dm-2             0.00      0.04     0.00   0.00   18.73   244.36    0.00      0.00     0.00   0.00    0.00     0.00    0.00      0.00     0.00   0.00    0.00     0.00    0.00    0.00    0.00   0.00
sda              1.00     66.11     0.05   4.68    6.30    65.92    8.13    118.47     1.18  12.67    1.92    14.58    0.00      0.00     0.00   0.00    0.00     0.00    0.00    0.00    0.02   1.17


avg-cpu:  %user   %nice %system %iowait  %steal   %idle
           0.19    0.00    0.06    0.00    0.00   99.75

Device            r/s     rkB/s   rrqm/s  %rrqm r_await rareq-sz     w/s     wkB/s   wrqm/s  %wrqm w_await wareq-sz     d/s     dkB/s   drqm/s  %drqm d_await dareq-sz     f/s f_await  aqu-sz  %util


avg-cpu:  %user   %nice %system %iowait  %steal   %idle
           0.31    0.00    1.19    0.00    0.00   98.50

Device            r/s     rkB/s   rrqm/s  %rrqm r_await rareq-sz     w/s     wkB/s   wrqm/s  %wrqm w_await wareq-sz     d/s     dkB/s   drqm/s  %drqm d_await dareq-sz     f/s f_await  aqu-sz  %util



--- sar -dp 1 2
    $ sar -dp 1 2
Linux 7.0.14-6-pve (pfv-tsys6) 	07/29/2026 	_x86_64_	(16 CPU)

05:14:47 AM       tps     rkB/s     wkB/s     dkB/s   areq-sz    aqu-sz     await     %util DEV
05:14:48 AM      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 sda
05:14:48 AM      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 pve-swap
05:14:48 AM      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 pve-root
05:14:48 AM      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 pve-data_tmeta

05:14:48 AM       tps     rkB/s     wkB/s     dkB/s   areq-sz    aqu-sz     await     %util DEV
05:14:49 AM      8.00     24.00     40.00      0.00      8.00      0.01      0.62      0.40 sda
05:14:49 AM      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 pve-swap
05:14:49 AM     16.00     24.00     40.00      0.00      4.00      0.02      1.38      0.40 pve-root
05:14:49 AM      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 pve-data_tmeta

Average:          tps     rkB/s     wkB/s     dkB/s   areq-sz    aqu-sz     await     %util DEV
Average:         4.00     12.00     20.00      0.00      8.00      0.00      0.62      0.20 sda
Average:         0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 pve-swap
Average:         8.00     12.00     20.00      0.00      4.00      0.01      1.38      0.20 pve-root
Average:         0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00 pve-data_tmeta

--- sar -n DEV 1 2
    $ sar -n DEV 1 2
Linux 7.0.14-6-pve (pfv-tsys6) 	07/29/2026 	_x86_64_	(16 CPU)

05:14:49 AM     IFACE   rxpck/s   txpck/s    rxkB/s    txkB/s   rxcmp/s   txcmp/s  rxmcst/s   %ifutil
05:14:50 AM        lo     15.00     15.00      0.93      0.93      0.00      0.00      0.00      0.00
05:14:50 AM      nic0     43.00     31.00     14.30     12.87      0.00      0.00      3.00      0.01
05:14:50 AM      nic1      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
05:14:50 AM      nic2      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
05:14:50 AM      nic3      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
05:14:50 AM      nic4      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
05:14:50 AM      nic5      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
05:14:50 AM     vmbr0     14.00     11.00      2.61      1.47      0.00      0.00      4.00      0.00
05:14:50 AM tailscale0      5.00     10.00      0.38      0.63      0.00      0.00      0.00      0.00
05:14:50 AM    nic3.2      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
05:14:50 AM br-rr-mgmt      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
05:14:50 AM     bond0      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
05:14:50 AM storagenet      1.00      0.00      0.04      0.00      0.00      0.00      1.00      0.00
05:14:50 AM  tap100i0      0.00      8.00      0.00      1.99      0.00      0.00      0.00      0.00
05:14:50 AM fwbr100i0      8.00      0.00      1.88      0.00      0.00      0.00      4.00      0.00
05:14:50 AM fwpr100p0      0.00      8.00      0.00      1.99      0.00      0.00      0.00      0.00
05:14:50 AM fwln100i0      8.00      0.00      1.99      0.00      0.00      0.00      0.00      0.00
05:14:50 AM  tap600i0      0.00      8.00      0.00      1.99      0.00      0.00      0.00      0.00
05:14:50 AM fwbr600i0      8.00      0.00      1.88      0.00      0.00      0.00      4.00      0.00
05:14:50 AM fwpr600p0      0.00      8.00      0.00      1.99      0.00      0.00      0.00      0.00
05:14:50 AM fwln600i0      8.00      0.00      1.99      0.00      0.00      0.00      0.00      0.00
05:14:50 AM  tap601i0      0.00      9.00      0.00      2.16      0.00      0.00      0.00      0.00
05:14:50 AM fwbr601i0      8.00      0.00      1.88      0.00      0.00      0.00      4.00      0.00
05:14:50 AM fwpr601p0      0.00      9.00      0.00      2.16      0.00      0.00      0.00      0.00
05:14:50 AM fwln601i0      9.00      0.00      2.16      0.00      0.00      0.00      0.00      0.00

05:14:50 AM     IFACE   rxpck/s   txpck/s    rxkB/s    txkB/s   rxcmp/s   txcmp/s  rxmcst/s   %ifutil
05:14:51 AM        lo     25.00     25.00      3.44      3.44      0.00      0.00      0.00      0.00
05:14:51 AM      nic0     18.00     15.00      2.51      2.50      0.00      0.00      2.00      0.00
05:14:51 AM      nic1      1.00      0.00      0.06      0.00      0.00      0.00      1.00      0.00
05:14:51 AM      nic2      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
05:14:51 AM      nic3      2.00      0.00      0.12      0.00      0.00      0.00      2.00      0.00
05:14:51 AM      nic4      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
05:14:51 AM      nic5      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
05:14:51 AM     vmbr0     27.00     24.00      4.05      4.44      0.00      0.00      3.00      0.00
05:14:51 AM tailscale0     11.00     17.00      1.75      2.10      0.00      0.00      0.00      0.00
05:14:51 AM    nic3.2      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
05:14:51 AM br-rr-mgmt      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
05:14:51 AM     bond0      1.00      0.00      0.06      0.00      0.00      0.00      1.00      0.00
05:14:51 AM storagenet      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
05:14:51 AM  tap100i0      0.00     10.00      0.00      0.86      0.00      0.00      0.00      0.00
05:14:51 AM fwbr100i0     10.00      0.00      0.73      0.00      0.00      0.00      3.00      0.00
05:14:51 AM fwpr100p0      0.00     10.00      0.00      0.86      0.00      0.00      0.00      0.00
05:14:51 AM fwln100i0     10.00      0.00      0.86      0.00      0.00      0.00      0.00      0.00
05:14:51 AM  tap600i0      0.00     10.00      0.00      0.86      0.00      0.00      0.00      0.00
05:14:51 AM fwbr600i0     10.00      0.00      0.73      0.00      0.00      0.00      3.00      0.00
05:14:51 AM fwpr600p0      0.00     10.00      0.00      0.86      0.00      0.00      0.00      0.00
05:14:51 AM fwln600i0     10.00      0.00      0.86      0.00      0.00      0.00      0.00      0.00
05:14:51 AM  tap601i0      3.00     14.00      0.58      1.19      0.00      0.00      0.00      0.00
05:14:51 AM fwbr601i0     10.00      0.00      0.73      0.00      0.00      0.00      3.00      0.00
05:14:51 AM fwpr601p0      3.00     14.00      0.58      1.19      0.00      0.00      0.00      0.00
05:14:51 AM fwln601i0     14.00      3.00      1.19      0.58      0.00      0.00      0.00      0.00

Average:        IFACE   rxpck/s   txpck/s    rxkB/s    txkB/s   rxcmp/s   txcmp/s  rxmcst/s   %ifutil
Average:           lo     20.00     20.00      2.19      2.19      0.00      0.00      0.00      0.00
Average:         nic0     30.50     23.00      8.41      7.68      0.00      0.00      2.50      0.01
Average:         nic1      0.50      0.00      0.03      0.00      0.00      0.00      0.50      0.00
Average:         nic2      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
Average:         nic3      1.00      0.00      0.06      0.00      0.00      0.00      1.00      0.00
Average:         nic4      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
Average:         nic5      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
Average:        vmbr0     20.50     17.50      3.33      2.95      0.00      0.00      3.50      0.00
Average:    tailscale0      8.00     13.50      1.06      1.37      0.00      0.00      0.00      0.00
Average:       nic3.2      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
Average:    br-rr-mgmt      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00
Average:        bond0      0.50      0.00      0.03      0.00      0.00      0.00      0.50      0.00
Average:    storagenet      0.50      0.00      0.02      0.00      0.00      0.00      0.50      0.00
Average:     tap100i0      0.00      9.00      0.00      1.43      0.00      0.00      0.00      0.00
Average:    fwbr100i0      9.00      0.00      1.31      0.00      0.00      0.00      3.50      0.00
Average:    fwpr100p0      0.00      9.00      0.00      1.43      0.00      0.00      0.00      0.00
Average:    fwln100i0      9.00      0.00      1.43      0.00      0.00      0.00      0.00      0.00
Average:     tap600i0      0.00      9.00      0.00      1.43      0.00      0.00      0.00      0.00
Average:    fwbr600i0      9.00      0.00      1.31      0.00      0.00      0.00      3.50      0.00
Average:    fwpr600p0      0.00      9.00      0.00      1.43      0.00      0.00      0.00      0.00
Average:    fwln600i0      9.00      0.00      1.43      0.00      0.00      0.00      0.00      0.00
Average:     tap601i0      1.50     11.50      0.29      1.67      0.00      0.00      0.00      0.00
Average:    fwbr601i0      9.00      0.00      1.31      0.00      0.00      0.00      3.50      0.00
Average:    fwpr601p0      1.50     11.50      0.29      1.67      0.00      0.00      0.00      0.00
Average:    fwln601i0     11.50      1.50      1.67      0.29      0.00      0.00      0.00      0.00

--- sar -n NFS,NFSD 1 2
    $ sar -n NFS,NFSD 1 2
Linux 7.0.14-6-pve (pfv-tsys6) 	07/29/2026 	_x86_64_	(16 CPU)

05:14:51 AM    call/s retrans/s    read/s   write/s  access/s  getatt/s
05:14:52 AM      2.00      0.00      0.00      2.00      0.00      0.00

05:14:51 AM   scall/s badcall/s  packet/s     udp/s     tcp/s     hit/s    miss/s   sread/s  swrite/s saccess/s sgetatt/s
05:14:52 AM      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00

05:14:52 AM    call/s retrans/s    read/s   write/s  access/s  getatt/s
05:14:53 AM      1.00      0.00      0.00      1.00      0.00      0.00

05:14:52 AM   scall/s badcall/s  packet/s     udp/s     tcp/s     hit/s    miss/s   sread/s  swrite/s saccess/s sgetatt/s
05:14:53 AM      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00

Average:       call/s retrans/s    read/s   write/s  access/s  getatt/s
Average:         1.50      0.00      0.00      1.50      0.00      0.00

Average:      scall/s badcall/s  packet/s     udp/s     tcp/s     hit/s    miss/s   sread/s  swrite/s saccess/s sgetatt/s
Average:         0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00      0.00

--- sar -n SOCK 1 1
    $ sar -n SOCK 1 1
Linux 7.0.14-6-pve (pfv-tsys6) 	07/29/2026 	_x86_64_	(16 CPU)

05:14:53 AM    totsck    tcpsck    udpsck    rawsck   ip-frag    tcp-tw
05:14:54 AM       368        21         4         0         0       152
Average:          368        21         4         0         0       152

--- sar -n TCP,ETCP 1 2
    $ sar -n TCP,ETCP 1 2
Linux 7.0.14-6-pve (pfv-tsys6) 	07/29/2026 	_x86_64_	(16 CPU)

05:14:54 AM  active/s passive/s    iseg/s    oseg/s
05:14:55 AM      5.00      1.00     54.00     69.00

05:14:54 AM  atmptf/s  estres/s retrans/s isegerr/s   orsts/s
05:14:55 AM      0.00      0.00      0.00      0.00      0.00

05:14:55 AM  active/s passive/s    iseg/s    oseg/s
05:14:56 AM      0.00      2.00     36.00     40.00

05:14:55 AM  atmptf/s  estres/s retrans/s isegerr/s   orsts/s
05:14:56 AM      0.00      0.00      0.00      0.00      0.00

Average:     active/s passive/s    iseg/s    oseg/s
Average:         2.50      1.50     45.00     54.50

Average:     atmptf/s  estres/s retrans/s isegerr/s   orsts/s
Average:         0.00      0.00      0.00      0.00      0.00

--- pidstat -d 1 2 (top disk)
    $ pidstat -d 1 2
Linux 7.0.14-6-pve (pfv-tsys6) 	07/29/2026 	_x86_64_	(16 CPU)

05:14:56 AM   UID       PID   kB_rd/s   kB_wr/s kB_ccwr/s iodelay  Command
05:14:57 AM     0       456      0.00     97.09      0.00       0  systemd-journal
05:14:57 AM     0       895      0.00      0.00      3.88       0  tailscaled
05:14:57 AM     0    283674      0.00      7.77      0.00       0  kvm

05:14:57 AM   UID       PID   kB_rd/s   kB_wr/s kB_ccwr/s iodelay  Command
05:14:58 AM     0       456      0.00     96.00      0.00       0  systemd-journal
05:14:58 AM     0    283519      0.00    204.00      0.00       0  kvm
05:14:58 AM     0   1081769      0.00      4.00      0.00       0  pidstat

Average:      UID       PID   kB_rd/s   kB_wr/s kB_ccwr/s iodelay  Command
Average:        0       456      0.00     96.55      0.00       0  systemd-journal
Average:        0       895      0.00      0.00      1.97       0  tailscaled
Average:        0    283519      0.00    100.49      0.00       0  kvm
Average:        0    283674      0.00      3.94      0.00       0  kvm
Average:        0   1081769      0.00      1.97      0.00       0  pidstat

--- pidstat -u 1 2 (top cpu)
    $ pidstat -u 1 2
Linux 7.0.14-6-pve (pfv-tsys6) 	07/29/2026 	_x86_64_	(16 CPU)

05:14:58 AM   UID       PID    %usr %system  %guest   %wait    %CPU   CPU  Command
05:14:59 AM     0       895    0.98    0.00    0.00    0.00    0.98     5  tailscaled
05:14:59 AM     0    283375    1.96    0.00    0.00    0.00    1.96    13  kvm
05:14:59 AM     0    283519    0.98    0.00    0.00    0.00    0.98    10  kvm
05:14:59 AM     0    283674    0.98    0.00    0.00    0.00    0.98    14  kvm
05:14:59 AM     0    949449    0.98    0.00    0.00    0.00    0.98    15  pvedaemon worke
05:14:59 AM    33    993541    0.98    0.00    0.00    0.00    0.98     2  pveproxy worker
05:14:59 AM     0   1081777    0.98    0.98    0.00    0.00    1.96    15  pidstat

05:14:59 AM   UID       PID    %usr %system  %guest   %wait    %CPU   CPU  Command
05:15:00 AM     0       895    1.00    1.00    0.00    0.00    2.00     5  tailscaled
05:15:00 AM     0      1491    2.00    3.00    0.00    0.00    5.00     8  pve-firewall
05:15:00 AM     0    283375    0.00    1.00    0.00    0.00    1.00    15  kvm
05:15:00 AM     0    283519    0.00    0.00    2.00    0.00    1.00    10  kvm
05:15:00 AM     0    283674    0.00    0.00    1.00    0.00    1.00    14  kvm
05:15:00 AM    33    993542    1.00    0.00    0.00    0.00    1.00    13  pveproxy worker
05:15:00 AM     0   1081777    1.00    1.00    0.00    0.00    2.00    15  pidstat

Average:      UID       PID    %usr %system  %guest   %wait    %CPU   CPU  Command
Average:        0       895    0.99    0.50    0.00    0.00    1.49     -  tailscaled
Average:        0      1491    0.99    1.49    0.00    0.00    2.48     -  pve-firewall
Average:        0    283375    0.99    0.50    0.00    0.00    1.49     -  kvm
Average:        0    283519    0.00    0.00    0.99    0.00    0.99     -  kvm
Average:        0    283674    0.50    0.00    0.50    0.00    0.99     -  kvm
Average:        0    949449    0.50    0.00    0.00    0.00    0.50     -  pvedaemon worke
Average:       33    993541    0.50    0.00    0.00    0.00    0.50     -  pveproxy worker
Average:       33    993542    0.50    0.00    0.00    0.00    0.50     -  pveproxy worker
Average:        0   1081777    0.99    0.99    0.00    0.00    1.98     -  pidstat

--- top (single snapshot, top 30)
    $ top -b -n 1
top - 05:15:00 up 2 days, 11:55,  1 user,  load average: 1.13, 0.83, 0.54
Tasks: 326 total,   1 running, 325 sleeping,   0 stopped,   0 zombie
%Cpu(s):  0.3 us,  0.3 sy,  0.0 ni, 90.4 id,  9.0 wa,  0.0 hi,  0.0 si,  0.0 st 
MiB Mem : 128897.5 total, 119855.5 free,   8179.1 used,   1607.6 buff/cache     
MiB Swap:   8192.0 total,   8192.0 free,      0.0 used. 120718.5 avail Mem 

    PID USER      PR  NI    VIRT    RES    SHR S  %CPU  %MEM     TIME+ COMMAND
 283519 root      20   0   12.5g   1.0g  11748 S   9.1   0.8  36:44.42 kvm
1081797 root      20   0   10424   5508   3408 R   9.1   0.0   0:00.02 top
      1 root      20   0   24752  15432  10688 S   0.0   0.0   0:27.53 systemd
      2 root      20   0       0      0      0 S   0.0   0.0   0:00.40 kthreadd
      3 root      20   0       0      0      0 S   0.0   0.0   0:00.00 pool_wo+
      4 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
      5 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
      6 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
      7 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
      8 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     10 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     13 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     14 root      20   0       0      0      0 S   0.0   0.0   0:07.54 ksoftir+
     15 root      20   0       0      0      0 I   0.0   0.0   1:08.46 rcu_pre+
     16 root      20   0       0      0      0 S   0.0   0.0   0:00.00 rcu_exp+
     17 root      20   0       0      0      0 S   0.0   0.0   0:00.00 rcu_exp+
     18 root      rt   0       0      0      0 S   0.0   0.0   0:00.50 migrati+
     19 root      20   0       0      0      0 S   0.0   0.0   0:00.00 kprobe-+
     20 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 idle_in+
     21 root      20   0       0      0      0 S   0.0   0.0   0:00.00 cpuhp/0
     22 root      20   0       0      0      0 S   0.0   0.0   0:00.00 cpuhp/1
     23 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 idle_in+
     24 root      rt   0       0      0      0 S   0.0   0.0   0:00.51 migrati+
     25 root      20   0       0      0      0 S   0.0   0.0   0:01.23 ksoftir+
     27 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     28 root      20   0       0      0      0 S   0.0   0.0   0:00.00 cpuhp/2
     29 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 idle_in+
     30 root      rt   0       0      0      0 S   0.0   0.0   0:00.44 migrati+
     31 root      20   0       0      0      0 S   0.0   0.0   0:04.13 ksoftir+
     33 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     34 root      20   0       0      0      0 S   0.0   0.0   0:00.00 cpuhp/3
     35 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 idle_in+
     36 root      rt   0       0      0      0 S   0.0   0.0   0:00.51 migrati+
     37 root      20   0       0      0      0 S   0.0   0.0   0:00.19 ksoftir+
     39 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     40 root      20   0       0      0      0 S   0.0   0.0   0:00.00 cpuhp/4
     41 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 idle_in+
     42 root      rt   0       0      0      0 S   0.0   0.0   0:00.44 migrati+
     43 root      20   0       0      0      0 S   0.0   0.0   0:00.08 ksoftir+
     45 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     46 root      20   0       0      0      0 S   0.0   0.0   0:00.00 cpuhp/5
     47 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 idle_in+
     48 root      rt   0       0      0      0 S   0.0   0.0   0:00.48 migrati+
     49 root      20   0       0      0      0 S   0.0   0.0   0:00.08 ksoftir+
     51 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     52 root      20   0       0      0      0 S   0.0   0.0   0:00.00 cpuhp/6
     53 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 idle_in+
     54 root      rt   0       0      0      0 S   0.0   0.0   0:00.44 migrati+
     55 root      20   0       0      0      0 S   0.0   0.0   0:00.07 ksoftir+
     57 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     58 root      20   0       0      0      0 S   0.0   0.0   0:00.00 cpuhp/7
     59 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 idle_in+
     60 root      rt   0       0      0      0 S   0.0   0.0   0:00.47 migrati+
     61 root      20   0       0      0      0 S   0.0   0.0   0:00.15 ksoftir+
     63 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     64 root      20   0       0      0      0 S   0.0   0.0   0:00.00 cpuhp/8
     65 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 idle_in+
     66 root      rt   0       0      0      0 S   0.0   0.0   0:00.41 migrati+
     67 root      20   0       0      0      0 S   0.0   0.0   0:00.07 ksoftir+
     69 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     70 root      20   0       0      0      0 S   0.0   0.0   0:00.00 cpuhp/9
     71 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 idle_in+
     72 root      rt   0       0      0      0 S   0.0   0.0   0:00.42 migrati+
     73 root      20   0       0      0      0 S   0.0   0.0   0:00.08 ksoftir+
     75 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     76 root      20   0       0      0      0 S   0.0   0.0   0:00.00 cpuhp/10
     77 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 idle_in+
     78 root      rt   0       0      0      0 S   0.0   0.0   0:00.42 migrati+
     79 root      20   0       0      0      0 S   0.0   0.0   0:00.12 ksoftir+
     81 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     82 root      20   0       0      0      0 S   0.0   0.0   0:00.00 cpuhp/11
     83 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 idle_in+
     84 root      rt   0       0      0      0 S   0.0   0.0   0:00.43 migrati+
     85 root      20   0       0      0      0 S   0.0   0.0   0:00.09 ksoftir+
     87 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     88 root      20   0       0      0      0 S   0.0   0.0   0:00.00 cpuhp/12
     89 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 idle_in+
     90 root      rt   0       0      0      0 S   0.0   0.0   0:00.42 migrati+
     91 root      20   0       0      0      0 S   0.0   0.0   0:00.64 ksoftir+
     93 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
     94 root      20   0       0      0      0 S   0.0   0.0   0:00.00 cpuhp/13
     95 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 idle_in+
     96 root      rt   0       0      0      0 S   0.0   0.0   0:00.42 migrati+
     97 root      20   0       0      0      0 S   0.0   0.0   0:00.08 ksoftir+
     99 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    100 root      20   0       0      0      0 S   0.0   0.0   0:00.00 cpuhp/14
    101 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 idle_in+
    102 root      rt   0       0      0      0 S   0.0   0.0   0:00.41 migrati+
    103 root      20   0       0      0      0 S   0.0   0.0   0:00.05 ksoftir+
    105 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    106 root      20   0       0      0      0 S   0.0   0.0   0:00.00 cpuhp/15
    107 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 idle_in+
    108 root      rt   0       0      0      0 S   0.0   0.0   0:00.42 migrati+
    109 root      20   0       0      0      0 S   0.0   0.0   0:00.28 ksoftir+
    111 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    114 root      20   0       0      0      0 S   0.0   0.0   0:00.00 kdevtmp+
    115 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    116 root      20   0       0      0      0 I   0.0   0.0   0:00.00 rcu_tas+
    117 root      20   0       0      0      0 I   0.0   0.0   0:00.00 rcu_tas+
    118 root      20   0       0      0      0 S   0.0   0.0   0:00.03 kauditd
    119 root      20   0       0      0      0 S   0.0   0.0   0:00.14 khungta+
    120 root      20   0       0      0      0 S   0.0   0.0   0:00.00 oom_rea+
    123 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    124 root      20   0       0      0      0 S   0.0   0.0   0:03.49 kcompac+
    125 root      20   0       0      0      0 S   0.0   0.0   0:03.78 kcompac+
    127 root      25   5       0      0      0 S   0.0   0.0   0:00.00 ksmd
    128 root      39  19       0      0      0 S   0.0   0.0   0:01.15 khugepa+
    129 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    130 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    131 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    132 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 irq/9-a+
    135 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    136 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    137 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    138 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    139 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    140 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    141 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    143 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 watchdo+
    144 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    145 root      20   0       0      0      0 S   0.0   0.0   0:00.00 kswapd0
    146 root      20   0       0      0      0 S   0.0   0.0   0:00.00 kswapd1
    147 root      20   0       0      0      0 S   0.0   0.0   0:00.00 ecryptf+
    148 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    149 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 irq/25-+
    150 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 irq/26-+
    151 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 irq/27-+
    152 root     -51   0       0      0      0 S   0.0   0.0   0:00.00 irq/28-+
    153 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    154 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    155 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    157 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    168 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    170 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    171 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    183 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    184 root       0 -20       0      0      0 I   0.0   0.0   0:00.40 kworker+
    193 root       0 -20       0      0      0 I   0.0   0.0   0:01.26 kworker+
    205 root       0 -20       0      0      0 I   0.0   0.0   0:00.50 kworker+
    218 root       0 -20       0      0      0 I   0.0   0.0   0:00.52 kworker+
    222 root       0 -20       0      0      0 I   0.0   0.0   0:00.91 kworker+
    230 root       0 -20       0      0      0 I   0.0   0.0   0:04.57 kworker+
    232 root       0 -20       0      0      0 I   0.0   0.0   0:00.55 kworker+
    234 root       0 -20       0      0      0 I   0.0   0.0   0:00.44 kworker+
    239 root       0 -20       0      0      0 I   0.0   0.0   0:00.53 kworker+
    248 root       0 -20       0      0      0 I   0.0   0.0   0:02.08 kworker+
    253 root       0 -20       0      0      0 I   0.0   0.0   0:00.52 kworker+
    259 root       0 -20       0      0      0 I   0.0   0.0   0:00.46 kworker+
    261 root       0 -20       0      0      0 I   0.0   0.0   0:01.34 kworker+
    264 root       0 -20       0      0      0 I   0.0   0.0   0:00.75 kworker+
    265 root       0 -20       0      0      0 I   0.0   0.0   0:05.55 kworker+
    269 root       0 -20       0      0      0 I   0.0   0.0   0:00.60 kworker+
    297 root      20   0       0      0      0 S   0.0   0.0   0:00.00 scsi_eh+
    298 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    299 root      20   0       0      0      0 S   0.0   0.0   1:19.67 usb-sto+
    300 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    341 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    342 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    352 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    353 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    354 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    390 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    391 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    392 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    407 root      20   0       0      0      0 S   0.0   0.0   0:05.93 jbd2/dm+
    408 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    438 root      -2   0       0      0      0 S   0.0   0.0   0:00.00 psimon
    456 root      20   0  108544  80624  79000 S   0.0   0.1   1:38.12 systemd+
    477 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    478 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    479 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    480 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    504 root       0 -20       0      0      0 S   0.0   0.0   0:00.00 spl_sys+
    505 root       0 -20       0      0      0 S   0.0   0.0   0:00.00 spl_del+
    506 root       0 -20       0      0      0 S   0.0   0.0   0:00.00 spl_dyn+
    507 root       0 -20       0      0      0 S   0.0   0.0   0:00.00 spl_kme+
    511 root      20   0   36972  10496   7944 S   0.0   0.0   1:55.52 systemd+
    514 root      20   0   77296  22300   9124 S   0.0   0.0   0:08.56 dmeventd
    517 root       0 -20       0      0      0 S   0.0   0.0   0:00.00 zvol_tq+
    518 root       0 -20       0      0      0 S   0.0   0.0   0:00.00 zvol_tq+
    519 root       0 -20       0      0      0 S   0.0   0.0   0:00.00 zvol_tq+
    521 root      20   0       0      0      0 S   0.0   0.0   0:00.00 arc_pru+
    522 root      20   0       0      0      0 S   0.0   0.0   0:00.00 arc_evi+
    523 root      20   0       0      0      0 S   0.0   0.0   0:00.00 arc_evi+
    524 root      20   0       0      0      0 S   0.0   0.0   0:00.00 arc_evi+
    525 root      20   0       0      0      0 S   0.0   0.0   0:00.00 arc_evi+
    526 root      20   0       0      0      0 S   0.0   0.0   0:00.00 arc_flu+
    527 root      20   0       0      0      0 S   0.0   0.0   0:02.33 arc_evi+
    528 root      39  19       0      0      0 S   0.0   0.0   0:02.45 arc_reap
    529 root      20   0       0      0      0 S   0.0   0.0   0:00.00 dbu_evi+
    530 root      39  19       0      0      0 S   0.0   0.0   0:02.36 dbuf_ev+
    531 root      39  19       0      0      0 S   0.0   0.0   0:00.00 z_vdev_+
    532 root      20   0       0      0      0 S   0.0   0.0   0:01.93 l2arc_f+
    538 root      -2   0       0      0      0 S   0.0   0.0   0:00.00 psimon
    635 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    638 root      39  19       0      0      0 S   0.0   0.0   0:00.00 kipmi0
    843 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    868 _rpc      20   0    6568   3792   3372 S   0.0   0.0   0:00.21 rpcbind
    870 _chrony   20   0   19940   5568   4796 S   0.0   0.0   0:00.40 chronyd
    871 message+  20   0    8476   5192   4232 S   0.0   0.0   0:20.94 dbus-da+
    879 root      20   0  276136   3592   3300 S   0.0   0.0   0:00.00 pve-lxc+
    882 root      20   0  691580   8324   6976 S   0.0   0.0   0:27.80 rrdcach+
    886 root      20   0   10080   6348   4896 S   0.0   0.0   0:00.17 smartd
    888 root      20   0   19100   9256   7884 S   0.0   0.0   0:05.35 systemd+
    895 root      20   0 1489496 119720  26684 S   0.0   0.1  16:10.89 tailsca+
    899 root      20   0    7216   2268   1928 S   0.0   0.0   0:04.76 ksmtuned
    901 root      20   0    2432   1656   1560 S   0.0   0.0   0:05.13 watchdo+
    904 root      20   0  104420   6416   5268 S   0.0   0.0   0:00.01 zed
    908 root      20   0  159036   2472   2108 S   0.0   0.0   0:00.00 lxcfs
    917 root      20   0    5748   2192   1996 S   0.0   0.0   0:00.07 qmeventd
    935 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    936 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
    939 root      20   0    5264   1696   1472 S   0.0   0.0   0:00.00 blkmapd
    974 _chrony   20   0   11612   2356   1724 S   0.0   0.0   0:00.00 chronyd
   1073 root      20   0    5972   3504   2652 S   0.0   0.0   0:01.74 dhclient
   1137 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
   1200 beszel    20   0 2600728  19588  10328 S   0.0   0.0   0:50.80 beszel-+
   1201 _lldpd    20   0   21376   6620   5456 S   0.0   0.0   0:00.15 lldpd
   1202 root      20   0    5520   2696   2444 S   0.0   0.0   0:00.00 lxc-mon+
   1210 root      20   0  266308  32432  15160 S   0.0   0.0   0:33.52 tuned
   1265 root      20   0    8168   2584   2352 S   0.0   0.0   0:00.13 agetty
   1270 root      20   0   11776   7812   6584 S   0.0   0.0   0:00.40 sshd
   1305 _lldpd    20   0   21504   2924   1736 S   0.0   0.0   0:07.03 lldpd
   1317 root      20   0  566052  67644  54376 S   0.0   0.1   2:36.40 pmxcfs
   1366 root      20   0    6864   2964   2712 S   0.0   0.0   0:00.48 cron
   1367 root      20   0   13584   6172   5220 S   0.0   0.0   0:19.94 proxmox+
   1467 root      20   0   43984   4832   4192 S   0.0   0.0   0:00.68 master
   1470 postfix   20   0   44524   7668   6972 S   0.0   0.0   0:00.13 qmgr
   1473 polkitd   20   0  306704   8284   7120 S   0.0   0.0   0:04.36 polkitd
   1491 root      20   0  186484 113080   7580 S   0.0   0.1  13:49.92 pve-fir+
   1505 root      20   0  195384 126224  13192 S   0.0   0.1  52:52.19 pvestatd
   1517 root      20   0  230000 153740   3520 S   0.0   0.1   0:03.35 pvedaem+
   1527 root      20   0  214120 126348   6088 S   0.0   0.1   0:19.51 pve-ha-+
   1532 www-data  20   0  231224 184156  32740 S   0.0   0.1   0:09.53 pveproxy
   1542 www-data  20   0   99256  69716  17660 S   0.0   0.1   0:04.92 spicepr+
   1545 root      20   0  213260 125320   6076 S   0.0   0.1   0:29.41 pve-ha-+
   1635 root       0 -20       0      0      0 I   0.0   0.0   0:00.00 kworker+
   1641 root      20   0       0      0      0 I   0.0   0.0   0:00.00 NFSv4 c+
   1762 root      20   0  209836 126496   3408 S   0.0   0.1   0:21.60 pvesche+
  24133 root      20   0       0      0      0 I   0.0   0.0   3:54.25 kworker+
  40835 root      20   0       0      0      0 I   0.0   0.0   3:34.91 kworker+
  52844 root      20   0       0      0      0 I   0.0   0.0   2:57.13 kworker+
 283375 root      20   0   32.2g   1.2g  13888 S   0.0   1.0  24:07.04 kvm
 283460 root      20   0       0      0      0 S   0.0   0.0   0:00.00 kvm-pit+
 283606 root      20   0       0      0      0 S   0.0   0.0   0:00.00 kvm-pit+
 283674 root      20   0 6680312   3.0g  13920 S   0.0   2.4  54:48.83 kvm
 283747 root      20   0       0      0      0 S   0.0   0.0   0:00.00 kvm-pit+
 747044 root      20   0       0      0      0 I   0.0   0.0   1:00.67 kworker+
 752544 root      20   0       0      0      0 I   0.0   0.0   0:57.68 kworker+
 879149 root      20   0       0      0      0 I   0.0   0.0   0:45.73 kworker+
 888175 root      20   0       0      0      0 I   0.0   0.0   1:09.30 kworker+
 910274 root      20   0       0      0      0 I   0.0   0.0   0:41.94 kworker+
 919447 root      20   0       0      0      0 I   0.0   0.0   0:01.41 kworker+
 936701 root      20   0       0      0      0 I   0.0   0.0   0:17.04 kworker+
 947600 root      20   0  239060 165740  13700 S   0.0   0.1   0:06.65 pvedaem+
 949449 root      20   0  239132 166252  14092 S   0.0   0.1   0:05.55 pvedaem+
 949846 root      20   0  238900 163588  11616 S   0.0   0.1   0:05.02 pvedaem+
 955595 root      20   0       0      0      0 I   0.0   0.0   0:01.01 kworker+
 960613 root      20   0       0      0      0 I   0.0   0.0   0:01.11 kworker+
 975521 root      20   0       0      0      0 I   0.0   0.0   0:21.12 kworker+
 991061 root      20   0       0      0      0 I   0.0   0.0   0:00.87 kworker+
 993531 root      20   0       0      0      0 I   0.0   0.0   0:25.14 kworker+
 993532 root      20   0   79620   2500   2292 S   0.0   0.0   0:01.19 pvefw-l+
 993539 www-data  20   0   99360  56212   4012 S   0.0   0.0   0:00.54 spicepr+
 993540 www-data  20   0  254324 183964  16544 S   0.0   0.1   0:09.40 pveprox+
 993541 www-data  20   0  291516 221612  21048 S   0.0   0.2   0:08.93 pveprox+
 993542 www-data  20   0  252064 179512  14432 S   0.0   0.1   0:06.58 pveprox+
1002498 root      20   0       0      0      0 I   0.0   0.0   0:17.25 kworker+
1011478 root      20   0       0      0      0 I   0.0   0.0   0:18.58 kworker+
1017484 root      20   0       0      0      0 I   0.0   0.0   0:13.89 kworker+
1018807 root      20   0       0      0      0 I   0.0   0.0   0:00.60 kworker+
1020956 root      20   0       0      0      0 I   0.0   0.0   0:00.90 kworker+
1023418 root      20   0       0      0      0 I   0.0   0.0   0:10.37 kworker+
1028889 root      20   0       0      0      0 I   0.0   0.0   0:00.46 kworker+
1048087 root      20   0       0      0      0 I   0.0   0.0   0:00.42 kworker+
1051155 postfix   20   0   44472   7844   7136 S   0.0   0.0   0:00.01 pickup
1053213 root      20   0       0      0      0 I   0.0   0.0   0:00.37 kworker+
1054976 root      20   0       0      0      0 I   0.0   0.0   0:00.22 kworker+
1056402 root      20   0       0      0      0 I   0.0   0.0   0:04.65 kworker+
1058367 root      20   0       0      0      0 I   0.0   0.0   0:00.25 kworker+
1064382 root      20   0       0      0      0 I   0.0   0.0   0:00.33 kworker+
1067095 root      20   0       0      0      0 I   0.0   0.0   0:00.11 kworker+
1068733 root      20   0       0      0      0 I   0.0   0.0   0:00.09 kworker+
1070040 root      20   0       0      0      0 I   0.0   0.0   0:00.08 kworker+
1070427 root      20   0       0      0      0 I   0.0   0.0   0:00.23 kworker+
1070866 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1071326 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1071523 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1071886 root      20   0       0      0      0 I   0.0   0.0   0:00.02 kworker+
1073219 root      20   0  238868 156304   4396 S   0.0   0.1   0:00.05 task UP+
1073221 root      20   0  204012 152376  32680 S   0.0   0.1   0:02.28 qm
1073534 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1073828 root      20   0       0      0      0 I   0.0   0.0   0:00.71 kworker+
1073925 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1074662 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1074854 root      20   0       0      0      0 I   0.0   0.0   0:02.61 kworker+
1074857 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1075055 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1075727 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1075854 root      20   0       0      0      0 I   0.0   0.0   0:00.03 kworker+
1076345 root      20   0       0      0      0 I   0.0   0.0   0:00.35 kworker+
1076447 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1076592 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1076805 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1076901 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1077101 root      20   0   22236  12608  10208 S   0.0   0.0   0:00.34 systemd
1077104 root      20   0   24404   3832   2036 S   0.0   0.0   0:00.00 (sd-pam)
1077109 root      -2   0       0      0      0 S   0.0   0.0   0:00.00 psimon
1077151 root      20   0   19648  11668   9896 S   0.0   0.0   0:00.01 sshd-se+
1077158 root      20   0   19904   7488   5444 S   0.0   0.0   0:00.00 sshd-se+
1077159 root      20   0    7316   3728   3192 S   0.0   0.0   0:00.69 bash
1077183 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1078216 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1079460 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1079512 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1079809 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1079969 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1080024 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1080070 root      20   0       0      0      0 I   0.0   0.0   0:00.01 kworker+
1080102 root      20   0       0      0      0 I   0.0   0.0   0:00.01 kworker+
1081400 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1081591 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1081641 root      20   0       0      0      0 I   0.0   0.0   0:00.00 kworker+
1081733 root      20   0    5580   2216   2100 S   0.0   0.0   0:00.00 sleep
1081795 root      20   0    7316   2328   1792 S   0.0   0.0   0:00.00 bash
1081796 root      20   0    5588   2196   2080 S   0.0   0.0   0:00.00 head

--- zpool iostat 1 2
    $ zpool iostat 1 2
no pools available
no pools available

--- arcstat 1 2
    $ arcstat 1 2
    time  read  ddread  ddh%  dmread  dmh%  pread  ph%   size      c  avail
05:15:01     0       0     0       0     0      0    0   3.8K   3.9G   113G
05:15:02     0       0     0       0     0      0    0   3.8K   3.9G   113G

--- /proc/net/dev delta (1s)
    $ awk '{print $1}' /proc/net/dev
echo "--- t0 ---"
cat /proc/net/dev
sleep 1
echo "--- t1 (1s later) ---"
cat /proc/net/dev
Inter-|
face
lo:
nic0:
nic1:
nic2:
nic3:
nic4:
nic5:
vmbr0:
tailscale0:
nic3.2:
br-rr-mgmt:
bond0:
storagenet:
tap100i0:
fwbr100i0:
fwpr100p0:
fwln100i0:
tap600i0:
fwbr600i0:
fwpr600p0:
fwln600i0:
tap601i0:
fwbr601i0:
fwpr601p0:
fwln601i0:
--- t0 ---
Inter-|   Receive                                                |  Transmit
 face |bytes    packets errs drop fifo frame compressed multicast|bytes    packets errs drop fifo colls carrier compressed
    lo: 62126802  385024    0    0    0     0          0         0 62126802  385024    0    0    0     0       0          0
  nic0: 3354702094 12219036    0 7194    0     0          0   5091016 5309918696 6222300    0    3    0     0       0          0
  nic1: 99928261826 70602056    0  175    0     0          0    147214 23566970003 33702496    0    0    0     0       0          0
  nic2: 22573329286 16422612    0    0    0     0          0     60173 5686749222 6978719    0    0    0     0       0          0
  nic3: 24157756  240077    0    0    0     0          0    214799  2048864    7874    0    0    0     0       0          0
  nic4:       0       0    0    0    0     0          0         0        0       0    0    0    0     0       0          0
  nic5:       0       0    0    0    0     0          0         0        0       0    0    0    0     0       0          0
 vmbr0: 1079069500 7943122    0    0    0     0          0   4223074 4830092634 1458467    0    3    0     0       0          0
tailscale0: 164813652 1151524    0    0    0     0          0         0 8058560608  984296    0    0    0     0       0          0
nic3.2:       0       0    0    0    0     0          0         0      906       7    0    0    0     0       0          0
br-rr-mgmt:       0       0    0    0    0     0          0         0      906       7    0    0    0     0       0          0
 bond0: 122501591112 87024668    0 14559    0     0          0    207387 29253719225 40681215    0    0    0     0       0          0
storagenet: 118059084154 31987985    0    5    0     0          0    178613 28196184459 27060363    0    0    0     0       0          0
tap100i0:  920005    9310    0    0    0     0          0         0 477586312 4421734    0    0    0     0       0          0
fwbr100i0: 413424502 4407744    0 6283    0     0          0   2969061        0       0    0    0    0     0       0          0
fwpr100p0: 2249167   14648    0 5338    0     0          0         0 477591650 4421734    0    0    0     0       0          0
fwln100i0: 477591650 4421734    0 5338    0     0          0         0  2249167   14648    0    0    0     0       0          0
tap600i0: 90374154  427457    0    0    0     0          0         0 677647593 5118738    0    0    0     0       0          0
fwbr600i0: 413414074 4407624    0 6282    0     0          0   2968991        0       0    0    0    0     0       0          0
fwpr600p0: 91703316  432795    0 5338    0     0          0         0 677653145 5118739    0    0    0     0       0          0
fwln600i0: 677653145 5118739    0 5338    0     0          0         0 91703316  432795    0    0    0     0       0          0
tap601i0: 89485124  439784    0    0    0     0          0         0 1009530299 5150124    0    0    0     0       0          0
fwbr601i0: 413399362 4407487    0 6282    0     0          0   2968922        0       0    0    0    0     0       0          0
fwpr601p0: 90814286  445122    0 5338    0     0          0         0 1009535637 5150124    0    0    0     0       0          0
fwln601i0: 1009535637 5150124    0 5338    0     0          0         0 90814286  445122    0    0    0     0       0          0
--- t1 (1s later) ---
Inter-|   Receive                                                |  Transmit
 face |bytes    packets errs drop fifo frame compressed multicast|bytes    packets errs drop fifo colls carrier compressed
    lo: 62129135  385049    0    0    0     0          0         0 62129135  385049    0    0    0     0       0          0
  nic0: 3354714509 12219096    0 7194    0     0          0   5091038 5309929056 6222332    0    3    0     0       0          0
  nic1: 99928266060 70602093    0  175    0     0          0    147214 23566974239 33702542    0    0    0     0       0          0
  nic2: 22573329286 16422612    0    0    0     0          0     60173 5686749222 6978719    0    0    0     0       0          0
  nic3: 24157820  240078    0    0    0     0          0    214800  2048864    7874    0    0    0     0       0          0
  nic4:       0       0    0    0    0     0          0         0        0       0    0    0    0     0       0          0
  nic5:       0       0    0    0    0     0          0         0        0       0    0    0    0     0       0          0
 vmbr0: 1079086039 7943183    0    0    0     0          0   4223085 4830117266 1458502    0    3    0     0       0          0
tailscale0: 164824347 1151560    0    0    0     0          0         0 8058580700  984327    0    0    0     0       0          0
nic3.2:       0       0    0    0    0     0          0         0      906       7    0    0    0     0       0          0
br-rr-mgmt:       0       0    0    0    0     0          0         0      906       7    0    0    0     0       0          0
 bond0: 122501595346 87024705    0 14559    0     0          0    207387 29253723461 40681261    0    0    0     0       0          0
storagenet: 118059090965 31988054    0    5    0     0          0    178615 28196193447 27060461    0    0    0     0       0          0
tap100i0:  920005    9310    0    0    0     0          0         0 477589167 4421755    0    0    0     0       0          0
fwbr100i0: 413427063 4407765    0 6283    0     0          0   2969072        0       0    0    0    0     0       0          0
fwpr100p0: 2249167   14648    0 5338    0     0          0         0 477594505 4421755    0    0    0     0       0          0
fwln100i0: 477594505 4421755    0 5338    0     0          0         0  2249167   14648    0    0    0     0       0          0
tap600i0: 90374512  427459    0    0    0     0          0         0 677650806 5118761    0    0    0     0       0          0
fwbr600i0: 413416635 4407645    0 6282    0     0          0   2969002        0       0    0    0    0     0       0          0
fwpr600p0: 91703674  432797    0 5338    0     0          0         0 677656358 5118762    0    0    0     0       0          0
fwln600i0: 677656358 5118762    0 5338    0     0          0         0 91703674  432797    0    0    0     0       0          0
tap601i0: 89485124  439784    0    0    0     0          0         0 1009533154 5150145    0    0    0     0       0          0
fwbr601i0: 413401923 4407508    0 6282    0     0          0   2968933        0       0    0    0    0     0       0          0
fwpr601p0: 90814286  445122    0 5338    0     0          0         0 1009538492 5150145    0    0    0     0       0          0
fwln601i0: 1009538492 5150145    0 5338    0     0          0         0 90814286  445122    0    0    0     0       0          0

###############################################################################
# 27. DNS / NTP / TIME
###############################################################################

--- /etc/resolv.conf
    --- /etc/resolv.conf ---
domain knel.net
search knel.net
nameserver 100.100.100.100

--- /etc/hosts
    --- /etc/hosts ---
127.0.0.1 localhost.localdomain localhost
192.168.100.2 pfv-tsys6.knel.net pfv-tsys6

# The following lines are desirable for IPv6 capable hosts

::1     ip6-localhost ip6-loopback
fe00::0 ip6-localnet
ff00::0 ip6-mcastprefix
ff02::1 ip6-allnodes
ff02::2 ip6-allrouters
ff02::3 ip6-allhosts

10.100.100.4 pfv-tsys4-nfs-stor
10.100.100.5 pfv-tsys5-nfs-stor

--- /etc/ntp.conf
    [missing: /etc/ntp.conf]

--- /etc/chrony/chrony.conf
    --- /etc/chrony/chrony.conf ---
# Welcome to the chrony configuration file. See chrony.conf(5) for more
# information about usable directives.

# Use Debian vendor zone.
pool 2.debian.pool.ntp.org iburst

# Use time sources from DHCP.
sourcedir /run/chrony-dhcp

# Use NTP sources found in /etc/chrony/sources.d.
sourcedir /etc/chrony/sources.d

# This directive specifies the location of the file containing ID/key pairs for
# NTP authentication.
keyfile /etc/chrony/chrony.keys

# This directive specifies the file into which chronyd will store the rate
# information.
driftfile /var/lib/chrony/chrony.drift

# Save NTS keys and cookies.
ntsdumpdir /var/lib/chrony

# Uncomment the following line to turn logging on.
#log tracking measurements statistics

# Log files location.
logdir /var/log/chrony

# Stop bad estimates upsetting machine clock.
maxupdateskew 100.0

# This directive enables kernel synchronisation (every 11 minutes) of the
# real-time clock. Note that it can't be used along with the 'rtcfile' directive.
rtcsync

# Step the system clock instead of slewing it if the adjustment is larger than
# one second, but only in the first three clock updates.
makestep 1 3

# Get TAI-UTC offset and leap seconds from the system tz database.
# This directive must be commented out when using time sources serving
# leap-smeared time.
leapseclist /usr/share/zoneinfo/leap-seconds.list

# Include configuration files found in /etc/chrony/conf.d.
confdir /etc/chrony/conf.d

--- timedatectl
    $ timedatectl
               Local time: Wed 2026-07-29 05:15:04 CDT
           Universal time: Wed 2026-07-29 10:15:04 UTC
                 RTC time: Wed 2026-07-29 10:15:04
                Time zone: America/Chicago (CDT, -0500)
System clock synchronized: yes
              NTP service: active
          RTC in local TZ: no

--- chronyc tracking
    $ chronyc tracking
Reference ID    : 178FC4C8 (time-usw3.crimpac.net)
Stratum         : 3
Ref time (UTC)  : Wed Jul 29 10:07:43 2026
System time     : 0.000889000 seconds fast of NTP time
Last offset     : -0.000134784 seconds
RMS offset      : 0.000228302 seconds
Frequency       : 37.658 ppm slow
Residual freq   : -0.014 ppm
Skew            : 0.114 ppm
Root delay      : 0.059029799 seconds
Root dispersion : 0.002018905 seconds
Update interval : 1038.3 seconds
Leap status     : Normal

--- chronyc sources
    $ chronyc sources
MS Name/IP address         Stratum Poll Reach LastRx Last sample               
===============================================================================
^+ ntp.maxhost.io                2  10   377   261  +4710us[+4710us] +/-   54ms
^+ 72-14-182-49.ip.linodeus>     2  10   377   42m    -11ms[  -11ms] +/-   81ms
^* time-usw3.crimpac.net         2  10   377   440    +76us[  -59us] +/-   31ms
^- time1.lshiy.com               2  10   377   285  +1675us[+1675us] +/-  112ms

--- ntpq peers
    $ ntpq -pn
/root/check.sh: line 45: ntpq: command not found
    [exit=127 / not installed or not permitted]

###############################################################################
# 28. FIREWALL / SECURITY
###############################################################################

--- pve-firewall status
    $ pve-firewall status
Status: disabled/running

--- nft ruleset (count)
    $ nft list ruleset

--- nft ruleset (head)
    $ nft list ruleset

--- iptables-save (legacy)
    $ iptables-save
# Generated by iptables-save v1.8.11 on Wed Jul 29 05:15:06 2026
*raw
:PREROUTING ACCEPT [44936240:120015441658]
:OUTPUT ACCEPT [27059171:40669155993]
COMMIT
# Completed on Wed Jul 29 05:15:06 2026
# Generated by iptables-save v1.8.11 on Wed Jul 29 05:15:06 2026
*mangle
:PREROUTING ACCEPT [44936680:120015573450]
:INPUT ACCEPT [35153690:118815866751]
:FORWARD ACCEPT [0:0]
:OUTPUT ACCEPT [27059359:40669186800]
:POSTROUTING ACCEPT [27059359:40669186800]
-A PREROUTING -m conntrack --ctstate RELATED,ESTABLISHED -j CONNMARK --restore-mark --nfmask 0xff0000 --ctmask 0xff0000
-A OUTPUT -m conntrack --ctstate NEW -m mark ! --mark 0x0/0xff0000 -j CONNMARK --save-mark --nfmask 0xff0000 --ctmask 0xff0000
COMMIT
# Completed on Wed Jul 29 05:15:06 2026
# Generated by iptables-save v1.8.11 on Wed Jul 29 05:15:06 2026
*nat
:PREROUTING ACCEPT [9427057:1127505720]
:INPUT ACCEPT [185312:49420008]
:OUTPUT ACCEPT [411442:26801382]
:POSTROUTING ACCEPT [411442:26801382]
:ts-postrouting - [0:0]
-A POSTROUTING -j ts-postrouting
-A ts-postrouting -m mark --mark 0x40000/0xff0000 -j MASQUERADE
COMMIT
# Completed on Wed Jul 29 05:15:06 2026
# Generated by iptables-save v1.8.11 on Wed Jul 29 05:15:06 2026
*filter
:INPUT ACCEPT [32632537:118362799592]
:FORWARD ACCEPT [0:0]
:OUTPUT ACCEPT [27059497:40669203272]
:ts-forward - [0:0]
:ts-input - [0:0]
-A INPUT -j ts-input
-A FORWARD -j ts-forward
-A ts-forward -i tailscale0 -j MARK --set-xmark 0x40000/0xff0000
-A ts-forward -m mark --mark 0x40000/0xff0000 -j ACCEPT
-A ts-forward -s 100.64.0.0/10 -o tailscale0 -j DROP
-A ts-forward -o tailscale0 -j ACCEPT
-A ts-input -s 100.73.35.111/32 -i lo -j ACCEPT
-A ts-input -i tailscale0 -j ACCEPT
-A ts-input -p udp -m udp --dport 41641 -j ACCEPT
-A ts-input -s 100.115.92.0/23 ! -i tailscale0 -j RETURN
-A ts-input -s 100.64.0.0/10 ! -i tailscale0 -j DROP
COMMIT
# Completed on Wed Jul 29 05:15:06 2026

--- ipset list (names)
    $ ipset list -n

--- apparmor status
    $ aa-status
apparmor module is loaded.
119 profiles are loaded.
20 profiles are in enforce mode.
   /usr/bin/lxc-copy
   /usr/bin/lxc-start
   /usr/bin/man
   /usr/lib/NetworkManager/nm-dhcp-client.action
   /usr/lib/connman/scripts/dhclient-script
   /usr/sbin/chronyd
   /usr/{lib/NetworkManager,libexec}/nm-dhcp-helper
   /{,usr/}sbin/dhclient
   lsb_release
   lxc-container-default
   lxc-container-default-cgns
   lxc-container-default-with-mounting
   lxc-container-default-with-nesting
   man_filter
   man_groff
   nvidia_modprobe
   nvidia_modprobe//kmod
   pve-container-mounthotplug
   swtpm
   tcpdump
23 profiles are in complain mode.
   Xorg
   plasmashell
   plasmashell//QtWebEngineProcess
   sbuild
   sbuild-abort
   sbuild-adduser
   sbuild-apt
   sbuild-checkpackages
   sbuild-clean
   sbuild-createchroot
   sbuild-destroychroot
   sbuild-distupgrade
   sbuild-hold
   sbuild-shell
   sbuild-unhold
   sbuild-update
   sbuild-upgrade
   transmission-cli
   transmission-daemon
   transmission-gtk
   transmission-qt
   unix-chkpwd
   unprivileged_userns
0 profiles are in prompt mode.
0 profiles are in kill mode.
76 profiles are in unconfined mode.
   1password
   Discord
   MongoDB Compass
   QtWebEngineProcess
   balena-etcher
   brave
   buildah
   busybox
   cam
   ch-checkns
   ch-run
   chrome
   chromium
   crun
   devhelp
   element-desktop
   epiphany
   evolution
   firefox
   flatpak
   foliate
   geary
   github-desktop
   goldendict
   ipa_verify
   kchmviewer
   keybase
   lc-compliance
   libcamerify
   linux-sandbox
   loupe
   lxc-attach
   lxc-create
   lxc-destroy
   lxc-execute
   lxc-stop
   lxc-unshare
   lxc-usernsexec
   mmdebstrap
   msedge
   nautilus
   notepadqq
   obsidian
   opam
   opera
   pageedit
   polypane
   privacybrowser
   qcam
   qmapshack
   qutebrowser
   rootlesskit
   rpm
   rssguard
   runc
   scide
   signal-desktop
   slack
   slirp4netns
   steam
   stress-ng
   surfshark
   systemd-coredump
   toybox
   trinity
   tup
   tuxedo-control-center
   userbindmount
   uwsgi-core
   vdens
   virtiofsd
   vivaldi-bin
   vpnns
   vscode
   wike
   wpcom
3 processes have profiles defined.
3 processes are in enforce mode.
   /usr/sbin/chronyd (870) 
   /usr/sbin/chronyd (974) 
   /usr/sbin/dhclient (1073) /{,usr/}sbin/dhclient
0 processes are in complain mode.
0 processes are in prompt mode.
0 processes are in kill mode.
0 processes are unconfined but have a profile defined.
0 processes are in mixed mode.

###############################################################################
# 29. TOP CONSUMERS
###############################################################################

--- top 10 memory hogs
    $ ps -eo pid,user,rss,vsz,pcpu,pmem,comm --sort=-rss | head -n 11
    PID USER       RSS    VSZ %CPU %MEM COMMAND
 283674 root     3156108 6680312 2.0  2.3 kvm
 283375 root     1272820 33718964 0.9  0.9 kvm
 283519 root     1039872 13097596 1.3  0.7 kvm
 993541 www-data 221616 291516 0.0  0.1 pveproxy worker
   1532 www-data 184156 231224 0.0  0.1 pveproxy
 993540 www-data 183964 254324 0.0  0.1 pveproxy worker
 993542 www-data 179512 252064 0.0  0.1 pveproxy worker
 949449 root     166252 239132 0.0  0.1 pvedaemon worke
 947600 root     165740 239060 0.0  0.1 pvedaemon worke
 949846 root     163588 238900 0.0  0.1 pvedaemon worke

--- top 10 CPU hogs
    $ ps -eo pid,user,pcpu,pmem,rss,comm --sort=-pcpu | head -n 11
    PID USER     %CPU %MEM   RSS COMMAND
1081840 root      3.3  0.0  7844 systemd-timedat
 283674 root      2.0  2.3 3156108 kvm
   1505 root      1.4  0.0 126224 pvestatd
 283519 root      1.3  0.7 1039872 kvm
 283375 root      0.9  0.9 1272820 kvm
    895 root      0.4  0.0 119720 tailscaled
   1491 root      0.3  0.0 113080 pve-firewall
1074854 root      0.3  0.0     0 kworker/1:2-mm_percpu_wq
1073221 root      0.1  0.1 152376 qm
1077159 root      0.1  0.0  3728 bash

--- top file-handle holders
    $ for pid in $(ps -e -o pid= | head -n 200); do
    n="$(ls /proc/$pid/fd 2>/dev/null | wc -l)"
    [ "$n" -gt 50 ] && printf '%6d fd=%-6s %s\n' "$pid" "$n" "$(cat /proc/$pid/comm 2>/dev/null)"
done | sort -k2 -t= -nr | head -n 15
     1 fd=183    systemd
   871 fd=54     dbus-daemon

--- largest files in /var/log (top 10)
    $ find /var/log -type f -size +10M -exec ls -lh {} \; 2>/dev/null | sort -k5 -h -r | head -n 10
-rw-r-----+ 1 root systemd-journal 48M Jul 26 21:41 /var/log/journal/3a16e11f1dd84d21b50d511e804fd378/system@c57197d92b4f425da80c8c1fe0cefbff-0000000000aaddb6-0006573b07494316.journal
-rw-r-----+ 1 root systemd-journal 40M Jul  9 21:03 /var/log/journal/3a16e11f1dd84d21b50d511e804fd378/system@c57197d92b4f425da80c8c1fe0cefbff-00000000006767b5-00065633481dab4d.journal
-rw-r-----+ 1 root systemd-journal 40M Jul  9 15:15 /var/log/journal/3a16e11f1dd84d21b50d511e804fd378/system@c57197d92b4f425da80c8c1fe0cefbff-0000000000662e14-0006562e61a1bc3f.journal
-rw-r-----+ 1 root systemd-journal 40M Jul  9 09:24 /var/log/journal/3a16e11f1dd84d21b50d511e804fd378/system@c57197d92b4f425da80c8c1fe0cefbff-000000000064f3c0-00065629babb9e3d.journal
-rw-r-----+ 1 root systemd-journal 40M Jul  9 03:51 /var/log/journal/3a16e11f1dd84d21b50d511e804fd378/system@c57197d92b4f425da80c8c1fe0cefbff-000000000063b9be-0006562510168ff4.journal
-rw-r-----+ 1 root systemd-journal 40M Jul  8 22:17 /var/log/journal/3a16e11f1dd84d21b50d511e804fd378/system@c57197d92b4f425da80c8c1fe0cefbff-0000000000628008-000656202e187c2b.journal
-rw-r-----+ 1 root systemd-journal 40M Jul  8 16:27 /var/log/journal/3a16e11f1dd84d21b50d511e804fd378/system@c57197d92b4f425da80c8c1fe0cefbff-000000000061464f-0006561b4b2696e9.journal
-rw-r-----+ 1 root systemd-journal 40M Jul  8 10:38 /var/log/journal/3a16e11f1dd84d21b50d511e804fd378/system@c57197d92b4f425da80c8c1fe0cefbff-0000000000600c6e-000656169ce48748.journal
-rw-r-----+ 1 root systemd-journal 40M Jul  8 05:03 /var/log/journal/3a16e11f1dd84d21b50d511e804fd378/system@c57197d92b4f425da80c8c1fe0cefbff-00000000005ed248-00065611f8efa18d.journal
-rw-r-----+ 1 root systemd-journal 40M Jul  7 23:30 /var/log/journal/3a16e11f1dd84d21b50d511e804fd378/system@c57197d92b4f425da80c8c1fe0cefbff-00000000005d9830-0006560d2d0793c0.journal

###############################################################################
# 30. QUICK-LOOK SUSPECT SUMMARY
###############################################################################

Auto-detected performance anti-patterns (verify against full data above):


--- [A] Network interfaces < 10 Gbps and up
    $ hits=0
for ifc in $NETIFS; do
    s=$(cat "/sys/class/net/$ifc/speed" 2>/dev/null)
    c=$(cat "/sys/class/net/$ifc/carrier" 2>/dev/null)
    case "$s" in
        10|100|1000)
            if [ "$c" = "1" ]; then
                printf '  %s : %s Mbps (UP)  <-- sub-10GbE; suspect if this carries storage/migration\n' "$ifc" "$s"
                hits=$((hits+1))
            fi
            ;;
    esac
done
[ "$hits" = "0" ] && echo "  no <10GbE interfaces are UP (or speed unreadable)"
  br-rr-mgmt : 100 Mbps (UP)  <-- sub-10GbE; suspect if this carries storage/migration
  nic0 : 1000 Mbps (UP)  <-- sub-10GbE; suspect if this carries storage/migration
  nic1 : 1000 Mbps (UP)  <-- sub-10GbE; suspect if this carries storage/migration
  nic2 : 1000 Mbps (UP)  <-- sub-10GbE; suspect if this carries storage/migration
  nic3 : 100 Mbps (UP)  <-- sub-10GbE; suspect if this carries storage/migration
  nic3.2 : 100 Mbps (UP)  <-- sub-10GbE; suspect if this carries storage/migration
    [exit=1]


--- [B] MTU not jumbo on carrier-up interfaces
    $ hits=0
for ifc in $NETIFS; do
    m=$(cat "/sys/class/net/$ifc/mtu" 2>/dev/null)
    c=$(cat "/sys/class/net/$ifc/carrier" 2>/dev/null)
    [ "$c" = "1" ] || continue
    if [ -n "$m" ] && [ "$m" != "9000" ]; then
        printf '  %s : mtu=%s\n' "$ifc" "$m"
        hits=$((hits+1))
    fi
done
[ "$hits" = "0" ] && echo "  all carrier-up interfaces have MTU 9000 (or none are up)"
  bond0 : mtu=1500
  br-rr-mgmt : mtu=1500
  fwbr100i0 : mtu=1500
  fwbr600i0 : mtu=1500
  fwbr601i0 : mtu=1500
  fwln100i0 : mtu=1500
  fwln600i0 : mtu=1500
  fwln601i0 : mtu=1500
  fwpr100p0 : mtu=1500
  fwpr600p0 : mtu=1500
  fwpr601p0 : mtu=1500
  nic0 : mtu=1500
  nic1 : mtu=1500
  nic2 : mtu=1500
  nic3 : mtu=1500
  nic3.2 : mtu=1500
  storagenet : mtu=1500
  tap100i0 : mtu=1500
  tap600i0 : mtu=1500
  tap601i0 : mtu=1500
  vmbr0 : mtu=1500
    [exit=1]


--- [C] CPU governor != performance
    $ g=$(cat /sys/devices/system/cpu/cpu0/cpufreq/scaling_governor 2>/dev/null)
if [ -z "$g" ]; then
    echo "  cpufreq driver not loaded (governor unknown)"
elif [ "$g" = "performance" ]; then
    echo "  OK: performance governor"
else
    echo "  <-- governor=$g  (recommend 'performance')"
fi
  OK: performance governor


--- [D] EPB / EPP not performance-bias
    $ epb=$(cat /sys/devices/system/cpu/cpu0/power/energy_perf_bias 2>/dev/null)
epp=$(cat /sys/devices/system/cpu/cpu0/cpufreq/energy_performance_preference 2>/dev/null)
echo "  EPB=$epb  EPP=$epp  (0=performance, 15=max-power on EPB; 'performance' on EPP)"
  EPB=  EPP=  (0=performance, 15=max-power on EPB; 'performance' on EPP)


--- [E] vm.swappiness and dirty ratios
    $ sw=$(sysctl -n vm.swappiness 2>/dev/null)
dr=$(sysctl -n vm.dirty_ratio 2>/dev/null)
dbr=$(sysctl -n vm.dirty_background_ratio 2>/dev/null)
echo "  swappiness=$sw  dirty_ratio=$dr  dirty_background_ratio=$dbr"
[ "$sw" != "10" ] && [ -n "$sw" ] && echo "    <-- swappiness not 10 (Proxmox default)"
  swappiness=10  dirty_ratio=40  dirty_background_ratio=5
    [exit=1]


--- [F] TCP congestion control
    $ cc=$(sysctl -n net.ipv4.tcp_congestion_control 2>/dev/null)
avail=$(sysctl -n net.ipv4.tcp_available_congestion_control 2>/dev/null)
echo "  active: $cc"
echo "  available: $avail"
[ "$cc" = "cubic" ] && echo "    <-- consider bbr (if available) for high-BDP NFS paths"
  active: bbr
  available: reno cubic bbr
    [exit=1]


--- [G] ZFS dataset red flags
    $ if ! command -v zfs >/dev/null 2>&1; then
    echo "  ZFS not present"
else
    zfs get -r -o name,property,value compression,atime,sync,recordsize,xattr 2>/dev/null \
      | awk '$2=="compression" && $3=="off" {print "  <-- "$1" has compression=off"}
             $2=="atime" && $3=="on"        {print "  <-- "$1" has atime=on"}
             $2=="sync" && $3=="always"     {print "  <-- "$1" has sync=always (slow without SLOG)"}
             $2=="xattr" && $3=="on"        {print "  <-- "$1" has xattr=on (use sa)"}'
fi


--- [H] ARC size vs RAM
    $ if [ -r /proc/spl/kstat/zfs/arcstats ]; then
    arc=$(awk '/^size /{print $3}' /proc/spl/kstat/zfs/arcstats 2>/dev/null)
    cmax=$(awk '/^c_max /{print $3}' /proc/spl/kstat/zfs/arcstats 2>/dev/null)
    ram=$(awk '/MemTotal/{print $2*1024}' /proc/meminfo)
    echo "  ARC current=$arc bytes  ARC max=$cmax bytes  RAM total=$ram bytes"
    if [ -n "$cmax" ] && [ -n "$ram" ] && [ "$ram" -gt 0 ]; then
        pct=$((cmax * 100 / ram))
        echo "  ARC max is ${pct}% of RAM (Proxmox default ~50%)"
    fi
    hits=$(awk '/^hits /{print $3}' /proc/spl/kstat/zfs/arcstats 2>/dev/null)
    miss=$(awk '/^misses /{print $3}' /proc/spl/kstat/zfs/arcstats 2>/dev/null)
    if [ -n "$hits" ] && [ -n "$miss" ] && [ "$((hits+miss))" -gt 0 ]; then
        hr=$((hits * 100 / (hits + miss)))
        echo "  ARC hit rate since boot: ${hr}% (hits=$hits misses=$miss)"
    fi
else
    echo "  ZFS ARC stats not available (ZFS not loaded?)"
fi
  ARC current=3840 bytes  ARC max=13515096064 bytes  RAM total=135158845440 bytes
  ARC max is 9% of RAM (Proxmox default ~50%)


--- [I] VMs with non-optimal storage/NIC models
    $ hits=0
for vmid in $(qm list 2>/dev/null | awk 'NR>1{print $1}'); do
    cfg=$(qm config "$vmid" 2>/dev/null)
    flags=""
    echo "$cfg" | grep -qE '^ide[0-9]'                 && flags="${flags}ide-disk "
    echo "$cfg" | grep -qE '^sata[0-9]'                && flags="${flags}sata-disk "
    echo "$cfg" | grep -qE '^scsi[0-9].*:,'            && echo "$cfg" | grep -E '^scsi[0-9]' | grep -qv 'virtio-scsi' && flags="${flags}scsi-no-virtio-scsi "
    echo "$cfg" | grep -qE '^scsihw: ' && ! echo "$cfg" | grep -qE '^scsihw: virtio-scsi-single' && flags="${flags}scsihw!=virtio-scsi-single "
    echo "$cfg" | grep -qE '^cpu: .*kvm64'             && flags="${flags}cpu=kvm64 "
    echo "$cfg" | grep -q '^iothread: 1'               || echo "$cfg" | grep -qE '^scsi[0-9].*iothread=1' || flags="${flags}no-iothread "
    echo "$cfg" | grep -qE '^net[0-9].*model=(e1000|rtl8139|vmxnet)' && flags="${flags}legacy-nic "
    echo "$cfg" | grep -qE '^net[0-9].*model=virtio' && ! echo "$cfg" | grep -qE 'multiqueue=|queues=' && flags="${flags}virtio-no-multiqueue "
    if [ -n "$flags" ]; then
        echo "  VM $vmid: $flags"
        hits=$((hits+1))
    fi
done
[ "$hits" = "0" ] && echo "  no obvious VM storage/NIC anti-patterns"
  VM 100: ide-disk 
  VM 600: ide-disk 
  VM 601: ide-disk 
    [exit=1]


--- [J] NFS client mount option red flags
    $ if ! command -v nfsstat >/dev/null 2>&1; then
    echo "  nfsstat not available"
else
    nfsstat -m 2>/dev/null | awk '
        /^.*:/ {mp=$0; next}
        /Flags:/ {
            gsub(/Flags:|,/,"",$0)
            line=$0
            if (line !~ /noatime/)        print "  "mp" : missing noatime"
            if (line !~ /nconnect/)       print "  "mp" : missing nconnect (kernel >=5.3)"
            if (line !~ /rsize=1048576/)  print "  "mp" : rsize<1M"
            if (line !~ /wsize=1048576/)  print "  "mp" : wsize<1M"
            if (line ~ /sync/)            print "  "mp" : sync mount (slow)"
        }
    '
fi


--- [K] Softnet / NIC drops (non-zero)
    $ awk 'NR<=32 && ($2+0 > 0 || $4+0 > 0) {printf "  cpu%d: dropped=%d time_squeezed=%d\n", NR-1, $2, $4}' /proc/net/softnet_stat
echo "  (also check ethtool -S sections above for rx_dropped/rx_missed_errors)"
  (also check ethtool -S sections above for rx_dropped/rx_missed_errors)


--- [L] Failed systemd services
    $ failed=$(systemctl --failed --no-legend 2>/dev/null | head -n 10)
if [ -n "$failed" ]; then
    echo "$failed" | sed 's/^/  /'
else
    echo "  no failed services"
fi
  no failed services


--- [M] Filesystem usage > 80%
    $ df -h 2>/dev/null | awk 'NR>1 && $5+0 > 80 {print "  "$0}'


--- [N] SMART / NVMe health warnings
    $ if command -v nvme >/dev/null 2>&1; then
    for n in /dev/nvme[0-9]*; do
        [ -b "$n" ] || continue
        crit=$(nvme smart-log "$n" 2>/dev/null | grep -iE 'critical_warning|media_and_data_integrity|available_spare' | head -n 5)
        [ -n "$crit" ] && echo "  $n: $crit" | tr '\n' ' '
    done
fi
if command -v smartctl >/dev/null 2>&1; then
    for d in $(ls /sys/block/ 2>/dev/null | grep -E '^sd'); do
        dev="/dev/$d"
        [ -b "$dev" ] || continue
        chk=$(smartctl -H "$dev" 2>/dev/null | grep -iE 'result|health|passed|failed')
        echo "$chk" | grep -qi fail && echo "  $dev: $chk"
    done
fi
echo "  (see section 20 for full smartctl/nvme output)"
  (see section 20 for full smartctl/nvme output)

###############################################################################
# Collection complete: pfv-tsys6
# Output:  /root/pfv-tsys6.log
# Size:    922774 bytes / 16570 lines
# Elapsed: 367 seconds
###############################################################################
