=== LACP per-slave distribution (sender) ===
Host: pfv-tsys7   Role: sender
Date: 2026-07-27T13:50:23Z
Bond: bond0

--- bond0 state ---
Bonding Mode: IEEE 802.3ad Dynamic link aggregation
Transmit Hash Policy: layer3+4 (1)
	Number of ports: 2
	Partner Mac Address: 00:13:72:46:95:e4
Slave Interface: nic1
Link Failure Count: 0
Slave Interface: nic2
Link Failure Count: 0


--- iperf3 output (raw tail) ---
[ 17]  11.00-12.00  sec  19.2 MBytes   161 Mbits/sec  1377   99.0 KBytes       
[ 19]  11.00-12.00  sec  23.0 MBytes   193 Mbits/sec   32    150 KBytes       
[SUM]  11.00-12.00  sec   218 MBytes  1.83 Gbits/sec  4583             
- - - - - - - - - - - - - - - - - - - - - - - - -
[ ID] Interval           Transfer     Bitrate         Retr
[  5]   0.00-12.00  sec   443 MBytes   309 Mbits/sec  2692            sender
[  5]   0.00-12.00  sec   443 MBytes   310 Mbits/sec                  receiver
[  7]   0.00-12.00  sec   236 MBytes   165 Mbits/sec  14462            sender
[  7]   0.00-12.00  sec   236 MBytes   165 Mbits/sec                  receiver
[  9]   0.00-12.00  sec   431 MBytes   302 Mbits/sec  11643            sender
[  9]   0.00-12.00  sec   431 MBytes   301 Mbits/sec                  receiver
[ 11]   0.00-12.00  sec   277 MBytes   194 Mbits/sec  708            sender
[ 11]   0.00-12.00  sec   276 MBytes   193 Mbits/sec                  receiver
[ 13]   0.00-12.00  sec   433 MBytes   302 Mbits/sec  11333            sender
[ 13]   0.00-12.00  sec   432 MBytes   302 Mbits/sec                  receiver
[ 15]   0.00-12.00  sec   276 MBytes   193 Mbits/sec  711            sender
[ 15]   0.00-12.00  sec   276 MBytes   193 Mbits/sec                  receiver
[ 17]   0.00-12.00  sec   239 MBytes   167 Mbits/sec  14169            sender
[ 17]   0.00-12.00  sec   239 MBytes   167 Mbits/sec                  receiver
[ 19]   0.00-12.00  sec   277 MBytes   194 Mbits/sec  702            sender
[ 19]   0.00-12.00  sec   277 MBytes   194 Mbits/sec                  receiver
[SUM]   0.00-12.00  sec  2.55 GBytes  1.83 Gbits/sec  56420             sender
[SUM]   0.00-12.00  sec  2.55 GBytes  1.82 Gbits/sec                  receiver

iperf Done.


--- Sender TX (control: should split if host hash=layer3+4) (bytes) ---
  SLAVE                BEFORE          AFTER          DELTA      PCT
  nic1             4576796928     6213933342     1637136414    50.0%
  nic2             1566733474     3206435063     1639701589    50.0%
  TOTAL                                          3276838003   100.0%

===================================================================
 VERDICT: host TX distributing OK (top slave 'nic2' = 50.0%).
===================================================================
