=== iperf3: tsys7→tsys6 UDP saturation ===
Client: pfv-tsys7  Server: pfv-tsys6 (10.100.100.6)
Date: 2026-07-26T21:35:31Z
Args: /home/reachableceo/projects/perfopt/returned-logs/iperf/tsys6-tsys7-05-udp.log -u -b 3G -t 10 -l 8972

warning: UDP block size 8972 exceeds TCP MSS 1448, may result in fragmentation / drops
Connecting to host 10.100.100.6, port 5201
[  5] local 10.100.100.7 port 56685 connected to 10.100.100.6 port 5201
[ ID] Interval           Transfer     Bitrate         Total Datagrams
[  5]   0.00-1.00   sec   358 MBytes  3.00 Gbits/sec  41823  
[  5]   1.00-2.00   sec   358 MBytes  3.00 Gbits/sec  41813  
[  5]   2.00-3.00   sec   358 MBytes  3.00 Gbits/sec  41797  
[  5]   3.00-4.00   sec   357 MBytes  3.00 Gbits/sec  41779  
[  5]   4.00-5.00   sec   358 MBytes  3.00 Gbits/sec  41814  
[  5]   5.00-6.00   sec   358 MBytes  3.00 Gbits/sec  41797  
[  5]   6.00-7.00   sec   358 MBytes  3.00 Gbits/sec  41795  
[  5]   7.00-8.00   sec   358 MBytes  3.00 Gbits/sec  41797  
[  5]   8.00-9.00   sec   358 MBytes  3.00 Gbits/sec  41799  
[  5]   9.00-10.00  sec   358 MBytes  3.00 Gbits/sec  41794  
- - - - - - - - - - - - - - - - - - - - - - - - -
[ ID] Interval           Transfer     Bitrate         Jitter    Lost/Total Datagrams
[  5]   0.00-10.00  sec  3.49 GBytes  3.00 Gbits/sec  0.000 ms  0/418008 (0%)  sender
[  5]   0.00-10.00  sec  23.4 MBytes  19.6 Mbits/sec  0.090 ms  6601/9333 (71%)  receiver

iperf Done.

=== END ===
