From 6cd77aa95a7ab46771874b72c7dba6b3600d9b29 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Micha=C5=82=20=C5=BBygowski?= <michal.zygowski@3mdeb.com>
Date: Mon, 13 May 2024 09:31:27 +0200
Subject: [PATCH] src/mainboard/clevo/adl-p/Kconfig: Add missing TPM PIRQ for
 NV41
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Michał Żygowski <michal.zygowski@3mdeb.com>
---
 src/mainboard/clevo/adl-p/Kconfig | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/src/mainboard/clevo/adl-p/Kconfig b/src/mainboard/clevo/adl-p/Kconfig
index 6e4b679d4d1..e9bcf53c7be 100644
--- a/src/mainboard/clevo/adl-p/Kconfig
+++ b/src/mainboard/clevo/adl-p/Kconfig
@@ -115,7 +115,7 @@ config FMDFILE
 	default "src/mainboard/\$(CONFIG_MAINBOARD_DIR)/vboot-rwa.fmd" if VBOOT && VBOOT_SLOTS_RW_A
 
 config TPM_PIRQ
-	default 0x27 if BOARD_CLEVO_NS50PU_BASE # GPP_E1
+	default 0x27 # GPP_E1
 
 config SOC_INTEL_CSE_SEND_EOP_EARLY
 	default n
