<?xml version="1.0" encoding="UTF-8"?>
<spirit:design xmlns:xilinx="http://www.xilinx.com" xmlns:spirit="http://www.spiritconsortium.org/XMLSchema/SPIRIT/1685-2009" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">
  <spirit:vendor>xilinx.com</spirit:vendor>
  <spirit:library>xci</spirit:library>
  <spirit:name>unknown</spirit:name>
  <spirit:version>1.0</spirit:version>
  <spirit:componentInstances>
    <spirit:componentInstance>
      <spirit:instanceName>div_gen_div_gen_0_0</spirit:instanceName>
      <spirit:componentRef spirit:vendor="xilinx.com" spirit:library="ip" spirit:name="div_gen" spirit:version="5.1"/>
      <spirit:configurableElementValues>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.ACLKEN_INTF.POLARITY">ACTIVE_LOW</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.ACLK_INTF.CLK_DOMAIN">div_gen_clk</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.ACLK_INTF.FREQ_HZ">200000000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.ACLK_INTF.INSERT_VIP">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.ACLK_INTF.PHASE">0.000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.ARESETN_INTF.INSERT_VIP">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DOUT.CLK_DOMAIN">div_gen_clk</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DOUT.FREQ_HZ">200000000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DOUT.HAS_TKEEP">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DOUT.HAS_TLAST">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DOUT.HAS_TREADY">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DOUT.HAS_TSTRB">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DOUT.INSERT_VIP">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DOUT.LAYERED_METADATA">xilinx.com:interface:datatypes:1.0 {TDATA {datatype {name {attribs {resolve_type immediate dependency {} format string minimum {} maximum {}} value {}} bitwidth {attribs {resolve_type automatic dependency {} format long minimum {} maximum {}} value 56} bitoffset {attribs {resolve_type immediate dependency {} format long minimum {} maximum {}} value 0} struct {field_fractional {name {attribs {resolve_type immediate dependency {} format string minimum {} maximum {}} value fractional} enabled {attr
ibs {resolve_type generated dependency fract_enabled format bool minimum {} maximum {}} value true} datatype {name {attribs {resolve_type immediate dependency {} format string minimum {} maximum {}} value {}} bitwidth {attribs {resolve_type generated dependency fract_width format long minimum {} maximum {}} value 24} bitoffset {attribs {resolve_type immediate dependency {} format long minimum {} maximum {}} value 0} real {fixed {fractwidth {attribs {resolve_type generated dependency fract_remain
der_fractwidth format long minimum {} maximum {}} value 23} signed {attribs {resolve_type generated dependency fract_remainder_signed format bool minimum {} maximum {}} value true}}}}} field_remainder {name {attribs {resolve_type immediate dependency {} format string minimum {} maximum {}} value remainder} enabled {attribs {resolve_type generated dependency remainder_enabled format bool minimum {} maximum {}} value false} datatype {name {attribs {resolve_type immediate dependency {} format strin
g minimum {} maximum {}} value {}} bitwidth {attribs {resolve_type generated dependency remainder_width format long minimum {} maximum {}} value 0} bitoffset {attribs {resolve_type immediate dependency {} format long minimum {} maximum {}} value 0} real {fixed {fractwidth {attribs {resolve_type generated dependency fract_remainder_fractwidth format long minimum {} maximum {}} value 23} signed {attribs {resolve_type generated dependency fract_remainder_signed format bool minimum {} maximum {}} va
lue true}}}}} field_quotient {name {attribs {resolve_type immediate dependency {} format string minimum {} maximum {}} value quotient} enabled {attribs {resolve_type immediate dependency {} format bool minimum {} maximum {}} value true} datatype {name {attribs {resolve_type immediate dependency {} format string minimum {} maximum {}} value {}} bitwidth {attribs {resolve_type generated dependency quotient_width format long minimum {} maximum {}} value 32} bitoffset {attribs {resolve_type generate
d dependency quotient_offset format long minimum {} maximum {}} value 24} integer {signed {attribs {resolve_type generated dependency quotient_signed format bool minimum {} maximum {}} value true}}}}}}} TDATA_WIDTH 56 TUSER {datatype {name {attribs {resolve_type immediate dependency {} format string minimum {} maximum {}} value {}} bitwidth {attribs {resolve_type automatic dependency {} format long minimum {} maximum {}} value 0} bitoffset {attribs {resolve_type immediate dependency {} format lo
ng minimum {} maximum {}} value 0} struct {field_divide_by_zero {name {attribs {resolve_type immediate dependency {} format string minimum {} maximum {}} value divide_by_zero} enabled {attribs {resolve_type generated dependency divbyzero_enabled format bool minimum {} maximum {}} value false} datatype {name {attribs {resolve_type immediate dependency {} format string minimum {} maximum {}} value {}} bitwidth {attribs {resolve_type generated dependency divbyzero_width format long minimum {} maxim
um {}} value 0} bitoffset {attribs {resolve_type immediate dependency {} format long minimum {} maximum {}} value 0}}} field_divisor_tuser {name {attribs {resolve_type immediate dependency {} format string minimum {} maximum {}} value divisor_tuser} enabled {attribs {resolve_type generated dependency divisor_enabled format bool minimum {} maximum {}} value false} datatype {name {attribs {resolve_type immediate dependency {} format string minimum {} maximum {}} value {}} bitwidth {attribs {resolv
e_type generated dependency divisor_width format long minimum {} maximum {}} value 0} bitoffset {attribs {resolve_type generated dependency divisor_offset format long minimum {} maximum {}} value 0} integer {signed {attribs {resolve_type immediate dependency {} format bool minimum {} maximum {}} value false}}}} field_dividend_tuser {name {attribs {resolve_type immediate dependency {} format string minimum {} maximum {}} value dividend_tuser} enabled {attribs {resolve_type generated dependency di
vidend_enabled format bool minimum {} maximum {}} value false} datatype {name {attribs {resolve_type immediate dependency {} format string minimum {} maximum {}} value {}} bitwidth {attribs {resolve_type generated dependency dividend_width format long minimum {} maximum {}} value 0} bitoffset {attribs {resolve_type generated dependency dividend_offset format long minimum {} maximum {}} value 0} integer {signed {attribs {resolve_type immediate dependency {} format bool minimum {} maximum {}} valu
e false}}}}}}} TUSER_WIDTH 0}</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DOUT.PHASE">0.000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DOUT.TDATA_NUM_BYTES">7</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DOUT.TDEST_WIDTH">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DOUT.TID_WIDTH">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DOUT.TUSER_WIDTH">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVIDEND.CLK_DOMAIN">div_gen_clk</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVIDEND.FREQ_HZ">200000000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVIDEND.HAS_TKEEP">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVIDEND.HAS_TLAST">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVIDEND.HAS_TREADY">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVIDEND.HAS_TSTRB">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVIDEND.INSERT_VIP">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVIDEND.LAYERED_METADATA">undef</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVIDEND.PHASE">0.000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVIDEND.TDATA_NUM_BYTES">4</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVIDEND.TDEST_WIDTH">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVIDEND.TID_WIDTH">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVIDEND.TUSER_WIDTH">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVISOR.CLK_DOMAIN">div_gen_clk</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVISOR.FREQ_HZ">200000000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVISOR.HAS_TKEEP">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVISOR.HAS_TLAST">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVISOR.HAS_TREADY">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVISOR.HAS_TSTRB">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVISOR.INSERT_VIP">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVISOR.LAYERED_METADATA">undef</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVISOR.PHASE">0.000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVISOR.TDATA_NUM_BYTES">3</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVISOR.TDEST_WIDTH">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVISOR.TID_WIDTH">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVISOR.TUSER_WIDTH">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.ALGORITHM_TYPE">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_HAS_ACLKEN">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_HAS_ARESETN">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_HAS_DIV_BY_ZERO">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_HAS_S_AXIS_DIVIDEND_TLAST">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_HAS_S_AXIS_DIVIDEND_TUSER">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_HAS_S_AXIS_DIVISOR_TLAST">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_HAS_S_AXIS_DIVISOR_TUSER">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_LATENCY">36</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_M_AXIS_DOUT_TDATA_WIDTH">56</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_M_AXIS_DOUT_TUSER_WIDTH">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_S_AXIS_DIVIDEND_TDATA_WIDTH">32</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_S_AXIS_DIVIDEND_TUSER_WIDTH">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_S_AXIS_DIVISOR_TDATA_WIDTH">24</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_S_AXIS_DIVISOR_TUSER_WIDTH">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_THROTTLE_SCHEME">3</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_TLAST_RESOLUTION">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_XDEVICEFAMILY">zynq</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.DIVCLK_SEL">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.DIVIDEND_WIDTH">32</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.DIVISOR_WIDTH">24</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.FRACTIONAL_B">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.FRACTIONAL_WIDTH">24</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.SIGNED_B">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.ACLKEN">false</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.ARESETN">false</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.Component_Name">div_gen_div_gen_0_0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.FlowControl">NonBlocking</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.OptimizeGoal">Performance</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.OutTLASTBehv">Null</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.OutTready">false</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.algorithm_type">Radix2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.clocks_per_division">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.divide_by_zero_detect">false</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.dividend_and_quotient_width">32</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.dividend_has_tlast">false</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.dividend_has_tuser">false</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.dividend_tuser_width">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.divisor_has_tlast">false</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.divisor_has_tuser">false</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.divisor_tuser_width">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.divisor_width">24</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.fractional_width">24</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.latency">36</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.latency_configuration">Manual</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.operand_sign">Signed</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.remainder_type">Fractional</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.ARCHITECTURE">zynq</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.BASE_BOARD_PART">xilinx.com:zc706:part0:1.2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.BOARD_CONNECTIONS"/>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.DEVICE">xc7z045</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.PACKAGE">ffg900</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.PREFHDL">VERILOG</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.SILICON_REVISION"/>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.SIMULATOR_LANGUAGE">MIXED</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.SPEEDGRADE">-2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.TEMPERATURE_GRADE"/>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.USE_RDI_CUSTOMIZATION">TRUE</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.USE_RDI_GENERATION">TRUE</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="RUNTIME_PARAM.IPCONTEXT">IP_Integrator</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="RUNTIME_PARAM.IPREVISION">14</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="RUNTIME_PARAM.MANAGED">TRUE</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="RUNTIME_PARAM.OUTPUTDIR">.</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="RUNTIME_PARAM.SELECTEDSIMMODEL"/>
        <spirit:configurableElementValue spirit:referenceId="RUNTIME_PARAM.SHAREDDIR">../../ipshared</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="RUNTIME_PARAM.SWVERSION">2018.3</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="RUNTIME_PARAM.SYNTHESISFLOW">OUT_OF_CONTEXT</spirit:configurableElementValue>
      </spirit:configurableElementValues>
      <spirit:vendorExtensions>
        <xilinx:componentInstanceExtensions>
          <xilinx:configElementInfos>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.ACLK_INTF.CLK_DOMAIN" xilinx:valueSource="default_prop" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.ACLK_INTF.FREQ_HZ" xilinx:valueSource="user_prop" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.M_AXIS_DOUT.CLK_DOMAIN" xilinx:valueSource="default_prop" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.M_AXIS_DOUT.FREQ_HZ" xilinx:valueSource="user_prop" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.M_AXIS_DOUT.HAS_TKEEP" xilinx:valueSource="constant" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.M_AXIS_DOUT.HAS_TLAST" xilinx:valueSource="auto" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.M_AXIS_DOUT.HAS_TREADY" xilinx:valueSource="auto" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.M_AXIS_DOUT.HAS_TSTRB" xilinx:valueSource="constant" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.M_AXIS_DOUT.LAYERED_METADATA" xilinx:valueSource="propagated" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.M_AXIS_DOUT.PHASE" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.M_AXIS_DOUT.TDATA_NUM_BYTES" xilinx:valueSource="auto" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.M_AXIS_DOUT.TDEST_WIDTH" xilinx:valueSource="constant" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.M_AXIS_DOUT.TID_WIDTH" xilinx:valueSource="constant" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.M_AXIS_DOUT.TUSER_WIDTH" xilinx:valueSource="auto" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVIDEND.CLK_DOMAIN" xilinx:valueSource="default_prop" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVIDEND.FREQ_HZ" xilinx:valueSource="user_prop" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVIDEND.HAS_TKEEP" xilinx:valueSource="constant" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVIDEND.HAS_TLAST" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVIDEND.HAS_TREADY" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVIDEND.HAS_TSTRB" xilinx:valueSource="constant" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVIDEND.TDATA_NUM_BYTES" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVIDEND.TDEST_WIDTH" xilinx:valueSource="constant" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVIDEND.TID_WIDTH" xilinx:valueSource="constant" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVIDEND.TUSER_WIDTH" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVISOR.CLK_DOMAIN" xilinx:valueSource="default_prop" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVISOR.FREQ_HZ" xilinx:valueSource="user_prop" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVISOR.HAS_TKEEP" xilinx:valueSource="constant" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVISOR.HAS_TLAST" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVISOR.HAS_TREADY" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVISOR.HAS_TSTRB" xilinx:valueSource="constant" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVISOR.TDATA_NUM_BYTES" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVISOR.TDEST_WIDTH" xilinx:valueSource="constant" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVISOR.TID_WIDTH" xilinx:valueSource="constant" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DIVISOR.TUSER_WIDTH" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="PARAM_VALUE.dividend_and_quotient_width" xilinx:valueSource="user"/>
            <xilinx:configElementInfo xilinx:referenceId="PARAM_VALUE.divisor_width" xilinx:valueSource="user"/>
            <xilinx:configElementInfo xilinx:referenceId="PARAM_VALUE.fractional_width" xilinx:valueSource="user"/>
            <xilinx:configElementInfo xilinx:referenceId="PARAM_VALUE.latency" xilinx:valueSource="user"/>
            <xilinx:configElementInfo xilinx:referenceId="PARAM_VALUE.latency_configuration" xilinx:valueSource="user"/>
            <xilinx:configElementInfo xilinx:referenceId="PARAM_VALUE.operand_sign" xilinx:valueSource="propagated" xilinx:valuePermission="bd_and_user"/>
            <xilinx:configElementInfo xilinx:referenceId="PARAM_VALUE.remainder_type" xilinx:valueSource="user"/>
          </xilinx:configElementInfos>
        </xilinx:componentInstanceExtensions>
      </spirit:vendorExtensions>
    </spirit:componentInstance>
  </spirit:componentInstances>
</spirit:design>
