From 536581825219e97fa2ae0c4de35605d2f6311416 Mon Sep 17 00:00:00 2001
From: Vincent Tremblay <vincent@vtremblay.dev>
Date: Tue, 27 Dec 2022 09:00:58 -0500
Subject: [PATCH 2/2] spidev: Add Silicon Labs SI3210 device compatible

Add compatible string for Silicon Labs SI3210 device.

Note: This patch is adapted from a patch submitted to the for-next branch (v6.3).

Signed-off-by: Vincent Tremblay <vincent@vtremblay.dev>
---
 drivers/spi/spidev.c | 2 ++
 1 file changed, 2 insertions(+)

--- a/drivers/spi/spidev.c
+++ b/drivers/spi/spidev.c
@@ -701,6 +701,7 @@ static const struct spi_device_id spidev
 	{ .name = "spi-petra" },
 	{ .name = "spi-authenta" },
 	{ .name = "em3581" },
+	{ .name = "si3210" },
 	{},
 };
 MODULE_DEVICE_TABLE(spi, spidev_spi_ids);
@@ -728,6 +729,7 @@ static const struct of_device_id spidev_
 	{ .compatible = "cisco,spi-petra", .data = &spidev_of_check },
 	{ .compatible = "micron,spi-authenta", .data = &spidev_of_check },
 	{ .compatible = "silabs,em3581", .data = &spidev_of_check },
+	{ .compatible = "silabs,si3210", .data = &spidev_of_check },
 	{},
 };
 MODULE_DEVICE_TABLE(of, spidev_dt_ids);
