--- a/arch/arm/Kconfig
+++ b/arch/arm/Kconfig
@@ -869,6 +869,20 @@ config ARCH_EXYNOS
 	help
 	  Support for SAMSUNG's EXYNOS SoCs (EXYNOS4/5)
 
+config ARCH_MCS814X
+	bool "Moschip MCS814x"
+	select CPU_ARM926T
+	select PCI
+	select FIQ
+	select GENERIC_IRQ_CHIP
+	select GENERIC_GPIO
+	select ARCH_REQUIRE_GPIOLIB
+	select CLKDEV_LOOKUP
+	select ARCH_USES_GETTIMEOFFSET
+	select NEED_MACH_MEMORY_H
+	help
+	  Support for Moschip MCS814x SoCs (MCS8140).
+
 config ARCH_SHARK
 	bool "Shark"
 	select CPU_SA110
@@ -1065,6 +1080,8 @@ source "arch/arm/plat-samsung/Kconfig"
 source "arch/arm/plat-s3c24xx/Kconfig"
 source "arch/arm/plat-s5p/Kconfig"
 
+source "arch/arm/mach-mcs814x/Kconfig"
+
 source "arch/arm/plat-spear/Kconfig"
 
 if ARCH_S3C2410
--- a/arch/arm/Makefile
+++ b/arch/arm/Makefile
@@ -179,6 +179,7 @@ machine-$(CONFIG_ARCH_S3C64XX)		:= s3c64
 machine-$(CONFIG_ARCH_S5P64X0)		:= s5p64x0
 machine-$(CONFIG_ARCH_S5PC100)		:= s5pc100
 machine-$(CONFIG_ARCH_S5PV210)		:= s5pv210
+machine-$(CONFIG_ARCH_MCS814X)		:= mcs814x
 machine-$(CONFIG_ARCH_EXYNOS4)		:= exynos
 machine-$(CONFIG_ARCH_SA1100)		:= sa1100
 machine-$(CONFIG_ARCH_SHARK)		:= shark
